
GEIST-V4-MIB DEFINITIONS ::= BEGIN

IMPORTS

DisplayString FROM SNMPv2-TC
MODULE-IDENTITY, OBJECT-TYPE, IpAddress, enterprises, Integer32, Gauge32, NOTIFICATION-TYPE FROM SNMPv2-SMI;

geist MODULE-IDENTITY
	LAST-UPDATED "201209110000Z"
	ORGANIZATION "Geist"
	CONTACT-INFO "support@geistglobal.com"
	DESCRIPTION "The MIB for Geist Products"
	REVISION "201209110000Z"
	DESCRIPTION "Original version"
	::= { enterprises 21239 }

blackbird OBJECT IDENTIFIER
	::= { geist 5 }
watchdog100 OBJECT IDENTIFIER
	::= { blackbird 1 }

--###########################################################################################--
--deviceInfo--
--###########################################################################################--

deviceInfo OBJECT IDENTIFIER
	::= { watchdog100 1 }

productTitle OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Product name"
	::= { deviceInfo 1 }

productVersion OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Product version"
	::= { deviceInfo 2 }

productFriendlyName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "User-assigned name"
	::= { deviceInfo 3 }

productMacAddress OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Product's unique MAC address"
	::= { deviceInfo 4 }

productUrl OBJECT-TYPE
	SYNTAX IpAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Product's main URL access point"
	::= { deviceInfo 5 }

deviceCount OBJECT-TYPE
	SYNTAX Integer32(0..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Total number of devices on unit"
	::= { deviceInfo 6 }

temperatureUnits OBJECT-TYPE
	SYNTAX Integer32(0..1)
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION "Current units for temperature values. 0 = Degrees Fahrenheit, 1 = Degrees Celsius"
	::= { deviceInfo 7 }

--###########################################################################################--
--internalTable--
--###########################################################################################--

internalTable OBJECT-TYPE
	SYNTAX SEQUENCE OF InternalEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Internal sensors for units"
	::= { watchdog100 2 }

internalEntry OBJECT-TYPE
	SYNTAX InternalEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the internalTable table: each entry contains an index and other sensor details"
	INDEX { internalIndex }
	::= { internalTable 1 }

InternalEntry ::= SEQUENCE {
	internalIndex				Integer32,
	internalSerial				DisplayString,
	internalName				DisplayString,
	internalAvail				Gauge32,
	internalTemp				Integer32,
	internalHumidity				Integer32,
	internalDewPoint				Integer32
}

internalIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { internalEntry 1 }

internalSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { internalEntry 2 }

internalName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { internalEntry 3 }

internalAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { internalEntry 4 }

internalTemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Temperature in tenths of degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { internalEntry 5 }

internalHumidity OBJECT-TYPE
	SYNTAX Integer32(0..100)
	UNITS "%"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Humidity reading"
	::= { internalEntry 6 }

internalDewPoint OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Dew-point in tenths of degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { internalEntry 7 }

--###########################################################################################--
--tempSensorTable--
--###########################################################################################--

tempSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF TempSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Remote Temperature Sensor"
	::= { watchdog100 4 }

tempSensorEntry OBJECT-TYPE
	SYNTAX TempSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the tempSensorTable table: each entry contains an index and other sensor details"
	INDEX { tempSensorIndex }
	::= { tempSensorTable 1 }

TempSensorEntry ::= SEQUENCE {
	tempSensorIndex				Integer32,
	tempSensorSerial				DisplayString,
	tempSensorName				DisplayString,
	tempSensorAvail				Gauge32,
	tempSensorTemp				Integer32
}

tempSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { tempSensorEntry 1 }

tempSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { tempSensorEntry 2 }

tempSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { tempSensorEntry 3 }

tempSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { tempSensorEntry 4 }

tempSensorTemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Temperature in tenths of degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { tempSensorEntry 5 }

--###########################################################################################--
--airFlowSensorTable--
--###########################################################################################--

airFlowSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF AirFlowSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Remote Airflow, Humidity, Temperature and Dewpoint Sensor "
	::= { watchdog100 5 }

airFlowSensorEntry OBJECT-TYPE
	SYNTAX AirFlowSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the airFlowSensorTable table: each entry contains an index and other sensor details"
	INDEX { airFlowSensorIndex }
	::= { airFlowSensorTable 1 }

AirFlowSensorEntry ::= SEQUENCE {
	airFlowSensorIndex				Integer32,
	airFlowSensorSerial				DisplayString,
	airFlowSensorName				DisplayString,
	airFlowSensorAvail				Gauge32,
	airFlowSensorTemp				Integer32,
	airFlowSensorFlow				Integer32,
	airFlowSensorHumidity				Integer32,
	airFlowSensorDewPoint				Integer32
}

airFlowSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { airFlowSensorEntry 1 }

airFlowSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { airFlowSensorEntry 2 }

airFlowSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { airFlowSensorEntry 3 }

airFlowSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { airFlowSensorEntry 4 }

airFlowSensorTemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Temperature in tenths of degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { airFlowSensorEntry 5 }

airFlowSensorFlow OBJECT-TYPE
	SYNTAX Integer32(0..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "AFHT3 Airflow reading"
	::= { airFlowSensorEntry 6 }

airFlowSensorHumidity OBJECT-TYPE
	SYNTAX Integer32(0..100)
	UNITS "%"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "AFHT3 Humidity reading"
	::= { airFlowSensorEntry 7 }

airFlowSensorDewPoint OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Dew Point in tenths of degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { airFlowSensorEntry 8 }

--###########################################################################################--
--dewPointSensorTable--
--###########################################################################################--

dewPointSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF DewPointSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Remote Dew Point sensor"
	::= { watchdog100 6 }

dewPointSensorEntry OBJECT-TYPE
	SYNTAX DewPointSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the dewPointSensorTable table: each entry contains an index and other sensor details"
	INDEX { dewPointSensorIndex }
	::= { dewPointSensorTable 1 }

DewPointSensorEntry ::= SEQUENCE {
	dewPointSensorIndex				Integer32,
	dewPointSensorSerial				DisplayString,
	dewPointSensorName				DisplayString,
	dewPointSensorAvail				Gauge32,
	dewPointSensorTemp				Integer32,
	dewPointSensorHumidity				Integer32,
	dewPointSensorDewPoint				Integer32
}

dewPointSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { dewPointSensorEntry 1 }

dewPointSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { dewPointSensorEntry 2 }

dewPointSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { dewPointSensorEntry 3 }

dewPointSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { dewPointSensorEntry 4 }

dewPointSensorTemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Temperature in tenths of degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { dewPointSensorEntry 5 }

dewPointSensorHumidity OBJECT-TYPE
	SYNTAX Integer32(0..100)
	UNITS "%"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Humidity reading"
	::= { dewPointSensorEntry 6 }

dewPointSensorDewPoint OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Dew-point in tenths of degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { dewPointSensorEntry 7 }

--###########################################################################################--
--ccatSensorTable--
--###########################################################################################--

ccatSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CcatSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Remote CCAT sensor"
	::= { watchdog100 7 }

ccatSensorEntry OBJECT-TYPE
	SYNTAX CcatSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the ccatSensorTable table: each entry contains an index and other sensor details"
	INDEX { ccatSensorIndex }
	::= { ccatSensorTable 1 }

CcatSensorEntry ::= SEQUENCE {
	ccatSensorIndex				Integer32,
	ccatSensorSerial				DisplayString,
	ccatSensorName				DisplayString,
	ccatSensorAvail				Gauge32,
	ccatSensorValue				Integer32,
	ccatSensorType				DisplayString,
	ccatSensorDescription				DisplayString
}

ccatSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { ccatSensorEntry 1 }

ccatSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { ccatSensorEntry 2 }

ccatSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { ccatSensorEntry 3 }

ccatSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { ccatSensorEntry 4 }

ccatSensorValue OBJECT-TYPE
	SYNTAX Integer32(-100..5000)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "CCAT sensor reading"
	::= { ccatSensorEntry 5 }

ccatSensorType OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "CCAT sensor type"
	::= { ccatSensorEntry 6 }

ccatSensorDescription OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "CCAT sensor value description"
	::= { ccatSensorEntry 7 }

--###########################################################################################--
--t3hdSensorTable--
--###########################################################################################--

t3hdSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF T3hdSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Remote Temperature x 3, Humidity and Dewpoint Sensor"
	::= { watchdog100 8 }

t3hdSensorEntry OBJECT-TYPE
	SYNTAX T3hdSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the t3hdSensorTable table: each entry contains an index and other sensor details"
	INDEX { t3hdSensorIndex }
	::= { t3hdSensorTable 1 }

T3hdSensorEntry ::= SEQUENCE {
	t3hdSensorIndex				Integer32,
	t3hdSensorSerial				DisplayString,
	t3hdSensorName				DisplayString,
	t3hdSensorAvail				Gauge32,
	t3hdSensorIntName				DisplayString,
	t3hdSensorIntTemp				Integer32,
	t3hdSensorIntHumidity				Integer32,
	t3hdSensorIntDewPoint				Integer32,
	t3hdSensorExtAAvail				Gauge32,
	t3hdSensorExtAName				DisplayString,
	t3hdSensorExtATemp				Integer32,
	t3hdSensorExtBAvail				Gauge32,
	t3hdSensorExtBName				DisplayString,
	t3hdSensorExtBTemp				Integer32
}

t3hdSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { t3hdSensorEntry 1 }

t3hdSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { t3hdSensorEntry 2 }

t3hdSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { t3hdSensorEntry 3 }

t3hdSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { t3hdSensorEntry 4 }

t3hdSensorIntName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "T3HD Sensor Internal Friendly Name"
	::= { t3hdSensorEntry 5 }

t3hdSensorIntTemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Internal Temperature in 0.1 degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { t3hdSensorEntry 6 }

t3hdSensorIntHumidity OBJECT-TYPE
	SYNTAX Integer32(0..100)
	UNITS "%"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "T3HD Sensor Internal Humidity"
	::= { t3hdSensorEntry 7 }

t3hdSensorIntDewPoint OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Internal DewPoint in 0.1 degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { t3hdSensorEntry 8 }

t3hdSensorExtAAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "T3HD External A status: 0 = Unavailable, 1 = Available"
	::= { t3hdSensorEntry 9 }

t3hdSensorExtAName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "T3HD External A Friendly Name"
	::= { t3hdSensorEntry 10 }

t3hdSensorExtATemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for External Temperature A in 0.1 degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { t3hdSensorEntry 11 }

t3hdSensorExtBAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "T3HD External B status: 0 = Unavailable, 1 = Available"
	::= { t3hdSensorEntry 12 }

t3hdSensorExtBName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "T3HD External B Friendly Name"
	::= { t3hdSensorEntry 13 }

t3hdSensorExtBTemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for External Temperature B in 0.1 degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { t3hdSensorEntry 14 }

--###########################################################################################--
--thdSensorTable--
--###########################################################################################--

thdSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ThdSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Remote Temperature, Humidity and Dewpoint Sensor"
	::= { watchdog100 9 }

thdSensorEntry OBJECT-TYPE
	SYNTAX ThdSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the thdSensorTable table: each entry contains an index and other sensor details"
	INDEX { thdSensorIndex }
	::= { thdSensorTable 1 }

ThdSensorEntry ::= SEQUENCE {
	thdSensorIndex				Integer32,
	thdSensorSerial				DisplayString,
	thdSensorName				DisplayString,
	thdSensorAvail				Gauge32,
	thdSensorTemp				Integer32,
	thdSensorHumidity				Integer32,
	thdSensorDewPoint				Integer32
}

thdSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { thdSensorEntry 1 }

thdSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { thdSensorEntry 2 }

thdSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { thdSensorEntry 3 }

thdSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { thdSensorEntry 4 }

thdSensorTemp OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for Temperature in 0.1 degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { thdSensorEntry 5 }

thdSensorHumidity OBJECT-TYPE
	SYNTAX Integer32(0..100)
	UNITS "%"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "THD Sensor Humidity"
	::= { thdSensorEntry 6 }

thdSensorDewPoint OBJECT-TYPE
	SYNTAX Integer32(-40..200)
	UNITS "0.1 Degrees"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current reading for DewPoint in 0.1 degrees. Units are given by temperatureUnits field in deviceInfo"
	::= { thdSensorEntry 7 }

--###########################################################################################--
--rpmSensorTable--
--###########################################################################################--

rpmSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF RpmSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Remote Power Manager Sensor"
	::= { watchdog100 10 }

rpmSensorEntry OBJECT-TYPE
	SYNTAX RpmSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the rpmSensorTable table: each entry contains an index and other sensor details"
	INDEX { rpmSensorIndex }
	::= { rpmSensorTable 1 }

RpmSensorEntry ::= SEQUENCE {
	rpmSensorIndex				Integer32,
	rpmSensorSerial				DisplayString,
	rpmSensorName				DisplayString,
	rpmSensorAvail				Gauge32,
	rpmSensorEnergy				Gauge32,
	rpmSensorVoltage				Gauge32,
	rpmSensorVoltageMax				Gauge32,
	rpmSensorVoltageMin				Gauge32,
	rpmSensorVoltagePeak				Gauge32,
	rpmSensorCurrent				Gauge32,
	rpmSensorRealPower				Gauge32,
	rpmSensorApparentPower				Gauge32,
	rpmSensorPowerFactor				Gauge32,
	rpmSensorOutlet1				Gauge32,
	rpmSensorOutlet2				Gauge32
}

rpmSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { rpmSensorEntry 1 }

rpmSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { rpmSensorEntry 2 }

rpmSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { rpmSensorEntry 3 }

rpmSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { rpmSensorEntry 4 }

rpmSensorEnergy OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "kWh"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Accumulated Energy"
	::= { rpmSensorEntry 5 }

rpmSensorVoltage OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "Volts (rms)"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Voltage"
	::= { rpmSensorEntry 6 }

rpmSensorVoltageMax OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "Volts (rms)"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Max)"
	::= { rpmSensorEntry 7 }

rpmSensorVoltageMin OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "Volts (rms)"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Min)"
	::= { rpmSensorEntry 8 }

rpmSensorVoltagePeak OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "Volts"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Peak)"
	::= { rpmSensorEntry 9 }

rpmSensorCurrent OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "0.1 Amps (rms)"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Current reading in deciAmps"
	::= { rpmSensorEntry 10 }

rpmSensorRealPower OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "Watts"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Real Power"
	::= { rpmSensorEntry 11 }

rpmSensorApparentPower OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "Volt-Amps"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Apparent Power"
	::= { rpmSensorEntry 12 }

rpmSensorPowerFactor OBJECT-TYPE
	SYNTAX Gauge32
	UNITS "%"
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Power Factor"
	::= { rpmSensorEntry 13 }

rpmSensorOutlet1 OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Outlet 1 State: 0 = off, 1 = on"
	::= { rpmSensorEntry 14 }

rpmSensorOutlet2 OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "RPM Sensor Outlet 2 State: 0 = off, 1 = on"
	::= { rpmSensorEntry 15 }

--###########################################################################################--
--a2dSensorTable--
--###########################################################################################--

a2dSensorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF A2DSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Analog Measurement Sensor (Voltage, Current, or Dry Contact)"
	::= { watchdog100 11 }

a2DSensorEntry OBJECT-TYPE
	SYNTAX A2DSensorEntry
	MAX-ACCESS  not-accessible
	STATUS current
	DESCRIPTION "Entry in the a2dSensorTable table: each entry contains an index and other sensor details"
	INDEX { a2dSensorIndex }
	::= { a2dSensorTable 1 }

A2DSensorEntry ::= SEQUENCE {
	a2dSensorIndex				Integer32,
	a2dSensorSerial				DisplayString,
	a2dSensorName				DisplayString,
	a2dSensorAvail				Gauge32,
	a2dSensorValue				Integer32
}

a2dSensorIndex OBJECT-TYPE
	SYNTAX Integer32(1..100)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Table entry index value"
	::= { a2DSensorEntry 1 }

a2dSensorSerial OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Serial Number"
	::= { a2DSensorEntry 2 }

a2dSensorName OBJECT-TYPE
	SYNTAX DisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Friendly Name"
	::= { a2DSensorEntry 3 }

a2dSensorAvail OBJECT-TYPE
	SYNTAX Gauge32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable"
	::= { a2DSensorEntry 4 }

a2dSensorValue OBJECT-TYPE
	SYNTAX Integer32(-1000000..1000000)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION "Current analog measurement reading within either a user defined or preset range depending on device mode."
	::= { a2DSensorEntry 5 }

--###########################################################################################--
--Notifications--
--###########################################################################################--

trap OBJECT IDENTIFIER ::= { watchdog100 32767 }
trapPrefix OBJECT IDENTIFIER ::= { trap 0 }

internalTestNOTIFY NOTIFICATION-TYPE
	STATUS current
	DESCRIPTION "Test SNMP Trap"
	::= { trapPrefix 10101 }

--#####deviceInfo#####--

--#####internalTable#####--

internalAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { internalAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 10204 }

internalAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { internalAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 20204 }

internalTempNOTIFY NOTIFICATION-TYPE
	OBJECTS { internalTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "Internal Temperature Sensor Trap"
	::= { trapPrefix 10205 }

internalTempCLEAR NOTIFICATION-TYPE
	OBJECTS { internalTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "Internal Temperature Sensor Clear Trap"
	::= { trapPrefix 20205 }

internalHumidityNOTIFY NOTIFICATION-TYPE
	OBJECTS { internalHumidity }
	STATUS current
	DESCRIPTION "Humidity reading Trap"
	::= { trapPrefix 10206 }

internalHumidityCLEAR NOTIFICATION-TYPE
	OBJECTS { internalHumidity }
	STATUS current
	DESCRIPTION "Humidity reading Clear Trap"
	::= { trapPrefix 20206 }

internalDewPointNOTIFY NOTIFICATION-TYPE
	OBJECTS { internalDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "Internal Dew Point Sensor Trap"
	::= { trapPrefix 10207 }

internalDewPointCLEAR NOTIFICATION-TYPE
	OBJECTS { internalDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "Internal Dew Point Sensor Clear Trap"
	::= { trapPrefix 20207 }

--#####tempSensorTable#####--

tempSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { tempSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 10404 }

tempSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { tempSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 20404 }

tempSensorTempNOTIFY NOTIFICATION-TYPE
	OBJECTS { tempSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "Remote Temperature Sensor Trap"
	::= { trapPrefix 10405 }

tempSensorTempCLEAR NOTIFICATION-TYPE
	OBJECTS { tempSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "Remote Temperature Sensor Clear Trap"
	::= { trapPrefix 20405 }

--#####airFlowSensorTable#####--

airFlowSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { airFlowSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 10504 }

airFlowSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { airFlowSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 20504 }

airFlowSensorTempNOTIFY NOTIFICATION-TYPE
	OBJECTS { airFlowSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "AFHT3 Sensor Temperature Trap"
	::= { trapPrefix 10505 }

airFlowSensorTempCLEAR NOTIFICATION-TYPE
	OBJECTS { airFlowSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "AFHT3 Sensor Temperature Clear Trap"
	::= { trapPrefix 20505 }

airFlowSensorFlowNOTIFY NOTIFICATION-TYPE
	OBJECTS { airFlowSensorFlow }
	STATUS current
	DESCRIPTION "AFHT3 Airflow reading Trap"
	::= { trapPrefix 10506 }

airFlowSensorFlowCLEAR NOTIFICATION-TYPE
	OBJECTS { airFlowSensorFlow }
	STATUS current
	DESCRIPTION "AFHT3 Airflow reading Clear Trap"
	::= { trapPrefix 20506 }

airFlowSensorHumidityNOTIFY NOTIFICATION-TYPE
	OBJECTS { airFlowSensorHumidity }
	STATUS current
	DESCRIPTION "AFHT3 Humidity reading Trap"
	::= { trapPrefix 10507 }

airFlowSensorHumidityCLEAR NOTIFICATION-TYPE
	OBJECTS { airFlowSensorHumidity }
	STATUS current
	DESCRIPTION "AFHT3 Humidity reading Clear Trap"
	::= { trapPrefix 20507 }

airFlowSensorDewPointNOTIFY NOTIFICATION-TYPE
	OBJECTS { airFlowSensorDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "AFHT3 Sensor Dew Point Trap"
	::= { trapPrefix 10508 }

airFlowSensorDewPointCLEAR NOTIFICATION-TYPE
	OBJECTS { airFlowSensorDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "AFHT3 Sensor Dew Point Clear Trap"
	::= { trapPrefix 20508 }

--#####dewPointSensorTable#####--

dewPointSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { dewPointSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 10604 }

dewPointSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { dewPointSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 20604 }

dewPointSensorTempNOTIFY NOTIFICATION-TYPE
	OBJECTS { dewPointSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "Remote Dew Point Sensor Temperature Trap"
	::= { trapPrefix 10605 }

dewPointSensorTempCLEAR NOTIFICATION-TYPE
	OBJECTS { dewPointSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "Remote Dew Point Sensor Temperature Clear Trap"
	::= { trapPrefix 20605 }

dewPointSensorHumidityNOTIFY NOTIFICATION-TYPE
	OBJECTS { dewPointSensorHumidity }
	STATUS current
	DESCRIPTION "Humidity reading Trap"
	::= { trapPrefix 10606 }

dewPointSensorHumidityCLEAR NOTIFICATION-TYPE
	OBJECTS { dewPointSensorHumidity }
	STATUS current
	DESCRIPTION "Humidity reading Clear Trap"
	::= { trapPrefix 20606 }

dewPointSensorDewPointNOTIFY NOTIFICATION-TYPE
	OBJECTS { dewPointSensorDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "Remote Dew Point Sensor Dew Point Trap"
	::= { trapPrefix 10607 }

dewPointSensorDewPointCLEAR NOTIFICATION-TYPE
	OBJECTS { dewPointSensorDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "Remote Dew Point Sensor Dew Point Clear Trap"
	::= { trapPrefix 20607 }

--#####ccatSensorTable#####--

ccatSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { ccatSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 10704 }

ccatSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { ccatSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 20704 }

ccatSensorValueNOTIFY NOTIFICATION-TYPE
	OBJECTS { ccatSensorValue, ccatSensorType }
	STATUS current
	DESCRIPTION "CCAT sensor reading Trap"
	::= { trapPrefix 10705 }

ccatSensorValueCLEAR NOTIFICATION-TYPE
	OBJECTS { ccatSensorValue, ccatSensorType }
	STATUS current
	DESCRIPTION "CCAT sensor reading Clear Trap"
	::= { trapPrefix 20705 }

--#####t3hdSensorTable#####--

t3hdSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { t3hdSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 10804 }

t3hdSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { t3hdSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 20804 }

t3hdSensorIntTempNOTIFY NOTIFICATION-TYPE
	OBJECTS { t3hdSensorIntTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor Temperature Trap"
	::= { trapPrefix 10806 }

t3hdSensorIntTempCLEAR NOTIFICATION-TYPE
	OBJECTS { t3hdSensorIntTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor Temperature Clear Trap"
	::= { trapPrefix 20806 }

t3hdSensorIntHumidityNOTIFY NOTIFICATION-TYPE
	OBJECTS { t3hdSensorIntHumidity }
	STATUS current
	DESCRIPTION "T3HD Sensor Internal Humidity Trap"
	::= { trapPrefix 10807 }

t3hdSensorIntHumidityCLEAR NOTIFICATION-TYPE
	OBJECTS { t3hdSensorIntHumidity }
	STATUS current
	DESCRIPTION "T3HD Sensor Internal Humidity Clear Trap"
	::= { trapPrefix 20807 }

t3hdSensorIntDewPointNOTIFY NOTIFICATION-TYPE
	OBJECTS { t3hdSensorIntDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor Dew Point Trap"
	::= { trapPrefix 10808 }

t3hdSensorIntDewPointCLEAR NOTIFICATION-TYPE
	OBJECTS { t3hdSensorIntDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor Dew Point Clear Trap"
	::= { trapPrefix 20808 }

t3hdSensorExtATempNOTIFY NOTIFICATION-TYPE
	OBJECTS { t3hdSensorExtATemp, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor External A Temperature Trap"
	::= { trapPrefix 10811 }

t3hdSensorExtATempCLEAR NOTIFICATION-TYPE
	OBJECTS { t3hdSensorExtATemp, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor External A Temperature Clear Trap"
	::= { trapPrefix 20811 }

t3hdSensorExtBTempNOTIFY NOTIFICATION-TYPE
	OBJECTS { t3hdSensorExtBTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor External B Temperature Trap"
	::= { trapPrefix 10814 }

t3hdSensorExtBTempCLEAR NOTIFICATION-TYPE
	OBJECTS { t3hdSensorExtBTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "T3HD Sensor External B Temperature Clear Trap"
	::= { trapPrefix 20814 }

--#####thdSensorTable#####--

thdSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { thdSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 10904 }

thdSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { thdSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 20904 }

thdSensorTempNOTIFY NOTIFICATION-TYPE
	OBJECTS { thdSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "THD Sensor Temperature Trap"
	::= { trapPrefix 10905 }

thdSensorTempCLEAR NOTIFICATION-TYPE
	OBJECTS { thdSensorTemp, temperatureUnits }
	STATUS current
	DESCRIPTION "THD Sensor Temperature Clear Trap"
	::= { trapPrefix 20905 }

thdSensorHumidityNOTIFY NOTIFICATION-TYPE
	OBJECTS { thdSensorHumidity }
	STATUS current
	DESCRIPTION "THD Sensor Humidity Trap"
	::= { trapPrefix 10906 }

thdSensorHumidityCLEAR NOTIFICATION-TYPE
	OBJECTS { thdSensorHumidity }
	STATUS current
	DESCRIPTION "THD Sensor Humidity Clear Trap"
	::= { trapPrefix 20906 }

thdSensorDewPointNOTIFY NOTIFICATION-TYPE
	OBJECTS { thdSensorDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "THD Sensor Dew Point Trap"
	::= { trapPrefix 10907 }

thdSensorDewPointCLEAR NOTIFICATION-TYPE
	OBJECTS { thdSensorDewPoint, temperatureUnits }
	STATUS current
	DESCRIPTION "THD Sensor Dew Point Clear Trap"
	::= { trapPrefix 20907 }

--#####rpmSensorTable#####--

rpmSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 11004 }

rpmSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 21004 }

rpmSensorEnergyNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorEnergy }
	STATUS current
	DESCRIPTION "RPM Sensor Accumulated Energy Trap"
	::= { trapPrefix 11005 }

rpmSensorEnergyCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorEnergy }
	STATUS current
	DESCRIPTION "RPM Sensor Accumulated Energy Clear Trap"
	::= { trapPrefix 21005 }

rpmSensorVoltageNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltage }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage Trap"
	::= { trapPrefix 11006 }

rpmSensorVoltageCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltage }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage Clear Trap"
	::= { trapPrefix 21006 }

rpmSensorVoltageMaxNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltageMax }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Max) Trap"
	::= { trapPrefix 11007 }

rpmSensorVoltageMaxCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltageMax }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Max) Clear Trap"
	::= { trapPrefix 21007 }

rpmSensorVoltageMinNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltageMin }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Min) Trap"
	::= { trapPrefix 11008 }

rpmSensorVoltageMinCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltageMin }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Min) Clear Trap"
	::= { trapPrefix 21008 }

rpmSensorVoltagePeakNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltagePeak }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Peak) Trap"
	::= { trapPrefix 11009 }

rpmSensorVoltagePeakCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorVoltagePeak }
	STATUS current
	DESCRIPTION "RPM Sensor Voltage (Peak) Clear Trap"
	::= { trapPrefix 21009 }

rpmSensorCurrentNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorCurrent }
	STATUS current
	DESCRIPTION "RPM Sensor Current Trap"
	::= { trapPrefix 11010 }

rpmSensorCurrentCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorCurrent }
	STATUS current
	DESCRIPTION "RPM Sensor Current Clear Trap"
	::= { trapPrefix 21010 }

rpmSensorRealPowerNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorRealPower }
	STATUS current
	DESCRIPTION "RPM Sensor Real Power Trap"
	::= { trapPrefix 11011 }

rpmSensorRealPowerCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorRealPower }
	STATUS current
	DESCRIPTION "RPM Sensor Real Power Clear Trap"
	::= { trapPrefix 21011 }

rpmSensorApparentPowerNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorApparentPower }
	STATUS current
	DESCRIPTION "RPM Sensor Apparent Power Trap"
	::= { trapPrefix 11012 }

rpmSensorApparentPowerCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorApparentPower }
	STATUS current
	DESCRIPTION "RPM Sensor Apparent Power Clear Trap"
	::= { trapPrefix 21012 }

rpmSensorPowerFactorNOTIFY NOTIFICATION-TYPE
	OBJECTS { rpmSensorPowerFactor }
	STATUS current
	DESCRIPTION "RPM Sensor Power Factor Trap"
	::= { trapPrefix 11013 }

rpmSensorPowerFactorCLEAR NOTIFICATION-TYPE
	OBJECTS { rpmSensorPowerFactor }
	STATUS current
	DESCRIPTION "RPM Sensor Power Factor Clear Trap"
	::= { trapPrefix 21013 }

--#####a2dSensorTable#####--

a2dSensorAvailNOTIFY NOTIFICATION-TYPE
	OBJECTS { a2dSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Trap"
	::= { trapPrefix 11104 }

a2dSensorAvailCLEAR NOTIFICATION-TYPE
	OBJECTS { a2dSensorAvail }
	STATUS current
	DESCRIPTION "Device availability. 0 = Unavailable, 1 = Available, 2 = Partially Unavailable Clear Trap"
	::= { trapPrefix 21104 }

a2dSensorValueNOTIFY NOTIFICATION-TYPE
	OBJECTS { a2dSensorValue }
	STATUS current
	DESCRIPTION "A2D Analog Sensor Measurement Trap"
	::= { trapPrefix 11105 }

a2dSensorValueCLEAR NOTIFICATION-TYPE
	OBJECTS { a2dSensorValue }
	STATUS current
	DESCRIPTION "A2D Analog Sensor Measurement Clear Trap"
	::= { trapPrefix 21105 }

END