
-- End - JUNIPER-WX-GLOBAL-REG Module

-- ========================================================================
-- Start - JUNIPER-WX-GLOBAL-TC Module

-- WX Global Textual Conventions
--
-- The convention described in "Understanding SNMP MIBs"
-- (David Perkins, Evan McGinnis), Chapter 8, has generally been followed.

JUNIPER-WX-GLOBAL-TC DEFINITIONS ::= BEGIN

	IMPORTS
		MODULE-IDENTITY
			FROM SNMPv2-SMI
		TEXTUAL-CONVENTION
			FROM SNMPv2-TC
		jnxWxModules
			FROM JUNIPER-WX-GLOBAL-REG;

	jnxWxGlobalTcModule MODULE-IDENTITY
		LAST-UPDATED			"200107292200Z"
		ORGANIZATION			"Juniper Networks, Inc"
		CONTACT-INFO			"
					Customer Support
					Juniper Networks, Inc.
					1194 North Mathilda Avenue
					Sunnyvale, CA  94089

					+1 888-314-JTAC
					support@juniper.net"

		DESCRIPTION				"
			A MIB module containing textual conventions
			for Juniper Networks' enterprise MIB modules.
			These textual conventions are used across all WX products."

		REVISION				"200606081800Z"
		DESCRIPTION				"
			Update contact and MIB with Juniper information
			Add wxc590 and wx60 chassis type."

		REVISION				"200505091010Z"
		DESCRIPTION				"
			Add wxc250 chassis type."

		REVISION				"200403151400Z"
		DESCRIPTION				"
			Add wx100 chassis type."

		REVISION				"200306262000Z"
		DESCRIPTION				"
			Add wx80 chassis type."

		REVISION				"200211071900Z"
		DESCRIPTION				"
			Add wx20 chassis type."

		REVISION				"200107292200Z"
		DESCRIPTION				"
			Rev 1.0
			Initial version of MIB module JUNIPER-WX-GLOBAL-TC."

		::= { jnxWxModules 2 }

	-- No WX textual conventions yet!

	TcAppName ::= TEXTUAL-CONVENTION
		DISPLAY-HINT			"64a"
		STATUS					current
		DESCRIPTION				"
			Represents the name of an application.

			This has all the restrictions of the DisplayString textual
			convention with the following additional ones:

			- Only the following characters/character ranges are allowed:
				0-9
				A-Z
				a-z
				:./#$&_-+()'
				<space>

			Any object defined using this syntax may not exceed 64
			characters in length."
		SYNTAX       OCTET STRING (SIZE (0..64))

	TcQosIdentifier ::= TEXTUAL-CONVENTION
		DISPLAY-HINT			"24a"
		STATUS					current
		DESCRIPTION				"
			Represents the name of a QoS class, a tunnel or
			a tunnel ip address encoded as a string.

			This has all the restrictions of the DisplayString textual
			convention with the following additional ones:

			- Only the following characters/character ranges are allowed:
				0-9
				A-Z
				a-z
				:./#$&_-+()'
				<space>

			Any object defined using this syntax may not exceed 24
			characters in length."
		SYNTAX       OCTET STRING (SIZE (0..24))

	TcChassisType ::= TEXTUAL-CONVENTION
		STATUS					current
		DESCRIPTION				"
			Enumerates all possible chassis types for WX devices."
		SYNTAX
			INTEGER
			{
				jnxWxOther(1),
				jnxWx50(2),
				jnxWx20(3),
				jnxWx80(4),
				jnxWx100(5),
				jnxWxc500(6),
				jnxWx15(7),
				jnxWxc250(8),
				jnxWx100V3(9),
				jnxWx60(10),
				jnxWxc590(11),
				jnxIsm200Wxc(12),
				jnxWxc1800(13),
				jnxWxc2600(14),
				jnxWxc3400(15)
			}
END
