--

-- Copyright (C) 2014 All Rights Reserved.

--



	DIGIPDU-MIB DEFINITIONS ::= BEGIN



	IMPORTS

      MODULE-IDENTITY, NOTIFICATION-TYPE,

      OBJECT-TYPE, enterprises                            FROM SNMPv2-SMI

      DisplayString                                       FROM SNMPv2-TC

      TRAP-TYPE     																			FROM RFC-1215;



  smart MODULE-IDENTITY

		LAST-UPDATED "200904161627Z" -- April 16 2009

		ORGANIZATION ""

		CONTACT-INFO 

			""



		DESCRIPTION "This is the MIB module for the All DIGIPDU Device"

		REVISION "200904161627Z" -- April 16 2009

		DESCRIPTION "V1.00 for the DIGIPDU Device"

		::= { digipdu 3 }



  digipdu OBJECT IDENTIFIER ::= { enterprises 10456 }

			

--

-- Product 

--



	product OBJECT IDENTIFIER 	::= { smart 1 }



	productModel OBJECT-TYPE

		SYNTAX 			DisplayString(SIZE(0..50))

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Model of Device."

	::= { product 1 }



	productPartNumber OBJECT-TYPE

		SYNTAX 			DisplayString(SIZE(0..32))

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"The part number of this appliance as shown on the label."

	::= { product 2 }



	productSerialNumber OBJECT-TYPE

		SYNTAX 			DisplayString(SIZE(0..32))

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"The serial number of this appliance as shown on the label."

	::= { product 3 }



	productFirmwareVersion OBJECT-TYPE

		SYNTAX 			DisplayString(SIZE(0..32))

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"The version of the firmware of this product."

	::= { product 4 }



	productTemperatureKind OBJECT-TYPE

		SYNTAX 			INTEGER(0..1)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Temperature Kind(0:CELSIUS, 1:FAHRENHEIT)."

	::= { product 11 }

		

	productResetDetector OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Display the Nearest Operated Time of Reset Buttom."

	::= { product 21 }

		

--

-- Device Tables

--



	deviceTable  OBJECT IDENTIFIER 	::= { smart 2 }



	deviceATSKind OBJECT-TYPE

		SYNTAX 			INTEGER(1..3)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Device ATS Kind."

	::= { deviceTable 1 }

	

	deviceInFeedTotal OBJECT-TYPE

		SYNTAX 			INTEGER(1..3)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Input Feed Total."

	::= { deviceTable 2 }



	deviceInFeedKind OBJECT-TYPE

		SYNTAX 			INTEGER(1..4)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Input Feed Kind."

	::= { deviceTable 3 }



	deviceInFeedBranch OBJECT-TYPE

		SYNTAX 			INTEGER(1..2)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Input Feed Kind."

	::= { deviceTable 4 }

	

	deviceOutTotal OBJECT-TYPE

		SYNTAX 			INTEGER(1..24)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Out Total."

	::= { deviceTable 5 }



	deviceOutKind OBJECT-TYPE

		SYNTAX 			INTEGER(1..4)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Out Kind."

	::= { deviceTable 6 }

	

	deviceInbuiltTempTotal OBJECT-TYPE

		SYNTAX 			INTEGER(0..1)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Inbuilt Temperature Total."

	::= { deviceTable 7 }



	deviceExtendTemperatureTotal OBJECT-TYPE

		SYNTAX 			INTEGER(0..6)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend ENV Total."

	::= { deviceTable 8 }



	deviceExtendRHTotal OBJECT-TYPE

		SYNTAX 			INTEGER(0..4)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend ENV Total."

	::= { deviceTable 9 }



	devicePDUTotal OBJECT-TYPE

		SYNTAX 			INTEGER(1..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"PDU Total."

	::= { deviceTable 10 }



	deviceInputTotal OBJECT-TYPE

		SYNTAX 			INTEGER(1..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Input Total."

	::= { deviceTable 11 }



	deviceUPS OBJECT-TYPE

		SYNTAX 			INTEGER{

			no(0),

			yes(1)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS."

	::= { deviceTable 12 }



	deviceDaisyChain OBJECT-TYPE

		SYNTAX 			INTEGER{

			no(0),

			yes(1)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Daisy Chain."

	::= { deviceTable 13 }



	deviceUnitTotal OBJECT-TYPE

		SYNTAX 			INTEGER(1..16)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Device Unit Total."

	::= { deviceTable 20 }



--

-- Device Unit Table

--



	deviceUnitTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF DeviceUnitEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Device Unit."

	::= { deviceTable 21 }



	deviceUnitEntry OBJECT-TYPE

		SYNTAX 			DeviceUnitEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Device Unit table."

		INDEX { deviceUnitIndex }

	::= { deviceUnitTable 1 }



	DeviceUnitEntry ::= SEQUENCE {

		deviceUnitIndex			 							INTEGER,

		deviceUnitStatus			 						INTEGER,

		deviceUnitInfeedTotal            	INTEGER, 

		deviceUnitOutTotal           			INTEGER 

	}

	

	deviceUnitIndex OBJECT-TYPE

		SYNTAX 			INTEGER(1..16)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Device Unit table index."

	::= { deviceUnitEntry 1 }



	deviceUnitStatus OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"status in the Device Unit."

	::= { deviceUnitEntry 2 }

	

	deviceUnitInfeedTotal OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Infeed Total of Device Unit."

	::= { deviceUnitEntry 3 }



	deviceUnitOutTotal OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Out Total of Device Unit."

	::= { deviceUnitEntry 4 }



--

-- peripheral Tables

--

	

	peripheralTables  OBJECT IDENTIFIER 	::= { smart 3 }



--

-- ATS Table

--



	aTSTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF ATSEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Auto Transfer Switch."

	::= { peripheralTables 1 }



	aTSEntry OBJECT-TYPE

		SYNTAX 			ATSEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Input Feed table."

		INDEX { aTSIndex }

	::= { aTSTable 1 }



	ATSEntry ::= SEQUENCE {

		aTSIndex			 							INTEGER,

		aTSStatus			 							INTEGER,

		aTSVoltage            			INTEGER, 

		aTSFrequency           			INTEGER 

	}

	

	aTSIndex OBJECT-TYPE

		SYNTAX 			INTEGER(1..2)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Auto Transfer Switch table index."

	::= { aTSEntry 1 }



	aTSStatus OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"status in the Auto Transfer Switch."

	::= { aTSEntry 2 }

	

	aTSVoltage OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Voltage of Auto Transfer Switch."

	::= { aTSEntry 3 }



	aTSFrequency OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Frequency of Auto Transfer Switch."

	::= { aTSEntry 4 }

    

--

-- InFeed Table

--



	inFeedTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF InFeedEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Input Feed."

	::= { peripheralTables 2 }



	inFeedEntry OBJECT-TYPE

		SYNTAX 			InFeedEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Input Feed table."

		INDEX {	inFeedIndex }

	::= { inFeedTable 1 }



	InFeedEntry ::= SEQUENCE {

		inFeedIndex			 							  INTEGER,

		inFeedStatus			 							INTEGER,

		inFeedVoltage            			  INTEGER, 

		inFeedFrequency                 INTEGER,

    inFeedCurrent									  INTEGER,

		inFeedPowerLoad         				INTEGER, 

		inFeedPowerFactor        			  INTEGER, 

		inFeedPowerEnergy         			INTEGER, 

		inFeedOverLoad								  INTEGER,

		inFeedHighWarning							  INTEGER,

		inFeedLowWarning							  INTEGER,

		inFeedBranch			              INTEGER,

		inFeedBranch1Current						INTEGER,

		inFeedBranch1PowerLoad     			INTEGER, 

		inFeedBranch1PowerFactor  			INTEGER, 

		inFeedBranch1OverLoad						INTEGER,

		inFeedBranch1HighWarning				INTEGER,

		inFeedBranch1LowWarning					INTEGER,

		inFeedBranch2Current						INTEGER,

		inFeedBranch2PowerLoad     			INTEGER, 

		inFeedBranch2PowerFactor  			INTEGER, 

		inFeedBranch2OverLoad						INTEGER,

		inFeedBranch2HighWarning				INTEGER,

		inFeedBranch2LowWarning					INTEGER

	}



	inFeedIndex OBJECT-TYPE

		SYNTAX 			INTEGER(1..3)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Input Feed table index."

	::= { inFeedEntry 1 }



	inFeedStatus OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"status in the Input Feed."

	::= { inFeedEntry 2 }

	

	inFeedVoltage OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Voltage of Input Feed."

	::= { inFeedEntry 3 }



	inFeedFrequency OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Frequency of Input Feed."

	::= { inFeedEntry 4 }

    

	inFeedCurrent OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Total Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 5 }



	inFeedPowerLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power in the Input Feed."

	::= { inFeedEntry 6 }



	inFeedPowerFactor OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power factor in the Input Feed."

	::= { inFeedEntry 7 }





	inFeedPowerEnergy OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of energy in the Input Feed."

	::= { inFeedEntry 8 }



	inFeedOverLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"OverLoad of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 9 }



	inFeedHighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"High Warning of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 10 }



	inFeedLowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Low Warning of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 11 }



	inFeedBranch OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 12 }



	inFeedBranch1Current OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 13 }



	inFeedBranch1PowerLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power in the PDU."

	::= { inFeedEntry 14 }



	inFeedBranch1PowerFactor OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power factor in the PDU."

	::= { inFeedEntry 15 }



	inFeedBranch1OverLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"OverLoad of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 16 }



	inFeedBranch1HighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 17 }



	inFeedBranch1LowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 18 }



	inFeedBranch2Current OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 19 }



	inFeedBranch2PowerLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power in the PDU."

	::= { inFeedEntry 20 }



	inFeedBranch2PowerFactor OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power factor in the PDU."

	::= { inFeedEntry 21 }



	inFeedBranch2OverLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"OverLoad of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 22 }



	inFeedBranch2HighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 23 }



	inFeedBranch2LowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { inFeedEntry 24 }



--

-- Outlet Table

--



	outTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF OutletEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Outlet."

	::= { peripheralTables 3 }



	outEntry OBJECT-TYPE

		SYNTAX 			OutletEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Outlet table."

		INDEX {	outIndex }

	::= { outTable 1 }



	OutletEntry ::= SEQUENCE {

		outIndex 											INTEGER,

		outComputerStatus							INTEGER,

		outCurrentStatus 							INTEGER,

		outSwitchStatus								INTEGER,

		outSwitchCtrl								  INTEGER,

		outVoltage      							INTEGER, 

		outCurrent										INTEGER,

		outPowerFactor  							INTEGER, 

		outPowerLoad    							INTEGER, 

		outOverload										INTEGER,

		outHighWarning								INTEGER,

		outLowWarning									INTEGER

	}

	

	outIndex OBJECT-TYPE

		SYNTAX 			INTEGER(1..24)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Out table index."

	::= { outEntry 1 }



	outComputerStatus OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Out computer status."

	::= { outEntry 2 }

	

	outCurrentStatus OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Out Current status."

	::= { outEntry 3 }



	outSwitchStatus OBJECT-TYPE

		SYNTAX 			INTEGER {

			off(0),

			on(1),

			off-act(2),

			on-act(3)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"This OID is provided for Outlet Status information.



		     '0'  if the out is Switch Off.

		     '1'  if the out is Switch On.

		     '2'  if the out is Switch Off Acting.

		     '3'  if the out is Switch On Acting.



			"

	::= { outEntry 4 }



	outSwitchCtrl OBJECT-TYPE

		SYNTAX 			INTEGER {

			none(0),

      ctrl-on(1),

			ctrl-off(2),

			ctrl-reboot(3),

      ctrl-on-off(4)}

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"This OID is provided for Outlet Status information.



		     '0'  if the out is None.

		     '1'  Switch Ctrl On.

		     '2'  Switch Ctrl Off.

		     '3'  Switch Ctrl Reboot.

		     '4'  Switch Ctrl On Off.



			"

	::= { outEntry 5 }

	

	outVoltage OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Voltage of Outlet."

	::= { outEntry 6 }

	

	outCurrent OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Current of Outlet(In tenths of amps, divide by 10 for value in amps)."

	::= { outEntry 7 }



	outPowerFactor OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power factor in the Outlet."

	::= { outEntry 8 }



	outPowerLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power in the Outlet."

	::= { outEntry 9 }



	outOverload OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Overload of Outlet(In tenths of amps, divide by 10 for value in amps)."

	::= { outEntry 10 }



	outHighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"High Warning of Outlet(In tenths of amps, divide by 10 for value in amps)."

	::= { outEntry 11 }



	outLowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Low Warning of Outlet(In tenths of amps, divide by 10 for value in amps)."

	::= { outEntry 12 }



--

-- PDU Table

--



	pduTables OBJECT-TYPE

		SYNTAX 			SEQUENCE OF PDUEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of PDU."

	::= { peripheralTables 4 }

	

	pduEntry OBJECT-TYPE

		SYNTAX 			PDUEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for PDU table."

		INDEX {	pduIndex }

	::= { pduTables 1 }



	PDUEntry ::= SEQUENCE {

		pduIndex 								    INTEGER,

		pduModel       				      DisplayString,

		pduMonitor							    INTEGER,

		pduStatus       				    INTEGER,

		pduVoltage      				    INTEGER, 

		pduFrequency                INTEGER,

		pduCurrent							    INTEGER,

		pduPowerLoad     				    INTEGER, 

		pduPowerFactor  				    INTEGER, 

		pduPowerEnergy     				  INTEGER, 

		pduOverload							    INTEGER,

		pduHighWarning					    INTEGER,

		pduLowWarning						    INTEGER,

		pduBranch                   INTEGER,

		pduBranch1Current						INTEGER,

		pduBranch1Overload					INTEGER,

		pduBranch1HighWarning				INTEGER,

		pduBranch1LowWarning				INTEGER,

		pduBranch2Current						INTEGER,

		pduBranch2Overload					INTEGER,

		pduBranch2HighWarning				INTEGER,

		pduBranch2LowWarning				INTEGER

	}



	pduIndex OBJECT-TYPE

		SYNTAX 			INTEGER(1..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"PDU table index."

	::= { pduEntry 1 }



	pduModel OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Now Power Data Log of PDU(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 2 }



	pduMonitor OBJECT-TYPE

		SYNTAX 			INTEGER {

			no(0),

			yes(1)}

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"PDU Monitor Status."

	::= { pduEntry 3 }



	pduStatus OBJECT-TYPE

		SYNTAX 			INTEGER {

			no(0),

			yes(1),

			warning(2)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"PDU Connect Status."

	::= { pduEntry 4 }



	pduVoltage OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Voltage of PDU."

	::= { pduEntry 5 }



	pduFrequency OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Frequency of PDU."

	::= { pduEntry 6 }

	

	pduCurrent OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Total Current of PDU(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 7 }



	pduPowerLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power in the PDU."

	::= { pduEntry 8 }



	pduPowerFactor OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power factor in the PDU."

	::= { pduEntry 9 }



	pduPowerEnergy OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Actual value of power in the PDU."

	::= { pduEntry 10 }



	pduOverload OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Overload of PDU(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 11 }



	pduHighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"High Warning of PDU(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 12 }



	pduLowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"High Warning of PDU(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 13 }



	pduBranch OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 14 }



	pduBranch1Current OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 15 }



	pduBranch1Overload OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Overload of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 16 }



	pduBranch1HighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 17 }



	pduBranch1LowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 18 }



	pduBranch2Current OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 19 }



	pduBranch2Overload OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Overload of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 20 }



	pduBranch2HighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 21 }



	pduBranch2LowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Average Current of Input Feed(In tenths of amps, divide by 10 for value in amps)."

	::= { pduEntry 22 }



--

-- InbuiltTemperature Table

--



	inbuiltTemperatureTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF InbuiltTemperatureEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Inbuilt Temperature Sensor."

	::= { peripheralTables 5 }



	inbuiltTemperatureEntry OBJECT-TYPE

		SYNTAX 			InbuiltTemperatureEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Inbuilt Temperature Sensor table."

		INDEX {	inbuiltTemperatureIndex }

	::= { inbuiltTemperatureTable 1 }



	InbuiltTemperatureEntry ::= SEQUENCE {

		inbuiltTemperatureIndex 			INTEGER,

		inbuiltTemperatureStatus			INTEGER,

		inbuiltTemperature						INTEGER,

		inbuiltTemperatureHighWarning	INTEGER,

		inbuiltTemperatureLowWarning	INTEGER

	}



	inbuiltTemperatureIndex OBJECT-TYPE

		SYNTAX 			INTEGER (0..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Index for the Inbuilt Temperature Sensor table."

	::= { inbuiltTemperatureEntry 1 }



	inbuiltTemperatureStatus OBJECT-TYPE

		SYNTAX 			INTEGER {

			no(0),

			yes(1)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Inbuilt Temperature Sensor Connect Status."

	::= { inbuiltTemperatureEntry 2 }



	inbuiltTemperature OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Detected Temperature from Inbuilt Temperature Sensor."

	::= { inbuiltTemperatureEntry 3 }



	inbuiltTemperatureHighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"High Warning Temperature from Inbuilt Temperature Sensor."

	::= { inbuiltTemperatureEntry 4 }



	inbuiltTemperatureLowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Low Warning Temperature from Inbuilt Temperature Sensor."

	::= { inbuiltTemperatureEntry 5 }



--

-- ExtendTemperature Table

--



	extendTemperatureTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF ExtendTemperatureEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Extend Temperature Sensor."

	::= { peripheralTables 6 }



	extendTemperatureEntry OBJECT-TYPE

		SYNTAX 			ExtendTemperatureEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Extend Temperature Sensor table."

		INDEX {	extendTemperatureIndex }

	::= { extendTemperatureTable 1 }



	ExtendTemperatureEntry ::= SEQUENCE {

		extendTemperatureIndex 				INTEGER,

		extendTemperatureDeviceId			INTEGER,

		extendTemperaturePort   			INTEGER,

		extendTemperatureMonitor			INTEGER,

		extendTemperatureStatus				INTEGER,

		extendTemperature							INTEGER,

		extendTemperatureHighWarning	INTEGER,

		extendTemperatureLowWarning		INTEGER

	}



	extendTemperatureIndex OBJECT-TYPE

		SYNTAX 			INTEGER (0..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Index for the Extend Temperature Sensor table."

	::= { extendTemperatureEntry 1 }



	extendTemperatureDeviceId OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend Temperature Monitor Status."

	::= { extendTemperatureEntry 2 }



	extendTemperaturePort OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend Temperature Monitor Status."

	::= { extendTemperatureEntry 3 }



	extendTemperatureMonitor OBJECT-TYPE

		SYNTAX 			INTEGER {

			no(0),

			yes(1)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend Temperature Monitor Status."

	::= { extendTemperatureEntry 4 }



	extendTemperatureStatus OBJECT-TYPE

		SYNTAX 			INTEGER {

			no(0),

			yes(1)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend Temperature Sensor Connect Status."

	::= { extendTemperatureEntry 5 }



	extendTemperature OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Detected Temperature from Inbuilt Temperature Sensor."

	::= { extendTemperatureEntry 6 }



	extendTemperatureHighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"High Warning Temperature from Extend Temperature Sensor."

	::= { extendTemperatureEntry 7 }



	extendTemperatureLowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Low Warning Temperature from Extend Temperature Sensor."

	::= { extendTemperatureEntry 8 }

	

--

-- extendRH Table

--



	extendRHTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF ExtendRHEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Extend RH Sensor."

	::= { peripheralTables 7 }



	extendRHEntry OBJECT-TYPE

		SYNTAX 			ExtendRHEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Extend RH table."

		INDEX {	extendRHIndex }

	::= { extendRHTable 1 }



	ExtendRHEntry ::= SEQUENCE {

		extendRHIndex 								INTEGER,

		extendRHDeviceId 							INTEGER,

		extendRHPort   								INTEGER,

		extendRHMonitor								INTEGER,

		extendRHStatus								INTEGER,

		extendRH										  INTEGER,

		extendRHHighWarning						INTEGER,

		extendRHLowWarning 						INTEGER

	}



	extendRHIndex OBJECT-TYPE

		SYNTAX 			INTEGER (0..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Index for the Extend RH Sensor table."

	::= { extendRHEntry 1 }



	extendRHDeviceId OBJECT-TYPE

		SYNTAX 			INTEGER (0..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Index for the Extend RH Sensor table."

	::= { extendRHEntry 2 }



	extendRHPort OBJECT-TYPE

		SYNTAX 			INTEGER (0..8)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Index for the Extend RH Sensor table."

	::= { extendRHEntry 3 }



	extendRHMonitor OBJECT-TYPE

		SYNTAX 			INTEGER {

			no(0),

			yes(1)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend RH Monitor Status."

	::= { extendRHEntry 4 }



	extendRHStatus OBJECT-TYPE

		SYNTAX 			INTEGER {

			no(0),

			yes(1)}

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Extend RH Sensor Connect Status."

	::= { extendRHEntry 5 }



	extendRH OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Detected RH from Inbuilt Temperature Sensor."

	::= { extendRHEntry 6 }



	extendRHHighWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"High Warning RH from Extend Temperature Sensor."

	::= { extendRHEntry 7 }



	extendRHLowWarning OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"Low Warning RH from Extend Temperature Sensor."

	::= { extendRHEntry 8 }

	

--

-- Input Table

--



	inputTable OBJECT-TYPE

		SYNTAX 			SEQUENCE OF InputEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"The table of Input."

	::= { peripheralTables 8 }



	inputEntry OBJECT-TYPE

		SYNTAX 			InputEntry

    MAX-ACCESS  not-accessible

		STATUS 			current

		DESCRIPTION

			"Row definition for Input table."

		INDEX {	inputIndex }

	::= { inputTable 1 }



	InputEntry ::= SEQUENCE {

		inputIndex   			INTEGER,

		inputStatus				INTEGER,

		inputState				INTEGER,

		inputTimeout			INTEGER,

		inputDefault			INTEGER,

		inputDetectTime		DisplayString

}



	inputIndex OBJECT-TYPE

		SYNTAX 			INTEGER (1)

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Index for Input table."

	::= { inputEntry 1 }



	inputStatus OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"This OID is provided for Input Status.

				'0'  NORMAL.

				'1'  WARNING.

				'2'  TIMEOUT.

			"

	::= { inputEntry 2 }



	inputState OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"This OID is provided for Input Default.

				'0'  NORMAL_CLOSE.

				'1'  NORMAL_OPEN.

			"

	::= { inputEntry 3 }

  

	inputTimeout OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"TimeOut of Input Status."

	::= { inputEntry 4 }

  

	inputDefault OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-write

		STATUS 			current

		DESCRIPTION

			"This OID is provided for Input Default.

				'0'  NORMAL_CLOSE.

				'1'  NORMAL_OPEN.

			"

	::= { inputEntry 5 }



	inputDetectTime OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Detect the nearest Changed Time of Input Status."

	::= { inputEntry 6 }



--

-- RFID reader

--



	rfidReader OBJECT IDENTIFIER 	::= { peripheralTables 9 }



	rfidCardNum OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"RFID Card Number."

	::= { rfidReader 1 }



	rfidDetectTime OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"The Nearest Time to detect RFID Card."

	::= { rfidReader 2 }



--

-- UPS

--



	uPS OBJECT IDENTIFIER 	::= { peripheralTables 10 }



	uPSModel OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Model."

	::= { uPS 1 }



	uPSConnectStatus OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Connect Status."

	::= { uPS 2 }



	uPSFirmware OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Firmware."

	::= { uPS 3 }



	uPSSerial OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Serial."

	::= { uPS 4 }



	uPSTemperature OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Temperature."

	::= { uPS 5 }



	uPSInputVoltage OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Input Voltage."

	::= { uPS 6 }



	uPSOutputOnBattery OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Output On Battery."

	::= { uPS 7 }



	uPSOutputVoltage OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Output Voltage."

	::= { uPS 8 }



	uPSOutputFrequency OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Output Voltage."

	::= { uPS 9 }



	uPSOutputCurrent OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Output Current."

	::= { uPS 10 }



	uPSOutputLoad OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Output Load."

	::= { uPS 11 }



	uPSOutputOverload OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Output Overload."

	::= { uPS 12 }



	uPSBatteryDate OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Battery Date."

	::= { uPS 13 }



	uPSBatteryVoltage OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Battery Voltage."

	::= { uPS 14 }



	uPSBatteryLevel OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Battery Level."

	::= { uPS 15 }



	uPSBatteryRunTime OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Battery RunTime."

	::= { uPS 16 }



	uPSBatteryLow OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Battery Low."

	::= { uPS 17 }



	uPSBatteryReplace OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS Battery Need Replace."

	::= { uPS 18 }



	uPSUARTId OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"UPS UART Id."

	::= { uPS 19 }



--

-- MIC Detect

--



	micDetec OBJECT IDENTIFIER 	::= { peripheralTables 11 }



	micDetectTimes OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"MIC Detect Times."

	::= { micDetec 1 }



	micDetectPeriod OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"MIC Detect Period."

	::= { micDetec 2 }



	micLastDetectTime OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"MIC Detect Detect Time."

	::= { micDetec 3 }



--

-- Vibration Detect

--



	vibrationDetec OBJECT IDENTIFIER 	::= { peripheralTables 12 }



	vibrationDetectTimes OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Vibration Detect Times."

	::= { vibrationDetec 1 }



	vibrationDetectPeriod OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Vibration Detect Period."

	::= { vibrationDetec 2 }



	vibrationLastDetectTime OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Vibration Detect Detect Time."

	::= { vibrationDetec 3 }



	dataLogTable  OBJECT IDENTIFIER 	::= { smart 4 }



--

-- Input Feed Data Table

--



	inFeedDataList OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Input Feed Data List."

	::= { dataLogTable 1 }

		

--

-- Outlet Table

--



	outDataList OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Outlet Data List."

	::= { dataLogTable 2 }



--

-- PDU Table

--



	pduDataList OBJECT-TYPE

		SYNTAX 			DisplayString

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"PDU Data List."

	::= { dataLogTable 3 }

	

--

--  Enterprise Traps

--

  smartTraps OBJECT IDENTIFIER ::= { smart 100 }



  trap OBJECT IDENTIFIER ::= { smartTraps 1 }

  -- the 0 is for V1 compatibility



  arg OBJECT IDENTIFIER ::= { smartTraps 2 }



	trapArg1 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg1."

	::= { arg 1 }



	trapArg2 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg2."

	::= { arg 2 }



	trapArg3 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg3."

	::= { arg 3 }



	trapArg4 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg4."

	::= { arg 4 }



	trapArg5 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg5."

	::= { arg 5 }



	trapArg6 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg6."

	::= { arg 6 }



	trapArg7 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg7."

	::= { arg 7 }



	trapArg8 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg8."

	::= { arg 8 }



	trapArg9 OBJECT-TYPE

		SYNTAX 			INTEGER

    MAX-ACCESS  read-only

		STATUS 			current

		DESCRIPTION

			"Indicate the Trap Arg9."

	::= { arg 9 }

		

	testTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1

    }

    STATUS      current

		DESCRIPTION

      "testData"

	::= { trap 1 }

		

  -- Input Feed Traps

	

	inFeedOverloadTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			inFeedIndex,

      inFeedStatus,

      inFeedCurrent,

      inFeedOverload

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 101 }



	inFeedHighCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			inFeedIndex,

      inFeedStatus,

      inFeedCurrent,

      inFeedHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 102 }



	inFeedLowCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			inFeedIndex,

      inFeedStatus,

      inFeedCurrent,

      inFeedHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 103 }



	inFeedBranchOverloadTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

			inFeedIndex,

			BranchIndex,

      inFeedStatus,

      inFeedCurrent,

      inFeedOverload

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 104 }

	

	inFeedBranchHighCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

			inFeedIndex,

			BranchIndex,

      inFeedStatus,

      inFeedCurrent,

      inFeedHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 105 }



	inFeedBranchLowCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

			inFeedIndex,

			BranchIndex,

      inFeedStatus,

      inFeedCurrent,

      inFeedHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 106 }

	

	outWebOperationTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3

    }

    STATUS      current

		DESCRIPTION

      "Outlet on/off change event.  If enabled, this trap is sent

       when the outStatus changes from any 'on' state ('on',

       'onWait', 'onError', or 'onFuse') to any 'off' state ('off',

       'offWait', 'offError', or 'offFuse'), and vice-versa."

		--#SUMMARY     "The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 201 }



	outPanelOperationTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3

    }

    STATUS      current

		DESCRIPTION

      "Outlet on/off change event.  If enabled, this trap is sent

       when the outStatus changes from any 'on' state ('on',

       'onWait', 'onError', or 'onFuse') to any 'off' state ('off',

       'offWait', 'offError', or 'offFuse'), and vice-versa."

		--#SUMMARY     "The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 202 }



	outAPIOperationTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3

    }

    STATUS      current

		DESCRIPTION

      "Outlet on/off change event.  If enabled, this trap is sent

       when the outStatus changes from any 'on' state ('on',

       'onWait', 'onError', or 'onFuse') to any 'off' state ('off',

       'offWait', 'offError', or 'offFuse'), and vice-versa."

		--#SUMMARY     "The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 203 }

	

	outScheduleTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

			trapArg5,

      trapArg6,

      trapArg7,

      trapArg8,

      trapArg9

    }

    STATUS      current

		DESCRIPTION

      "Outlet on/off change event.  If enabled, this trap is sent

       when the outStatus changes from any 'on' state ('on',

       'onWait', 'onError', or 'onFuse') to any 'off' state ('off',

       'offWait', 'offError', or 'offFuse'), and vice-versa."

		--#SUMMARY     "The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 211 }



	outScheduleErrorTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

			trapArg5,

      trapArg6,

      trapArg7

    }

    STATUS      current

		DESCRIPTION

      "Outlet on/off change event.  If enabled, this trap is sent

       when the outStatus changes from any 'on' state ('on',

       'onWait', 'onError', or 'onFuse') to any 'off' state ('off',

       'offWait', 'offError', or 'offFuse'), and vice-versa."

		--#SUMMARY     "The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 212 }



	outPingTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4

    }

    STATUS      current

		DESCRIPTION

      "Outlet on/off change event.  If enabled, this trap is sent

       when the outStatus changes from any 'on' state ('on',

       'onWait', 'onError', or 'onFuse') to any 'off' state ('off',

       'offWait', 'offError', or 'offFuse'), and vice-versa."

		--#SUMMARY     "The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 221 }



	outPingRebootTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4

    }

    STATUS      current

		DESCRIPTION

      "Outlet on/off change event.  If enabled, this trap is sent

       when the outStatus changes from any 'on' state ('on',

       'onWait', 'onError', or 'onFuse') to any 'off' state ('off',

       'offWait', 'offError', or 'offFuse'), and vice-versa."

		--#SUMMARY     "The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 222 }

	

	outOverloadTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      outIndex,

      outCurrentStatus,

      outCurrent,

      outHighWarning

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 231 }

	

	outHighCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      outIndex,

      outCurrentStatus,

      outCurrent,

      outHighWarning

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 232 }



	outLowCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      outIndex,

      outCurrentStatus,

      outCurrent,

      outLowWarning

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 233 }



	outConditionCtrlTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      outIndex,

      outCurrentStatus,

      outCurrent,

      outLowWarning

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 241 }



	outUPSACFaultOffTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

      trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      value

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 311 }



	outUPSBatteryLevelOffTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

      trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      value

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 312 }



	outUPSBatteryLowOffTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

      trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      value

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 313 }



	outUPSACRecoveryOnTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

      trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      value

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 314 }



	outUPSBatteryLevelOnTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

      trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      value

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 315 }



	outUPSBatteryLowRecoveryOnTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

      trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

      value

			Outlet load event.  If enabled, this trap is sent when the

       outLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the outLoadStatus

       remains in an error state.  If the outLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error outLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT 				evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 316 }

  

	pduConnectTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			PDUIndex,

      PDUConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 401 }



	pduOverloadTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			PDUIndex,

      PDUStatus,

      PDUCurrent,

      PDUOverload

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 402 }



	pduHighCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			PDUIndex,

      PDUStatus,

      PDUCurrent,

      PDUHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 403 }



	pduLowCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			PDUIndex,

      PDUStatus,

      PDUCurrent,

      PDUHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 404 }



	pduBranchOverloadTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

			PDUIndex,

			BranchIndex,

      PDUStatus,

      PDUCurrent,

      PDUOverload

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 405 }



	pduBranchHighCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

			PDUIndex,

			BranchIndex,

      PDUStatus,

      PDUCurrent,

      PDUHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 406 }



	pduBranchLowCurrentTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

			PDUIndex,

			BranchIndex,

      PDUStatus,

      PDUCurrent,

      PDUHighWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 407 }



	inbuiltTemperatureHighTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4

    }

    STATUS      current

		DESCRIPTION

      "

			InTempId,

			InTempStatus,

			InTempTemperature,

      InTempTemperatureWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 501 }



	inbuiltTemperatureLowTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4

    }

    STATUS      current

		DESCRIPTION

      "

			InTempId,

			InTempStatus,

			InTempTemperature,

      InTempTemperatureWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 502 }



	envConnectTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			ENVIndex,

      ENVConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 511 }



	envTemperatureConnectTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			ENVIndex,

      ENVConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 512 }

  

	envTemperatureHighTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5,

      trapArg6

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			EnvId,

			EnvStatus,

			EnvTemperature,

      EnvTemperatureWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 513 }



	envTemperatureLowTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5,

      trapArg6

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			EnvId,

			EnvStatus,

			EnvTemperature,

      EnvTemperatureWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 514 }



	envRHConnectTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			EnvId,

			EnvStatus,

			EnvRH,

      EnvRHWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 515 }



	envRHHighTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			EnvId,

			EnvStatus,

			EnvRH,

      EnvRHWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 516 }



	envRHLowTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4,

      trapArg5

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			EnvId,

			EnvStatus,

			EnvRH,

      EnvRHWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 517 }



	inputTimeOutTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			EnvId,

			EnvStatus,

			EnvTemperature,

      EnvTemperatureWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 601 }

	

	inputTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2,

      trapArg3,

      trapArg4

    }

    STATUS      current

		DESCRIPTION

      "

      deviceIndex,

			EnvId,

			EnvStatus,

			EnvTemperature,

      EnvTemperatureWarning

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 602 }

  

	upsConnectTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 701 }

  

	upsOnBatteryTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 702 }



	upsOverloadTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 703 }



	upsBatteryLowTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 704 }

  

	upsBatteryReplace NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 705 }

  

	daisyChainConnectTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 801 }



	micDetectOccurTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 901 }



	vibrationDetectOccurTrap NOTIFICATION-TYPE

		OBJECTS { 

      trapArg1,

			trapArg2

    }

    STATUS      current

		DESCRIPTION

      "

			Model,

      ConnectStatus

			Input feed load event.  If enabled, this trap is sent when

       the infeedLoadStatus indicates an error state ('loadLow',

       'loadHigh', 'overLoad', 'readError', or 'noComm').  This

       trap is repeated periodically while the infeedLoadStatus

       remains in an error state.  If the infeedLoadStatus returns

       to a non-error state ('normal' or 'notOn'), this trap is

       sent once more with the non-error infeedLoadStatus, and then

       stops being repeated."

		--#SUMMARY     	"The appliance is rebooting. Command issued by user: %s."

		--#ARGUMENTS   	{ 0 }

		--#SEVERITY    	INFORMATIONAL

		--#CATEGORY    	"Status Events"

		--NAME      		"Appliance Rebooting"

		--SHORT     		"appliance rebooting"

		--EVENT evt_reboot

		--% TrapTypeEnum=15 

	::= { trap 902 }

  

END

