ALCATEL-IND1-RIP-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, IpAddress, TimeTicks, Integer32
            FROM SNMPv2-SMI
        rip2IfConfEntry
            FROM RIPv2-MIB
        RowStatus, TEXTUAL-CONVENTION
            FROM SNMPv2-TC
        SnmpAdminString
            FROM SNMP-FRAMEWORK-MIB
        MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
            FROM SNMPv2-CONF
        routingIND1Rip
            FROM ALCATEL-IND1-BASE;


    alcatelIND1RIPMIB MODULE-IDENTITY
        LAST-UPDATED "201010260000Z"
        ORGANIZATION "Alcatel-Lucent"
        CONTACT-INFO
                " Please consult with Customer Service to ensure the most appropriate
                  version of this document is used with the products in question:

                            Alcatel-Lucent, Enterprise Solutions Division
                           (Formerly Alcatel Internetworking, Incorporated)
                                   26801 West Agoura Road
                                Agoura Hills, CA  91301-5122
                                  United States Of America

                Telephone:               North America  +1 800 995 2696
                                         Latin America  +1 877 919 9526
                                         Europe         +31 23 556 0100
                                         Asia           +65 394 7933
                                         All Other      +1 818 878 4507

                Electronic Mail:         support@ind.alcatel.com
                World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
                File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

        DESCRIPTION
                "This module describes an authoritative enterprise-specific Simple
                 Network Management Protocol (SNMP) Management Information Base (MIB):

                     For the Birds Of Prey Product Line
                     Configuration Of Global RIP Configuration Parameters.

                 The right to make changes in specification and other information
                 contained in this document without prior notice is reserved.

                 No liability shall be assumed for any incidental, indirect, special, or
                 consequential damages whatsoever arising from or related to this
                 document or the information contained herein.

                 Vendors, end-users, and other interested parties are granted
                 non-exclusive license to use this specification in connection with
                 management of the products for which it is intended to be used.

                             Copyright (C) 1995-2007 Alcatel-Lucent
                                 ALL RIGHTS RESERVED WORLDWIDE"

        REVISION         "200704030000Z"
        DESCRIPTION
            "The latest version of this MIB Module."

        ::= { routingIND1Rip 1 }

    alcatelIND1RIPMIBObjects OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch for Routing Information Protocol (RIP)
             Subsystem Managed Objects."
        ::= { alcatelIND1RIPMIB 1 }


    alcatelIND1RIPMIBConformance OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch for Routing Information Protocol (RIP)
             Subsystem Conformance Information."
        ::= { alcatelIND1RIPMIB 2 }


    alcatelIND1RIPMIBGroups OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch for Routing Information Protocol (RIP)
             Subsystem Units Of Conformance."
        ::= { alcatelIND1RIPMIBConformance 1 }


    alcatelIND1RIPMIBCompliances OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch for Routing Information Protocol (RIP)
             Subsystem Compliance Statements."
        ::= { alcatelIND1RIPMIBConformance 2 }


--********************************************************************
--************************ Textual Conventions ***********************
--********************************************************************
        AlaAuthenticationEncryptKey ::= TEXTUAL-CONVENTION
                STATUS         current
                DESCRIPTION
                        "The authentication encryption key that is used to decypher
                        RIP simple passwords."
                SYNTAX  OCTET STRING (SIZE(16))



-- ************************************************************************
--  RIP Global Protocol configuration
-- ************************************************************************

    alaProtocolRip      OBJECT IDENTIFIER ::= { alcatelIND1RIPMIBObjects 1 }

    alaRipProtoStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                        enable(1),
                        disable(2)
                    }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "Global administration status of RIP."
        DEFVAL { disable }
        ::= { alaProtocolRip 1 }

    alaRipHostRouteSupport OBJECT-TYPE
        SYNTAX  INTEGER {
                            enable(1),
                            disable(2)
                        }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "Enable or disable support for host routes."
        DEFVAL { enable }
        ::= { alaProtocolRip 2 }

    alaRipRedistRouteTag OBJECT-TYPE
        SYNTAX  Integer32 ( 0 .. 2147483647 )
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "A 32-bit value tagged to each RIP internal route while
        it is redistributed in to other routing protocol domains. The
        lower 16-bits typically indicate the autonomous system number."
        DEFVAL { 0 }
    ::= { alaProtocolRip 4 }

    alaRipForceHolddownTimer OBJECT-TYPE
        SYNTAX Integer32 ( 0 .. 120 )
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Interval in seconds during which routing information regarding
        better paths is suppressed. A route enters into a forced holddown
        state when an update packet is received that indicates the route is
        unreachable and when this timer value is nonzero. After this timer
        has expired, if the value is less that 120 - the route enters a
        holddown state for the rest of the period until 120. During this time
        advertisements for better paths are accepted if any."
        ::= { alaProtocolRip 5 }

    alaRipRouteNumber OBJECT-TYPE
        SYNTAX  Integer32 ( 0 .. 2147483647 )
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
            "The number of network routes in RIP routing table."
        ::= { alaProtocolRip 6 }

    alaRipUpdateInterval OBJECT-TYPE
        SYNTAX  Integer32 (1 .. 120)
        UNITS "seconds"
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "Interval (in seconds) that RIP routing updates will
            be sent out.  The value must be less than or equal to
            one-third the value of the invalid timer."
        DEFVAL { 30 }
    ::= { alaProtocolRip 13 }

    alaRipInvalidTimer OBJECT-TYPE
        SYNTAX  Integer32 (3 .. 360)
        UNITS "seconds"
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "Time in seconds that a route will remain active
            in RIB before being moved to the invalid state.
            The value must be at least three times the
            update interval."
        DEFVAL { 180 }
    ::= { alaProtocolRip 14 }

    alaRipHolddownTimer OBJECT-TYPE
        SYNTAX  Integer32 (0 .. 120)
        UNITS "seconds"
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "Time to keep a route in the holddown state."
        DEFVAL { 0 }
    ::= { alaProtocolRip 15 }

    alaRipGarbageTimer OBJECT-TYPE
        SYNTAX Integer32 (0 .. 180)
        UNITS "seconds"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Time to keep a route before garbage collection."
        DEFVAL { 120 }
    ::= { alaProtocolRip 16 }


-- ************************************************************************
-- Expansion of rip2IfCOnf
-- ************************************************************************
        alaRip2IfConfAugTable OBJECT-TYPE
                SYNTAX SEQUENCE OF AlaRip2IfConfAugEntry
                MAX-ACCESS not-accessible
                STATUS current
                DESCRIPTION
                        "Expansion for rip2ifconftable"
        ::= { alaProtocolRip 11 }

        alaRip2IfConfAugEntry OBJECT-TYPE
        SYNTAX   AlaRip2IfConfAugEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
            "An entry of alaRip2IfConfAugTable"
        AUGMENTS { rip2IfConfEntry }
        ::= { alaRip2IfConfAugTable 1 }

    AlaRip2IfConfAugEntry ::=
        SEQUENCE {
                alaRip2IfConfEncryptKey AlaAuthenticationEncryptKey,
                alaRip2IfIpConfStatus   INTEGER,
                alaRip2IfRecvPkts       Integer32,
                alaRip2IfConfName       SnmpAdminString,
                alaRip2IfConfType       INTEGER,
            alaRip2IfConfPtoPPeer            IpAddress,
            alaRip2IfConfIngressFilterRouteMapName SnmpAdminString,
            alaRip2IfConfEgressFilterRouteMapName  SnmpAdminString
        }

    alaRip2IfConfEncryptKey OBJECT-TYPE
        SYNTAX          AlaAuthenticationEncryptKey
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                        "The authentication encryption key that is used to decypher
                        RIP passwords."
       ::= { alaRip2IfConfAugEntry 1 }

    alaRip2IfIpConfStatus OBJECT-TYPE
        SYNTAX          INTEGER { enable(1), disable(2), none(3) }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                        "The status of the associated IP interface"
       ::= { alaRip2IfConfAugEntry 2 }

    alaRip2IfRecvPkts OBJECT-TYPE
        SYNTAX          Integer32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                        "Number of packets received on this interface"
       ::= { alaRip2IfConfAugEntry 3 }

    alaRip2IfConfName OBJECT-TYPE
        SYNTAX          SnmpAdminString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The user defined name used to identify the IP interface"
       ::= { alaRip2IfConfAugEntry 4 }

    alaRip2IfConfType OBJECT-TYPE
        SYNTAX          INTEGER
                        { broadcast (1), point2point(2) }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
            "The type of the rip interface"
       ::= { alaRip2IfConfAugEntry 5 }

    alaRip2IfConfPtoPPeer OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
            "The address of the peer for a point-to-point rip interface"
       ::= { alaRip2IfConfAugEntry 6 }

    alaRip2IfConfIngressFilterRouteMapName OBJECT-TYPE

        SYNTAX          SnmpAdminString (SIZE (0..20))
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
            "The name of a Route Map to be applied when filtering
             RIP routing updates received on this RIP interface. RIP
             routes that are explicitly denied by a Route Map are
             filtered. An empty string indicates that no filtering
             action is performed (this is the default). If the Route
             Map is specified and a RIP route doesn't match any Route
             Map route or if there is a match that is permitted, the
             RIP route is not filtered.
             Route Map manipulators (SET commands configured for
             a Route Map) are not applied when filtering is performed.
             (cf. alaRouteMapNameTable.AlaRouteMapNameEntry.alaRouteMapName)"
        DEFVAL { ''H }    -- the empty string
       ::= { alaRip2IfConfAugEntry 7 }

    alaRip2IfConfEgressFilterRouteMapName OBJECT-TYPE

        SYNTAX          SnmpAdminString (SIZE (0..20))
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
            "The name of a Route Map to be applied when filtering
             RIP routing updates sent out this RIP interface. RIP
             routes that are explicitly denied by a Route Map are
             filtered. An empty string indicates that no filtering
             action is performed (this is the default). If the Route
             Map is specified and a RIP route doesn't match any Route
             Map route or if there is a match that is permitted, the
             RIP route is not filtered.
             Route Map manipulators (SET commands configured for
             a Route Map) are not applied when filtering is performed.
             (cf. alaRouteMapNameTable.AlaRouteMapNameEntry.alaRouteMapName)"
        DEFVAL { ''H }    -- the empty string
       ::= { alaRip2IfConfAugEntry 8 }

-- ************************************************************************
-- ************************************************************************

     alaRipEcmpRouteTable OBJECT-TYPE
         SYNTAX    SEQUENCE OF AlaRipEcmpRouteEntry
         MAX-ACCESS    not-accessible
         STATUS    current
         DESCRIPTION
             "ECMP-enabled RIP routing table which contains the network routes."
         ::= { alaProtocolRip 12 }

     alaRipEcmpRouteEntry OBJECT-TYPE
         SYNTAX   AlaRipEcmpRouteEntry
         MAX-ACCESS   not-accessible
         STATUS   current
         DESCRIPTION
             "ECMP-enabled RIP routing table which contains the network routes."
         INDEX {
                 alaRipEcmpRouteDest,
                 alaRipEcmpRouteMask,
                 alaRipEcmpRouteNextHop
               }
         ::= { alaRipEcmpRouteTable 1 }

     AlaRipEcmpRouteEntry ::=
         SEQUENCE {
             alaRipEcmpRouteDest
                 IpAddress,
             alaRipEcmpRouteMask
                 IpAddress,
             alaRipEcmpRouteNextHop
                 IpAddress,
             alaRipEcmpRouteType
                 INTEGER,
             alaRipEcmpRouteAge
                 TimeTicks,
             alaRipEcmpRouteTag
                 Integer32,
             alaRipEcmpRouteMetric
                 Integer32,
             alaRipEcmpRouteStatus
                 RowStatus,
             alaRipEcmpRouteState
                 INTEGER
         }

     alaRipEcmpRouteDest OBJECT-TYPE
         SYNTAX   IpAddress
         MAX-ACCESS   not-accessible
         STATUS   current
         DESCRIPTION
            "The destination IP address of this route."
         ::= { alaRipEcmpRouteEntry 1 }

     alaRipEcmpRouteMask OBJECT-TYPE
         SYNTAX   IpAddress
         MAX-ACCESS   not-accessible
         STATUS   current
         DESCRIPTION
            "The network mask for this route."
         ::= { alaRipEcmpRouteEntry 2 }

     alaRipEcmpRouteNextHop OBJECT-TYPE
         SYNTAX   IpAddress
         MAX-ACCESS   not-accessible
         STATUS   current
         DESCRIPTION
            "The address of the next hop to reach this route."
         ::= { alaRipEcmpRouteEntry 3 }

     alaRipEcmpRouteType OBJECT-TYPE
         SYNTAX   INTEGER
                  {
                     local  (1), -- local route
                     remote (2), -- remote route
                     redistribute (3)  -- redistributed route
                  }
         MAX-ACCESS   read-only
         STATUS   current
         DESCRIPTION
            "The type of route."
         ::= { alaRipEcmpRouteEntry 4 }

     alaRipEcmpRouteAge OBJECT-TYPE
         SYNTAX   TimeTicks
         MAX-ACCESS   read-only
         STATUS   current
         DESCRIPTION
            "The number of seconds since this route  was last
            updated or otherwise determined to be correct."
         ::= { alaRipEcmpRouteEntry 5 }

     alaRipEcmpRouteTag OBJECT-TYPE
         SYNTAX   Integer32 ( 0 .. 2147483647 )
         MAX-ACCESS   read-only
         STATUS   current
         DESCRIPTION
            "The associated route tag."
         DEFVAL { 0 }
         ::= { alaRipEcmpRouteEntry 6 }

     alaRipEcmpRouteMetric OBJECT-TYPE
         SYNTAX   Integer32 ( 0 .. 15 )
         MAX-ACCESS   read-only
         STATUS   current
         DESCRIPTION
            "The routing  metric  for  this  route."
         ::= { alaRipEcmpRouteEntry 7 }

     alaRipEcmpRouteStatus OBJECT-TYPE
         SYNTAX   RowStatus
         MAX-ACCESS read-only
         STATUS    current
         DESCRIPTION
            "The row status variable, used according to
            row installation and removal conventions."
         ::= { alaRipEcmpRouteEntry 8 }

     alaRipEcmpRouteState OBJECT-TYPE
         SYNTAX   INTEGER
                  {
                     active   (1),
                     garbage  (2),
                     holddown (3),
                     unknown  (4)
                  }
         MAX-ACCESS   read-only
         STATUS   current
         DESCRIPTION
            "The associated state for this route."
         ::= { alaRipEcmpRouteEntry 9 }


-- ************************************************************************
-- ************************************************************************

--
-- Compliance Statements
--

     alcatelIND1RIPMIBCompliance MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION
            "Compliance statement for
             Routing Information Protocol (RIP) Subsystem."
        MODULE -- this module

            MANDATORY-GROUPS
            {
               alaRipMiscellaneousGroup,
               alaRipEcmpRouteGroup
            }

        ::= { alcatelIND1RIPMIBCompliances 1 }


--
-- Units of Conformance
--

     alaRipMiscellaneousGroup OBJECT-GROUP
        OBJECTS
        {
           alaRipRedistRouteTag,
           alaRipForceHolddownTimer,
           alaRipRouteNumber
        }
        STATUS current
        DESCRIPTION
            "Collection of Miscellaneous objects for management of RIP."
        ::= { alcatelIND1RIPMIBGroups 1 }

     alaRip2IfConfAugGroup OBJECT-GROUP
        OBJECTS
        {
            alaRip2IfConfEncryptKey ,
            alaRip2IfIpConfStatus   ,
            alaRip2IfRecvPkts       ,
            alaRip2IfConfName       ,
            alaRip2IfConfType       ,
            alaRip2IfConfPtoPPeer            ,
            alaRip2IfConfIngressFilterRouteMapName ,
            alaRip2IfConfEgressFilterRouteMapName
        }
        STATUS current
        DESCRIPTION
            "Collection of RIP2 Interface objects."
        ::= { alcatelIND1RIPMIBGroups 2 }


     alaProtocolRipGroup OBJECT-GROUP
        OBJECTS
        {
            alaRipProtoStatus ,
            alaRipHostRouteSupport ,
            alaRipRedistRouteTag ,
            alaRipForceHolddownTimer ,
            alaRipRouteNumber ,
            alaRipUpdateInterval ,
            alaRipInvalidTimer ,
            alaRipHolddownTimer ,
            alaRipGarbageTimer

        }
        STATUS current
        DESCRIPTION
            "Collection of RIP Protocol objects."
        ::= { alcatelIND1RIPMIBGroups 3 }

     alaRipEcmpRouteGroup OBJECT-GROUP
        OBJECTS
        {
           alaRipRouteNumber,
           alaRipEcmpRouteType,
           alaRipEcmpRouteAge,
           alaRipEcmpRouteTag,
           alaRipEcmpRouteMetric,
           alaRipEcmpRouteStatus,
           alaRipEcmpRouteState
        }
        STATUS current
        DESCRIPTION
            "Collection of objects for management of Network Route configuration."
        ::= { alcatelIND1RIPMIBGroups 6 }


--
-- Trap definitions
--

alcatelIND1RIPTraps                OBJECT IDENTIFIER ::= { alcatelIND1RIPMIB 3}
alcatelIND1RIPTrapsRoot            OBJECT IDENTIFIER ::= { alcatelIND1RIPTraps 0}

ripRouteMaxLimitReached NOTIFICATION-TYPE
     STATUS             current
     DESCRIPTION
           " This notification is generated as RIP database reached supported
             Maximum entries. RIP will discard any new updates."
::= {alcatelIND1RIPTrapsRoot 1}

alcatelIND1RIPTrapsGroup NOTIFICATION-GROUP
        NOTIFICATIONS {
            ripRouteMaxLimitReached
        }
        STATUS  current
        DESCRIPTION
            "Collection of RIP Trap Objects."
        ::= { alcatelIND1RIPMIBGroups 7 }



END

