LINKSYS-DHCPv6 DEFINITIONS ::= BEGIN

-- Version:    7.60

-- Date:       10-May-2012

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Unsigned32, IpAddress, Counter32                FROM SNMPv2-SMI
    InterfaceIndex, ifIndex                         FROM IF-MIB
    RowStatus, TEXTUAL-CONVENTION, MacAddress,
    DisplayString, TruthValue                       FROM SNMPv2-TC
    InetAddressType,InetAddress,InetAddressIPv6     FROM INET-ADDRESS-MIB -- RFC2851
    rnd                                             FROM LINKSYS-MIB;

rlDhcpv6 MODULE-IDENTITY
        LAST-UPDATED "200604020000Z"
        ORGANIZATION ""
        CONTACT-INFO ""
        DESCRIPTION
                "The private MIB module definition for DHCP v6 features."
        ::= { rnd  214}

rlDhcpv6Common OBJECT IDENTIFIER ::= { rlDhcpv6 1}

rlDhcpv6Client OBJECT IDENTIFIER ::= { rlDhcpv6 2}

rlDhcpv6Relay OBJECT IDENTIFIER ::= { rlDhcpv6 3}

------------------------------
-- DHCP DUID
------------------------------

-- rlDhcpv6DuidEn --

rlDhcpv6DuidEn OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(7..38))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION ""
    ::= { rlDhcpv6Common 1 }

END
