LINKSYS-LLDP-MIB DEFINITIONS ::= BEGIN

-- Title:                LINKSYS LLDP ROS
--                       Private LLDP MIB
-- Version:              7.42
-- Date:                 12 Dec 2005

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Gauge32, Unsigned32,
    NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue, RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    rnd, rndNotifications
        FROM LINKSYS-MIB
    LldpPortList, LldpPortNumber, LldpManAddress
        FROM LLDP-MIB
    PortList
        FROM Q-BRIDGE-MIB
    Dscp
        FROM DIFFSERV-DSCP-TC
    AddressFamilyNumbers
        FROM IANA-ADDRESS-FAMILY-NUMBERS-MIB
    lldpRemTimeMark, lldpRemLocalPortNum, lldpRemIndex
        FROM LLDP-MIB
    LldpXMedCapabilities
        FROM LLDP-EXT-MED-MIB
    rndErrorDesc, rndErrorSeverity
        FROM LINKSYS-DEVICEPARAMS-MIB;


rlLldp MODULE-IDENTITY
         LAST-UPDATED "200506200000Z"
         ORGANIZATION "Linksys LLC."
         CONTACT-INFO
                "www.linksys.com/business/support"
         DESCRIPTION
                "This private MIB module adds MIBs to LLDP (Link Layer Discovery Protocol)."
         REVISION "200506200000Z"
         DESCRIPTION
                "Initial revision."
        ::= { rnd 110 }

rlLldpObjects          OBJECT IDENTIFIER ::= { rlLldp 1 }

rlLldpConfig           OBJECT IDENTIFIER ::= { rlLldpObjects 1 }
rlLldpXMedConfig       OBJECT IDENTIFIER ::= { rlLldpObjects 2 }

PolicyNumber ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS     current
    DESCRIPTION
            "Policy Number in the Media Policy Container.

            Policy numbers should be in the range of 1 and 32768 since 8 policies
            can be configured for each particular port and the number of ports range is
            1 to 4096."
    SYNTAX         Integer32(1..32768)

-- Policy Application Type Textual Convention

PolicyContainerAppType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            "The media type that defines the primary function of the
             application for the policy advertised by an endpoint.

             A value of voice(1) indicates that the media type defining
             a primary function of the application for the policy advertised on
             the local port is voice.

             A value of voiceSignaling(3) indicates that the media type
             defining a primary function of the application for the policy
             advertised on the local port is voice signaling.

             A value of guestVoice(4) indicates that the media type
             Defining a primary function of the application for the policy
             advertised on the local port is guest voice.

             A value of guestVoiceSignaling(5) indicates that the media
             type defining a primary function of the application for the policy
             advertised on the local port is guest voice signaling.

             A value of softPhoneVoice(6) indicates that the media type
             Defining a primary function of the application for the policy
             advertised on the local port is softphone voice.

             A value of videoConferencing(7) indicates that the media
             type defining a primary function of the application for the policy
             advertised on the local port is voice.

             A value of streamingVideo(8) indicates that the media type
             defining a primary function of the application for the policy
             advertised on  the local port is streaming video.

             A value of videoSignaling(2) indicates that the media type
             defining a primary function of the application for the policy
             advertised on the local port is video signaling."
    SYNTAX      INTEGER  {
                    unknown(0),
                    voice(1),
                    voiceSignaling(2),
                    guestVoice(3),
                    guestVoiceSignaling(4),
                    softPhoneVoice(5),
                    videoconferencing(6),
                    streamingVideo(7),
                    videoSignaling(8)
                }


PolicyAppVoiceUpdateMode ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION ""
    SYNTAX      INTEGER  {
                    manual(0),
                    auto(1)
                }

rlLldpEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Setting this variable to 'true' will globally enable the LLDP feature
             (both transmit and receive functionalities). Setting this variable
             to 'false' will globally disable the LLDP feature. Thus, the
             administratively desired status of a local port is determined by
             both this variable and the MIB lldpPortConfigAdminStatus."
    ::= { rlLldpConfig 1 }

rlLldpClearRx OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "A set of ports that are identified by a PortList, in which
            each port is represented as a bit.
            Clears the Rx information about the remote agents accordingly to the
            specified PortList.
            The default value for rlLldpClearRx object is an empty binary string,
            which means no ports are specified to be cleared from the Rx Info.
            This object behaviors as an event (write-only) than
            reading this object always results in an Empty Port List of length zero."
    REFERENCE
            ""
    DEFVAL  { ''H } -- empty octet string
    ::= { rlLldpConfig 2 }

rlLldpDuMode OBJECT-TYPE
    SYNTAX      INTEGER {
                    filtering(1),
                    flooding(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Action with LLDPDU upon globally disabled LLDP.

            If the associated rlLldpDuMode object has a value of
            'filtering(1)', then received frames are containing LLDPDU
            will be dropped.

            If the associated rlLldpDuMode object has a value of
            'flooding(2)', then received frames are containing LLDPDU
            will flood all active ports."
    REFERENCE
            "Linksys LLDP System Specifications"
    DEFVAL  { filtering }
    ::= { rlLldpConfig 3 }

rlLldpAutoAdvLocPortManAddrTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlLldpAutoAdvLocPortManAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains automaticaly selected management address,
            advertised on the local port."
    REFERENCE
            "Linksys LLDP"
    ::= { rlLldpConfig 4 }

rlLldpAutoAdvLocPortManAddrEntry OBJECT-TYPE
    SYNTAX      RlLldpAutoAdvLocPortManAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about a local port, which advertises the Management
            address automatically. Entry also included an interface number, on
            which the Management address is assigned.
            Each management address should have distinct 'management address
            type' (rlLldpAutoAdvManAddrSubtype) and 'management address'
            (rlLldpAutoAdvManAddr)."

    INDEX   { rlLldpAutoAdvLocPortNum }
    ::= { rlLldpAutoAdvLocPortManAddrTable 1 }

RlLldpAutoAdvLocPortManAddrEntry ::= SEQUENCE {
      rlLldpAutoAdvLocPortNum           LldpPortNumber,
      rlLldpAutoAdvManAddrOwnerIfId     Integer32,
      rlLldpAutoAdvManAddrNone          TruthValue,
      rlLldpAutoAdvManAddrSubtype       AddressFamilyNumbers,
      rlLldpAutoAdvManAddr              LldpManAddress,
      rlLldpAutoAdvPortsStatus          RowStatus
}

rlLldpAutoAdvLocPortNum   OBJECT-TYPE
    SYNTAX      LldpPortNumber
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The index value used to identify the port component
            (contained in the local chassis with the LLDP agent)
            associated with this entry.

            The value of this object is used as a port index to the
            rlLldpAutoAdvLocPortManAddrTable."
    ::= { rlLldpAutoAdvLocPortManAddrEntry 1 }

rlLldpAutoAdvManAddrOwnerIfId  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The integer value is used to identify the interface number
            (port, trunk or vlan). The management address, automatically
            advertised from associated 'rlLldpAutoAdvLocPortNum'local port is
            assigned to mentioned 'rlLldpAutoAdvManAddrOwnerIfId' interface.
            In case of 0 the management address is automatically calculated
            without care to the ifIndex it was defined on."
    DEFVAL  { 0 }
    ::= { rlLldpAutoAdvLocPortManAddrEntry 2 }

rlLldpAutoAdvManAddrNone  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "A value of 'true' indicates that the any management address hasn't advertised
             by the local port. Moreover, the configuration of automatic management address
             advertisment is disabled.
             A value of 'false' indicates that the configuration of automatic management address
             advertisment is enabled."
    DEFVAL { false }
    ::= { rlLldpAutoAdvLocPortManAddrEntry 3 }

rlLldpAutoAdvManAddrSubtype  OBJECT-TYPE
    SYNTAX      AddressFamilyNumbers
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The type of management address identifier encoding used in
            the associated 'rlLldpAutoAdvManAddr' object."
    ::= { rlLldpAutoAdvLocPortManAddrEntry 4 }

rlLldpAutoAdvManAddr  OBJECT-TYPE
    SYNTAX      LldpManAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The string value used to identify the management address is
            automaticaly advertised by local port, and assigned on the
            associated 'rlLldpAutoAdvManAddrOwnerIfId' interface."
    ::= { rlLldpAutoAdvLocPortManAddrEntry 5 }

rlLldpAutoAdvPortsStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlLldpAutoAdvLocPortManAddrEntry 6 }

--rlLldpLocChassisId  OBJECT-TYPE
--    SYNTAX      OCTET STRING(SIZE(1..20))
--    MAX-ACCESS  read-write
--    STATUS      current
--    DESCRIPTION
--            "The string value used to identify the chassis component associated
--             with the local system. As a result of updating this variable,
--             lldpLocChassisid will have the same value, and the MIB
--             lldpLocChassisIdSubtype will have the value local(7). "
--    ::= { rlLldp 2}



------------------------------------------------------------------------------
-- LLDP-MED - Local Device Configuration
------------------------------------------------------------------------------
---
--- rlLldpXMedLocMediaPolicyContainerTable: Local Media Policy Container
---                                         Configuration Table
---
---
rlLldpXMedLocMediaPolicyContainerTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlLldpXMedLocMediaPolicyContainerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one row per policy number
             of media policy container configuration."
    ::= { rlLldpXMedConfig 1 }

rlLldpXMedLocMediaPolicyContainerEntry OBJECT-TYPE
    SYNTAX      RlLldpXMedLocMediaPolicyContainerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Configuration of a particular policy in the media policy container."
    INDEX   { rlLldpXMedLocMediaPolicyContainerIndex }
    ::= { rlLldpXMedLocMediaPolicyContainerTable 1 }

RlLldpXMedLocMediaPolicyContainerEntry ::= SEQUENCE {
              rlLldpXMedLocMediaPolicyContainerIndex          PolicyNumber,
              rlLldpXMedLocMediaPolicyContainerAppType        PolicyContainerAppType,
              rlLldpXMedLocMediaPolicyContainerVlanID         Integer32,
              rlLldpXMedLocMediaPolicyContainerPriority       Integer32,
              rlLldpXMedLocMediaPolicyContainerDscp           Dscp,
              rlLldpXMedLocMediaPolicyContainerUnknown        TruthValue,
              rlLldpXMedLocMediaPolicyContainerTagged         TruthValue,
              rlLldpXMedLocMediaPolicyContainerPorts          PortList,
              rlLldpXMedLocMediaPolicyContainerRowStatus      RowStatus
}

rlLldpXMedLocMediaPolicyContainerIndex  OBJECT-TYPE
    SYNTAX      PolicyNumber
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The index value used to identify the Media Policy
            associated with this entry.
            The value of this object is used as a policy number index to the
            rlLldpXMedLocMediaPolicyContainerTable."
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 1 }

rlLldpXMedLocMediaPolicyContainerAppType OBJECT-TYPE
    SYNTAX      PolicyContainerAppType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The media type that defines the primary function of the
             application for the policy advertised by an endpoint."
    REFERENCE
            "ANSI/TIA-1057, Section 10.2.3.1"
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 2 }

rlLldpXMedLocMediaPolicyContainerVlanID  OBJECT-TYPE
    SYNTAX      Integer32 (0|1..4094|4095)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "An extension of the VLAN Identifier for the port,
             as defined in IEEE 802.1P-1998.

             A value of 1 through 4094 is used to define a valid PVID.

             A value of 0 shall be used if the device is using priority tagged
             frames, meaning that only the 802.1p priority level is significant
             and the default VID of the ingress port is being used instead.

             A value of 4095 is reserved for implementation use."
    REFERENCE
            " ANSI/TIA-1057, Section 10.2.3.5"
    DEFVAL  { 0 }
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 3 }

rlLldpXMedLocMediaPolicyContainerPriority  OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "This object contains the value of the 802.1p priority
            which is associated with the given port on the
            local system."
    REFERENCE
            " ANSI/TIA-1057, Section 10.2.3.6 "
    DEFVAL  { 0 }
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 4 }

rlLldpXMedLocMediaPolicyContainerDscp  OBJECT-TYPE
    SYNTAX             Dscp
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "This object contains the value of the Differentiated Service
            Code Point (DSCP) as defined in IETF RFC 2474 and RFC 2475
            which is associated with the given port on the local system."
    REFERENCE
            " ANSI/TIA-1057, Section 10.2.3.7"
    DEFVAL  { 0 }
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 5 }

rlLldpXMedLocMediaPolicyContainerUnknown  OBJECT-TYPE
    SYNTAX             TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "A value of 'true' indicates that the
             network policy for the specified application type is
             currently unknown.  In this case, the VLAN ID, the
             layer 2 priority and the DSCP value fields are ignored.
             A value of 'false' indicates that this network policy
             is defined  "
    REFERENCE
            " ANSI/TIA-1057, Section 10.2.3.2"
    DEFVAL { false }
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 6 }

rlLldpXMedLocMediaPolicyContainerTagged  OBJECT-TYPE
    SYNTAX             TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "A value of 'true' indicates that the application is using a
             tagged VLAN.
             A value of 'false' indicates that for the specific application
             the device either is using an untagged VLAN or does not
             support port based VLAN operation.  In this case, both the
             VLAN ID and the Layer 2 priority fields are ignored and
             only the DSCP value has relevance "
    REFERENCE
            " ANSI/TIA-1057, Section 10.2.3.3"
    DEFVAL { false }
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 7 }

rlLldpXMedLocMediaPolicyContainerPorts  OBJECT-TYPE
    SYNTAX        PortList
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
            "A set of ports that are identified by a PortList, in which
            each port is represented as a bit.  The local Media Policy Number
            will be associated with (or attached to) the ports specified at
            the rlLldpXMedLocMediaPolicyContainerPorts.

            The default value for rlLldpXMedLocMediaPolicyContainerPorts object
            is empty binary string, which means no ports are specified
            for advertising indicated management address instance."
    REFERENCE
            "IEEE 802.1AB-2004 10.2.1.1"
    DEFVAL  { ''H }     -- empty binary string
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 8 }

rlLldpXMedLocMediaPolicyContainerRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlLldpXMedLocMediaPolicyContainerEntry 9 }

------------------------------------------------------------------------------
-- LLDP - TX TLV overloading
------------------------------------------------------------------------------


rlLldpTLVsTxOverloadingTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlLldpTLVsTxOverloadingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A table that show the which of the LLDP TLVs are not transmitted
            on individual ports due to insufficient room in the frame
            and the size of each TLV."
    ::= {  rlLldpObjects 3 }


rlLldpTLVsTxOverloadingEntry  OBJECT-TYPE
    SYNTAX      RlLldpTLVsTxOverloadingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP TX overloading information that shows the
            transmission of TLVs on LLDP transmission capable ports."
   INDEX  { rlLldpTxOverloadingPortNum,
            rlLldpTxOverloadingIndex }
    ::= { rlLldpTLVsTxOverloadingTable 1 }

RlLldpTLVsTxOverloadingEntry ::= SEQUENCE {
    rlLldpTxOverloadingPortNum                  LldpPortNumber,
    rlLldpTxOverloadingIndex                    Unsigned32,
    rlLldpTxOverloadingGroupId                  INTEGER,
    rlLldpTLVsTxSize                            Unsigned32,
    rlLldpTLVsTxGroupOverloading                TruthValue,
    rlLldpTLVsTxLeftSize                        Unsigned32
}

rlLldpTxOverloadingPortNum   OBJECT-TYPE
    SYNTAX      LldpPortNumber
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            " The value of this object is used as a port index to the
              TLVs TX overloading Table ."
    ::= { rlLldpTLVsTxOverloadingEntry 1 }

rlLldpTxOverloadingIndex   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The sequence number of the group into sent LLDP PPDU starting from 1."
    ::= { rlLldpTLVsTxOverloadingEntry 2 }

rlLldpTxOverloadingGroupId OBJECT-TYPE
    SYNTAX      INTEGER  {
                    -- LLDP mandatory TLVs
                    mandatory(1),
                    optional(2),
                    -- LLDP MED
                    medCap(3),
                    medLocation(4),
                    medNetPolicy(5),
                    medPoe(6),
                    -- LLDP MED - Inventory
                    medInventory(7),
                    -- 802.3 TLVs
                    xDot3(8),
                    -- 802.1 TLVs
                    xDot1(9),
                    -- DCBX TLVs
                    dcbx(10)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Defines the TLVs groups.
            A value of mandatory(1) defines LLDP mandatory TLVs group
            A value of optinal(2) defines LLDP optional TLVs group
            A value of medCap(3) defines LLDP MED - Capabilities group
            A value of medLocation(4) defines LLDP MED - Location group
            A value of medNetPolicy(5) defines LLDP MED - Network Policy group
            A value of medPoe(6) defines  LLDP MED - Extended Power via MDI group
            A value of medInventory(7) defines LLDP MED - Inventory group
            A value of Xdot3(8) defines 802.3 TLVs group
            A value of Xdot1(9) defines 802.1 TLVs group "
    ::= { rlLldpTLVsTxOverloadingEntry 3 }

rlLldpTLVsTxSize   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            " The size of the TLV in Bytes."
    ::= { rlLldpTLVsTxOverloadingEntry  4 }

rlLldpTLVsTxGroupOverloading  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Boolean Flag, When TRUE indicating that LLDP TLVs were overloaded
            and the value of left size is negative"
    ::= { rlLldpTLVsTxOverloadingEntry  5 }

rlLldpTLVsTxLeftSize   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            " The size in Bytes of the available space left in the LLDPDU after adding the TLVs group.
            In case the Overloading Flag is TRUE, there not enough space in the LLDPDU for the TLVs group
            and this is the size of the additional scpace that required for the TLVs group"

    ::= { rlLldpTLVsTxOverloadingEntry  6 }

------------------------------------------------------------------------------
-- LLDP - TX TLV overloading Size
------------------------------------------------------------------------------

rlLldpTLVsTxOverloadingSizeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlLldpTLVsTxOverloadingSizeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A table that show the total size of the all TLVs
            and the LLDPDU free size  ."
    ::= {  rlLldpObjects 4 }

rlLldpTLVsTxOverloadingSizeEntry  OBJECT-TYPE
    SYNTAX      RlLldpTLVsTxOverloadingSizeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP TX overloading information"
   INDEX  { rlLldpTxOverloadingPortNum }
    ::= { rlLldpTLVsTxOverloadingSizeTable 1 }

RlLldpTLVsTxOverloadingSizeEntry ::= SEQUENCE {

    -- LLDP Total and Left Size
    rlLldpTotalTLVsTxSize                       Unsigned32,
    rlLldpTLVsTxOverloading                     TruthValue,
    rlLldpLeftTLVsTxSize                        Unsigned32
}

rlLldpTotalTLVsTxSize   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            " The Total size of all TLVs group in Bytes."
    ::= { rlLldpTLVsTxOverloadingSizeEntry 2 }

rlLldpTLVsTxOverloading  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Boolean Flag, When TRUE indicating that LLDP TLVs group were overloaded
             and the value of left size is negative"
    ::= { rlLldpTLVsTxOverloadingSizeEntry 3 }

rlLldpLeftTLVsTxSize   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            " The size in Bytes of the available space left in the LLDPDU after adding all TLVs group.
            In case the Overloading Flag is TRUE, there not enough space in the LLDPDU for all the TLVs group
            and this is the size of the additional scpace that required for all the TLVs group"
    ::= { rlLldpTLVsTxOverloadingSizeEntry 4 }

------------------------------------------------------------------------------
-- LLDP - TX TLV overloading port list
------------------------------------------------------------------------------

rlLldpTLVsTxOverloadingPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Port list that represent the overloading state of each port"
    ::= { rlLldpObjects 5 }

------------------------------------------------------------------------------
-- LLDP - TX TLV overloading trap
------------------------------------------------------------------------------
rlLldpTLVsTxOverloadingStateEnterTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Informational trap indicating that the port has entered the overloading state."
    ::= { rndNotifications 209 }

rlLldpTLVsTxOverloadingStateExitTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Informational trap indicating that the port is no longer in the overloading state.."
    ::= { rndNotifications 210 }


------------------------------------------------------------------------------
-- LLDP - MED Local Voice VLAN update mode
------------------------------------------------------------------------------

rlLldpXMedNetPolVoiceUpdateMode OBJECT-TYPE
    SYNTAX      PolicyAppVoiceUpdateMode
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            ""
    ::= { rlLldpObjects 7 }

------------------------------------------------------------------------------
-- LLDP - Remote Time to Live
------------------------------------------------------------------------------

rlLldpRemTtlTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlLldpRemTtlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
                "This table contains the remote device Time To Live LLDP TLV."
     ::= { rlLldpObjects 8 }

rlLldpRemTtlEntry  OBJECT-TYPE
    SYNTAX      RlLldpRemTtlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP Time To TTL remove TLV.
            This uses the key as defind in lldpRemTable of the LLDP-MIB."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex }
    ::= { rlLldpRemTtlTable 1 }

RlLldpRemTtlEntry ::= SEQUENCE {
    rlLldpRemTtl    Unsigned32
}

rlLldpRemTtl OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the remote device Time To Live LLDP TLV."
    ::= { rlLldpRemTtlEntry 1 }

rlLldpChassisIdSubtype OBJECT-TYPE
    SYNTAX      INTEGER {
                    macAddress(4),
                    local(7)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The type of encoding used to identify the chassis
            associated with the local system."

    REFERENCE
            "IEEE 802.1AB-2004 9.5.2.2"
    DEFVAL  { macAddress }
    ::= { rlLldpConfig 5 }


END

