--
-- RADWIN Management Information Base (MIB)
-- Generated 01/05/16 14:23:32 Version: 10.2.40_b9653
--
	RADWIN-MIB-WINLINK1000 DEFINITIONS ::= BEGIN

	IMPORTS 
		enterprises, IpAddress, Counter, Gauge, TimeTicks
			FROM RFC1155-SMI
		OBJECT-TYPE
			FROM RFC-1212
		DisplayString, ifIndex
			FROM RFC1213-MIB
		TRAP-TYPE
		    FROM RFC-1215;
	

	radwin			OBJECT IDENTIFIER ::= { enterprises 4458 }
	winlink1000		OBJECT IDENTIFIER ::= { radwin 1000 }

	-- ###########################################################
	--                      ODU
	-- ###########################################################

	winlink1000Odu OBJECT IDENTIFIER ::= { winlink1000 1 }

	-- ###########################################################
	--                      ODU Admin
	-- ###########################################################

	winlink1000OduAdmin OBJECT IDENTIFIER ::= { winlink1000Odu 1 }

	winlink1000OduAdmProductType OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU configuration description."
		::= { winlink1000OduAdmin 1 }

	winlink1000OduAdmHwRev OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU Hardware Version."
		::= { winlink1000OduAdmin 2 }

	winlink1000OduAdmSwRev OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU Software Version."
		::= { winlink1000OduAdmin 3 }

	winlink1000OduAdmLinkName OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Link Name. A change is effective immediately."
		::= { winlink1000OduAdmin 4 }

	winlink1000OduAdmResetCmd OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Reset Command. 
		A set command with a value of 3 will cause a device reset.
		HBS only: A set command with a value of 4 will cause a device reset for the entire sector.
		The read value is always 0."
		::= { winlink1000OduAdmin 5 }

	winlink1000OduAdmAddres OBJECT-TYPE
		SYNTAX  IpAddress
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"ODU IP address. A change is effective after reset.
		 The parameter is kept for backward compatibility.
		 Using the alternative parameter: winlink1000OduAdmIpParamsCnfg is recommended."
		::= { winlink1000OduAdmin 6 }

	winlink1000OduAdmMask OBJECT-TYPE
		SYNTAX  IpAddress
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"ODU Subnet Mask. A change is effective after reset.
		 The parameter is kept for backward compatibility.
		 Using the alternative parameter: winlink1000OduAdmIpParamsCnfg is recommended."
		::= { winlink1000OduAdmin 7 }

	winlink1000OduAdmGateway OBJECT-TYPE
		SYNTAX  IpAddress
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"ODU default gateway. A change is effective after reset.
		 The parameter is kept for backward compatibility.
		 Using the alternative parameter: winlink1000OduAdmIpParamsCnfg is recommended."
		::= { winlink1000OduAdmin 8 }	

	winlink1000OduAdmBroadcast OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"This parameter is reserved for the Manager application provided with the product."
		::= { winlink1000OduAdmin 10 }
	
	-- ###########################################################
	--                      ODU Admin Hosts Table
	-- ###########################################################

	winlink1000OduAdmHostsTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAdmHostsEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Trap destinations table. Each trap destination is defined by an IP address and a UDP port.
		Up to 10 addresses can be configured."
		::= { winlink1000OduAdmin 12 }

	winlink1000OduAdmHostsEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAdmHostsEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Trap destinations table entry."
		INDEX { winlink1000OduAdmHostsIndex }
		::= { winlink1000OduAdmHostsTable 1 }

	Winlink1000OduAdmHostsEntry ::= SEQUENCE {
		winlink1000OduAdmHostsIndex
			INTEGER,
		winlink1000OduAdmHostsIp
			IpAddress,
		winlink1000OduAdmHostsPort
			INTEGER,
		winlink1000OduAdmHostsSecurityModel
			INTEGER,
		winlink1000OduAdmHostsUserName
			DisplayString,
		winlink1000OduAdmHostsPassword
			DisplayString,
		winlink1000OduAdmHostsIPv6
			DisplayString
		}

	winlink1000OduAdmHostsIndex OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Trap destinations table index."
		::= { winlink1000OduAdmHostsEntry 1 }

	winlink1000OduAdmHostsIp OBJECT-TYPE
		SYNTAX  IpAddress
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Trap destination IP address. A change is effective immediately."
		::= { winlink1000OduAdmHostsEntry 2 }

	winlink1000OduAdmHostsPort OBJECT-TYPE
		SYNTAX  INTEGER (1..65535)
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"UDP port of the trap destination. A change is effective immediately."
		::= { winlink1000OduAdmHostsEntry 3 }
		
	winlink1000OduAdmHostsSecurityModel OBJECT-TYPE
		SYNTAX  INTEGER {
			snmpv1(1),
			snmpv3(3)		
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Security model used for this trap generation."
		::= { winlink1000OduAdmHostsEntry 4 }
		
	winlink1000OduAdmHostsUserName OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"User name used to generate the snmpv3 trap."
		::= { winlink1000OduAdmHostsEntry 5 }
		
	winlink1000OduAdmHostsPassword OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Password used to generate the snmpv3 trap."
		::= { winlink1000OduAdmHostsEntry 6 }

	winlink1000OduAdmHostsIPv6 OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Trap destination IPv6 address. A change is effective immediately."
		::= { winlink1000OduAdmHostsEntry 7 }
		
	winlink1000OduBuzzerAdminState OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"This parameter controls the activation of the buzzer while the unit is in install mode.
		A change is effective immediately. The valid values are: disabled (0), enabledAuto (1), enabledConstantly(2), advancedAuto (3)."
		::= { winlink1000OduAdmin 13 }

	winlink1000OduProductId OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"This parameter is reserved for the Manager application provided with the product."
		::= { winlink1000OduAdmin 14 }

	winlink1000OduReadCommunity OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Read Community String. This parameter always returns ***** when retrieving its value.
		It is used by the Manager application to change the Read Community String.
		The SNMP agent accepts only encrypted values."
		::= { winlink1000OduAdmin 15 }

	winlink1000OduReadWriteCommunity OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Read/Write Community String. This parameter always returns ***** when retrieving its value.
		It is used by the Manager application to change the Read/Write Community String.
		The SNMP agent accepts only encrypted values."
		::= { winlink1000OduAdmin 16 }

	winlink1000OduTrapCommunity OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Trap Community String. This parameter is used by the Manager application to change the Trap Community String.
		The SNMP agent accepts only encrypted values."
		::= { winlink1000OduAdmin 17 }

	winlink1000OduAdmSnmpAgentVersion OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Major version of the SNMP agent."
		::= { winlink1000OduAdmin 18 }

	winlink1000OduAdmRemoteSiteName OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Remote site name. Returns the same value as sysLocation parameter of the remote site."
		::= { winlink1000OduAdmin 19 }

	winlink1000OduAdmSnmpAgentMinorVersion OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Minor version of the SNMP agent."
		::= { winlink1000OduAdmin 20 }

	winlink1000OduAdmLinkPassword OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Link Password. This parameter always returns ***** when retrieving its value.
		It is used by the Manager application to change the Link Password.
		The SNMP agent accepts only encrypted values."
		::= { winlink1000OduAdmin 21 }

	winlink1000OduAdmSiteLinkPassword OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Site Link Password. This parameter always returns ***** when retrieving its value.
		It is used by the Manager application to change the Link Password of the site.
		The SNMP agent accepts only encrypted values."
		::= { winlink1000OduAdmin 22 }

	winlink1000OduAdmDefaultPassword OBJECT-TYPE
		SYNTAX  INTEGER {
			default(1),
			nonDefault(2)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"This parameter indicates if the current Link Password is the default password."
		::= { winlink1000OduAdmin 23 }

	winlink1000OduAdmConnectionType OBJECT-TYPE
		SYNTAX  INTEGER {
			directConnection(1),
			indirectConnection(2),
			unknown(3)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"This parameter indicates if the Manager application is connected to the local ODU
		or to the remote ODU over the air. A value of 'unknown' indicates community string mismatch."
		::= { winlink1000OduAdmin 24 }

	winlink1000OduAdmBackToFactorySettingsCmd OBJECT-TYPE
		SYNTAX  INTEGER {
			withIP(1),
			withoutIP(2)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Back to factory settings Command. A change is effective after reset. 
		The read value is always 0."
		::= { winlink1000OduAdmin 25 }
		
	winlink1000OduAdmIpParamsCnfg OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"ODU IP address Configuration. The format is: |||"
		::= { winlink1000OduAdmin 26 }

	winlink1000OduAdmVlanID OBJECT-TYPE
		SYNTAX INTEGER (0..4094)
		ACCESS  read-write
		STATUS mandatory
		DESCRIPTION
		"VLAN ID. Valid values are 1 to 4094.
		Initial value is 0 meaning VLAN unaware."
		::= { winlink1000OduAdmin 27 }  

	winlink1000OduAdmVlanPriority OBJECT-TYPE
		SYNTAX INTEGER (0..7)
		ACCESS  read-write
		STATUS mandatory
		DESCRIPTION
		"VLAN Priority. 0 is lowest priority, 7 is highest priority."
		::= { winlink1000OduAdmin 28 }  
		
	winlink1000OduAdmSN OBJECT-TYPE
        SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
        DESCRIPTION
        "ODU Serial Number"
        ::= { winlink1000OduAdmin 29 }

	winlink1000OduAdmProductName OBJECT-TYPE
		SYNTAX DisplayString
		ACCESS  read-only
		STATUS mandatory
		DESCRIPTION
		"This is the product name as it exists at EC"
		::= { winlink1000OduAdmin 30 }
		
	winlink1000OduAdmActivationKey OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Activates a general key."
		::= { winlink1000OduAdmin 31 }
		
	winlink1000OduAdmRmtPermittedOduType OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Mobile Application: permitted partner OduType."
		::= { winlink1000OduAdmin 32 }
		
	winlink1000OduAdmCpuID OBJECT-TYPE
		SYNTAX  INTEGER (0..64)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"CPU ID"
		::= { winlink1000OduAdmin 33 }
		
	winlink1000OduAdmOvrdCmd OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Ability to perform special command in the ODU."
		::= { winlink1000OduAdmin 34 }
				
	winlink1000OduAdmLinkMode OBJECT-TYPE
		SYNTAX  INTEGER {
			pmpHbs (1),
			pmpHsu (2),
			pmpHsuHyb (3),
			pmpHbsHyb (4)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Unit PMP operation mode."
		::= { winlink1000OduAdmin 35 }
		
	winlink1000OduAdmActualConnectMode OBJECT-TYPE
		SYNTAX  INTEGER {
			none (1),
			ptp (2),
			ptmp (3)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Unit connected as part to ptp or ptmp."
		::= { winlink1000OduAdmin 36 }
		
	winlink1000OduAdmAES256Support OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported (1),
			supported (2)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"AES-256 security support indication."
		::= { winlink1000OduAdmin 37 }
		
	winlink1000OduAdmAES256State OBJECT-TYPE
		SYNTAX  INTEGER {
			disabled (1),
			enabled (2)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Enable/Disable AES-256 security mode over the air link."
		::= { winlink1000OduAdmin 38 }
		
	winlink1000OduAdmAES256Status OBJECT-TYPE
		SYNTAX  INTEGER {
			notOperating (1),
			partiallyOperating (2),
			operating (3)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"AES256 operating status"
		::= { winlink1000OduAdmin 39 }

	winlink1000OduAdmBatterySavingShutdownTime OBJECT-TYPE
		SYNTAX  INTEGER (0..1000)
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Battery Saving Shutdown Time in minutes, 0 till battery run out, -1 if not supported."
		::= { winlink1000OduAdmin 40 }

	winlink1000OduAdmWiFiPowerMode OBJECT-TYPE
		SYNTAX  INTEGER {
			undefined (1),
			powerON (2),
			powerOFF (3),
			alwaysON (4)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"WIFI unit power mode."
		::= { winlink1000OduAdmin 41 }
	
	winlink1000OduAdmShutdownTimer OBJECT-TYPE
		SYNTAX  INTEGER (0..2147483647)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Shutdown Timer in seconds."
		::= { winlink1000OduAdmin 42 }
	
	winlink1000OduAdmGPSState OBJECT-TYPE
		SYNTAX  INTEGER {
			undefined (1),
			notSynchronized (2),
			fixed (3),
			shortCircuit (4),
			faulty (5),
			synchronized (6),
			synchronizedGlonass (7)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"GPS state"
		::= { winlink1000OduAdmin 43 }
		
	winlink1000OduAdmTemperatureC OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"The temperature (Celsius) inside the Board."
		::= { winlink1000OduAdmin 44 }	
	
	winlink1000OduAdmIPStackMode OBJECT-TYPE
		SYNTAX  INTEGER {
			v4 (1),
			v6 (2),
			v4andv6 (3)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"The IP stack mode."
		::= { winlink1000OduAdmin 45 }	
		
	winlink1000OduAdmIPv6ParamsCnfg OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"ODU IPv6 address Configuration. The format is: |||"
		::= { winlink1000OduAdmin 46 }

	winlink1000OduAdmIPv6Address OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU IPv6 address."
		::= { winlink1000OduAdmin 47 }

	winlink1000OduAdmIPv6Prefix OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU IPv6 subnet mask."
		::= { winlink1000OduAdmin 48 }	

	winlink1000OduAdmIPv6DefaultGateWay OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU IPv6 default gateway."
		::= { winlink1000OduAdmin 49 }
					
	winlink1000OduAdmPowerConsumption OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Power Consumption (mWatt)"
		::= { winlink1000OduAdmin 50 }	
	
	-- ###########################################################
	--                      ODU Wifi
	-- ###########################################################
	
	winlink1000OduAdmWifi OBJECT IDENTIFIER ::= { winlink1000OduAdmin 51 }
	
	winlink1000OduAdmWifiChannel OBJECT-TYPE
		SYNTAX  INTEGER (1..11)
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Wifi Channel"
		::= { winlink1000OduAdmWifi 1 }	

	winlink1000OduAdmWifiTxPower OBJECT-TYPE
		SYNTAX  INTEGER (11..15)
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Wifi TX Power"
		::= { winlink1000OduAdmWifi 2 }				

	winlink1000OduAdmWifiSSID OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Wifi SSID"
		::= { winlink1000OduAdmWifi 3 }		

	winlink1000OduAdmWifiSecurityType OBJECT-TYPE
		SYNTAX  INTEGER {
			open (1),
			wep (2),
			wpa2 (3)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Wifi Security type"
		::= { winlink1000OduAdmWifi 4 }			

	winlink1000OduAdmWifiPassword OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Wifi Password"
		::= { winlink1000OduAdmWifi 5 }		
		
	winlink1000OduAdmWifiNetwork OBJECT-TYPE
		SYNTAX  IpAddress
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Wifi Network"
		::= { winlink1000OduAdmWifi 6 }	

	winlink1000OduAdmWifiRssi OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Wifi RSSI"
		::= { winlink1000OduAdmWifi 7 }	

	winlink1000OduAdmWifiStationMAC OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Wifi Station MAC"
		::= { winlink1000OduAdmWifi 8 }		

	winlink1000OduAdmWifiRestart OBJECT-TYPE
		SYNTAX  INTEGER (1)
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"A set command with a value of 1 will cause a Wifi restart.
		The read value is always 0."
		::= { winlink1000OduAdmWifi 9 }		

	winlink1000OduAdmWifiApStatus OBJECT-TYPE
		SYNTAX  INTEGER {
			off (1),
			on (2),
			connected (3)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Wifi AP Status"
		::= { winlink1000OduAdmWifi 10 }

	winlink1000OduAdmBsaOperationMode OBJECT-TYPE
		SYNTAX  INTEGER {
			inactive (1),
			hbsTracking (2),
			hsuAlignment (3)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"BSA Operation Mode"
		::= { winlink1000OduAdmin 52 }
		
	winlink1000OduAdmMngConnection OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Management Connection"
		::= { winlink1000OduAdmin 53 }
		
	winlink1000OduAdm1588TCSupport OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported (1),
			supported (2)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Indicates that 1588TC license activated"
		::= { winlink1000OduAdmin 54 }

	winlink1000OduAdmSyncESupport OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported (1),
			supported (2)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ndicates that SyncE license activated"
		::= { winlink1000OduAdmin 55 }

	winlink1000OduAdmRadioRev OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Radio Revision"
		::= { winlink1000OduAdmin 56 }
		
	winlink1000OduAdmProductRev OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Product Revision"
		::= { winlink1000OduAdmin 57 }		
		
	winlink1000OduAdmPMPSUSupport OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported (1),
			supported (2)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Indicates that PMP SU license is activated"
		::= { winlink1000OduAdmin 58 }	
		
	winlink1000OduAdmManagerDownloadURL OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"This is the URL from which management tool can be downloaded"
		::= { winlink1000OduAdmin 59 }
		
	winlink1000OduAdmAntennaDescription OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"The is a description of the antenna connected to the ODU"
		::= { winlink1000OduAdmin 60 }
		
	winlink1000OduAdmSwCapabilities OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"This is used to describe which Software Capabilities the current ODU supports"
		::= { winlink1000OduAdmin 61 }
		
	-- ###########################################################
	--                      ODU Service
	-- ###########################################################

	winlink1000OduService OBJECT IDENTIFIER ::= { winlink1000Odu 2 }

	winlink1000OduSrvMode OBJECT-TYPE
		SYNTAX  INTEGER {
			installMode (1),
			normalMode (2),
			slaveMode (3),
			tempInstallMode (4),
			inactiveMode (5)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"System mode. The only values that can be set are installMode and slaveMode;
		normalMode reserved to the Manager application provided with the product.
		A change is effective after link re-synchronization."
		::= { winlink1000OduService 1 }

	winlink1000OduSrvBridging OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Bridging Mode. Valid values are: disabled (0), enabled (1)."
		::= { winlink1000OduService 3 }
		
	-- ###########################################################
	--                      ODU Ring Topology
	-- ###########################################################
	
	winlink1000OduServiceRingTopology OBJECT IDENTIFIER ::= { winlink1000OduService 4 }
	
	winlink1000OduSrvRingLinkMode OBJECT-TYPE
		SYNTAX  INTEGER {
			independentLink (1),				
			nonRpl (2),
			rpl (3)	
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Mode of the link regarding ring topology."
		::= { winlink1000OduServiceRingTopology 1 }		

	winlink1000OduSrvRingTopologySupported OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported (1),
			supported (2)			
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Ring Topology, options are: supported, not supported"
		::= { winlink1000OduServiceRingTopology 2 }
		
	winlink1000OduSrvRingVlanIdTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduSrvRingVlanIdEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Ring VLAN IDs table."
		::= { winlink1000OduServiceRingTopology 3 }

	winlink1000OduSrvRingVlanIdEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduSrvRingVlanIdEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"VLAN ID of the internal ring messages. Valid values are 1 to 4094.
		Initial value is 0 meaning VLAN unaware."
		INDEX { winlink1000OduSrvRingVlanIdIndex }
		::= { winlink1000OduSrvRingVlanIdTable 1 }

	Winlink1000OduSrvRingVlanIdEntry ::= SEQUENCE {
		winlink1000OduSrvRingVlanIdIndex
			INTEGER,
		winlink1000OduSrvRingVlanId
			INTEGER
		}

	winlink1000OduSrvRingVlanIdIndex OBJECT-TYPE
		SYNTAX  INTEGER (0..3)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Index of VLAN ID of the internal ring messages."			
		::= { winlink1000OduSrvRingVlanIdEntry 1 }

	winlink1000OduSrvRingVlanId OBJECT-TYPE
		SYNTAX  INTEGER (0..4094)
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"VLAN ID of the internal ring messages. Valid values are 1 to 4094.
		Initial value is 0 meaning VLAN unaware."
		::= { winlink1000OduSrvRingVlanIdEntry 2 }
		
		
	winlink1000OduSrvRingEthStatus OBJECT-TYPE
		SYNTAX  INTEGER {				
			unblocked(1),				
			blocked(2),
			notApplicable(3)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the Ethernet service blocking state of a Rings link"
		::= { winlink1000OduServiceRingTopology 4 } 			
			
	winlink1000OduSrvRingMaxAllowedTimeFromLastRpm OBJECT-TYPE
		SYNTAX  INTEGER 
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Defines the minimal time (in ms) required for determination of ring failure."
		::= { winlink1000OduServiceRingTopology 5 }			
			
	winlink1000OduSrvRingWTR OBJECT-TYPE
		SYNTAX  INTEGER 
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Defines the minimal time (in ms) required for ring recovery."
		::= { winlink1000OduServiceRingTopology 6 }			
		-- ###########################################################
		--                      ODU QoS
		-- ###########################################################
		
		winlink1000OduServiceQoS OBJECT IDENTIFIER ::= { winlink1000OduService 5 }
		
		winlink1000OduSrvQoSMode OBJECT-TYPE
			SYNTAX  INTEGER {
				notSupported (1),				
				notActive (2),
				classVlan (3),
				classDiffserv (4)
				}
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"Mode of QoS feature."
			::= { winlink1000OduServiceQoS 1 }
			
		winlink1000OduSrvQoSConfTable OBJECT-TYPE
			SYNTAX  SEQUENCE OF Winlink1000OduSrvQoSConfEntry
			ACCESS  not-accessible
			STATUS  mandatory
			DESCRIPTION
			"QoS configuration table."
			::= { winlink1000OduServiceQoS 2 }
			
		winlink1000OduSrvQoSConfEntry OBJECT-TYPE
			SYNTAX  Winlink1000OduSrvQoSConfEntry
			ACCESS  not-accessible
			STATUS  mandatory
			DESCRIPTION
			"QoS configuration table."
			INDEX { winlink1000OduSrvQoSConfIndex }
			::= { winlink1000OduSrvQoSConfTable 1 }
			
		Winlink1000OduSrvQoSConfEntry ::= SEQUENCE {
			winlink1000OduSrvQoSConfIndex
				INTEGER,
			winlink1000OduSrvConfVlanQGroups
				INTEGER,
			winlink1000OduSrvConfDiffservQGroups
				INTEGER,
			winlink1000OduSrvConfQueMir
				INTEGER,
			winlink1000OduSrvConfQueWeight
				INTEGER
			}
			
		winlink1000OduSrvQoSConfIndex OBJECT-TYPE
			SYNTAX  INTEGER (0..3)
			ACCESS  read-only
			STATUS  mandatory
			DESCRIPTION
			"Index of QoS Configuration."			
			::= { winlink1000OduSrvQoSConfEntry 1 }
			
		winlink1000OduSrvConfVlanQGroups OBJECT-TYPE
			SYNTAX  INTEGER (0..7)
			ACCESS  read-only
			STATUS  mandatory
			DESCRIPTION
			"Frames classification according to VLAN Priority IDs."			
			::= { winlink1000OduSrvQoSConfEntry 2 }
			
		winlink1000OduSrvConfDiffservQGroups OBJECT-TYPE
			SYNTAX  INTEGER (0..48)
			ACCESS  read-only
			STATUS  mandatory
			DESCRIPTION
			"Frames classification according to Diffserv."			
			::= { winlink1000OduSrvQoSConfEntry 3 }
			
		winlink1000OduSrvConfQueMir OBJECT-TYPE
			SYNTAX  INTEGER 
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"Desired Private MIR."			
			::= { winlink1000OduSrvQoSConfEntry 4 }
			
		winlink1000OduSrvConfQueWeight OBJECT-TYPE
			SYNTAX  INTEGER (0..100)
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"QoS queueu's weights in percent."			
			::= { winlink1000OduSrvQoSConfEntry 5 }		
			
		winlink1000OduSrvQoSVlanQGroupsSetStr OBJECT-TYPE
			SYNTAX  DisplayString
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"Frames classification according to VLAN IDs string for set."
			::= { winlink1000OduServiceQoS 3 }
			
		winlink1000OduSrvQoSDiffservQGroupsSetStr OBJECT-TYPE
			SYNTAX  DisplayString
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"Frames classification according to Diffserv IDs string for set."
			::= { winlink1000OduServiceQoS 4 }
			
		winlink1000OduSrvQoSMaxRTQuePercent OBJECT-TYPE
			SYNTAX  INTEGER (0..100)				
			ACCESS  read-only
			STATUS  mandatory
			DESCRIPTION
			"Maximal percent for RT & NRT queues."
			::= { winlink1000OduServiceQoS 5 }
		
		-- ###########################################################
		--                      ODU VLAN Configuration
		-- ###########################################################
		
		winlink1000OduServiceVlan OBJECT IDENTIFIER ::= { winlink1000OduService 6 }
		
		winlink1000OduSrvVlanSupport OBJECT-TYPE
			SYNTAX  INTEGER {
				notSupported (1),				
				supported(2),
				available(3)
				}
			ACCESS  read-only
			STATUS  mandatory
			DESCRIPTION
			"ODU Ethernet port VLAN support and configuration availability indication.
			1 - ODU VLAN Functionality Not Supported
			2 - ODU VLAN Functionality Supported
			3 - ODU VLAN Functionality Supported and Available"
			::= { winlink1000OduServiceVlan 1 }
			
		winlink1000OduSrvVlanIngressMode OBJECT-TYPE
			SYNTAX  INTEGER {
				transparent (1),				
				untagAll    (2),
				filter      (3)
				}
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"ODU Ethernet port ingress VLAN mode."
			::= { winlink1000OduServiceVlan 2 }
			
		winlink1000OduSrvVlanEgressMode OBJECT-TYPE
			SYNTAX  INTEGER {
				transparent (1),				
				tag (2),
				provider (3)
				}
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"ODU Ethernet port egress VLAN mode."
			::= { winlink1000OduServiceVlan 3 }
			
		winlink1000OduSrvEgressTag OBJECT-TYPE
			SYNTAX  INTEGER (0..40947)
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"ODU ethernet port egress VLAN tag.
			Right most digit is Vlan priority (0-7), 
			other digits compose Vlan Id (2-4094)"
			::= { winlink1000OduServiceVlan 4 }
			
		winlink1000OduSrvEgressProviderTag OBJECT-TYPE
			SYNTAX  INTEGER (0..40947)
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"ODU ethernet port egress Provider VLAN tag.
			Right most digit is Vlan priority (0-7), 
			other digits compose Vlan Id (2-4094)"
			::= { winlink1000OduServiceVlan 5 }
			
		winlink1000OduSrvVlanIngressAllowedVIDs OBJECT-TYPE
			SYNTAX  DisplayString
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"ODU ethernet port VLAN IDs that will not be filtered on ingress.
			w|w|w|w|w|w|w|w| ( where w = {0-4094} and w != 1 )"
			::= { winlink1000OduServiceVlan 6 }
			
		winlink1000OduSrvVlanDisable OBJECT-TYPE
			SYNTAX  INTEGER
			ACCESS  read-write
			STATUS  mandatory
			DESCRIPTION
			"Disable VLAN functionality. The following values can be set:
			3 - Disable ODU & IDU VLAN Configurations."
			::= { winlink1000OduServiceVlan 7 }	
			
		winlink1000OduServiceVlanProviderListTPIDstr OBJECT-TYPE
			SYNTAX  DisplayString
			ACCESS  read-only
			STATUS  mandatory
			DESCRIPTION
			"Holds the possible Provider TPIDs."
			::= { winlink1000OduServiceVlan 8 }
			
	-- ###########################################################
	--                      ODU Ethernet
	-- ###########################################################

	winlink1000OduEthernet OBJECT IDENTIFIER ::= { winlink1000Odu 3 }

	winlink1000OduEthernetRemainingRate OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Current Ethernet bandwidth in bps."
		::= { winlink1000OduEthernet 1 }	

	-- ###########################################################
	--                      ODU Ethernet Interface Table
	-- ###########################################################

	winlink1000OduEthernetIfTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduEthernetIfEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Ethernet Interface table."
		::= { winlink1000OduEthernet 2 }

	winlink1000OduEthernetIfEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduEthernetIfEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Ethernet Interface table entry."
		INDEX { winlink1000OduEthernetIfIndex }
		::= { winlink1000OduEthernetIfTable 1 }

	Winlink1000OduEthernetIfEntry ::= SEQUENCE {
		winlink1000OduEthernetIfIndex
			INTEGER,
		winlink1000OduEthernetIfAddress
			DisplayString,
		winlink1000OduEthernetIfAdminStatus
			INTEGER,
		winlink1000OduEthernetIfOperStatus
			INTEGER,
		winlink1000OduEthernetIfFailAction
			INTEGER,
		winlink1000OduEthernetIf1588v2PTPEventRXRate
			INTEGER,
		winlink1000OduEthernetIf1588v2PTPEventTXRate
			INTEGER
		}

	winlink1000OduEthernetIfIndex OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU Ethernet Interface Index." 
		::= { winlink1000OduEthernetIfEntry 1 }	

	winlink1000OduEthernetIfAddress OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU MAC address."
		::= { winlink1000OduEthernetIfEntry 5 }

	winlink1000OduEthernetIfAdminStatus OBJECT-TYPE
		SYNTAX  INTEGER {
			portAutoSense(1),
			portAutoSense100Mbps(5),			
			forceHalfDuplex10Mbps(10),			
			forceFullDuplex10Mbps(11),
			forceHalfDuplex100Mbps(15),
			forceFullDuplex100Mbps(16),
			forceFullDuplex1000Mbps(21),
			disablePoePort(254),			
			disablePort(255)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Required state of the interface."
		::= { winlink1000OduEthernetIfEntry 6 }	

	winlink1000OduEthernetIfOperStatus OBJECT-TYPE
		SYNTAX  INTEGER {
			notConnected(1),
			connectedHalfDuplex10Mbps(10),
			connectedFullDuplex10Mbps(11),
			connectedHalfDuplex100Mbps(15),
			connectedFullDuplex100Mbps(16),
			connectedHalfDuplex1000Mbps(20),
			connectedFullDuplex1000Mbps(21),
			unknown(65535)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Current operational state of the interface."
		::= { winlink1000OduEthernetIfEntry 7 }
		
	winlink1000OduEthernetIfFailAction OBJECT-TYPE
		SYNTAX  INTEGER {
			faNoAction(1),
			faForceHalfDuplex10Mbps(10),			
			faForceFullDuplex10Mbps(11),
			faDisablePort(255)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Failure action of the interface."
		::= { winlink1000OduEthernetIfEntry 8 }			
		
	winlink1000OduEthernetIf1588v2PTPEventRXRate OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"For debug use"
		::= { winlink1000OduEthernetIfEntry 9 }
		
	winlink1000OduEthernetIf1588v2PTPEventTXRate OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"For debug use"
		::= { winlink1000OduEthernetIfEntry 10 }		

	winlink1000OduEthernetNumOfPorts OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number of ODU network interfaces."
		::= { winlink1000OduEthernet 3 }
		
	
	winlink1000OduEthernetGbeSupported OBJECT-TYPE
		SYNTAX  INTEGER {notSupported(1), supported(2)}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Supported Giga bit Ethernet in ODU."
		::= { winlink1000OduEthernet 4 }

	winlink1000OduEthernetSfpProperties OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Sfp port properties."
		::= { winlink1000OduEthernet 5 }			

	-- ###########################################################
	--                      ODU Bridge
	-- ###########################################################

	winlink1000OduBridge OBJECT IDENTIFIER ::= { winlink1000Odu 4 }

	-- ###########################################################
	--                      ODU Bridge Base
	-- ###########################################################

	winlink1000OduBridgeBase OBJECT IDENTIFIER ::= { winlink1000OduBridge 1 }

	-- ###########################################################
	--                      ODU Bridge Ports Table
	-- ###########################################################

	winlink1000OduBridgeBasePortTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduBridgeBasePortEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Bridge Ports table."
		::= { winlink1000OduBridgeBase 4 }

	winlink1000OduBridgeBasePortEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduBridgeBasePortEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Bridge Ports table entry."
		INDEX { winlink1000OduBridgeBasePortIndex }
		::= { winlink1000OduBridgeBasePortTable 1 }

	Winlink1000OduBridgeBasePortEntry ::= SEQUENCE {
		winlink1000OduBridgeBasePortIndex
			INTEGER,
		winlink1000OduBridgeBaseIfIndex
			INTEGER
		}

	winlink1000OduBridgeBasePortIndex OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU Bridge Port Number."
		::= { winlink1000OduBridgeBasePortEntry 1 }

	winlink1000OduBridgeBaseIfIndex OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"IfIndex corresponding to ODU Bridge port."
		::= { winlink1000OduBridgeBasePortEntry 2 }

	-- ###########################################################
	--                      ODU Bridge Tp
	-- ###########################################################

	winlink1000OduBridgeTp OBJECT IDENTIFIER ::= { winlink1000OduBridge 4 }

	winlink1000OduBridgeTpMode OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"ODU bridge mode. 
		A change is effective after reset. Valid values: hubMode (0), bridgeMode (1)."
		::= { winlink1000OduBridgeTp 101 }

	-- ###########################################################
	--                      ODU Transparent Bridge Ports Table
	-- ###########################################################

	winlink1000OduBridgeTpPortTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduBridgeTpPortEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Transparent Bridge Ports table."
		::= { winlink1000OduBridgeTp 3 }

	winlink1000OduBridgeTpPortEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduBridgeTpPortEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Transparent Bridge Ports table entry."
		INDEX { winlink1000OduBridgeTpPortIndex }
		::= { winlink1000OduBridgeTpPortTable 1 }

	Winlink1000OduBridgeTpPortEntry ::= SEQUENCE {
		winlink1000OduBridgeTpPortIndex
			INTEGER,
		winlink1000OduBridgeTpPortInFrames
			Counter,
		winlink1000OduBridgeTpPortOutFrames
			Counter,
		winlink1000OduBridgeTpPortInBytes
			Counter,
		winlink1000OduBridgeTpPortOutBytes
			Counter
		}

	winlink1000OduBridgeTpPortIndex OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU Transparent Bridge Port Number."
		::= { winlink1000OduBridgeTpPortEntry 1 }

	winlink1000OduBridgeTpPortInFrames OBJECT-TYPE
		SYNTAX  Counter
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number of frames received by this port."
		::= { winlink1000OduBridgeTpPortEntry 3 }

	winlink1000OduBridgeTpPortOutFrames OBJECT-TYPE
		SYNTAX  Counter
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number of frames transmitted by this port."
		::= { winlink1000OduBridgeTpPortEntry 4 }

	winlink1000OduBridgeTpPortInBytes OBJECT-TYPE
		SYNTAX  Counter
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number of bytes received by this port."
		::= { winlink1000OduBridgeTpPortEntry 101 }

	winlink1000OduBridgeTpPortOutBytes OBJECT-TYPE
		SYNTAX  Counter
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number of bytes transmitted by this port."
		::= { winlink1000OduBridgeTpPortEntry 102 }
		
	winlink1000OduBridgeConfigMode OBJECT-TYPE
		SYNTAX  INTEGER{
			enable (1),
			disable (2)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU bridge configuration mode"
		::= { winlink1000OduBridgeTp 102 }

	-- ###########################################################
	--                      ODU Air
	-- ###########################################################

	winlink1000OduAir OBJECT IDENTIFIER ::= { winlink1000Odu 5 }

	winlink1000OduAirFreq OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Installation Center Frequency. Valid values are product dependent. A change is effective after link re-synchronization."
		::= { winlink1000OduAir 1 }

	winlink1000OduAirDesiredRate OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  deprecated
		DESCRIPTION
		"Deprecated parameter, actual behavior is read-only. 
		Required Air Rate. For Channel Bandwidth of 20, 10, 5 MHz divide the value by 1, 2, 4 respectively."
		::= { winlink1000OduAir 2 }

	winlink1000OduAirSSID OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Reserved for the Manager application provided with the product.
		 The Sector ID in Point-To-Multi-Point systems."
		::= { winlink1000OduAir 3 }

	winlink1000OduAirTxPower OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Required Transmit power in dBm . This is a nominal value while the actual transmit power includes additional attenuation.
		The min and max values are product specific. A change is effective immediately."
		::= { winlink1000OduAir 4 }

	winlink1000OduAirSesState OBJECT-TYPE
		SYNTAX  INTEGER {
			sessionDown (1),
			basicRate (2),
			active (3),
			installation (4),
			scanning (5),
			probing (6),
			transmitting (7),
			activeWithDefaultEncryptionKey (8),
			installationWithDefaultEncryptionKey (9),
			bitFailed (10),
			activeWithVersionsMismatch (11),
			installationWithVersionsMismatch (12),
			inactive (13),
			iduIncompatible (14),
			spectrumAnalysis (15)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Current Link State. The value is active (3) during normal operation." 
		::= { winlink1000OduAir 5 }

	winlink1000OduAirMstrSlv OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"This parameter indicates if the device was automatically selected into the radio link master or slave. 
		The value is undefined if there is no link.
		The value is relevant only for point to point systems."
		::= { winlink1000OduAir 6 }	

	winlink1000OduAirResync OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Setting this parameter to 1 will cause the link to restart the synchronization process."
		::= { winlink1000OduAir 8 }

	-- ###########################################################
	--                      ODU Air Perf
	-- ###########################################################

	winlink1000OduAirPerf OBJECT IDENTIFIER ::= { winlink1000OduAir 9 }

	winlink1000OduAirRxPower OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Received Signal Strength in dBm. Relevant only for point to point systems."
		::= { winlink1000OduAirPerf 1 }

	winlink1000OduAirTotalFrames OBJECT-TYPE
		SYNTAX  Counter
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Total number of radio frames."
		::= { winlink1000OduAirPerf 2 }

	winlink1000OduAirBadFrames OBJECT-TYPE
		SYNTAX  Counter
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Total number of received radio frames with CRC error. The value is relevant only for point to point systems ."
		::= { winlink1000OduAirPerf 3 }

	winlink1000OduAirCurrentRate OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  deprecated
		DESCRIPTION
		"Deprecated parameter. Actual rate of the air interface in Mbps. 
		For Channel Bandwidth of 20, 10, 5 MHz divide the value by 1, 2, 4 respectively."
		::= { winlink1000OduAirPerf 4 }

	winlink1000OduAirCurrentRateIdx OBJECT-TYPE
		SYNTAX  INTEGER 
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Index of current air rate."
		::= { winlink1000OduAirPerf 5 }
		
	winlink1000OduAirChainsRxPower OBJECT-TYPE
		SYNTAX  OCTET STRING
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Received Signal Strength of Cpe chains in dBm.
		Chain 1 RSS: (1 Byte)
		Chain 2 RSS: (1 Byte)
		Chain 3 RSS: (1 Byte)"
		::= { winlink1000OduAirPerf 6 }

	winlink1000OduAirCurrentRateCBW OBJECT-TYPE
		SYNTAX  INTEGER 
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"CBW of current air rate."
		::= { winlink1000OduAirPerf 7 }
		
	winlink1000OduAirCurrentRateGI OBJECT-TYPE
		SYNTAX  INTEGER 
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"GI of current air rate."
		::= { winlink1000OduAirPerf 8 }
		
	winlink1000OduAirTxPower36 OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  deprecated
		DESCRIPTION
		"Deprecated parameter. Actual behavior is read-only."
		::= { winlink1000OduAir 10 }

	winlink1000OduAirTxPower48 OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  deprecated
		DESCRIPTION
		"Deprecated parameter. Actual behavior is read-only."
		::= { winlink1000OduAir 11 }

	winlink1000OduAirCurrentTxPower OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Current Transmit Power in dBm. This is a nominal value while the actual transmit power includes additional attenuation."
		::= { winlink1000OduAir 12 }

	winlink1000OduAirMinFrequency OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Minimum center frequency in MHz."
		::= { winlink1000OduAir 13 }

	winlink1000OduAirMaxFrequency OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Maximum center frequency in MHz."
		::= { winlink1000OduAir 14 }

	winlink1000OduAirFreqResolution OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Center Frequency resolution. 
		Measured in MHz if value < 100, otherwise in KHz."
		::= { winlink1000OduAir 15 }

	winlink1000OduAirCurrentFreq OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Current Center Frequency.
		Measured in MHz if center frequency resolution value < 100, otherwise in KHz."
		::= { winlink1000OduAir 16 }

	winlink1000OduAirNumberOfChannels OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number of channels that can be used."
		::= { winlink1000OduAir 17 }

	-- ###########################################################
	--                      Channels Table
	-- ###########################################################

	winlink1000OduAirChannelsTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAirChannelsEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Table of channels used by automatic channels selection (ACS)."
		::= { winlink1000OduAir 18 }

	winlink1000OduAirChannelsEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAirChannelsEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ACS channels table entry."
		INDEX { winlink1000OduAirChannelsIndex }
		::= { winlink1000OduAirChannelsTable 1 }

	Winlink1000OduAirChannelsEntry ::= SEQUENCE {
		winlink1000OduAirChannelsIndex
			INTEGER,
		winlink1000OduAirChannelsFrequency
			INTEGER,
		winlink1000OduAirChannelsOperState
			INTEGER,
		winlink1000OduAirChannelsAvail
			INTEGER,
		winlink1000OduAirChannelsDefaultFreq
			INTEGER
		}

	winlink1000OduAirChannelsIndex OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Channel Index."
		::= { winlink1000OduAirChannelsEntry 1 }

	winlink1000OduAirChannelsFrequency OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Channel frequency in MHz."
		::= { winlink1000OduAirChannelsEntry 2 }

	winlink1000OduAirChannelsOperState OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Channel state. Can be set by the user. 
		 Automatic Channel Selection uses channels that are AirChannelsOperState enabled and AirChannelsAvail enabled. 
		 A change is effective after link re-synchronization. Valid values: disabled (0), enabled (1).
		 Rewriteable only in Point-To-Point products."
		::= { winlink1000OduAirChannelsEntry 3 }

	winlink1000OduAirChannelsAvail OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Channel state. Product specific and cannot be changed by the user. 
		Automatic Channel Selection uses channels that are AirChannelsOperState enabled and AirChannelsAvail enabled. 
		Valid values: disabled (0), enabled (1)."
		::= { winlink1000OduAirChannelsEntry 4 }

	winlink1000OduAirChannelsDefaultFreq OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Default channel's availability for all CBWs.
		The valid values are: forbidden (0), available (1)."
		::= { winlink1000OduAirChannelsEntry 5 }

	winlink1000OduAirDfsState OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Radar detection state. Valid values: disabled (0), enabled (1)."
		::= { winlink1000OduAir 19 }

	winlink1000OduAirAutoChannelSelectionState OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  deprecated
		DESCRIPTION
		"Deprecated parameter. Indicating Automatic Channel Selection availability at current channel bandwidth. 
		Valid values: disabled (0), enabled (1)."
		::= { winlink1000OduAir 20 }

	winlink1000OduAirEnableTxPower OBJECT-TYPE
		SYNTAX  INTEGER {
			enabled (1),
			disabled (2)
			}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Indicating Transmit power configuration enabled or disabled."
		::= { winlink1000OduAir 21 }

	winlink1000OduAirMinTxPower OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Minimum Transmit power in dBm."
		::= { winlink1000OduAir 22 }

	-- ###########################################################
	--                      Max Tx Power Table
	-- ###########################################################

	winlink1000OduAirMaxTxPowerTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAirMaxTxPowerEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Table of Maximum transmit power per air rate, in dBm."
		::= { winlink1000OduAir 23 }

	winlink1000OduAirMaxTxPowerEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAirMaxTxPowerEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Maximum Transmit power table entry."
		INDEX { winlink1000OduAirMaxTxPowerIndex }
		::= { winlink1000OduAirMaxTxPowerTable 1 }

	Winlink1000OduAirMaxTxPowerEntry ::= SEQUENCE {
		winlink1000OduAirMaxTxPowerIndex
			INTEGER,
		winlink1000OduAirMaxTxPower
			INTEGER
		}

	winlink1000OduAirMaxTxPowerIndex OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Air interface rate index."
		::= { winlink1000OduAirMaxTxPowerEntry 1 }

	winlink1000OduAirMaxTxPower OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Maximum Transmit power in dBm."
		::= { winlink1000OduAirMaxTxPowerEntry 2 }

	winlink1000OduAirChannelBandwidth OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Channel bandwidth in KHz. A change is effective after reset."
		::= { winlink1000OduAir 24 }

	-- ###########################################################
	--                      Channel BW Table
	-- ###########################################################

	winlink1000OduAirChannelBWTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAirChannelBWEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Channel Bandwidths table."
		::= { winlink1000OduAir 25 }

	winlink1000OduAirChannelBWEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAirChannelBWEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Channel Bandwidth table entry."
		INDEX { winlink1000OduAirChannelBWIndex }
		::= { winlink1000OduAirChannelBWTable 1 }

	Winlink1000OduAirChannelBWEntry ::= SEQUENCE {
		winlink1000OduAirChannelBWIndex
			INTEGER,
		winlink1000OduAirChannelBWAvail
			INTEGER,
		winlink1000OduAirChannelsAdminState
			DisplayString,
		winlink1000OduAirChannelBWHSSATDDConflictPerCBW
			INTEGER,
		winlink1000OduAirChannelBWMinRatioForSupporting
			INTEGER,
		winlink1000OduAirChannelBWMaxRatioForSupporting
			INTEGER	
		}

	winlink1000OduAirChannelBWIndex OBJECT-TYPE
		SYNTAX  INTEGER {
				channelBW5MHz(1),
				channelBW10MHz(2),
				channelBW20MHz(3),
				channelBW40MHz(4),
				channelBW80MHz(5),
				channelBW7MHz(6),
				channelBW14MHz(7)				
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Channel Bandwidth index."
		::= { winlink1000OduAirChannelBWEntry 1 }

	winlink1000OduAirChannelBWAvail OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported(1),
			supportedManual(2),
			supportedWithACS(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Channel Bandwidth availability, product specific.
		Options are: Not supported, supported with manual channel selection, supported with Automatic Channel Selection."
		::= { winlink1000OduAirChannelBWEntry 2 }

	winlink1000OduAirChannelsAdminState OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Channels' availability per CBW."
		::= { winlink1000OduAirChannelBWEntry 3 }

	winlink1000OduAirChannelBWHSSATDDConflictPerCBW OBJECT-TYPE
		SYNTAX  INTEGER {
			noConflict(1),
			conflictSingle(2),
			conflictDual(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Indication for possible Link drop per CBW due to conflict between HSS and ATDD."
		::= { winlink1000OduAirChannelBWEntry 4 }

	winlink1000OduAirChannelBWMinRatioForSupporting OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Minimal TX ratio that may be used by the HSM and still enable proper operation of the aforementioned CBW."
		::= { winlink1000OduAirChannelBWEntry 5 }

	winlink1000OduAirChannelBWMaxRatioForSupporting OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Maximal TX ratio that may be used by the HSM and still enable proper operation of the aforementioned CBW."
		::= { winlink1000OduAirChannelBWEntry 6 }

	winlink1000OduAirRFD OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Current radio frame duration in microseconds."
		::= { winlink1000OduAir 26 }

	-- ###########################################################
	--                      Available Rates Table
	-- ###########################################################

	winlink1000OduAirRatesTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAirRatesEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Air Rate indexes table for current channel bandwidth."
		::= { winlink1000OduAir 27 }

	winlink1000OduAirRatesEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAirRatesEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Air Rate indexes table entry."
		INDEX { winlink1000OduAirRatesIndex }
		::= { winlink1000OduAirRatesTable 1 }

	Winlink1000OduAirRatesEntry ::= SEQUENCE {
		winlink1000OduAirRatesIndex
			INTEGER,
		winlink1000OduAirRatesAvail
			INTEGER
		}

	winlink1000OduAirRatesIndex OBJECT-TYPE
		SYNTAX  INTEGER 
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Air Rate index."
		::= { winlink1000OduAirRatesEntry 1 }

	winlink1000OduAirRatesAvail OBJECT-TYPE
		SYNTAX  INTEGER {
			rateNotAvailable(1),
			rateAvailable(2)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Air Rate availability, depending on air interface conditions."
		::= { winlink1000OduAirRatesEntry 2 }

	winlink1000OduAirDesiredRateIdx OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Required Air Rate index. 0 reserved for Adaptive Rate.
		A change is effective immediately after Set operation to the master side
		while the link is up."
		::= { winlink1000OduAir 28 }

	winlink1000OduAirLinkDistance OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Link distance in meters. 
		A value of -1 indicates an illegal value and is also used when a link is not established."
		::= { winlink1000OduAir 29 }

	winlink1000OduAirLinkWorkingMode OBJECT-TYPE
		SYNTAX  INTEGER {
			unknown(1),
			normal(2),
			fullCompatibilityRemoteUpgradeAvailable(3),
			fullCompatibilityLocalUpgradeAvailable(4),
			restrictedCompatibilityRemoteUpgradeRecomended(5),
			restrictedCompatibilityLocalUpgradeRecomended(6),
			softwareUpgradeRemoteUpgradeRequired(7),
			softwareUpgradeLocalUpgradeRequired(8),
			versionsIncompatibilityRemoteUpgradeRequired(9),
			versionsIncompatibilityLocalUpgradeRequired(10)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Link working mode as a result of comparing versions of both sides of the link. 
		Possible modes are: Unknown - no link, Normal - versions on both sides are identical with full compatibility, 
		with restricted compatibility, or versions on both sides are different with software upgrade or versions incompatibility."
		::= { winlink1000OduAir 30 }

	winlink1000OduAirMajorLinkIfVersion OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Major link interface version"
		::= { winlink1000OduAir 31 }

	winlink1000OduAirMinorLinkIfVersion OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Minor link interface version"
		::= { winlink1000OduAir 32 }

	winlink1000OduAirHss OBJECT IDENTIFIER ::= { winlink1000OduAir 40 }

	winlink1000OduAirHssDesiredOpState OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported(1),
			independentUnit(2),
			hubSyncMaster(3),
			hubSyncClientContinueTx(4),
			hubSyncClientDisableTx(5),
			gpsSync(6),
			independentSyncUnit-ISU(7)
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Required Hub Site Synchronization operating state.
		For HssSyncUnits : 	For hssISU :[2,7] ,For hssGSU :[2,6]
		For HBS:			[2,3,4,5]"		
		::= { winlink1000OduAirHss 1 }

	winlink1000OduAirHssCurrentOpState OBJECT-TYPE
		SYNTAX  INTEGER {
			notSupported(1),
			independentUnit(2),
			hubSyncMaster(3),
			hubSyncClientContinueTx(4),
			hubSyncClientDisableTx(5),
			gpsSync(6),
			independentSyncUnit-ISU(7)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Current Hub Site Synchronization operating state."		
		::= { winlink1000OduAirHss 2 }

	winlink1000OduAirHssSyncStatus OBJECT-TYPE
		SYNTAX  INTEGER {
			notApplicable(1),
			notSynchronized(2),
			synchronized(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization sync status."		
		::= { winlink1000OduAirHss 3 }

	winlink1000OduAirHssExtPulseStatus OBJECT-TYPE
		SYNTAX  INTEGER {
			notDetected(1),
			generating(2),
			generatingAndDetected(3),
			generatingAndImproperDetected(4),
			detected(5),
			improperDetected(6),
			multipleSourcesDetected(7)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization external pulse detection status.
		In GSS mode: 
		if generating then 1PSP is auto generated by the GSS Unit.
		if generatingAndDetecting then 1PSP is generated by GPS satellites signal."		
		::= { winlink1000OduAirHss 4 }

	winlink1000OduAirHssExtPulseType OBJECT-TYPE
		SYNTAX  INTEGER {
			notApplicable(1),
			typeA(2),
			typeB(3),
			typeC(4),
			typeD(5),
			typeE(6),
			typeF(7)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization external pulse type."		
		::= { winlink1000OduAirHss 5 }
		
	winlink1000OduAirHssDesiredExtPulseType OBJECT-TYPE
		SYNTAX  INTEGER {
			notApplicable(1),
			typeA(2),
			typeB(3),
			typeC(4),
			typeD(5),
			typeE(6),
			typeF(7)
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization required external pulse type. Valid values for read write:
		 {typeA(2),typeB(3),typeC(4),typeD(5),typeE(6),typeF(7)}. Valid value for read only:
		 {notApplicable(1)}."		
		::= { winlink1000OduAirHss 6 }
		
	-- ###########################################################
	--                      HSS Radio Frame Pattern Table
	-- ###########################################################
	winlink1000OduAirHssRfpTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAirHssRfpEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Radio Frame Patterns (RFP) Table."
		::= { winlink1000OduAirHss 7 }

	winlink1000OduAirHssRfpEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAirHssRfpEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU RFP Table entry."
		INDEX { winlink1000OduAirHssRfpIndex }
		::= { winlink1000OduAirHssRfpTable 1 }

	Winlink1000OduAirHssRfpEntry ::= SEQUENCE {
		winlink1000OduAirHssRfpIndex
			INTEGER,
		winlink1000OduAirHssRfpEthChannelBW5MHz
			INTEGER,
		winlink1000OduAirHssRfpTdmChannelBW5MHz
			INTEGER,
		winlink1000OduAirHssRfpEthChannelBW10MHz
			INTEGER,
		winlink1000OduAirHssRfpTdmChannelBW10MHz
			INTEGER,
		winlink1000OduAirHssRfpEthChannelBW20MHz
			INTEGER,
		winlink1000OduAirHssRfpTdmChannelBW20MHz
			INTEGER,
		winlink1000OduAirHssRfpEthChannelBW40MHz
			INTEGER,
		winlink1000OduAirHssRfpTdmChannelBW40MHz
			INTEGER,
		winlink1000OduAirHssRfpEthChannelBW80MHz
			INTEGER,
		winlink1000OduAirHssRfpEthChannelBW7MHz
			INTEGER,
		winlink1000OduAirHssRfpEthChannelBW14MHz
			INTEGER
		}
		
	winlink1000OduAirHssRfpIndex OBJECT-TYPE
		SYNTAX  INTEGER (2..7)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"ODU RFP Table index. The index represent the Radio Frame Pattern:
		 typeA(2), typeB(3), typeC(4), typeD(5),typeE(6),typeF(7)."
		::= { winlink1000OduAirHssRfpEntry 1 }
		
	winlink1000OduAirHssRfpEthChannelBW5MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of Ethernet service under Channel BW of 5MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 2 }
		
	winlink1000OduAirHssRfpTdmChannelBW5MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of TDM service under Channel BW of 5MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 3 }
		
		winlink1000OduAirHssRfpEthChannelBW10MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of Ethernet service under Channel BW of 10MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 4 }
		
	winlink1000OduAirHssRfpTdmChannelBW10MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of TDM service under Channel BW of 10MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 5 }
		
	winlink1000OduAirHssRfpEthChannelBW20MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of Ethernet service under Channel BW of 20MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 6 }
		
	winlink1000OduAirHssRfpTdmChannelBW20MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of TDM service under Channel BW of 20MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 7 }
		
	winlink1000OduAirHssRfpEthChannelBW40MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of Ethernet service under Channel BW of 40MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 8 }
		
	winlink1000OduAirHssRfpTdmChannelBW40MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of TDM service under Channel BW of 40MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 9 }
	
	winlink1000OduAirHssRfpEthChannelBW80MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of Ethernet service under Channel BW of 80MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 10 }
		
	winlink1000OduAirHssRfpEthChannelBW7MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of Ethernet service under Channel BW of 7MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 11 }
	
	winlink1000OduAirHssRfpEthChannelBW14MHz OBJECT-TYPE
		SYNTAX  INTEGER {
			bestFit(1),
			nonOptimal(2),
			notAvailable(3)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Represents the compatibility of Ethernet service under Channel BW of 14MHz 
		 in the specific Radio Frame Pattern."
		::= { winlink1000OduAirHssRfpEntry 12 }
	
	winlink1000OduAirHssRfpStr OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization supported patterns"
		::= { winlink1000OduAirHss 8 }
		
	winlink1000OduAirHssHsmID OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"A  unique ID which is common to the HSM and all its collocated ODUs"
		::= { winlink1000OduAirHss 9 }
		
	winlink1000OduAirHssTime OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS time"
		::= { winlink1000OduAirHss 10 }
		
	winlink1000OduAirHssLatitude OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS Latitude"
		::= { winlink1000OduAirHss 11 }
		
	winlink1000OduAirHssNSIndicator OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS N/S Indicator"
		::= { winlink1000OduAirHss 12 }
		
	winlink1000OduAirHssLongitude OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS Longitude"
		::= { winlink1000OduAirHss 13 }
		
	winlink1000OduAirHssEWIndicator OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS E/W Indicator"
		::= { winlink1000OduAirHss 14 }
		
	winlink1000OduAirHssNumSatellites OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS Number of satellites"
		::= { winlink1000OduAirHss 15 }
		
	winlink1000OduAirHssAltitude OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS Altitude"
		::= { winlink1000OduAirHss 16 }
		
	winlink1000OduAirHssRfpPhase OBJECT-TYPE
		SYNTAX  INTEGER {
			rfpNormalPhase(1),
			rfpShiftedPhase(2)
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Hub Site Synchronization GPS RFP phase"
		::= { winlink1000OduAirHss 17 }
		
	winlink1000OduAirHssInterSiteSynchronizationMode OBJECT-TYPE
		SYNTAX  INTEGER {
			independent(1),
			synchronized(2)
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Inter-Site Synchronization Mode - independent / synchronized"
		::= { winlink1000OduAirHss 18 }
		
	winlink1000OduAirHssInterSiteSynchronizationAvailability OBJECT-TYPE
		SYNTAX  INTEGER {
			notAvailable(1),
			available(2)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Inter-Site Synchronization Availability"
		::= { winlink1000OduAirHss 19 }
		
	winlink1000OduAirHssSatellitesSatSyncRequired OBJECT-TYPE
		SYNTAX  INTEGER {
			notRequired(1),
			required(2)
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Satellites Synchronization Is Required"
		::= { winlink1000OduAirHss 20 }
		
	winlink1000OduAirHssDomainID OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"EHSS domain. Indentify set of CUs with same HSS synchronization"
		::= { winlink1000OduAirHss 21 }
		
	winlink1000OduAirHssSupportedSynchronizationProtocol OBJECT-TYPE
		SYNTAX  INTEGER {
			serialOnly(1),
			ethOnly(2),
			both(3),
			ghssAndEth(4),
			ghssEthSerial(5)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Supported Synchronization Protocols"
		::= { winlink1000OduAirHss 22 }
		
	winlink1000OduAirHssDesiredSynchronizationProtocol OBJECT-TYPE
		SYNTAX  INTEGER {
			serialOnly(1),
			ethOnly(2),
			both(3),
			ghssOnly(4)
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Desired Synchronization Protocols"
		::= { winlink1000OduAirHss 23 }
		
	winlink1000OduAirHssDiscover OBJECT-TYPE
		SYNTAX  INTEGER {
			startAll(1),
			startAllMstr(2),
			startMyDmn(3),
			startMyMstr(4)
		}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Initiate Discovery process of ODUs on the network."
		::= { winlink1000OduAirHss 24 }
		
	winlink1000OduAirHssNumberOfDiscoveredODUs OBJECT-TYPE
		SYNTAX  INTEGER (0..1000)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number OF Discovered ODUs in network."
		::= { winlink1000OduAirHss 25 }
		
	-- ###########################################################
	--                      HSS Discover Table
	-- ###########################################################
	
	winlink1000OduAirHssDiscoverTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAirHssDiscoverEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"HSS Discover Table."
		::= { winlink1000OduAirHss 26 }

	winlink1000OduAirHssDiscoverEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAirHssDiscoverEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"ODU Discover Table entry."
		INDEX { winlink1000OduAirHssDiscoverIndex }
		::= { winlink1000OduAirHssDiscoverTable 1 }

	Winlink1000OduAirHssDiscoverEntry ::= SEQUENCE {
		winlink1000OduAirHssDiscoverIndex
			INTEGER,
		winlink1000OduAirHssDiscoverODUDescription
			DisplayString
		}
		
	winlink1000OduAirHssDiscoverIndex OBJECT-TYPE
		SYNTAX  INTEGER (1..256)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"HSS Discover Table Index."
		::= { winlink1000OduAirHssDiscoverEntry 1 }
		
	winlink1000OduAirHssDiscoverODUDescription OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Hold ODU HSS status in compress format:
		Domain,IP,HSS Role,Hss support,
		Enabled HSS protocol,Sync Status,
		Location, IPv6."
		::= { winlink1000OduAirHssDiscoverEntry 2 }
		
	-- ###################### End of Discover Table ###################
	
	winlink1000OduAirHssMasterSlaveCompatibility OBJECT-TYPE
		SYNTAX  INTEGER {
			compatible(1),
			notCompatible(2)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"EHSM version compatibility. Relevant to Ethernet HSS Clients only."
		::= { winlink1000OduAirHss 27 }
		
	winlink1000OduAirHssNumberOfAssociatedCU OBJECT-TYPE
		SYNTAX  INTEGER (0..256)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Number of associated Ethernet HSS Clients. Relevant to Ethernet HSS Masters only"
		::= { winlink1000OduAirHss 28 }
		
	-- ###########################################################
	--                      HSS Associated CU Table
	-- ###########################################################
		
	winlink1000OduAirHssAssociatedCUTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF Winlink1000OduAirHssAssociatedCUTableEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Associated Ethernet HSS Clients Table. Releant for Ethernet HSS Masters only."
		::= { winlink1000OduAirHss 29 }

	winlink1000OduAirHssAssociatedCUTableEntry OBJECT-TYPE
		SYNTAX  Winlink1000OduAirHssAssociatedCUTableEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
		"Associated Ethernet HSS Clients Table Entry. Releant for Ethernet HSS Masters only."
		INDEX { winlink1000OduAirHssAssociatedCUIndex }
		::= { winlink1000OduAirHssAssociatedCUTable 1 }

	Winlink1000OduAirHssAssociatedCUTableEntry ::= SEQUENCE {
		winlink1000OduAirHssAssociatedCUIndex
			INTEGER,
		winlink1000OduAirHssAssociatedCUDescription
			DisplayString
		}
		
	winlink1000OduAirHssAssociatedCUIndex OBJECT-TYPE
		SYNTAX  INTEGER (1..256)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Associated Ethernet HSS Clients Table Index. Releant for Ethernet HSS Masters only."
		::= { winlink1000OduAirHssAssociatedCUTableEntry 1 }
		
	winlink1000OduAirHssAssociatedCUDescription OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Holds Associated Ethernet HSS Clients Description in compress format:
		IP,Delay,Compatibility,Ethernet Speed, Ethernet Rx rate, IPv6"
		::= { winlink1000OduAirHssAssociatedCUTableEntry 2 }
		
	-- ###################### End of Associated CU Table ###################
		
	winlink1000OduAirHssSyncStatusEth OBJECT-TYPE
		SYNTAX  INTEGER {
			notApplicable(1),
			notSynchronized(2),
			goodSynchronizationLevel(3),
			mediumSynchronizationLevel(4),
			badSynchronizationLevel(5),
			startSynchronization(6)
		}
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Ethernet HSS Client Synchronization Level"
		::= { winlink1000OduAirHss 30 }
		
	winlink1000OduAirHssEthVLANTag OBJECT-TYPE
		SYNTAX  INTEGER (1..40947)
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Ethernet HSS VLan Tag: 
		The least significate decimal digit is the VLan Priority(0-6) 
		and the rest of the digits represents VLan ID (2-4094)"
		::= { winlink1000OduAirHss 31 }
	
	winlink1000OduAirHssHSMIPAddress OBJECT-TYPE
		SYNTAX  IpAddress
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"HSMs IP address. Relevant for HSC synchronized over Ethernet."
		::= { winlink1000OduAirHss 32 }

	winlink1000OduAirHssDelayToHSM OBJECT-TYPE
		SYNTAX  INTEGER (0..1000000)
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"Delay in microseconds to HSM. Relevant for HSC synchronized over Ethernet."
		::= { winlink1000OduAirHss 33 }

	winlink1000OduAirHssSyncAcquisitionSeconds OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Accumulated quantity of seconds in clock acquisition while connected to current HSM"
		::= { winlink1000OduAirHss 34 }
		
	winlink1000OduAirHssHSMIPv6Address OBJECT-TYPE
		SYNTAX  DisplayString
		ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
		"HSMs IPv6 address. Relevant for HSC synchronized over Ethernet."
		::= { winlink1000OduAirHss 35 }
		
	-- ###################### End of HSS Section ###################
	
	winlink1000OduAirLockRemote OBJECT-TYPE
		SYNTAX  INTEGER {
			unlock(1),
			lock(2)
			}
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"This parameter enables locking the link with a specific ODU.
		 The following values can be set:
		 Unlock (default) - The ODU is not locked on a specific remote ODU. Unlock can only be performed when the link is not connected.
		 Lock - The ODU is locked on a specific remote ODU. Lock can only be performed when the link is active."
		::= { winlink1000OduAir 41 }

	winlink1000OduAirAntennaGain OBJECT-TYPE
		SYNTAX  INTEGER
		ACCESS  read-write
		STATUS  mandatory
		DESCRIPTION
		"Current Antenna Gain in 0.1 dBi resolution. User defined value for 
		external antenna.
		Legal range: MinAntennaGain - Alarm.
		"
		::= { winlink1000OduAir 42 }

	externalAlarmInPort1Alarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent every time an alarm occurs in the External Alarm Input of port #1.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 1 -  - Alarm.
		"
		::= 105

	externalAlarmInPort2Alarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent every time an alarm occurs in the External Alarm Input of port #2.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 2 -  - Alarm.
		"
		::= 106

	bitFailedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { critical }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent if there is no way to recover from the situation.		
		Contains two parameters:
		1 - Description: ODU power up built in test failed. Error code is: %n
		2 - %n number
		"
		::= 107

	wrongConfigurationLoadedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent if there is a way to recover from the situation.		
		Contains two parameters:
		1 - Description: Wrong configuration loaded. Error code is: %n
		2 - %n number
		"
		::= 108

	lanPort1DisconnectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the LAN port 1 status changed to disconnected.		
		Contains a single parameter, which is its description:
		1 - Description: LAN port 1 status changed to disconnected.
		"
		::= 109

	lanPort2DisconnectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the LAN port 2 status changed to disconnected.		
		Contains a single parameter, which is its description:
		1 - Description: LAN port 2 status changed to disconnected.
		"
		::= 110

	mngPortDisconnectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the LAN1 port status changed to disconnected.		
		Contains a single parameter, which is its description:
		1 - Description: LAN1 port status changed to disconnected.
		"
		::= 111

	externalAlarmInPort3Alarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent every time an alarm occurs in the External Alarm Input of port #3.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 3 -  - Alarm.
		"
		::= 112

	externalAlarmInPort4Alarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent every time an alarm occurs in the External Alarm Input of port #4.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 4 -  - Alarm.
		"
		::= 113

	swVersionsMismatchFullCompatibilityAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { warning }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions mismatch with full link functionality.
		Contains a single parameter, which is its description:
		1 - Description: Software versions mismatch - full link functionality
		"
		::= 114

	swVersionsMismatchRestrictedCompatibilityAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { minor }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions mismatch with restricted link functionality.
		Contains a single parameter, which is its description:
		1 - Description: Software versions mismatch - restricted link functionality
		"
		::= 115

	swVersionsMismatchSoftwareUpgradeRequired TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions mismatch and SW upgrade is required.
		Contains a single parameter, which is its description:
		1 - Description: Software versions mismatch - Software upgrade required
		"
		::= 116

	swVersionsIncompatible TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { critical }
		--&MESG "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions are incompatible.
		Contains a single parameter, which is its description:
		1 - Description: SW Versions incompatible
		"
		::= 117

	hssMultipleSourcesDetectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates that multiple sync pulse sources were detected.
		Contains a single parameter, which is its description:
		1 - Description: HSS multiple sync sources were detected.
		"
		::= 118

	hssSyncToProperSourceStoppedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates that synchronization to a proper sync pulse source was stopped.
		Contains a single parameter, which is its description:
		1 - Description: HSS sync pulse - Down. The reason is: %s.
		%s - Is the reason for the sync down.
		"
		::= 119

	hssSyncPulseDetectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that HSS additional sync pulse was detected.
		Contains a single parameter, which is its description:
		1 - Description: HSS additional sync pulse was detected.		
		"
		::= 120

	tdmBackupAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the TDM backup link was activated.
		Contains a single parameter, which is its description:
		1 - Description: TDM backup alarm - backup link was activated.
		"
		::= 121
		
	linkLockUnauthorizedRemoteODU TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the remote ODU is unauthorized. 
		Contains a single parameter, which is its description:
		1 - Description: Unauthorized remote ODU connection rejected.
		"
		::= 122
		
	linkLockUnauthorizedODU TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the ODU is unauthorized. 
		Contains a single parameter, which is its description:
		1 - Description: Unauthorized ODU connection rejected.
		"
		::= 123
		
	hotStandbyAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the hot standby secondary link was activated.
		Contains a single parameter, which is its description:
		1 - Description: Secondary Link Is Active.
		"
		::= 124

	sfpInsertion TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that a device was inserted to SFP Port
		"
		::= 126

	sfpPort1DisconnectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the SFP port 1 status changed to disconnected.		
		Contains a single parameter which is its description:
		1 - Description: SFP port 1 status changed to disconnected.
		"
		::= 127
		
	ringRplStateActiveAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		RPL state changed to Active.
		"
		::= 128
			

	desiredRatioCanNotBeAppliedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { minor }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates Desired UL/DL RAtio Can Not Be Applied.
		"
		::= 129
		
	cbwMismatch TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates that a Channel Bandwidth mismatch was detected.		
		Contains two parameters:
		1 - Description: Channel Bandwidth Mismatch: one side is %n0 MHz and the other is %n1 MHz.
		%n0 is the local Channel Bandwidth value in MHz.
		%n1 is the remoet Channel Bandwidth value in MHz."
		::= 130

	gpsNotSynchronized TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the GPS is not synchronized with satellites.
		Pulses are self generated.
		"
		::= 131
		
	pdTooHighDueCbwLimitations TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that link cannot be established because 
		link range is too large for channel bandwidth.
		"
		::= 132
		
	hbsEncryptionAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates an encryption key mismatch.
		Contains a single parameter, which is its description, including the HSU's name
		"
		::= 133
		
	hbsEhServiceClosedToHsu TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates an encryption key mismatch.
		Contains a single parameter, which is its description, including the HSU's name
		"
		::= 134

	hbsUnsynchronizedHsuAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { critical }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates a registered HSU lost synchronization.
		"
		::= 135
		
	hbsInactiveHbsAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates HBS is InActive.
		"
		::= 136
		
	incompatibleHsu TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { critical }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates that the HSU is not compatible to HBS.
		Contains a single parameter, which is its description:
		1 - Description: Incompatible ODUs.
		"
		::= 137
		
	hsuUnsupportedBeacon TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { warning }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates an unsupported beacon has arrived at HSU
		"
		::= 138
		
	lanPortDisconnectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the LAN port status changed to disconnected.		
		Contains a single parameter, which is its description:
		1 - Description: LAN port status changed to disconnected.
		"
		::= 139
		
	poePortDisconnectedAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the LAN2 port status changed to disconnected.		
		Contains a single parameter, which is its description:
		1 - Description: LAN2 port status changed to disconnected.
		"
		::= 140
		
	poePowerConsumptionAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the POE Power Consumption is above allowed maximum.		
		Contains a single parameter, which is its description:
		1 - Description: POE consumption above allowed maximum. port closed.
		"
		::= 141
		
	hobupFaultyStateAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		This Alarm will indicate that the Hot Backup module is in faulty state.
		1 - Description: Hot Backup fault detected: %s unit.
		%s - Primary Or Secondary Unit
		"
		::= 149

	gpsOverCurrentAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the GPS Antenna current consumption is above allowed maximum.		
		Contains a single parameter, which is its description:
		1 - Description: GPS Antenna current consumption above allowed maximum. GPS closed.
		"
		::= 150
		
	gpsCommunicationFailiureAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the GPS data isn't received.		
		Contains a single parameter, which is its description:
		1 - Description: GPS Communication failiure.
		"
		::= 151
	
	temperatureThresholdAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		Indicates the board temperature is above allowed maximum.		
		Contains a single parameter, which is its description:
		1 - Description: GPS Antenna current consumption above allowed maximum. GPS closed.
		"
		::= 152
		
	localRouterDiscoveryStatus TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		This Alarm will indicate that we have no connection with local train router.
		1 - Description: MacLearningUpdate detected disconnection with local train router %s
		%s - local train IP
		"
		::= 153
	
	trackRouterDiscoveryStatus TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		This Alarm will indicate that we have no connection with Track side router.
		1 - Description: MacLearningUpdate detected disconnection with Track side router %s
		%s - Default gateway IP
		"
		::= 154
		
	lastUserSnmpAccessOverHourAgo TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG "$'1"
		DESCRIPTION
		"
		This trap will indicate that the last access of the accessing user was more than an hour ago.
		1 - Description: User %s performed SNMP access after more than an hour.
		%s - user name
		"
		::= 155
		
	btsTargetUnreachable TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG "$'1"
		DESCRIPTION
		"
		This Alarm will indicate that we have no connection with Bts desired target.
		1 - Description: TNC detected disconnection with the BTS target %s
		%s - Default gateway IP
		"
		::= 156
		
	tdmServiceClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 100 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that TDM Service fault is cleared.
		Contains a single parameter, which is its description:
		1 - Description: TDM Service - Normal.
		"
		::= 200

	ethServiceOpened TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 101 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that Ethernet Service has been opened.
		Contains a single parameter, which is its description:
		1 - Description: Ethernet Service has been opened.
		"
		::= 201

	encryptionClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 103 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that encryption is OK.
		Contains a single parameter, which is its description:
		1 - Description: Encryption Status - Normal.
		"
		::= 203

	changeLinkPasswordClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 104 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the Link Password was changed successfully.
		Contains a single parameter, which is its description:
		1 - Description: Link Password has been changed at/on: %s.
		%s - Is the Local Site name or Remote Site name or both sides of the Link.
		"
		::= 204

	externalAlarmInPort1Clear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 105 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		This Trap is sent every time an External Alarm Input fault of port # 1 is cleared.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 1 -  - Alarm Cleared.
		"
		::= 205	

	externalAlarmInPort2Clear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 106 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		This Trap is sent every time an External Alarm Input fault of port # 2 is cleared.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 2 -  - Alarm Cleared.
		"
		::= 206
		
	lanPort1Clear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 109 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the LAN port 1 status changed to connected.
		Contains two parameters:
		1 - Description: LAN port 1 status changed to connected - %s
		2 - %s Is the Eth. mode (speed & duplex)
		"
		::= 209
		
	lanPort2Clear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 110 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the LAN port 2 status changed to connected.
		Contains two parameters:
		1 - Description: LAN port 2 status changed to connected - %s.
		2 - %s Is the Eth. mode (speed & duplex).
		"
		::= 210
		
	mngPortClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 111 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the LAN1 port status changed to connected.
		Contains two parameters:
		1 - Description: LAN1 port status changed to connected - %s
		2 - %s Is the Eth. mode (speed & duplex)
		"
		::= 211

	externalAlarmInPort3Clear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 112 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		This Trap is sent every time an External Alarm Input fault of port # 3 is cleared.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 3 -  - Alarm Cleared.
		"
		::= 212	

	externalAlarmInPort4Clear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 113 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		This Trap is sent every time an External Alarm Input fault of port # 4 is cleared.
		Contains a single parameter, which is its description:
		1 - Description: External Alarm 4 -  - Alarm Cleared.
		"
		::= 213
	
	swVersionsMatchFullCompatibilityClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 114 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions match.
		Contains a single parameter, which is its description:
		1 - Description: Software Versions compatible
		"
		::= 214

	swVersionsMatchRestrictedCompatibilityClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 115 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions match and link functionality is not restricted.
		Contains a single parameter, which is its description:
		1 - Description: Software Versions compatible
		"
		::= 215

	swVersionsMatchSoftwareUpgradeRequiredClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 116 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions match and SW upgrade is successful.
		Contains a single parameter, which is its description:
		1 - Description: Software Versions compatible
		"
		::= 216

	swVersionsCompatibleClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 117 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		The trap is sent if SW versions compatible
		Contains a single parameter, which is its description:
		1 - Description: Software Versions compatible
		"
		::= 217

	hssMultipleSourcesDisappearedClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 118 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that multiple sync pulse sources disappeared.
		Contains a single parameter, which is its description:
		1 - Description: HSS multiple sync pulse sources disappeared.
		"
		::= 218

	hssSyncToProperSourceAchievedClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 119 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that synchronization to a proper Sync source was achieved.
		Contains a single parameter, which is its description:
		1 - Description: HSS sync pulse - Up.
		"
		::= 219

	hssSyncPulseDisappearedClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 120 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that HSS additional sync pulse disappeared.
		Contains a single parameter, which is its description:
		1 - Description: HSS additional sync pulse was disappeared.		
		"
		::= 220

	tdmBackupClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 121 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the TDM main link was activated.
		Contains a single parameter, which is its description:
		1 - Description: TDM main link was activated.
		"
		::= 221
		
	linkLockAuthorizedRemoteODU TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 122 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the remote ODU is authorized.
		Contains a single parameter, which is its description:
		1 - Description: Authorized remote ODU connection accepted.
		"
		::= 222

	linkLockAuthorizedODU TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 123 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the ODU is authorized.
		Contains a single parameter, which is its description:
		1 - Description: Authorized ODU connection permitted.
		"
		::= 223		

	linkAuthenticationDisabled TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 122 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the Link Lock is disabled.
		Contains a single parameter, which is its description:
		1 - Description: Link Authentication has been disabled.
		"
		::= 224	

	hotStandbyClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 124 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the Primary Link Was Activated.
		Contains a single parameter, which is its description:
		1 - Description: Primary Link Is Active.
		"
		::= 225
		
	sfpExtraction TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that a device was extracted from SFP Port
		"
		::= 226

	sfpPort1Clear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 127 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the SFP port 1 status changed to connected.
		Contains two parameters:
		1 - Description: SFP port 1 status changed to connected - %s
		2 - %s Is the Eth. mode (speed & duplex)
		"
		::= 227

	compatibleIdus TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 10 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the ODU has identified compatible Idus on both sides of the link.
		"
		::= 228	

	desiredRatioCanNotBeAppliedClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 129 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates Current UL/DL Ratio Is Equal To Desired Ratio.
		"
		::= 229
		
	cbwMatch TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 130 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that a Channel Bandwidth match was detected.
		Contains a single parameter, which is its description:
		1 - Channel Bandwidth value in MHz.
		"
		::= 230
		
	switchCbwAndChannel TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the system is switching Channel Bandwidth and channel frequency.
		Contains two parameters:
		1 - Switching to Channel Bandwith %n0 MHz and to channel %n1 GHz.
		"
		::= 231			
		
	ringRplStateIdle TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 128 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		RPL state changed to Idle.
		"
		::= 232
		
	ringEthServiceStatus TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }		
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates Ethernet service's state - blocked \ unblocked.
		Contains a single parameter:
		1 - Description: Ethernet's state (blocked \ unblocked)
		"
		::= 233
		
	ringFirstRpmReceived TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }		
		--&MESG     "$'1"
		DESCRIPTION
		"
		Ring application: in non-RPL link indicates first from a specific RPL was received.
		Contains a single parameter:
		1 - Description: RPM's VLAN ID
		"
		::= 234
		
	ringEthernetSrviceUnblockedTO TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }		
		--&MESG     "$'1"
		DESCRIPTION
		"
		Ring application: in non-RPL link Ethernet service is unblocked due to RPM timeout.		
		"
		::= 235
		
	gpsSynchronized TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 131 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that the GPS is synchronized with satellites.
		"
		::= 236

	hbsEncryptionClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 133 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that encryption is OK.
		Contains a single parameter, which is its description, including the HSU's name
		"
		::= 237
		
	hbsEhServiceOpenedToHsu TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 134 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates that encryption is OK.
		Contains a single parameter, which is its description, including the HSU's name
		"
		::= 238

	hbsSynchronizedHsuAlarm TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 135 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates a registered HSU is synchronized.
		"
		::= 239
		
	hbsActiveHbs TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 136 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates when HBS has been activated.
		"
		::= 240
		
	switchCBW TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Switching Channel Bandwidth.
		"
		::= 241		

	changeRatio TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		HBS Tx ratio has changed.
		"
		::= 242			

	lanPortClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 139 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the LAN port status changed to connected.
		Contains two parameters:
		1 - Description: LAN port status changed to connected - %s
		2 - %s Is the Eth. mode (speed & duplex)
		"
		::= 243

	poePortClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 140 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the LAN2 port status changed to connected.
		Contains two parameters:
		1 - Description: LAN2 port status changed to connected - %s
		2 - %s Is the Eth. mode (speed & duplex)
		"
		::= 244	
		
	poePowerConsumptionClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 141 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the POE power consumption is valid.
		Contains two parameters:
		1 - Description: POE consumption within limits. port is opened.
		2 - %s Is the Eth. mode (speed & duplex)
		"
		::= 245

	incompatibleHbsHsu TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Incompatible HBS/HSU software versions - no service.
		"
		::= 246

	mobilityLinkOff TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Mobility - Link cannot be established due to:
		1 - The HBS does not support Mobility
		2 - Lack of resources in the HBS for HSU level
		"
		::= 247

	enterLocalConnection TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Entering Local Connection (Broadcast) Mode.
		"
		::= 248	
	
	hobupActiveStateFaultyClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 149 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		this clear alarm will indicate that the Hot Backup unit is in active state.
		Contains a single parameter, which is its description:
		1 - Description: Hot Backup %s unit activated.
		%s - Primary Or Secondary Unit
		"	
		::= 249	
		
	hobupStandbyState TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		This info fault will indicate that the Hot backup module has entered standby/peer_detection state
		Contains a single parameter, which is its description:
		1 - Description: Hot Backup in Standby state: %s unit.
		%s - Primary Or Secondary Unit
		"	
		::= 250		

	gpsOverCurrentClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 150 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the GPS Antenna current consumption is valid.
		"
		::= 251
		
	temperatureThresholdClear TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 152 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicates the board temperature is valid.
		"
		::= 252		
		
	localRouterDiscoverySucceed TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 153 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicated the we succeeded to discover train router in ip %s MAC address %s
		%s Train IP
		%s Train MAC Address
		"
		::= 253	
	
	trackRouterDiscoverySucceed TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 154 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicated the we succeeded to discover track router in ip %s MAC address %s
		%s Train IP
		%s Train MAC Address
		"
		::= 254	
		
	qosVersion2StrictMismatch TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		CPE  doesn't support strict QOS configuration.
		"	
		::= 255
		
	qosVersion2TtlMismatch TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		CPE doesn't support TTL configuration.
		"	
		::= 256
		
	btsTargetIsReachable TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 156 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicated the we succeeded to establish connection with the Bts desired target (%s)
		%s Target IP
		"
		::= 257
		
	tcNotSupportedByHSU TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		CPE doesn't support TC functionality.
		"	
		::= 258
		
	syncEPortHOStateChange TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Enter/leave HO state of SyncE port.
		"	
		::= 259
		
	syncEPortFailureStateChange TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Enter/leave Failure state of SyncE port.
		"	
		::= 260
		
	btsCpeUpdateServiceFailed TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Update service Failed
		"	
		::= 261
		
	btsCpeUpdateServiceSucceed TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Update service Succeed
		"	
		::= 262
	radiusServerNoREsponse TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		No response from radius server
		"	
		::= 263	
	noRadiusServerRespond TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { major }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Alarm indicates that no Radius server is connected
		"	
		::= 264	
	radiusServerRespondedSuccessfully TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&CLEARS   { 264 }
		--&MESG     "$'1"
		DESCRIPTION
		"
		indicates that Radius server responded seccessfully.
		"	
		::= 265	

	bsaAlignmentStarted TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicate the beginning of Alignment Process
		"
		::= 266
		
	bsaAlignmentFinished TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicate the completion of Alignment Process
		"
		::= 267
		
	bsaAlignmentTriggered TRAP-TYPE
		ENTERPRISE winlink1000
		VARIABLES   { winlink1000GeneralTrapDescription, winlink1000OduAgnCurrAlarmSeverity, winlink1000OduAgnCurrAlarmIfIndex,
		winlink1000OduAgnCurrAlarmUnit, winlink1000OduAgnCurrAlarmTimeT, winlink1000OduAgnCurrAlarmId }
		--&ACTIONS  { normal }
		--&MESG     "$'1"
		DESCRIPTION
		"
		Indicate the triggering of Alignment Process due to exceeding thresholds
		"
		::= 268

	-- ###########################################################
	--                 Products Section
	-- ###########################################################


	radwinProducts			OBJECT IDENTIFIER ::= { radwin 20 }
	winlink1000Family		OBJECT IDENTIFIER ::= { radwinProducts 2 } 
	radwin2000Family		OBJECT IDENTIFIER ::= { radwinProducts 3 }
	gpsSynchronizerFamily	OBJECT IDENTIFIER ::= { radwinProducts 4 }
	radwin5000HBSFamily		OBJECT IDENTIFIER ::= { radwinProducts 5 }
	radwin5000HSUFamily		OBJECT IDENTIFIER ::= { radwinProducts 6 }
	radwin6000Family		OBJECT IDENTIFIER ::= { radwinProducts 10 }
	radwinWiFiAPFamily		OBJECT IDENTIFIER ::= { radwinProducts 20 }


	--
	-- the following identifiers are assigned to ODU Products
	--        

	odu	       					OBJECT IDENTIFIER ::= { winlink1000Family 1 }

	oduIntegratedAntenna        OBJECT IDENTIFIER ::= { odu 1 }
	oduExternalAntenna          OBJECT IDENTIFIER ::= { odu 2 }

	--
	-- Suffix 3,4,5,6,7,8,9,10,11,12,13,14,15,16 in the products section
	-- are reserved for backward compatibility.
	--

	odu2000    					OBJECT IDENTIFIER ::= { radwin2000Family 1 }

	odu2KIntegratedAntenna        OBJECT IDENTIFIER ::= { odu2000 1 }
	odu2KExternalAntenna          OBJECT IDENTIFIER ::= { odu2000 2 }

	oduGSU						OBJECT IDENTIFIER ::= { gpsSynchronizerFamily 1 }
	
	oduGSUExternalAntenna		OBJECT IDENTIFIER ::= { oduGSU 2 }

	hssSyncUnits				OBJECT IDENTIFIER ::= { gpsSynchronizerFamily 2 }
	
	hssISU						OBJECT IDENTIFIER ::= { hssSyncUnits 1 }
	hssGSU						OBJECT IDENTIFIER ::= { hssSyncUnits 2 }

	oduHBS    					OBJECT IDENTIFIER ::= { radwin5000HBSFamily 1 }

	oduHBSIntegratedAntenna		OBJECT IDENTIFIER ::= { oduHBS 1 }
	oduHBSExternalAntenna		OBJECT IDENTIFIER ::= { oduHBS 2 }
	
	oduHSU    					OBJECT IDENTIFIER ::= { radwin5000HSUFamily 1 }

	oduHSUIntegratedAntenna		OBJECT IDENTIFIER ::= { oduHSU 1 }
	oduHSUExternalAntenna		OBJECT IDENTIFIER ::= { oduHSU 2 }	

	odu6000    					OBJECT IDENTIFIER ::= { radwin6000Family 1 }

	odu6K						OBJECT IDENTIFIER ::= { odu6000 1 }
	
	gateway6000    				OBJECT IDENTIFIER ::= { radwin6000Family 2 }

	gateway6K						OBJECT IDENTIFIER ::= { gateway6000 1 }
	
	odu600    					OBJECT IDENTIFIER ::= { radwinWiFiAPFamily 1 }

	oduWiFiAP					OBJECT IDENTIFIER ::= { odu600 1 }
	
	END

