--
-- Juniper Enterprise Specifics MIB
-- 
-- Copyright (c) 2003-2004, Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--

JUNIPER-Services-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter64, Gauge32
        FROM SNMPv2-SMI
    ifIndex
        FROM IF-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    jnxMibs
        FROM JUNIPER-SMI;

jnxServicesInfoMib  	MODULE-IDENTITY
    LAST-UPDATED 	"200307182154Z" -- Fri Jul 18 21:54:00 2003 UTC
    ORGANIZATION 	"Juniper Networks, Inc."
    CONTACT-INFO
            		"Juniper Technical Assistance Center
			Juniper Networks, Inc.
			1133 Innovation Way
			Sunnyvale, CA 94089
			E-mail: support@juniper.net"

    DESCRIPTION
            "This is Juniper Networks' implementation of enterprise
	     specific MIB for monitoring services properties"

    -- revision history -- 
    
	REVISION "200401300000Z"    -- 30 January, 2004
	DESCRIPTION
		"Initial version."

    ::= { jnxMibs 27 }


--
-- Flow table aggregate statistics information
--
-- These statistics concern the basic flow table functionality 
-- available on both AS PICs and GGSN-I PICs
--


jnxSvcFlowTableAggStatsTable	OBJECT-TYPE
    SYNTAX       		SEQUENCE OF JnxSvcFlowTableAggStatsEntry
    MAX-ACCESS   		not-accessible
    STATUS       		current
    DESCRIPTION
	"Aggregated statistics information about all flow tables on 
	 the service PIC interface."
    ::= { jnxServicesInfoMib 1 }

jnxSvcFlowTableAggStatsEntry	OBJECT-TYPE
    SYNTAX			JnxSvcFlowTableAggStatsEntry
    MAX-ACCESS			not-accessible
    STATUS			current
    DESCRIPTION
	"An entry containing aggregated statistics for all 
	 flow tables for a particular service pic interface."
    INDEX   		{ ifIndex }
    ::= { jnxSvcFlowTableAggStatsTable 1 }

JnxSvcFlowTableAggStatsEntry ::= SEQUENCE {

    --- flow creation, cleanup, counts
    
    jnxSvcAggFlow			Gauge32,
    jnxSvcAggFlowMaximum		Gauge32,
    jnxSvcAggFlowCreated		Counter64,
    jnxSvcAggFlowFreed			Counter64,
    jnxSvcAggFlowIdleFreed		Counter64,

    --- TCP flows (all types)

    jnxSvcAggFlowTcp			Gauge32,
    jnxSvcAggFlowTcpMaximum		Gauge32,
    jnxSvcAggFlowTcpCreated		Counter64,
    jnxSvcAggFlowTcpFreed		Counter64,
    jnxSvcAggFlowTcpIdleFreed		Counter64,

    --- UDP flows (all types)

    jnxSvcAggFlowUdp			Gauge32,
    jnxSvcAggFlowUdpMaximum		Gauge32,
    jnxSvcAggFlowUdpCreated		Counter64,
    jnxSvcAggFlowUdpFreed		Counter64,
    jnxSvcAggFlowUdpIdleFreed		Counter64,

    -- general counters for packets 

    jnxSvcAggFlowPkt			Counter64, -- total
    jnxSvcAggFlowPktErr		Counter64,
    jnxSvcAggFlowByte			Counter64, -- total 
    jnxSvcAggFlowByteErr		Counter64,

    -- ICMP packets are a special case
    
    jnxSvcAggFlowIcmpPkt		Counter64, -- total
    jnxSvcAggFlowIcmpPktErr		Counter64,
    jnxSvcAggFlowIcmpPktErrBadFlow	Counter64,
    jnxSvcAggFlowIcmpByte		Counter64, -- total
    jnxSvcAggFlowIcmpByteErr	Counter64,
    
    -- TCP packets overall statistics
    
    jnxSvcAggFlowTcpPkt			Counter64, -- total 
    jnxSvcAggFlowTcpPktErr		Counter64,
    jnxSvcAggFlowTcpPktErrBadFlow	Counter64,
    jnxSvcAggFlowTcpByte		Counter64, -- total
    jnxSvcAggFlowTcpByteErr	Counter64,
    
    -- UDP packets overall statistics

    jnxSvcAggFlowUdpPkt			Counter64, -- total 
    jnxSvcAggFlowUdpPktErr		Counter64,
    jnxSvcAggFlowUdpPktErrBadFlow	Counter64, 
    jnxSvcAggFlowUdpByte		Counter64, -- total
    jnxSvcAggFlowUdpByteErr	Counter64
}

jnxSvcAggFlow		OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of flows of any kind in the flow table."
    ::= { jnxSvcFlowTableAggStatsEntry 1 }
    
jnxSvcAggFlowMaximum	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Maximum number of flows of any kind in the flow table
    	 (high water mark)."
    ::= { jnxSvcFlowTableAggStatsEntry 2 }
    
jnxSvcAggFlowCreated	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of flows of any kind that have been
    	 created in the flow table."
    ::= { jnxSvcFlowTableAggStatsEntry 3 }
    
jnxSvcAggFlowFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of flows of any kind that have been
    	 freed from the flow table for any reason."
    ::= { jnxSvcFlowTableAggStatsEntry 4 }
    
jnxSvcAggFlowIdleFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of flows of any kind that have been
    	 freed from the flow table by idle flow detection."
    ::= { jnxSvcFlowTableAggStatsEntry 5 }
    
jnxSvcAggFlowTcp	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP flows in the flow table."
    ::= { jnxSvcFlowTableAggStatsEntry 6 }
    
jnxSvcAggFlowTcpMaximum	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Maximum number of TCP flows in the flow table
    	 (high water mark)."
    ::= { jnxSvcFlowTableAggStatsEntry 7 }
    
jnxSvcAggFlowTcpCreated	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP flows that have been
    	 created in the flow table."
    ::= { jnxSvcFlowTableAggStatsEntry 8 }
    
jnxSvcAggFlowTcpFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP flows that have been
    	 freed from the flow table for any reason."
    ::= { jnxSvcFlowTableAggStatsEntry 9 }
    
jnxSvcAggFlowTcpIdleFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP flows that have been
    	 freed from the flow table by idle flow detection."
    ::= { jnxSvcFlowTableAggStatsEntry 10 }
    
jnxSvcAggFlowUdp	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of UDP flows in the flow table."
    ::= { jnxSvcFlowTableAggStatsEntry 11 }
    
jnxSvcAggFlowUdpMaximum	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Maximum number of TCP flows in the flow table
    	 (high water mark)."
    ::= { jnxSvcFlowTableAggStatsEntry 12 }
    
jnxSvcAggFlowUdpCreated	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP flows that have been
    	 created in the flow table."
    ::= { jnxSvcFlowTableAggStatsEntry 13 }
    
jnxSvcAggFlowUdpFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of UDP flows that have been
    	 freed from the flow table for any reason."
    ::= { jnxSvcFlowTableAggStatsEntry 14 }
    
jnxSvcAggFlowUdpIdleFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP flows that have been
    	 freed from the flow table by idle flow detection."
    ::= { jnxSvcFlowTableAggStatsEntry 15 }
    
jnxSvcAggFlowPkt	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of packets processed by all flows."
    ::= { jnxSvcFlowTableAggStatsEntry 16 }
    
jnxSvcAggFlowPktErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of packets 
    	 found to be in invalid  in processing by all flows."
    ::= { jnxSvcFlowTableAggStatsEntry 17 }
    
jnxSvcAggFlowByte	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for packets processed by all flows."
    ::= { jnxSvcFlowTableAggStatsEntry 18 }
    
jnxSvcAggFlowByteErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for packets
    	found to be in invalid in processing by all flows."
    ::= { jnxSvcFlowTableAggStatsEntry 19 }
    
jnxSvcAggFlowIcmpPkt	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of ICMP packets processed."
    ::= { jnxSvcFlowTableAggStatsEntry 20 }
    
jnxSvcAggFlowIcmpPktErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of ICMP packets 
    	found to be in invalid for any reason."
    ::= { jnxSvcFlowTableAggStatsEntry 21 }
    
jnxSvcAggFlowIcmpPktErrBadFlow	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of ICMP packets 
    	 found to be in invalid because the flow was invalid."
    ::= { jnxSvcFlowTableAggStatsEntry 22 }
    
jnxSvcAggFlowIcmpByte	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for all ICMP packets processed."
    ::= { jnxSvcFlowTableAggStatsEntry 23 }
    
jnxSvcAggFlowIcmpByteErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for all 
    	ICMP packets found to be in invalid."
    ::= { jnxSvcFlowTableAggStatsEntry 24 }
    
jnxSvcAggFlowTcpPkt	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP packets processed."
    ::= { jnxSvcFlowTableAggStatsEntry 25 }
    
jnxSvcAggFlowTcpPktErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP packets found to be in invalid 
    	 for any reason."
    ::= { jnxSvcFlowTableAggStatsEntry 26 }
    
jnxSvcAggFlowTcpPktErrBadFlow	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of TCP packets found to be in invalid 
    	 because the flow was invalid."
    ::= { jnxSvcFlowTableAggStatsEntry 27 }
    
jnxSvcAggFlowTcpByte	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for all TCP packets processed."
    ::= { jnxSvcFlowTableAggStatsEntry 28 }
    
jnxSvcAggFlowTcpByteErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for all TCP packets found to be in invalid"
    ::= { jnxSvcFlowTableAggStatsEntry 29 }
    
jnxSvcAggFlowUdpPkt	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of UDP packets processed."
    ::= { jnxSvcFlowTableAggStatsEntry 30 }
    
jnxSvcAggFlowUdpPktErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of UDP packets found to be in invalid 
    	 for any reason."
    ::= { jnxSvcFlowTableAggStatsEntry 31 }
    
jnxSvcAggFlowUdpPktErrBadFlow	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of UDP packets 
    	 found to be in invalid because the flow
    	 was invalid."
    ::= { jnxSvcFlowTableAggStatsEntry 32 }
    
jnxSvcAggFlowUdpByte	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for all UDP packets processed."
    ::= { jnxSvcFlowTableAggStatsEntry 33 }
    
jnxSvcAggFlowUdpByteErr	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
    	"Total number of bytes for all TCP packets
    	found to be in invalid."
    ::= { jnxSvcFlowTableAggStatsEntry 34 }


--
-- Service Identification Service Statistics
--
-- Service Indentification is supported only by the GGSN-I 
-- PIC.
--


jnxSvcServIdTable		OBJECT-TYPE
    SYNTAX       		SEQUENCE OF JnxSvcServIdTableEntry
    MAX-ACCESS   		not-accessible
    STATUS       		current
    DESCRIPTION
	"Information about the service-identification service for
	 the service PIC interface."
    ::= { jnxServicesInfoMib 2 }

jnxSvcServIdTableEntry	OBJECT-TYPE
    SYNTAX			JnxSvcServIdTableEntry
    MAX-ACCESS			not-accessible
    STATUS			current
    DESCRIPTION
	"An entry containing aggregate Service Identification service
	 information applicable to particular service pic interfaces."
    INDEX   		{ ifIndex }
    ::= { jnxSvcServIdTable 1 }

JnxSvcServIdTableEntry ::= SEQUENCE {
    -- packet statistics for the service
    jnxSvcServIdPkt				Counter64,
    jnxSvcServIdByte				Counter64,
    jnxSvcServIdErrPkt			Counter64,
    jnxSvcServIdErrByte			Counter64,
   
    -- header examination functionality statistics
    jnxSvcServIdHeadExPkt			Counter64,
    jnxSvcServIdHeadExByte			Counter64,
    jnxSvcServIdHeadExFlow			Counter64,
    jnxSvcServIdHeadExFlowMtch			Counter64,
    jnxSvcServIdHeadExProtoReq			Counter64,
    jnxSvcServIdHeadExHttpProtoReq		Counter64,
    jnxSvcServIdHeadExWapProtoReq		Counter64,

    -- protocol identification and URI extraction 
    jnxSvcServIdProtFlow			Gauge32,
    jnxSvcServIdProtInsPkt			Counter64,
    jnxSvcServIdProtInsByte			Counter64,
    jnxSvcServIdProtInsFlowInsp			Counter64,
    jnxSvcServIdProtInsFlowProtIdent		Counter64,
    
    -- URI matching
    jnxSvcServIdProtInsHttpUri			Counter64,
    jnxSvcServIdProtInsHttpUriMtch		Counter64,
    jnxSvcServIdProtInsWapUri			Counter64,
    jnxSvcServIdProtInsWapUriMtch		Counter64,

    -- Detailed packet drop-or-in-error information
    jnxSvcServIdPktTcpMalform			Counter64,
    jnxSvcServIdWAPInvalidTxn			Counter64,
    jnxSvcServIdErrWAPTxn			Counter64,
    jnxSvcServIdErrHTTPTxn			Counter64,

    -- Configuration-related Error counters    
    jnxSvcServIdHeadExFailCfgState		Counter64,
    jnxSvcServIdProtInsFailCfgState		Counter64,
    
    -- Transaction counters
    jnxSvcTransactionWapCreated			Counter64,
    jnxSvcTransactionWapMaximum			Gauge32,
    jnxSvcTransactionWapFreed			Counter64,
    jnxSvcTransactionWapIdleFreed		Counter64,
    jnxSvcTransactionHttpCreated		Counter64,
    jnxSvcTransactionHttpMaximum		Gauge32,
    jnxSvcTransactionHttpFreed			Counter64,
    jnxSvcTransactionHttpIdleFreed		Counter64,

    -- Transaction error counters
    jnxSvcServidProtInsUriErrProcess		Counter64,
    jnxSvcServidProtInsUriErrTooLong		Counter64,
    jnxSvcServidProtInsErrParseTx		Counter64,
    jnxSvcServidProtInsUriErrNoRes		Counter64
}

jnxSvcServIdPkt	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Total count for all packets processed by service."
    ::= { jnxSvcServIdTableEntry 1 }

jnxSvcServIdByte	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Total bytes for all packets processed by service."
    ::= { jnxSvcServIdTableEntry 2 }

jnxSvcServIdErrPkt	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Total number of all packets 
	     found to be in invalid by this service 
	     during or as a result of processing."
    ::= { jnxSvcServIdTableEntry 3 }

jnxSvcServIdErrByte	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Total butes for all packets 
	     found to be in invalid by this service 
	     during or as a result of processing."
    ::= { jnxSvcServIdTableEntry 4 }

jnxSvcServIdHeadExPkt	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Packets processed by the service header 
	     examination function.  This is the first 
	     packet for a flow for any service set 
	     specifying a header inspection rule set."
    ::= { jnxSvcServIdTableEntry 5 }

jnxSvcServIdHeadExByte	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Bytes for all packets processed by the service header 
	     examination function.  This is the first 
	     packet for a flow for any service set 
	     specifying a header inspection rule set."
    ::= { jnxSvcServIdTableEntry 6 }

jnxSvcServIdHeadExFlow	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Packets processed by the service header 
	     examination function.  This is the first 
	     packet for a flow for any service set 
	     specifying a header inspection rule set and
	     only includes processing of packets that result
	     in the creation of a flow."
    ::= { jnxSvcServIdTableEntry 7 }

jnxSvcServIdHeadExFlowMtch	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Flows that matched any rule configured for the  
	     header examination function for the service set
	     associated with the flow."
    ::= { jnxSvcServIdTableEntry 8 }

jnxSvcServIdHeadExProtoReq	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Flows identified as requiring protocol 
	     inspection and URI extraction as a result of 
	     the header examination function."
    ::= { jnxSvcServIdTableEntry 13 }

jnxSvcServIdHeadExHttpProtoReq	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Flows identified by header examination function as 
	     potentially requiring HTTP protocol inspection and 
	     URI extraction."
    ::= { jnxSvcServIdTableEntry 14 }

jnxSvcServIdHeadExWapProtoReq	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Flows identified by header examination function as 
	     potentially requiring WAP protocol inspection and 
	     URI extraction."
    ::= { jnxSvcServIdTableEntry 15 }


jnxSvcServIdProtFlow	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Flows currently undergoing protocol inspection and
	     URI extraction. Does not include flows that have been
	     marked as no longer requiring inspection or flows
	     that are in an error state."
    ::= { jnxSvcServIdTableEntry 16 }

jnxSvcServIdProtInsPkt	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Total number of packets processed by protocol 
	     inspection function while attempting to parse a 
	     transaction and extract URIs."
    ::= { jnxSvcServIdTableEntry 17 }

jnxSvcServIdProtInsByte	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Total bytes for all packets processed by protocol 
	     inspection function while attempting to parse a 
	     transaction and extract URIs."
    ::= { jnxSvcServIdTableEntry 18 }


jnxSvcServIdProtInsFlowInsp	OBJECT-TYPE
    SYNTAX 		Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
      	    "Total number of flows that have been inspected or 
      	     are at present being inspected by the protocol 
      	     inspection and identification function."
    ::= { jnxSvcServIdTableEntry 19 }

jnxSvcServIdProtInsFlowProtIdent	OBJECT-TYPE
    SYNTAX 		Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
      	    "Flows for which the protocol inspection and 
      	     identification function has determined the 
      	     protocol in use and begun transaction processing."
    ::= { jnxSvcServIdTableEntry 20 }

jnxSvcServIdProtInsHttpUri	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Number of HTTP transactions that have successfully
	     extracted a URI."
    ::= { jnxSvcServIdTableEntry 24 }

jnxSvcServIdProtInsHttpUriMtch	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Number of HTTP transaction URIs that were matched
	     by a URI rule configured for the active service set."
    ::= { jnxSvcServIdTableEntry 25 }

jnxSvcServIdProtInsWapUri	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Number of WAP transactions that have successfully
	     extracted a URI."
    ::= { jnxSvcServIdTableEntry 26 }

jnxSvcServIdProtInsWapUriMtch	OBJECT-TYPE
    SYNTAX      	Counter64
    MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
	    "Number of WAP transaction URIs that were matched
	     by a URI rule configured for the active service set."
    ::= { jnxSvcServIdTableEntry 27 }

jnxSvcServIdPktTcpMalform	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of TCP packets found to be in invalid due 
	     to being malformed, for an incorrect sequence 
	     number, or other reason."
    ::= { jnxSvcServIdTableEntry 28 }

jnxSvcServIdWAPInvalidTxn	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Numbee of packets found to be in invalid 
	     due to invalid WAP transaction identifier."
    ::= { jnxSvcServIdTableEntry 29 }

jnxSvcServIdErrWAPTxn	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of packets found to be in invalid 
	    because the WAP transaction 
	    or flow was in an error state."
    ::= { jnxSvcServIdTableEntry 30 }

jnxSvcServIdErrHTTPTxn	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of packets found to be in invalid 
	     because the HTTP transaction or flow was 
	     in an error state."
    ::= { jnxSvcServIdTableEntry 31 }

jnxSvcServIdHeadExFailCfgState	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of header inspections that failed due to 
	     internal configuration state."
    ::= { jnxSvcServIdTableEntry 32 }

jnxSvcServIdProtInsFailCfgState	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of URI inspections that failed due to 
	    internal configuration state. "
    ::= { jnxSvcServIdTableEntry 33 }

jnxSvcTransactionWapCreated	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of WAP transaction sessions created."
    ::= { jnxSvcServIdTableEntry 34 }

jnxSvcTransactionWapMaximum	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Peak number of simultaneous of WAP transaction 
	    sessions since start."
    ::= { jnxSvcServIdTableEntry 35 }
	
jnxSvcTransactionWapFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of WAP transaction sessions freed."
    ::= { jnxSvcServIdTableEntry 36 }
	
jnxSvcTransactionWapIdleFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of WAP transaction sessions freed by idle clean-up."
    ::= { jnxSvcServIdTableEntry 37 }
	
jnxSvcTransactionHttpCreated	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of HTTP transaction sessions created."
    ::= { jnxSvcServIdTableEntry 38 }

jnxSvcTransactionHttpMaximum	OBJECT-TYPE
    SYNTAX		Gauge32
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Peak number of simultaneous of HTTP 
	     transaction sessions since start."
    ::= { jnxSvcServIdTableEntry 39 }
	
jnxSvcTransactionHttpFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of WAP transaction sessions freed."
    ::= { jnxSvcServIdTableEntry 40 }
	
jnxSvcTransactionHttpIdleFreed	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of WAP transaction sessions freed by idle clean-up."
    ::= { jnxSvcServIdTableEntry 41 }

jnxSvcServidProtInsUriErrProcess	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of URIs that failed to process due to 
	     internal processing error."
    ::= { jnxSvcServIdTableEntry 42 }

jnxSvcServidProtInsUriErrTooLong	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of URIs that were not processed because 
	     they exceeded the maximum supported URI length."
    ::= { jnxSvcServIdTableEntry 43 }
	
jnxSvcServidProtInsErrParseTx	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of flows which experienced a transaction 
	     parse error or any kind that prevented URI extraction.
	     This does not include length limitations or 
	     processing errors."
    ::= { jnxSvcServIdTableEntry 44 }

jnxSvcServidProtInsUriErrNoRes	OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS		read-only
    STATUS		current
    DESCRIPTION
	    "Number of URIs that were not processed due to lack 
	     of system resources."
    ::= { jnxSvcServIdTableEntry 45 }

--
-- Conformance & compliance (lint hush.. )
--

jnxSvcMIBConformance
         OBJECT IDENTIFIER ::= { jnxServicesInfoMib 20 }
jnxSvcMIBCompliances
         OBJECT IDENTIFIER ::= { jnxSvcMIBConformance 1 }
jnxSvcMIBGroups
         OBJECT IDENTIFIER ::= { jnxSvcMIBConformance 2 }

jnxSvcMIBCompliance		MODULE-COMPLIANCE
   STATUS			current
   DESCRIPTION 
         "Compliance statement for the Juniper enterprise-specific
          service PIC interface service information MIB."
   MODULE
   MANDATORY-GROUPS { 
	jnxSvcFlowTableAggStatsGroup,
	jnxSvcServIdiceGroup
   }
   ::= { jnxSvcMIBCompliances 1 }


jnxSvcFlowTableAggStatsGroup 	OBJECT-GROUP
   OBJECTS { 
	jnxSvcAggFlow,
	jnxSvcAggFlowMaximum,
	jnxSvcAggFlowCreated,
	jnxSvcAggFlowFreed,
	jnxSvcAggFlowIdleFreed,
	jnxSvcAggFlowTcp,
	jnxSvcAggFlowTcpMaximum,
	jnxSvcAggFlowTcpCreated,
	jnxSvcAggFlowTcpFreed,
	jnxSvcAggFlowTcpIdleFreed,
	jnxSvcAggFlowUdp,
	jnxSvcAggFlowUdpMaximum,
	jnxSvcAggFlowUdpCreated,
	jnxSvcAggFlowUdpFreed,
	jnxSvcAggFlowUdpIdleFreed,
	jnxSvcAggFlowPkt,
	jnxSvcAggFlowPktErr,
	jnxSvcAggFlowByte,
	jnxSvcAggFlowByteErr,
	jnxSvcAggFlowIcmpPkt,
	jnxSvcAggFlowIcmpPktErr,
	jnxSvcAggFlowIcmpPktErrBadFlow,
	jnxSvcAggFlowIcmpByte,
	jnxSvcAggFlowIcmpByteErr,
	jnxSvcAggFlowTcpPkt,
	jnxSvcAggFlowTcpPktErr,
	jnxSvcAggFlowTcpPktErrBadFlow,
	jnxSvcAggFlowTcpByte,
	jnxSvcAggFlowTcpByteErr,
	jnxSvcAggFlowUdpPkt,
	jnxSvcAggFlowUdpPktErr,
	jnxSvcAggFlowUdpPktErrBadFlow,
	jnxSvcAggFlowUdpByte,
	jnxSvcAggFlowUdpByteErr
   }
   STATUS current
   DESCRIPTION
         "Basic aggregate statistics for flow table activity."
   ::= { jnxSvcMIBGroups 1 }


jnxSvcServIdiceGroup 	OBJECT-GROUP
   OBJECTS { 
	jnxSvcServIdPkt,
	jnxSvcServIdByte,
	jnxSvcServIdErrPkt,
	jnxSvcServIdErrByte,
	jnxSvcServIdHeadExPkt,
	jnxSvcServIdHeadExByte,
	jnxSvcServIdHeadExFlow,
	jnxSvcServIdHeadExFlowMtch,
	jnxSvcServIdHeadExProtoReq,
	jnxSvcServIdHeadExHttpProtoReq,
	jnxSvcServIdHeadExWapProtoReq,
	jnxSvcServIdProtFlow,
	jnxSvcServIdProtInsPkt,
	jnxSvcServIdProtInsByte,
	jnxSvcServIdProtInsFlowInsp,
	jnxSvcServIdProtInsFlowProtIdent,
	jnxSvcServIdProtInsHttpUri,
	jnxSvcServIdProtInsHttpUriMtch,
	jnxSvcServIdProtInsWapUri,
	jnxSvcServIdProtInsWapUriMtch,
	jnxSvcServIdPktTcpMalform,
	jnxSvcServIdWAPInvalidTxn,
	jnxSvcServIdErrWAPTxn,
	jnxSvcServIdErrHTTPTxn,
	jnxSvcServIdHeadExFailCfgState,
	jnxSvcServIdProtInsFailCfgState,
	jnxSvcTransactionWapCreated,
	jnxSvcTransactionWapMaximum,
	jnxSvcTransactionWapFreed,
	jnxSvcTransactionWapIdleFreed,
	jnxSvcTransactionHttpCreated,
	jnxSvcTransactionHttpMaximum,
	jnxSvcTransactionHttpFreed,
	jnxSvcTransactionHttpIdleFreed,
	jnxSvcServidProtInsUriErrProcess,
	jnxSvcServidProtInsUriErrTooLong,
	jnxSvcServidProtInsErrParseTx,
	jnxSvcServidProtInsUriErrNoRes
   }
   STATUS current
   DESCRIPTION
         "Basic aggregate statistics for the Service Identification 
          service."
   ::= { jnxSvcMIBGroups 2 }



END


