-- *********************************************************************
-- CISCO-UNIFIED-COMPUTING-MEMORY-MIB.my
-- 
-- MIB representation of the Cisco Unified Computing System
-- MEMORY management information model package
-- 
-- Created October 2017 by Charles Bullis
-- 
-- Copyright (c) 2005-2017 Cisco Systems, Inc. All rights reserved.
-- 
-- *********************************************************************

CISCO-UNIFIED-COMPUTING-MEMORY-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    Gauge32,
    TimeTicks,
    Counter64,
    Unsigned32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION,
    RowPointer,
    DateAndTime,
    DisplayString,
    MacAddress,
    TimeInterval,
    TimeStamp,
    TruthValue
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InetAddressIPv4,
    InetAddressIPv6
        FROM INET-ADDRESS-MIB
    ciscoMgmt
        FROM CISCO-SMI
    CiscoNetworkAddress,
    Unsigned64,
    CiscoInetAddressMask,
    CiscoAlarmSeverity,
    TimeIntervalSec
        FROM CISCO-TC
    ciscoUnifiedComputingMIBObjects,
    CucsManagedObjectId,
    CucsManagedObjectDn
        FROM CISCO-UNIFIED-COMPUTING-MIB
    CucsEquipmentOperability,
    CucsEquipmentPowerState,
    CucsEquipmentPresence,
    CucsEquipmentSensorThresholdStatus,
    CucsMemoryAdminState,
    CucsMemoryArrayEnvStatsHistThresholded,
    CucsMemoryArrayEnvStatsThresholded,
    CucsMemoryArrayId,
    CucsMemoryBufferUnitEnvStatsHistThresholded,
    CucsMemoryBufferUnitEnvStatsThresholded,
    CucsMemoryBufferUnitId,
    CucsMemoryErrorCorrection,
    CucsMemoryErrorStatsThresholded,
    CucsMemoryFormFactor,
    CucsMemoryIssues,
    CucsMemoryRuntimeHistThresholded,
    CucsMemoryRuntimeThresholded,
    CucsMemoryRuntimeType,
    CucsMemoryType,
    CucsMemoryUnitEnvStatsHistThresholded,
    CucsMemoryUnitEnvStatsThresholded,
    CucsMemoryUnitId,
    CucsMemoryUnitOperability,
    CucsMemoryVisibility
        FROM CISCO-UNIFIED-COMPUTING-TC-MIB;

cucsMemoryObjects MODULE-IDENTITY
    LAST-UPDATED    "201710060000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
        "Cisco Systems
        Customer Service
        
        Postal: 170 W Tasman Drive
        San Jose, CA  95134
        USA
        
        Tel: +1 800 553 -NETS
        
        E-mail: cs-san@cisco.com, cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "MIB representation of the Cisco Unified Computing System
        MEMORY management information model package"
    ::= { ciscoUnifiedComputingMIBObjects 30 }

cucsMemoryArrayTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryArrayEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:Array managed object table"
    ::= { cucsMemoryObjects 1 }

cucsMemoryArrayEntry OBJECT-TYPE
    SYNTAX           CucsMemoryArrayEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryArrayTable table."
    INDEX { cucsMemoryArrayInstanceId }
    ::= { cucsMemoryArrayTable 1 }

CucsMemoryArrayEntry ::= SEQUENCE {
    cucsMemoryArrayInstanceId                                        CucsManagedObjectId,
    cucsMemoryArrayDn                                                CucsManagedObjectDn,
    cucsMemoryArrayRn                                                SnmpAdminString,
    cucsMemoryArrayCpuId                                             Gauge32,
    cucsMemoryArrayCurrCapacity                                      Gauge32,
    cucsMemoryArrayErrorCorrection                                   CucsMemoryErrorCorrection,
    cucsMemoryArrayId                                                CucsMemoryArrayId,
    cucsMemoryArrayMaxCapacity                                       Gauge32,
    cucsMemoryArrayMaxDevices                                        Gauge32,
    cucsMemoryArrayModel                                             SnmpAdminString,
    cucsMemoryArrayOperState                                         CucsEquipmentOperability,
    cucsMemoryArrayOperability                                       CucsEquipmentOperability,
    cucsMemoryArrayPerf                                              CucsEquipmentSensorThresholdStatus,
    cucsMemoryArrayPopulated                                         Gauge32,
    cucsMemoryArrayPower                                             CucsEquipmentPowerState,
    cucsMemoryArrayPresence                                          CucsEquipmentPresence,
    cucsMemoryArrayRevision                                          SnmpAdminString,
    cucsMemoryArraySerial                                            SnmpAdminString,
    cucsMemoryArrayThermal                                           CucsEquipmentSensorThresholdStatus,
    cucsMemoryArrayVendor                                            SnmpAdminString,
    cucsMemoryArrayVoltage                                           CucsEquipmentSensorThresholdStatus,
    cucsMemoryArrayOperQualifierReason                               SnmpAdminString,
    cucsMemoryArrayLocationDn                                        SnmpAdminString
}

cucsMemoryArrayInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryArrayEntry 1 }

cucsMemoryArrayDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:dn managed object property"
    ::= { cucsMemoryArrayEntry 2 }

cucsMemoryArrayRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:rn managed object property"
    ::= { cucsMemoryArrayEntry 3 }

cucsMemoryArrayCpuId OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:cpuId managed object property"
    ::= { cucsMemoryArrayEntry 4 }

cucsMemoryArrayCurrCapacity OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:currCapacity managed object property"
    ::= { cucsMemoryArrayEntry 5 }

cucsMemoryArrayErrorCorrection OBJECT-TYPE
    SYNTAX       CucsMemoryErrorCorrection
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:errorCorrection managed object property"
    ::= { cucsMemoryArrayEntry 6 }

cucsMemoryArrayId OBJECT-TYPE
    SYNTAX       CucsMemoryArrayId
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:id managed object property"
    ::= { cucsMemoryArrayEntry 7 }

cucsMemoryArrayMaxCapacity OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:maxCapacity managed object property"
    ::= { cucsMemoryArrayEntry 8 }

cucsMemoryArrayMaxDevices OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:maxDevices managed object property"
    ::= { cucsMemoryArrayEntry 9 }

cucsMemoryArrayModel OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:model managed object property"
    ::= { cucsMemoryArrayEntry 10 }

cucsMemoryArrayOperState OBJECT-TYPE
    SYNTAX       CucsEquipmentOperability
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:operState managed object property"
    ::= { cucsMemoryArrayEntry 11 }

cucsMemoryArrayOperability OBJECT-TYPE
    SYNTAX       CucsEquipmentOperability
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:operability managed object property"
    ::= { cucsMemoryArrayEntry 12 }

cucsMemoryArrayPerf OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:perf managed object property"
    ::= { cucsMemoryArrayEntry 13 }

cucsMemoryArrayPopulated OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:populated managed object property"
    ::= { cucsMemoryArrayEntry 14 }

cucsMemoryArrayPower OBJECT-TYPE
    SYNTAX       CucsEquipmentPowerState
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:power managed object property"
    ::= { cucsMemoryArrayEntry 15 }

cucsMemoryArrayPresence OBJECT-TYPE
    SYNTAX       CucsEquipmentPresence
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:presence managed object property"
    ::= { cucsMemoryArrayEntry 16 }

cucsMemoryArrayRevision OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:revision managed object property"
    ::= { cucsMemoryArrayEntry 17 }

cucsMemoryArraySerial OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:serial managed object property"
    ::= { cucsMemoryArrayEntry 18 }

cucsMemoryArrayThermal OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:thermal managed object property"
    ::= { cucsMemoryArrayEntry 19 }

cucsMemoryArrayVendor OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:vendor managed object property"
    ::= { cucsMemoryArrayEntry 20 }

cucsMemoryArrayVoltage OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:voltage managed object property"
    ::= { cucsMemoryArrayEntry 21 }

cucsMemoryArrayOperQualifierReason OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:operQualifierReason managed
        object property"
    ::= { cucsMemoryArrayEntry 22 }

cucsMemoryArrayLocationDn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Array:locationDn managed object property"
    ::= { cucsMemoryArrayEntry 23 }

cucsMemoryArrayEnvStatsTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryArrayEnvStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats managed object table"
    ::= { cucsMemoryObjects 2 }

cucsMemoryArrayEnvStatsEntry OBJECT-TYPE
    SYNTAX           CucsMemoryArrayEnvStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryArrayEnvStatsTable table."
    INDEX { cucsMemoryArrayEnvStatsInstanceId }
    ::= { cucsMemoryArrayEnvStatsTable 1 }

CucsMemoryArrayEnvStatsEntry ::= SEQUENCE {
    cucsMemoryArrayEnvStatsInstanceId                                CucsManagedObjectId,
    cucsMemoryArrayEnvStatsDn                                        CucsManagedObjectDn,
    cucsMemoryArrayEnvStatsRn                                        SnmpAdminString,
    cucsMemoryArrayEnvStatsInputCurrent                              SnmpAdminString,
    cucsMemoryArrayEnvStatsInputCurrentAvg                           SnmpAdminString,
    cucsMemoryArrayEnvStatsInputCurrentMax                           SnmpAdminString,
    cucsMemoryArrayEnvStatsInputCurrentMin                           SnmpAdminString,
    cucsMemoryArrayEnvStatsIntervals                                 Gauge32,
    cucsMemoryArrayEnvStatsSuspect                                   TruthValue,
    cucsMemoryArrayEnvStatsThresholded                               CucsMemoryArrayEnvStatsThresholded,
    cucsMemoryArrayEnvStatsTimeCollected                             DateAndTime,
    cucsMemoryArrayEnvStatsUpdate                                    Gauge32
}

cucsMemoryArrayEnvStatsInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryArrayEnvStatsEntry 1 }

cucsMemoryArrayEnvStatsDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:dn managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 2 }

cucsMemoryArrayEnvStatsRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:rn managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 3 }

cucsMemoryArrayEnvStatsInputCurrent OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:inputCurrent managed
        object property"
    ::= { cucsMemoryArrayEnvStatsEntry 4 }

cucsMemoryArrayEnvStatsInputCurrentAvg OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:inputCurrentAvg
        managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 5 }

cucsMemoryArrayEnvStatsInputCurrentMax OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:inputCurrentMax
        managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 6 }

cucsMemoryArrayEnvStatsInputCurrentMin OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:inputCurrentMin
        managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 7 }

cucsMemoryArrayEnvStatsIntervals OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:intervals managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 8 }

cucsMemoryArrayEnvStatsSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:suspect managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 9 }

cucsMemoryArrayEnvStatsThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryArrayEnvStatsThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:thresholded managed
        object property"
    ::= { cucsMemoryArrayEnvStatsEntry 10 }

cucsMemoryArrayEnvStatsTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:timeCollected managed
        object property"
    ::= { cucsMemoryArrayEnvStatsEntry 11 }

cucsMemoryArrayEnvStatsUpdate OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStats:update managed object property"
    ::= { cucsMemoryArrayEnvStatsEntry 12 }

cucsMemoryArrayEnvStatsHistTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryArrayEnvStatsHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist managed object table"
    ::= { cucsMemoryObjects 3 }

cucsMemoryArrayEnvStatsHistEntry OBJECT-TYPE
    SYNTAX           CucsMemoryArrayEnvStatsHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryArrayEnvStatsHistTable table."
    INDEX { cucsMemoryArrayEnvStatsHistInstanceId }
    ::= { cucsMemoryArrayEnvStatsHistTable 1 }

CucsMemoryArrayEnvStatsHistEntry ::= SEQUENCE {
    cucsMemoryArrayEnvStatsHistInstanceId                            CucsManagedObjectId,
    cucsMemoryArrayEnvStatsHistDn                                    CucsManagedObjectDn,
    cucsMemoryArrayEnvStatsHistRn                                    SnmpAdminString,
    cucsMemoryArrayEnvStatsHistId                                    Unsigned64,
    cucsMemoryArrayEnvStatsHistInputCurrent                          SnmpAdminString,
    cucsMemoryArrayEnvStatsHistInputCurrentAvg                       SnmpAdminString,
    cucsMemoryArrayEnvStatsHistInputCurrentMax                       SnmpAdminString,
    cucsMemoryArrayEnvStatsHistInputCurrentMin                       SnmpAdminString,
    cucsMemoryArrayEnvStatsHistMostRecent                            TruthValue,
    cucsMemoryArrayEnvStatsHistSuspect                               TruthValue,
    cucsMemoryArrayEnvStatsHistThresholded                           CucsMemoryArrayEnvStatsHistThresholded,
    cucsMemoryArrayEnvStatsHistTimeCollected                         DateAndTime
}

cucsMemoryArrayEnvStatsHistInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryArrayEnvStatsHistEntry 1 }

cucsMemoryArrayEnvStatsHistDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:dn managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 2 }

cucsMemoryArrayEnvStatsHistRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:rn managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 3 }

cucsMemoryArrayEnvStatsHistId OBJECT-TYPE
    SYNTAX       Unsigned64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:id managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 4 }

cucsMemoryArrayEnvStatsHistInputCurrent OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:inputCurrent
        managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 5 }

cucsMemoryArrayEnvStatsHistInputCurrentAvg OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:inputCurrentAvg
        managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 6 }

cucsMemoryArrayEnvStatsHistInputCurrentMax OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:inputCurrentMax
        managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 7 }

cucsMemoryArrayEnvStatsHistInputCurrentMin OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:inputCurrentMin
        managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 8 }

cucsMemoryArrayEnvStatsHistMostRecent OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:mostRecent
        managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 9 }

cucsMemoryArrayEnvStatsHistSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:suspect managed
        object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 10 }

cucsMemoryArrayEnvStatsHistThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryArrayEnvStatsHistThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:thresholded
        managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 11 }

cucsMemoryArrayEnvStatsHistTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ArrayEnvStatsHist:timeCollected
        managed object property"
    ::= { cucsMemoryArrayEnvStatsHistEntry 12 }

cucsMemoryBufferUnitTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryBufferUnitEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit managed object table"
    ::= { cucsMemoryObjects 4 }

cucsMemoryBufferUnitEntry OBJECT-TYPE
    SYNTAX           CucsMemoryBufferUnitEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryBufferUnitTable table."
    INDEX { cucsMemoryBufferUnitInstanceId }
    ::= { cucsMemoryBufferUnitTable 1 }

CucsMemoryBufferUnitEntry ::= SEQUENCE {
    cucsMemoryBufferUnitInstanceId                                   CucsManagedObjectId,
    cucsMemoryBufferUnitDn                                           CucsManagedObjectDn,
    cucsMemoryBufferUnitRn                                           SnmpAdminString,
    cucsMemoryBufferUnitId                                           CucsMemoryBufferUnitId,
    cucsMemoryBufferUnitModel                                        SnmpAdminString,
    cucsMemoryBufferUnitOperState                                    CucsEquipmentOperability,
    cucsMemoryBufferUnitOperability                                  CucsEquipmentOperability,
    cucsMemoryBufferUnitPerf                                         CucsEquipmentSensorThresholdStatus,
    cucsMemoryBufferUnitPower                                        CucsEquipmentPowerState,
    cucsMemoryBufferUnitPresence                                     CucsEquipmentPresence,
    cucsMemoryBufferUnitRevision                                     SnmpAdminString,
    cucsMemoryBufferUnitSerial                                       SnmpAdminString,
    cucsMemoryBufferUnitThermal                                      CucsEquipmentSensorThresholdStatus,
    cucsMemoryBufferUnitVendor                                       SnmpAdminString,
    cucsMemoryBufferUnitVoltage                                      CucsEquipmentSensorThresholdStatus,
    cucsMemoryBufferUnitOperQualifierReason                          SnmpAdminString,
    cucsMemoryBufferUnitLocationDn                                   SnmpAdminString
}

cucsMemoryBufferUnitInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryBufferUnitEntry 1 }

cucsMemoryBufferUnitDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:dn managed object property"
    ::= { cucsMemoryBufferUnitEntry 2 }

cucsMemoryBufferUnitRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:rn managed object property"
    ::= { cucsMemoryBufferUnitEntry 3 }

cucsMemoryBufferUnitId OBJECT-TYPE
    SYNTAX       CucsMemoryBufferUnitId
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:id managed object property"
    ::= { cucsMemoryBufferUnitEntry 4 }

cucsMemoryBufferUnitModel OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:model managed object property"
    ::= { cucsMemoryBufferUnitEntry 5 }

cucsMemoryBufferUnitOperState OBJECT-TYPE
    SYNTAX       CucsEquipmentOperability
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:operState managed object property"
    ::= { cucsMemoryBufferUnitEntry 6 }

cucsMemoryBufferUnitOperability OBJECT-TYPE
    SYNTAX       CucsEquipmentOperability
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:operability managed object property"
    ::= { cucsMemoryBufferUnitEntry 7 }

cucsMemoryBufferUnitPerf OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:perf managed object property"
    ::= { cucsMemoryBufferUnitEntry 8 }

cucsMemoryBufferUnitPower OBJECT-TYPE
    SYNTAX       CucsEquipmentPowerState
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:power managed object property"
    ::= { cucsMemoryBufferUnitEntry 9 }

cucsMemoryBufferUnitPresence OBJECT-TYPE
    SYNTAX       CucsEquipmentPresence
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:presence managed object property"
    ::= { cucsMemoryBufferUnitEntry 10 }

cucsMemoryBufferUnitRevision OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:revision managed object property"
    ::= { cucsMemoryBufferUnitEntry 11 }

cucsMemoryBufferUnitSerial OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:serial managed object property"
    ::= { cucsMemoryBufferUnitEntry 12 }

cucsMemoryBufferUnitThermal OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:thermal managed object property"
    ::= { cucsMemoryBufferUnitEntry 13 }

cucsMemoryBufferUnitVendor OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:vendor managed object property"
    ::= { cucsMemoryBufferUnitEntry 14 }

cucsMemoryBufferUnitVoltage OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:voltage managed object property"
    ::= { cucsMemoryBufferUnitEntry 15 }

cucsMemoryBufferUnitOperQualifierReason OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:operQualifierReason
        managed object property"
    ::= { cucsMemoryBufferUnitEntry 16 }

cucsMemoryBufferUnitLocationDn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnit:locationDn managed object property"
    ::= { cucsMemoryBufferUnitEntry 17 }

cucsMemoryBufferUnitEnvStatsTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryBufferUnitEnvStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats managed object table"
    ::= { cucsMemoryObjects 5 }

cucsMemoryBufferUnitEnvStatsEntry OBJECT-TYPE
    SYNTAX           CucsMemoryBufferUnitEnvStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryBufferUnitEnvStatsTable table."
    INDEX { cucsMemoryBufferUnitEnvStatsInstanceId }
    ::= { cucsMemoryBufferUnitEnvStatsTable 1 }

CucsMemoryBufferUnitEnvStatsEntry ::= SEQUENCE {
    cucsMemoryBufferUnitEnvStatsInstanceId                           CucsManagedObjectId,
    cucsMemoryBufferUnitEnvStatsDn                                   CucsManagedObjectDn,
    cucsMemoryBufferUnitEnvStatsRn                                   SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsIntervals                            Gauge32,
    cucsMemoryBufferUnitEnvStatsSuspect                              TruthValue,
    cucsMemoryBufferUnitEnvStatsTemperature                          SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsTemperatureAvg                       SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsTemperatureMax                       SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsTemperatureMin                       SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsThresholded                          CucsMemoryBufferUnitEnvStatsThresholded,
    cucsMemoryBufferUnitEnvStatsTimeCollected                        DateAndTime,
    cucsMemoryBufferUnitEnvStatsUpdate                               Gauge32
}

cucsMemoryBufferUnitEnvStatsInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryBufferUnitEnvStatsEntry 1 }

cucsMemoryBufferUnitEnvStatsDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:dn managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 2 }

cucsMemoryBufferUnitEnvStatsRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:rn managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 3 }

cucsMemoryBufferUnitEnvStatsIntervals OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:intervals
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 4 }

cucsMemoryBufferUnitEnvStatsSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:suspect managed
        object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 5 }

cucsMemoryBufferUnitEnvStatsTemperature OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:temperature
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 6 }

cucsMemoryBufferUnitEnvStatsTemperatureAvg OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:temperatureAvg
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 7 }

cucsMemoryBufferUnitEnvStatsTemperatureMax OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:temperatureMax
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 8 }

cucsMemoryBufferUnitEnvStatsTemperatureMin OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:temperatureMin
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 9 }

cucsMemoryBufferUnitEnvStatsThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryBufferUnitEnvStatsThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:thresholded
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 10 }

cucsMemoryBufferUnitEnvStatsTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:timeCollected
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 11 }

cucsMemoryBufferUnitEnvStatsUpdate OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStats:update managed
        object property"
    ::= { cucsMemoryBufferUnitEnvStatsEntry 12 }

cucsMemoryBufferUnitEnvStatsHistTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryBufferUnitEnvStatsHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist managed object table"
    ::= { cucsMemoryObjects 6 }

cucsMemoryBufferUnitEnvStatsHistEntry OBJECT-TYPE
    SYNTAX           CucsMemoryBufferUnitEnvStatsHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryBufferUnitEnvStatsHistTable table."
    INDEX { cucsMemoryBufferUnitEnvStatsHistInstanceId }
    ::= { cucsMemoryBufferUnitEnvStatsHistTable 1 }

CucsMemoryBufferUnitEnvStatsHistEntry ::= SEQUENCE {
    cucsMemoryBufferUnitEnvStatsHistInstanceId                       CucsManagedObjectId,
    cucsMemoryBufferUnitEnvStatsHistDn                               CucsManagedObjectDn,
    cucsMemoryBufferUnitEnvStatsHistRn                               SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsHistId                               Unsigned64,
    cucsMemoryBufferUnitEnvStatsHistMostRecent                       TruthValue,
    cucsMemoryBufferUnitEnvStatsHistSuspect                          TruthValue,
    cucsMemoryBufferUnitEnvStatsHistTemperature                      SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsHistTemperatureAvg                   SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsHistTemperatureMax                   SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsHistTemperatureMin                   SnmpAdminString,
    cucsMemoryBufferUnitEnvStatsHistThresholded                      CucsMemoryBufferUnitEnvStatsHistThresholded,
    cucsMemoryBufferUnitEnvStatsHistTimeCollected                    DateAndTime
}

cucsMemoryBufferUnitEnvStatsHistInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 1 }

cucsMemoryBufferUnitEnvStatsHistDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:dn managed
        object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 2 }

cucsMemoryBufferUnitEnvStatsHistRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:rn managed
        object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 3 }

cucsMemoryBufferUnitEnvStatsHistId OBJECT-TYPE
    SYNTAX       Unsigned64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:id managed
        object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 4 }

cucsMemoryBufferUnitEnvStatsHistMostRecent OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:mostRecent
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 5 }

cucsMemoryBufferUnitEnvStatsHistSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:suspect
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 6 }

cucsMemoryBufferUnitEnvStatsHistTemperature OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:temperature
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 7 }

cucsMemoryBufferUnitEnvStatsHistTemperatureAvg OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:temperatureAvg
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 8 }

cucsMemoryBufferUnitEnvStatsHistTemperatureMax OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:temperatureMax
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 9 }

cucsMemoryBufferUnitEnvStatsHistTemperatureMin OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:temperatureMin
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 10 }

cucsMemoryBufferUnitEnvStatsHistThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryBufferUnitEnvStatsHistThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:thresholded
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 11 }

cucsMemoryBufferUnitEnvStatsHistTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:BufferUnitEnvStatsHist:timeCollected
        managed object property"
    ::= { cucsMemoryBufferUnitEnvStatsHistEntry 12 }

cucsMemoryErrorStatsTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryErrorStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats managed object table"
    ::= { cucsMemoryObjects 7 }

cucsMemoryErrorStatsEntry OBJECT-TYPE
    SYNTAX           CucsMemoryErrorStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryErrorStatsTable table."
    INDEX { cucsMemoryErrorStatsInstanceId }
    ::= { cucsMemoryErrorStatsTable 1 }

CucsMemoryErrorStatsEntry ::= SEQUENCE {
    cucsMemoryErrorStatsInstanceId                                   CucsManagedObjectId,
    cucsMemoryErrorStatsDn                                           CucsManagedObjectDn,
    cucsMemoryErrorStatsRn                                           SnmpAdminString,
    cucsMemoryErrorStatsAddressParityErrors                          Counter32,
    cucsMemoryErrorStatsAddressParityErrors15Min                     Gauge32,
    cucsMemoryErrorStatsAddressParityErrors15MinH                    Gauge32,
    cucsMemoryErrorStatsAddressParityErrors1Day                      Gauge32,
    cucsMemoryErrorStatsAddressParityErrors1DayH                     Gauge32,
    cucsMemoryErrorStatsAddressParityErrors1Hour                     Gauge32,
    cucsMemoryErrorStatsAddressParityErrors1HourH                    Gauge32,
    cucsMemoryErrorStatsAddressParityErrors1Week                     Gauge32,
    cucsMemoryErrorStatsAddressParityErrors1WeekH                    Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors                            Counter32,
    cucsMemoryErrorStatsEccMultibitErrors15Min                       Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors15MinH                      Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors1Day                        Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors1DayH                       Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors1Hour                       Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors1HourH                      Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors1Week                       Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors1WeekH                      Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors                           Counter32,
    cucsMemoryErrorStatsEccSinglebitErrors15Min                      Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors15MinH                     Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors1Day                       Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors1DayH                      Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors1Hour                      Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors1HourH                     Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors1Week                      Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors1WeekH                     Gauge32,
    cucsMemoryErrorStatsIntervals                                    Gauge32,
    cucsMemoryErrorStatsMismatchErrors                               Counter32,
    cucsMemoryErrorStatsMismatchErrors15Min                          Gauge32,
    cucsMemoryErrorStatsMismatchErrors15MinH                         Gauge32,
    cucsMemoryErrorStatsMismatchErrors1Day                           Gauge32,
    cucsMemoryErrorStatsMismatchErrors1DayH                          Gauge32,
    cucsMemoryErrorStatsMismatchErrors1Hour                          Gauge32,
    cucsMemoryErrorStatsMismatchErrors1HourH                         Gauge32,
    cucsMemoryErrorStatsMismatchErrors1Week                          Gauge32,
    cucsMemoryErrorStatsMismatchErrors1WeekH                         Gauge32,
    cucsMemoryErrorStatsSuspect                                      TruthValue,
    cucsMemoryErrorStatsThresholded                                  CucsMemoryErrorStatsThresholded,
    cucsMemoryErrorStatsTimeCollected                                DateAndTime,
    cucsMemoryErrorStatsUpdate                                       Gauge32,
    cucsMemoryErrorStatsAddressParityErrors2Weeks                    Gauge32,
    cucsMemoryErrorStatsAddressParityErrors2WeeksH                   Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors2Weeks                      Gauge32,
    cucsMemoryErrorStatsEccMultibitErrors2WeeksH                     Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors2Weeks                     Gauge32,
    cucsMemoryErrorStatsEccSinglebitErrors2WeeksH                    Gauge32,
    cucsMemoryErrorStatsMismatchErrors2Weeks                         Gauge32,
    cucsMemoryErrorStatsMismatchErrors2WeeksH                        Gauge32
}

cucsMemoryErrorStatsInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryErrorStatsEntry 1 }

cucsMemoryErrorStatsDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:dn managed object property"
    ::= { cucsMemoryErrorStatsEntry 2 }

cucsMemoryErrorStatsRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:rn managed object property"
    ::= { cucsMemoryErrorStatsEntry 3 }

cucsMemoryErrorStatsAddressParityErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 4 }

cucsMemoryErrorStatsAddressParityErrors15Min OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors15Min
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 5 }

cucsMemoryErrorStatsAddressParityErrors15MinH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors15MinH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 6 }

cucsMemoryErrorStatsAddressParityErrors1Day OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors1Day
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 7 }

cucsMemoryErrorStatsAddressParityErrors1DayH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors1DayH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 8 }

cucsMemoryErrorStatsAddressParityErrors1Hour OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors1Hour
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 9 }

cucsMemoryErrorStatsAddressParityErrors1HourH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors1HourH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 10 }

cucsMemoryErrorStatsAddressParityErrors1Week OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors1Week
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 11 }

cucsMemoryErrorStatsAddressParityErrors1WeekH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors1WeekH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 12 }

cucsMemoryErrorStatsEccMultibitErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 13 }

cucsMemoryErrorStatsEccMultibitErrors15Min OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors15Min
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 14 }

cucsMemoryErrorStatsEccMultibitErrors15MinH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors15MinH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 15 }

cucsMemoryErrorStatsEccMultibitErrors1Day OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors1Day
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 16 }

cucsMemoryErrorStatsEccMultibitErrors1DayH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors1DayH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 17 }

cucsMemoryErrorStatsEccMultibitErrors1Hour OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors1Hour
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 18 }

cucsMemoryErrorStatsEccMultibitErrors1HourH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors1HourH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 19 }

cucsMemoryErrorStatsEccMultibitErrors1Week OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors1Week
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 20 }

cucsMemoryErrorStatsEccMultibitErrors1WeekH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors1WeekH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 21 }

cucsMemoryErrorStatsEccSinglebitErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 22 }

cucsMemoryErrorStatsEccSinglebitErrors15Min OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors15Min
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 23 }

cucsMemoryErrorStatsEccSinglebitErrors15MinH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors15MinH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 24 }

cucsMemoryErrorStatsEccSinglebitErrors1Day OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors1Day
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 25 }

cucsMemoryErrorStatsEccSinglebitErrors1DayH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors1DayH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 26 }

cucsMemoryErrorStatsEccSinglebitErrors1Hour OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors1Hour
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 27 }

cucsMemoryErrorStatsEccSinglebitErrors1HourH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors1HourH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 28 }

cucsMemoryErrorStatsEccSinglebitErrors1Week OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors1Week
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 29 }

cucsMemoryErrorStatsEccSinglebitErrors1WeekH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors1WeekH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 30 }

cucsMemoryErrorStatsIntervals OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:intervals managed object property"
    ::= { cucsMemoryErrorStatsEntry 31 }

cucsMemoryErrorStatsMismatchErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors managed
        object property"
    ::= { cucsMemoryErrorStatsEntry 32 }

cucsMemoryErrorStatsMismatchErrors15Min OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors15Min
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 33 }

cucsMemoryErrorStatsMismatchErrors15MinH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors15MinH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 34 }

cucsMemoryErrorStatsMismatchErrors1Day OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors1Day
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 35 }

cucsMemoryErrorStatsMismatchErrors1DayH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors1DayH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 36 }

cucsMemoryErrorStatsMismatchErrors1Hour OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors1Hour
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 37 }

cucsMemoryErrorStatsMismatchErrors1HourH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors1HourH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 38 }

cucsMemoryErrorStatsMismatchErrors1Week OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors1Week
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 39 }

cucsMemoryErrorStatsMismatchErrors1WeekH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors1WeekH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 40 }

cucsMemoryErrorStatsSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:suspect managed object property"
    ::= { cucsMemoryErrorStatsEntry 41 }

cucsMemoryErrorStatsThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryErrorStatsThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:thresholded managed object property"
    ::= { cucsMemoryErrorStatsEntry 42 }

cucsMemoryErrorStatsTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:timeCollected managed
        object property"
    ::= { cucsMemoryErrorStatsEntry 43 }

cucsMemoryErrorStatsUpdate OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:update managed object property"
    ::= { cucsMemoryErrorStatsEntry 44 }

cucsMemoryErrorStatsAddressParityErrors2Weeks OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors2Weeks
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 45 }

cucsMemoryErrorStatsAddressParityErrors2WeeksH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:addressParityErrors2WeeksH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 46 }

cucsMemoryErrorStatsEccMultibitErrors2Weeks OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors2Weeks
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 47 }

cucsMemoryErrorStatsEccMultibitErrors2WeeksH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccMultibitErrors2WeeksH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 48 }

cucsMemoryErrorStatsEccSinglebitErrors2Weeks OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors2Weeks
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 49 }

cucsMemoryErrorStatsEccSinglebitErrors2WeeksH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:eccSinglebitErrors2WeeksH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 50 }

cucsMemoryErrorStatsMismatchErrors2Weeks OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors2Weeks
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 51 }

cucsMemoryErrorStatsMismatchErrors2WeeksH OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:ErrorStats:mismatchErrors2WeeksH
        managed object property"
    ::= { cucsMemoryErrorStatsEntry 52 }

cucsMemoryQualTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryQualEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:Qual managed object table"
    ::= { cucsMemoryObjects 8 }

cucsMemoryQualEntry OBJECT-TYPE
    SYNTAX           CucsMemoryQualEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryQualTable table."
    INDEX { cucsMemoryQualInstanceId }
    ::= { cucsMemoryQualTable 1 }

CucsMemoryQualEntry ::= SEQUENCE {
    cucsMemoryQualInstanceId                                         CucsManagedObjectId,
    cucsMemoryQualDn                                                 CucsManagedObjectDn,
    cucsMemoryQualRn                                                 SnmpAdminString,
    cucsMemoryQualClock                                              Gauge32,
    cucsMemoryQualLatency                                            SnmpAdminString,
    cucsMemoryQualMaxCap                                             Gauge32,
    cucsMemoryQualMinCap                                             Gauge32,
    cucsMemoryQualSpeed                                              Gauge32,
    cucsMemoryQualUnits                                              Gauge32,
    cucsMemoryQualWidth                                              Gauge32
}

cucsMemoryQualInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryQualEntry 1 }

cucsMemoryQualDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:dn managed object property"
    ::= { cucsMemoryQualEntry 2 }

cucsMemoryQualRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:rn managed object property"
    ::= { cucsMemoryQualEntry 3 }

cucsMemoryQualClock OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:clock managed object property"
    ::= { cucsMemoryQualEntry 4 }

cucsMemoryQualLatency OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:latency managed object property"
    ::= { cucsMemoryQualEntry 5 }

cucsMemoryQualMaxCap OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:maxCap managed object property"
    ::= { cucsMemoryQualEntry 6 }

cucsMemoryQualMinCap OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:minCap managed object property"
    ::= { cucsMemoryQualEntry 7 }

cucsMemoryQualSpeed OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:speed managed object property"
    ::= { cucsMemoryQualEntry 8 }

cucsMemoryQualUnits OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:units managed object property"
    ::= { cucsMemoryQualEntry 9 }

cucsMemoryQualWidth OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Qual:width managed object property"
    ::= { cucsMemoryQualEntry 10 }

cucsMemoryRuntimeTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryRuntimeEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:Runtime managed object table"
    ::= { cucsMemoryObjects 9 }

cucsMemoryRuntimeEntry OBJECT-TYPE
    SYNTAX           CucsMemoryRuntimeEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryRuntimeTable table."
    INDEX { cucsMemoryRuntimeInstanceId }
    ::= { cucsMemoryRuntimeTable 1 }

CucsMemoryRuntimeEntry ::= SEQUENCE {
    cucsMemoryRuntimeInstanceId                                      CucsManagedObjectId,
    cucsMemoryRuntimeDn                                              CucsManagedObjectDn,
    cucsMemoryRuntimeRn                                              SnmpAdminString,
    cucsMemoryRuntimeAvailable                                       Gauge32,
    cucsMemoryRuntimeAvailableAvg                                    Gauge32,
    cucsMemoryRuntimeAvailableMax                                    Gauge32,
    cucsMemoryRuntimeAvailableMin                                    Gauge32,
    cucsMemoryRuntimeCached                                          Gauge32,
    cucsMemoryRuntimeCachedAvg                                       Gauge32,
    cucsMemoryRuntimeCachedMax                                       Gauge32,
    cucsMemoryRuntimeCachedMin                                       Gauge32,
    cucsMemoryRuntimeIntervals                                       Gauge32,
    cucsMemoryRuntimeSuspect                                         TruthValue,
    cucsMemoryRuntimeThresholded                                     CucsMemoryRuntimeThresholded,
    cucsMemoryRuntimeTimeCollected                                   DateAndTime,
    cucsMemoryRuntimeTotal                                           Gauge32,
    cucsMemoryRuntimeTotalAvg                                        Gauge32,
    cucsMemoryRuntimeTotalMax                                        Gauge32,
    cucsMemoryRuntimeTotalMin                                        Gauge32,
    cucsMemoryRuntimeType                                            CucsMemoryRuntimeType,
    cucsMemoryRuntimeUpdate                                          Gauge32
}

cucsMemoryRuntimeInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryRuntimeEntry 1 }

cucsMemoryRuntimeDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:dn managed object property"
    ::= { cucsMemoryRuntimeEntry 2 }

cucsMemoryRuntimeRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:rn managed object property"
    ::= { cucsMemoryRuntimeEntry 3 }

cucsMemoryRuntimeAvailable OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:available managed object property"
    ::= { cucsMemoryRuntimeEntry 4 }

cucsMemoryRuntimeAvailableAvg OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:availableAvg managed object property"
    ::= { cucsMemoryRuntimeEntry 5 }

cucsMemoryRuntimeAvailableMax OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:availableMax managed object property"
    ::= { cucsMemoryRuntimeEntry 6 }

cucsMemoryRuntimeAvailableMin OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:availableMin managed object property"
    ::= { cucsMemoryRuntimeEntry 7 }

cucsMemoryRuntimeCached OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:cached managed object property"
    ::= { cucsMemoryRuntimeEntry 8 }

cucsMemoryRuntimeCachedAvg OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:cachedAvg managed object property"
    ::= { cucsMemoryRuntimeEntry 9 }

cucsMemoryRuntimeCachedMax OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:cachedMax managed object property"
    ::= { cucsMemoryRuntimeEntry 10 }

cucsMemoryRuntimeCachedMin OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:cachedMin managed object property"
    ::= { cucsMemoryRuntimeEntry 11 }

cucsMemoryRuntimeIntervals OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:intervals managed object property"
    ::= { cucsMemoryRuntimeEntry 12 }

cucsMemoryRuntimeSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:suspect managed object property"
    ::= { cucsMemoryRuntimeEntry 13 }

cucsMemoryRuntimeThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryRuntimeThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:thresholded managed object property"
    ::= { cucsMemoryRuntimeEntry 14 }

cucsMemoryRuntimeTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:timeCollected managed object property"
    ::= { cucsMemoryRuntimeEntry 15 }

cucsMemoryRuntimeTotal OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:total managed object property"
    ::= { cucsMemoryRuntimeEntry 16 }

cucsMemoryRuntimeTotalAvg OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:totalAvg managed object property"
    ::= { cucsMemoryRuntimeEntry 17 }

cucsMemoryRuntimeTotalMax OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:totalMax managed object property"
    ::= { cucsMemoryRuntimeEntry 18 }

cucsMemoryRuntimeTotalMin OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:totalMin managed object property"
    ::= { cucsMemoryRuntimeEntry 19 }

cucsMemoryRuntimeType OBJECT-TYPE
    SYNTAX       CucsMemoryRuntimeType
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:type managed object property"
    ::= { cucsMemoryRuntimeEntry 20 }

cucsMemoryRuntimeUpdate OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Runtime:update managed object property"
    ::= { cucsMemoryRuntimeEntry 21 }

cucsMemoryRuntimeHistTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryRuntimeHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist managed object table"
    ::= { cucsMemoryObjects 10 }

cucsMemoryRuntimeHistEntry OBJECT-TYPE
    SYNTAX           CucsMemoryRuntimeHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryRuntimeHistTable table."
    INDEX { cucsMemoryRuntimeHistInstanceId }
    ::= { cucsMemoryRuntimeHistTable 1 }

CucsMemoryRuntimeHistEntry ::= SEQUENCE {
    cucsMemoryRuntimeHistInstanceId                                  CucsManagedObjectId,
    cucsMemoryRuntimeHistDn                                          CucsManagedObjectDn,
    cucsMemoryRuntimeHistRn                                          SnmpAdminString,
    cucsMemoryRuntimeHistAvailable                                   Gauge32,
    cucsMemoryRuntimeHistAvailableAvg                                Gauge32,
    cucsMemoryRuntimeHistAvailableMax                                Gauge32,
    cucsMemoryRuntimeHistAvailableMin                                Gauge32,
    cucsMemoryRuntimeHistCached                                      Gauge32,
    cucsMemoryRuntimeHistCachedAvg                                   Gauge32,
    cucsMemoryRuntimeHistCachedMax                                   Gauge32,
    cucsMemoryRuntimeHistCachedMin                                   Gauge32,
    cucsMemoryRuntimeHistId                                          Unsigned64,
    cucsMemoryRuntimeHistMostRecent                                  TruthValue,
    cucsMemoryRuntimeHistSuspect                                     TruthValue,
    cucsMemoryRuntimeHistThresholded                                 CucsMemoryRuntimeHistThresholded,
    cucsMemoryRuntimeHistTimeCollected                               DateAndTime,
    cucsMemoryRuntimeHistTotal                                       Gauge32,
    cucsMemoryRuntimeHistTotalAvg                                    Gauge32,
    cucsMemoryRuntimeHistTotalMax                                    Gauge32,
    cucsMemoryRuntimeHistTotalMin                                    Gauge32
}

cucsMemoryRuntimeHistInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryRuntimeHistEntry 1 }

cucsMemoryRuntimeHistDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:dn managed object property"
    ::= { cucsMemoryRuntimeHistEntry 2 }

cucsMemoryRuntimeHistRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:rn managed object property"
    ::= { cucsMemoryRuntimeHistEntry 3 }

cucsMemoryRuntimeHistAvailable OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:available managed object property"
    ::= { cucsMemoryRuntimeHistEntry 4 }

cucsMemoryRuntimeHistAvailableAvg OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:availableAvg managed
        object property"
    ::= { cucsMemoryRuntimeHistEntry 5 }

cucsMemoryRuntimeHistAvailableMax OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:availableMax managed
        object property"
    ::= { cucsMemoryRuntimeHistEntry 6 }

cucsMemoryRuntimeHistAvailableMin OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:availableMin managed
        object property"
    ::= { cucsMemoryRuntimeHistEntry 7 }

cucsMemoryRuntimeHistCached OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:cached managed object property"
    ::= { cucsMemoryRuntimeHistEntry 8 }

cucsMemoryRuntimeHistCachedAvg OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:cachedAvg managed object property"
    ::= { cucsMemoryRuntimeHistEntry 9 }

cucsMemoryRuntimeHistCachedMax OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:cachedMax managed object property"
    ::= { cucsMemoryRuntimeHistEntry 10 }

cucsMemoryRuntimeHistCachedMin OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:cachedMin managed object property"
    ::= { cucsMemoryRuntimeHistEntry 11 }

cucsMemoryRuntimeHistId OBJECT-TYPE
    SYNTAX       Unsigned64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:id managed object property"
    ::= { cucsMemoryRuntimeHistEntry 12 }

cucsMemoryRuntimeHistMostRecent OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:mostRecent managed object property"
    ::= { cucsMemoryRuntimeHistEntry 13 }

cucsMemoryRuntimeHistSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:suspect managed object property"
    ::= { cucsMemoryRuntimeHistEntry 14 }

cucsMemoryRuntimeHistThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryRuntimeHistThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:thresholded managed object property"
    ::= { cucsMemoryRuntimeHistEntry 15 }

cucsMemoryRuntimeHistTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:timeCollected managed
        object property"
    ::= { cucsMemoryRuntimeHistEntry 16 }

cucsMemoryRuntimeHistTotal OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:total managed object property"
    ::= { cucsMemoryRuntimeHistEntry 17 }

cucsMemoryRuntimeHistTotalAvg OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:totalAvg managed object property"
    ::= { cucsMemoryRuntimeHistEntry 18 }

cucsMemoryRuntimeHistTotalMax OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:totalMax managed object property"
    ::= { cucsMemoryRuntimeHistEntry 19 }

cucsMemoryRuntimeHistTotalMin OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:RuntimeHist:totalMin managed object property"
    ::= { cucsMemoryRuntimeHistEntry 20 }

cucsMemoryUnitTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryUnitEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:Unit managed object table"
    ::= { cucsMemoryObjects 11 }

cucsMemoryUnitEntry OBJECT-TYPE
    SYNTAX           CucsMemoryUnitEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryUnitTable table."
    INDEX { cucsMemoryUnitInstanceId }
    ::= { cucsMemoryUnitTable 1 }

CucsMemoryUnitEntry ::= SEQUENCE {
    cucsMemoryUnitInstanceId                                         CucsManagedObjectId,
    cucsMemoryUnitDn                                                 CucsManagedObjectDn,
    cucsMemoryUnitRn                                                 SnmpAdminString,
    cucsMemoryUnitArray                                              Gauge32,
    cucsMemoryUnitBank                                               Gauge32,
    cucsMemoryUnitCapacity                                           Gauge32,
    cucsMemoryUnitClock                                              Gauge32,
    cucsMemoryUnitFormFactor                                         CucsMemoryFormFactor,
    cucsMemoryUnitId                                                 CucsMemoryUnitId,
    cucsMemoryUnitLatency                                            SnmpAdminString,
    cucsMemoryUnitLocation                                           SnmpAdminString,
    cucsMemoryUnitModel                                              SnmpAdminString,
    cucsMemoryUnitOperState                                          CucsEquipmentOperability,
    cucsMemoryUnitOperability                                        CucsMemoryUnitOperability,
    cucsMemoryUnitPerf                                               CucsEquipmentSensorThresholdStatus,
    cucsMemoryUnitPower                                              CucsEquipmentPowerState,
    cucsMemoryUnitPresence                                           CucsEquipmentPresence,
    cucsMemoryUnitRevision                                           SnmpAdminString,
    cucsMemoryUnitSerial                                             SnmpAdminString,
    cucsMemoryUnitSet                                                Gauge32,
    cucsMemoryUnitSpeed                                              Gauge32,
    cucsMemoryUnitThermal                                            CucsEquipmentSensorThresholdStatus,
    cucsMemoryUnitType                                               CucsMemoryType,
    cucsMemoryUnitVendor                                             SnmpAdminString,
    cucsMemoryUnitVisibility                                         CucsMemoryVisibility,
    cucsMemoryUnitVoltage                                            CucsEquipmentSensorThresholdStatus,
    cucsMemoryUnitWidth                                              Gauge32,
    cucsMemoryUnitAdminState                                         CucsMemoryAdminState,
    cucsMemoryUnitOperQualifier                                      CucsMemoryIssues,
    cucsMemoryUnitOperQualifierReason                                SnmpAdminString,
    cucsMemoryUnitLocationDn                                         SnmpAdminString
}

cucsMemoryUnitInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryUnitEntry 1 }

cucsMemoryUnitDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:dn managed object property"
    ::= { cucsMemoryUnitEntry 2 }

cucsMemoryUnitRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:rn managed object property"
    ::= { cucsMemoryUnitEntry 3 }

cucsMemoryUnitArray OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:array managed object property"
    ::= { cucsMemoryUnitEntry 4 }

cucsMemoryUnitBank OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:bank managed object property"
    ::= { cucsMemoryUnitEntry 5 }

cucsMemoryUnitCapacity OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:capacity managed object property"
    ::= { cucsMemoryUnitEntry 6 }

cucsMemoryUnitClock OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:clock managed object property"
    ::= { cucsMemoryUnitEntry 7 }

cucsMemoryUnitFormFactor OBJECT-TYPE
    SYNTAX       CucsMemoryFormFactor
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:formFactor managed object property"
    ::= { cucsMemoryUnitEntry 8 }

cucsMemoryUnitId OBJECT-TYPE
    SYNTAX       CucsMemoryUnitId
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:id managed object property"
    ::= { cucsMemoryUnitEntry 9 }

cucsMemoryUnitLatency OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:latency managed object property"
    ::= { cucsMemoryUnitEntry 10 }

cucsMemoryUnitLocation OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:location managed object property"
    ::= { cucsMemoryUnitEntry 11 }

cucsMemoryUnitModel OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:model managed object property"
    ::= { cucsMemoryUnitEntry 12 }

cucsMemoryUnitOperState OBJECT-TYPE
    SYNTAX       CucsEquipmentOperability
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:operState managed object property"
    ::= { cucsMemoryUnitEntry 13 }

cucsMemoryUnitOperability OBJECT-TYPE
    SYNTAX       CucsMemoryUnitOperability
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:operability managed object property"
    ::= { cucsMemoryUnitEntry 14 }

cucsMemoryUnitPerf OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:perf managed object property"
    ::= { cucsMemoryUnitEntry 15 }

cucsMemoryUnitPower OBJECT-TYPE
    SYNTAX       CucsEquipmentPowerState
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:power managed object property"
    ::= { cucsMemoryUnitEntry 16 }

cucsMemoryUnitPresence OBJECT-TYPE
    SYNTAX       CucsEquipmentPresence
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:presence managed object property"
    ::= { cucsMemoryUnitEntry 17 }

cucsMemoryUnitRevision OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:revision managed object property"
    ::= { cucsMemoryUnitEntry 18 }

cucsMemoryUnitSerial OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:serial managed object property"
    ::= { cucsMemoryUnitEntry 19 }

cucsMemoryUnitSet OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:set managed object property"
    ::= { cucsMemoryUnitEntry 20 }

cucsMemoryUnitSpeed OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:speed managed object property"
    ::= { cucsMemoryUnitEntry 21 }

cucsMemoryUnitThermal OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:thermal managed object property"
    ::= { cucsMemoryUnitEntry 22 }

cucsMemoryUnitType OBJECT-TYPE
    SYNTAX       CucsMemoryType
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:type managed object property"
    ::= { cucsMemoryUnitEntry 23 }

cucsMemoryUnitVendor OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:vendor managed object property"
    ::= { cucsMemoryUnitEntry 24 }

cucsMemoryUnitVisibility OBJECT-TYPE
    SYNTAX       CucsMemoryVisibility
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:visibility managed object property"
    ::= { cucsMemoryUnitEntry 25 }

cucsMemoryUnitVoltage OBJECT-TYPE
    SYNTAX       CucsEquipmentSensorThresholdStatus
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:voltage managed object property"
    ::= { cucsMemoryUnitEntry 26 }

cucsMemoryUnitWidth OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:width managed object property"
    ::= { cucsMemoryUnitEntry 27 }

cucsMemoryUnitAdminState OBJECT-TYPE
    SYNTAX       CucsMemoryAdminState
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:adminState managed object property"
    ::= { cucsMemoryUnitEntry 28 }

cucsMemoryUnitOperQualifier OBJECT-TYPE
    SYNTAX       CucsMemoryIssues
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:operQualifier managed object property"
    ::= { cucsMemoryUnitEntry 29 }

cucsMemoryUnitOperQualifierReason OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:operQualifierReason managed
        object property"
    ::= { cucsMemoryUnitEntry 30 }

cucsMemoryUnitLocationDn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:Unit:locationDn managed object property"
    ::= { cucsMemoryUnitEntry 31 }

cucsMemoryUnitEnvStatsTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryUnitEnvStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats managed object table"
    ::= { cucsMemoryObjects 12 }

cucsMemoryUnitEnvStatsEntry OBJECT-TYPE
    SYNTAX           CucsMemoryUnitEnvStatsEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryUnitEnvStatsTable table."
    INDEX { cucsMemoryUnitEnvStatsInstanceId }
    ::= { cucsMemoryUnitEnvStatsTable 1 }

CucsMemoryUnitEnvStatsEntry ::= SEQUENCE {
    cucsMemoryUnitEnvStatsInstanceId                                 CucsManagedObjectId,
    cucsMemoryUnitEnvStatsDn                                         CucsManagedObjectDn,
    cucsMemoryUnitEnvStatsRn                                         SnmpAdminString,
    cucsMemoryUnitEnvStatsIntervals                                  Gauge32,
    cucsMemoryUnitEnvStatsSuspect                                    TruthValue,
    cucsMemoryUnitEnvStatsTemperature                                SnmpAdminString,
    cucsMemoryUnitEnvStatsTemperatureAvg                             SnmpAdminString,
    cucsMemoryUnitEnvStatsTemperatureMax                             SnmpAdminString,
    cucsMemoryUnitEnvStatsTemperatureMin                             SnmpAdminString,
    cucsMemoryUnitEnvStatsThresholded                                CucsMemoryUnitEnvStatsThresholded,
    cucsMemoryUnitEnvStatsTimeCollected                              DateAndTime,
    cucsMemoryUnitEnvStatsUpdate                                     Gauge32
}

cucsMemoryUnitEnvStatsInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryUnitEnvStatsEntry 1 }

cucsMemoryUnitEnvStatsDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:dn managed object property"
    ::= { cucsMemoryUnitEnvStatsEntry 2 }

cucsMemoryUnitEnvStatsRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:rn managed object property"
    ::= { cucsMemoryUnitEnvStatsEntry 3 }

cucsMemoryUnitEnvStatsIntervals OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:intervals managed object property"
    ::= { cucsMemoryUnitEnvStatsEntry 4 }

cucsMemoryUnitEnvStatsSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:suspect managed object property"
    ::= { cucsMemoryUnitEnvStatsEntry 5 }

cucsMemoryUnitEnvStatsTemperature OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:temperature managed
        object property"
    ::= { cucsMemoryUnitEnvStatsEntry 6 }

cucsMemoryUnitEnvStatsTemperatureAvg OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:temperatureAvg managed
        object property"
    ::= { cucsMemoryUnitEnvStatsEntry 7 }

cucsMemoryUnitEnvStatsTemperatureMax OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:temperatureMax managed
        object property"
    ::= { cucsMemoryUnitEnvStatsEntry 8 }

cucsMemoryUnitEnvStatsTemperatureMin OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:temperatureMin managed
        object property"
    ::= { cucsMemoryUnitEnvStatsEntry 9 }

cucsMemoryUnitEnvStatsThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryUnitEnvStatsThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:thresholded managed
        object property"
    ::= { cucsMemoryUnitEnvStatsEntry 10 }

cucsMemoryUnitEnvStatsTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:timeCollected managed
        object property"
    ::= { cucsMemoryUnitEnvStatsEntry 11 }

cucsMemoryUnitEnvStatsUpdate OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStats:update managed object property"
    ::= { cucsMemoryUnitEnvStatsEntry 12 }

cucsMemoryUnitEnvStatsHistTable OBJECT-TYPE
    SYNTAX           SEQUENCE OF CucsMemoryUnitEnvStatsHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist managed object table"
    ::= { cucsMemoryObjects 13 }

cucsMemoryUnitEnvStatsHistEntry OBJECT-TYPE
    SYNTAX           CucsMemoryUnitEnvStatsHistEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "Entry for the cucsMemoryUnitEnvStatsHistTable table."
    INDEX { cucsMemoryUnitEnvStatsHistInstanceId }
    ::= { cucsMemoryUnitEnvStatsHistTable 1 }

CucsMemoryUnitEnvStatsHistEntry ::= SEQUENCE {
    cucsMemoryUnitEnvStatsHistInstanceId                             CucsManagedObjectId,
    cucsMemoryUnitEnvStatsHistDn                                     CucsManagedObjectDn,
    cucsMemoryUnitEnvStatsHistRn                                     SnmpAdminString,
    cucsMemoryUnitEnvStatsHistId                                     Unsigned64,
    cucsMemoryUnitEnvStatsHistMostRecent                             TruthValue,
    cucsMemoryUnitEnvStatsHistSuspect                                TruthValue,
    cucsMemoryUnitEnvStatsHistTemperature                            SnmpAdminString,
    cucsMemoryUnitEnvStatsHistTemperatureAvg                         SnmpAdminString,
    cucsMemoryUnitEnvStatsHistTemperatureMax                         SnmpAdminString,
    cucsMemoryUnitEnvStatsHistTemperatureMin                         SnmpAdminString,
    cucsMemoryUnitEnvStatsHistThresholded                            CucsMemoryUnitEnvStatsHistThresholded,
    cucsMemoryUnitEnvStatsHistTimeCollected                          DateAndTime
}

cucsMemoryUnitEnvStatsHistInstanceId OBJECT-TYPE
    SYNTAX       CucsManagedObjectId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Instance identifier of the managed object."
    ::= { cucsMemoryUnitEnvStatsHistEntry 1 }

cucsMemoryUnitEnvStatsHistDn OBJECT-TYPE
    SYNTAX       CucsManagedObjectDn
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:dn managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 2 }

cucsMemoryUnitEnvStatsHistRn OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:rn managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 3 }

cucsMemoryUnitEnvStatsHistId OBJECT-TYPE
    SYNTAX       Unsigned64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:id managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 4 }

cucsMemoryUnitEnvStatsHistMostRecent OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:mostRecent managed
        object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 5 }

cucsMemoryUnitEnvStatsHistSuspect OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:suspect managed
        object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 6 }

cucsMemoryUnitEnvStatsHistTemperature OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:temperature
        managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 7 }

cucsMemoryUnitEnvStatsHistTemperatureAvg OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:temperatureAvg
        managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 8 }

cucsMemoryUnitEnvStatsHistTemperatureMax OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:temperatureMax
        managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 9 }

cucsMemoryUnitEnvStatsHistTemperatureMin OBJECT-TYPE
    SYNTAX       SnmpAdminString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:temperatureMin
        managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 10 }

cucsMemoryUnitEnvStatsHistThresholded OBJECT-TYPE
    SYNTAX       CucsMemoryUnitEnvStatsHistThresholded
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:thresholded
        managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 11 }

cucsMemoryUnitEnvStatsHistTimeCollected OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Cisco UCS memory:UnitEnvStatsHist:timeCollected
        managed object property"
    ::= { cucsMemoryUnitEnvStatsHistEntry 12 }

END