-- =================================================================
-- Copyright (C) 2016 by  HUAWEI TECHNOLOGIES. All rights reserved.
--
-- Description: Huawei DHCP Server MIB
-- Reference:   HUAWEI Enterprise MIB
-- Version:     V2.07
-- History:
--              V2.05
--              modified by Huangjun 2009-12-08
-- =================================================================

HUAWEI-DHCPS-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        hwDhcp            
            FROM HUAWEI-MIB            
        ifIndex            
            FROM RFC1213-MIB            
        OBJECT-GROUP            
            FROM SNMPv2-CONF            
        IpAddress, Integer32, OBJECT-TYPE, MODULE-IDENTITY  --,TEXTUAL-CONVENTION            
            FROM SNMPv2-SMI            
        EnabledStatus
            FROM P-BRIDGE-MIB         
        RowStatus, TruthValue, MacAddress            
            FROM SNMPv2-TC
        MODULE-COMPLIANCE    
           FROM SNMPv2-CONF;

    hwDHCPServerMib MODULE-IDENTITY 
        LAST-UPDATED "201606220000Z"        -- June22, 2016 at 16:00 GMT
        ORGANIZATION 
            "Huawei Technologies Co.,Ltd."
        CONTACT-INFO 
            "Huawei Industrial Base
             Bantian, Longgang
             Shenzhen 518129
             People's Republic of China
             Website: http://www.huawei.com
             Email: support@huawei.com
            "
   DESCRIPTION
            "modify  the description of node hwDHCPSWriteDataDelay"
        REVISION "201606220000Z"       

   DESCRIPTION 
            "Add node hwDHCPSGlobalPoolConflictRecycleTime hwDHCPSInterfacePoolConflictRecycleTime"
        REVISION "201503050000Z"       

    DESCRIPTION 
            "This MIB describes objects used for managing DHCP server,
             including objects used for DHCP server global pool, 
             interface pool and informations of ip address used and conflicted
             in DHCP server, some Statistic informations about DHCP server"
        REVISION "201408250000Z"        -- Mar174, 2014 at 00:00 GMT
        
    DESCRIPTION 
            "This MIB describes objects used for managing DHCP server,
             including objects used for DHCP server global pool, 
             interface pool and informations of ip address used and conflicted
             in DHCP server, some Statistic informations about DHCP server"
        REVISION "201403170000Z"        -- Mar17, 2014 at 00:00 GMT

    DESCRIPTION 
            "This MIB describes objects used for managing DHCP server,
             including objects used for DHCP server global pool, 
             interface pool and informations of ip address used and conflicted
             in DHCP server, some Statistic informations about DHCP server"
        REVISION "201307040000Z"        -- Jul4, 2013 at 00:00 GMT

     DESCRIPTION 
            "This MIB describes objects used for managing DHCP server,
             including objects used for DHCP server global pool, 
             interface pool and informations of ip address used and conflicted
             in DHCP server, some Statistic informations about DHCP server"
        REVISION "201306190000Z"        -- Jun19, 2013 at 00:00 GMT

        DESCRIPTION 
            "This MIB describes objects used for managing DHCP server,
             including objects used for DHCP server global pool, 
             interface pool and informations of ip address used and conflicted
             in DHCP server, some Statistic informations about DHCP server"
        REVISION "201305170000Z"        -- May 17, 2013 at 00:00 GMT
        DESCRIPTION
            "The modify revision of this MIB module."

        REVISION "200302120000Z"        -- February 12, 2003 at 00:00 GMT
        DESCRIPTION
            "The initial revision of this MIB module."
        ::= { hwDhcp 2 }
    
    --
    -- Node definitions
    --

    -- 1.3.6.1.4.1.2011.5.7.2.1
    hwDHCPServerMibObject OBJECT IDENTIFIER ::= { hwDHCPServerMib 1 }
    
    --  Part 1: For DHCP server global pool 
    -- 
    -- =================================================================
    -- 1st Table of hwDHCPServerMibObject: hwDHCPSGlobalPoolTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.1
    hwDHCPSGlobalPoolTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSGlobalPoolEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "DHCP Server Global Pool table for creating 
            and deleting DHCP server global pool"
        ::= { hwDHCPServerMibObject 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.1.1
    hwDHCPSGlobalPoolEntry OBJECT-TYPE
        SYNTAX HwDHCPSGlobalPoolEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in DHCP Server Global Pool table 
             containing objects for creating or
            deleting a global pool for the DHCP server"
        INDEX { hwDHCPSGlobalPoolName }
        ::= { hwDHCPSGlobalPoolTable 1 }
    
    HwDHCPSGlobalPoolEntry ::=
        SEQUENCE { 
            hwDHCPSGlobalPoolName
                OCTET STRING,
            hwDHCPSGlobalPoolRowStatus
                RowStatus
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.1.1.1
    hwDHCPSGlobalPoolName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "DHCP server global pool name for creating or deleting
            DHCP server global pool "
        ::= { hwDHCPSGlobalPoolEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.1.1.2
    hwDHCPSGlobalPoolRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
               "This object is used to create new rows in this
            table, modify existing rows, and to delete
            existing rows.Only three actions are used: active(1),
            createAndGo(4), destroy(6).While the hwDHCPSGlobalPoolRowStatus 
            object is in the `createAndGo(4),The DHCP server global pool to
            be deleted must be exist"
        ::= { hwDHCPSGlobalPoolEntry 2 }
    
    --  =================================================================
    -- 2nd Table of hwDHCPServerMibObject: hwDHCPSGlobalPoolConfigTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.2
    hwDHCPSGlobalPoolConfigTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSGlobalPoolConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table containing the configuration informations of DHCP 
            server global pools, such as pool type, ip address, mask"
        ::= { hwDHCPServerMibObject 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1
    hwDHCPSGlobalPoolConfigEntry OBJECT-TYPE
        SYNTAX HwDHCPSGlobalPoolConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry containing the objects for configuring
            the network ip or host ip etc. to global pools for
            DHCP server"
        INDEX { hwDHCPSGlobalPoolName }
        ::= { hwDHCPSGlobalPoolConfigTable 1 }
    
    HwDHCPSGlobalPoolConfigEntry ::=
        SEQUENCE { 
            hwDHCPSGlobalPoolType
                INTEGER,
            hwDHCPSGlobalPoolNetwork
                IpAddress,
            hwDHCPSGlobalPoolNetworkMask
                IpAddress,
            hwDHCPSGlobalPoolHostIPAddr
                IpAddress,
            hwDHCPSGlobalPoolHostMask
                IpAddress,
            hwDHCPSGlobalPoolHostHAddr
                MacAddress,
            hwDHCPSGlobalPoolConfigUndoFlag
                INTEGER
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1.1
    hwDHCPSGlobalPoolType OBJECT-TYPE
        SYNTAX INTEGER
            {
            null(0),
            host(1),
            network(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Type of a DHCP global pool. Any operations of
            this object will be bound with the operations
            of hwDHCPSGlobalPoolNetwork and
            hwDHCPSGlobalPoolNetworkMask or with the 
            operations of hwDHCPSGlobalPoolHostIPAddr,
            hwDHCPSGlobalPoolMask and
            hwDHCPSGlobalPoolHostHAddr. That means any
            operation of this object alone will be regarded
            as invalid operation.
            The value means:
            null(0)- It is a pool without ip address,
            host(1)- It is a pool with manual allocation,
            network(2)- It is a pool with automatic allocation"
        ::= { hwDHCPSGlobalPoolConfigEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1.2
    hwDHCPSGlobalPoolNetwork OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Network ip address of a DHCP Server global pool. 
            To delete a configured network ip, please set
            hwDHCPSGlobalPoolConfigUndoFlag to 1"
        ::= { hwDHCPSGlobalPoolConfigEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1.3
    hwDHCPSGlobalPoolNetworkMask OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Net mask of a DHCP Server global pool(network).
            The SET operation to this object ought to be with
            the SET of hwDHCPSGlobalPoolNetwork together, and
            any SET operation alone to this object will be
            regarded as an invalid operation.
            When a network ip of a DHCP server global pool was 
            deleted, the net mask would also be deleted
            automatically, and no further operation needed"
        ::= { hwDHCPSGlobalPoolConfigEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1.4
    hwDHCPSGlobalPoolHostIPAddr OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Host ip of a DHCP server global pool
            To detete a configured Host ip, please set
            hwDHCPSGlobalPoolConfigUndoFlag to 2"
        ::= { hwDHCPSGlobalPoolConfigEntry 4 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1.5
    hwDHCPSGlobalPoolHostMask OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Host mask of a DHCP server global pool(host)
            The SET operation to this object ought to be with
            the SET of hwDHCPSGlobalPoolHostIPAddr together,
            and any SET operation alone to this object will be
            regarded as an invalid operation.
            When a host ip of a DHCP server global pool was 
            deleted, the Host mask would also be deleted
            automatically, and no further operation needed"
        ::= { hwDHCPSGlobalPoolConfigEntry 5 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1.6
    hwDHCPSGlobalPoolHostHAddr OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Hardware address of a DHCP server global pool(host).
            To delete a configured hardware address, please
            set hwDHCPSGlobalPoolConfigUndoFlag to 3"
        ::= { hwDHCPSGlobalPoolConfigEntry 6 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.2.1.7
    hwDHCPSGlobalPoolConfigUndoFlag OBJECT-TYPE
        SYNTAX INTEGER
            {
            undonetworkip(1),
            undohostip(2),
            undohosthaddr(3),
            invalid(4)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Flag of undo operation for
            hwDHCPSGlobalPoolConfigTable
            
            Each value has the following meaning:
            undonetworkip(1): The value identifies the flag to delete a configured network ip
            undohostip(2): The value identifies the flag to delete a configured host ip
            undohosthaddr(3):The value identifies the flag to delete a configured hardware address
            invalid(4):The value is a default value,do nothing 
            "
        ::= { hwDHCPSGlobalPoolConfigEntry 7 }
    
    --  =================================================================
    -- 3rd Table of hwDHCPServerMibObject: hwDHCPSGlobalPoolParaTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.3
    hwDHCPSGlobalPoolParaTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSGlobalPoolParaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring parameters to DHCP server global
            pool, include lease, Domain name,GateWayIP,DNSIP and so on"
        ::= { hwDHCPServerMibObject 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1
    hwDHCPSGlobalPoolParaEntry OBJECT-TYPE
        SYNTAX HwDHCPSGlobalPoolParaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry containing the objects for the
            configurations of parameters of DHCP server global pools"
        INDEX { hwDHCPSGlobalPoolName }
        ::= { hwDHCPSGlobalPoolParaTable 1 }
    
    HwDHCPSGlobalPoolParaEntry ::=
        SEQUENCE { 
            hwDHCPSGlobalPoolLeaseDay
                Integer32,
            hwDHCPSGlobalPoolLeaseHour
                Integer32,
            hwDHCPSGlobalPoolLeaseMinute
                Integer32,
            hwDHCPSGlobalPoolLeaseUnlimited
                INTEGER,
            hwDHCPSGlobalPoolDomainName
                OCTET STRING,
            hwDHCPSGlobalPoolClientGatewayIPString
                OCTET STRING,
            hwDHCPSGlobalPoolClientGatewayIPUndo
                IpAddress,
            hwDHCPSGlobalPoolClientDNSIPString
                OCTET STRING,
            hwDHCPSGlobalPoolClientDNSIPUndo
                IpAddress,
            hwDHCPSGlobalPoolClientNetbiosType
                INTEGER,
            hwDHCPSGlobalPoolClientNbnsIPString
                OCTET STRING,
            hwDHCPSGlobalPoolClientNbnsIPUndo
                IpAddress,
            hwDHCPSGlobalPoolParaUndoFlag
                INTEGER,
            hwDHCPSGlobalPoolIPInUseReset
                INTEGER,
           hwDHCPSGlobalPoolLogging
                INTEGER,
           hwDHCPSGlobalPoolConflictRecycleTime
                Integer32
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.1
    hwDHCPSGlobalPoolLeaseDay OBJECT-TYPE
        SYNTAX Integer32 (0..365)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A value which indicates number of days of the lease,
             The period over which a network address
             is allocated to a client is referred to as a 'lease'."
        DEFVAL { 1 }
        ::= { hwDHCPSGlobalPoolParaEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.2
    hwDHCPSGlobalPoolLeaseHour OBJECT-TYPE
        SYNTAX Integer32 (0..23)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A value which indicates number of hours of the lease,
            The period over which a network address
            is allocated to a client is referred to as a 'lease'."
        DEFVAL { 0 }
        ::= { hwDHCPSGlobalPoolParaEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.3
    hwDHCPSGlobalPoolLeaseMinute OBJECT-TYPE
        SYNTAX Integer32 (0..59)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A value which indicates number of minutes of the lease,
            The period over which a network address
            is allocated to a client is referred to as a 'lease'."
        DEFVAL { 0 }
        ::= { hwDHCPSGlobalPoolParaEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.4
    hwDHCPSGlobalPoolLeaseUnlimited OBJECT-TYPE
        SYNTAX INTEGER
            {
            invalid(0),
            unlimited(1)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A flag denoting if the lease of a pool is
            unlimited.
            
            The value means:
            invalid(0)- The lease of the network address that clients be assigned is finite, 
                        the period is decided by hwDHCPSGlobalPoolLeaseDay,hwDHCPSGlobalPoolLeaseHour and
                        hwDHCPSGlobalPoolLeaseMinute
                        
            unlimited(1)-The lease of the network address that clients be assigned is infinite"
        ::= { hwDHCPSGlobalPoolParaEntry 4 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.5
    hwDHCPSGlobalPoolDomainName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..63))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Domain name for DHCP Clients,
            the domain name that client should use when
            resolving hostnames via the Domain Name System."
        ::= { hwDHCPSGlobalPoolParaEntry 5 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.6
    hwDHCPSGlobalPoolClientGatewayIPString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "String of gateway ip addresses for DHCP clients.
            Since mostly 8 ip addresses can be configured for a pool
            totally, a string is defined to get or configure 8 ip
            addresses at a time"
        ::= { hwDHCPSGlobalPoolParaEntry 6 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.7
    hwDHCPSGlobalPoolClientGatewayIPUndo OBJECT-TYPE
        SYNTAX IpAddress 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A gateway ip address to be deleted. This object is
                only for deleting a given ip address of gateway router"
        ::= { hwDHCPSGlobalPoolParaEntry 7 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.8
    hwDHCPSGlobalPoolClientDNSIPString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "String of DNS server ip addresses for DHCP clients.
            Since mostly 8 ip addresses can be configured for a pool
            totally, a string is defined to get or configure 8
            ip addresses at a time"
        ::= { hwDHCPSGlobalPoolParaEntry 8 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.9
    hwDHCPSGlobalPoolClientDNSIPUndo OBJECT-TYPE
        SYNTAX IpAddress 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A DNS server ip address to be deleted. This object
                is only for deleting a given ip address of DNS server"
        ::= { hwDHCPSGlobalPoolParaEntry 9 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.10
    hwDHCPSGlobalPoolClientNetbiosType OBJECT-TYPE
        SYNTAX INTEGER
            {             
            null(0),
            bnode(1),
            pnode(2),
            mnode(4),
            hnode(8)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "NetBios node type for DHCP Clients
            
            Each value has the following meaning:
            null(0)-  no type designated
            bnode(1)- Broadcast ('B') nodes,Broadcast (or 'B') nodes communicate using a mix of UDP datagrams
                      (both broadcast and directed) and TCP connections.
            pnode(2)- Point-to-point ('P') nodes,Point-to-point (or 'P') nodes communicate using only directed UDP
                      datagrams and TCP sessions. 
            mnode(4)- Mixed mode ('M') nodes,Mixed mode nodes (or 'M') nodes are P nodes which have been given
                      certain B node characteristics.
            hnode(8)- Hybrid mode ('H') nodes.
            "
        DEFVAL { 0 }
        ::= { hwDHCPSGlobalPoolParaEntry 10 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.11
    hwDHCPSGlobalPoolClientNbnsIPString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "String of NetBios server ip addresses for DHCP
            clients. Since mostly 8 ip addresses can be configured for
            a pool totally, so a string is defined to get or
            configure 8 ip addresses at a time"
        ::= { hwDHCPSGlobalPoolParaEntry 11 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.12
    hwDHCPSGlobalPoolClientNbnsIPUndo OBJECT-TYPE
        SYNTAX IpAddress 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A NetBios server ip address to delete. This
            object is only for deleting a given ip address of NetBios
            server"
        ::= { hwDHCPSGlobalPoolParaEntry 12 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.13
    hwDHCPSGlobalPoolParaUndoFlag OBJECT-TYPE
        SYNTAX INTEGER
            {
            undoDomain(1),
            undoLease(2),
            undoGateway(3),
            undoDns(4),
            undoNbns(5),
            undoNbType(6),
            invalid(7)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Flag of undo-operation for
            hwDHCPSGlobalPoolParaTable
            
            Each value has the following meaning:                
            undoDomain(1)  - It means to delete Domain,
            undoLease(2)   - It means to delete lease of a given ip address,
            undoGateway(3) - It means to delete a given ip address of gateway router,
            undoDns(4)     - It means to delete a given ip address of DNS server,
            undoNbns(5)    - It means to deletd a given ip address of NetBios
                             server,
            undoNbType(6)  - It means to delete NetBios node type ,
            invalid(7)     - The value is a default value,do nothing"
        ::= { hwDHCPSGlobalPoolParaEntry 13 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.14
    hwDHCPSGlobalPoolIPInUseReset OBJECT-TYPE
        SYNTAX INTEGER { reset(1),invalid(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Reset the auto binding ip of the given global
                pool for DHCP server. The invalid(2) is a 
                default vlaue, do nothing"
        ::= { hwDHCPSGlobalPoolParaEntry 14 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.15
    hwDHCPSGlobalPoolLogging OBJECT-TYPE
        SYNTAX INTEGER { disable(0),enable(1) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Log the assigning IP addresses information  of the given global pool for DHCP server. "
         DEFVAL { disable }
        ::= { hwDHCPSGlobalPoolParaEntry 15 }

		
    -- 1.3.6.1.4.1.2011.5.7.2.1.3.1.16
    hwDHCPSGlobalPoolConflictRecycleTime OBJECT-TYPE
         SYNTAX Integer32 (0..1439999)
         UNITS "minute"
         MAX-ACCESS read-write
         STATUS current
         DESCRIPTION
              "Description."
         DEFVAL { 0 }
         ::= { hwDHCPSGlobalPoolParaEntry 16 }
    --  =================================================================
    -- 4th Table of hwDHCPServerMibObject: hwDHCPSGlobalPoolOptionTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.4
    hwDHCPSGlobalPoolOptionTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSGlobalPoolOptionEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring options to DHCP server global pools,
            include option code type and value and so on "
        ::= { hwDHCPServerMibObject 4 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.4.1
    hwDHCPSGlobalPoolOptionEntry OBJECT-TYPE
        SYNTAX HwDHCPSGlobalPoolOptionEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry containing the objects for configuring
            options to DHCP global pools"
        INDEX { hwDHCPSGlobalPoolName, hwDHCPSGlobalPoolOptionCode }
        ::= { hwDHCPSGlobalPoolOptionTable 1 }
    
    HwDHCPSGlobalPoolOptionEntry ::=
        SEQUENCE { 
            hwDHCPSGlobalPoolOptionCode
                Integer32,
            hwDHCPSGlobalPoolOptionType
                INTEGER,
            hwDHCPSGlobalPoolOptionAscii
                OCTET STRING,
            hwDHCPSGlobalPoolOptionHexString
                OCTET STRING,
            hwDHCPSGlobalPoolOptionIPString
                OCTET STRING,
            hwDHCPSGlobalPoolOptionRowStatus
                RowStatus,
            hwDHCPSGlobalPoolOptionCipher
                OCTET STRING
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.4.1.1
    hwDHCPSGlobalPoolOptionCode OBJECT-TYPE
        SYNTAX Integer32 (2..254)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Option code, All options begin with a tag octet, which uniquely
              identifies the option."
        ::= { hwDHCPSGlobalPoolOptionEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.4.1.2
    hwDHCPSGlobalPoolOptionType OBJECT-TYPE
        SYNTAX INTEGER
            {
            ascii(1),
            hex(2),
            ip(3),
            cipher(4)
            }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The object means option type in DHCP server global pool
            
            The value means :
            ascii(1)- The option type is ascii string
            hex(2)  - The option type is hex number
            ip(3)   - The option type is ip address
           cipher(4) - The option type is cipher string"
        ::= { hwDHCPSGlobalPoolOptionEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.4.1.3
    hwDHCPSGlobalPoolOptionAscii OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..63))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Ascii string of a option"
        ::= { hwDHCPSGlobalPoolOptionEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.4.1.4
    hwDHCPSGlobalPoolOptionHexString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Hex string of a option. 1 to 10 2 bytes or 4 bytes
            hex string can be configured at most simultaneously"
        ::= { hwDHCPSGlobalPoolOptionEntry 4 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.4.1.5
    hwDHCPSGlobalPoolOptionIPString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Ip string of a option. 1 to 8 ip addresses  can
            be configured at most simultaneously"
        ::= { hwDHCPSGlobalPoolOptionEntry 5 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.4.1.6
    hwDHCPSGlobalPoolOptionRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object is used to configuration new rows in this
            table, modify existing rows, and to delete
            existing rows.Only three actions are used: active(1),
            createAndGo(4), destroy(6).
            while configuration new option, you must specify option type 
            and value"
        ::= { hwDHCPSGlobalPoolOptionEntry 6 }
    
    hwDHCPSGlobalPoolOptionCipher OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..104))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Cipher string of a option."
       ::= { hwDHCPSGlobalPoolOptionEntry 7 }
    --  =================================================================
    -- 5th Table of hwDHCPServerMibObject:hwDHCPSGlobalTreeTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.5
    hwDHCPSGlobalTreeTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSGlobalTreeEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table containing the information of the tree of
            DHCP global pools, and the relationship between the pools,"
        ::= { hwDHCPServerMibObject 5 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.5.1
    hwDHCPSGlobalTreeEntry OBJECT-TYPE
        SYNTAX HwDHCPSGlobalTreeEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry of objects containing the information
            for displaying the tree of DHCP global pools"
        INDEX { hwDHCPSGlobalPoolName }
        ::= { hwDHCPSGlobalTreeTable 1 }
    
    HwDHCPSGlobalTreeEntry ::=
        SEQUENCE { 
            hwDHCPSGlobalTreeParentNodeName
                OCTET STRING,
            hwDHCPSGlobalTreeChildNodeName
                OCTET STRING,
            hwDHCPSGlobalTreePreSiblingNodeName
                OCTET STRING,
            hwDHCPSGlobalTreeSiblingNodeName
                OCTET STRING
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.5.1.1
    hwDHCPSGlobalTreeParentNodeName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Pool name of the parent node"
        ::= { hwDHCPSGlobalTreeEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.5.1.2
    hwDHCPSGlobalTreeChildNodeName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Pool name of the child node"
        ::= { hwDHCPSGlobalTreeEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.5.1.3
    hwDHCPSGlobalTreePreSiblingNodeName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Pool name of the presibling node"
        ::= { hwDHCPSGlobalTreeEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.5.1.4
    hwDHCPSGlobalTreeSiblingNodeName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Pool name of the sibling node"
        ::= { hwDHCPSGlobalTreeEntry 4 }
    
    --  Part 2: For DHCP server interface pool
    -- 
    -- =================================================================
    -- 6th Table of hwDHCPServerMibObject: hwDHCPSInterfacePoolParaTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.6
    hwDHCPSInterfacePoolParaTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSInterfacePoolParaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring parameters to DHCP server interface
            pools, include lease, Domain Name, DNS and so on"
        ::= { hwDHCPServerMibObject 6 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1
    hwDHCPSInterfacePoolParaEntry OBJECT-TYPE
        SYNTAX HwDHCPSInterfacePoolParaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry of objects for configuring parameters
            to DHCP interface pools.
            The index of this entry is the ifIndex of ethernet"
        INDEX { ifIndex }
        ::= { hwDHCPSInterfacePoolParaTable 1 }
    
    HwDHCPSInterfacePoolParaEntry ::=
        SEQUENCE { 
            hwDHCPSInterfacePoolLeaseDay
                Integer32,
            hwDHCPSInterfacePoolLeaseHour
                Integer32,
            hwDHCPSInterfacePoolLeaseMinute
                Integer32,
            hwDHCPSInterfacePoolLeaseUnlimited
                INTEGER,
            hwDHCPSInterfacePoolDomainName
                OCTET STRING,
            hwDHCPSInterfacePoolClientDNSIPString
                OCTET STRING,
            hwDHCPSInterfacePoolClientDNSIPUndo
                IpAddress,
            hwDHCPSInterfacePoolClientNetbiosType
                INTEGER,
            hwDHCPSInterfacePoolClientNbnsIPString
                OCTET STRING,
            hwDHCPSInterfacePoolClientNbnsIPUndo
                IpAddress,
            hwDHCPSInterfacePoolParaUndoFlag
                INTEGER,
            hwDHCPSInterfacePoolIPInUseReset
                INTEGER,
           hwDHCPSInterfacePoolLogging
                INTEGER,
           hwDHCPSInterfacePoolConflictRecycleTime
                Integer32
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.1
    hwDHCPSInterfacePoolLeaseDay OBJECT-TYPE
        SYNTAX Integer32 (0..365)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A value which indicates number of days of the lease,
             The period over which a network address
             is allocated to a client is referred to as a 'lease'."
        DEFVAL { 1 }
        ::= { hwDHCPSInterfacePoolParaEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.2
    hwDHCPSInterfacePoolLeaseHour OBJECT-TYPE
        SYNTAX Integer32 (0..23)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A value which indicates number of hours of the lease,
            The period over which a network address
            is allocated to a client is referred to as a 'lease'."
        DEFVAL { 0 }
        ::= { hwDHCPSInterfacePoolParaEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.3
    hwDHCPSInterfacePoolLeaseMinute OBJECT-TYPE
        SYNTAX Integer32 (0..59)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A value which indicates number of minutes of the lease,
            The period over which a network address
            is allocated to a client is referred to as a 'lease'."
        DEFVAL { 0 }
        ::= { hwDHCPSInterfacePoolParaEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.4
    hwDHCPSInterfacePoolLeaseUnlimited OBJECT-TYPE
        SYNTAX INTEGER
            {
            invalid(0),
            unlimited(1)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A flag denoting if the lease of a pool is unlimited.
            
            The value means:
            invalid(0)- The lease of the network address that clients be assigned is finite, 
                        the period is decided by hwDHCPSGlobalPoolLeaseDay,hwDHCPSGlobalPoolLeaseHour and
                        hwDHCPSGlobalPoolLeaseMinute
                        
            unlimited(1)-The lease of the network address that clients be assigned is infinite"
        ::= { hwDHCPSInterfacePoolParaEntry 4 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.5
    hwDHCPSInterfacePoolDomainName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..63))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Domain name for DHCP Clients,
            the domain name that client should use when
            resolving hostnames via the Domain Name System."
        ::= { hwDHCPSInterfacePoolParaEntry 5 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.6
    hwDHCPSInterfacePoolClientDNSIPString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "String of DNS server ip addresses for DHCP clients.
            Since mostly 8 ip can be configured for a pool
            totally, a string is defined to get or configure 8
            ip at a time"
        ::= { hwDHCPSInterfacePoolParaEntry 6 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.7
    hwDHCPSInterfacePoolClientDNSIPUndo OBJECT-TYPE
        SYNTAX IpAddress 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A DNS server ip address to delete. This object
                is only for deleting a given ip of DNS server"
        ::= { hwDHCPSInterfacePoolParaEntry 7 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.8
    hwDHCPSInterfacePoolClientNetbiosType OBJECT-TYPE
        SYNTAX INTEGER
            {
            null(0),
            bnode(1),
            pnode(2),
            mnode(4),
            hnode(8)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "NetBios node type for DHCP Clients
            
            Each value has the following meaning:
            null(0)-  no type designated
            bnode(1)- Broadcast ('B') nodes,Broadcast (or 'B') nodes communicate
                      using a mix of UDP datagrams (both broadcast and directed)
                      and TCP connections.
            pnode(2)- Point-to-point ('P') nodes,Point-to-point (or 'P') nodes 
                      communicate using only directed UDP datagrams and TCP sessions. 
            mnode(4)- Mixed mode ('M') nodes,Mixed mode nodes (or 'M') nodes are
                      P nodes which have been given certain B node characteristics.
            hnode(8)- Hybrid mode ('H') nodes.
            "
        DEFVAL { 8 }
        ::= { hwDHCPSInterfacePoolParaEntry 8 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.9
    hwDHCPSInterfacePoolClientNbnsIPString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "String of NetBios server ip addresses for DHCP
            clients. Since mostly 8 ip can be configured for
            a pool totally, so a string is defined to get or
            configure 8 ip at a time"
        ::= { hwDHCPSInterfacePoolParaEntry 9 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.10
    hwDHCPSInterfacePoolClientNbnsIPUndo OBJECT-TYPE
        SYNTAX IpAddress 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A NetBios server ip address to delete. This
            object is only for deleting a given ip of NetBios
            server"
        ::= { hwDHCPSInterfacePoolParaEntry 10 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.11
    hwDHCPSInterfacePoolParaUndoFlag OBJECT-TYPE
        SYNTAX INTEGER
            {
            undoDomain(1),
            undoLease(2),
            undoDns(4),
            undoNbns(5),
            undoNbType(6),
            invalid(7)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Flag of undo-operation for
            hwDHCPSInterfacePoolParaTable
            
            Each value has the following meaning:                
            undoDomain(1)  - It means to delete Domain,
            undoLease(2)   - It means to delete lease of a given ip address,
            undoGateway(3) - It means to delete a given ip address of gateway router,
            undoDns(4)     - It means to delete a given ip address of DNS server,
            undoNbns(5)    - It means to deletd a given ip address of NetBios
                             server,
            undoNbType(6)  - It means to delete NetBios node type
            invalid(7)     - The value is a default value,do nothing
            "
        ::= { hwDHCPSInterfacePoolParaEntry 11 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.12
    hwDHCPSInterfacePoolIPInUseReset OBJECT-TYPE
        SYNTAX INTEGER { reset(1),invalid(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Reset the auto or manual binding ip of the given interface
                pool for DHCP server. The invalid(2) is a default 
                vlaue, do nothing"
        ::= { hwDHCPSInterfacePoolParaEntry 12 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.13
    hwDHCPSInterfacePoolLogging OBJECT-TYPE
        SYNTAX INTEGER { disable(0),enable(1) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Log the assigning IP addresses information of the given interface pool for DHCP server. "
        DEFVAL { disable }
        ::= { hwDHCPSInterfacePoolParaEntry 13 }

		
    -- 1.3.6.1.4.1.2011.5.7.2.1.6.1.14
    hwDHCPSInterfacePoolConflictRecycleTime OBJECT-TYPE
        SYNTAX Integer32 (0..1439999)
        UNITS "minute"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "Description."
        DEFVAL { 0 }
        ::= { hwDHCPSInterfacePoolParaEntry 14 }
    --  =====================================================================
    -- 7th Table of hwDHCPServerMibObject: hwDHCPSInterfacePoolOptionTable
    -- =====================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.7
    hwDHCPSInterfacePoolOptionTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSInterfacePoolOptionEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring options to DHCP interface pools,
            include option code type and value and so on"
        ::= { hwDHCPServerMibObject 7 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.7.1
    hwDHCPSInterfacePoolOptionEntry OBJECT-TYPE
        SYNTAX HwDHCPSInterfacePoolOptionEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry of objects for configuring options
            to DHCP interface pools.
            The index of this entry is the inIndex of ethernet"
        INDEX { ifIndex, hwDHCPSInterfacePoolOptionCode }
        ::= { hwDHCPSInterfacePoolOptionTable 1 }
    
    HwDHCPSInterfacePoolOptionEntry ::=
        SEQUENCE { 
            hwDHCPSInterfacePoolOptionCode
                Integer32,
            hwDHCPSInterfacePoolOptionType
                INTEGER,
            hwDHCPSInterfacePoolOptionAscii
                OCTET STRING,
            hwDHCPSInterfacePoolOptionHexString
                OCTET STRING,
            hwDHCPSInterfacePoolOptionIPString
                OCTET STRING,
            hwDHCPSInterfacePoolOptionRowStatus
                RowStatus,
            hwDHCPSInterfacePoolOptionCipher
                OCTET STRING
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.7.1.1
    hwDHCPSInterfacePoolOptionCode OBJECT-TYPE
        SYNTAX Integer32 (2..254)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Option Code,All options begin with a tag octet, which uniquely
              identifies the option."
        ::= { hwDHCPSInterfacePoolOptionEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.7.1.2
    hwDHCPSInterfacePoolOptionType OBJECT-TYPE
        SYNTAX INTEGER
            {
            ascii(1),
            hex(2),
            ip(3),
            cipher(4)
            }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The object means option type in DHCP server interface pool
            
            The value means :
            ascii(1)- The option type is ascii string
            hex(2)  - The option type is hex number
            ip(3)   - The option type is ip address
           cipher(4) - The option type is cipher string
            "
        ::= { hwDHCPSInterfacePoolOptionEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.7.1.3
    hwDHCPSInterfacePoolOptionAscii OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..63))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Ascii string of an option"
        ::= { hwDHCPSInterfacePoolOptionEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.7.1.4
    hwDHCPSInterfacePoolOptionHexString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Hex string of a option. 1 to 10 2 bytes or 4 bytes
            hex string can be configured at most simultaneously"
        ::= { hwDHCPSInterfacePoolOptionEntry 4 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.7.1.5
    hwDHCPSInterfacePoolOptionIPString OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..129))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Ip string of a option. 1 to 8 ip addresses  can
            be configured at most simultaneously"
        ::= { hwDHCPSInterfacePoolOptionEntry 5 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.7.1.6
    hwDHCPSInterfacePoolOptionRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object is used to configuration new rows in this
            table, modify existing rows, and to delete
            existing rows.Only three actions are used: active(1),
            createAndGo(4), destroy(6).
            while configuration new option, you must specify option type 
            and value"
        ::= { hwDHCPSInterfacePoolOptionEntry 6 }
    
    hwDHCPSInterfacePoolOptionCipher OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..104))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Cipher string of an option"
       ::= { hwDHCPSInterfacePoolOptionEntry 7 }
    --  =========================================================================
    -- 8th Table of hwDHCPServerMibObject: hwDHCPSInterfacePoolStaticBindTable
    -- =========================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.8
    hwDHCPSInterfacePoolStaticBindTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSInterfacePoolStaticBindEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring static binding to DHCP
            interface pools,which manual binding ip address and Hardware address"
        ::= { hwDHCPServerMibObject 8 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.8.1
    hwDHCPSInterfacePoolStaticBindEntry OBJECT-TYPE
        SYNTAX HwDHCPSInterfacePoolStaticBindEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry of objects for configuring static
            binding to DHCP interface pools.
            The index of this entry is the inIndex of ethernet"
        INDEX { ifIndex, hwDHCPSInterfacePoolStaticBindIP }
        ::= { hwDHCPSInterfacePoolStaticBindTable 1 }
    
    HwDHCPSInterfacePoolStaticBindEntry ::=
        SEQUENCE { 
            hwDHCPSInterfacePoolStaticBindIP
                IpAddress,
            hwDHCPSInterfacePoolStaticBindMac
                MacAddress,
            hwDHCPSInterfacePoolStaticBindRowStatus
                RowStatus
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.8.1.1
    hwDHCPSInterfacePoolStaticBindIP OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Ip address in static binding for DHCP
            interface pools"
        ::= { hwDHCPSInterfacePoolStaticBindEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.8.1.2
    hwDHCPSInterfacePoolStaticBindMac OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Hardware address in static binding for DHCP 
            interface pools"
        ::= { hwDHCPSInterfacePoolStaticBindEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.8.1.3
    hwDHCPSInterfacePoolStaticBindRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object is used to configuration new rows in this
            table, modify existing rows, and to delete
            existing rows.Only three actions are used: active(1),
            createAndGo(4), destroy(6).
            while configuration static binding, you must specify ip address
            and hardware address
            "
        ::= { hwDHCPSInterfacePoolStaticBindEntry 3 }
    
    --  Part 3: For DHCP server
    -- 
    -- =================================================================
    -- 9th Table of hwDHCPServerMibObject: hwDHCPSIPInUseTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.9
    hwDHCPSIPInUseTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSIPInUseEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for displaying the information of ip allocation to clients
            for DHCP server pools"
        ::= { hwDHCPServerMibObject 9 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1
    hwDHCPSIPInUseEntry OBJECT-TYPE
        SYNTAX HwDHCPSIPInUseEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry of objects for displaying information
            of ip in use for DHCP server pools"
        INDEX { hwDHCPSIPInUseHAddr }
        ::= { hwDHCPSIPInUseTable 1 }
    
    HwDHCPSIPInUseEntry ::=
        SEQUENCE { 
            hwDHCPSIPInUseHAddr
                MacAddress,
            hwDHCPSIPInUseIP
                IpAddress,
            hwDHCPSIPInUseEndLease
                OCTET STRING,
            hwDHCPSIPInUseType
                INTEGER,
            hwDHCPSIPInUsePoolName
                OCTET STRING,
            hwDHCPSIPInUseInterface
                Integer32,
            hwDHCPSIPInUseVlan
                Integer32,
            hwDHCPSIPInUseAtmpvc
                Integer32
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.1
    hwDHCPSIPInUseHAddr OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The MAC addreess of host use the ip address in DHCP pools"
        ::= { hwDHCPSIPInUseEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.2
    hwDHCPSIPInUseIP OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Ip address allocation to clients in DHCP pools"
        ::= { hwDHCPSIPInUseEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.3
    hwDHCPSIPInUseEndLease OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..20))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "End time of ip address leasese.
            The structure of the OCTET STRING is
            year/month/day:hour:munite:second --
            YYYY/MM/DD:hh:mm:ss"
        ::= { hwDHCPSIPInUseEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.4
    hwDHCPSIPInUseType OBJECT-TYPE
        SYNTAX INTEGER
            {
            manual(1),
            auto(2),
            release(3),
            offered(4)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Type of binding
            
            The value means
                manual(1) - manual allocation
                auto(2)   - automatic allocation
                release(3)- The ip is automatic allocation,but it is already released            
                offered(4)-The ip is offered to client          
            "
        ::= { hwDHCPSIPInUseEntry 4 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.5
    hwDHCPSIPInUsePoolName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Name of the DHCP server pool that allocated ip belongs to"
        ::= { hwDHCPSIPInUseEntry 5 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.6
    hwDHCPSIPInUseInterface OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Interface index information that ip address belong to"
        ::= { hwDHCPSIPInUseEntry 6 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.7
    hwDHCPSIPInUseVlan OBJECT-TYPE
        SYNTAX Integer32 (1..4094)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Vlan informationg that ip address belong to"
        ::= { hwDHCPSIPInUseEntry 7 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.9.1.8
    hwDHCPSIPInUseAtmpvc OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "ATM Pvc informationg that ip address belong to"
        ::= { hwDHCPSIPInUseEntry 8 }
    
    --  =================================================================
    -- 10th Table of hwDHCPServerMibObject: hwDHCPSForbiddenIPTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.10
    hwDHCPSForbiddenIPTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSForbiddenIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring forbidden ip to DHCP server, which 
            don't allow to allocate to clients"
        ::= { hwDHCPServerMibObject 10 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.10.1
    hwDHCPSForbiddenIPEntry OBJECT-TYPE
        SYNTAX HwDHCPSForbiddenIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry for configuring forbidden ip to DHCP
            server"
        INDEX { hwDHCPSForbiddenIPStart, hwDHCPSForbiddenIPEnd }
        ::= { hwDHCPSForbiddenIPTable 1 }
    
    HwDHCPSForbiddenIPEntry ::=
        SEQUENCE { 
            hwDHCPSForbiddenIPStart
                IpAddress,
            hwDHCPSForbiddenIPEnd
                IpAddress,
            hwDHCPSForbiddenIPRowStatus
                RowStatus
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.10.1.1
    hwDHCPSForbiddenIPStart OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Start ip address of forbidden ip"
        ::= { hwDHCPSForbiddenIPEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.10.1.2
    hwDHCPSForbiddenIPEnd OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "End ip address of forbidden ip"
        ::= { hwDHCPSForbiddenIPEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.10.1.3
    hwDHCPSForbiddenIPRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object is used to configuration new rows in this
            table, modify existing rows, and to delete
            existing rows.Only three actions are used: active(1),
            createAndGo(4), destroy(6)
            "
        ::= { hwDHCPSForbiddenIPEntry 3 }
    
    --  =================================================================
    -- 11th Table of hwDHCPServerMibObject: hwDHCPSConflictIPTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.11
    hwDHCPSConflictIPTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSConflictIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "
            A table for displaying the information of conflict
            ip for DHCP server,ip address is uesed by others 
            when allocate the address.
            "
        ::= { hwDHCPServerMibObject 11 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.11.1
    hwDHCPSConflictIPEntry OBJECT-TYPE
        SYNTAX HwDHCPSConflictIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry for displaying the information of
            conflict ip for DHCP server"
        INDEX { hwDHCPSConflictIP }
        ::= { hwDHCPSConflictIPTable 1 }
    
    HwDHCPSConflictIPEntry ::=
        SEQUENCE { 
            hwDHCPSConflictIP
                IpAddress,
            hwDHCPSConflictIPType
                INTEGER,
            hwDHCPSConflictIPDetectTime
                OCTET STRING
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.11.1.1
    hwDHCPSConflictIP OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Conflict ip address"
        ::= { hwDHCPSConflictIPEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.11.1.2
    hwDHCPSConflictIPType OBJECT-TYPE
        SYNTAX INTEGER
            {
            ping(1),
            arp(2)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Type of the detection of conflict ip,
             As a consistency check, the allocating
             server SHOULD probe the reused address before allocating the address,
             e.g., with ping or ARP"
        ::= { hwDHCPSConflictIPEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.11.1.3
    hwDHCPSConflictIPDetectTime OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (20))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Time when the confict is detected.
            The structure of the OCTET STRING is
            year/month/day:hour:munite:second --
            YYYY/MM/DD:hh:mm:ss"
        ::= { hwDHCPSConflictIPEntry 3 }
    
    --  Part 4: Non-table object
    -- 
    -- 1.3.6.1.4.1.2011.5.7.2.1.12
    hwDHCPSServiceStatus OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The status of DHCP service, The default value is disabled, which
            mean disabled the DHCP service; the other value is enabled, which
            mean enable the DHCP service"
        ::= { hwDHCPServerMibObject 12 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.13
    hwDHCPSDetectingServerStatus OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The status of DHCP servers detecting function.
             If the value is enabled, It will check whether have other DHCP Servers.
             The default value is disabled"
        ::= { hwDHCPServerMibObject 13 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.14
    hwDHCPSPingNum OBJECT-TYPE
        SYNTAX Integer32 (0..10)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The number of ping packets sent out when check address conflict,the default value is 2."
        ::= { hwDHCPServerMibObject 14 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.15
    hwDHCPSPingTimeout OBJECT-TYPE
        SYNTAX Integer32 (0..10000)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The delay for the reply of a ping packet when check address conflict.
            Unit: millisecond, the default value is 500."
        ::= { hwDHCPServerMibObject 15 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.16
    hwDHCPSWriteDataStatus OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The status of the function writing data to the
            harddisk, It does not write data to the harddisk default,
            The information that written are the content that hwDHCPSConflictIPTable and hwDHCPSIPInUseTable,
            the default value is disable."
        ::= { hwDHCPServerMibObject 16 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.17
    hwDHCPSWriteDataDirection OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The directory of writing data to a harddisk, The format is
             directory and file name"
        ::= { hwDHCPServerMibObject 17 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.18
    hwDHCPSWriteDataDelay OBJECT-TYPE
        SYNTAX Integer32 (300..86400)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The allowable delay of writing data to the
            harddisk. Unit: second."
        ::= { hwDHCPServerMibObject 18 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.19
    hwDHCPSWriteDataRecover OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The flag used to recover DHCP data with the data on
            the harddisk,It means whether recover data from the data on
            the harddisk when system startup.
            The default value is disabled
            "
        ::= { hwDHCPServerMibObject 19 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.20
    hwDHCPSIPInUseResetIP OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "An ip in use that will be cleared. 0 returned for SET
            operation"
        ::= { hwDHCPServerMibObject 20 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.21
    hwDHCPSConflictIPResetIP OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "An conflict ip that will be cleared. 0 returned for
            SET operation"
        ::= { hwDHCPServerMibObject 21 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.22
    hwDHCPSIPResetFlag OBJECT-TYPE
        SYNTAX INTEGER
            {
            ipInUse(1),
            conflictIp(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A flag that descript the reset operation,
            1 means deleting ip in use
            2 means deleting conflict ip addresses"
        ::= { hwDHCPServerMibObject 22 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.23
    hwDHCPSGlobalPoolNumber OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of DHCP server global pools"
        ::= { hwDHCPServerMibObject 23 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.24
    hwDHCPSGlobalPoolAutoBindingNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of auto binding ip in DHCP server"
        ::= { hwDHCPServerMibObject 24 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.25
    hwDHCPSGlobalPoolManualBindingNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of manual binding ip in DHCP server"
        ::= { hwDHCPServerMibObject 25 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.26
    hwDHCPSGlobalPoolExpiredBindingNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of expired binding ip in DHCP server"
        ::= { hwDHCPServerMibObject 26 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.27
    hwDHCPSInterfacePoolNumber OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of DHCP server interface pools"
        ::= { hwDHCPServerMibObject 27 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.28
    hwDHCPSInterfacePoolAutoBindingNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of auto binding ip in DHCP server interface pools"
        ::= { hwDHCPServerMibObject 28 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.29
    hwDHCPSInterfacePoolManualBindingNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of manual binding ip in DHCP server interface pool"
        ::= { hwDHCPServerMibObject 29 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.30
    hwDHCPSInterfacePoolExpiredBindingNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of expired binding ip in DHCP server interface pool"
        ::= { hwDHCPServerMibObject 30 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.31
    hwDHCPSBadPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the bad packets received by DHCP server"
        ::= { hwDHCPServerMibObject 31 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.32
    hwDHCPSBootRequestPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the boot request packets recieved by DHCP
            Server from DHCP clients"
        ::= { hwDHCPServerMibObject 32 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.33
    hwDHCPSDiscoverPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Discover packets 
            received from the DHCP clients"
        ::= { hwDHCPServerMibObject 33 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.34
    hwDHCPSRequestPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Request packets 
            received from the DHCP clients"
        ::= { hwDHCPServerMibObject 34 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.35
    hwDHCPSDeclinePktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Decline packets 
            received from the DHCP clients"
        ::= { hwDHCPServerMibObject 35 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.36
    hwDHCPSReleasePktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Release packets 
            received from the DHCP clients"
        ::= { hwDHCPServerMibObject 36 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.37
    hwDHCPSInformPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Inform packets 
            received from the DHCP clients"
        ::= { hwDHCPServerMibObject 37 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.38
    hwDHCPSBootReplyPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the boot reply packets sent by DHCP server
            to DHCP clients"
        ::= { hwDHCPServerMibObject 38 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.39
    hwDHCPSOfferPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Offer packets 
            sent by the DHCP server"
        ::= { hwDHCPServerMibObject 39 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.40
    hwDHCPSAckPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Ack packets 
            sent by the DHCP server"
        ::= { hwDHCPServerMibObject 40 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.41
    hwDHCPSNakPktNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The total number of the DHCP Nak packets 
            sent by the DHCP server"
        ::= { hwDHCPServerMibObject 41 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.42
    hwDHCPSStatisticsReset OBJECT-TYPE
        SYNTAX INTEGER { invalid(0),
                reset(1)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Reset the above statictics information of packets
            received and sent by the DHCP server.
            The value 1 means clear the statictics information"
        ::= { hwDHCPServerMibObject 42 }
        
    --  =================================================================
    -- 43th Table of hwDHCPServerMibObject: hwDHCPChastenTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.43
    hwDHCPChastenTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPChastenEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring parameters of chasten , which 
            don't allow to deal with packet of clients"
        ::= { hwDHCPServerMibObject 43 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.43.1
    hwDHCPChastenEntry OBJECT-TYPE
        SYNTAX HwDHCPChastenEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry for configuring parameters of chasten"
        INDEX { hwDHCPChastenIndex }
        ::= { hwDHCPChastenTable 1 }
    
    HwDHCPChastenEntry ::=
        SEQUENCE { 
            hwDHCPChastenIndex
                Integer32,
            hwDHCPChastenPktNum
                Integer32,  
            hwDHCPChastenAutenPktNum
                Integer32,
            hwDHCPChastenCheckPeriod
                Integer32,
            hwDHCPChastenChastenPeriod
                Integer32,  
            hwDHCPChastenChastenRowStatus 
                RowStatus 
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.43.1.1
    hwDHCPChastenIndex OBJECT-TYPE
        SYNTAX Integer32 (0..16)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Slot of LPU"
        ::= { hwDHCPChastenEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.43.1.2
    hwDHCPChastenPktNum OBJECT-TYPE
        SYNTAX Integer32 (0..10000)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The threshold number of DHCP Discover packet"
        ::= { hwDHCPChastenEntry 2 }     
        
    -- 1.3.6.1.4.1.2011.5.7.2.1.43.1.3   
    hwDHCPChastenAutenPktNum OBJECT-TYPE
        SYNTAX Integer32 (0..10000)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The threshold number of DHCP Discover packet"
        ::= { hwDHCPChastenEntry 3 }
     
    -- 1.3.6.1.4.1.2011.5.7.2.1.43.1.4
    hwDHCPChastenCheckPeriod OBJECT-TYPE
        SYNTAX Integer32 (1..3600)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The period of checking"
        ::= { hwDHCPChastenEntry 4 }
    -- 1.3.6.1.4.1.2011.5.7.2.1.43.1.5
    hwDHCPChastenChastenPeriod OBJECT-TYPE
        SYNTAX Integer32 (0..3600)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The period of chasten"
        ::= { hwDHCPChastenEntry 5 }  
    -- 1.3.6.1.4.1.2011.5.7.2.1.43.1.6    
    hwDHCPChastenChastenRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object is used to configuration new rows in this
            table, modify existing rows, and to delete
            existing rows.Only three actions are used: active(1),
            createAndGo(4), destroy(6).
            while configuration new suboption, you must specify suboption type 
            and value"
            ::= { hwDHCPChastenEntry 6 }    

--  =================================================================
    -- 45th Table of hwDHCPServerMibObject: hwDHCPSIPPOOLForbiddenIPTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.45
    hwDHCPSIPPOOLForbiddenIPTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSIPPOOLForbiddenIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table for configuring forbidden ip to DHCP server, which 
            don't allow to allocate to clients"
        ::= { hwDHCPServerMibObject 45 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.45.1
    hwDHCPSIPPOOLForbiddenIPEntry OBJECT-TYPE
        SYNTAX HwDHCPSIPPOOLForbiddenIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry for configuring forbidden ip to DHCP
            server"
        INDEX { hwDHCPSIPPOOLForbiddenIPStart, hwDHCPSIPPOOLForbiddenIPEnd, hwDHCPSIPPOOLForbiddenIPVRFName }
        ::= { hwDHCPSIPPOOLForbiddenIPTable 1 }
    
    HwDHCPSIPPOOLForbiddenIPEntry ::=
        SEQUENCE { 
            hwDHCPSIPPOOLForbiddenIPStart
                IpAddress,
            hwDHCPSIPPOOLForbiddenIPEnd
                IpAddress,
            hwDHCPSIPPOOLForbiddenIPVRFName
                OCTET STRING,
            hwDHCPSIPPOOLForbiddenIPRowStatus
                RowStatus
         }

    -- 1.3.6.1.4.1.2011.5.7.2.1.45.1.1
    hwDHCPSIPPOOLForbiddenIPStart OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Start ip address of forbidden ip"
        ::= { hwDHCPSIPPOOLForbiddenIPEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.45.1.2
    hwDHCPSIPPOOLForbiddenIPEnd OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "End ip address of forbidden ip"
        ::= { hwDHCPSIPPOOLForbiddenIPEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.45.1.3
    hwDHCPSIPPOOLForbiddenIPVRFName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..31))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Index: the VRFNAME of forbidden ip."
        ::= { hwDHCPSIPPOOLForbiddenIPEntry 3 }
        
    -- 1.3.6.1.4.1.2011.5.7.2.1.45.1.4
    hwDHCPSIPPOOLForbiddenIPRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object is used to configuration new rows in this
            table, modify existing rows, and to delete
            existing rows.Only three actions are used: active(1),
            createAndGo(4), destroy(6)
            "
        ::= { hwDHCPSIPPOOLForbiddenIPEntry 4 }
    
    --  =================================================================
    -- 46th Table of hwDHCPServerMibObject: hwDHCPSIPPOOLConflictIPTable
    -- =================================================================
    -- 1.3.6.1.4.1.2011.5.7.2.1.46
    hwDHCPSIPPOOLConflictIPTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwDHCPSIPPOOLConflictIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "
            A table for displaying the information of conflict
            ip for DHCP server,ip address is uesed by others 
            when allocate the address.
            "
        ::= { hwDHCPServerMibObject 46 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.46.1
    hwDHCPSIPPOOLConflictIPEntry OBJECT-TYPE
        SYNTAX HwDHCPSIPPOOLConflictIPEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry for displaying the information of
            conflict ip for DHCP server"
        INDEX { hwDHCPSIPPOOLConflictIP, hwDHCPSIPPOOLConflictIPVRFName }
        ::= { hwDHCPSIPPOOLConflictIPTable 1 }
    
    HwDHCPSIPPOOLConflictIPEntry ::=
        SEQUENCE { 
            hwDHCPSIPPOOLConflictIP
                IpAddress,
            hwDHCPSIPPOOLConflictIPVRFName
                OCTET STRING,
            hwDHCPSIPPOOLConflictIPType
                INTEGER,
            hwDHCPSIPPOOLConflictIPDetectTime
                OCTET STRING
         }
        
    -- 1.3.6.1.4.1.2011.5.7.2.1.46.1.1
    hwDHCPSIPPOOLConflictIP OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Conflict ip address"
        ::= { hwDHCPSIPPOOLConflictIPEntry 1 }
        
    -- 1.3.6.1.4.1.2011.5.7.2.1.46.1.2
    hwDHCPSIPPOOLConflictIPVRFName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..31))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Index: the VRFNAME of conflict ip."
        ::= { hwDHCPSIPPOOLConflictIPEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.46.1.3
    hwDHCPSIPPOOLConflictIPType OBJECT-TYPE
        SYNTAX INTEGER
            {
            ping(1),
            arp(2)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Type of the detection of conflict ip,
             As a consistency check, the allocating
             server SHOULD probe the reused address before allocating the address,
             e.g., with ping or ARP"
        ::= { hwDHCPSIPPOOLConflictIPEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.1.46.1.4
    hwDHCPSIPPOOLConflictIPDetectTime OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (20))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Time when the confict is detected.
            The structure of the OCTET STRING is
            year/month/day:hour:munite:second --
            YYYY/MM/DD:hh:mm:ss"
        ::= { hwDHCPSIPPOOLConflictIPEntry 4 }
        
    hwDHCPThroughPacket OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Set client request packet through"
    ::= { hwDHCPServerMibObject 47 }
        
-- Reserved for H3C
--    hwDHCPSIPInUseExTable OBJECT-TYPE
--        SYNTAX SEQUENCE OF HwDHCPSIPInUseExEntry
--        MAX-ACCESS not-accessible
--        STATUS current
--        DESCRIPTION
--            "A table for displaying the information of ip in use
--            for DHCP Server pools. "
--        ::= { hwDHCPServerMibObject 45 }
        
        
    --  Conformance information
    -- 
    -- 1.3.6.1.4.1.2011.5.7.2.2
    hwDHCPServerMIBConformance OBJECT IDENTIFIER ::= { hwDHCPServerMib 2 }
    
    -- 1.3.6.1.4.1.2011.5.7.2.2.1
    hwDHCPServerMIBCompliances OBJECT IDENTIFIER ::= { hwDHCPServerMIBConformance 1 }
    hwDHCPServerMIBCompliance MODULE-COMPLIANCE
               STATUS      current
               DESCRIPTION
                   "The compliance statement for systems supporting 
                this module."

               MODULE      -- this module     1.3.6.1.4.1.2011.5.7.2.2.2      
               MANDATORY-GROUPS    {hwDHCPServerMIBGroup}  
                                               
              ::= { hwDHCPServerMIBCompliances 1 }
    hwDHCPServerMIBGroups OBJECT IDENTIFIER ::= { hwDHCPServerMIBConformance 2 }
    
    --  Units of conformance
    -- 
    -- 1.3.6.1.4.1.2011.5.7.2.2.2.1
    hwDHCPServerMIBGroup OBJECT-GROUP
        OBJECTS { hwDHCPSGlobalPoolName, hwDHCPSGlobalPoolRowStatus, hwDHCPSGlobalPoolType, hwDHCPSGlobalPoolNetwork, hwDHCPSGlobalPoolNetworkMask, 
            hwDHCPSGlobalPoolHostIPAddr, hwDHCPSGlobalPoolHostMask, hwDHCPSGlobalPoolHostHAddr, hwDHCPSGlobalPoolConfigUndoFlag, hwDHCPSGlobalPoolLeaseDay, 
            hwDHCPSGlobalPoolLeaseHour, hwDHCPSGlobalPoolLeaseMinute, hwDHCPSGlobalPoolLeaseUnlimited, hwDHCPSGlobalPoolDomainName, hwDHCPSGlobalPoolClientGatewayIPString, 
            hwDHCPSGlobalPoolClientGatewayIPUndo, hwDHCPSGlobalPoolClientDNSIPString, hwDHCPSGlobalPoolClientDNSIPUndo, hwDHCPSGlobalPoolClientNetbiosType, hwDHCPSGlobalPoolClientNbnsIPString, 
            hwDHCPSGlobalPoolClientNbnsIPUndo, hwDHCPSGlobalPoolParaUndoFlag, hwDHCPSGlobalPoolIPInUseReset, hwDHCPSGlobalPoolOptionCode, hwDHCPSGlobalPoolOptionType, 
            hwDHCPSGlobalPoolOptionAscii, hwDHCPSGlobalPoolOptionHexString, hwDHCPSGlobalPoolOptionIPString, hwDHCPSGlobalPoolOptionRowStatus, hwDHCPSGlobalTreeParentNodeName, 
            hwDHCPSGlobalTreeChildNodeName, hwDHCPSGlobalTreePreSiblingNodeName, hwDHCPSGlobalTreeSiblingNodeName, hwDHCPSInterfacePoolLeaseDay, hwDHCPSInterfacePoolLeaseHour, 
            hwDHCPSInterfacePoolLeaseMinute, hwDHCPSInterfacePoolLeaseUnlimited, hwDHCPSInterfacePoolDomainName, hwDHCPSInterfacePoolClientDNSIPString, hwDHCPSInterfacePoolClientDNSIPUndo, 
            hwDHCPSInterfacePoolClientNetbiosType, hwDHCPSInterfacePoolClientNbnsIPString, hwDHCPSInterfacePoolClientNbnsIPUndo, hwDHCPSInterfacePoolParaUndoFlag, hwDHCPSInterfacePoolIPInUseReset, 
            hwDHCPSInterfacePoolOptionCode, hwDHCPSInterfacePoolOptionType, hwDHCPSInterfacePoolOptionAscii, hwDHCPSInterfacePoolOptionHexString, hwDHCPSInterfacePoolOptionIPString, 
            hwDHCPSInterfacePoolOptionRowStatus, hwDHCPSInterfacePoolStaticBindIP, hwDHCPSInterfacePoolStaticBindMac, hwDHCPSInterfacePoolStaticBindRowStatus, hwDHCPSIPInUseHAddr, 
            hwDHCPSIPInUseIP, hwDHCPSIPInUseEndLease, hwDHCPSIPInUseType, hwDHCPSIPInUsePoolName, hwDHCPSIPInUseInterface, 
            hwDHCPSIPInUseVlan, hwDHCPSIPInUseAtmpvc, hwDHCPSForbiddenIPStart, hwDHCPSForbiddenIPEnd, hwDHCPSForbiddenIPRowStatus, 
            hwDHCPSConflictIP, hwDHCPSConflictIPType, hwDHCPSConflictIPDetectTime, hwDHCPSServiceStatus, hwDHCPSDetectingServerStatus, 
            hwDHCPSPingNum, hwDHCPSPingTimeout, hwDHCPSWriteDataStatus, hwDHCPSWriteDataDirection, hwDHCPSWriteDataDelay, 
            hwDHCPSWriteDataRecover, hwDHCPSIPInUseResetIP, hwDHCPSConflictIPResetIP, hwDHCPSIPResetFlag, hwDHCPSGlobalPoolNumber, 
            hwDHCPSGlobalPoolAutoBindingNum, hwDHCPSGlobalPoolManualBindingNum, hwDHCPSGlobalPoolExpiredBindingNum, hwDHCPSInterfacePoolNumber, hwDHCPSInterfacePoolAutoBindingNum, 
            hwDHCPSInterfacePoolManualBindingNum, hwDHCPSInterfacePoolExpiredBindingNum, hwDHCPSBadPktNum, hwDHCPSBootRequestPktNum, hwDHCPSDiscoverPktNum, 
            hwDHCPSRequestPktNum, hwDHCPSDeclinePktNum, hwDHCPSReleasePktNum, hwDHCPSInformPktNum, hwDHCPSBootReplyPktNum, 
            hwDHCPSOfferPktNum, hwDHCPSAckPktNum, hwDHCPSNakPktNum, hwDHCPSStatisticsReset, hwDHCPSIPPOOLForbiddenIPStart, hwDHCPSIPPOOLForbiddenIPEnd, hwDHCPSIPPOOLForbiddenIPVRFName, 
            hwDHCPSIPPOOLForbiddenIPRowStatus, hwDHCPSIPPOOLConflictIP, hwDHCPSIPPOOLConflictIPVRFName, hwDHCPSIPPOOLConflictIPType, hwDHCPSIPPOOLConflictIPDetectTime, hwDHCPThroughPacket,
            hwDHCPSGlobalPoolConflictRecycleTime, hwDHCPSInterfacePoolConflictRecycleTime }
        STATUS current
        DESCRIPTION 
            "The basic collection of objects providing management of
            DHCP server."
        ::= { hwDHCPServerMIBGroups 1 }
    

END