   CAMBIUM-PTP600-MIB DEFINITIONS ::= BEGIN

   IMPORTS
      MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
      Integer32, IpAddress,
      enterprises
         FROM SNMPv2-SMI
      MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
         FROM SNMPv2-CONF
      DisplayString
         FROM SNMPv2-TC
      InetAddress, InetAddressType
         FROM INET-ADDRESS-MIB;

   cambium MODULE-IDENTITY
      LAST-UPDATED "201403041414Z"
      ORGANIZATION "Cambium Networks Ltd."
      CONTACT-INFO
         "Post:  Simon Whitaker
                 Cambium Networks Ltd.
                 Unit B2,
                 Linhay Business Park,
                 Eastern Road,
                 Ashburton,
                 Devon.
                 TQ13 7UP
                 United Kingdom
         Phone:  +44 (0) 1364 655 500
         Email:  simon.whitaker@cambiumnetworks.com"
      DESCRIPTION
         "MIB for 300Mbps non-line-of-sight (NLOS) wireless ethernet bridge."
      REVISION "201403041414Z"
      DESCRIPTION
         "PTP600-10-07:
         Reinstated incompatibleRegionCodesTrap.
         Reinstated incompatibleMasterAndSlaveTrap.
         Reinstated encryptionEnabledMismatchTrap."
      REVISION "201309142338Z"
      DESCRIPTION
         "PTP600-10-06:
         Removed incompatibleRegionCodesTrap.
         Removed incompatibleMasterAndSlaveTrap.
         Removed encryptionEnabledMismatchTrap."
      REVISION "201208131812Z"
      DESCRIPTION
         "PTP600-10-04:
         Added ethernetBridgingStatus, ethernetBridgingAvailability.
         Added ethernetBridgingStatusAlarm, ethernetBridgingStatusAlarmTrap."
      REVISION "201205011158Z"
      DESCRIPTION
         "PTP600-10-03: make linkName & groupID read-write."
      REVISION "201202131238Z"
      DESCRIPTION
         "PTP600-10-01: Updated ORGANIZATION and CONTACT-INFO."
      REVISION "201111081347Z"
      DESCRIPTION
         "PTP600-10-00:
         Added new SNTP attributes, replace syslogLocalLog with syslogState. Add L2/L3 QoS attributes.
         Added securityLevel. Renamed vLANPriorityQueueMapping with ethernetPriorityQueueMapping.
         Added syslogClient and secureModeAlarm traps."
      REVISION "201012071328Z"
      DESCRIPTION "PTP600-09-10: Added searchState, accessMethod and groupID."
      REVISION "201011021333Z"
      DESCRIPTION "PTP600-09-02: Added latitude, longitude, altitude."
      REVISION "201007161541Z"
      DESCRIPTION
         "PTP600-09-01:
         Changed root OID.
         Renamed ethernet & fiber attributes & traps.
         Replaced vLANManagementVIDValidation with managementMode.
         Added linkName, siteName, hTTPSAccessEnabled, tDDSynchronizationMode.
         Added syslog attributes & traps.
         Added SNMPTrapTable for dual trap receivers."
      REVISION "201004231007Z"
      DESCRIPTION "PTP600-08-50: Security enhancements."
      REVISION "201002191855Z"
      DESCRIPTION "PTP600-08-04: Added SNMPv3 support, DFS Table, Automatic Tx Power Control. BIT STRING types now OCTET STRING."
      REVISION "200907101520Z"
      DESCRIPTION "PTP600-08-03: Added VLAN Priority Table, more read-only attributes, plus alarm tidy-up."
      REVISION "200902271711Z"
      DESCRIPTION "PTP600-08-01: Improve TDD Synchronization status and alarms."
      REVISION "200812151219Z"
      DESCRIPTION "PTP600-08-00: Support 4.8 & 4.9 GHz variant & 20 MHz bandwidth, Link Symmetry, TDD Synchronization."
      REVISION "200806301016Z"
      DESCRIPTION "PTP600-07-00: Added IEEE 802.1q & 802.1ad VLAN support."
      REVISION "200802290942Z"
      DESCRIPTION "PTP600-06-00: Added OOB, HTTP & telnet access controls."
      REVISION "200707311839Z"
      DESCRIPTION "PTP600-05-00: Added groups, attributes and notifications for diagnostic alarms."
      REVISION "200611231436Z"
      DESCRIPTION "PTP600-04-00: Converted to SMIv2."
      REVISION "200607241008Z"
      DESCRIPTION "PTP600-03-01"
      ::= { enterprises 17713 }

   -- Groups in cambium
   ptp                OBJECT IDENTIFIER ::= { cambium 1 }
   ptmp               OBJECT IDENTIFIER ::= { cambium 2 }
   ptp600             OBJECT IDENTIFIER ::= { cambium 6 }

   -- Groups in ptp600
   dfs                OBJECT IDENTIFIER ::= { ptp600 3 }
   bridge             OBJECT IDENTIFIER ::= { ptp600 4 }
   configuration      OBJECT IDENTIFIER ::= { ptp600 5 }
   ethernet           OBJECT IDENTIFIER ::= { ptp600 6 }
   telecom            OBJECT IDENTIFIER ::= { ptp600 7 }
   licence            OBJECT IDENTIFIER ::= { ptp600 8 }
   management         OBJECT IDENTIFIER ::= { ptp600 9 }
   phyControl         OBJECT IDENTIFIER ::= { ptp600 10 }
   phyStatus          OBJECT IDENTIFIER ::= { ptp600 12 }
   alarms             OBJECT IDENTIFIER ::= { ptp600 13 }
   smtp               OBJECT IDENTIFIER ::= { ptp600 15 }
   snmpControl        OBJECT IDENTIFIER ::= { ptp600 16 }
   sntp               OBJECT IDENTIFIER ::= { ptp600 17 }
   reset              OBJECT IDENTIFIER ::= { ptp600 18 }
   versions           OBJECT IDENTIFIER ::= { ptp600 19 }
   pubStats           OBJECT IDENTIFIER ::= { ptp600 20 }
   encryption         OBJECT IDENTIFIER ::= { ptp600 22 }
   tDDControl         OBJECT IDENTIFIER ::= { ptp600 23 }
   aAAControl         OBJECT IDENTIFIER ::= { ptp600 25 }
   syslogControl      OBJECT IDENTIFIER ::= { ptp600 24 }
   supplementary      OBJECT IDENTIFIER ::= { ptp600 96 }
   ptpGroups          OBJECT IDENTIFIER ::= { ptp600 98 }
   ptpTraps           OBJECT IDENTIFIER ::= { ptp600 99 }
   ptpTrapPrefix      OBJECT IDENTIFIER ::= { ptpTraps 0 }

   -- Compliance information
   --
   ptpCompliance MODULE-COMPLIANCE
      STATUS current
      DESCRIPTION
         "The compliance statement for the Cambium PTP MIB"
      MODULE -- this module
         MANDATORY-GROUPS { dfsGroup
                          , bridgeGroup
                          , configurationGroup
                          , ethernetGroup
                          , telecomGroup
                          , licenceGroup
                          , managementGroup
                          , phyControlGroup
                          , phyStatusGroup
                          , alarmsGroup
                          , smtpGroup
                          , snmpControlGroup
                          , sntpGroup
                          , resetGroup
                          , versionsGroup
                          , pubStatsGroup
                          , encryptionGroup
                          , tDDControlGroup
                          , aAAControlGroup
                          , syslogControlGroup
                          , supplementaryGroup
                          , notificationsGroup
                          } 
         ::= { ptp600 97 }

   dfsGroup OBJECT-GROUP
      OBJECTS { dfsTableNumber
              , dfsMeans
              , dfsNineNinePointNinePercentiles
              , dfsPeaks
              }
      STATUS  current
      DESCRIPTION "The dfs object group."
      ::= { ptpGroups 3 }

   bridgeGroup OBJECT-GROUP
      OBJECTS { localPacketFiltering
              }
      STATUS  current
      DESCRIPTION "The bridge object group."
      ::= { ptpGroups 4 }

   configurationGroup OBJECT-GROUP
      OBJECTS { iPv4Address
              , subnetMask
              , gatewayIPAddress
              , targetMACAddress
              , masterSlaveMode
              , maximumTransmitPower
              , antennaGain
              , cableLoss
              , eIRP
              , ethernetCappedMaxWirelessSpeed
              , channelBandwidth
              , remoteIPAddress
              , linkName
              , siteName
              , accessMethod
              , groupID
              , iPv6Address
              , iPVersion
              , iPv6AutoConfiguredLinkLocalAddress
              , iPv6PrefixLength
              , iPv6GatewayAddress
              , remoteInternetAddressType
              , remoteInternetAddress
              }
      STATUS  current
      DESCRIPTION "The configuration object group."
      ::= { ptpGroups 5 }

   ethernetGroup OBJECT-GROUP
      OBJECTS { dataPortAutoNegotiation
              , dataPortAutoNegAdvertisement
              , dataPortAutoMdix
              , dataPortStatus
              , dataPortSpeedAndDuplex
              , dataPortWirelessDownAlert
              , useVLANForManagementInterfaces
              , vLANManagementPriority
              , vLANManagementVID
              , managementPortStatus
              , managementPortSpeedAndDuplex
              , ethernetPriorityTableNumber
              , l2CPPriorityTableNumber
              , iPDSCPPriorityTableNumber
              , mPLSTCPriorityTableNumber
              , managementMode
              , managementPortWirelessDownAlert
              , qOSPriorityScheme
              , unknownNetworkPriorityQueueMapping
              , dSCPManagementPriority
              , ethernetBridgingStatus
              , ethernetPriorityQueueMapping
              , l2CPPriorityQueueMapping
              , iPDSCPPriorityQueueMapping
              , mPLSTCPriorityQueueMapping
              }
      STATUS  current
      DESCRIPTION "The ethernet object group."
      ::= { ptpGroups 6 }

   telecomGroup OBJECT-GROUP
      OBJECTS { telecomsInterface
              , telecomsChannelAStatus
              , telecomsChannelBStatus
              , channelALineCode
              , channelBLineCode
              , channelACableLength
              , channelBCableLength
              , channelALoopback
              , channelBLoopback
              , telecomsChannelSelection
              }
      STATUS  current
      DESCRIPTION "The telecom object group."
      ::= { ptpGroups 7 }

   licenceGroup OBJECT-GROUP
      OBJECTS { regionCode
              , productVariant
              , productName
              , ethernetFiberSupport
              , frequencyVariant
              , bandwidthVariant
              , constantPowerSpectralDensity
              , sNMPv3Enable
              , hAZLOCConfiguration
              , securityLevel
              }
      STATUS  current
      DESCRIPTION "The licence object group."
      ::= { ptpGroups 8 }

   managementGroup OBJECT-GROUP
      OBJECTS { targetRange
              , rangingMode
              , installStatus
              , installArmState
              , tFTPServerIPAddress
              , tFTPServerPortNumber
              , tFTPSoftwareUpgradeFileName
              , tFTPStartSoftwareUpgrade
              , tFTPSoftwareUpgradeStatus
              , tFTPSoftwareUpgradeStatusText
              , tFTPSoftwareUpgradeStatusAdditionalText
              , hTTPAccessEnabled
              , telnetAccessEnabled
              , hTTPPortNumber
              , hTTPSPortNumber
              , telnetPortNumber
              , hTTPSAccessEnabled
              , tFTPServerInternetAddressType
              , tFTPServerInternetAddress
              }
      STATUS  current
      DESCRIPTION "The management object group."
      ::= { ptpGroups 9 }

   phyControlGroup OBJECT-GROUP
      OBJECTS { linkSymmetry
              , linkModeOptimisation
              , userConfiguredMaxModulationMode
              , remoteMaximumTransmitPower
              , txColorCode
              , rxColorCode
              , automaticTxPowerControl
              , remoteRxTargetPower
              }
      STATUS  current
      DESCRIPTION "The phyControl object group."
      ::= { ptpGroups 10 }

   phyStatusGroup OBJECT-GROUP
      OBJECTS { receivePower
              , vectorError
              , transmitPower
              , range
              , linkLoss
              , receiveChannel
              , transmitChannel
              , receiveModulationMode
              , transmitModulationMode
              , receiveFreqMHz
              , transmitFreqMHz
              , signalStrengthRatio
              , receiveFreqKHz
              , transmitFreqKHz
              , searchState
              , rawReceivePower
              }
      STATUS  current
      DESCRIPTION "The phyStatus object group."
      ::= { ptpGroups 12 }

   alarmsGroup OBJECT-GROUP
      OBJECTS { unitOutOfCalibration
              , incompatibleRegionCodes
              , noWirelessChannelAvailable
              , wirelessLinkDisabledWarning
              , dataPortDisabledWarning
              , dataPortFiberStatus
              , dataPortConfigurationMismatch
              , incompatibleMasterAndSlave
              , tDDSynchronizationStatus
              , managementPortDisabledWarning
              , tDDSynchronizationAlarm
              , linkModeOptimizationMismatch
              , managementPortConfigurationMismatch
              , secureModeAlarm
              , ethernetBridgingStatusAlarm
              }
      STATUS  current
      DESCRIPTION "The alarms object group."
      ::= { ptpGroups 13 }

   smtpGroup OBJECT-GROUP
      OBJECTS { sMTPEmailAlert
              , sMTPServerIPAddress
              , sMTPServerPortNumber
              , sMTPSourceEmailAddress
              , sMTPDestinationEmailAddress
              , sMTPEnabledMessages
              , sMTPServerInternetAddressType
              , sMTPServerInternetAddress
              }
      STATUS  current
      DESCRIPTION "The smtp object group."
      ::= { ptpGroups 15 }

   snmpControlGroup OBJECT-GROUP
      OBJECTS { sNMPPortNumber
              , sNMPCommunityString
              , sNMPTrapTableNumber
              , sNMPTrapVersion
              , sNMPEnabledTraps
              , enabledDiagnosticAlarms
              , sNMPSendAllTrapsAtStartup
              , sNMPTrapIPAddress
              , sNMPTrapPortNumber
              , sNMPTrapInternetAddressType
              , sNMPTrapInternetAddress
              , sNMPTrapReceiverEnabled
              }
      STATUS  current
      DESCRIPTION "The snmpControl object group."
      ::= { ptpGroups 16 }

   sntpGroup OBJECT-GROUP
      OBJECTS { sNTPState
              , sNTPPollInterval
              , sNTPSync
              , sNTPLastSync
              , systemClock
              , timeZone
              , daylightSaving
              , sNTPPrimaryServer
              , sNTPPrimaryServerDeadTime
              , sNTPServerRetries
              , sNTPServerTimeout
              , sNTPServerTableNumber
              , sNTPServerIPAddress
              , sNTPServerPortNumber
              , sNTPServerStatus
              , sNTPServerInternetAddressType
              , sNTPServerInternetAddress
              }
      STATUS  current
      DESCRIPTION "The sntp object group."
      ::= { ptpGroups 17 }

   resetGroup OBJECT-GROUP
      OBJECTS { systemReset
              }
      STATUS  current
      DESCRIPTION "The reset object group."
      ::= { ptpGroups 18 }

   versionsGroup OBJECT-GROUP
      OBJECTS { softwareVersion
              , hardwareVersion
              , secondarySoftwareVersion
              , bootVersion
              }
      STATUS  current
      DESCRIPTION "The versions object group."
      ::= { ptpGroups 19 }

   pubStatsGroup OBJECT-GROUP
      OBJECTS { receiveDataRate
              , transmitDataRate
              , aggregateDataRate
              , wirelessLinkAvailability
              , wirelessLinkStatus
              , byteErrorRatio
              , receiveModulationModeDetail
              , ethernetBridgingAvailability
              }
      STATUS  current
      DESCRIPTION "The pubStats object group."
      ::= { ptpGroups 20 }

   encryptionGroup OBJECT-GROUP
      OBJECTS { encryptionAlgorithm
              }
      STATUS  current
      DESCRIPTION "The encryption object group."
      ::= { ptpGroups 22 }

   tDDControlGroup OBJECT-GROUP
      OBJECTS { tDDSynchronizationMode
              }
      STATUS  current
      DESCRIPTION "The tDDControl object group."
      ::= { ptpGroups 23 }

   aAAControlGroup OBJECT-GROUP
      OBJECTS { userTableNumber
              , userName
              , userRole
              , userEnabled
              , userPassword
              }
      STATUS  current
      DESCRIPTION "The aAAControl object group."
      ::= { ptpGroups 25 }

   syslogControlGroup OBJECT-GROUP
      OBJECTS { syslogClient
              , syslogState
              }
      STATUS  current
      DESCRIPTION "The syslogControl object group."
      ::= { ptpGroups 24 }

   supplementaryGroup OBJECT-GROUP
      OBJECTS { longitude
              , latitude
              , altitude
              }
      STATUS  current
      DESCRIPTION "The supplementary object group."
      ::= { ptpGroups 96 }

   notificationsGroup NOTIFICATION-GROUP
      NOTIFICATIONS { channelChangeTrap
                    , dfsImpulsiveInterferenceTrap
                    , dataPortStatusTrap
                    , telecomsChannelAStatusTrap
                    , telecomsChannelBStatusTrap
                    , channelALoopbackTrap
                    , channelBLoopbackTrap
                    , regionCodeTrap
                    , installStatusTrap
                    , installArmStateTrap
                    , unitOutOfCalibrationTrap
                    , incompatibleRegionCodesTrap
                    , noWirelessChannelAvailableTrap
                    , wirelessLinkDisabledWarningTrap
                    , dataPortDisabledWarningTrap
                    , dataPortFiberStatusTrap
                    , dataPortConfigurationMismatchTrap
                    , incompatibleMasterAndSlaveTrap
                    , sNTPSyncTrap
                    , tDDSynchronizationAlarmTrap
                    , managementPortStatusTrap
                    , managementPortDisabledWarningTrap
                    , linkModeOptimizationMismatchTrap
                    , managementPortConfigurationMismatchTrap
                    , syslogStateTrap
                    , syslogLocalNearlyFullTrap
                    , syslogLocalWrappedTrap
                    , syslogClientTrap
                    , secureModeAlarmTrap
                    , ethernetBridgingStatusAlarmTrap
                    }
      STATUS current
      DESCRIPTION "The notifications group."
      ::= { ptpGroups 99 }

 
   DfsTableEntry ::=
      SEQUENCE { dfsTableIndex INTEGER
               , dfsMeans Integer32
               , dfsNineNinePointNinePercentiles Integer32
               , dfsPeaks Integer32
      }
 
   dfsTable OBJECT-TYPE
      SYNTAX SEQUENCE OF DfsTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        " A table storing a snapshot of various DFS measurements for each channel"
      ::= { dfs 2 }
 
   dfsTableEntry OBJECT-TYPE
      SYNTAX DfsTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table DfsTable"
      INDEX { dfsTableIndex }
      ::= { dfsTable 1 }
 
   EthernetPriorityTableEntry ::=
      SEQUENCE { ethernetPriorityTableIndex INTEGER
               , ethernetPriorityQueueMapping INTEGER
      }
 
   ethernetPriorityTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EthernetPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        " A priority queue mapping table. This is a list of packet queues indexed by Ethernet priority."
      ::= { ethernet 15 }
 
   ethernetPriorityTableEntry OBJECT-TYPE
      SYNTAX EthernetPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table EthernetPriorityTable"
      INDEX { ethernetPriorityTableIndex }
      ::= { ethernetPriorityTable 1 }
 
   L2CPPriorityTableEntry ::=
      SEQUENCE { l2CPPriorityTableIndex INTEGER
               , l2CPPriorityQueueMapping INTEGER
      }
 
   l2CPPriorityTable OBJECT-TYPE
      SYNTAX SEQUENCE OF L2CPPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        " A priority queue mapping table. This is a list of packet queues indexed by L2CP priority."
      ::= { ethernet 17 }
 
   l2CPPriorityTableEntry OBJECT-TYPE
      SYNTAX L2CPPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table L2CPPriorityTable"
      INDEX { l2CPPriorityTableIndex }
      ::= { l2CPPriorityTable 1 }
 
   IPDSCPPriorityTableEntry ::=
      SEQUENCE { iPDSCPPriorityTableIndex INTEGER
               , iPDSCPPriorityQueueMapping INTEGER
      }
 
   iPDSCPPriorityTable OBJECT-TYPE
      SYNTAX SEQUENCE OF IPDSCPPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        " A priority queue mapping table. This is a list of packet queues indexed by L3 IP DSCP priority."
      ::= { ethernet 19 }
 
   iPDSCPPriorityTableEntry OBJECT-TYPE
      SYNTAX IPDSCPPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table IPDSCPPriorityTable"
      INDEX { iPDSCPPriorityTableIndex }
      ::= { iPDSCPPriorityTable 1 }
 
   MPLSTCPriorityTableEntry ::=
      SEQUENCE { mPLSTCPriorityTableIndex INTEGER
               , mPLSTCPriorityQueueMapping INTEGER
      }
 
   mPLSTCPriorityTable OBJECT-TYPE
      SYNTAX SEQUENCE OF MPLSTCPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        " A priority queue mapping table. This is a list of priority queues indexed by MPLS TC priority."
      ::= { ethernet 21 }
 
   mPLSTCPriorityTableEntry OBJECT-TYPE
      SYNTAX MPLSTCPriorityTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table MPLSTCPriorityTable"
      INDEX { mPLSTCPriorityTableIndex }
      ::= { mPLSTCPriorityTable 1 }
 
   SNMPTrapTableEntry ::=
      SEQUENCE { sNMPTrapTableIndex INTEGER
               , sNMPTrapIPAddress IpAddress
               , sNMPTrapPortNumber INTEGER
               , sNMPTrapInternetAddressType INTEGER
               , sNMPTrapInternetAddress InetAddress
               , sNMPTrapReceiverEnabled INTEGER
      }
 
   sNMPTrapTable OBJECT-TYPE
      SYNTAX SEQUENCE OF SNMPTrapTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        " SNMP trap configuration table."
      ::= { snmpControl 4 }
 
   sNMPTrapTableEntry OBJECT-TYPE
      SYNTAX SNMPTrapTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table SNMPTrapTable"
      INDEX { sNMPTrapTableIndex }
      ::= { sNMPTrapTable 1 }
 
   SNTPServerTableEntry ::=
      SEQUENCE { sNTPServerTableIndex INTEGER
               , sNTPServerIPAddress IpAddress
               , sNTPServerPortNumber INTEGER
               , sNTPServerStatus DisplayString
               , sNTPServerInternetAddressType INTEGER
               , sNTPServerInternetAddress InetAddress
      }
 
   sNTPServerTable OBJECT-TYPE
      SYNTAX SEQUENCE OF SNTPServerTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        ""
      ::= { sntp 15 }
 
   sNTPServerTableEntry OBJECT-TYPE
      SYNTAX SNTPServerTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table SNTPServerTable"
      INDEX { sNTPServerTableIndex }
      ::= { sNTPServerTable 1 }
 
   UserTableEntry ::=
      SEQUENCE { userTableIndex INTEGER
               , userName OCTET STRING
               , userRole INTEGER
               , userEnabled INTEGER
               , userPassword OCTET STRING
      }
 
   userTable OBJECT-TYPE
      SYNTAX SEQUENCE OF UserTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        " The User Table Control group contains objects specifically for user account management."
      ::= { aAAControl 2 }
 
   userTableEntry OBJECT-TYPE
      SYNTAX UserTableEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
        "Table UserTable"
      INDEX { userTableIndex }
      ::= { userTable 1 }
 
   -- Dfs group attribute definitions 
   --
   dfsTableNumber OBJECT-TYPE
      SYNTAX INTEGER (1..63)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the dfsTable"  
      ::= { dfs 1 } 
 
   -- DfsTable group attribute definitions 
   --
   dfsTableIndex OBJECT-TYPE
      SYNTAX INTEGER (1..63)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "used to index values in the dfsTable."  
      ::= { dfsTableEntry 1 } 
 
   dfsMeans OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Snapshot of DFS means"  
      ::= { dfsTableEntry 2 } 
 
   dfsNineNinePointNinePercentiles OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Snapshot of DFS 99.9 percentiles"  
      ::= { dfsTableEntry 3 } 
 
   dfsPeaks OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Snapshot of DFS peaks"  
      ::= { dfsTableEntry 4 } 
 
   -- Bridge group attribute definitions 
   --
   localPacketFiltering OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "When Local Packet Filtering is Enabled, the bridge 
             learns the source MAC addresses of devices transmitting 
             Ethernet packets on the local Ethernet network, and only 
             bridges packets to the remote unit if the destination MAC 
             address has not been learnt as a 'local' device. When 
             Local Packet Filtering is Disabled then the bridge does 
             not learn the source MAC addresses of devices 
             transmitting Ethernet packets on the local Ethernet 
             network, and bridges ALL Ethernet packets received to the 
             remote unit. Local Packet Filtering should be enabled if 
             no external routing hardware is present"  
      ::= { bridge 1 } 
 
   -- Configuration group attribute definitions 
   --
   iPv4Address OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Internet protocol (IPv4) address. This address is used 
             by the family of Internet protocols to uniquely identify 
             the unit on a network. NB: A system reboot is required to 
             activate changes to this attribute."  
      ::= { configuration 1 } 
 
   subnetMask OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "A subnet allows the flow of network traffic between 
             hosts to be segregated based on a network configuration. 
             By organizing hosts into logical groups, subnetting can 
             improve network security and performance. NB: A system 
             reboot is required to activate changes to this attribute"  
      ::= { configuration 2 } 
 
   gatewayIPAddress OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The IPv4 address of a computer on the current network 
             that is currently acting as an IPv4 network gateway. A 
             gateway acts as an entrance / exit to packets from / to 
             other networks. NB: A system reboot is required to 
             activate changes to this attribute"  
      ::= { configuration 3 } 
 
   targetMACAddress OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE(6))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "MAC address of the PTP wireless unit forming the other 
             end of the PTP link"  
      ::= { configuration 4 } 
 
   masterSlaveMode OBJECT-TYPE
      SYNTAX INTEGER {
                       master(0),
                       slave(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The PTP wireless link operates using a master and slave 
             relationship"  
      ::= { configuration 5 } 
 
   maximumTransmitPower OBJECT-TYPE
      SYNTAX INTEGER (-15..27)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Maximum transmit power the wireless unit is permitted to 
             use when establishing and maintaining the wireless link"  
      ::= { configuration 6 } 
 
   antennaGain OBJECT-TYPE
      SYNTAX INTEGER (0..610)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Antenna Gain. Expressed in 10ths of dBi. NB: This 
             attribute is ignored for variants with an integral 
             antenna."  
      ::= { configuration 7 } 
 
   cableLoss OBJECT-TYPE
      SYNTAX INTEGER (0..255)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Loss in the cable between the ODU and the antenna. 
             Expressed in 10ths of dB. NB: This attribute is ignored 
             for variants with an integral antenna."  
      ::= { configuration 8 } 
 
   eIRP OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Effective Isotropic Radiated Power (EIRP) describes the 
             strength of the radio signal leaving the wireless unit. 
             Expressed in 10ths of dBm"  
      ::= { configuration 9 } 
 
   ethernetCappedMaxWirelessSpeed OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Ethernet frames will be discarded in the ODU if the data 
             rate over the wireless link exceeds the Ethernet link 
             speed at the local or remote Data port. The Ethernet 
             Capped Max Wireless Speed control limits the wireless 
             data rate based on the local and remote Ethernet link 
             speed. Set this control to Enabled if either ODU is 
             connected to an Ethernet link operating at less than 1000 
             Mbps. NB: This attribute is automatically disabled when 
             the installation agent is armed. To disarm the 
             installation agent use the installation wizard."  
      ::= { configuration 10 } 
 
   channelBandwidth OBJECT-TYPE
      SYNTAX INTEGER {
                       bw30MHz(0),
                       bw15MHz(1),
                       bw10MHz(2),
                       bw5MHz(3),
                       bw20MHz(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "This control sets the bandwidth of the transmit and 
             receive radio channels"  
      ::= { configuration 11 } 
 
   remoteIPAddress OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "IP Address of the peer wireless unit"  
      ::= { configuration 12 } 
 
   linkName OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Name of the PTP link allocated by the System 
             Administrator. Used to establish a connection with the 
             correct PTP wireless unit at the other end of the link. 
             NOTE: The link name MUST be the same at both ends of the 
             PTP link."  
      ::= { configuration 14 } 
 
   siteName OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This field contains a user-provided description of the 
             site name together with any additional notes"  
      ::= { configuration 15 } 
 
   accessMethod OBJECT-TYPE
      SYNTAX INTEGER {
                       linkAccess(0),
                       linkNameAccess(1),
                       groupAccess(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "ODUs must be configured in pairs before a link can be 
             established. The Access Method attribute determines how 
             the paired ODUs will recognise each other. For the Link 
             Access method, each ODU must be configured with Target 
             MAC Address equal to the MAC Address of the other unit. 
             For the Link Name Access method, both units must be 
             configured with the same Link Name. For the Group Access 
             method, both units must be configured with the same Group 
             ID."  
      ::= { configuration 16 } 
 
   groupID OBJECT-TYPE
      SYNTAX INTEGER (0..255)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "When Access Method is set to Group Access, the Group ID 
             identifies all the units belonging to the same group"  
      ::= { configuration 17 } 
 
   iPv6Address OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..39))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Internet protocol (IPv6) address. This address is used 
             by the family of Internet protocols to uniquely identify 
             the unit on a network. NB: A system reboot is required to 
             activate changes to this attribute."  
      ::= { configuration 18 } 
 
   iPVersion OBJECT-TYPE
      SYNTAX INTEGER {
                       iPv4(0),
                       iPv6(1),
                       dualIPv4andIPv6(2)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "IP protocol selection. Choice of IPv4, IPv6 or Dual."  
      ::= { configuration 20 } 
 
   iPv6AutoConfiguredLinkLocalAddress OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..39))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The auto configured link local IPv6 address"  
      ::= { configuration 21 } 
 
   iPv6PrefixLength OBJECT-TYPE
      SYNTAX INTEGER (0..128)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "IPv6 prefix length"  
      ::= { configuration 22 } 
 
   iPv6GatewayAddress OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..39))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The IPv6 address of a computer on the current network 
             that is currently acting as an IPv6 network gateway. A 
             gateway acts as an entrance / exit to packets from / to 
             other networks. Note that it is usual to use the 
             link-local address of the gateway. NB: A system reboot is 
             required to activate changes to this attribute"  
      ::= { configuration 23 } 
 
   remoteInternetAddressType OBJECT-TYPE
      SYNTAX INTEGER {
                       unknown(0),
                       ipv4(1),
                       ipv6(2),
                       ipv4z(3),
                       ipv6z(4),
                       unknown6(5),
                       unknown7(6),
                       unknown8(7),
                       unknown9(8),
                       unknown10(9),
                       unknown11(10),
                       unknown12(11),
                       unknown13(12),
                       unknown14(13),
                       unknown15(14),
                       unknown16(15),
                       dns(16)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The type of Internet address specified by the associated 
             remoteInternetAddressType."  
      ::= { configuration 24 } 
 
   remoteInternetAddress OBJECT-TYPE
      SYNTAX InetAddress
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "INET address used to identify the peer wireless unit"  
      ::= { configuration 25 } 
 
   -- Ethernet group attribute definitions 
   --
   dataPortAutoNegotiation OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls whether the local Ethernet interface 
             configuration is automatically negotiated or forced. Do 
             not use a forced setting together with auto negotiation 
             at the Ethernet link partner. If you want to run your 
             Ethernet link at a fixed speed and duplex then you would 
             normally leave auto negotiation enabled and only enable 
             the single Auto Neg Advertisement option that you want 
             the link to run in - FORCING ETHERNET CONFIGURATION IS A 
             LAST RESORT WHICH SHOULD ONLY BE PERFORMED IF YOU ARE 
             HAVING PROBLEMS WITH AUTO NEGOTIATION - AND YOU MUST 
             ENSURE THAT YOU CONFIGURE BOTH THIS UNIT AND THE ETHERNET 
             LINK PARTNER TO WHICH IT IS CONNECTED IDENTICALLY (THE 
             LINK PARTNER MUST NOT HAVE AUTO NEGOTIATION ENABLED 
             EITHER, OTHERWISE A DUPLEX MISMATCH WILL OCCUR). NB: The 
             new setting will only take effect after a system reboot."  
      ::= { ethernet 1 } 
 
   dataPortAutoNegAdvertisement OBJECT-TYPE
      SYNTAX BITS {
                    negInvalid(2),
                    neg10MbpsHalfDuplex(3),
                    neg10MbpsFullDuplex(4),
                    neg100MbpsHalfDuplex(5),
                    neg100MbpsFullDuplex(6),
                    neg1000MbpsFullDuplex(7)
                  }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This sets the different Ethernet configurations that 
             will be advertised during auto negotiation. Note the new 
             setting will only take effect after a system reboot. 
             WARNING: Duplex mismatch may result if both ends of the 
             Ethernet link do not have the same settings. Do not auto 
             negotiation together with a fixed setting at the Ethernet 
             link partner. WARNING: Make sure that you select 
             option(s) that you know your connected equipment can 
             cater for!"  
      ::= { ethernet 2 } 
 
   dataPortAutoMdix OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This enables/disables the Auto MDI/MDIX capability. NB: 
             The new setting will only take effect after a system 
             reboot"  
      ::= { ethernet 3 } 
 
   dataPortStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       down(0),
                       copperLinkUp(1),
                       fiberLinkUp(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current status of the Ethernet link. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { ethernet 4 } 
 
   dataPortSpeedAndDuplex OBJECT-TYPE
      SYNTAX INTEGER {
                       speed1000MbpsFullDuplex(0),
                       speed100MbpsFullDuplex(1),
                       speed100MbpsHalfDuplex(2),
                       speed10MbpsFullDuplex(3),
                       speed10MbpsHalfDuplex(4),
                       speedUnknown6(5)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The current speed and duplex of the Ethernet link"  
      ::= { ethernet 5 } 
 
   dataPortWirelessDownAlert OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "When enabled, this causes the Ethernet link to be 
             dropped briefly when the wireless link drops. This is so 
             that spanning tree algorithms can quickly detect that 
             there is a problem."  
      ::= { ethernet 6 } 
 
   useVLANForManagementInterfaces OBJECT-TYPE
      SYNTAX INTEGER {
                       noVLANTagging(0),
                       iEEE8021QTaggedCTagType8100(1),
                       iEEE8021adTaggedSTagorBTagType88a8(2)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls whether the management interfaces 
             (WWW/SNMP/SMTP/SNTP) use VLAN tags or not. NB: The new 
             setting will only take effect after a system reboot"  
      ::= { ethernet 7 } 
 
   vLANManagementPriority OBJECT-TYPE
      SYNTAX INTEGER {
                       p0(0),
                       p1(1),
                       p2(2),
                       p3(3),
                       p4(4),
                       p5(5),
                       p6(6),
                       p7(7)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This VLAN Priority (0-7) will be included in packets 
             generated by the management interfaces. NB: The new 
             setting will only take effect after a system reboot"  
      ::= { ethernet 8 } 
 
   vLANManagementVID OBJECT-TYPE
      SYNTAX INTEGER (0..4094)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This VLAN VID (0-4094) will be included in packets 
             generated by the management interfaces. Note the new 
             setting will only take effect after a system reboot"  
      ::= { ethernet 11 } 
 
   managementPortStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       down(0),
                       copperLinkUp(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current status of the out-of-band management link. NB: a 
             change of state may generate an SNMP trap and/or SMTP 
             email alert"  
      ::= { ethernet 12 } 
 
   managementPortSpeedAndDuplex OBJECT-TYPE
      SYNTAX INTEGER {
                       speed100MbpsFullDuplex(1),
                       speed100MbpsHalfDuplex(2),
                       speed10MbpsFullDuplex(3),
                       speed10MbpsHalfDuplex(4),
                       speedUnknown6(5)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The current speed and duplex of the out-of-band 
             management link"  
      ::= { ethernet 13 } 
 
   ethernetPriorityTableNumber OBJECT-TYPE
      SYNTAX INTEGER (9)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the vLANPriorityTable."  
      ::= { ethernet 14 } 
 
   l2CPPriorityTableNumber OBJECT-TYPE
      SYNTAX INTEGER (5)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the l2CPPriorityTable."  
      ::= { ethernet 16 } 
 
   iPDSCPPriorityTableNumber OBJECT-TYPE
      SYNTAX INTEGER (64)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the iPDSCPPriorityTable."  
      ::= { ethernet 18 } 
 
   mPLSTCPriorityTableNumber OBJECT-TYPE
      SYNTAX INTEGER (8)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the mPLSTCPriorityTable."  
      ::= { ethernet 20 } 
 
   managementMode OBJECT-TYPE
      SYNTAX INTEGER {
                       outofBandLocal(0),
                       outofBand(1),
                       inBand(2),
                       inBandLocal(3)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Out-of-Band Management (only available on certain 
             hardware models): End-to-end out-of-band mode in which 
             the management agent can be reached from the management 
             port at the local ODU and (assuming that the wireless 
             link is established) the management port at the remote 
             ODU. Out-of-Band Local Management (only available on 
             certain hardware models): Similar to the standard 
             Out-of-Band mode, except that management frames are not 
             forwarded over the wireless link. In-Band Management 
             (default): The management agent can be reached from the 
             data port at the local ODU and (assuming that the 
             wireless link is established) the data port at the remote 
             ODU. In this mode the management port is disabled. 
             In-Band Local Management (only available when 'Use VLAN 
             For Management Interfaces' configures a VLAN tag): 
             Similar to the standard In-Band mode, except that 
             management frames are not forwarded over the wireless 
             link."  
      ::= { ethernet 22 } 
 
   managementPortWirelessDownAlert OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "When enabled, this causes the management link to be 
             dropped briefly when the wireless link drops. This is so 
             that spanning tree algorithms can quickly detect that 
             there is a problem."  
      ::= { ethernet 23 } 
 
   qOSPriorityScheme OBJECT-TYPE
      SYNTAX INTEGER {
                       ethernet(0),
                       iPMPLS(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Selects classification based on fields in the Ethernet 
             header (Layer 2) or in the Network header (Layer 3). The 
             unit recognises two network layer protocols: IP and MPLS"  
      ::= { ethernet 24 } 
 
   unknownNetworkPriorityQueueMapping OBJECT-TYPE
      SYNTAX INTEGER {
                       q0(0),
                       q1(1),
                       q2(2),
                       q3(3),
                       q4(4),
                       q5(5),
                       q6(6),
                       q7(7)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Configures the classification of unknown network 
             protocols to an egress queue at the wireless port. 
             Unknown means something other than IP and MPLS"  
      ::= { ethernet 25 } 
 
   dSCPManagementPriority OBJECT-TYPE
      SYNTAX INTEGER (0..63)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "This Differentiated Services Code Point value will be 
             inserted in the IP Header of all IP Datagrams transmitted 
             by the management interfaces"  
      ::= { ethernet 26 } 
 
   ethernetBridgingStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current status of Ethernet packet bridging over the 
             wireless link"  
      ::= { ethernet 27 } 
 
   -- EthernetPriorityTable group attribute definitions 
   --
   ethernetPriorityTableIndex OBJECT-TYPE
      SYNTAX INTEGER {
                       p0(1),
                       p1(2),
                       p2(3),
                       p3(4),
                       p4(5),
                       p5(6),
                       p6(7),
                       p7(8),
                       untagged(9)
                     }
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "Ethernet priority flag, used to index values in the 
             ethernetPriorityTable"  
      ::= { ethernetPriorityTableEntry 1 } 
 
   ethernetPriorityQueueMapping OBJECT-TYPE
      SYNTAX INTEGER {
                       q0(0),
                       q1(1),
                       q2(2),
                       q3(3),
                       q4(4),
                       q5(5),
                       q6(6),
                       q7(7)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Configures the classification of this Ethernet priority 
             (also known as IEEE 802.1p value) to an egress queue at 
             the wireless port"  
      ::= { ethernetPriorityTableEntry 2 } 
 
   -- L2CPPriorityTable group attribute definitions 
   --
   l2CPPriorityTableIndex OBJECT-TYPE
      SYNTAX INTEGER {
                       bridge(1),
                       mRP(2),
                       cFM(3),
                       rAPS(4),
                       eAPS(5)
                     }
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "L2CP priority flag, used to index values in the 
             l2CPPriorityTable"  
      ::= { l2CPPriorityTableEntry 1 } 
 
   l2CPPriorityQueueMapping OBJECT-TYPE
      SYNTAX INTEGER {
                       q0(0),
                       q1(1),
                       q2(2),
                       q3(3),
                       q4(4),
                       q5(5),
                       q6(6),
                       q7(7)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Configures the classification of this layer two control 
             protocol (L2CP) to an egress queue at the wireless port"  
      ::= { l2CPPriorityTableEntry 2 } 
 
   -- IPDSCPPriorityTable group attribute definitions 
   --
   iPDSCPPriorityTableIndex OBJECT-TYPE
      SYNTAX INTEGER (1..64)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "IP DSCP priority flag, used to index values in the 
             iPDSCPPriorityTable"  
      ::= { iPDSCPPriorityTableEntry 1 } 
 
   iPDSCPPriorityQueueMapping OBJECT-TYPE
      SYNTAX INTEGER {
                       q0(0),
                       q1(1),
                       q2(2),
                       q3(3),
                       q4(4),
                       q5(5),
                       q6(6),
                       q7(7)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Configures the classification of this IP differentiated 
             services code point (DSCP) value to an egress queue at 
             the wireless port"  
      ::= { iPDSCPPriorityTableEntry 2 } 
 
   -- MPLSTCPriorityTable group attribute definitions 
   --
   mPLSTCPriorityTableIndex OBJECT-TYPE
      SYNTAX INTEGER (1..8)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "MPLS TC priority flag, used to index values in the 
             mPLSTCPriorityTable"  
      ::= { mPLSTCPriorityTableEntry 1 } 
 
   mPLSTCPriorityQueueMapping OBJECT-TYPE
      SYNTAX INTEGER {
                       q0(0),
                       q1(1),
                       q2(2),
                       q3(3),
                       q4(4),
                       q5(5),
                       q6(6),
                       q7(7)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Configures the classification of this MPLS traffic class 
             (the field formerly known as EXP) to an egress queue at 
             the wireless port"  
      ::= { mPLSTCPriorityTableEntry 2 } 
 
   -- Telecom group attribute definitions 
   --
   telecomsInterface OBJECT-TYPE
      SYNTAX INTEGER {
                       none(0),
                       e1(1),
                       t1(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The line interface type. If this is set to 'None' then 
             the telecoms interfaces are disabled, and the telecom 
             group attributes will be ignored."  
      ::= { telecom 1 } 
 
   telecomsChannelAStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       noSignalLocal(1),
                       noSignalRemote(2),
                       noSignalLocalandRemote(3),
                       up(4),
                       remoteTiming(5),
                       noSignalLocalandRemoteTiming(6)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current status of telecoms channel A. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { telecom 2 } 
 
   telecomsChannelBStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       noSignalLocal(1),
                       noSignalRemote(2),
                       noSignalLocalandRemote(3),
                       up(4),
                       remoteTiming(5),
                       noSignalLocalandRemoteTiming(6)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current status of telecoms channel B. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { telecom 3 } 
 
   channelALineCode OBJECT-TYPE
      SYNTAX INTEGER {
                       aMI(0),
                       b8ZSHDB3(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The line code setting of the telecoms interface. This 
             must match the setting of the device connected to this 
             interface"  
      ::= { telecom 4 } 
 
   channelBLineCode OBJECT-TYPE
      SYNTAX INTEGER {
                       aMI(0),
                       b8ZSHDB3(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The line code setting of the telecoms interface. This 
             must match the setting of the device connected to this 
             interface"  
      ::= { telecom 5 } 
 
   channelACableLength OBJECT-TYPE
      SYNTAX INTEGER {
                       feet133(0),
                       feet266(1),
                       feet399(2),
                       feet533(3),
                       feet655(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The length of the cable connected to the telecoms 
             interface, measured in feet"  
      ::= { telecom 6 } 
 
   channelBCableLength OBJECT-TYPE
      SYNTAX INTEGER {
                       feet133(0),
                       feet266(1),
                       feet399(2),
                       feet533(3),
                       feet655(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The length of the cable connected to the telecoms 
             interface, measured in feet"  
      ::= { telecom 7 } 
 
   channelALoopback OBJECT-TYPE
      SYNTAX INTEGER {
                       none(0),
                       copper(1),
                       wireless(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The loopback status of telecoms channel A. This is 
             intended for installation testing and should be set to 
             'None' for normal operation. The wire connections to a 
             unit can be tested by applying a 'Copper' loopback to the 
             local unit. The wireless connection to the remote unit 
             can be tested by applying a 'Wireless' loopback to the 
             remote unit with no loopback on the local unit. NB: a 
             change of state may generate an SNMP trap and/or SMTP 
             email alert"  
      ::= { telecom 8 } 
 
   channelBLoopback OBJECT-TYPE
      SYNTAX INTEGER {
                       none(0),
                       copper(1),
                       wireless(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The loopback status of telecoms channel B. This is 
             intended for installation testing and should be set to 
             'None' for normal operation. The wire connections to a 
             unit can be tested by applying a 'Copper' loopback to the 
             local unit. The wireless connection to the remote unit 
             can be tested by applying a 'Wireless' loopback to the 
             remote unit with no loopback on the local unit. NB: a 
             change of state may generate an SNMP trap and/or SMTP 
             email alert"  
      ::= { telecom 9 } 
 
   telecomsChannelSelection OBJECT-TYPE
      SYNTAX INTEGER {
                       channelAOnly(0),
                       channelsAandB(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Indicates which telecoms channels have been enabled. If 
             only Channel A has been enabled, then the Channel B 
             attributes will be ignored."  
      ::= { telecom 10 } 
 
   -- Licence group attribute definitions 
   --
   regionCode OBJECT-TYPE
      SYNTAX INTEGER {
                       regionCodeInvalid(0),
                       regionCode1(1),
                       regionCode2(2),
                       regionCode3(3),
                       regionCode4(4),
                       regionCode5(5),
                       regionCode6(6),
                       regionCode7(7),
                       regionCode8(8),
                       regionCode9(9),
                       regionCode10(10),
                       regionCode11(11),
                       regionCode12(12),
                       regionCode13(13),
                       regionCode14(14),
                       regionCode15(15),
                       regionCode16(16),
                       regionCode17(17),
                       regionCode18(18),
                       regionCode19(19),
                       regionCode20(20),
                       regionCode21(21),
                       regionCode22(22),
                       regionCode23(23),
                       regionCode24(24),
                       regionCode25(25),
                       regionCode26(26),
                       regionCode27(27),
                       regionCode28(28),
                       regionCode29(29),
                       regionCode30(30),
                       regionCode31(31)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The region code prohibits the wireless unit from 
             operating outside the regulated limits. An invalid region 
             code indicates a corrupted license key. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { licence 1 } 
 
   productVariant OBJECT-TYPE
      SYNTAX INTEGER {
                       pTPxx400Full(0),
                       pTPxx400Deprecated1(1),
                       pTPxx400Deprecated2(2),
                       pTPxx400Lite(3),
                       spare1(4),
                       pTPxx300(5),
                       spare2(6),
                       spare3(7),
                       pTPxx500FullDeprecated(8),
                       pTPxx500LiteDeprecated(9),
                       pTPxx500(10),
                       pTPxx600Lite(11),
                       pTPxx600Full(12),
                       spare5(13),
                       spare6(14),
                       pTP800(15)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The product variant"  
      ::= { licence 2 } 
 
   productName OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Name of the product variant"  
      ::= { licence 3 } 
 
   ethernetFiberSupport OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Ethernet fiber support availability on this wireless 
             unit"  
      ::= { licence 4 } 
 
   frequencyVariant OBJECT-TYPE
      SYNTAX INTEGER {
                       freq5800MHz(0),
                       freq5400MHz(1),
                       freq4900MHz(2),
                       freq2500MHz(3),
                       freq5800MHz2(4),
                       freq5400MHz2(5),
                       freq4500MHz(6),
                       freq5900MHz(7),
                       freq5200MHz(8),
                       freq5100MHz(9),
                       freq4800MHz(10)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Frequency variant of the wireless unit"  
      ::= { licence 5 } 
 
   bandwidthVariant OBJECT-TYPE
      SYNTAX INTEGER {
                       bw30MHz(0),
                       bw15MHz(1),
                       bw10MHz(2),
                       bw5MHz(3),
                       bw20MHz(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Bandwidth variant of the wireless unit"  
      ::= { licence 6 } 
 
   constantPowerSpectralDensity OBJECT-TYPE
      SYNTAX INTEGER {
                       constant(0),
                       fullPower(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Constant power spectral density mode control"  
      ::= { licence 7 } 
 
   sNMPv3Enable OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "SNMPv3 availability control"  
      ::= { licence 9 } 
 
   hAZLOCConfiguration OBJECT-TYPE
      SYNTAX INTEGER {
                       nonHAZLOCUnit(0),
                       gasGroupA(1),
                       gasGroupB(2),
                       gasGroupC(3),
                       gasGroupD(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The HAZLOC/ATEX Configuration of this unit. The Gas 
             Group is configured by the license key."  
      ::= { licence 10 } 
 
   securityLevel OBJECT-TYPE
      SYNTAX INTEGER {
                       normal(0),
                       fIPS(1),
                       uCAPL(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The maximum configurable security level"  
      ::= { licence 11 } 
 
   -- Management group attribute definitions 
   --
   targetRange OBJECT-TYPE
      SYNTAX INTEGER (0..2000)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Initial target range used in installation +/-1, 
             expressed in tenths of a kilometer. When Auto-Ranging 
             this must be set to 0"  
      ::= { management 1 } 
 
   rangingMode OBJECT-TYPE
      SYNTAX INTEGER {
                       auto0to40km(0),
                       auto0to100km(1),
                       auto0to200km(2),
                       targetRange(3)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Type of ranging to use during installation, either 
             Auto-Ranging or use a selectable Target Range"  
      ::= { management 2 } 
 
   installStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       wrongPeer(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "A non-zero value indicates that signalling was received 
             with the wrong MAC address or a mismatched link name. NB: 
             It is very unusual to detect this, because units with 
             mis-configured Target MAC Address will normally fail to 
             establish a wireless link. However, rare circumstances 
             may establish a partial wireless link and detect this 
             situation. NB: A non-zero value on start-up, or a change 
             of value during operation, may generate an SNMP trap 
             and/or SMTP email alert"  
      ::= { management 3 } 
 
   installArmState OBJECT-TYPE
      SYNTAX INTEGER {
                       disarmed(0),
                       armed(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Indicates if the unit is being installed. NB: a change 
             of state may generate an SNMP trap and/or SMTP email 
             alert"  
      ::= { management 4 } 
 
   tFTPServerIPAddress OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "IP address of the TFTP Server from which the TFTP 
             Software Upgrade File Name will be retrieved"  
      ::= { management 5 } 
 
   tFTPServerPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The port number of the TFTP Server from which the TFTP 
             Software Upgrade File Name will be retrieved"  
      ::= { management 6 } 
 
   tFTPSoftwareUpgradeFileName OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..127))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Filename of the Software Upgrade to be loaded from the 
             TFTP Server"  
      ::= { management 7 } 
 
   tFTPStartSoftwareUpgrade OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Write '1' to this attribute to start the TFTP software 
             upgrade process. The attribute will be reset to 0 when 
             the upgrade process has finished. Continuing with the 
             software upgrade will cause spectrum management (DSO) 
             channel metrics collection to stop. The wireless unit 
             will no longer search for the optimal operational radio 
             channel. The performance of this wireless link may 
             deterioate over time. If operating in a region where 
             RADAR detection is mandatory you must complete the 
             software upgrade and reboot the unit. Channel metrics 
             collection will only be restarted after the wireless unit 
             has been rebooted"  
      ::= { management 8 } 
 
   tFTPSoftwareUpgradeStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       idle(0),
                       uploadinprogress(1),
                       uploadsuccessfulprogrammingFLASH(2),
                       upgradesuccessfulreboottorunthenewsoftwareimage(3),
                       upgradefailed(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The current status of the TFTP Software upgrade process"  
      ::= { management 9 } 
 
   tFTPSoftwareUpgradeStatusText OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..127))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Descriptive text describing the status of the TFTP 
             Software upgrade process, including any error details"  
      ::= { management 10 } 
 
   tFTPSoftwareUpgradeStatusAdditionalText OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..127))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Any additional text describing the status of the TFTP 
             Software upgrade process, including any error details"  
      ::= { management 11 } 
 
   hTTPAccessEnabled OBJECT-TYPE
      SYNTAX INTEGER {
                       no(0),
                       yes(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls whether or not HTTP access is enabled, 
             i.e. if this is disabled (0) then the unit will not 
             respond to any requests on the HTTP port. Remote 
             management via HTTPS is not affected by this setting. Any 
             change in this setting will not take effect until the 
             unit has been rebooted. (Factory default = Enabled)"  
      ::= { management 12 } 
 
   telnetAccessEnabled OBJECT-TYPE
      SYNTAX INTEGER {
                       no(0),
                       yes(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls whether or not Telnet access is enabled, 
             i.e. if this is disabled (0) then the unit will not 
             respond to any requests on the TELNET port. Any change in 
             this setting will not take effect until the unit has been 
             rebooted. (Factory default = Disabled)"  
      ::= { management 13 } 
 
   hTTPPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls the port number for HTTP access. A value 
             of zero will use the default port number. Any change in 
             this setting will not take effect until the unit has been 
             rebooted. (Factory default = 80)"  
      ::= { management 14 } 
 
   hTTPSPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls the port number for HTTPS access. A value 
             of zero will use the default port number. Availability of 
             HTTPS is controlled via the License Key. Any change in 
             this setting will not take effect until the unit has been 
             rebooted. (Factory default = 443)"  
      ::= { management 15 } 
 
   telnetPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls the port number for TELNET access. A value 
             of zero will use the default port number. Any change in 
             this setting will not take effect until the unit has been 
             rebooted. (Factory default = 23)"  
      ::= { management 16 } 
 
   hTTPSAccessEnabled OBJECT-TYPE
      SYNTAX INTEGER {
                       no(0),
                       yes(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls whether or not HTTPS access is enabled, 
             i.e. if this is disabled (0) then the unit will not 
             respond to any requests on the HTTPS port. Remote 
             management via HTTP is not affected by this setting. Any 
             change in this setting will not take effect until the 
             unit has been rebooted. (Factory default = Enabled)"  
      ::= { management 17 } 
 
   tFTPServerInternetAddressType OBJECT-TYPE
      SYNTAX INTEGER {
                       unknown(0),
                       ipv4(1),
                       ipv6(2),
                       ipv4z(3),
                       ipv6z(4),
                       unknown6(5),
                       unknown7(6),
                       unknown8(7),
                       unknown9(8),
                       unknown10(9),
                       unknown11(10),
                       unknown12(11),
                       unknown13(12),
                       unknown14(13),
                       unknown15(14),
                       unknown16(15),
                       dns(16)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The type of Internet address specified by the associated 
             tFTPServerInternetAddress."  
      ::= { management 18 } 
 
   tFTPServerInternetAddress OBJECT-TYPE
      SYNTAX InetAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "INET address of the TFTP Server from which the TFTP 
             Software Upgrade File Name will be retrieved"  
      ::= { management 19 } 
 
   -- PhyControl group attribute definitions 
   --
   linkSymmetry OBJECT-TYPE
      SYNTAX INTEGER {
                       symmetryAdaptive(0),
                       symmetry2to1(1),
                       symmetry1to1(2),
                       symmetry1to2(3)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Link Symmetry: in fixed symmetric mode the master spends 
             an equal amount of time transmitting and receiving; in 
             fixed asymmetric modes the master transmit and receive 
             times have a fixed ratio; in adaptive mode the transmit 
             and receive periods adjust with applied load."  
      ::= { phyControl 1 } 
 
   linkModeOptimisation OBJECT-TYPE
      SYNTAX INTEGER {
                       iPTraffic(0),
                       tDMTraffic(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Optimises the wireless link behavior for the type of 
             traffic to be carried. In 'IP Traffic' mode, the wireless 
             link will minimise transmission errors by automatically 
             adapting the modulation mode. In 'TDM Traffic' mode, the 
             wireless link will minimise transmission latency and 
             preserve throughput by maintaining a higher modulation 
             mode in the presence of a limited number of errors. The 
             'TDM Traffic' mode is recommended for E1/T1 applications 
             and connectionless protocols."  
      ::= { phyControl 2 } 
 
   userConfiguredMaxModulationMode OBJECT-TYPE
      SYNTAX INTEGER {
                       modBpsk63percent(0),
                       modQpsk63percent(1),
                       modQpsk87percent(2),
                       mod16qam63percent(3),
                       mod16qam87percent(4),
                       mod64qam75percent(5),
                       mod64qam92percent(6),
                       mod256qam81percent(7)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The maximum receive modulation mode controls the MAX 
             mode used for adaptive modulation. NOTE: This attribute 
             is automatically disabled when the installation agent is 
             armed. To disarm the installation agent use the 
             installation wizard"  
      ::= { phyControl 3 } 
 
   remoteMaximumTransmitPower OBJECT-TYPE
      SYNTAX INTEGER (-15..27)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Maximum transmit power the remote wireless unit is 
             permitted to use when establishing and maintaining the 
             wireless link"  
      ::= { phyControl 4 } 
 
   txColorCode OBJECT-TYPE
      SYNTAX INTEGER {
                       a(0),
                       b(1),
                       c(2),
                       d(3),
                       e(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Transmit Color Code. This attribute need only be 
             considered when the unit is installed in a network of 
             PTP600 units and where some of the units are operating on 
             the same frequency. In this case, the value would 
             normally be derived by a network planner. In all other 
             cases, it is recommended that this attribute is left at 
             the default value. NOTE: For the link to operate, the 
             value of this parameter must in all cases match the value 
             of the Rx Color Code parameter at the far end of the 
             link."  
      ::= { phyControl 5 } 
 
   rxColorCode OBJECT-TYPE
      SYNTAX INTEGER {
                       a(0),
                       b(1),
                       c(2),
                       d(3),
                       e(4)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Receive Color Code. This attribute need only be 
             considered when the unit is installed in a network of 
             PTP600 units and where some of the units are operating on 
             the same frequency. In this case, the value would 
             normally be derived by a network planner. In all other 
             cases, it is recommended that this attribute is left at 
             the default value. NOTE: For the link to operate, the 
             value of this parameter must in all cases match the value 
             of the Tx Color Code parameter at the far end of the 
             link."  
      ::= { phyControl 6 } 
 
   automaticTxPowerControl OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1),
                       enabledwithinitialestimate(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "When enabled, the transmit power of the local end is 
             automatically adjusted to maintain a configurable target 
             receive signal level at the remote end of the link. When 
             set to Enable with initial estimate, the Slave estimates 
             the optional transmit power before it responds to the 
             Master."  
      ::= { phyControl 8 } 
 
   remoteRxTargetPower OBJECT-TYPE
      SYNTAX INTEGER (-600..-400)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "This is the target receive level for the end of the link 
             which is remote from the end being configured. When 
             Automatic Power Control is enabled, the transmit power of 
             the local end is automatically adjusted in order to 
             maintain the receive signal level at the remote end 
             within a range centered on this value"  
      ::= { phyControl 9 } 
 
   -- PhyStatus group attribute definitions 
   --
   receivePower OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Receive power expressed in tenths of a dBm"  
      ::= { phyStatus 1 } 
 
   vectorError OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The vector error measurement compares the received 
             signal's IQ modulation characteristics to an ideal signal 
             to determine the composite error vector magnitude. The 
             value represented by this attribute is the average vector 
             error over the previous second expressed in tenths of a 
             dB"  
      ::= { phyStatus 2 } 
 
   transmitPower OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Transmit power expressed in tenths of a dBm"  
      ::= { phyStatus 3 } 
 
   range OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Distance between the two peer wireless units expressed 
             in tenths of a kilometer"  
      ::= { phyStatus 4 } 
 
   linkLoss OBJECT-TYPE
      SYNTAX INTEGER (-500..500)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The wireless link loss expressed in tenths of a dB"  
      ::= { phyStatus 5 } 
 
   receiveChannel OBJECT-TYPE
      SYNTAX INTEGER (0..63)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current active receive channel"  
      ::= { phyStatus 6 } 
 
   transmitChannel OBJECT-TYPE
      SYNTAX INTEGER (0..63)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current active transmit channel"  
      ::= { phyStatus 7 } 
 
   receiveModulationMode OBJECT-TYPE
      SYNTAX INTEGER {
                       modAcquisition(0),
                       modBpsk63percent(1),
                       modQpsk63percentSingle(2),
                       modTransient1(3),
                       modQpsk87percentSingle(4),
                       modTransient2(5),
                       mod16qam63percentSingleA(6),
                       modTransient3(7),
                       mod16qam87percentSingle(8),
                       modTransient4(9),
                       mod64qam75percentSingle(10),
                       modTransient5(11),
                       mod64qam92percentSingle(12),
                       modTransient6(13),
                       mod256qam81percentSingle(14),
                       mod16qam63percentSingleB(15),
                       mod16qam63percentDual(16),
                       modTransient7(17),
                       mod16qam87percentDual(18),
                       modTransient8(19),
                       mod64qam75percentDual(20),
                       modTransient9(21),
                       mod64qam92percentDual(22),
                       modTransient10(23),
                       mod256qam81percentDual(24)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current active receive modulation mode"  
      ::= { phyStatus 8 } 
 
   transmitModulationMode OBJECT-TYPE
      SYNTAX INTEGER {
                       modAcquisition(0),
                       modBpsk63percent(1),
                       modQpsk63percentSingle(2),
                       modTransient1(3),
                       modQpsk87percentSingle(4),
                       modTransient2(5),
                       mod16qam63percentSingleA(6),
                       modTransient3(7),
                       mod16qam87percentSingle(8),
                       modTransient4(9),
                       mod64qam75percentSingle(10),
                       modTransient5(11),
                       mod64qam92percentSingle(12),
                       modTransient6(13),
                       mod256qam81percentSingle(14),
                       mod16qam63percentSingleB(15),
                       mod16qam63percentDual(16),
                       modTransient7(17),
                       mod16qam87percentDual(18),
                       modTransient8(19),
                       mod64qam75percentDual(20),
                       modTransient9(21),
                       mod64qam92percentDual(22),
                       modTransient10(23),
                       mod256qam81percentDual(24)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current active transmit modulation mode"  
      ::= { phyStatus 9 } 
 
   receiveFreqMHz OBJECT-TYPE
      SYNTAX INTEGER (0..5925)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current receive frequency expressed in integer MHz"  
      ::= { phyStatus 11 } 
 
   transmitFreqMHz OBJECT-TYPE
      SYNTAX INTEGER (0..5925)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current transmit frequency expressed in integer MHz"  
      ::= { phyStatus 12 } 
 
   signalStrengthRatio OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Signal strength ratio (Vertical / Horizontal) : the 
             number of dB larger the Vertical antenna input is than 
             the Horizontal antenna input expressed in tenths of a dB"  
      ::= { phyStatus 13 } 
 
   receiveFreqKHz OBJECT-TYPE
      SYNTAX INTEGER (0..5925000)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current receive frequency expressed as KHz"  
      ::= { phyStatus 14 } 
 
   transmitFreqKHz OBJECT-TYPE
      SYNTAX INTEGER (0..5925000)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current transmit frequency expressed as KHz"  
      ::= { phyStatus 15 } 
 
   searchState OBJECT-TYPE
      SYNTAX INTEGER {
                       registering(0),
                       searching(1),
                       acquiring(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Search status of the wireless modem. 'Registering' means 
             that the modem has locked to an OFDM signal, and the 
             wireless link is up. 'Searching' means that no wireless 
             signal has been detected. 'Acquiring' means that a 
             wireless signal has been detected, but the modem has not 
             locked to an OFDM signal."  
      ::= { phyStatus 16 } 
 
   rawReceivePower OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Raw receive power expressed in tenths of a dBm"  
      ::= { phyStatus 17 } 
 
   -- Alarms group attribute definitions 
   --
   unitOutOfCalibration OBJECT-TYPE
      SYNTAX INTEGER {
                       calibrated(0),
                       outOfCalibration(1),
                       outOfCalibrationPAsShutdown(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The unit is out of calibration"  
      ::= { alarms 1 } 
 
   incompatibleRegionCodes OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       incompatibleLicenceKeys(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The master and slave units have incompatible region 
             codes. NB: Both units must have compatible license keys"  
      ::= { alarms 4 } 
 
   noWirelessChannelAvailable OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       noWirelessChannelAvailable(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Spectrum Management was unable to locate a suitable 
             wireless channel to operate on"  
      ::= { alarms 5 } 
 
   wirelessLinkDisabledWarning OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       disabledBySNMPifAdminStatus(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The SNMP ifAdminStatus of the wireless interface has 
             disabled wireless traffic"  
      ::= { alarms 6 } 
 
   dataPortDisabledWarning OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       disabledBySNMPifAdminStatus(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The SNMP ifAdminStatus of the Ethernet interface has 
             disabled Ethernet traffic"  
      ::= { alarms 7 } 
 
   dataPortFiberStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       installedFiberNotLicensed(1),
                       fiberLinkNotEstablishedButLOSNotDetected(2),
                       fiberLinkNotEstablishedAndLOSDetected(3)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "If the fiber link is not OK, there are three possible 
             causes: Either the fiber link has been installed but 
             disabled (because the license key does not include fiber 
             support), the link could not be established even though 
             no LOS was detected (i.e. an optical carrier was 
             detected, which could be due to a broken TX fiber, or 
             because the link is disabled at the fiber link partner), 
             or the link could not be established and LOS is detected 
             (i.e. no optical carrier is detected). NB: a change of 
             status may generate an SNMP trap and/or SMTP email alert"  
      ::= { alarms 8 } 
 
   dataPortConfigurationMismatch OBJECT-TYPE
      SYNTAX INTEGER {
                       noError(0),
                       mismatchDetected(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The detection of Ethernet fragments (runt packets) when 
             the link is in full duplex is an indication of an 
             auto-negotiation or forced configuration mismatch"  
      ::= { alarms 9 } 
 
   incompatibleMasterAndSlave OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       incompatibleProductVariants(1),
                       differentSoftwareVersionsRunning(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "A non-zero value indicates that the master and slave 
             ends of a link are different hardware products, or have 
             different software versions. NB: It is very unusual to 
             detect this, because incompatible units will normally 
             fail to establish a wireless link. However, some 
             combinations may establish a partial wireless link and 
             detect this situation. NB: A non-zero value may generate 
             an SNMP trap and/or SMTP email alert"  
      ::= { alarms 10 } 
 
   tDDSynchronizationStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       locked(0),
                       holdover(1),
                       holdoverNotConnected(2),
                       acquiringLock(3),
                       noTimingReference(4),
                       timingSystemNotConnected(5),
                       initialising(6),
                       clusterTimingMaster(7),
                       tDDSyncNotActive(8)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "An alarm value (displayed in red) indicates that one of 
             the following conditions has not been met (i) An external 
             timing system is connected or internal timing has been 
             configured. (ii) The timing system is providing a useable 
             reference. (iii) The ODU is locked to this reference."  
      ::= { alarms 11 } 
 
   managementPortDisabledWarning OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       disabledBySNMPifAdminStatus(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The SNMP ifAdminStatus of the out-of-band management 
             interface has disabled Ethernet traffic"  
      ::= { alarms 12 } 
 
   tDDSynchronizationAlarm OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       notSynchronized(1),
                       timingSystemFailure(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Not Synchronized indicates failure of the external 
             timing system for a period greater than the holdover 
             timer. TDD frame timing will have drifted, and this link 
             may cause interference with other links in a synchronized 
             network. Timing System Failure is an early warning, 
             indicating that 80% of the holdover period has expired."  
      ::= { alarms 13 } 
 
   linkModeOptimizationMismatch OBJECT-TYPE
      SYNTAX INTEGER {
                       ok(0),
                       linkModeOptimizationMismatch(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The remote node of this link has been configured with a 
             different link mode optimization"  
      ::= { alarms 14 } 
 
   managementPortConfigurationMismatch OBJECT-TYPE
      SYNTAX INTEGER {
                       noError(0),
                       mismatchDetected(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The detection of Ethernet fragments (runt packets) when 
             the link is in full duplex is an indication of an 
             auto-negotiation or forced configuration mismatch. This 
             alarm is only raised if an Out-of-Band Management Mode 
             has been configured."  
      ::= { alarms 15 } 
 
   secureModeAlarm OBJECT-TYPE
      SYNTAX INTEGER {
                       secureModeIsActive(0),
                       secureModeIsNotConfigured(1),
                       secureModeIsConfiguredButNotActive(2),
                       secureModeIsNotSupported(3)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The secure mode (e.g. FIPS, UC-APL) state of the unit. 
             The secure mode is not configured(1) state indicates that 
             the unit is capable of secure mode operation, and one or 
             more of the following security materials has not been 
             configured: Key Of Keys, Private Key, Public Certificate, 
             DRNG Entropy Status, Wireless Encryption Key. The secure 
             mode mode is configured but not active(2) state indicates 
             that the unit is capable of secure mode operation, and 
             the security material has been configured, but the 
             configuration of interfaces is not consistent with secure 
             mode operation. The secure mode is not supported(3) state 
             indicates that the unit is not capable of secure mode 
             operation. The secure mode capability requires 
             appropriate hardware compatibility, license key and 
             software image."  
      ::= { alarms 16 } 
 
   ethernetBridgingStatusAlarm OBJECT-TYPE
      SYNTAX INTEGER {
                       ethernetBridgingEnabled(0),
                       ethernetBridgingDisabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Ethernet traffic bridging is disabled because the 
             wireless link is not operating at the configured Lowest 
             Ethernet Modulation Mode"  
      ::= { alarms 17 } 
 
   -- Smtp group attribute definitions 
   --
   sMTPEmailAlert OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Simple Mail Transfer Protocol is used to send equipment 
             alerts via email to a specified email address"  
      ::= { smtp 1 } 
 
   sMTPServerIPAddress OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "IP address of the SMTP server"  
      ::= { smtp 2 } 
 
   sMTPServerPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Port number of the SMTP server"  
      ::= { smtp 3 } 
 
   sMTPSourceEmailAddress OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The 'from' email address used when constructing the 
             automatically generated e-mail message"  
      ::= { smtp 4 } 
 
   sMTPDestinationEmailAddress OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The 'to' email address used when constructing the 
             automatically generated e-mail message"  
      ::= { smtp 5 } 
 
   sMTPEnabledMessages OBJECT-TYPE
      SYNTAX BITS {
                    telecomsChannelUpDown(1),
                    managementPortUpDown(2),
                    dataPortUpDown(3),
                    enabledDiagnosticAlarms(4),
                    dFSImpulseInterference(5),
                    channelChange(6),
                    wirelessLinkUpDown(7)
                  }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls which SMTP messages the unit will send"  
      ::= { smtp 6 } 
 
   sMTPServerInternetAddressType OBJECT-TYPE
      SYNTAX INTEGER {
                       unknown(0),
                       ipv4(1),
                       ipv6(2),
                       ipv4z(3),
                       ipv6z(4),
                       unknown6(5),
                       unknown7(6),
                       unknown8(7),
                       unknown9(8),
                       unknown10(9),
                       unknown11(10),
                       unknown12(11),
                       unknown13(12),
                       unknown14(13),
                       unknown15(14),
                       unknown16(15),
                       dns(16)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The type of Internet address specified by the associated 
             sMTPServerInternetAddress."  
      ::= { smtp 7 } 
 
   sMTPServerInternetAddress OBJECT-TYPE
      SYNTAX InetAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Internet address of the SMTP server"  
      ::= { smtp 8 } 
 
   -- SnmpControl group attribute definitions 
   --
   sNMPPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The IP port number used to access the SNMP MIB (i.e. 
             Gets and Sets) (default = 161). NB: A system reboot is 
             required to activate changes to this attribute"  
      ::= { snmpControl 1 } 
 
   sNMPCommunityString OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The SNMP community string. NB: A system reboot is 
             required to activate changes to this attribute"  
      ::= { snmpControl 2 } 
 
   sNMPTrapTableNumber OBJECT-TYPE
      SYNTAX INTEGER (2)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the sNMPTrapTable."  
      ::= { snmpControl 3 } 
 
   sNMPTrapVersion OBJECT-TYPE
      SYNTAX INTEGER {
                       v1(0),
                       v2c(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The SNMP protocol version to use for SNMP Traps. NB: A 
             system reboot is required to activate changes to this 
             attribute"  
      ::= { snmpControl 5 } 
 
   sNMPEnabledTraps OBJECT-TYPE
      SYNTAX BITS {
                    managementPortUpDown(0),
                    dataPortUpDown(1),
                    authenticationFailure(2),
                    enabledDiagnosticAlarms(3),
                    dFSImpulseInterference(4),
                    channelChange(5),
                    wirelessLinkUpDown(6),
                    coldStart(7),
                    telecomsChannelUpDown(15)
                  }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "This controls which SNMP Traps the unit will send"  
      ::= { snmpControl 6 } 
 
   enabledDiagnosticAlarms OBJECT-TYPE
      SYNTAX BITS {
                    incompatibleMasterAndSlave(0),
                    incompatibleRegionCodes(1),
                    unknown6(2),
                    unknown5(3),
                    unitOutOfCalibration(4),
                    installArmState(5),
                    installStatus(6),
                    regionCode(7),
                    telecomsChannelAStatus(8),
                    dataPortFiberStatus(9),
                    dataPortStatus(10),
                    dataPortDisabledWarning(11),
                    wirelessLinkDisabledWarning(12),
                    sNTPSynchronizationFailed(13),
                    noWirelessChannelAvailable(14),
                    dataPortConfigurationMismatch(15),
                    syslogDisabledWarning(16),
                    linkModeOptimizationMismatch(17),
                    managementPortStatus(18),
                    managementPortDisabledWarning(19),
                    tDDSynchronizationAlarm(20),
                    telecomsChannelBLoopback(21),
                    telecomsChannelALoopback(22),
                    telecomsChannelBStatus(23),
                    ethernetBridgingStatus(26),
                    secureMode(27),
                    syslogClientDisabledWarning(28),
                    managementPortConfigurationMismatch(29),
                    syslogLocalWrapped(30),
                    syslogLocalNearlyFull(31)
                  }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Controls which individual diagnostic alarms are enabled. 
             The unit may be configured to generate SNMP traps and/or 
             SMTP email alerts for these enabled alarms by selecting 
             'Enabled Diagnostic Alarms' on the 'SNMP Enabled Traps' 
             and/or 'SMTP Enabled Messages' attributes"  
      ::= { snmpControl 7 } 
 
   sNMPSendAllTrapsAtStartup OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Controls whether or not all the enabled traps and alarms 
             (including cleared alarms) are reported at start-up."  
      ::= { snmpControl 8 } 
 
   -- SNMPTrapTable group attribute definitions 
   --
   sNMPTrapTableIndex OBJECT-TYPE
      SYNTAX INTEGER (1..2)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "SNMP trap value, used to index the SNMPTrapTable."  
      ::= { sNMPTrapTableEntry 1 } 
 
   sNMPTrapIPAddress OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The IP address to which all SNMP Traps are sent. NB: A 
             system reboot is required to activate changes to this 
             attribute."  
      ::= { sNMPTrapTableEntry 2 } 
 
   sNMPTrapPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Destination port for SNMP Traps (default=162). NB: A 
             system reboot is required to activate changes to this 
             attribute."  
      ::= { sNMPTrapTableEntry 3 } 
 
   sNMPTrapInternetAddressType OBJECT-TYPE
      SYNTAX INTEGER {
                       unknown(0),
                       ipv4(1),
                       ipv6(2),
                       ipv4z(3),
                       ipv6z(4),
                       unknown6(5),
                       unknown7(6),
                       unknown8(7),
                       unknown9(8),
                       unknown10(9),
                       unknown11(10),
                       unknown12(11),
                       unknown13(12),
                       unknown14(13),
                       unknown15(14),
                       unknown16(15),
                       dns(16)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The type of Internet address specified by the associated 
             sNMPTrapInternetAddress."  
      ::= { sNMPTrapTableEntry 4 } 
 
   sNMPTrapInternetAddress OBJECT-TYPE
      SYNTAX InetAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The Internet address to which all SNMP Traps are sent."  
      ::= { sNMPTrapTableEntry 5 } 
 
   sNMPTrapReceiverEnabled OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "A value of 0 disables the sending of SNMP trap to 
             corresponding receiver. A value of 1 enables the sending 
             of SNMP trap to corresponding receiver."  
      ::= { sNMPTrapTableEntry 6 } 
 
   -- Sntp group attribute definitions 
   --
   sNTPState OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "SNTP control state"  
      ::= { sntp 1 } 
 
   sNTPPollInterval OBJECT-TYPE
      SYNTAX INTEGER (60..43200)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The SNTP server polling interval"  
      ::= { sntp 4 } 
 
   sNTPSync OBJECT-TYPE
      SYNTAX INTEGER {
                       noSync(0),
                       inSync(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "If SNTP Sync fails then check the server settings in the 
             Remote Management page, or disable SNTP"  
      ::= { sntp 5 } 
 
   sNTPLastSync OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Last SNTP sync time"  
      ::= { sntp 6 } 
 
   systemClock OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "System clock presented as local time"  
      ::= { sntp 7 } 
 
   timeZone OBJECT-TYPE
      SYNTAX INTEGER {
                       gmtMinus1200(0),
                       gmtMinus1130(1),
                       gmtMinus1100(2),
                       gmtMinus1030(3),
                       gmtMinus1000(4),
                       gmtMinus0930(5),
                       gmtMinus0900(6),
                       gmtMinus0830(7),
                       gmtMinus0800(8),
                       gmtMinus0730(9),
                       gmtMinus0700(10),
                       gmtMinus0630(11),
                       gmtMinus0600(12),
                       gmtMinus0530(13),
                       gmtMinus0500(14),
                       gmtMinus0430(15),
                       gmtMinus0400(16),
                       gmtMinus0330(17),
                       gmtMinus0300(18),
                       gmtMinus0230(19),
                       gmtMinus0200(20),
                       gmtMinus0130(21),
                       gmtMinus0100(22),
                       gmtMinus0030(23),
                       gmtZero(24),
                       gmtPlus0030(25),
                       gmtPlus0100(26),
                       gmtPlus0130(27),
                       gmtPlus0200(28),
                       gmtPlus0230(29),
                       gmtPlus0300(30),
                       gmtPlus0330(31),
                       gmtPlus0400(32),
                       gmtPlus0430(33),
                       gmtPlus0500(34),
                       gmtPlus0530(35),
                       gmtPlus0600(36),
                       gmtPlus0630(37),
                       gmtPlus0700(38),
                       gmtPlus0730(39),
                       gmtPlus0800(40),
                       gmtPlus0830(41),
                       gmtPlus0900(42),
                       gmtPlus0930(43),
                       gmtPlus1000(44),
                       gmtPlus1030(45),
                       gmtPlus1100(46),
                       gmtPlus1130(47),
                       gmtPlus1200(48),
                       gmtPlus1230(49),
                       gmtPlus1300(50)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Time zone offsets from Greenwich Mean Time (GMT)"  
      ::= { sntp 8 } 
 
   daylightSaving OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Daylight Saving Time"  
      ::= { sntp 9 } 
 
   sNTPPrimaryServer OBJECT-TYPE
      SYNTAX INTEGER {
                       server1(0),
                       server2(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Specifies the primary SNTP server, determining the order 
             in which the servers are tried."  
      ::= { sntp 10 } 
 
   sNTPPrimaryServerDeadTime OBJECT-TYPE
      SYNTAX INTEGER (0..86400)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Time (in seconds) to wait before retrying communications 
             with an unresponsive primary SNTP server. Setting the 
             value to 0 disables the timer."  
      ::= { sntp 11 } 
 
   sNTPServerRetries OBJECT-TYPE
      SYNTAX INTEGER (0..10)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Number of times the PTP will retry after an SNTP server 
             fails to respond."  
      ::= { sntp 12 } 
 
   sNTPServerTimeout OBJECT-TYPE
      SYNTAX INTEGER (1..15)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Time (in seconds) the PTP will wait for a response from 
             an SNTP server."  
      ::= { sntp 13 } 
 
   sNTPServerTableNumber OBJECT-TYPE
      SYNTAX INTEGER (2)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the SNTPServerTable."  
      ::= { sntp 14 } 
 
   -- SNTPServerTable group attribute definitions 
   --
   sNTPServerTableIndex OBJECT-TYPE
      SYNTAX INTEGER (1..2)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "Index range for the SNTPServerTable."  
      ::= { sNTPServerTableEntry 1 } 
 
   sNTPServerIPAddress OBJECT-TYPE
      SYNTAX IpAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The IP address of a valid SNTP server"  
      ::= { sNTPServerTableEntry 2 } 
 
   sNTPServerPortNumber OBJECT-TYPE
      SYNTAX INTEGER (0..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The IP port number of the SNTP server. Defaults to port 
             123."  
      ::= { sNTPServerTableEntry 3 } 
 
   sNTPServerStatus OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..127))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Status message reflecting the result of communications 
             with the SNTP server when last polled"  
      ::= { sNTPServerTableEntry 4 } 
 
   sNTPServerInternetAddressType OBJECT-TYPE
      SYNTAX INTEGER {
                       unknown(0),
                       ipv4(1),
                       ipv6(2),
                       ipv4z(3),
                       ipv6z(4),
                       unknown6(5),
                       unknown7(6),
                       unknown8(7),
                       unknown9(8),
                       unknown10(9),
                       unknown11(10),
                       unknown12(11),
                       unknown13(12),
                       unknown14(13),
                       unknown15(14),
                       unknown16(15),
                       dns(16)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The type of Internet address specified by the associated 
             sNTPServerInternetAddress."  
      ::= { sNTPServerTableEntry 5 } 
 
   sNTPServerInternetAddress OBJECT-TYPE
      SYNTAX InetAddress
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The Internet address of a valid SNTP server"  
      ::= { sNTPServerTableEntry 6 } 
 
   -- Reset group attribute definitions 
   --
   systemReset OBJECT-TYPE
      SYNTAX INTEGER {
                       running(0),
                       consoleReboot(1)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "Setting this attribute to '1' will cause a system 
             reboot. NB: a system reboot will apply any pending new 
             settings held in memory"  
      ::= { reset 1 } 
 
   -- Versions group attribute definitions 
   --
   softwareVersion OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current software version"  
      ::= { versions 1 } 
 
   hardwareVersion OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Hardware platform version"  
      ::= { versions 2 } 
 
   secondarySoftwareVersion OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Secondary software version, used when the primary 
             software image is invalid or erased"  
      ::= { versions 3 } 
 
   bootVersion OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..63))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Boot code software version"  
      ::= { versions 4 } 
 
   -- PubStats group attribute definitions 
   --
   receiveDataRate OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Average data rate over the last one second interval 
             (kbps)"  
      ::= { pubStats 1 } 
 
   transmitDataRate OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Average data rate over the last one second interval 
             (kbps)"  
      ::= { pubStats 2 } 
 
   aggregateDataRate OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Average data rate over the last one second interval 
             (kbps)"  
      ::= { pubStats 3 } 
 
   wirelessLinkAvailability OBJECT-TYPE
      SYNTAX INTEGER (0..1000000)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Link availability calculated since the last reset of the 
             system counters, as a percentage multiplied by 10000 to 
             give four decimal places of precision"  
      ::= { pubStats 4 } 
 
   wirelessLinkStatus OBJECT-TYPE
      SYNTAX INTEGER {
                       up(0),
                       registering(1),
                       searching(2),
                       acquiring(3),
                       radarCAC(4),
                       initialising(5)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Current status of the wireless link"  
      ::= { pubStats 5 } 
 
   byteErrorRatio OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Reciprocal of the byte error ratio calculated since the 
             last reset of the system counters"  
      ::= { pubStats 6 } 
 
   receiveModulationModeDetail OBJECT-TYPE
      SYNTAX INTEGER {
                       runningAtMaximumReceiveMode(0),
                       runningAtUserConfiguredMaxModulationMode(1),
                       restrictedBecauseInstallationIsArmed(2),
                       restrictedBecauseOfByteErrorsOnTheWirelessLink(3),
                       restrictedBecauseTheLinkParametersAreUpdating(4),
                       restrictedBecauseChannelChangeIsInProgress(5),
                       restrictedDueToTheLowEthernetLinkSpeed(6),
                       runningAtMaximumReceiveModeForChannelBandwidth(7),
                       limitedByTheWirelessConditions(8)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The reason for the current receive modulation mode"  
      ::= { pubStats 7 } 
 
   ethernetBridgingAvailability OBJECT-TYPE
      SYNTAX INTEGER (0..1000000)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Link availability bridging Ethernet traffic calculated 
             since the last reset of the system counters, as a 
             percentage multiplied by 10000 to give four decimal 
             places of precision"  
      ::= { pubStats 8 } 
 
   -- Encryption group attribute definitions 
   --
   encryptionAlgorithm OBJECT-TYPE
      SYNTAX INTEGER {
                       none(0),
                       aESRijndael(1),
                       aES256bitRijndael(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The Encryption Algorithm used by the wireless link. NB: 
             A system reboot is required to activate changes to this 
             attribute. NB: The same Encryption Algorithm must be 
             configured at BOTH ends of the link for it to function 
             correctly"  
      ::= { encryption 1 } 
 
   -- TDDControl group attribute definitions 
   --
   tDDSynchronizationMode OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "TDD Synchronization Mode selection"  
      ::= { tDDControl 1 } 
 
   -- AAAControl group attribute definitions 
   --
   userTableNumber OBJECT-TYPE
      SYNTAX INTEGER (1..10)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Number of entries in the userTable"  
      ::= { aAAControl 1 } 
 
   -- UserTable group attribute definitions 
   --
   userTableIndex OBJECT-TYPE
      SYNTAX INTEGER (1..10)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
             "used to index values in the userTable."  
      ::= { userTableEntry 1 } 
 
   userName OBJECT-TYPE
      SYNTAX OCTET STRING
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "User name which must be entered, along with the 
             appropriate password, in order to gain access to the 
             system."  
      ::= { userTableEntry 2 } 
 
   userRole OBJECT-TYPE
      SYNTAX INTEGER {
                       readOnly(0),
                       systemAdministrator(1),
                       securityOfficer(2)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Role of the selected user. A Security Officer has access 
             to and can modify all settings. A System Administrator 
             has access to and can modify all non-security settings. A 
             Read Only user can view settings, but cannot make any 
             changes."  
      ::= { userTableEntry 3 } 
 
   userEnabled OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Enable / Disable the selected user"  
      ::= { userTableEntry 4 } 
 
   userPassword OBJECT-TYPE
      SYNTAX OCTET STRING
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "User password, which must be entered in order to gain 
             access to the system."  
      ::= { userTableEntry 5 } 
 
   -- SyslogControl group attribute definitions 
   --
   syslogClient OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "Enable or disable the syslog client"  
      ::= { syslogControl 1 } 
 
   syslogState OBJECT-TYPE
      SYNTAX INTEGER {
                       disabled(0),
                       enabled(1)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The syslog service has been enabled or disabled"  
      ::= { syslogControl 2 } 
 
   -- Supplementary group attribute definitions 
   --
   longitude OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..19))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The longitude of the unit, measured in decimal degrees. 
             This object is set by the SNMP manager and has no 
             internal function."  
      ::= { supplementary 1 } 
 
   latitude OBJECT-TYPE
      SYNTAX DisplayString (SIZE(0..19))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The latitude of the unit, measured in decimal degrees. 
             This object is set by the SNMP manager and has no 
             internal function."  
      ::= { supplementary 2 } 
 
   altitude OBJECT-TYPE
      SYNTAX Integer32
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
             "The altitude of the unit, measured in metres. This 
             object is set by the SNMP manager and has no internal 
             function."  
      ::= { supplementary 3 } 
 
   -- Enterprise NOTIFICATION definitions
   --

   channelChangeTrap NOTIFICATION-TYPE
      OBJECTS { receiveChannel }
      STATUS current
      DESCRIPTION "The PTP radio has changed wireless channel.
                 This has been caused by either
                 i) mandatory radar avoidance,
                    a DFS impulsive interference event will also be
                    detected,
                 or
                 ii) Dynamic Spectrum Optimization, (DSO)
                     DSO improves link performance by selecting the
                     most appropriate transmit and receive channels
                     with the lowest level of interference."
      ::= { ptpTrapPrefix 1 }

   dfsImpulsiveInterferenceTrap NOTIFICATION-TYPE
      OBJECTS { receiveChannel }
      STATUS current
      DESCRIPTION "DFS impulsive interference detected event"
      ::= { ptpTrapPrefix 2 }

   dataPortStatusTrap NOTIFICATION-TYPE
      OBJECTS { dataPortStatus }
      STATUS current
      DESCRIPTION
             "Current status of the Ethernet link. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { ptpTrapPrefix 3 }

   telecomsChannelAStatusTrap NOTIFICATION-TYPE
      OBJECTS { telecomsChannelAStatus }
      STATUS current
      DESCRIPTION
             "Current status of telecoms channel A. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { ptpTrapPrefix 4 }

   telecomsChannelBStatusTrap NOTIFICATION-TYPE
      OBJECTS { telecomsChannelBStatus }
      STATUS current
      DESCRIPTION
             "Current status of telecoms channel B. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { ptpTrapPrefix 5 }

   channelALoopbackTrap NOTIFICATION-TYPE
      OBJECTS { channelALoopback }
      STATUS current
      DESCRIPTION
             "The loopback status of telecoms channel A. This is 
             intended for installation testing and should be set to 
             'None' for normal operation. The wire connections to a 
             unit can be tested by applying a 'Copper' loopback to the 
             local unit. The wireless connection to the remote unit 
             can be tested by applying a 'Wireless' loopback to the 
             remote unit with no loopback on the local unit. NB: a 
             change of state may generate an SNMP trap and/or SMTP 
             email alert"  
      ::= { ptpTrapPrefix 6 }

   channelBLoopbackTrap NOTIFICATION-TYPE
      OBJECTS { channelBLoopback }
      STATUS current
      DESCRIPTION
             "The loopback status of telecoms channel B. This is 
             intended for installation testing and should be set to 
             'None' for normal operation. The wire connections to a 
             unit can be tested by applying a 'Copper' loopback to the 
             local unit. The wireless connection to the remote unit 
             can be tested by applying a 'Wireless' loopback to the 
             remote unit with no loopback on the local unit. NB: a 
             change of state may generate an SNMP trap and/or SMTP 
             email alert"  
      ::= { ptpTrapPrefix 7 }

   regionCodeTrap NOTIFICATION-TYPE
      OBJECTS { regionCode }
      STATUS current
      DESCRIPTION
             "The region code prohibits the wireless unit from 
             operating outside the regulated limits. An invalid region 
             code indicates a corrupted license key. NB: a change of 
             state may generate an SNMP trap and/or SMTP email alert"  
      ::= { ptpTrapPrefix 8 }

   installStatusTrap NOTIFICATION-TYPE
      OBJECTS { installStatus }
      STATUS current
      DESCRIPTION
             "A non-zero value indicates that signalling was received 
             with the wrong MAC address or a mismatched link name. NB: 
             It is very unusual to detect this, because units with 
             mis-configured Target MAC Address will normally fail to 
             establish a wireless link. However, rare circumstances 
             may establish a partial wireless link and detect this 
             situation. NB: A non-zero value on start-up, or a change 
             of value during operation, may generate an SNMP trap 
             and/or SMTP email alert"  
      ::= { ptpTrapPrefix 9 }

   installArmStateTrap NOTIFICATION-TYPE
      OBJECTS { installArmState }
      STATUS current
      DESCRIPTION
             "Indicates if the unit is being installed. NB: a change 
             of state may generate an SNMP trap and/or SMTP email 
             alert"  
      ::= { ptpTrapPrefix 10 }

   unitOutOfCalibrationTrap NOTIFICATION-TYPE
      OBJECTS { unitOutOfCalibration }
      STATUS current
      DESCRIPTION
             "The unit is out of calibration"  
      ::= { ptpTrapPrefix 11 }

   incompatibleRegionCodesTrap NOTIFICATION-TYPE
      OBJECTS { incompatibleRegionCodes }
      STATUS current
      DESCRIPTION
             "The master and slave units have incompatible region 
             codes. NB: Both units must have compatible license keys"  
      ::= { ptpTrapPrefix 14 }

   noWirelessChannelAvailableTrap NOTIFICATION-TYPE
      OBJECTS { noWirelessChannelAvailable }
      STATUS current
      DESCRIPTION
             "Spectrum Management was unable to locate a suitable 
             wireless channel to operate on"  
      ::= { ptpTrapPrefix 15 }

   wirelessLinkDisabledWarningTrap NOTIFICATION-TYPE
      OBJECTS { wirelessLinkDisabledWarning }
      STATUS current
      DESCRIPTION
             "The SNMP ifAdminStatus of the wireless interface has 
             disabled wireless traffic"  
      ::= { ptpTrapPrefix 16 }

   dataPortDisabledWarningTrap NOTIFICATION-TYPE
      OBJECTS { dataPortDisabledWarning }
      STATUS current
      DESCRIPTION
             "The SNMP ifAdminStatus of the Ethernet interface has 
             disabled Ethernet traffic"  
      ::= { ptpTrapPrefix 17 }

   dataPortFiberStatusTrap NOTIFICATION-TYPE
      OBJECTS { dataPortFiberStatus }
      STATUS current
      DESCRIPTION
             "If the fiber link is not OK, there are three possible 
             causes: Either the fiber link has been installed but 
             disabled (because the license key does not include fiber 
             support), the link could not be established even though 
             no LOS was detected (i.e. an optical carrier was 
             detected, which could be due to a broken TX fiber, or 
             because the link is disabled at the fiber link partner), 
             or the link could not be established and LOS is detected 
             (i.e. no optical carrier is detected). NB: a change of 
             status may generate an SNMP trap and/or SMTP email alert"  
      ::= { ptpTrapPrefix 18 }

   dataPortConfigurationMismatchTrap NOTIFICATION-TYPE
      OBJECTS { dataPortConfigurationMismatch }
      STATUS current
      DESCRIPTION
             "The detection of Ethernet fragments (runt packets) when 
             the link is in full duplex is an indication of an 
             auto-negotiation or forced configuration mismatch"  
      ::= { ptpTrapPrefix 19 }

   incompatibleMasterAndSlaveTrap NOTIFICATION-TYPE
      OBJECTS { incompatibleMasterAndSlave }
      STATUS current
      DESCRIPTION
             "A non-zero value indicates that the master and slave 
             ends of a link are different hardware products, or have 
             different software versions. NB: It is very unusual to 
             detect this, because incompatible units will normally 
             fail to establish a wireless link. However, some 
             combinations may establish a partial wireless link and 
             detect this situation. NB: A non-zero value may generate 
             an SNMP trap and/or SMTP email alert"  
      ::= { ptpTrapPrefix 20 }

   sNTPSyncTrap NOTIFICATION-TYPE
      OBJECTS { sNTPSync }
      STATUS current
      DESCRIPTION
             "If SNTP Sync fails then check the server settings in the 
             Remote Management page, or disable SNTP"  
      ::= { ptpTrapPrefix 21 }

   tDDSynchronizationAlarmTrap NOTIFICATION-TYPE
      OBJECTS { tDDSynchronizationAlarm }
      STATUS current
      DESCRIPTION
             "Not Synchronized indicates failure of the external 
             timing system for a period greater than the holdover 
             timer. TDD frame timing will have drifted, and this link 
             may cause interference with other links in a synchronized 
             network. Timing System Failure is an early warning, 
             indicating that 80% of the holdover period has expired."  
      ::= { ptpTrapPrefix 22 }

   managementPortStatusTrap NOTIFICATION-TYPE
      OBJECTS { managementPortStatus }
      STATUS current
      DESCRIPTION
             "Current status of the out-of-band management link. NB: a 
             change of state may generate an SNMP trap and/or SMTP 
             email alert"  
      ::= { ptpTrapPrefix 23 }

   managementPortDisabledWarningTrap NOTIFICATION-TYPE
      OBJECTS { managementPortDisabledWarning }
      STATUS current
      DESCRIPTION
             "The SNMP ifAdminStatus of the out-of-band management 
             interface has disabled Ethernet traffic"  
      ::= { ptpTrapPrefix 24 }

   linkModeOptimizationMismatchTrap NOTIFICATION-TYPE
      OBJECTS { linkModeOptimizationMismatch }
      STATUS current
      DESCRIPTION
             "The remote node of this link has been configured with a 
             different link mode optimization"  
      ::= { ptpTrapPrefix 25 }

   managementPortConfigurationMismatchTrap NOTIFICATION-TYPE
      OBJECTS { managementPortConfigurationMismatch }
      STATUS current
      DESCRIPTION
             "The detection of Ethernet fragments (runt packets) when 
             the link is in full duplex is an indication of an 
             auto-negotiation or forced configuration mismatch. This 
             alarm is only raised if an Out-of-Band Management Mode 
             has been configured."  
      ::= { ptpTrapPrefix 28 }

   syslogStateTrap NOTIFICATION-TYPE
      OBJECTS { syslogState }
      STATUS current
      DESCRIPTION
             "The syslog service has been enabled or disabled"  
      ::= { ptpTrapPrefix 30 }

   syslogLocalNearlyFullTrap NOTIFICATION-TYPE
      STATUS current
      DESCRIPTION "The syslog local log is nearly full (90%)"
      ::= { ptpTrapPrefix 31 }

   syslogLocalWrappedTrap NOTIFICATION-TYPE
      STATUS current
      DESCRIPTION "The syslog local log has wrapped"
      ::= { ptpTrapPrefix 32 }

   syslogClientTrap NOTIFICATION-TYPE
      OBJECTS { syslogClient }
      STATUS current
      DESCRIPTION
             "Enable or disable the syslog client"  
      ::= { ptpTrapPrefix 33 }

   secureModeAlarmTrap NOTIFICATION-TYPE
      OBJECTS { secureModeAlarm }
      STATUS current
      DESCRIPTION
             "The secure mode (e.g. FIPS, UC-APL) state of the unit. 
             The secure mode is not configured(1) state indicates that 
             the unit is capable of secure mode operation, and one or 
             more of the following security materials has not been 
             configured: Key Of Keys, Private Key, Public Certificate, 
             DRNG Entropy Status, Wireless Encryption Key. The secure 
             mode mode is configured but not active(2) state indicates 
             that the unit is capable of secure mode operation, and 
             the security material has been configured, but the 
             configuration of interfaces is not consistent with secure 
             mode operation. The secure mode is not supported(3) state 
             indicates that the unit is not capable of secure mode 
             operation. The secure mode capability requires 
             appropriate hardware compatibility, license key and 
             software image."  
      ::= { ptpTrapPrefix 34 }

   ethernetBridgingStatusAlarmTrap NOTIFICATION-TYPE
      OBJECTS { ethernetBridgingStatusAlarm }
      STATUS current
      DESCRIPTION
             "Ethernet traffic bridging is disabled because the 
             wireless link is not operating at the configured Lowest 
             Ethernet Modulation Mode"  
      ::= { ptpTrapPrefix 35 }

   END
