TELTONIKA-MIB DEFINITIONS ::= BEGIN

IMPORTS
    OBJECT-TYPE, NOTIFICATION-TYPE, MODULE-IDENTITY,
    Integer32, Opaque, enterprises, Counter32
        FROM SNMPv2-SMI

    TEXTUAL-CONVENTION, DisplayString, TruthValue
	FROM SNMPv2-TC

	NetworkAddress
	FROM SNMPv2-SMI;

teltonika MODULE-IDENTITY
    LAST-UPDATED "201307240000Z"
    ORGANIZATION "TELTONIKA"
    CONTACT-INFO "TELTONIKA"
    DESCRIPTION
            "The MIB module for TELTONIKA routers.
            "
    REVISION      "201307240000Z"
    DESCRIPTION
            "Initial version"
    ::= { enterprises 48690 }

-- the GSM group
--
-- a collection of objects to represent RUT2xx status.

static   OBJECT IDENTIFIER ::= { teltonika 1}

ModemImei OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx modem IMEI"
    ::= { static 1 }

ModemModel OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx modem model"
    ::= { static 2 }

ModemManufacturer OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx modem manufacturer"
    ::= { static 3 }

ModemRevision OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx modem revision"
    ::= { static 4 }

ModemSerial OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx modem serial number"
    ::= { static 5 }

Imsi OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx IMSI"
    ::= { static 6 }

RouterName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx router name"
    ::= { static 7 }

ProductCode OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx router product code"
    ::= { static 8 }

BatchNumber OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx router batch number"
    ::= { static 9 }

HardwareRevision OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx router hardware revision"
    ::= { static 10 }

gsm   OBJECT IDENTIFIER ::= { teltonika 2 }
SimState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx SIM status"
    ::= { gsm 1 }

PinState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx PIN status"
    ::= { gsm 2 }

NetState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx mobile network registration status"
    ::= { gsm 3 }

Signal OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx signal level"
    ::= { gsm 4 }

Operator OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx operator currently in use"
    ::= { gsm 5 }

OperatorNumber OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx operator number (MCC+MNC)"
    ::= { gsm 6 }

ConnectionState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx data session connection state"
    ::= { gsm 7 }

ConnectionType OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx data session connection type"
    ::= { gsm 8 }

Temperature OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx module temperature"
    ::= { gsm 9 }

ReceivedToday OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx 3G connection received bytes today"
    ::= { gsm 10 }

SentToday OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx 3G connection sent bytes today"
    ::= { gsm 11 }

ReceivedYesterday OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx 3G connection received bytes yesterday"
    ::= { gsm 12 }

SentYesterday OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx 3G connection sent bytes yesterday"
    ::= { gsm 13 }

FirmwareVersion OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx firmware version"
    ::= { gsm 14 }

SimSlot OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx sim slot in use"
    ::= { gsm 15 }

RouterUptime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx router uptime"
    ::= { gsm 16 }

ConnectionUptime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx mobile connection uptime"
    ::= { gsm 17 }

MobileIP OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx mobile connection IP"
    ::= { gsm 18 }

Sent OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx bytes sent"
    ::= { gsm 19 }

Received OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx bytes received"
    ::= { gsm 20 }

CellID OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx cellid parameter"
    ::= { gsm 21 }

SINR OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx LTE sinr level"
    ::= { gsm 22 }

RSRP OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx LTE rsrp level"
    ::= { gsm 23 }

RSRQ OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx LTE rsrq level"
    ::= { gsm 24 }

trap   OBJECT IDENTIFIER ::= { teltonika 4 }

trapSignalStrength NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION
            "RUT2xx Signal strength trap"
    ::= { trap 1 }

trapConnectionType NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION
            "RUT2xx Connection type trap"
    ::= { trap 2 }

trapDigitalInput NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION
            "RUT2xx Digital input trap"
    ::= { trap 3 }

trapDigitalInputStatus NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION
            "RUT2xx Digital input status"
    ::= { trap 4 }

trapDigitalOutput NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION
            "RUT2xx Digital output trap"
    ::= { trap 9 }

trapDigitalOutputStatus NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION
            "RUT2xx Digital output status"
    ::= { trap 10 }

rut2xx   OBJECT IDENTIFIER ::= { teltonika 5 }

DigitalInput OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx digital input"
    ::= { rut2xx 1 }

--
--
-- Hot Spot group
--
--
hotspot   OBJECT IDENTIFIER ::= { teltonika 3 }
hotspot1	OBJECT IDENTIFIER ::= { hotspot 1 }
hotspot2	OBJECT IDENTIFIER ::= { hotspot 2 }
hotspot3	OBJECT IDENTIFIER ::= { hotspot 3 }
hotspot4	OBJECT IDENTIFIER ::= { hotspot 4 }


--HOTSPOT1
--
--

hotSpotId OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Rut2xx hot spot id"
    ::= { hotspot1 1 }

hotSpotSsid OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Rut2xx hot spot ssid"
    ::= { hotspot1 2 }

hotSpotEnableState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot enable status"
    ::= { hotspot1 3 }

hotSpotIP OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot ip address"
    ::= { hotspot1 4 }

hotSpotDownloadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot download band width"
    ::= { hotspot1 5 }

hotSpotUploadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot upload band width"
    ::= { hotspot1 6 }

hotSpotUsers OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot existing users"
    ::= { hotspot1 7 }

hotSpotUsersPass OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot users passwords"
    ::= { hotspot1 8 }

hotSpotUsersActive OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot active users"
    ::= { hotspot1 9 }

hotSpotUsersMac OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user mac"
    ::= { hotspot1 10 }

hotSpotUsersIp OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user ip address"
    ::= { hotspot1 11 }

hotSpotUsersStartTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user connection to hotspot time"
    ::= { hotspot1 12 }

hotSpotUsersUseTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user active time"
    ::= { hotspot1 13 }

hotSpotUsersDownload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user downloaded data"
    ::= { hotspot1 14 }

hotSpotUsersUpload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user uploaded data"
    ::= { hotspot1 15 }

hotSpotEndTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user last connection time"
    ::= { hotspot1 16 }

--HOTSPOT2
--
--
--

hotSpotId OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Rut2xx hot spot id"
    ::= { hotspot2 1 }

hotSpotSsid OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Rut2xx hot spot ssid"
    ::= { hotspot2 2 }

hotSpotEnableState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot enable state"
    ::= { hotspot2 3 }

hotSpotIP OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot ip address"
    ::= { hotspot2 4 }

hotSpotDownloadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot download band width"
    ::= { hotspot2 5 }

hotSpotUploadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot upload band width"
    ::= { hotspot2 6 }

hotSpotUsers OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot existing users"
    ::= { hotspot2 7 }

hotSpotUsersPass OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot users passwords"
    ::= { hotspot2 8 }

hotSpotUsersActive OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot active users"
    ::= { hotspot2 9 }

hotSpotUsersMac OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user mac"
    ::= { hotspot2 10 }

hotSpotUsersIp OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user ip address"
    ::= { hotspot2 11 }

hotSpotUsersStartTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user connection to hotspot time"
    ::= { hotspot2 12 }

hotSpotUsersUseTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user active time"
    ::= { hotspot2 13 }

hotSpotUsersDownload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user downloaded data"
    ::= { hotspot2 14 }

hotSpotUsersUpload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user uploaded data"
    ::= { hotspot2 15 }

hotSpotEndTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user last connection time"
    ::= { hotspot2 16 }

--HOTSPOT3
--
--
--

hotSpotId OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Rut2xx hot spot id"
    ::= { hotspot3 1 }

hotSpotSsid OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Rut2xx hot spot ssid"
    ::= { hotspot3 2 }

hotSpotEnableState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot enable state"
    ::= { hotspot3 3 }

hotSpotIP OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot ip address"
    ::= { hotspot3 4 }

hotSpotDownloadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot download band width"
    ::= { hotspot3 5 }

hotSpotUploadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot upload band width"
    ::= { hotspot3 6 }

hotSpotUsers OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot existing users"
    ::= { hotspot3 7 }

hotSpotUsersPass OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot users passwords"
    ::= { hotspot3 8 }

hotSpotUsersActive OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot active users"
    ::= { hotspot3 9 }

hotSpotUsersMac OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user mac"
    ::= { hotspot3 10 }

hotSpotUsersIp OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user ip address"
    ::= { hotspot3 11 }

hotSpotUsersStartTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user connection to hotspot time"
    ::= { hotspot3 12 }

hotSpotUsersUseTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user active time"
    ::= { hotspot3 13 }

hotSpotUsersDownload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user downloaded data"
    ::= { hotspot3 14 }

hotSpotUsersUpload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user uploaded data"
    ::= { hotspot3 15 }

hotSpotEndTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user last connection time"
    ::= { hotspot3 16 }

--HOTPSOT4
--
--
--

hotSpotId OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Rut2xx hot spot id"
    ::= { hotspot4 1 }

hotSpotSsid OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Rut2xx hot spot ssid"
    ::= { hotspot4 2 }

hotSpotEnableState OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot enable state"
    ::= { hotspot4 3 }

hotSpotIP OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot ip address"
    ::= { hotspot4 4 }

hotSpotDownloadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot download band width"
    ::= { hotspot4 5 }

hotSpotUploadBandWidth OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot upload band width"
    ::= { hotspot4 6 }

hotSpotUsers OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot existing users"
    ::= { hotspot4 7 }

hotSpotUsersPass OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot users passwords"
    ::= { hotspot4 8 }

hotSpotUsersActive OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot active users"
    ::= { hotspot4 9 }

hotSpotUsersMac OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user mac"
    ::= { hotspot4 10 }

hotSpotUsersIp OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user ip address"
    ::= { hotspot4 11 }

hotSpotUsersStartTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user connection to hotspot time"
    ::= { hotspot4 12 }

hotSpotUsersUseTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user active time"
    ::= { hotspot4 13 }

hotSpotUsersDownload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user downloaded data"
    ::= { hotspot4 14 }

hotSpotUsersUpload OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user uploaded data"
    ::= { hotspot4 15 }

hotSpotEndTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "RUT2xx hot spot user last connection time"
    ::= { hotspot4 16 }

END