OAW-AP1232 DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE, 
        enterprises, Integer32, Unsigned32, OBJECT-TYPE, MODULE-IDENTITY,
        NOTIFICATION-TYPE, Counter32
                 FROM SNMPv2-SMI
		deviceNGOAWAp1232
				FROM
		ALCATEL-NGOAW-DEVICES-MIB				 
        DisplayString , MacAddress, RowStatus,
        TruthValue                              FROM SNMPv2-TC

        MODULE-COMPLIANCE, OBJECT-GROUP, 
        NOTIFICATION-GROUP                      FROM SNMPv2-CONF 

        ifIndex                                 FROM RFC1213-MIB;			
	
	apInfo      OBJECT IDENTIFIER ::= { deviceNGOAWAp1232 1 }


DisplayString ::=
    OCTET STRING

apBaseInfo       OBJECT IDENTIFIER ::= { apInfo 1 }
apRadioInfo       OBJECT IDENTIFIER ::= { apInfo 2 }
apWlanInfo       OBJECT IDENTIFIER ::= { apInfo 3 }
apClientInfo       OBJECT IDENTIFIER ::= { apInfo 4 }

-- the System group
-- **********************************************************************
-- * AP Info Table
-- **********************************************************************

apMacAddress OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 1 }

apSysName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 2 }

apIPAddress OBJECT-TYPE
    SYNTAX  NetworkAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 3 }
	
apGroupName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 4 }
	
apModel OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 5 }

apSerial  OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 6 }

apMemoryUtilization OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 7 }

apCpuUtilization OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 8}	
	
apSysUpTime OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { apBaseInfo 9 }

-- **********************************************************************
-- *apRadioInfoTable
-- **********************************************************************
apRadioInfoTable  OBJECT-TYPE
SYNTAX SEQUENCE OF ApRadioInfoEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
" "
::= { apRadioInfo  1}

ApRadioInfoEntry  OBJECT-TYPE
SYNTAX ApRadioInfoEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"  "
INDEX {apRadioIndex}
::= { apRadioInfoTable 1 }

ApRadioInfoEntry   ::=SEQUENCE {
apRadioIndex  Integer32,
apRadioMacAddress    DisplayString,
apRadioBand    INTEGER,
apRadioChannel       INTEGER,
apRadioTxpower     INTEGER,
apRadioUtilization     INTEGER,
apRadioTxTotalFrames     Counter64,
apRadioTxManagementFrames     Counter64,
apRadioTxDataFrames      Counter64,
apRadioTxBytes     Counter64,
apRadioTxDrops     Counter64,
apRadioRxTotalFrames     Counter64,
apRadioRxManagementFrames     Counter64,
apRadioRxDataFrames     Counter64,
apRadioRxBytes     Counter64,
apRadioRxBadFrames     Counter64}

apRadioIndex  OBJECT-TYPE
SYNTAX Integer32(1..20)
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
""
::={ApRadioInfoEntry 1}

apRadioMacAddress OBJECT-TYPE
SYNTAX  DisplayString
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApRadioInfoEntry 2}

apRadioBand   OBJECT-TYPE
SYNTAX  INTEGER
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApRadioInfoEntry 3}

apRadioChannel  OBJECT-TYPE
SYNTAX  INTEGER
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApRadioInfoEntry 4}

apRadioTxpower  OBJECT-TYPE
SYNTAX  INTEGER
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApRadioInfoEntry 5}

apRadioUtilization   OBJECT-TYPE
SYNTAX   INTEGER
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 6 }

apRadioTxTotalFrames  OBJECT-TYPE
SYNTAX    Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 7}

apRadioTxManagementFrames OBJECT-TYPE
SYNTAX    Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 8}

apRadioTxDataFrames  OBJECT-TYPE
SYNTAX   Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 9}

apRadioTxBytes  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 10}

apRadioTxDrops  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 11}

apRadioRxTotalFrames  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 12}

apRadioRxManagementFrames  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 13}

apRadioRxDataFrames  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 14}

apRadioRxBytes  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 15}

apRadioRxBadFrames  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
" "
::= { ApRadioInfoEntry 16}

-- **********************************************************************
-- *apWlanInfoTable
-- **********************************************************************
apWlanInfoTable  OBJECT-TYPE
SYNTAX SEQUENCE OF ApWlanInfoEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
" "
::= { apWlanInfo  1}

ApWlanInfoEntry  OBJECT-TYPE
SYNTAX ApWlanInfoEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
""
INDEX {apWlanIndex}
::= { apWlanInfoTable 1 }

ApWlanInfoEntry   ::=SEQUENCE {
apWlanIndex  Integer32,
apWlanMacAddress    DisplayString,
apWlanEssid   	 OCTET STRING,
apWlanTxTotalFrames     Counter64,
apWlanTxBytes     Counter64,
apWlanRxTotalFrames     Counter64,
apWlanRxBytes     Counter64}

apWlanIndex  OBJECT-TYPE
SYNTAX Integer32(1..20)
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
""
::={ApWlanInfoEntry 1}


apWlanEssid OBJECT-TYPE
SYNTAX  OCTET STRING
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApWlanInfoEntry 2}

apWlanMacAddress OBJECT-TYPE
SYNTAX  DisplayString
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApWlanInfoEntry 3}

apWlanTxTotalFrames   OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApWlanInfoEntry 4}

apWlanTxBytes  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApWlanInfoEntry 5}

apWlanRxTotalFrames  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApWlanInfoEntry 6}

apWlanRxBytes  OBJECT-TYPE
SYNTAX  Counter64
MAX-ACCESS  read-only
STATUS  current
DESCRIPTION
""
::= {ApWlanInfoEntry 7}

-- **********************************************************************
-- *apClientInfoTable
-- **********************************************************************
apClientInfoTable  OBJECT-TYPE
SYNTAX SEQUENCE OF ApClientInfoEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
" "
::= { apClientInfo  1}

ApClientInfoEntry  OBJECT-TYPE
SYNTAX ApClientInfoEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"  "
INDEX {apClientIndex}
::= { apClientInfoTable 1 }

ApClientInfoEntry   ::=SEQUENCE {
apClientIndex  Integer32,
apClientMacAddress    DisplayString,
apClientIPAddress    IpAddress,
apClientWlanService   	 OCTET STRING,
apClientSNR     INTEGER,
apClientDeviceFamily     OCTET STRING,
apClientOS     OCTET STRING,
apClientUptime     Integer32,
apClientTxFrames    Counter64,
apClientTxBytes   Counter64,
apClientTxRate   Counter64,
apClientTxRetries   Counter64,
apClientRxFrames   Counter64,
apClientRxBytes  Counter64,
apClientRxRate  Counter64,
apClientRxRetries Counter64
}

apClientIndex  OBJECT-TYPE
SYNTAX Integer32(1..20)
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
""
::={ApClientInfoEntry 1}

apClientMacAddress OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { ApClientInfoEntry 2 }

apClientIPAddress OBJECT-TYPE
    SYNTAX  NetworkAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { ApClientInfoEntry 3 }

apClientWlanService OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { ApClientInfoEntry 4 }
	
apClientSNR OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    ""
    ::= { ApClientInfoEntry 5 }

apClientDeviceFamily OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 6 }

apClientOS OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 7 }

apClientUptime OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 8}

apClientTxFrames OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 9}	

apClientTxBytes OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 10}	
	
apClientTxRate OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 11}	

apClientTxRetries OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 12}
	
apClientRxFrames OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 13}	

apClientRxBytes OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 14}	

apClientRxRate OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 15}		

apClientRxRetries OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	""
    ::= { ApClientInfoEntry 16}	
	
END
