-- file: rfc1442v.smi - SNMPv1 version of RFC 1442

SNMPv2-SMI-v1 DEFINITIONS ::= BEGIN

          IMPORTS
                  NetworkAddress, IpAddress, Counter, Gauge,
                  TimeTicks
                    FROM RFC1155-SMI
                  OBJECT-TYPE
                    FROM RFC-1212;

-- No macro MODULE-IDENTITY in SNMPv1
-- No macro OBJECT-IDENTITY in SNMPv1
-- SMI Counter
Counter-32 ::= Counter
-- Counter64 - no equivalent in SNMPv1
-- SMI Gauge
Gauge-32 ::= Gauge
Integer-32 ::= INTEGER (-2147483648..2147483647)
Unsigned-32 ::= Gauge
-- SMI IpAddress
-- NsapAddress - no equivalent in SNMPv1
-- SMI Opaque
-- SMI TimeTicks
-- UInteger32 - no equivalent in SNMPv1
-- Using defintion of macro OBJECT-TYPE from RFC 1212
-- No macro NOTIFICATION-TYPE in SNMPv1

internet        OBJECT IDENTIFIER ::= { iso org(3) dod(6) 1 }
directory       OBJECT IDENTIFIER ::= { internet 1 }
mgmt            OBJECT IDENTIFIER ::= { internet 2 }
experimental    OBJECT IDENTIFIER ::= { internet 3 }
private         OBJECT IDENTIFIER ::= { internet 4 }
enterprises     OBJECT IDENTIFIER ::= { private 1 }
security        OBJECT IDENTIFIER ::= { internet 5 }
snmpV2          OBJECT IDENTIFIER ::= { internet 6 }
snmpDomains     OBJECT IDENTIFIER ::= { snmpV2 1 }
snmpProxys      OBJECT IDENTIFIER ::= { snmpV2 2 }
snmpModules     OBJECT IDENTIFIER ::= { snmpV2 3 }


END

