
	ALCATEL-IND1-LAG-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE, Integer32, Counter32, TimeTicks
			FROM SNMPv2-SMI
		DisplayString, MacAddress, TEXTUAL-CONVENTION, RowStatus
			FROM SNMPv2-TC
	        NOTIFICATION-TYPE              FROM SNMPv2-SMI
		NOTIFICATION-GROUP             FROM SNMPv2-CONF
		MODULE-COMPLIANCE, OBJECT-GROUP
			FROM SNMPv2-CONF
		InterfaceIndex
			FROM IF-MIB
		PortList
			FROM Q-BRIDGE-MIB
                LacpKey,LacpState,ChurnState
			FROM IEEE8023-LAG-MIB

                lnkaggTraps,
		softentIND1LnkAgg
			FROM ALCATEL-IND1-BASE 

	;
	alcatelIND1LAGMIB MODULE-IDENTITY
		LAST-UPDATED "200704030000Z"
		ORGANIZATION "Alcatel-Lucent"
		CONTACT-INFO
		    "Please consult with Customer Service to ensure the most appropriate
		     version of this document is used with the products in question:
 	
				Alcatel-Lucent, Enterprise Solutions Division
			       (Formerly Alcatel Internetworking, Incorporated)
				       26801 West Agoura Road
			 	   Agoura Hills, CA  91301-5122
			      		United States Of America
	
	    	     Telephone:              North America  +1 800 995 2696
			 	     	     Latin America  +1 877 919 9526
					     Europe         +31 23 556 0100
				     	     Asia           +65 394 7933
				     	     All Other      +1 818 878 4507
	
	             Electronic Mail:         support@ind.alcatel.com
	             World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
	             File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

	DESCRIPTION
        "This module describes an authoritative enterprise-specific Simple
         Network Management Protocol (SNMP) Management Information Base (MIB):
         
			   The Link Aggregation module for managing  ALCATEL FALCON product
			   This MIB is an image of the  802.3ad standard. 
     		 The aim of this proprietary MIB is to allow the creation of
         aggregate objects with their size.
         
         The right to make changes in specification and other information
         contained in this document without prior notice is reserved.
         
         No liability shall be assumed for any incidental, indirect, special, or
         consequential damages whatsoever arising from or related to this
         document or the information contained herein.
         
         Vendors, end-users, and other interested parties are granted
         non-exclusive license to use this specification in connection with
         management of the products for which it is intended to be used.
         
                     Copyright (C) 1995-2007 Alcatel-Lucent
                         ALL RIGHTS RESERVED WORLDWIDE"

		::= { softentIND1LnkAgg 1 }


	alcatelIND1LAGMIBObjects OBJECT IDENTIFIER ::= { alcatelIND1LAGMIB 1 }


	-- -------------------------------------------------------------
	-- Textual Conventions
	-- -------------------------------------------------------------





--	- Local Declares

   LacpType ::= TEXTUAL-CONVENTION
		STATUS current
		DESCRIPTION
			"The object supports or not (Omnichannel) the LACP protocol ."
		SYNTAX INTEGER {
			lacpOff(0),
			lacpOn(1)
				}

		
		
	-- -------------------------------------------------------------
	

	-- -------------------------------------------------------------
	-- groups in the LAG MIB
	-- -------------------------------------------------------------


	alclnkaggAgg OBJECT IDENTIFIER ::= { alcatelIND1LAGMIBObjects 1 }
	alclnkaggAggPort OBJECT IDENTIFIER ::= { alcatelIND1LAGMIBObjects 2 }


	-- -------------------------------------------------------------
	
	-- -------------------------------------------------------------
	-- The Tables Last Changed Object
	-- -------------------------------------------------------------



	alclnkaggTablesLastChanged OBJECT-TYPE
		SYNTAX TimeTicks
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This object indicates the time of the
			most recent change to the alclnkaggAggTable,
			alclnkaggAggPortListTable, or
			alclnkaggAggPortTable."
	::= { alcatelIND1LAGMIBObjects 3 }
	



	
	-- -------------------------------------------------------------
	-- The Aggregator Configuration Table
	-- -------------------------------------------------------------
	

	alclnkaggAggTable OBJECT-TYPE
		SYNTAX SEQUENCE OF AlclnkaggAggEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A table that contains information about every
			Aggregator that is associated with this System.
                        To create specify alclnkaggAggIndex,alclnkaggAggSize
                        and alclnkaggAggLacpType. "
    
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1"
		::= { alclnkaggAgg 1 }


	alclnkaggAggEntry OBJECT-TYPE
		SYNTAX AlclnkaggAggEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A list of the Aggregator parameters. This is indexed
			by the ifIndex of the Aggregator."
		INDEX { alclnkaggAggIndex }
		::= { alclnkaggAggTable 1 }


	AlclnkaggAggEntry ::=
		SEQUENCE {
		alclnkaggAggIndex
			InterfaceIndex,
		alclnkaggAggMACAddress
			MacAddress,
        	alclnkaggAggActorSystemPriority
			INTEGER,
		alclnkaggAggActorSystemID
			MacAddress,
		alclnkaggAggPartnerAdminKey
			 LacpKey,
		alclnkaggAggActorAdminKey
			LacpKey,
		alclnkaggAggActorOperKey
			LacpKey,
		alclnkaggAggPartnerSystemID
			MacAddress,
		alclnkaggAggPartnerSystemPriority
			INTEGER,
		alclnkaggAggPartnerOperKey
			LacpKey,
--------------------------------
--   Specific Proprietary Part
------------------------------ 
		alclnkaggAggSize
			 INTEGER,
		alclnkaggAggNumber
			 INTEGER,
		alclnkaggAggDescr
			 DisplayString,
  	        alclnkaggAggName
			 DisplayString,
		alclnkaggAggLacpType
			 LacpType,
		alclnkaggAggAdminState
--           Adminstate,
			 INTEGER,
		alclnkaggAggOperState
			 INTEGER,	
                alclnkaggAggNbrSelectedPorts
                         INTEGER,
                alclnkaggAggNbrAttachedPorts
                         INTEGER,
                alclnkaggAggPrimaryPortIndex
                        InterfaceIndex,
		alclnkaggAggPrimaryPortPosition
                        INTEGER,
	        alclnkaggAggRowStatus
			 RowStatus,
		alclnkaggAggPreemptState   
			INTEGER,   	
		alclnkaggAggPreemptValue   
			Integer32 
		}
	
	
	alclnkaggAggIndex OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The unique identifier allocated to this Aggregator by the local
			System.
			This attribute identifies an Aggregator instance among the subordinate
			managed objects of the containing object. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.1"
		::= { alclnkaggAggEntry 1 }
	
	
	alclnkaggAggMACAddress OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"A 6-octet read-only value carrying the individual
			MAC address assigned to the Aggregator."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.9"
		::= { alclnkaggAggEntry 2 }
	
	
	alclnkaggAggActorSystemPriority OBJECT-TYPE
		SYNTAX INTEGER (0..65535)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 2-octet read-create value indicating the priority value
			associated with the Actor's System ID."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.5"
		::= { alclnkaggAggEntry 3 }
	
	
	alclnkaggAggActorSystemID OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 6-octet read-create MAC address value used as a unique
			identifier for the System that contains this Aggregator.
			NOTE-From the perspective of the Link Aggregation mechanisms
			described in Clause , only a single combination of
			Actor's System ID and System Priority are considered, and no
			distinction is made between the values of these parameters
			for an Aggregator and the port(s) that are associated with
			it; i.e., the protocol is described in terms of the operation
			of aggregation within a single System. However, the managed.
			objects provided for the Aggregator and the port both allow
			management of these parameters. The result of this is to
			permit a single piece of equipment to be configured by
			management to contain more than one System from the point of
			view of the operation of Link Aggregation. This may be of
			particular use in the configuration of equipment that has
			limited aggregation capability (see )."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.4"
		::= { alclnkaggAggEntry 4 }
	
	alclnkaggAggPartnerAdminKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The current Administrative value of the Key accepted for the
			Aggregator's current protocol Partner. Optional this is
			a 16-bit read-create value. If the aggregation is manually
			configured, this Key value will be a value assigned by the
			local System. The administrative Key value may differ from 
                                   the operational "
		REFERENCE
			" specific to ALCATEL "
		::= { alclnkaggAggEntry 5 }

		
	alclnkaggAggActorAdminKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The current administrative value of the Key for the Aggregator.
			The administrative Key value may differ from the operational
			Key value for the reasons discussed in . This is a 16-bit,
			read-create value. The meaning of particular Key values
			is of local significance."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.7"
		::= { alclnkaggAggEntry 6 }
	
	
	alclnkaggAggActorOperKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The current operational value of the Key for the Aggregator.
			The administrative Key value may differ from the operational
			Key value for the reasons discussed in .
			This is a 16-bit read-only value. The meaning of particular Key
			values is of local significance."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.8"
		::= { alclnkaggAggEntry 7 }
	
	
	alclnkaggAggPartnerSystemID OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 6-octet read-create MAC address value consisting
			of the unique identifier for the current protocol Partner of
			this Aggregator. A value of zero indicates that there is no
			known Partner. If the aggregation is manually configured, this
			System ID value will be a value assigned by the local System."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.10"
		::= { alclnkaggAggEntry 8 }
	
	
	alclnkaggAggPartnerSystemPriority OBJECT-TYPE
		SYNTAX INTEGER (0..65535)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 2-octet read-create value that indicates the priority
			value associated with the Partner's System ID. If the
			aggregation is manually configured, this System Priority value
			will be a value assigned by the local System."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.11"
		::= { alclnkaggAggEntry 9 }
	
	
	alclnkaggAggPartnerOperKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The current operational value of the Key for the
			Aggregator's current protocol Partner. This is
			a 16-bit read-create value. If the aggregation is manually
			configured, this Key value will be a value assigned by the
			local System."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.12"
		::= { alclnkaggAggEntry 10 }


------------------------------------------------------------
-- Specific Proprietary Part
-----------------------------------------------------------

	
	alclnkaggAggSize OBJECT-TYPE
		SYNTAX INTEGER (1..16)
		MAX-ACCESS read-create
		STATUS  current
		DESCRIPTION
			"Maximum number of links that could be attached to this
                         aggregator, This nominator is mandatory and is a required
                         field in order to create a row in this table"
		REFERENCE
			"specific to ALCATEL"
		::= { alclnkaggAggEntry 11 }
         
	alclnkaggAggNumber OBJECT-TYPE
		SYNTAX INTEGER(0..127)
--		MAX-ACCESS read-create
		MAX-ACCESS read-only
		 STATUS  current
		DESCRIPTION
--			"Aggreagtor number to assign a reference  number at the creation of 
--                       an aggregator mandatory for the Omnichhannel object creation"
			"Aggreagtor number reference the aggregate dedicated from the 
                         ifindex at the creation"
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggEntry 12 }

           -- alclnkaggAggDescr is equivalent to ifDescr in ifTable 

	alclnkaggAggDescr OBJECT-TYPE
		SYNTAX DisplayString (SIZE (0..255))
		MAX-ACCESS read-only
		 STATUS  current
		DESCRIPTION
			"Description is a human readable string which describes of 
             the type of aggregator object OMNICHANNEL / LACP  etc …  "
		REFERENCE
			" IEEE 802.3 Subclause 30.7.1.1.2"
		::= { alclnkaggAggEntry 13 }
	
            -- alclnkaggAggDescr is equivalent to ifDescr in ifXTable 

	alclnkaggAggName OBJECT-TYPE
		SYNTAX DisplayString (SIZE (0..255))
		MAX-ACCESS read-create
		 STATUS current
		DESCRIPTION
			"Name of the aggregator is human readable string manually given by
                                      the operator"
		REFERENCE
			" IEEE 802.3 Subclause 30.7.1.1.3"
		::= { alclnkaggAggEntry 14 }


	alclnkaggAggLacpType OBJECT-TYPE
		SYNTAX LacpType
		MAX-ACCESS read-create
		 STATUS current
		DESCRIPTION
			"Aggreagtor set with LACP protocol or not (case of Omnichannel)
                         mandatory at the creation of the aggregator, cannot be modified
                         later "
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggEntry 15 }


           -- alclnkaggAggAdminState is equivalent to ifAdminStatus in ifTable 

	alclnkaggAggAdminState OBJECT-TYPE
--		SYNTAX AdminState
                SYNTAX  INTEGER {
                	    enable(1),       -- ready to pass packets
                	    disable(2)
                      }
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"status assigned by the admnistrator. The activation of the aggregator 
                                     is managed by this nominator"
		REFERENCE
			" IEEE 802.3 Subclause 30.7.1.1.13"
		::= { alclnkaggAggEntry 16 }

           -- alclnkaggAggOperState is similar  to ifOperStatus in ifTable but the nominator  
           -- does not take exactly the same values.

	alclnkaggAggOperState OBJECT-TYPE
		  SYNTAX  INTEGER {
		                           up(1),
                                           down(2),
		                           logicPortCreatFailed(3),
                                           qReservationFailed(4)
                                                  }
		MAX-ACCESS read-only
		 STATUS current
		DESCRIPTION
			"Operational status of the aggregator with proprietary values
                         operational state from iftable corresponds to UP state "
		REFERENCE
			" IEEE 802.3 Subclause 30.7.1.1.14"
		::= { alclnkaggAggEntry 17 }

	 alclnkaggAggNbrSelectedPorts OBJECT-TYPE
		SYNTAX INTEGER (0..16)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of ports selected at the momemt ."
		REFERENCE
			"Specific to ALCATEL"
		::= { alclnkaggAggEntry 18 }
	
	  alclnkaggAggNbrAttachedPorts OBJECT-TYPE
		SYNTAX INTEGER (0..16)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of ports attached at the momemt ."
		REFERENCE
			"Specific to ALCATEL"
		::= { alclnkaggAggEntry 19 }
	
	  alclnkaggAggPrimaryPortIndex OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"the ifindex of the primary port in the aggregator used to send  
                         BPDUs and flooding frames Zeo indicates no primary port is
                         available ."
		REFERENCE
			"Specific to ALCATEL"
		::= { alclnkaggAggEntry 20 }

	  alclnkaggAggPrimaryPortPosition OBJECT-TYPE
		SYNTAX INTEGER (-1..15)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"the port index number in the aggregator used to send  
                         BPDUs and flooding frames ."
		REFERENCE
			"Specific to ALCATEL"
		::= { alclnkaggAggEntry 21 }

	
	alclnkaggAggRowStatus OBJECT-TYPE
                SYNTAX RowStatus   	
      		MAX-ACCESS read-create
      		STATUS current
      		DESCRIPTION
         		"This object is the RowStatus (locking flag) for creating or
  			deleting aggregator objects. alclnkaggAggSize, alclnkaggAggLacpType 
                        and  must be supplied in the request to create a row, it is a 
                        required field."
		REFERENCE
			" specific to ALCATEL "
		::= { alclnkaggAggEntry 22 }

	alclnkaggAggPreemptState OBJECT-TYPE
                SYNTAX INTEGER {
                    enable(1),
                    disable(2)
                   }
                MAX-ACCESS read-create
                STATUS current
                DESCRIPTION
                       "This sets the pre-emption state for an aggregate. The default value is disable."
                REFERENCE
                        "specific to ALCATEL"
                ::={ alclnkaggAggEntry 23}

          alclnkaggAggPreemptValue OBJECT-TYPE
                SYNTAX Integer32 (30..300)
                MAX-ACCESS read-create
                STATUS current
                DESCRIPTION
                       "This sets the pre-empt timer value in seconds for an aggregate. The default value is 30 seconds."
                REFERENCE
                        "specific to ALCATEL"
                ::={ alclnkaggAggEntry 24}


	
	
	-- -------------------------------------------------------------
	-- The Aggregation Port List Table
	-- -------------------------------------------------------------


	alclnkaggAggPortListTable OBJECT-TYPE
		SYNTAX SEQUENCE OF AlclnkaggAggPortListEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A table that contains a list of all the ports
			associated with each Aggregator."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.31"
		::= { alclnkaggAgg 2 }

	
	alclnkaggAggPortListEntry OBJECT-TYPE
		SYNTAX AlclnkaggAggPortListEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A list of the ports associated with a given Aggregator.
			This is indexed by the ifIndex of the Aggregator."
		INDEX { alclnkaggAggIndex }
		::= { alclnkaggAggPortListTable 1 }
	

	AlclnkaggAggPortListEntry ::=
		SEQUENCE {
			alclnkaggAggPortListPorts
				PortList
		}


	alclnkaggAggPortListPorts OBJECT-TYPE
		SYNTAX PortList
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The complete set of ports currently associated with
			this Aggregator. Each bit set in this list represents
			an Actor Port member of this Link Aggregation."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.1.1.31"
		::= { alclnkaggAggPortListEntry 1 }	


	-- -------------------------------------------------------------
	-- The Aggregation Port Table
	-- -------------------------------------------------------------


	alclnkaggAggPortTable OBJECT-TYPE
		SYNTAX SEQUENCE OF AlclnkaggAggPortEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A table that contains Link Aggregation Control
			configuration information about every
			Aggregation Port associated with this device.
			A row appears in this table for each physical port."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2"
		::= { alclnkaggAggPort 1 }
	
	alclnkaggAggPortEntry OBJECT-TYPE
		SYNTAX AlclnkaggAggPortEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A list of Link Aggregation Control configuration
			parameters for each Aggregation Port on this device."
		INDEX { alclnkaggAggPortIndex }
		::= { alclnkaggAggPortTable 1 }


	AlclnkaggAggPortEntry ::=
		SEQUENCE {
			alclnkaggAggPortIndex
				InterfaceIndex,
			alclnkaggAggPortActorSystemPriority
				INTEGER,
			alclnkaggAggPortActorSystemID
				MacAddress,
			alclnkaggAggPortActorAdminKey
				LacpKey,
			alclnkaggAggPortActorOperKey
				LacpKey,
			alclnkaggAggPortPartnerAdminSystemPriority
				INTEGER,
			alclnkaggAggPortPartnerOperSystemPriority
				INTEGER,
			alclnkaggAggPortPartnerAdminSystemID
				MacAddress,
			alclnkaggAggPortPartnerOperSystemID
				MacAddress,
			alclnkaggAggPortPartnerAdminKey
				LacpKey,
			alclnkaggAggPortPartnerOperKey
				LacpKey,
			alclnkaggAggPortSelectedAggID
				InterfaceIndex,
			alclnkaggAggPortAttachedAggID
				InterfaceIndex,
			alclnkaggAggPortActorPort
				INTEGER,
			alclnkaggAggPortActorPortPriority
				INTEGER,
			alclnkaggAggPortPartnerAdminPort
				INTEGER,
			alclnkaggAggPortPartnerOperPort
				INTEGER,
			alclnkaggAggPortPartnerAdminPortPriority
				INTEGER,
			alclnkaggAggPortPartnerOperPortPriority
				INTEGER,
			alclnkaggAggPortActorAdminState
				LacpState,
			alclnkaggAggPortActorOperState
				LacpState,
			alclnkaggAggPortPartnerAdminState
				LacpState,
			alclnkaggAggPortPartnerOperState
				LacpState,

------------------------------------------------------------
-- Specific Proprietary Part
-----------------------------------------------------------
 	
            		alclnkaggAggPortSelectedAggNumber
		        	INTEGER,
            		alclnkaggAggPortGlobalPortNumber
		        	 INTEGER,
            		alclnkaggAggPortAdminState
--	   			AdminState,
                 		INTEGER,
		    	alclnkaggAggPortOperState
--			     	OperState,
                 		INTEGER,
		    	alclnkaggAggPortState
                 		INTEGER,
			alclnkaggAggPortLinkState
                 		INTEGER,
		        alclnkaggAggPortPrimary 
		                INTEGER,
			alclnkaggAggPortLacpType
				 LacpType,
 	        	alclnkaggAggPortRowStatus
				 RowStatus,
			alclnkaggAggPortStandbyState
				 INTEGER
		}


	alclnkaggAggPortIndex OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The ifIndex of the port"
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.1"
		::= { alclnkaggAggPortEntry 1 }
	

	alclnkaggAggPortActorSystemPriority OBJECT-TYPE
		SYNTAX INTEGER (0..255)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 2-octet read-create value used to define the priority
			value associated with the Actor's System ID."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.2"
		::= { alclnkaggAggPortEntry 2 }
	
	alclnkaggAggPortActorSystemID OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 6-octet read-create MAC address value that defines
			the value of the System ID for the System that contains this
			Aggregation Port."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.3"
		::= { alclnkaggAggPortEntry 3 }
	
	alclnkaggAggPortActorAdminKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The current administrative value of the Key for the
			Aggregation Port. This is a 16-bit read-create value.
			The meaning of particular Key values is of local significance."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.4"
		::= { alclnkaggAggPortEntry 4 }
	

	alclnkaggAggPortActorOperKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The current operational value of the Key for the
			Aggregation Port. This is a 16-bit read-only value.
			The meaning of particular Key values is of local significance."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.5"
		::= { alclnkaggAggPortEntry 5 }


	alclnkaggAggPortPartnerAdminSystemPriority OBJECT-TYPE
		SYNTAX INTEGER (0..255)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 2-octet read-create value used to define the administrative
			value of priority associated with the Partner's System ID. The
			assigned value is used, along with the value of
			aAggPortPartnerAdminSystemID, aAggPortPartnerAdminKey,
			aAggPortPartnerAdminPort, and aAggPortPartnerAdminPortPriority,
			in order to achieve manually configured aggregation."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.6"
		::= { alclnkaggAggPortEntry 6 }
	
	alclnkaggAggPortPartnerOperSystemPriority OBJECT-TYPE
		SYNTAX INTEGER (0..255)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"A 2-octet read-only value indicating the operational value
			of priority associated with the Partner's System ID. The
			value of this attribute may contain the manually configured value
			carried in aAggPortPartnerAdminSystemPriority
			if there is no protocol Partner."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.7"
		::= { alclnkaggAggPortEntry 7 }
		
	alclnkaggAggPortPartnerAdminSystemID OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A 6-octet read-create MACAddress value representing
			the administrative value of the Aggregation Port's protocol
			Partner's System ID. The assigned value is used, along with
			the value of aAggPortPartnerAdminSystemPriority,
			aAggPortPartnerAdminKey, aAggPortPartnerAdminPort,
			and aAggPortPartnerAdminPortPriority, in order to
			achieve manually configured aggregation."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.8"
		::= { alclnkaggAggPortEntry 8 }
	
	alclnkaggAggPortPartnerOperSystemID OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"A 6-octet read-only MACAddress value representing
			the current value of the Aggregation Port's protocol Partner's
			System ID. A value of zero indicates that there is no known
			protocol Partner. The value of this attribute may contain the
			manually configured value carried in
			aAggPortPartnerAdminSystemID if there is no protocol Partner."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.9"
		::= { alclnkaggAggPortEntry 9 }
	

	alclnkaggAggPortPartnerAdminKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The current administrative value of the Key for the
			protocol Partner. This is a 16-bit read-create value.
			The assigned value is used, along with the value of
			aAggPortPartnerAdminSystemPriority, aAggPortPartnerAdminSystemID,
			aAggPortPartnerAdminPort, and aAggPortPartnerAdminPortPriority,
			in order to achieve manually configured aggregation."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.10"
		::= { alclnkaggAggPortEntry 10 }
	

	alclnkaggAggPortPartnerOperKey OBJECT-TYPE
		SYNTAX LacpKey
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The current operational value of the Key for the
			protocol Partner. The value of this attribute may contain
			the manually configured value carried in
			aAggPortPartnerAdminKey if there is no protocol Partner.
			This is a 16-bit read-only value."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.11"
		::= { alclnkaggAggPortEntry 11 }
	

	alclnkaggAggPortSelectedAggID OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The identifier value of the Aggregator that this Aggregation
			Port has currently selected. Zero indicates that the Aggregation
			Port has not selected an Aggregator, either because it is in the
			process of detaching from an Aggregator or because there is no
			suitable Aggregator available for it to select. This value is
			read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.12"
		::= { alclnkaggAggPortEntry 12 }


	alclnkaggAggPortAttachedAggID OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The identifier value of the Aggregator that this Aggregation
			Port is currently attached to. Zero indicates that the Aggregation
			Port is not currently attached to an Aggregator. This value is
			read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.13"
		::= { alclnkaggAggPortEntry 13 }


	alclnkaggAggPortActorPort OBJECT-TYPE
		SYNTAX INTEGER (0..65535)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The port number locally assigned to the Aggregation Port.
			The port number is communicated in LACPDUs as the
			Actor_Port. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.14"
		::= { alclnkaggAggPortEntry 14 }


	alclnkaggAggPortActorPortPriority OBJECT-TYPE
		SYNTAX INTEGER (0..255)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The priority value assigned to this Aggregation Port.
			This 16-bit value is read-create."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.15"
		::= { alclnkaggAggPortEntry 15 }


	alclnkaggAggPortPartnerAdminPort OBJECT-TYPE
		SYNTAX INTEGER (0..65535)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The current administrative value of the port number
			for the protocol Partner. This is a 16-bit read-create value.
			The assigned value is used, along with the value of
			aAggPortPartnerAdminSystemPriority,
			aAggPortPartnerAdminSystemID, aAggPortPartnerAdminKey,
			and aAggPortPartnerAdminPortPriority,
			in order to achieve manually configured aggregation."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.16"
		::= { alclnkaggAggPortEntry 16 }


	alclnkaggAggPortPartnerOperPort OBJECT-TYPE
		SYNTAX INTEGER (0..65535)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The operational port number assigned to this Aggregation
			Port by the Aggregation Port's protocol Partner. The value
			of this attribute may contain the manually configured value
			carried in aAggPortPartnerAdminPort if there is no protocol
			Partner. This 16-bit value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.17"
		::= { alclnkaggAggPortEntry 17 }


	alclnkaggAggPortPartnerAdminPortPriority OBJECT-TYPE
		SYNTAX INTEGER (0..255)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The current administrative value of the port priority
			for the protocol Partner. This is a 16-bit read-create value.
			The assigned value is used, along with the value of
			aAggPortPartnerAdminSystemPriority, aAggPortPartnerAdminSystemID,
			aAggPortPartnerAdminKey, and aAggPortPartnerAdminPort,
			in order to achieve manually configured aggregation."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.18"
		::= { alclnkaggAggPortEntry 18 }


	alclnkaggAggPortPartnerOperPortPriority OBJECT-TYPE
		SYNTAX INTEGER (0..255)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The priority value assigned to this Aggregation Port
			by the Partner. The value of this attribute may contain the
			manually configured value carried in
			aAggPortPartnerAdminPortPriority if there is no
			protocol Partner. This 16-bit value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.19"
		::= { alclnkaggAggPortEntry 19 }


	alclnkaggAggPortActorAdminState OBJECT-TYPE
		SYNTAX LacpState
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A string of 8 bits, corresponding to the administrative values
			of Actor_State () as transmitted by the Actor in LACPDUs.
			The first bit corresponds to bit 0 of Actor_State (LACP_Activity),
			the second bit corresponds to bit 1 (LACP_Timeout), the third bit
			corresponds to bit 2 (Aggregation), the fourth bit corresponds to
			bit 3 (Synchronization), the fifth bit corresponds to bit 4
			(Collecting), the sixth bit corresponds to bit 5 (Distributing),
			the seventh bit corresponds to bit 6 (Defaulted), and the eighth
			bit corresponds to bit 7 (Expired). These values allow
			administrative control over the values of LACP_Activity,
			LACP_Timeout and Aggregation. This attribute value is read-create."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.20"
		::= { alclnkaggAggPortEntry 20 }


	alclnkaggAggPortActorOperState OBJECT-TYPE
		SYNTAX LacpState
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"A string of 8 bits, corresponding to the current
			operational values of Actor_State as transmitted by the
			Actor in LACPDUs. The bit allocations are as defined in
			. This attribute value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.21"
		::= { alclnkaggAggPortEntry 21 }


	alclnkaggAggPortPartnerAdminState OBJECT-TYPE
		SYNTAX LacpState
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"A string of 8 bits, corresponding to the current administrative
			value of Actor_State for the protocol Partner. The bit
			allocations are as defined in . This attribute value is
			read-create. The assigned value is used in order to achieve
			manually configured aggregation."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.22"
		::= { alclnkaggAggPortEntry 22 }


	alclnkaggAggPortPartnerOperState OBJECT-TYPE
		SYNTAX LacpState
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"A string of 8 bits, corresponding to the current values of
			Actor_State in the most recently received LACPDU transmitted
			by the protocol Partner. The bit allocations are as defined in
			. In the absence of an active protocol Partner, this
			value may reflect the manually configured value
			aAggPortPartnerAdminState. This attribute value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.2.1.23"
		::= { alclnkaggAggPortEntry 23 }


------------------------------------------------------------
-- Specific Proprietary Part
-----------------------------------------------------------


	alclnkaggAggPortSelectedAggNumber OBJECT-TYPE
		SYNTAX INTEGER(-1..127)
		MAX-ACCESS read-create
		 STATUS current
		DESCRIPTION
			"Aggreagtor number to attach a  port at its creation  
                         mandatory and only used for the 
                         Omnichhannel not allowed for LACP
                         (-1) value displayed when it is not significant"
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggPortEntry 24 }

	alclnkaggAggPortGlobalPortNumber OBJECT-TYPE
		SYNTAX INTEGER (0..65535)
		MAX-ACCESS read-only
		 STATUS current
		DESCRIPTION
			"Physical reference of the port "
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggPortEntry 25 }


           -- alclnkaggAggPortAdminState is equivalent to ifAdminStatus in ifTable 

	alclnkaggAggPortAdminState OBJECT-TYPE
                SYNTAX  INTEGER {
                	    enable(1),       -- ready to pass packets
                	    disable(2)
                      }
		MAX-ACCESS read-only
		 STATUS current
		DESCRIPTION
			"status assigned by the admnistrator. port activation done by iftable
                         this nominator is equivalent to ifAdminStatus in ifTable  "
		REFERENCE
			" IEEE 802.3 Subclause 30.7.1.1.13"
		::= { alclnkaggAggPortEntry 26 }


	alclnkaggAggPortOperState OBJECT-TYPE
		  SYNTAX  INTEGER {
		                    up(1),
                                    down(2),
		                    notAttached(3),
                                    notAggregable(4)
                                   }
		MAX-ACCESS read-only
		 STATUS current
		DESCRIPTION
			"Operational status of the port regarding the traffic"
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggPortEntry 27 }

	alclnkaggAggPortState OBJECT-TYPE
		  SYNTAX  INTEGER {
		                    created(1),
                                    configurable(2),
		                    configured(3),
                                    selected(4),
                                    reserved(5),
                                    attached(6)
                                   }
		MAX-ACCESS read-only
		 STATUS current
		DESCRIPTION
			"aggregation status of the port"
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggPortEntry 28 }

	alclnkaggAggPortLinkState OBJECT-TYPE
		  SYNTAX  INTEGER {
		                    up(1),
                                    down(2)
                                   }
		MAX-ACCESS read-only
		 STATUS current
		DESCRIPTION
			"Operational status of the link"
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggPortEntry 29 }

	 -- alclnkaggAggPortLinkState is equivalent to ifOperStatus 

	alclnkaggAggPortPrimary OBJECT-TYPE
		  SYNTAX  INTEGER {
		                    yes(1),
                                    no(2),
                                    notSignificant(3)
                                   }
		MAX-ACCESS read-only
		 STATUS current
		DESCRIPTION
			"port primary or not"
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggPortEntry 30 }


	alclnkaggAggPortLacpType OBJECT-TYPE
		SYNTAX LacpType
		MAX-ACCESS read-create
--		 STATUS mandatory
		 STATUS current
		DESCRIPTION
			"Port set with LACP protocol or not (case of Omnichannel)
                          mandatory at the creation of the port"
		REFERENCE
			" specific to ALCATEL"
		::= { alclnkaggAggPortEntry 31 }


	alclnkaggAggPortRowStatus OBJECT-TYPE
	SYNTAX RowStatus   
      		MAX-ACCESS read-create
      		STATUS current
      		DESCRIPTION
         		"This object is the RowStatus (locking flag) for creating or
  			 deleting aggregatable port objects. alclnkaggAggPortActorAdminKey
                         and alclnkaggAggPortSlotSlice must be supplied 
                         in the request to create a row, it is a required field."
		REFERENCE
			" specific to ALCATEL "
		::= { alclnkaggAggPortEntry 32 }

	alclnkaggAggPortStandbyState OBJECT-TYPE
                 SYNTAX INTEGER {
                                enable(1),
                                disable(2)
                               }
                 MAX-ACCESS read-create
                 STATUS current
                 DESCRIPTION
                         "This sets the standby state for a port. The default value is disable."
                 ::= { alclnkaggAggPortEntry 33 }

	
	-- -------------------------------------------------------------
	-- LACP Statistics Table
	-- -------------------------------------------------------------


	alclnkaggAggPortStatsTable OBJECT-TYPE
		SYNTAX SEQUENCE OF AlclnkaggAggPortStatsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A table that contains Link Aggregation information
			 about every port that is associated with this device.
			 A row appears in this table for each physical port."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3"
		::= { alclnkaggAggPort 2 }


	alclnkaggAggPortStatsEntry OBJECT-TYPE
		SYNTAX AlclnkaggAggPortStatsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A list of Link Aggregation Control Protocol statistics
			for each port on this device."
		INDEX { alclnkaggAggPortIndex }
		::= { alclnkaggAggPortStatsTable 1 }


	AlclnkaggAggPortStatsEntry ::=
		SEQUENCE {
			alclnkaggAggPortStatsLACPDUsRx
				Counter32,
			alclnkaggAggPortStatsMarkerPDUsRx
				Counter32,
			alclnkaggAggPortStatsMarkerResponsePDUsRx
				Counter32,
			alclnkaggAggPortStatsUnknownRx
				Counter32,
			alclnkaggAggPortStatsIllegalRx
				Counter32,
			alclnkaggAggPortStatsLACPDUsTx
				Counter32,
			alclnkaggAggPortStatsMarkerPDUsTx
				Counter32,
			alclnkaggAggPortStatsMarkerResponsePDUsTx
				Counter32
		}


	alclnkaggAggPortStatsLACPDUsRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of valid LACPDUs received on this
			Aggregation Port. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3.1.2"
		::= { alclnkaggAggPortStatsEntry 1 }


	alclnkaggAggPortStatsMarkerPDUsRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of valid Marker PDUs received on this
			Aggregation Port. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3.1.3"
		::= { alclnkaggAggPortStatsEntry 2 }


	alclnkaggAggPortStatsMarkerResponsePDUsRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of valid Marker Response PDUs received on this
			 Aggregation Port. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3.1.4"
		::= { alclnkaggAggPortStatsEntry 3 }


	alclnkaggAggPortStatsUnknownRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of frames received that either:
			- carry the Slow Protocols Ethernet Type value (),
			but contain an unknown PDU, or:
			- are addressed to the Slow Protocols group MAC
			Address (), but do not carry the Slow Protocols Ethernet Type.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3.1.5"
		::= { alclnkaggAggPortStatsEntry 4 }


	alclnkaggAggPortStatsIllegalRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of frames received that carry the Slow
			Protocols Ethernet Type value (), but contain a badly formed
			PDU or an illegal value of Protocol Subtype ().
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3.1.6"
		::= { alclnkaggAggPortStatsEntry 5 }


	alclnkaggAggPortStatsLACPDUsTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of LACPDUs transmitted on this
			Aggregation Port. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3.1.7"
		::= { alclnkaggAggPortStatsEntry 6 }


	alclnkaggAggPortStatsMarkerPDUsTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of Marker PDUs transmitted on this
			Aggregation Port. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.3.1.8"
		::= { alclnkaggAggPortStatsEntry 7 }


	alclnkaggAggPortStatsMarkerResponsePDUsTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of Marker Response PDUs transmitted
			 on this Aggregation Port. This value is read-only."
		REFERENCE
		"IEEE 802.3 Subclause 30.7.3.1.9"
		::= { alclnkaggAggPortStatsEntry 8 }


	-- -------------------------------------------------------------
	-- LACP Debug Table
	-- -------------------------------------------------------------



	alclnkaggAggPortDebugTable OBJECT-TYPE
		SYNTAX SEQUENCE OF AlclnkaggAggPortDebugEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A table that contains Link Aggregation debug
			information about every port that is associated with
			this device. A row appears in this table for each
			physical port."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4"
		::= { alclnkaggAggPort 3 }


	alclnkaggAggPortDebugEntry OBJECT-TYPE
		SYNTAX AlclnkaggAggPortDebugEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A list of the debug parameters for a port."
		INDEX { alclnkaggAggPortIndex }
		::= { alclnkaggAggPortDebugTable 1 }
	
	AlclnkaggAggPortDebugEntry ::=
		SEQUENCE {
			alclnkaggAggPortDebugRxState
				INTEGER,
			alclnkaggAggPortDebugLastRxTime
				TimeTicks,   
			alclnkaggAggPortDebugMuxState
            			INTEGER,
        		alclnkaggAggPortDebugMuxReason
            			DisplayString,
			alclnkaggAggPortDebugActorChurnState
				ChurnState,
			alclnkaggAggPortDebugPartnerChurnState
				ChurnState,
			alclnkaggAggPortDebugActorChurnCount
				Counter32,
			alclnkaggAggPortDebugPartnerChurnCount
				Counter32,
			alclnkaggAggPortDebugActorSyncTransitionCount
				Counter32,
			alclnkaggAggPortDebugPartnerSyncTransitionCount
				Counter32,
			alclnkaggAggPortDebugActorChangeCount
				Counter32,
			alclnkaggAggPortDebugPartnerChangeCount
				Counter32
		}


	alclnkaggAggPortDebugRxState OBJECT-TYPE
		SYNTAX INTEGER {
					current(1),
					expired(2),
					defaulted(3),
					initialize(4),
					lacpDisabled(5),
					portDisabled(6)
			}
	MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute holds the value 'current' if the Receive
			state machine for the Aggregation Port is in the
			CURRENT state, 'expired' if the Receive state machine.
			is in the EXPIRED state, 'defaulted' if the Receive state
			machine is in the DEFAULTED state, 'initialize' if the
			Receive state machine is in the INITIALIZE state,
			'lacpDisabled' if the Receive state machine is in the
			LACP_DISABLED state, or 'portDisabled' if the Receive
			state machine is in the PORT_DISABLED state.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.2"
		::= { alclnkaggAggPortDebugEntry 1 }


	alclnkaggAggPortDebugLastRxTime OBJECT-TYPE
		SYNTAX TimeTicks
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The value of aTimeSinceSystemReset (F.2.1) when
			the last LACPDU was received by this Aggregation Port.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.3"
		::= { alclnkaggAggPortDebugEntry 2 }

       alclnkaggAggPortDebugMuxState OBJECT-TYPE
    		SYNTAX       INTEGER {
                    detached(1),
                    waiting(2),
                    attached(3),
                    collecting(4),
                    distributing(5),
                    collectingDistributing(6)
             	}
    		MAX-ACCESS   read-only
    		STATUS       current
    		DESCRIPTION
        		"This attribute holds the value `detached' if the Mux
       			state machine (43.4.14) for the Aggregation Port is in
        		the DETACHED state, `waiting' if the Mux state machine
        		is in the WAITING state, `attached' if the Mux state
        		machine for the Aggregation Port is in the ATTACHED
        		state, `collecting' if the Mux state machine for the
        		Aggregation Port is in the COLLECTING state,
        		`distributing' if the Mux state machine for the
        		Aggregation Port is in the DISTRIBUTING state, and
        		`collectingDistributing' if the Mux state machine for
        		the Aggregation Port is in the COLLECTING_DISTRIBUTING
        		state. This value is read-only."
    		REFERENCE
        	"IEEE 802.3 Subclause 30.7.4.1.4"
    		::= { alclnkaggAggPortDebugEntry 3 }


	alclnkaggAggPortDebugMuxReason OBJECT-TYPE
    		SYNTAX       DisplayString
    		MAX-ACCESS   read-only
    		STATUS       current
    		DESCRIPTION
        		"A human-readable text string indicating the reason
        		for the most recent change of Mux machine state.
        		This value is read-only."
    		REFERENCE
        		"IEEE 802.3 Subclause 30.7.4.1.5"
    		::= { alclnkaggAggPortDebugEntry 4 }


	alclnkaggAggPortDebugActorChurnState OBJECT-TYPE
		SYNTAX ChurnState
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The state of the Actor Churn Detection machine
			() for the Aggregation Port. A value of 'noChurn'
			indicates that the state machine is in either the
			NO_ACTOR_CHURN or the ACTOR_CHURN_MONITOR
			state, and 'churn' indicates that the state machine is in the
			ACTOR_CHURN state. This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.6"
		::= { alclnkaggAggPortDebugEntry 5 }


	alclnkaggAggPortDebugPartnerChurnState OBJECT-TYPE
		SYNTAX ChurnState
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The state of the Partner Churn Detection machine
			() for the Aggregation Port. A value of 'noChurn'
			indicates that the state machine is in either the
			NO_PARTNER_CHURN or the PARTNER_CHURN_MONITOR
			state, and 'churn' indicates that the state machine is
			in the PARTNER_CHURN state.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.7"
		::= { alclnkaggAggPortDebugEntry 6 }

 

	alclnkaggAggPortDebugActorChurnCount OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Count of the number of times the Actor Churn state
			machine has entered the ACTOR_CHURN state.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.8"
		::= { alclnkaggAggPortDebugEntry 7 }


	alclnkaggAggPortDebugPartnerChurnCount OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Count of the number of times the Partner Churn
			state machine has entered the PARTNER_CHURN state.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.9"
		::= { alclnkaggAggPortDebugEntry 8 }


	alclnkaggAggPortDebugActorSyncTransitionCount OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Count of the number of times the Actor's Mux state
			machine () has entered the IN_SYNC state.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.10"
		::= { alclnkaggAggPortDebugEntry 9 }
	

	alclnkaggAggPortDebugPartnerSyncTransitionCount OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Count of the number of times the Partner's Mux
			state machine () has entered the IN_SYNC state.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.11"
		::= { alclnkaggAggPortDebugEntry 10 }


	alclnkaggAggPortDebugActorChangeCount OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Count of the number of times the Actor's perception of
			the LAG ID for this Aggregation Port has changed.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.12"
		::= { alclnkaggAggPortDebugEntry 11 }


	alclnkaggAggPortDebugPartnerChangeCount OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Count of the number of times the Partner's perception of
			the LAG ID (see ) for this Aggregation Port has changed.
			This value is read-only."
		REFERENCE
			"IEEE 802.3 Subclause 30.7.4.1.13"
		::= { alclnkaggAggPortDebugEntry 12 }



	-- -------------------------------------------------------------
	-- Link Aggregation additional parameters
	-- -------------------------------------------------------------

        alclnkaggAggEniActivate OBJECT-TYPE

		SYNTAX INTEGER {
			enable(1),
			disable(2)
		       }
		MAX-ACCESS read-create
		STATUS obsolete
		DESCRIPTION
			"This variable activates or deactivates link aggregation for ENI"
		::= { alclnkaggAgg 3 }

	
	alclnkaggSlotTable OBJECT-TYPE
		SYNTAX SEQUENCE OF AlclnkaggSlotEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Each row in this table represents the link aggregation status
			for the associated slot. "
		REFERENCE
			"specific to Alcatel"
		::= { alclnkaggAgg 4 }


	alclnkaggSlotEntry OBJECT-TYPE
		SYNTAX AlclnkaggSlotEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Configuration parameters for link aggregation."
		INDEX { alclnkaggSlotNum }
		::= { alclnkaggSlotTable 1 }


	AlclnkaggSlotEntry ::=
		SEQUENCE {
		alclnkaggSlotNum
			INTEGER,
		alclnkaggSlotStatus
			INTEGER,
		alclnkaggMultipleAggPerSlot
			INTEGER
		}
	
	

	alclnkaggSlotNum OBJECT-TYPE
		SYNTAX INTEGER (1..16)
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The slot number."
		REFERENCE
			"specific to Alcatel"
		::= { alclnkaggSlotEntry 1 }
	

	alclnkaggSlotStatus OBJECT-TYPE
		SYNTAX INTEGER {
			enable(1),
			disable(2)
			}

		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"Link aggregation enable/disable"
		::= { alclnkaggSlotEntry 2 }

	alclnkaggMultipleAggPerSlot OBJECT-TYPE
		SYNTAX INTEGER {
			enable(1),
			disable(2)
			}

		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"Enable/disable multiple Link aggregation per slot"
		::= { alclnkaggSlotEntry 3 }

	----------------------------------------------------------------
	-- Table for mapping LAG Id to the ifIndex of this aggregate
	---------------------------------------------------------------

	alclnkaggAggIdIfIndexTable OBJECT-TYPE
		SYNTAX SEQUENCE OF AlclnkaggAggIdIfIndexEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Each row in this table represents the link aggregation 
			aggregate id's corresponding ifIndex. "
		REFERENCE
			"specific to Alcatel"
		::= { alclnkaggAgg 5 }


	alclnkaggAggIdIfIndexEntry OBJECT-TYPE
		SYNTAX AlclnkaggAggIdIfIndexEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Parameters for link aggregation aggregate id relationship to ifIndex."
		INDEX { alclnkaggIfIndex }
		::= { alclnkaggAggIdIfIndexTable 1 }


	AlclnkaggAggIdIfIndexEntry ::=
		SEQUENCE {
		
		alclnkaggIfIndex
			INTEGER,
		alclnkaggAggId
			INTEGER	
		}
	
	alclnkaggIfIndex OBJECT-TYPE
		SYNTAX INTEGER  (1..2147483647)
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"IfIndex for the given Aggregate ID"
		::= { alclnkaggAggIdIfIndexEntry 1 }
	
	alclnkaggAggId OBJECT-TYPE
		SYNTAX INTEGER (0..127)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The aggregate id number."
		REFERENCE
			"specific to Alcatel"
		::= { alclnkaggAggIdIfIndexEntry 2 }
	

	

	
	-- -------------------------------------------------------------
	-- IEEE 802.3ad MIB - Conformance Information
	-- -------------------------------------------------------------


   	alcatelIND1LAGMIBConformance OBJECT-IDENTITY
        	STATUS current
        	DESCRIPTION
            		"Branch For Link Aggregation Subsystem Conformance Information."
        ::= { alcatelIND1LAGMIB 2 }	

    	alcatelIND1LAGMIBGroups OBJECT-IDENTITY
        	STATUS current
        	DESCRIPTION
            		"Branch For Link Aggregation Subsystem Units Of Conformance."
        	::= { alcatelIND1LAGMIBConformance 1 }
	

    	alcatelIND1LAGMIBCompliances OBJECT-IDENTITY
        	STATUS current
        	DESCRIPTION
            		"Branch For Link Aggregation Subsystem Compliance Statements."
        	::= { alcatelIND1LAGMIBConformance 2 }


	-- -------------------------------------------------------------
	-- units of conformance
	-- -------------------------------------------------------------


	alclnkaggAggGroup OBJECT-GROUP
		OBJECTS {
			alclnkaggAggActorSystemID,
			alclnkaggAggActorSystemPriority,
			alclnkaggAggActorAdminKey,
			alclnkaggAggMACAddress,
			alclnkaggAggActorOperKey,
			alclnkaggAggPartnerSystemID,
			alclnkaggAggPartnerSystemPriority,
			alclnkaggAggPartnerOperKey,
--------------------------------
--   Specific Proprietary Part
------------------------------ 
		        alclnkaggAggSize,
		        alclnkaggAggNumber,
		        alclnkaggAggDescr,
  	                alclnkaggAggName,
		        alclnkaggAggLacpType,
		        alclnkaggAggAdminState,
		        alclnkaggAggOperState,	
                        alclnkaggAggNbrSelectedPorts,
                        alclnkaggAggNbrAttachedPorts,
                        alclnkaggAggPrimaryPortIndex, 
	                alclnkaggAggPrimaryPortPosition,
			alclnkaggAggPreemptState,
			alclnkaggAggPreemptValue
		}
		STATUS current
		DESCRIPTION
			"A collection of objects providing information about an
			aggregation."
		::= { alcatelIND1LAGMIBGroups 1 }
	

	alclnkaggAggPortListGroup OBJECT-GROUP
		OBJECTS {
			alclnkaggAggPortListPorts
		}
		STATUS current
		DESCRIPTION
			"A collection of objects providing information about every
			port in an aggregation."
		::= { alcatelIND1LAGMIBGroups 2 }

	
	alclnkaggAggPortGroup OBJECT-GROUP
		OBJECTS {
			alclnkaggAggPortActorSystemPriority,
			alclnkaggAggPortActorSystemID,
			alclnkaggAggPortActorAdminKey,
			alclnkaggAggPortActorOperKey,
			alclnkaggAggPortPartnerAdminSystemPriority,
			alclnkaggAggPortPartnerOperSystemPriority,
			alclnkaggAggPortPartnerAdminSystemID,
			alclnkaggAggPortPartnerOperSystemID,
			alclnkaggAggPortPartnerAdminKey,
			alclnkaggAggPortPartnerOperKey,
			alclnkaggAggPortSelectedAggID,
			alclnkaggAggPortAttachedAggID,
			alclnkaggAggPortActorPort,
			alclnkaggAggPortActorPortPriority,
			alclnkaggAggPortPartnerAdminPort,
			alclnkaggAggPortPartnerOperPort,
			alclnkaggAggPortPartnerAdminPortPriority,
			alclnkaggAggPortPartnerOperPortPriority,
			alclnkaggAggPortActorAdminState,
			alclnkaggAggPortActorOperState,
			alclnkaggAggPortPartnerAdminState,
			alclnkaggAggPortPartnerOperState,
                        alclnkaggAggPortSelectedAggNumber,
                        alclnkaggAggPortGlobalPortNumber,
                        alclnkaggAggPortAdminState,
		        alclnkaggAggPortOperState,
		        alclnkaggAggPortState,
			alclnkaggAggPortLinkState,
			alclnkaggAggPortPrimary,
		        alclnkaggAggPortLacpType,
			alclnkaggAggPortStandbyState 
			}
		STATUS current
		DESCRIPTION
			"A collection of objects providing information about every
			port in an aggregation."
		::= { alcatelIND1LAGMIBGroups 3 }
	

	alclnkaggAggPortStatsGroup OBJECT-GROUP
		OBJECTS {
			alclnkaggAggPortStatsLACPDUsRx,
			alclnkaggAggPortStatsMarkerPDUsRx,
			alclnkaggAggPortStatsMarkerResponsePDUsRx,
			alclnkaggAggPortStatsUnknownRx,
			alclnkaggAggPortStatsIllegalRx,
			alclnkaggAggPortStatsLACPDUsTx,
			alclnkaggAggPortStatsMarkerPDUsTx,
			alclnkaggAggPortStatsMarkerResponsePDUsTx
		}	
		STATUS current
		DESCRIPTION
			"A collection of objects providing information about every
			port in an aggregation."
		::= { alcatelIND1LAGMIBGroups 4 }
	

	alclnkaggAggPortDebugGroup OBJECT-GROUP
		OBJECTS {
			alclnkaggAggPortDebugRxState,
			alclnkaggAggPortDebugLastRxTime,
			alclnkaggAggPortDebugActorChurnState,
			alclnkaggAggPortDebugPartnerChurnState,
			alclnkaggAggPortDebugActorChurnCount,
			alclnkaggAggPortDebugPartnerChurnCount,
			alclnkaggAggPortDebugActorSyncTransitionCount,
			alclnkaggAggPortDebugPartnerSyncTransitionCount,
			alclnkaggAggPortDebugActorChangeCount,
			alclnkaggAggPortDebugPartnerChangeCount
		}
		STATUS current
		DESCRIPTION
			"A collection of objects providing debug information about.
			every aggregated port."
		::= { alcatelIND1LAGMIBGroups 5 }
	

	alclnkaggTablesLastChangedGroup OBJECT-GROUP
		OBJECTS {
			alclnkaggTablesLastChanged
		}
		STATUS current
		DESCRIPTION
			"A collection of objects providing information about the time
			of changes to the configuration of aggregations and their ports."
		::= { alclnkaggAggGroup 6 }


	-- -------------------------------------------------------------
	-- compliance statements
	-- -------------------------------------------------------------


	alclnkaggAggCompliance MODULE-COMPLIANCE
		STATUS current
		DESCRIPTION
			"The compliance statement for device support of
			Link Aggregation."
		

		MODULE
			MANDATORY-GROUPS {
				alclnkaggAggGroup,
				alclnkaggAggPortGroup,
				alclnkaggTablesLastChangedGroup,
				lnkaggNotificationVarsGroup 
			}


			GROUP alclnkaggAggPortListGroup
			DESCRIPTION
				"This group is optional."


			GROUP alclnkaggAggPortStatsGroup
			DESCRIPTION
				"This group is optional."
	

			GROUP alclnkaggAggPortDebugGroup
			DESCRIPTION
				"This group is optional."


		::= { alcatelIND1LAGMIBCompliances 1 }

 

lnkaggNotificationVarsGroup OBJECT-GROUP
        OBJECTS
        {
                       traplnkaggAggId,
                       traplnkaggPortIfIndex
        }
        STATUS  current
        DESCRIPTION
            "Collection of objects which appear only in notifications."
        ::= {alcatelIND1LAGMIBGroups  7 } 

lnkaggTrapsGroup NOTIFICATION-GROUP
        NOTIFICATIONS {
            lnkaggAggUp,
            lnkaggAggDown,
            lnkaggPortJoin,
            lnkaggPortLeave,
            lnkaggPortRemove,
	    lnkaggPortReserve 
        }
        STATUS  current
        DESCRIPTION
            "Collection of Traps for Link Aggregation ."
        ::= { alcatelIND1LAGMIBGroups 8 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	lnkaggNotificationVars  OBJECT IDENTIFIER ::= { alcatelIND1LAGMIBObjects 4 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	traplnkaggAggId OBJECT-TYPE
                SYNTAX  INTEGER  (0..32)
                MAX-ACCESS  accessible-for-notify
                STATUS  current
                DESCRIPTION
                        "Index Value of Link Aggregation group  ."
           ::= {lnkaggNotificationVars  1 }

        traplnkaggPortIfIndex OBJECT-TYPE
                SYNTAX  INTEGER  (1..2147483647)
                MAX-ACCESS  accessible-for-notify
                STATUS  current
                DESCRIPTION
                        "Port of  Link Aggregate group ."
           ::= {lnkaggNotificationVars   2 }

 
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
--  NOTIFICATIONS
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
lnkaggAggUp NOTIFICATION-TYPE
        OBJECTS {
                traplnkaggAggId,
                traplnkaggPortIfIndex  
                }
        STATUS current
        DESCRIPTION
                "The Link Aggregation  is  active .
                This trap is sent when any one port of the link aggregation 
		goes to attached state."
        ::= { lnkaggTraps 0 1 }



lnkaggAggDown NOTIFICATION-TYPE
        OBJECTS {
                traplnkaggAggId,
                traplnkaggPortIfIndex  
                }
        STATUS current
        DESCRIPTION
                "The Link Aggregation  is  not active .
                This trap is sent when all  ports of the link aggregation 
		goes out of attached state."
        ::= { lnkaggTraps 0 2 }




lnkaggPortJoin NOTIFICATION-TYPE
        OBJECTS {
                traplnkaggAggId,
                traplnkaggPortIfIndex  
                }
        STATUS current
        DESCRIPTION
                "The Link Aggregation port  joins  the aggregate .
                This trap is sent when given  port of the link aggregation 
		goes to attached state."
        ::= { lnkaggTraps 0 3 }

lnkaggPortLeave NOTIFICATION-TYPE
        OBJECTS {
                traplnkaggAggId,
                traplnkaggPortIfIndex  
                }
        STATUS current
        DESCRIPTION
                "The Link Aggregation port  leaves  the aggregate .
                This trap is sent when given  port of the link aggregation 
		goes out of  attached state."
        ::= { lnkaggTraps 0 4 }

lnkaggPortRemove NOTIFICATION-TYPE
        OBJECTS {
                traplnkaggAggId,
                traplnkaggPortIfIndex  
                }
        STATUS current
        DESCRIPTION
                "The Link Aggregation port removed from the aggregate  .
                This trap is sent when given  port of the link aggregation 
		removed due to invalid configuration ."
        ::= { lnkaggTraps 0 5 }

lnkaggPortReserve NOTIFICATION-TYPE
	OBJECTS {
		traplnkaggAggId,
		traplnkaggPortIfIndex
		}
	STATUS current
	DESCRIPTION
		"The Link Aggregation port  is reserved for this aggregate .
		This trap is sent when given  port of the link aggregation
		goes to reserved state."
	::= { lnkaggTraps 0 6 }
	END
