-- File Name   : SPC200.txt

-- Date        : Wed Aug 23 14:03:00 CEST 2006
-- Author      : Gilles Marceau

-- Date        : Tue Jul 06 18:48:54 CEST 2004
-- Author      : Luc Capanaccia

-- Date        : Tue Jul 22 12:00:00 CEST 2004
-- Reviewed by : Gilles Dupont

-- Date        : Mon Sep 13 12:00:00 CEST 2004
-- Reviewed by : Gilles Dupont

-- Date        : Mon Sep 21 12:00:00 CEST 2004
-- Reviewed by : Gilles Dupont

-- Date        : Tue Nov 16 12:30:00 CEST 2004
-- Reviewed by : Luc Capanaccia

-- Date        : Fri Dec 17 12:30:00 CEST 2004
-- Reviewed by : Luc Capanaccia

-- Date        : Thu Sep 15 14:00:00 CEST 2005
-- Reviewed by : Philippe Rimauro (Tag PR01)

-- Date        : Thu Feb 08 14:03:00 CEST 2007
-- Author      : Gilles Marceau

SPC200  DEFINITIONS ::= BEGIN
        IMPORTS
                RowStatus, TruthValue, MacAddress, DisplayString, TEXTUAL-CONVENTION
                        FROM SNMPv2-TC
                AGENT-CAPABILITIES, OBJECT-GROUP, MODULE-COMPLIANCE
                        FROM SNMPv2-CONF
                MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE, Integer32, 
                Counter32, IpAddress, Unsigned32, Gauge32
                        FROM SNMPv2-SMI
                interfaces, ifIndex
                        FROM IF-MIB                        
                spidcom 
                        FROM SPIDCOM-MIB;

                spc200MIB       MODULE-IDENTITY

                LAST-UPDATED    "200412171230Z" -- December 17, 2004

                ORGANIZATION    "Organization"
                CONTACT-INFO    "Contact-info"
                DESCRIPTION     "Description"
                
                REVISION        "200412171230Z"
                DESCRIPTION     "Add software upgrade features"

                REVISION        "200411161230Z"
                DESCRIPTION     "Add adapt level table , commit and reset command"
                                
                REVISION        "200409211200Z"
                DESCRIPTION     "Add quick access to channel modulation and pilots"
                                
                REVISION        "200409131200Z"
                DESCRIPTION     "Add quick access to notches"

                REVISION        "200407221200Z"
                DESCRIPTION     "Corrected compilation errors"

                REVISION        "200407011757Z"
                DESCRIPTION     "Initial revision"
           
                ::=  {  spidcom  1  }

-- TEXTUAL-CONVENTIONS --
        ModulationValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "Modulation amplitude used by a group of carriers."
                SYNTAX                  INTEGER  { none ( 1 ) , 
                                                   bpsk ( 2 ) , 
                                                   qpsk ( 3 )  , 
                                                   qam16 ( 4 ) , 
                                                   qam64 ( 5 ) , 
                                                   qam256 ( 6 ) } 

        CarrierValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "A group is composed of 8 carriers."
                SYNTAX                  Integer32  ( 1 .. 8  ) 

        PilotValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "The pilot carrier wave can be chosen between 
                        the carrier 1 up to carrier 128 inside a band carrier range."
                SYNTAX                  Integer32  ( 1 .. 128  ) 

        BandValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "A channel is composed of 7 bands."
                SYNTAX                  Integer32  ( 1 .. 7  ) 

        PlcChannelType ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "The different type of plc channels:
                          rx for the current reception channel,
                          rx last for the last reception channel,
                          tx for the current transmission channel."
                SYNTAX                  INTEGER  { rx ( 1 ) , 
                                                   rxLast ( 2 ) , 
                                                   tx ( 3 ) } 

        EstimationMode ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "The type of Channel estimation process. Two are available:
                          - automatic, the equipment negociates the best configuration
                            with the remote equipment,
                          - manual, the operator defines the configuration."
                SYNTAX                  INTEGER  { automatic ( 1 ) , 
                                                   manual ( 2 ) } 

        GroupValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "A band is composed of 16 groups."
                SYNTAX                  Integer32  ( 1 .. 16  ) 

        ResultValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "Result value of input vectors."
                SYNTAX                  INTEGER  { success ( 1 ) , 
                                                   fail ( 2 ) } 
                                                   
        AdaptValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "The adapt level integer value."
                SYNTAX                  Integer32  ( 0 .. 8191  )
           
        ChannelBandwidthValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "The channel bandwidth integer value."
                SYNTAX                  Integer32 --PR01
                
        SoftwareIndex ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "The software index."
                SYNTAX                  Integer32  ( 1 .. 10  )
                                                                   
        SoftwareActionResultValue ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "Result value of software action process."
                SYNTAX                  INTEGER  { success ( 0 ) , 
                                                   on-going ( 1 ) ,
                                                   fileNotExist ( 2 ) ,
                                                   flashExhausted ( 3 ),
                                                   flashCorrupted ( 4 ),
                                                   notEnoughMemory ( 5 ),
                                                   invalidParameter ( 6 ),
                                                   genericError ( 7 ) } 
                                                   
        SoftwareActionType ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "Type of software management action."
                SYNTAX                  INTEGER  { switch ( 1 ) , 
                                                   remove ( 2 ) } 
                                                       
--PR01 BEGIN
       PlcModeType ::= TEXTUAL-CONVENTION 
                STATUS                  current
                DESCRIPTION
                        "Type of software management action."
                SYNTAX                  INTEGER  { ad-hoc ( 0 ) , 
                                                   slave  ( 1 ) ,
                                                   master ( 2 ) } 
--PR01 END

-- PLC data

        plc OBJECT IDENTIFIER
                ::=  {  spc200MIB  1  }

-- statistic data

        stats OBJECT IDENTIFIER
                ::=  {  plc  1  }
--PR01 BEGIN                
--        protocol OBJECT IDENTIFIER
--                ::=  {  stats  1  }

--        ip      OBJECT IDENTIFIER
--                ::=  {  protocol  1  }

--        mac     OBJECT IDENTIFIER
--                ::=  {  protocol  2  }

--        plcp    OBJECT IDENTIFIER
--                ::=  {  protocol  3  }

--        ipStatsTable OBJECT-TYPE
--                SYNTAX          SEQUENCE  OF  IpStatsEntry
--                MAX-ACCESS      not-accessible
--                STATUS          current
--                DESCRIPTION     "This table gathers all statistic data specific to 
--                                SPC200 chip relative to IP protocol. The data is 
--                                relative to the underlying interface that is under 
--                                the IP protocol layer. So the table index is 
--                                the ifIndex of such an interface."
--                ::=  { ip  1 }

--        ipStatsEntry OBJECT-TYPE
--                SYNTAX          IpStatsEntry
--                MAX-ACCESS      not-accessible
--                STATUS          current
--                DESCRIPTION     "This row contains IP statistic data specific to 
--                                SPC200  chip. The data is relevant for the interface 
--                                under the IP protocol layer."
--                INDEX           {  ifIndex  }
--                ::=  { ipStatsTable 1 }

--        IpStatsEntry  ::=  SEQUENCE {
--                ipInPkts  Counter32,
--                ipInErrorPkts  Counter32,
--                ipOutPkts  Counter32,
--                ipOutErrorPkts  Counter32,
--                ipInBridgedPkts  Counter32
--                }


--        ipInPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of IP packets received by the interface 
--                                        associated with this entry"
--                ::=  {  ipStatsEntry  1  }


--        ipInErrorPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of inbound IP packets that contained 
--                                        errors preventing them from being deliverable to a
--                                        higher -layer protocol on the interface associated
--                                        with this entry."
--                ::=  {  ipStatsEntry  2  }


--        ipOutPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of outbound IP packets transmitted 
--                                        out the interface associated with this entry"
--                ::=  {  ipStatsEntry  3  }


--        ipOutErrorPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of outbound IP packets that could not be
--                                        transmitted because of errors."
--                ::=  {  ipStatsEntry  4  }


--        ipInBridgedPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of IP packets bridged from the interface,
--                                        associated with this entry, and another one"
--                ::=  {  ipStatsEntry  5  }

--        ipInPackets OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of IP packets received 
--                                        by the SPC200 CHIP"
--                ::=  {  ip  2  }

--        ipInErrorPackets OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of inbound IP packets that 
--                                        contained errors preventing them from being delivered."
--                ::=  {  ip  3  }

--        ipOutPackets OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of outbound IP packets transmitted 
--                                        out the interfaces"
--                ::=  {  ip  4  }

--        ipOutErrorPackets OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of outbound IP packets that could 
--                                        not be transmitted because of errors."
--                ::=  {  ip  5  }

--        ipBridgedPackets OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of IP packets bridged"
--                ::=  {  ip  6  }

--        macStatsTable OBJECT-TYPE
--                SYNTAX          SEQUENCE  OF  MacStatsEntry
--                MAX-ACCESS      not-accessible
--                STATUS          current
--                DESCRIPTION     "This table gathers all SPC200 chip specific packet 
--                                statistics relative to MAC layer.
--                                The data is relative to the underlying interface 
--                                that is under the MAC layer. So the table index is
--                                the ifIndex of such an interface."
--                ::=  { mac  1 }

--        macStatsEntry OBJECT-TYPE
--                SYNTAX          MacStatsEntry
--                MAX-ACCESS      not-accessible
--                STATUS          current
--                DESCRIPTION     "This row contains MAC statistic data specific 
--                                to SPC200 chip. The data is relevant for the interface
--                                under the MAC layer."
--                INDEX           {  ifIndex  }
--                ::=  { macStatsTable 1 }
--
--        MacStatsEntry  ::=  SEQUENCE {
--                macInPkts  Counter32,
--                macInErrorPkts  Counter32,
--                macOutPackets  Counter32,
--                macOutErrorPkts  Counter32
--                }


--        macInPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of MAC  packets received by the interface 
--                                        associated with this entry"
--                ::=  {  macStatsEntry  1  }
--
--
--        macInErrorPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of inbound MAC packets that contained 
--                                        errors preventing them from being deliverable to 
--                                        a higher -layer protocol on the interface
--                                        associated with this entry."
--                ::=  {  macStatsEntry  2  }


--        macOutPackets OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of outbound MAC packets transmitted
--                                        out the interface associated with this entry"
--                ::=  {  macStatsEntry  3  }


--        macOutErrorPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of outbound MAC packets that could not be
--                                        transmitted because of errors."
--                ::=  {  macStatsEntry  4  }

--        plcpStatsTable OBJECT-TYPE
--                SYNTAX          SEQUENCE  OF  PlcpStatsEntry
--                MAX-ACCESS      not-accessible
--                STATUS          current
--                DESCRIPTION     "This table gathers all SPC200 chip specific packet 
--                                statistics relative to PLCP protocol.
--                                The data is relative to the underlying interface that
--                                is under the PLCP protocol layer. So the table index 
--                                is the ifIndex of such an interface."
--                ::=  { plcp  1 }

--        plcpStatsEntry OBJECT-TYPE
--                SYNTAX          PlcpStatsEntry
--                MAX-ACCESS      not-accessible
--                STATUS          current
--                DESCRIPTION     "This row contains PLCP statistic data specific 
--                                to SPC200 chip. The data is relevant for the interface
--                                under the PLCP layer."
--                INDEX           {  ifIndex  }
--                ::=  { plcpStatsTable 1 }

--        PlcpStatsEntry  ::=  SEQUENCE {
--                plcpInPkts  Counter32,
--                plcpInErrorPkts  Counter32,
--                plcpOutPkts  Counter32,
--                plcpOutErrorPkts  Counter32
--                }


--       plcpInPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of PLCP packets received by the interface
--                                        associated with this entry"
--                ::=  {  plcpStatsEntry  1  }


--        plcpInErrorPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of inbound PLCP packets that contained 
--                                        errors preventing them from being deliverable to a
--                                        higher -layer protocol on the interface associated 
--                                        with this entry."
--                ::=  {  plcpStatsEntry  2  }


--        plcpOutPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The total number of outbound PLCP packets transmitted
--                                        out the interface associated with this entry"
--                ::=  {  plcpStatsEntry  3  }


--        plcpOutErrorPkts OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The number of outbound PLCP packets that could not be
--                                        transmitted because of errors."
--                ::=  {  plcpStatsEntry  4  }
--PR01 END                


        portStatsTable OBJECT-TYPE
                SYNTAX          SEQUENCE  OF  PortStatsEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This table gathers all statistic data specific 
                                to SPC200 chip relative to plc connection."
                ::=  { stats  2 }

        portStatsEntry OBJECT-TYPE
                SYNTAX          PortStatsEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This row contains statistic data specific to 
                                SPC200 chip  relative to a connection."
                INDEX           {  plcBasePortIndex,
                                   portStatsBandIndex,
                                   portStatsGroupIndex,
                                   portStatsCarrierIndex }
                ::=  { portStatsTable 1 }

        PortStatsEntry  ::=  SEQUENCE {
                portStatsBandIndex  BandValue,
                portStatsGroupIndex  GroupValue,
                portStatsCarrierIndex  CarrierValue,
                portStatsSignal Counter32,
                portStatsNoise  Counter32
--                portStatsBer Counter32
                }


        portStatsBandIndex OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The band number on which the signal, 
                                        noise, ber data are collected."
                ::=  {  portStatsEntry  1  }


        portStatsGroupIndex OBJECT-TYPE     
                SYNTAX                  GroupValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The group number on which the signal, 
                                        noise, ber data are collected"
                ::=  {  portStatsEntry  2  }


        portStatsCarrierIndex OBJECT-TYPE     
                SYNTAX                  CarrierValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The group number on which the signal, 
                                        noise, ber data are collected"
                ::=  {  portStatsEntry  3  }


        portStatsSignal OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The DB value of the signal associated 
                                        with the carrier wave entry."
                ::=  {  portStatsEntry  4  }


        portStatsNoise OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The DB value of the noise associated 
                                        with the carrier wave entry."
                ::=  {  portStatsEntry  5  }
--PR01 BEGIN
--        portStatsBer OBJECT-TYPE     
--                SYNTAX                  Counter32
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The BER value * 100 associated 
--                                        with the carrier wave entry."
--                ::=  {  portStatsEntry  6  }
--PR01 END

        portStats2Table OBJECT-TYPE
                SYNTAX          SEQUENCE  OF  PortStats2Entry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This table gathers all statistic data specific to 
                                SPC200 chip relative to plc channels. This table has 
                                the same information as the portChannelStatsTable 
                                but in a more compact way. This table has been added 
                                to deal with possible slow performances."
                ::=  { stats  3 }

        portStats2Entry OBJECT-TYPE
                SYNTAX          PortStats2Entry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This row contains statistic data specific to 
                                SPC200 chip  relative to a connection."
                INDEX           {  plcBasePortIndex,
                                   plcModBandIndex  }
                ::=  { portStats2Table 1        }

        PortStats2Entry ::=  SEQUENCE {
                portStats2Signal     OCTET STRING,
                portStats2Noise      OCTET STRING,


--PR01 BEGIN
--                portStats2Ber        OCTET STRING,
                portStats2AvgBandAtt Counter32,
                portStats2AvgBandSNR Counter32
--PR01 END
                }


        portStats2Signal OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The values of the signal for all the carrier waves. 
                                        The expected format is VALUE VALUE VALUE ... VALUE. 
                                        Each value is coded on two bytes. 
                                        There is one value for each 128 carriers of the 
                                        considered band."
                ::=  {  portStats2Entry 1  }


        portStats2Noise OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The values of the noise for all the carrier waves. 
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is coded on two bytes. 
                                        There is one value for each 128 carriers of the 
                                        considered band."
                ::=  {  portStats2Entry 2  }

--        portStats2Ber OBJECT-TYPE     
--                SYNTAX                  OCTET STRING
--                MAX-ACCESS              read-only
--                STATUS                  current
--                DESCRIPTION             "The values of the signal for all the carrier waves. 
--                                        The expected format is VALUE VALUE VALUE ... VALUE. 
--                                        Each value is coded on two bytes. 
--                                        There is one value for each 128 carriers of the 
--                                        considered band.
--                                        The VALUE represents the BER value * 10000."
--                ::=  {  portStats2Entry 3  }

--PR01 BEGIN
       portStats2AvgBandAtt OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Average attenuation per band (dB)." 
                ::=  {  portStats2Entry  3  }


        portStats2AvgBandSNR OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Average SNR per band (dB)."
                ::=  {  portStats2Entry  4  }
--PR01 END
--PR01 BEGIN
        portStats3Table OBJECT-TYPE
                SYNTAX          SEQUENCE  OF  PortStats3Entry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This table gathers all statistic data specific to 
                                SPC200 chip relative to plc channels. This table has 
                                the same information as the portChannelStatsTable 
                                but in a more compact way. This table has been added 
                                to deal with possible slow performances."
                ::=  { stats  4 }

        portStats3Entry OBJECT-TYPE
                SYNTAX          PortStats3Entry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This row contains statistic data specific to 
                                SPC200 chip  relative to a connection."
                INDEX           {  plcBasePortIndex  }
                ::=  { portStats3Table 1 }

        PortStats3Entry ::=  SEQUENCE {
                portStats3AvgAtt      Counter32,
                portStats3AvgSNR      Counter32
                }

       portStats3AvgAtt OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Average attenuation on the link (dB)." 
                ::=  {  portStats3Entry 1  }

       portStats3AvgSNR OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Average SNR on the link (dB)." 
                ::=  {  portStats3Entry 2  }                            
                         
	   bootstats OBJECT-IDENTITY
                STATUS  current
                DESCRIPTION   "boot statistics"
                ::= { stats 5 }

	   bootstatsBoot OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Boot"
                ::=  { bootstats 1 }
       
	   bootstatsManualReset OBJECT-TYPE     
       			SYNTAX                  Counter32
		        MAX-ACCESS              read-only
		        STATUS                  current
		        DESCRIPTION             "Manual reset"
		        ::=  { bootstats 2 }
       
	   bootstatsFailureReset OBJECT-TYPE     
 	            SYNTAX                  Counter32
		        MAX-ACCESS              read-only
		        STATUS                  current
		        DESCRIPTION             "Failure reset"
		        ::=  { bootstats 3 }              
                            
--PR01 END
                
-- configuration data
        plcObjects OBJECT IDENTIFIER
                ::=  {  plc  2  }

        plcMode OBJECT-TYPE     -- PR01
                SYNTAX                  PlcModeType --PR01
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "Plc Mode"
                ::=  {  plcObjects  1  }

        plcTopo OBJECT IDENTIFIER
                ::=  {  plcObjects  2  }

        plcNodeConfiguration OBJECT IDENTIFIER
                ::=  {  plcObjects  3  }

--PR01 BEGIN
         plcSNAnalyser OBJECT IDENTIFIER 
                ::= { plcObjects  4 }

         plcSNAnalyserEnable OBJECT-TYPE     
                SYNTAX                  INTEGER { true ( 1 ) , 
                                                  false ( 2 )  }
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "true if the modem should turn to spectrum analyser mode.
                                        In this mode the modem enters a receive only mode,
                                        and captures periodic samples of the signal on the powerline.
                                        The spectrum analyser mode shall be disabled for normal
                                        powerline modem operation."
                ::=  {  plcSNAnalyser 1  }

         plcSNAnalyserTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcSNAnalyserEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table gathers all statistic data specific to 
                                        SPC200 chip relative to plc analyser."
                ::=  { plcSNAnalyser  2 }

        plcSNAnalyserEntry OBJECT-TYPE
                SYNTAX                  PlcSNAnalyserEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains statistic data specific to 
                                        SPC200 chip relative to a band."
                INDEX                   {  plcModBandIndex   }
                ::=  { plcSNAnalyserTable 1 }

        PlcSNAnalyserEntry  ::=  SEQUENCE {
                plcSNAnalyserMinSignal    OCTET STRING,
                plcSNAnalyserMaxSignal    OCTET STRING,
                plcSNAnalyserAvgSignal    OCTET STRING,
                plcSNAnalyserLastSignal   OCTET STRING,
                plcSNAnalyserFFTDiv       Counter32     
                 }

        plcSNAnalyserMinSignal OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Minimum signal measured over several samples for the
                                        associated carrier wave entry. The value is expressed
                                        in Glomer© which can be converted in dBm/Hz using the
                                        following formula: dBm/Hz = 19*log10(Glomer©) - 113"
                ::=  {  plcSNAnalyserEntry 1  }


        plcSNAnalyserMaxSignal OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Maximum signal measured on several samples for the
                                        associated carrier wave entry. The value is expressed
                                        in Glomer© which can be converted in dBm/Hz using the
                                        following formula: dBm/Hz = 19*log10(Glomer©) - 113"
                ::=  {  plcSNAnalyserEntry  2  }


        plcSNAnalyserAvgSignal OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Average signal measured on several samples for the
                                        associated carrier wave entry. The value is expressed
                                        in Glomer© which can be converted in dBm/Hz using the
                                        following formula: dBm/Hz = 19*log10(Glomer©) - 113"
                ::=  {  plcSNAnalyserEntry  3  }

        plcSNAnalyserLastSignal OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Signal measured for last sample on the associated
                                        carrier wave entry. The value is expressed
                                        in Glomer© which can be converted in dBm/Hz using the
                                        following formula: dBm/Hz = 19*log10(Glomer©) - 113"
                ::=  {  plcSNAnalyserEntry  4  }

        plcSNAnalyserFFTDiv OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "FFT division factor on the associated band."
                ::=  {  plcSNAnalyserEntry 5  }

        plcSNAnalyserAGC OBJECT-TYPE
                SYNTAX                  Integer32 ( 0..255 )
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Gain factor in dB, as used by the
                                        Automatic Gain Control last sample"
                ::=  {  plcSNAnalyser 3  }


         plcAGCAnalyser OBJECT IDENTIFIER 
                ::= { plcObjects  5 }

         plcAGCAnalyserEnable OBJECT-TYPE     
                SYNTAX                  INTEGER { true ( 1 ) , 
                                                  false ( 2 )  }
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             " "
                ::=  {  plcAGCAnalyser  1  }

        plcAGCAnalyserSamplesPart1 OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             " "
                ::=  {  plcAGCAnalyser  2  }

        plcAGCAnalyserSamplesPart2 OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             " "
                ::=  {  plcAGCAnalyser  3  }
--PR01 END

        plcTopoChanges OBJECT-TYPE     
                SYNTAX                  Counter32
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The total number of topology changes detected 
                                        by this plc bridge since the management entity 
                                        was last reset or initialized. Such changes 
                                        concerns only 
                                        - the plcBasePortTable rows 
                                        - the plcBasePortTable columns 
                                        except for plcBasePortChannelEstimation"
                ::=  {  plcTopo  1  }

        plcBasePortTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcBasePortEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains the list of plc remote connection"
                ::=  { plcTopo  2 }

        plcBasePortEntry OBJECT-TYPE
                SYNTAX                  PlcBasePortEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains plc remote connection information"
                INDEX                   {  plcBasePortIndex  }
                ::=  { plcBasePortTable 1 }

        PlcBasePortEntry  ::=  SEQUENCE {
                plcBasePortIndex                MacAddress,
                plcBasePortAddress              MacAddress,
                plcBasePortChannelEstimation    EstimationMode,
                plcBasePortAttenuation          Counter32  }


        plcBasePortIndex OBJECT-TYPE     
                SYNTAX                  MacAddress
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The MAC address of the MAC layer above 
                                        the plc interface of the remote PLC equipment."
                ::=  {  plcBasePortEntry  1  }


        plcBasePortAddress OBJECT-TYPE     
                SYNTAX                  MacAddress
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The MAC address of the MAC layer above 
                                        the plc interface of the remote PLC equipment."
                ::=  {  plcBasePortEntry  2  }


        plcBasePortChannelEstimation    OBJECT-TYPE     
                SYNTAX                  EstimationMode
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "Enable or disable the automatic channel 
                                        estimation processus."
                ::=  {  plcBasePortEntry  3  }                     
                
		plcBasePortAttenuation			OBJECT-TYPE     
                SYNTAX                  Counter32 
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Link attenuation (dB)."
                ::=  {  plcBasePortEntry  4 }       


        plcChannelModulationStringTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcChannelModulationStringEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains string values for a quick access to
                                        the modulation amplitude configurations of all active
                                        channels."
                ::=  { plcTopo  3 }


        plcChannelModulationStringEntry OBJECT-TYPE
                SYNTAX                  PlcChannelModulationStringEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains string values for a quick access to 
                                        the modulation amplitude configuration
                                        of each active channel of the remote 
                                        connection referenced by plcBasePortIndex."
                INDEX                   { plcBasePortIndex }
                ::=  { plcChannelModulationStringTable 1 }


                PlcChannelModulationStringEntry  ::=  SEQUENCE {
                plcRxChannelModulation          OCTET STRING,
                plcRxLastChannelModulation      OCTET STRING,
                plcTxChannelModulation          OCTET STRING }


        plcRxChannelModulation OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude values for the Rx channel of 
                                        a given remote connection entry.
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is an octet representing two modulation values.
                                        Each modulation is coded on 4 bits.
                                        There are ( 16 groups * 7 bands ) / 2 = 66 values."
                ::=  {  plcChannelModulationStringEntry 1  }


        plcRxLastChannelModulation OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude values for the Rx Last channel of 
                                        a given remote connection entry.
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is an octet representing two modulation values.
                                        Each modulation is coded on 4 bits representing ModulationValue - 1.
                                        There are ( 16 groups * 7 bands ) / 2 = 66 values."
                ::=  {  plcChannelModulationStringEntry 2  }

        plcTxChannelModulation OBJECT-TYPE
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude values for the Tx channel of 
                                        a given remote connection entry.
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is an octet representing two modulation values.
                                        Each modulation is coded on 4 bits.
                                        There are ( 16 groups * 7 bands ) / 2 = 66 values."
                ::=  { plcChannelModulationStringEntry  3 }


        plcChannelModulationTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcChannelModulationEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains the modulation amplitude 
                                        configuration of all active channels."
                ::=  { plcTopo  4 }


       plcChannelModulationEntry OBJECT-TYPE
                SYNTAX                  PlcChannelModulationEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains modulation amplitude configuration
                                        of the channel, referenced by the plcPortChannelIndex, 
                                        of the remote connection referenced by 
                                        plcBasePortIndex."
                INDEX                   { plcBasePortIndex, 
                                        plcPortChannelIndex,
                                        plcModBandIndex  }
                ::=  { plcChannelModulationTable 1 }

        PlcChannelModulationEntry  ::=  SEQUENCE {
                plcModBandIndex         BandValue,
                plcModGroup1            ModulationValue,
                plcModGroup2            ModulationValue,
                plcModGroup3            ModulationValue,
                plcModGroup4            ModulationValue,
                plcModGroup5            ModulationValue,
                plcModGroup6            ModulationValue,
                plcModGroup7            ModulationValue,
                plcModGroup8            ModulationValue,
                plcModGroup9            ModulationValue,
                plcModGroup10           ModulationValue,
                plcModGroup11           ModulationValue,
                plcModGroup12           ModulationValue,
                plcModGroup13           ModulationValue,
                plcModGroup14           ModulationValue,
                plcModGroup15           ModulationValue,
                plcModGroup16           ModulationValue
                }


        plcModBandIndex OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The band number of which the modulations are defined"
                ::=  {  plcChannelModulationEntry  1  }


        plcModGroup1 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the first group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  2  }


        plcModGroup2 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the second group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  3  }


        plcModGroup3 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the third group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  4  }


        plcModGroup4 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the fourth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  5  }


        plcModGroup5 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the fifth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  6  }


        plcModGroup6 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the sixth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  7  }


        plcModGroup7 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the seventh group 
                                         of the band entry of the channel entry 
                                         for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  8  }


        plcModGroup8 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the eighth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  9  }


        plcModGroup9 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the nineth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  10  }


        plcModGroup10 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the tenth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  11  }


        plcModGroup11 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the eleventh group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  12  }


        plcModGroup12 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the twelveth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  13  }


        plcModGroup13 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the thirteenth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  14  }


        plcModGroup14 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the fourteenth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  15  }


        plcModGroup15 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the fifteenth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  16  }


        plcModGroup16 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The modulation amplitude of the sixteenth group 
                                        of the band entry of the channel entry 
                                        for a given remote connection entry."
                ::=  {  plcChannelModulationEntry  17  }


        plcChannelModulationInput OBJECT IDENTIFIER
                ::=  { plcTopo  5 }
        
        plcModulationInputAddr OBJECT-TYPE     
                SYNTAX                  MacAddress
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The MAC address of the MAC layer above 
                                        the plc interface of the remote 
                                        PLC equipment for which the modulation 
                                        value changes are requested."
                ::=  {  plcChannelModulationInput  1  }

        plcModulationInputChannel OBJECT-TYPE     
                SYNTAX                  PlcChannelType
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The channel type of the remote PLC equipment
                                        for which the modulation value changes 
                                        are requested."
                ::=  {  plcChannelModulationInput  2  }
                                
        plcModulationInputBand OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The band number of which the modulation value 
                                        changes are requested."
                ::=  {  plcChannelModulationInput  3  }
                                                                
        plcInputModulationGroup1 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        first group of the considered band and 
                                        channel input values."
                ::=  {  plcChannelModulationInput  4  }

        plcInputModulationGroup2 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        second group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  5  }

        plcInputModulationGroup3 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        third group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  6  }

        plcInputModulationGroup4 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        fourth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  7  }

        plcInputModulationGroup5 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        fifth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  8  }

        plcInputModulationGroup6 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        sixth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  9  }

        plcInputModulationGroup7 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        seventh group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  10  }

        plcInputModulationGroup8 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        eighth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  11  }

        plcInputModulationGroup9 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        nineth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  12  }

        plcInputModulationGroup10 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        tenth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  13  }

        plcInputModulationGroup11 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        eleventh group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  14  }

        plcInputModulationGroup12 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        twelveth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  15  }

        plcInputModulationGroup13 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        thirteenth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  16  }

        plcInputModulationGroup14 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        fourteenth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  17  }

        plcInputModulationGroup15 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        fifteenth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  18  }

        plcInputModulationGroup16 OBJECT-TYPE     
                SYNTAX                  ModulationValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The new requested modulation amplitude of the 
                                        sixteenth group of the considered band and
                                        channel input values."
                ::=  {  plcChannelModulationInput  19  }


        plcModulationInputProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request a modification of all the modulations
                                        associated to a band and a channel of a remote
                                        PLC equipment."
                ::=  {  plcChannelModulationInput  20  }

         plcModulationInputResult OBJECT-TYPE     
                SYNTAX                  ResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested modulation value changes."
                ::=  {  plcChannelModulationInput  21  }

        plcPortChannelTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcPortChannelEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains the list of plc channels"
                ::=  { plcTopo  6 }

        plcPortChannelEntry OBJECT-TYPE
                SYNTAX                  PlcPortChannelEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains plc channel information"
                INDEX           {  plcBasePortIndex, plcPortChannelIndex   }
                ::=  { plcPortChannelTable 1 }

        PlcPortChannelEntry  ::=  SEQUENCE {
                plcPortChannelIndex        			Unsigned32,
                plcPortChannelType         			PlcChannelType,
                plcPortChannelGain         			Integer32,
                plcPortChannelBandwidth   			ChannelBandwidthValue,
                plcPortChannelMaxBandwidth 			ChannelBandwidthValue,
                plcPortChannelSynchronizationBand 	BandValue
                }


        plcPortChannelIndex OBJECT-TYPE     
                SYNTAX                  Unsigned32
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The channel number belongs to the remote connection 
                                        with plc equipment associated with the 
                                        plcBasePortIndex        value. 
                                        Only three channels are expected.
                                        Index 1 for RX channel
                                        Index 2 for RXLast channel
                                        index 3 for TX channel"
                ::=  {  plcPortChannelEntry  1  }


        plcPortChannelType OBJECT-TYPE     
                SYNTAX                  PlcChannelType
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The channel type."
                ::=  {  plcPortChannelEntry  2  }


        plcPortChannelGain OBJECT-TYPE     
                SYNTAX                  Integer32
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The gain associated with the channel."
                ::=  {  plcPortChannelEntry  3  }
                
        plcPortChannelBandwidth OBJECT-TYPE     
                SYNTAX                  ChannelBandwidthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The bandwidth of the channel in Kbit/s."
                ::=  {  plcPortChannelEntry  4  }
                                                        
--PR01 BEGIN
        plcPortChannelMaxBandwidth OBJECT-TYPE     
                SYNTAX                  ChannelBandwidthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The maximum bandwidth of the channel in Kbit/s."
                ::=  {  plcPortChannelEntry  5  }
--PR01 END

		plcPortChannelSynchronizationBand OBJECT-TYPE       
				SYNTAX					BandValue
				MAX-ACCESS              read-only
				STATUS					current
				DESCRIPTION				"The synchronization band used for this channel."
				::=  {  plcPortChannelEntry  6  }

        plcChannelPilotStringTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcChannelPilotStringEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains the string values representing
                                        of pilot values of all active channels."
                ::=  { plcTopo  7 }


       plcChannelPilotStringEntry OBJECT-TYPE
                SYNTAX                  PlcChannelPilotStringEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains a quick access for pilot values , 
                                        of the remote connection referenced by 
                                        plcBasePortIndex."
                INDEX                   { plcBasePortIndex }
                ::=  { plcChannelPilotStringTable 1 }


        PlcChannelPilotStringEntry  ::=  SEQUENCE {
                plcRxChannelPilots      OCTET STRING,
                plcRxLastChannelPilots  OCTET STRING,
                plcTxChannelPilots      OCTET STRING}


        plcRxChannelPilots OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The carrier wave numbers which support  
                                        the pilot waves for the Rx Channel.
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is a pair of octets representing the pilot 
                                        values. There is one pair (pilot1 pilot2) for each
                                        of the 7 bands."
                ::=  {  plcChannelPilotStringEntry 1  }


        plcRxLastChannelPilots OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The carrier wave numbers which support  
                                        the pilot waves for the Rx Last Channel.
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is a pair of octets representing the pilot 
                                        values. There is one pair (pilot1 pilot2) for each
                                        of the 7 bands."
                ::=  {  plcChannelPilotStringEntry 2  }
                                
                                
        plcTxChannelPilots OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The carrier wave numbers which support  
                                        the pilot waves for the Tx Channel.
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is a pair of octets representing the pilot 
                                        values. There is one pair (pilot1 pilot2) for each
                                        of the 7 bands."
                ::=  {  plcChannelPilotStringEntry 3  }


        plcChannelPilotsTable OBJECT-TYPE
                SYNTAX                   SEQUENCE  OF  PlcChannelPilotsEntry
                MAX-ACCESS               not-accessible
                STATUS                   current
                DESCRIPTION              "This tabel contains pilots configuration 
                                         for each plc channel."
                ::=  { plcTopo  8 }


        plcChannelPilotsEntry OBJECT-TYPE
                SYNTAX                   PlcChannelPilotsEntry
                MAX-ACCESS               not-accessible
                STATUS                   current
                DESCRIPTION              "This row contains the pilots 1 and 2 configuration 
                                         for a channel defined by the 
                                         couple (plcBasePortIndex, plcPortChannelIndex)"
                INDEX                    {   plcBasePortIndex, 
                                             plcPortChannelIndex,
                                             plcChannelPilotBandIndex  }
                ::=  { plcChannelPilotsTable 1 }

        PlcChannelPilotsEntry  ::=  SEQUENCE {
                plcChannelPilotBandIndex        BandValue,
                plcChannelPilot1                PilotValue,
                plcChannePilot2                 PilotValue
                }


        plcChannelPilotBandIndex OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The band number on which the pilots are defined."
                ::=  {  plcChannelPilotsEntry  1  }


        plcChannelPilot1 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The carrier wave number which supports  
                                        the first pilot wave for the channel
                                        associated with this entry."
                ::=  {  plcChannelPilotsEntry  2  }


        plcChannePilot2 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The carrier wave number which supports 
                                        the second pilot wave for the channel
                                        associated with this entry."
                ::=  {  plcChannelPilotsEntry  3  }


        plcChannelPilotsInput OBJECT IDENTIFIER
                ::=  { plcTopo  9 }
                                
                plcPilotsInputAddr OBJECT-TYPE     
                SYNTAX                  MacAddress
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The MAC address of the MAC layer above 
                                        the plc interface of the remote 
                                        PLC equipment for which the pilot 
                                        value changes are requested."
                ::=  {  plcChannelPilotsInput  1  }

        plcPilotsInputChannel OBJECT-TYPE     
                SYNTAX                  PlcChannelType
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The channel type of the remote PLC equipment
                                        for which the pilot value changes 
                                        are requested."
                ::=  {  plcChannelPilotsInput  2  }
                                
        plcPilotsInputBand OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The band number of which the pilots value 
                                        changes are requested."
                ::=  {  plcChannelPilotsInput  3  }


        plcInputChannelPilot1 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The carrier wave number which supports  
                                        the first pilot wave for the considered band and
                                        channel input values."
                ::=  {  plcChannelPilotsInput  4  }

        plcInputChannelPilot2 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The carrier wave number which supports  
                                        the second pilot wave for the considered band and
                                        channel input values."
                ::=  {  plcChannelPilotsInput  5  }

        plcPilotsInputProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request a modification of the first and second pilot
                                        associated to a band and a channel of a remote
                                        PLC equipment."
                ::=  {  plcChannelPilotsInput  6  }

         plcPilotsInputResult OBJECT-TYPE     
                SYNTAX                  ResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested pilot values changes."
                ::=  {  plcChannelPilotsInput  7  }

        plcNodeNotches OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The values of the notches for all the node bands. 
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is an octet representing the 8 notches of 
                                        each group. There is one value for each 7 * 16 bands."
                ::=  {  plcNodeConfiguration 1  }

        plcNodeNotchesTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcNodeNotchesEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains Notches configuration 
                                        for the SPC200 chip."
                ::=  { plcNodeConfiguration  2 }

        plcNodeNotchesEntry OBJECT-TYPE
                SYNTAX                  PlcNodeNotchesEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains Notches configuration for a group. 
                                        The group is defined by the couple 
                                        (plcNodeNotchesGroupIndex, plcNodeNotchesBandIndex)."
                INDEX                   {  plcNodeNotchesBandIndex, plcNodeNotchesGroupIndex   }
                ::=  { plcNodeNotchesTable 1 }

        PlcNodeNotchesEntry  ::=  SEQUENCE {
                plcNodeNotchesBandIndex  BandValue,
                plcNodeNotchesGroupIndex GroupValue,
                plcNodeNotchesCarrier1   TruthValue,
                plcNodeNotchesCarrier2   TruthValue,
                plcNodeNotchesCarrier3   TruthValue,
                plcNodeNotchesCarrier4   TruthValue,
                plcNodeNotchesCarrier5   TruthValue,
                plcNodeNotchesCarrier6   TruthValue,
                plcNodeNotchesCarrier7   TruthValue,
                plcNodeNotchesCarrier8   TruthValue
                }


        plcNodeNotchesBandIndex OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The band number on which the notches are defined."
                ::=  {  plcNodeNotchesEntry  1  }


        plcNodeNotchesGroupIndex OBJECT-TYPE     
                SYNTAX                  GroupValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The group number on which the notches are defined."
                ::=  {  plcNodeNotchesEntry  2  }


        plcNodeNotchesCarrier1 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the first carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  3  }


        plcNodeNotchesCarrier2 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the second carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  4  }


        plcNodeNotchesCarrier3 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the third carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  5  }


        plcNodeNotchesCarrier4 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the fourth carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  6  }


        plcNodeNotchesCarrier5 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the fifth carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  7  }


        plcNodeNotchesCarrier6 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the sixth carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  8  }


        plcNodeNotchesCarrier7 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the seventh carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  9  }


        plcNodeNotchesCarrier8 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Tell if the eighth carrier of the group entry 
                                        of the band entry is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesEntry  10  }

        plcNodeNotchesInput OBJECT IDENTIFIER
                ::=  { plcNodeConfiguration  3 }
                                
        plcNodeNotchesInputBand OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The band number on which the notches value 
                                        changes are requested."
                ::=  {  plcNodeNotchesInput  1  }


        plcNodeNotchesInputGroup OBJECT-TYPE     
                SYNTAX                  GroupValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The group number on which the notches value 
                                        changes are requested."
                ::=  {  plcNodeNotchesInput  2  }

        plcNodeNotchesInputCarrier1 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The first carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  3  }
                                
        plcNodeNotchesInputCarrier2 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The second carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  4  }
                                
        plcNodeNotchesInputCarrier3 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The third carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  5  }
                                
        plcNodeNotchesInputCarrier4 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The fourth carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  6  }

        plcNodeNotchesInputCarrier5 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The eighth carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  7  }
                                
        plcNodeNotchesInputCarrier6 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The eighth carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  8  }
                                
        plcNodeNotchesInputCarrier7 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The seventh carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  9  }
                                
        plcNodeNotchesInputCarrier8 OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The eighth carrier of the considered group and 
                                        band is a notch carrier. 
                                        The true value means the current carrier is a notch."
                ::=  {  plcNodeNotchesInput  10  }
                              
        plcNodeNotchesInputProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request a modification of the carrier notches
                                        associated to the considered group and 
                                        band."
                ::=  {  plcNodeNotchesInput  11  }

         plcNodeNotchesInputResult OBJECT-TYPE     
                SYNTAX                  ResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested node carrier notches value changes."
                ::=  {  plcNodeNotchesInput  12  }


        plcNodePilots OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The values of the pilot for all the node bands. 
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is a pair of octets representing the pilot 
                                        values. There is one pair (pilot1 pilot2) for each
                                        of the 7 bands."
                ::=  {  plcNodeConfiguration 4  }

        plcNodePilotsTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcNodePilotsEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains pilot values 
                                        used by default on all channels."
                ::=  { plcNodeConfiguration  5 }

        plcNodePilotsEntry OBJECT-TYPE
                SYNTAX                  PlcNodePilotsEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains pilot values 
                                        used by default on a band. 
                                        The band is defined by the index 
                                        plcNodePilotsBandIndex."
                INDEX                   {  plcNodePilotsBandIndex  }
                ::=  { plcNodePilotsTable 1 }

        PlcNodePilotsEntry  ::=  SEQUENCE {
                plcNodePilotsBandIndex  BandValue,
                plcNodePilot1           PilotValue,
                plcNodePilot2           PilotValue
                }


        plcNodePilotsBandIndex OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The band number on which the pilot values are defined."
                ::=  {  plcNodePilotsEntry  1  }


        plcNodePilot1 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The default carrier wave number 
                                        which supports the first pilot wave."
                ::=  {  plcNodePilotsEntry  2  }


        plcNodePilot2 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The default carrier wave number 
                                        which supports the second pilot wave."
                ::=  {  plcNodePilotsEntry  3  }


        plcNodePilotsInput OBJECT IDENTIFIER
                ::=  { plcNodeConfiguration  6 }
                                
        plcNodePilotsInputBand OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The band number on which the pilot values 
                                        changes are requested."
                ::=  {  plcNodePilotsInput  1  }


        plcInputNodePilot1 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The default carrier wave number 
                                        which supports the first pilot wave of 
                                        the considered band."
                ::=  {  plcNodePilotsInput  2  }
                                
        plcInputNodePilot2 OBJECT-TYPE     
                SYNTAX                  PilotValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The default carrier wave number 
                                        which supports the second pilot wave of 
                                        the considered band."
                ::=  {  plcNodePilotsInput  3  }

                              
        plcNodePilotsInputProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request a modification of the pilot values
                                        associated to the considered band."
                ::=  {  plcNodePilotsInput  4  }

         plcNodePilotsInputResult OBJECT-TYPE     
                SYNTAX                  ResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested node pilot values changes."
                ::=  {  plcNodePilotsInput  5  }
                
       plcNodeAdaptsStringTable OBJECT-TYPE
                SYNTAX                  SEQUENCE OF PlcNodeAdaptsStringEntry               
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains string values for a 
                                        quick access to the adapt configurations 
                                        of all the carriers."
                ::=  { plcNodeConfiguration  7 }


       plcNodeAdaptsStringEntry OBJECT-TYPE
                SYNTAX                  PlcNodeAdaptsStringEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains string values for a quick access to 
                                        the adapt configuration
                                        of each carrier of a band."
                INDEX                   { plcBasePortIndex , plcNodeAdaptsStringBandIndex  }
                ::=  { plcNodeAdaptsStringTable 1 }

        PlcNodeAdaptsStringEntry  ::=  SEQUENCE {
                plcNodeAdaptsStringBandIndex BandValue,
                plcNodeAdaptsStringBand      OCTET STRING }

        plcNodeAdaptsStringBandIndex OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The band number on which the adapt values are defined."
                ::=  {  plcNodeAdaptsStringEntry  1  }

        plcNodeAdaptsStringBand OBJECT-TYPE     
                SYNTAX                  OCTET STRING
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt values of the 128 carriers of a band.
                                        The expected format is VALUE VALUE VALUE ... VALUE.
                                        Each value is two octets representing one adapt carrier 
                                        level.
                                        There are ( 16 groups * 8 carriers)  = 128 values."
                ::=  {  plcNodeAdaptsStringEntry 2  }
       
       plcNodeAdaptsTable OBJECT-TYPE
                SYNTAX                  SEQUENCE OF PlcNodeAdaptsEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains adapt level configuration 
                                        for each carrier of the node."
                ::=  { plcNodeConfiguration  8 }

        plcNodeAdaptsEntry OBJECT-TYPE
                SYNTAX                  PlcNodeAdaptsEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains adapt level values 
                                        for a group of carriers. 
                                        The group is defined by the couple
                                        (plcNodeAdaptsBandIndex,plcNodeAdaptsGroupIndex)."
                INDEX                   {  plcNodeAdaptsBandIndex,plcNodeAdaptsGroupIndex  }
                ::=  { plcNodeAdaptsTable 1 }

        PlcNodeAdaptsEntry  ::=  SEQUENCE {
                plcNodeAdaptsBandIndex  BandValue,
                plcNodeAdaptsGroupIndex GroupValue,
                plcNodeAdaptsCarrier1   AdaptValue,
                plcNodeAdaptsCarrier2   AdaptValue,
                plcNodeAdaptsCarrier3   AdaptValue,
                plcNodeAdaptsCarrier4   AdaptValue,
                plcNodeAdaptsCarrier5   AdaptValue,
                plcNodeAdaptsCarrier6   AdaptValue,
                plcNodeAdaptsCarrier7   AdaptValue,
                plcNodeAdaptsCarrier8   AdaptValue
                }


        plcNodeAdaptsBandIndex OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The band number on which the adapt values are defined."
                ::=  {  plcNodeAdaptsEntry  1  }

        plcNodeAdaptsGroupIndex OBJECT-TYPE     
                SYNTAX                  GroupValue
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The group number on which the adapt values are defined."
                ::=  {  plcNodeAdaptsEntry  2  }

        plcNodeAdaptsCarrier1 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the first carrier of the group."
                ::=  {  plcNodeAdaptsEntry  3  }
                
        plcNodeAdaptsCarrier2 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the second carrier of the group."
                ::=  {  plcNodeAdaptsEntry  4  }

        plcNodeAdaptsCarrier3 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the third carrier of the group."
                ::=  {  plcNodeAdaptsEntry  5  }

        plcNodeAdaptsCarrier4 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the fourth carrier of the group."
                ::=  {  plcNodeAdaptsEntry  6 }         
                
        plcNodeAdaptsCarrier5 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the fifth carrier of the group."
                ::=  {  plcNodeAdaptsEntry  7 }         
                
        plcNodeAdaptsCarrier6 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the sixth carrier of the group."
                ::=  {  plcNodeAdaptsEntry  8 }         

        plcNodeAdaptsCarrier7 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the seventh carrier of the group."
                ::=  {  plcNodeAdaptsEntry  9 }                         
                
        plcNodeAdaptsCarrier8 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The adapt level of the eighth carrier of the group."
                ::=  {  plcNodeAdaptsEntry  10 }  
                               
        plcNodeAdaptsInput OBJECT IDENTIFIER
                ::=  { plcNodeConfiguration  9 }
                                
        plcNodeAdaptsInputBand OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The band number on which the adapt level value 
                                        changes are requested."
                ::=  {  plcNodeAdaptsInput  1  }


        plcNodeAdaptsInputGroup OBJECT-TYPE     
                SYNTAX                  GroupValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The group number on which the adapt level value 
                                         changes are requested."
                ::=  {  plcNodeAdaptsInput  2  }

        plcNodeAdaptsInputCarrier1 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the first carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  3  }
                                
        plcNodeAdaptsInputCarrier2 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the second carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  4  }
                                
        plcNodeAdaptsInputCarrier3 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the third carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  5  }
                                
        plcNodeAdaptsInputCarrier4 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the fourth carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  6  }

        plcNodeAdaptsInputCarrier5 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the fifth carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  7  }
                                
        plcNodeAdaptsInputCarrier6 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the sixth carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  8  }
                                
        plcNodeAdaptsInputCarrier7 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the seventh carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  9  }
                                
        plcNodeAdaptsInputCarrier8 OBJECT-TYPE     
                SYNTAX                  AdaptValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The adapt level of the eighth carrier of the 
                                        considered group of the chosen band."
                ::=  {  plcNodeAdaptsInput  10  }
                              
        plcNodeAdaptsInputProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request a modification of the carrier 
                                        adapt level associated to the considered group and 
                                        band."
                ::=  {  plcNodeAdaptsInput  11  }

         plcNodeAdaptsInputResult OBJECT-TYPE     
                SYNTAX                  ResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested node adapt level 
                                        value changes."
                ::=  {  plcNodeAdaptsInput  12  }
       
        plcNodeNetConfigTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  PlcNodeNetConfigEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains ip and mac 
                                        addresses of the node."
                ::=  { plcNodeConfiguration  10 }

        plcNodeNetConfigEntry OBJECT-TYPE
                SYNTAX                  PlcNodeNetConfigEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains ip and mac address
                                        used by an interface."
                INDEX                   {  ifIndex  }
                ::=  { plcNodeNetConfigTable 1 }

        PlcNodeNetConfigEntry  ::=  SEQUENCE {
                plcNodeIpAddr   IpAddress,
                plcNodeNetMask  IpAddress,
                plcNodeMacAddr  MacAddress,
                plcNodeGateway  IpAddress
                }


        plcNodeIpAddr OBJECT-TYPE     
                SYNTAX                  IpAddress
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The IP address of the IP layer above the interface."
                ::=  {  plcNodeNetConfigEntry  1  }


        plcNodeNetMask OBJECT-TYPE     
                SYNTAX                  IpAddress
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The IP Subnet mask of the IP layer above the interface."
                ::=  {  plcNodeNetConfigEntry  2  }


        plcNodeMacAddr OBJECT-TYPE     
                SYNTAX                  MacAddress
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The MAC address of the MAC layer above the interface."
                ::=  {  plcNodeNetConfigEntry  3  }
                
        plcNodeGateway OBJECT-TYPE     
                SYNTAX                  IpAddress
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The Gateway address of the IP layer above the interface."
                ::=  {  plcNodeNetConfigEntry  4  }
                
        plcNodeActions OBJECT IDENTIFIER
                ::=  { plcNodeConfiguration  11 }
                
        plcNodeActionsCommit OBJECT IDENTIFIER
                ::=  { plcNodeActions  1 }
                
        plcNodeActionsCommitProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request the commit of the configuration 
                                        changes into the flash memory"
                ::=  {  plcNodeActionsCommit  1  }

         plcNodeActionsCommitResult OBJECT-TYPE     
                SYNTAX                  ResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested flash commit operation."
                ::=  {  plcNodeActionsCommit  2  }
            
         plcNodeActionsReset OBJECT IDENTIFIER
                ::=  { plcNodeActions  2 }
                
         plcNodeActionsResetProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request the reset of the node.
                                        This operation will terminate the communication 
                                        between the manager and the node"
                ::=  {  plcNodeActionsReset  1  }
                
         plcNodeActionsCarrier OBJECT IDENTIFIER
                ::=  { plcNodeActions  3 }
                
         plcNodeActionsCarrierFlatProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request the equipment to flat the signal"
                ::=  {  plcNodeActionsCarrier  1  }
                
                
plcBssId OBJECT IDENTIFIER
                  ::=  {  plcObjects  6  }
                
plcMasterBssId  OBJECT-TYPE
	  SYNTAX                  INTEGER(0..99)
          MAX-ACCESS              read-write
          STATUS                  current
          DESCRIPTION             "The value of the master Bss Id"
                  ::=  {  plcBssId  1  }   
                  
plcSlaveBssId  OBJECT-TYPE
	  SYNTAX                  INTEGER(0..99)
          MAX-ACCESS              read-write
          STATUS                  current
          DESCRIPTION             "The value of the slave Bss Id"
                  ::=  {  plcBssId  2  }                     
                  
plcSpy OBJECT IDENTIFIER
                  ::=  {  plcObjects  7  }

plcSpyIsDynamic OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to set the spy dynamic mode"
                ::=  {  plcSpy  1  }

plcStaticSpySynchBandNb OBJECT-TYPE     
                SYNTAX                  BandValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The synchronization band number used for static spy mode"
                ::=  {  plcSpy  2  }
                           
                                                                                                                                        
-- software upload
        softwareMgnt  OBJECT IDENTIFIER
                ::=  {  plc  3  }
                
        -- current version
        currentSoftwareVersion OBJECT-TYPE     
                SYNTAX                  DisplayString (SIZE (0..255))
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The name of the current software release."
                ::=  {  softwareMgnt  1 }
                
        currentSoftwareBoardVersion OBJECT-TYPE     
                SYNTAX                  DisplayString (SIZE (0..255))
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The name of the current software board release."
                ::=  {  softwareMgnt  2 }
             
        currentSoftwareAFEVersion OBJECT-TYPE     
                SYNTAX                  DisplayString (SIZE (0..255))
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The name of the current software Analog Front End  release."
                ::=  {  softwareMgnt  3 }
                
-- table of software
        softwareTable OBJECT-TYPE
                SYNTAX                  SEQUENCE  OF  SoftwareEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This table contains the current and reserve 
                                        softwares of the node."
                ::=  { softwareMgnt  4 }

        softwareEntry OBJECT-TYPE
                SYNTAX                  SoftwareEntry
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "This row contains software information."
                INDEX                   {  softwareIndex  }
                ::=  { softwareTable 1 }

        SoftwareEntry  ::=  SEQUENCE {
                softwareIndex           SoftwareIndex,
                softwareVersion         DisplayString
                }

        softwareIndex OBJECT-TYPE     
                SYNTAX                  SoftwareIndex
                MAX-ACCESS              not-accessible
                STATUS                  current
                DESCRIPTION             "The index number of the software."
                ::=  {  softwareEntry  1  }
                
        softwareVersion OBJECT-TYPE     
                SYNTAX                  DisplayString (SIZE (0..255))
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "The name of the software release."
                ::=  {  softwareEntry  2  }
                
        -- upload software action
        softwareUpload OBJECT IDENTIFIER
                ::=  {  softwareMgnt  5 }
                
        softwareUploadTFTPServerIP OBJECT-TYPE     
                SYNTAX                  IpAddress
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The IP address of the TFTP serveur"
                ::=  {  softwareUpload  1  }


        softwareUploadLogin OBJECT-TYPE     
                SYNTAX                  DisplayString (SIZE (0..16))
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The user login on the TFTP server"
                ::=  {  softwareUpload  2  }
               
        softwareUploadPassword OBJECT-TYPE     
                SYNTAX                  DisplayString (SIZE (0..16))
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The user password on the TFTP server. 
                                        Warning: This field is displayed using 6 * characters"
                ::=  {  softwareUpload  3  }
         
        softwareUploadFileName OBJECT-TYPE     
                SYNTAX                  DisplayString (SIZE (0..255))
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The software file name to upload"
                ::=  {  softwareUpload  4  }

         softwareUploadProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request the uploading to start"
                ::=  {  softwareUpload  5  }
                
         softwareUploadResult OBJECT-TYPE     
                SYNTAX                  SoftwareActionResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested uploading"
                ::=  {  softwareUpload  6  }

         softwareUploadTFTPServerPort OBJECT-TYPE     -- PR01
                SYNTAX                  Integer32 ( 0..65535 )
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The service port of the TFTP server"
                ::=  {  softwareUpload  7  }

         
-- software action
        softwareAction  OBJECT IDENTIFIER
                ::=  {  softwareMgnt  6 }
                
        softwareActionIndex OBJECT-TYPE     
                SYNTAX                  SoftwareIndex
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "The index of the reserve software"
                ::=  {  softwareAction  1  }
                
         softwareActionType OBJECT-TYPE     
                SYNTAX                  SoftwareActionType
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "Type of the software action software:
                                        switch, remove "
                ::=  {  softwareAction  2  }

         softwareActionProceed OBJECT-TYPE     
                SYNTAX                  TruthValue
                MAX-ACCESS              read-write
                STATUS                  current
                DESCRIPTION             "True to request the switch between the current 
                                        and the reserver software to start"
                ::=  {  softwareAction  3  }
           
         softwareActionResult OBJECT-TYPE     
                SYNTAX                  SoftwareActionResultValue
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION             "Result value of the requested action"
                ::=  {  softwareAction  4  }

         
-- compliance
        plcConformance OBJECT IDENTIFIER
                ::=  {  plc  4  }
                
        plcCompliances OBJECT IDENTIFIER
                ::=  {  plcConformance  1  }

        plcGroups OBJECT IDENTIFIER
                ::=  {  plcConformance  2  }
                
        plcCompliance MODULE-COMPLIANCE
                STATUS                  current
                DESCRIPTION             "The compliance statement for SPC200 chip."

                MODULE  
                MANDATORY-GROUPS        { nodeGroup, topologyGroup }
                GROUP                   statisticGroup
                DESCRIPTION             "This group is mandatory for 
                                        channel performances analysis"
                ::=  {  plcCompliances  1  }

        nodeGroup OBJECT-GROUP
                OBJECTS                 { plcNodeNotches, plcMode,
                                          plcNodeNotchesCarrier1, plcNodeNotchesCarrier2, 
                                          plcNodeNotchesCarrier3, plcNodeNotchesCarrier4,
                                          plcNodeNotchesCarrier5, plcNodeNotchesCarrier6, 
                                          plcNodeNotchesCarrier7, plcNodeNotchesCarrier8, 
                                          plcNodePilots, plcNodePilot1, plcNodePilot2,
                                          plcNodeAdaptsStringBand, plcNodeAdaptsCarrier1,
                                          plcNodeAdaptsCarrier2, plcNodeAdaptsCarrier3,
                                          plcNodeAdaptsCarrier4, plcNodeAdaptsCarrier5,
                                          plcNodeAdaptsCarrier6, plcNodeAdaptsCarrier7,
                                          plcNodeAdaptsCarrier8,
                                          plcNodeIpAddr, plcNodeNetMask, plcNodeMacAddr,
                                          plcNodeGateway, plcMasterBssId, plcSlaveBssId,
                                          plcSpyIsDynamic, plcStaticSpySynchBandNb }
                STATUS                  current
                DESCRIPTION             "A collection of objects providing 
                                        node configuration information."
                ::=  {  plcGroups  1  }

                inputNodeGroup OBJECT-GROUP
               OBJECTS                 { plcNodeNotchesInputBand, plcNodeNotchesInputGroup,
                                         plcNodeNotchesInputCarrier1, plcNodeNotchesInputCarrier2, 
                                         plcNodeNotchesInputCarrier3, plcNodeNotchesInputCarrier4,
                                         plcNodeNotchesInputCarrier5, plcNodeNotchesInputCarrier6, 
                                         plcNodeNotchesInputCarrier7, plcNodeNotchesInputCarrier8, 
                                         plcNodeNotchesInputProceed,  plcNodeNotchesInputResult,
                                         plcNodePilotsInputBand,
                                         plcInputNodePilot1, plcInputNodePilot2,
                                         plcNodePilotsInputProceed,plcNodePilotsInputResult,                                        
                                         plcNodeAdaptsInputBand, plcNodeAdaptsInputGroup,  
                                         plcNodeAdaptsInputCarrier1, plcNodeAdaptsInputCarrier2,
                                         plcNodeAdaptsInputCarrier3, plcNodeAdaptsInputCarrier4,
                                         plcNodeAdaptsInputCarrier5, plcNodeAdaptsInputCarrier6,
                                         plcNodeAdaptsInputCarrier7, plcNodeAdaptsInputCarrier8,
                                         plcNodeAdaptsInputProceed,  plcNodeAdaptsInputResult,
                                         plcNodeActionsCommitProceed, plcNodeActionsCommitResult,
                                         plcNodeActionsResetProceed, plcNodeActionsCarrierFlatProceed}
                STATUS                  current
                DESCRIPTION             "A collection of objects used to request  
                                        node configuration information changes."
                ::=  {  plcGroups  2  }

        topologyGroup OBJECT-GROUP
                OBJECTS         { plcBasePortAddress, plcBasePortChannelEstimation,
                				  plcBasePortAttenuation ,
                                        plcChannePilot2, plcChannelPilot1,
                                        plcRxChannelPilots,
                                        plcRxLastChannelPilots,
                                        plcTxChannelPilots, 
                                        plcRxChannelModulation,
                                        plcRxLastChannelModulation,
                                        plcTxChannelModulation, 
                                        plcModGroup1, plcModGroup10, plcModGroup11, 
                                        plcModGroup12, plcModGroup13, plcModGroup14, 
                                        plcModGroup15, plcModGroup16, plcModGroup2, 
                                        plcModGroup3, plcModGroup4, plcModGroup5, 
                                        plcModGroup6, plcModGroup7, plcModGroup8, 
                                        plcModGroup9, 
                                        plcPortChannelGain, 
                                        plcPortChannelBandwidth,
                                        plcPortChannelMaxBandwidth, 
                                        plcPortChannelSynchronizationBand,
                                        plcPortChannelType, plcTopoChanges }
                STATUS                  current
                DESCRIPTION             "A collection of objects providing 
                                        topology configuration."
                ::=  {  plcGroups  3  }

        inputTopologyGroup OBJECT-GROUP
                OBJECTS         {       plcModulationInputAddr, plcModulationInputChannel, plcModulationInputBand,
                                        plcInputModulationGroup1, plcInputModulationGroup2,
                                        plcInputModulationGroup3, plcInputModulationGroup4, 
                                        plcInputModulationGroup5, plcInputModulationGroup6, 
                                        plcInputModulationGroup7, plcInputModulationGroup8, 
                                        plcInputModulationGroup9, plcInputModulationGroup10, 
                                        plcInputModulationGroup11, plcInputModulationGroup12,
                                        plcInputModulationGroup13, plcInputModulationGroup14,
                                        plcInputModulationGroup15, plcInputModulationGroup16,
                                        plcModulationInputProceed, plcModulationInputResult,
                                        plcPilotsInputAddr, plcPilotsInputChannel, plcPilotsInputBand,
                                        plcInputChannelPilot1, plcInputChannelPilot2,
                                        plcPilotsInputProceed, plcPilotsInputResult }
                STATUS                  current
                DESCRIPTION             "A collection of objects used to request  
                                        topology configuration changes."
                ::=  {  plcGroups  4  }

        statisticGroup OBJECT-GROUP
                OBJECTS         {    --PR01 BEGIN
                                     --   ipBridgedPackets, ipInBridgedPkts, 
                                     --   ipInErrorPackets, ipInErrorPkts, ipInPackets, 
                                     --   ipInPkts, ipOutErrorPackets, ipOutErrorPkts, 
                                     --   ipOutPackets, ipOutPkts, macInErrorPkts, 
                                     --   macInPkts, macOutErrorPkts, macOutPackets, 
                                     --   plcpInErrorPkts, plcpInPkts, plcpOutErrorPkts,
                                     --   plcpOutPkts, 
                                     --PR01 END
                                        portStats2AvgBandAtt, portStats2AvgBandSNR, --PR01
                                     --   portStats2Ber,
                                        portStats2Noise, portStats2Signal,       
                                     --   portStatsBer,
                                        portStatsNoise, portStatsSignal,
                                        portStats3AvgAtt, portStats3AvgSNR  ,
                                        bootstatsBoot, bootstatsManualReset, bootstatsFailureReset
                                         } --PR01
                STATUS                  current
                DESCRIPTION             "A collection of objects providing 
                                        statistic data on node and plc link performances."
                ::=  {  plcGroups  5  }

        softwareGroup OBJECT-GROUP
                OBJECTS         {       currentSoftwareVersion, currentSoftwareBoardVersion, 
                                        currentSoftwareAFEVersion, softwareVersion,
                                        softwareUploadTFTPServerIP, softwareUploadLogin,
                                        softwareUploadPassword, softwareUploadFileName,
                                        softwareUploadProceed, softwareUploadResult,
                                        softwareUploadTFTPServerPort, --PR01
                                        softwareActionIndex, softwareActionType,
                                        softwareActionProceed, softwareActionResult }
                STATUS                  current
                DESCRIPTION             "A collection of objects providing 
                                        software management"
                ::=  {  plcGroups  6  }

--PR01 BEGIN
        analyserGroup OBJECT-GROUP
                OBJECTS         {       plcSNAnalyserAGC, plcSNAnalyserEnable,
                                        plcSNAnalyserMinSignal, plcSNAnalyserMaxSignal,
                                        plcSNAnalyserAvgSignal, plcSNAnalyserLastSignal,
                                        plcSNAnalyserFFTDiv,
                                        plcAGCAnalyserEnable,
                                        plcAGCAnalyserSamplesPart1, plcAGCAnalyserSamplesPart2 }
                STATUS                  current
                DESCRIPTION             "A collection of objects providing 
                                        spectrum analyser data"
                ::=  {  plcGroups  7  }
--PR01 END

        agentCapabilities AGENT-CAPABILITIES
                PRODUCT-RELEASE         "Product-Release"
                STATUS                  current
                DESCRIPTION             "The SPC200 chip SNMP agent capabilities"

                SUPPORTS                SPC200
                        INCLUDES        { nodeGroup, inputNodeGroup, 
                                          topologyGroup, inputTopologyGroup, 
                                          statisticGroup, softwareGroup,
                                          analyserGroup } --PR01
                                                                  
--OK                SUPPORTS               IF-MIB
--OK                        INCLUDES        { ifGeneralInformationGroup, ifHCPacketGroup }                   
--OK                        VARIATION       ifAdminStatus
--OK                                ACCESS                          read-only
--OK                                DESCRIPTION                     "Forbid the update of the administrative status"                    
--OK                       VARIATION       ifLinkUpDownTrapEnable
--OK                                ACCESS                          not-implemented
--OK                                DESCRIPTION                     "No trap supported"
--KO                       VARIATION       ifAlias
--KO                                ACCESS                          not-implemented
--KO                                DESCRIPTION                     "The non volatile alias name 
--KO                                                                cannot be saved on the SPC200 chip"
--KO                        VARIATION       ifMtu
--KO                                ACCESS                          not-implemented
--KO                                DESCRIPTION                     "Information not available on SPC200 chip"
                                
                SUPPORTS               MAU-MIB
                        INCLUDES        { mauIfGrpBasic }
                        VARIATION       ifMauIndex
                                DESCRIPTION                     "Only one MAU. So the value is always 1"
                        VARIATION       ifMauMediaAvailable
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ifMauMediaAvailableStateExits
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ifMauJabberState
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ifMauJabberingStateEnters
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                                
                SUPPORTS               IP-MIB
                        INCLUDES        { ipGroup }
                        VARIATION       ipForwarding
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipDefaultTTL
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipInHdrErrors
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipInAddrErrors
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipForwDatagrams
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipInUnknownProtos
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipInDiscards
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipInDelivers
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipOutDiscards
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipOutNoRoutes
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipReasmTimeout
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipReasmReqds
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipReasmOKs
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipReasmFails
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipFragOKs
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipFragFails
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipFragCreates
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipAdEntBcastAddr
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipAdEntReasmMaxSize
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                        VARIATION       ipRoutingDiscards
                                ACCESS                          not-implemented
                                DESCRIPTION                     "Information not available on SPC200 chip"
                                
                SUPPORTS                        SNMPv2-MIB
                        INCLUDES        { systemGroup }
                        
--OK                SUPPORTS                        BRIDGE-MIB
--OK                        INCLUDES        { dot1dBase }
--KO                        VARIATION       dot1dBasePortDelayExceededDiscards
--KO                                ACCESS                          not-implemented
--KO                                DESCRIPTION                     "Information not available on SPC200 chip"
--KO                        VARIATION       dot1dBasePortMtuExceededDiscards
--KO                                ACCESS                          not-implemented
--KO                                DESCRIPTION                     "Information not available on SPC200 chip"
                                
                ::=  {  plcConformance  3  }
                        
                
-- ifTableExt data

--ifTableExt OBJECT-TYPE                                  
--       SYNTAX SEQUENCE OF IfEntryExt
--	MAX-ACCESS not-accessible
--	STATUS current
--	DESCRIPTION
--		"A list of interface entries.  The number of entries is
--		given by the value of ifNumber. This Table is an Ext of the
--		standard ifTable located in the IF-MIB."
--	::=  {  spc200MIB  2  }


--ifEntryExt OBJECT-TYPE
--	SYNTAX IfEntryExt
--	MAX-ACCESS not-accessible
--	STATUS current
--	DESCRIPTION
--		"An entry containing management information applicable to a
--		particular interface. These entries are indexed using the ifIndex
--		of the standard IF-MIB."
--	INDEX { ifIndex }
--	::= { ifTableExt 1 }


--IfEntryExt ::= SEQUENCE {
--	ifDefaultSpeed              Gauge32,
--	ifSpeedAutoNegAdminStatus   INTEGER }
	
	
--ifDefaultSpeed OBJECT-TYPE
--	SYNTAX Gauge32
--	MAX-ACCESS read-write
--	STATUS current
--	DESCRIPTION 
--	        "This field is used to set the speed for a given interface.
--	        It contains a default value which will be copied into ifSpeed if
--	        the ifSpeedAutoNegAdminStatus is disabled"		
--	::= { ifEntryExt 1 }	
        
       
--ifSpeedAutoNegAdminStatus OBJECT-TYPE
--	SYNTAX INTEGER {
--			enabled(1),
--			disabled(2) }
--	MAX-ACCESS read-write
--	STATUS current
--	DESCRIPTION
--	       "This field is used to enable/disable the speed auto negotiation 
--	       process for a given interface. If the status is disabled, the user
--	       can set the speed by setting ifDefaultSpeed.
--	       When the speed auto negotiation status is enabled, the hardware 
--	       select a speed and set it in ifSpeed. When the speed auto negotiation 
--	       status is disabled, the content of ifDefaultSpeed is copied into 
--	       ifSpeed."	        		
--	::= { ifEntryExt 2 }                        


--ifGroupExt OBJECT-GROUP
--	OBJECTS {
--		ifDefaultSpeed,
--		ifSpeedAutoNegAdminStatus }
--	STATUS current
--	DESCRIPTION
--		"The fields needed by the SPiDCOM functionalities"
		
--	::= { ifTableExt 2 }


-- ipExt data , for DHCP mode

ipExt OBJECT-IDENTITY
      STATUS  current
      DESCRIPTION
            "Extended ip needed for SPiDCOM functionalities"
       ::= { spc200MIB 4 }

ipDynamic OBJECT-TYPE     
       SYNTAX                  TruthValue
       MAX-ACCESS              read-write
       STATUS                  current
       DESCRIPTION             "True if Ip address is set dynamically"
       ::=  { ipExt 1  }

ipExtGroup OBJECT-GROUP
       OBJECTS {
		ipDynamic 
		}
       STATUS current
       DESCRIPTION             "The fields needed by the SPiDCOM functionalities"		
       ::= { ipExt 2 }

END
