   TPLINK-DDMMANAGE-MIB DEFINITIONS ::= BEGIN

         IMPORTS
            MODULE-IDENTITY, OBJECT-TYPE
          	  	        FROM SNMPv2-SMI
          	ifIndex
						FROM RFC1213-MIB
			DisplayString
						FROM SNMPv2-TC
            tplinkMgmt
						FROM TPLINK-MIB; 
						
				tplinkDdmManageMIB MODULE-IDENTITY
					LAST-UPDATED    "200908270000Z"
					ORGANIZATION    "TPLINK"
					CONTACT-INFO    "www.tplink.com"
					DESCRIPTION	    "Private MIB for DDM configuration."
					REVISION        "200908270000Z"
					DESCRIPTION
					"Initial version of this MIB module."
				::= { tplinkMgmt 96 }
				
				tplinkDdmManageMIBObjects		OBJECT IDENTIFIER	::= { tplinkDdmManageMIB 1 }
				tplinkDdmManageNotifications	OBJECT IDENTIFIER	::= { tplinkDdmManageMIB 2 }
			 												
				tempExceedThreshold NOTIFICATION-TYPE    
					OBJECTS
					{
						ifIndex		
					}
					STATUS          current
					DESCRIPTION
					"A tempExceedThreshold notification is sent when the 
					value of temperature exceeds the threshold. "
					::= { tplinkDdmManageNotifications 1 }

				volExceedThreshold NOTIFICATION-TYPE    
					OBJECTS
					{
						ifIndex		
					}
					STATUS          current
					DESCRIPTION
					"A volExceedThreshold notification is sent when the 
					value of voltage exceeds the threshold. "
					::= { tplinkDdmManageNotifications 2 }

				biasCurExceedThreshold NOTIFICATION-TYPE    
					OBJECTS
					{
						ifIndex		
					}
					STATUS          current
					DESCRIPTION
					"A biasCurExceedThreshold notification is sent when the 
					value of bias current exceeds the threshold. "
					::= { tplinkDdmManageNotifications 3 }  

				txPowExceedThreshold NOTIFICATION-TYPE    
					OBJECTS
					{
						ifIndex		
					}
					STATUS          current
					DESCRIPTION
					"A txPowExceedThreshold notification is sent when the 
					value of Tx power exceeds the threshold. "
					::= { tplinkDdmManageNotifications 4 }        

				rxPowExceedThreshold NOTIFICATION-TYPE    
					OBJECTS
					{
						ifIndex		
					}
					STATUS          current
					DESCRIPTION
					"A rxPowExceedThreshold notification is sent when the 
					value of Rx power exceeds the threshold. "
					::= { tplinkDdmManageNotifications 5 }

END