DKT-CATV-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    Counter32                   FROM SNMPv2-SMI
    OBJECT-GROUP				FROM SNMPv2-CONF
    dkt                         FROM DKT-MIB;

catvMIB MODULE-IDENTITY
    LAST-UPDATED  "200812170000Z"
    ORGANIZATION "DKT A/S"
    CONTACT-INFO
        "postal:  DKT A/S
                  Fanoevej 6
                  DK-4060 Kirke Saaby
                  Denmark

         email:   info@dktcomega.com"
    DESCRIPTION   "DKT CATV MIB."
    ::= { dkt 11 }

catvVersion OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Version string for the CATV module"
    ::= { catvMIB 1 }

catvSwitch OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Switch CATV module on or off. 1 = on 0 = off"
    ::= { catvMIB 2 }

catvSignalDetect OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "CATV Rx signal detect. 1 = signal, 0 = no signal"
    ::= { catvMIB 3 }


catvModuleGroup OBJECT-GROUP
    OBJECTS {
		catvVersion,
		catvSwitch,
		catvSignalDetect
    }
    STATUS current
    DESCRIPTION
        "The objects are related to the DKT CATV module."
    ::= { catvMIB 4 }

END


