-- *****************************************************************
-- Meru Networks Enterprise Specific MIB
--
-- Copyright (c) 2005 by Meru Networks
-- All rights reserved
--
-- *****************************************************************

MERU-CONFIG-AP-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    NOTIFICATION-TYPE, 
    OBJECT-TYPE, 
    MODULE-IDENTITY, 
    OBJECT-IDENTITY,
    enterprises, 
    Counter32, 
    Counter64, 
    Gauge32, 
    TimeTicks, 
    IpAddress, 
    Integer32
        FROM SNMPv2-SMI
    Ipv6Address
        FROM IPV6-TC
    TEXTUAL-CONVENTION, 
    TimeInterval, 
    TimeStamp,
    DateAndTime, 
    TruthValue, 
    DisplayString, 
    MacAddress, 
    RowStatus
        FROM SNMPv2-TC
    mwConfiguration
        FROM MERU-SMI
    MwlAlarmState,
    MwlLedMode,
    MwlOnOffSwitch,
    MwlPowerSupply,
    MwlApIndoorOutdoorType,
    MwlApIpAssignmentType,
    MwlDiscoveryOrder,
    MwlApDiscoveryState,
    MwlEnableDisableOption,
    MwlVpnMode,
    MwlVpnAuthenticationType,
    MwlOperationalState,
    MwlAvailabilityStatus,
    MwlApHwType,
    MwlCertificateStatus,
    MwlCertRequestStatus,
    MwlVpnConnectivityStatus,
    MwlVpnAuthenticationStatus
        FROM MERU-TC;

  mwConfigAp  MODULE-IDENTITY
    LAST-UPDATED "200506050000Z"
    ORGANIZATION "Meru Networks"
    CONTACT-INFO "support@merunetworks.com"
    DESCRIPTION
        "This MIB defines all the managed objects used to manage the Meru WLAN 
         AP Configuration infrastructure"
    ::= { mwConfiguration 2 } 
  
    
  
  mwApTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Table "
    ::= { mwConfigAp 1 }

  mwApEntry  OBJECT-TYPE
    SYNTAX MwApEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Table "
    INDEX {  mwApTableIndex  }
    ::= { mwApTable 1 }

  MwApEntry  ::=  SEQUENCE { 
       mwApTableIndex                                              Integer32, 
       mwApDescr                                                   DisplayString(SIZE (1..63)),
       mwApFloor                                                   DisplayString(SIZE (0..64)),
       mwApNodeId                                                  Unsigned32,
       mwApContact                                                 DisplayString(SIZE (0..64)),
       mwApLedMode                                                 MwlLedMode,
       mwApLocation                                                DisplayString(SIZE (0..64)),
       mwApBuilding                                                DisplayString(SIZE (0..64)),
       mwApParentId                                                Unsigned32,
       mwApInitScript                                              DisplayString(SIZE (0..64)),
       mwApEncryption                                              MwlOnOffSwitch,
       mwApSerialNumber                                            MacAddress,
       mwApIndoorOutdoor                                           MwlApIndoorOutdoorType,
       mwApPowerSupplyType                                         MwlPowerSupply,
       mwApKeepAliveTimeout                                        Integer32(1..1800),
       mwApLinkProbingDuration                                     Unsigned32,
       mwApUpTime                                                  TimeTicks,
       mwApHwRev                                                   DisplayString,
       mwApHwType                                                  MwlApHwType,
       mwApVlanName                                                DisplayString,
       mwApParentMac                                               MacAddress,
       mwApAlarmState                                              MwlAlarmState,
       mwApBootVersion                                             DisplayString,
       mwApFPGAVersion                                             DisplayString,
       mwApIpAddress                                               IpAddress,
       mwApRuntimeVersion                                          DisplayString,
       mwApOperationalState                                        MwlOperationalState,
       mwApAvailabilityStatus                                      MwlAvailabilityStatus,
       mwApRuntimeDiscoveryOrder                                   MwlApDiscoveryState,
       mwApRowStatus                                               RowStatus 
  }
   
   
  mwApTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApEntry 1 }

  mwApDescr  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (1..63))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwApEntry    2 }

  mwApFloor  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..64))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Floor"
    ::= { mwApEntry    3 }

  mwApNodeId  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwApEntry    4 }

  mwApContact  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..64))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Contact"
    ::= { mwApEntry    6 }

  mwApLedMode  OBJECT-TYPE
    SYNTAX MwlLedMode
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes LED Mode"
    ::= { mwApEntry    7 }

  mwApLocation  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..64))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Location"
    ::= { mwApEntry    8 }

  mwApBuilding  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..64))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Building"
    ::= { mwApEntry    9 }

  mwApParentId  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Parent AP ID"
    ::= { mwApEntry   10 }

  mwApInitScript  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..64))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP Init Script"
    ::= { mwApEntry   11 }

  mwApEncryption  OBJECT-TYPE
    SYNTAX MwlOnOffSwitch
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Dataplane Encryption"
    ::= { mwApEntry   12 }

  mwApSerialNumber  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes MAC Address"
    ::= { mwApEntry   13 }

  mwApIndoorOutdoor  OBJECT-TYPE
    SYNTAX MwlApIndoorOutdoorType
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP Indoor/Outdoor type"
    ::= { mwApEntry   14 }

  mwApLinkProbingDuration  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Link Probing Duration"
    ::= { mwApEntry   16 }

  mwApUpTime  OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Uptime"
    ::= { mwApEntry   17 }

  mwApHwRev  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Hardware Revision"
    ::= { mwApEntry   18 }

  mwApHwType  OBJECT-TYPE
    SYNTAX MwlApHwType
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes AP Model"
    ::= { mwApEntry   19 }

  mwApParentMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Parent MAC Address"
    ::= { mwApEntry   20 }

  mwApAlarmState  OBJECT-TYPE
    SYNTAX MwlAlarmState
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Alarm State"
    ::= { mwApEntry   21 }

  mwApBootVersion  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Boot Image Version"
    ::= { mwApEntry   22 }

  mwApFPGAVersion  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes FPGA Version"
    ::= { mwApEntry   23 }

  mwApRuntimeVersion  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Runtime Image Version"
    ::= { mwApEntry   24 }

  mwApOperationalState  OBJECT-TYPE
    SYNTAX MwlOperationalState
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Operational State"
    ::= { mwApEntry   26 }

  mwApAvailabilityStatus  OBJECT-TYPE
    SYNTAX MwlAvailabilityStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Availability Status"
    ::= { mwApEntry   27 }

  mwApRuntimeDiscoveryOrder  OBJECT-TYPE
    SYNTAX MwlApDiscoveryState
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Connectivity Layer"
    ::= { mwApEntry   28 }

  mwApPowerSupplyType  OBJECT-TYPE
    SYNTAX MwlPowerSupply
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Power Supply Type"
    ::= { mwApEntry   29 }

  mwApKeepAliveTimeout  OBJECT-TYPE
    SYNTAX Integer32(1..1800)
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes KeepAlive Timeout(seconds)"
    ::= { mwApEntry   30 }

  mwApVlanName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes VLAN Name"
    ::= { mwApEntry   38 }

  mwApIpAddress  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes AP IP Address for L3"
    ::= { mwApEntry   39 }

  mwApRowStatus  OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object is used to create and delete rows in the table"
    ::= { mwApEntry 56 }

  mwAp2controllerMapTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwAp2controllerMapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Assignments of APs to Controllers "
    ::= { mwConfigAp 2 }

  mwAp2controllerMapEntry  OBJECT-TYPE
    SYNTAX MwAp2controllerMapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Assignments of APs to Controllers "
    INDEX {  mwAp2controllerMapTableIndex  }
    ::= { mwAp2controllerMapTable 1 }

  MwAp2controllerMapEntry  ::=  SEQUENCE { 
       mwAp2controllerMapTableIndex                                Integer32, 
       mwAp2controllerMapApMac                                     MacAddress,
       mwAp2controllerMapDestinationController                     DisplayString,
       mwAp2controllerMapRowStatus                                 RowStatus 
  }
   
   
  mwAp2controllerMapTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwAp2controllerMapEntry 1 }

  mwAp2controllerMapApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP MAC Address"
    ::= { mwAp2controllerMapEntry    2 }

  mwAp2controllerMapDestinationController  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Destination Controller"
    ::= { mwAp2controllerMapEntry    3 }

  mwAp2controllerMapRowStatus  OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object is used to create and delete rows in the table"
    ::= { mwAp2controllerMapEntry 4 }

  mwApip2controllerMapTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApip2controllerMapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Assignments of AP subnet to Controllers "
    ::= { mwConfigAp 3 }

  mwApip2controllerMapEntry  OBJECT-TYPE
    SYNTAX MwApip2controllerMapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Assignments of AP subnet to Controllers "
    INDEX {  mwApip2controllerMapTableIndex  }
    ::= { mwApip2controllerMapTable 1 }

  MwApip2controllerMapEntry  ::=  SEQUENCE { 
       mwApip2controllerMapTableIndex                              Integer32, 
       mwApip2controllerMapApSubnetIp                              IpAddress,
       mwApip2controllerMapApSubnetMask                            IpAddress,
       mwApip2controllerMapDestinationController                   DisplayString,
       mwApip2controllerMapRowStatus                               RowStatus 
  }
   
   
  mwApip2controllerMapTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApip2controllerMapEntry 1 }

  mwApip2controllerMapApSubnetIp  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP IP Subnet"
    ::= { mwApip2controllerMapEntry    2 }

  mwApip2controllerMapApSubnetMask  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP Netmask"
    ::= { mwApip2controllerMapEntry    3 }

  mwApip2controllerMapDestinationController  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Destination Controller"
    ::= { mwApip2controllerMapEntry    4 }

  mwApip2controllerMapRowStatus  OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object is used to create and delete rows in the table"
    ::= { mwApip2controllerMapEntry 5 }

  mwApSwapTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApSwapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Replacement Table "
    ::= { mwConfigAp 4 }

  mwApSwapEntry  OBJECT-TYPE
    SYNTAX MwApSwapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Replacement Table "
    INDEX {  mwApSwapTableIndex  }
    ::= { mwApSwapTable 1 }

  MwApSwapEntry  ::=  SEQUENCE { 
       mwApSwapTableIndex                                          Integer32, 
       mwApSwapNewApMac                                            MacAddress,
       mwApSwapCurrentApMac                                        MacAddress,
       mwApSwapRowStatus                                           RowStatus 
  }
   
   
  mwApSwapTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApSwapEntry 1 }

  mwApSwapNewApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes New AP MAC Address"
    ::= { mwApSwapEntry    2 }

  mwApSwapCurrentApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes AP MAC Address"
    ::= { mwApSwapEntry    3 }

  mwApSwapRowStatus  OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object is used to create and delete rows in the table"
    ::= { mwApSwapEntry 4 }

  mwApConnectivityTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApConnectivityEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Network Connectivity configuration "
    ::= { mwConfigAp 5 }

  mwApConnectivityEntry  OBJECT-TYPE
    SYNTAX MwApConnectivityEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Network Connectivity configuration "
    INDEX {  mwApConnectivityTableIndex  }
    ::= { mwApConnectivityTable 1 }

  MwApConnectivityEntry  ::=  SEQUENCE { 
       mwApConnectivityTableIndex                                  Integer32, 
       mwApConnectivityWncIp                                       IpAddress,
       mwApConnectivityHostName                                    DisplayString(SIZE (0..63)),
       mwApConnectivityPrimaryDns                                  IpAddress,
       mwApConnectivityWncHostName                                 DisplayString(SIZE (0..63)),
       mwApConnectivityAssignedType                                MwlApIpAssignmentType,
       mwApConnectivitySecondaryDns                                IpAddress,
       mwApConnectivityWncDomainName                               DisplayString,
       mwApConnectivityConfigureIpAddr                             IpAddress,
       mwApConnectivityConfigureNetMask                            IpAddress,
       mwApConnectivityConfigureGatewayAddr                        IpAddress,
       mwApConnectivityConfiguredDiscoveryOrder                    MwlDiscoveryOrder,
       mwApConnectivityNodeId                                      Integer32,
       mwApConnectivityNodeName                                    DisplayString,
       mwApConnectivityVPNState                                    MwlEnableDisableOption,
       mwApConnectivityVPNStatus                                   MwlVpnMode,
       mwApConnectivityDomainName                                  DisplayString,
       mwApConnectivityVpnServerIp                                 IpAddress,
       mwApConnectivityWncTunnelIp                                 IpAddress,
       mwApConnectivityRuntimeDns1                                 IpAddress,
       mwApConnectivityRuntimeDns2                                 IpAddress,
       mwApConnectivityRuntimeDns3                                 IpAddress,
       mwApConnectivityRuntimeDns4                                 IpAddress,
       mwApConnectivityRuntimeDns5                                 IpAddress,
       mwApConnectivityRuntimeDns6                                 IpAddress,
       mwApConnectivityRuntimeDns7                                 IpAddress,
       mwApConnectivityRuntimeDns8                                 IpAddress,
       mwApConnectivityVpnServerPort                               Unsigned32,
       mwApConnectivityRuntimeIpAddr                               IpAddress,
       mwApConnectivityVPNAuthMethod                               MwlVpnAuthenticationType,
       mwApConnectivityRuntimeNetMask                              IpAddress,
       mwApConnectivityVpnServerHostName                           DisplayString(SIZE (0..63)),
       mwApConnectivityRuntimeGatewayAddr                          IpAddress,
       mwApConnectivityRuntimeTunnelIpAddr                         IpAddress,
       mwApConnectivityRuntimeDiscoveryState                       MwlApDiscoveryState 
  }
   
   
  mwApConnectivityTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApConnectivityEntry 1 }

  mwApConnectivityWncIp  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Controller Address"
    ::= { mwApConnectivityEntry    2 }

  mwApConnectivityHostName  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes AP Host Name"
    ::= { mwApConnectivityEntry    3 }

  mwApConnectivityPrimaryDns  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Primary DNS Server"
    ::= { mwApConnectivityEntry    4 }

  mwApConnectivityWncHostName  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Controller Host Name"
    ::= { mwApConnectivityEntry    5 }

  mwApConnectivityAssignedType  OBJECT-TYPE
    SYNTAX MwlApIpAssignmentType
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes IP Type"
    ::= { mwApConnectivityEntry    6 }

  mwApConnectivitySecondaryDns  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Secondary DNS Server "
    ::= { mwApConnectivityEntry    7 }

  mwApConnectivityWncDomainName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Controller Domain Name"
    ::= { mwApConnectivityEntry    8 }

  mwApConnectivityConfigureIpAddr  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Static IP Address"
    ::= { mwApConnectivityEntry    9 }

  mwApConnectivityConfigureNetMask  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Static IP Netmask"
    ::= { mwApConnectivityEntry   10 }

  mwApConnectivityConfigureGatewayAddr  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Static Default Gateway"
    ::= { mwApConnectivityEntry   11 }

  mwApConnectivityConfiguredDiscoveryOrder  OBJECT-TYPE
    SYNTAX MwlDiscoveryOrder
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This object describes Discovery Protocol"
    ::= { mwApConnectivityEntry   12 }

  mwApConnectivityNodeId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwApConnectivityEntry   13 }

  mwApConnectivityNodeName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwApConnectivityEntry   14 }

  mwApConnectivityDomainName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Domain Name"
    ::= { mwApConnectivityEntry   15 }

  mwApConnectivityRuntimeDns1  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 1"
    ::= { mwApConnectivityEntry   16 }

  mwApConnectivityRuntimeDns2  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 2"
    ::= { mwApConnectivityEntry   17 }

  mwApConnectivityRuntimeDns3  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 3"
    ::= { mwApConnectivityEntry   18 }

  mwApConnectivityRuntimeDns4  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 4"
    ::= { mwApConnectivityEntry   19 }

  mwApConnectivityRuntimeDns5  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 5"
    ::= { mwApConnectivityEntry   20 }

  mwApConnectivityRuntimeDns6  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 6"
    ::= { mwApConnectivityEntry   21 }

  mwApConnectivityRuntimeDns7  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 7"
    ::= { mwApConnectivityEntry   22 }

  mwApConnectivityRuntimeDns8  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes DNS Server 8"
    ::= { mwApConnectivityEntry   23 }

  mwApConnectivityRuntimeIpAddr  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes IP Address "
    ::= { mwApConnectivityEntry   24 }

  mwApConnectivityRuntimeNetMask  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes NetMask"
    ::= { mwApConnectivityEntry   25 }

  mwApConnectivityRuntimeGatewayAddr  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Gateway"
    ::= { mwApConnectivityEntry   26 }

  mwApConnectivityRuntimeDiscoveryState  OBJECT-TYPE
    SYNTAX MwlApDiscoveryState
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Connectivity Layer"
    ::= { mwApConnectivityEntry   27 }

  mwApConnectivityVPNState  OBJECT-TYPE
    SYNTAX MwlEnableDisableOption
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes VPN"
    ::= { mwApConnectivityEntry   28 }

  mwApConnectivityVPNAuthMethod  OBJECT-TYPE
    SYNTAX MwlVpnAuthenticationType
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes VPN Authentication Method"
    ::= { mwApConnectivityEntry   29 }

  mwApConnectivityWncTunnelIp  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Controller Tunnel IP Address"
    ::= { mwApConnectivityEntry   30 }

  mwApConnectivityRuntimeTunnelIpAddr  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Tunnel IP "
    ::= { mwApConnectivityEntry   31 }

  mwApConnectivityVpnServerIp  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes VPN Server IP"
    ::= { mwApConnectivityEntry   32 }

  mwApConnectivityVpnServerHostName  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes VPN Server Host Name"
    ::= { mwApConnectivityEntry   33 }

  mwApConnectivityVpnServerPort  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes VPN Server Port"
    ::= { mwApConnectivityEntry   34 }

  mwApConnectivityVPNStatus  OBJECT-TYPE
    SYNTAX MwlVpnMode
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes VPN Connectivity Mode"
    ::= { mwApConnectivityEntry   35 }

  mwApCertificateTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApCertificateEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Certificate configuration "
    ::= { mwConfigAp 6 }

  mwApCertificateEntry  OBJECT-TYPE
    SYNTAX MwApCertificateEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Certificate configuration "
    INDEX {  mwApCertificateTableIndex  }
    ::= { mwApCertificateTable 1 }

  MwApCertificateEntry  ::=  SEQUENCE { 
       mwApCertificateTableIndex                                   Integer32, 
       mwApCertificateNodeId                                       Integer32,
       mwApCertificateNodeName                                     DisplayString,
       mwApCertificateApHwType                                     MwlApHwType,
       mwApCertificateValidity                                     DateAndTime,
       mwApCertificateSerialNumber                                 MacAddress,
       mwApCertificateApCertReqStatus                              MwlCertRequestStatus,
       mwApCertificateOperationalState                             MwlOperationalState,
       mwApCertificateAvailabilityStatus                           MwlAvailabilityStatus,
       mwApCertificateStatus                                       MwlCertificateStatus,
       mwApCertificateCertificateAuthority                         DisplayString,
       mwApCertificateRowStatus                                    RowStatus 
  }
   
   
  mwApCertificateTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApCertificateEntry 1 }

  mwApCertificateNodeId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwApCertificateEntry    2 }

  mwApCertificateNodeName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwApCertificateEntry    3 }

  mwApCertificateSerialNumber  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes MAC Address"
    ::= { mwApCertificateEntry    4 }

  mwApCertificateOperationalState  OBJECT-TYPE
    SYNTAX MwlOperationalState
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Operational State"
    ::= { mwApCertificateEntry    5 }

  mwApCertificateAvailabilityStatus  OBJECT-TYPE
    SYNTAX MwlAvailabilityStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Availability Status"
    ::= { mwApCertificateEntry    6 }

  mwApCertificateStatus  OBJECT-TYPE
    SYNTAX MwlCertificateStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Certificate Status"
    ::= { mwApCertificateEntry    7 }

  mwApCertificateApCertReqStatus  OBJECT-TYPE
    SYNTAX MwlCertRequestStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes User Req Status"
    ::= { mwApCertificateEntry    8 }

  mwApCertificateCertificateAuthority  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes CA"
    ::= { mwApCertificateEntry    9 }

  mwApCertificateValidity  OBJECT-TYPE
    SYNTAX DateAndTime
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Validity (MM/DD/YYYY)"
    ::= { mwApCertificateEntry   10 }

  mwApCertificateApHwType  OBJECT-TYPE
    SYNTAX MwlApHwType
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes AP Model"
    ::= { mwApCertificateEntry   11 }

  mwApCertificateRowStatus  OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object is used to create and delete rows in the table"
    ::= { mwApCertificateEntry 20 }

  mwApVpnClientInfoTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApVpnClientInfoEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP VPN Clients Info "
    ::= { mwConfigAp 7 }

  mwApVpnClientInfoEntry  OBJECT-TYPE
    SYNTAX MwApVpnClientInfoEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP VPN Clients Info "
    INDEX {  mwApVpnClientInfoTableIndex  }
    ::= { mwApVpnClientInfoTable 1 }

  MwApVpnClientInfoEntry  ::=  SEQUENCE { 
       mwApVpnClientInfoTableIndex                                 Integer32, 
       mwApVpnClientInfoApMac                                      MacAddress,
       mwApVpnClientInfoNodeId                                     Integer32,
       mwApVpnClientInfoNodeName                                   DisplayString,
       mwApVpnClientInfoRealIpAddr                                 IpAddress,
       mwApVpnClientInfoTunnelIpAddr                               IpAddress,
       mwApVpnClientInfoVpnConnectivityStatus                      MwlVpnConnectivityStatus,
       mwApVpnClientInfoVpnAuthenticationStatus                    MwlVpnAuthenticationStatus 
  }
   
   
  mwApVpnClientInfoTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApVpnClientInfoEntry 1 }

  mwApVpnClientInfoNodeId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwApVpnClientInfoEntry    2 }

  mwApVpnClientInfoNodeName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwApVpnClientInfoEntry    3 }

  mwApVpnClientInfoApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP MAC"
    ::= { mwApVpnClientInfoEntry    4 }

  mwApVpnClientInfoTunnelIpAddr  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes VPN IP Address "
    ::= { mwApVpnClientInfoEntry    5 }

  mwApVpnClientInfoRealIpAddr  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Real IP Address "
    ::= { mwApVpnClientInfoEntry    6 }

  mwApVpnClientInfoVpnConnectivityStatus  OBJECT-TYPE
    SYNTAX MwlVpnConnectivityStatus
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes VPN Connectivity Status"
    ::= { mwApVpnClientInfoEntry    7 }

  mwApVpnClientInfoVpnAuthenticationStatus  OBJECT-TYPE
    SYNTAX MwlVpnAuthenticationStatus
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes VPN Authentication Status"
    ::= { mwApVpnClientInfoEntry    8 }

  
END
   