ICOTERA-I6400-SERIES DEFINITIONS ::= BEGIN
--
-- Copyright (c) 2015-2017 Icotera A/S --
--

IMPORTS
  MODULE-IDENTITY,
  OBJECT-IDENTITY,
  OBJECT-TYPE,
  enterprises,
  Counter32,
  Gauge32,
  Integer32,
  Counter64,
  IpAddress
    	FROM SNMPv2-SMI
  TEXTUAL-CONVENTION
        FROM SNMPv2-TC
  DisplayString
        FROM RFC1213-MIB;

--
-- IcoteraEnterprise SMI --
--

icotera MODULE-IDENTITY
    LAST-UPDATED "201703011646Z"
    ORGANIZATION "Icotera A/S"
    CONTACT-INFO
    "Icotera A/S
     Customer Support

     Mail : Kongevejen 400D
            2840 Holte
            Danmark

     Tel  : +45 7010 0033

     E-mail: support@icotera.com
     Web   : http://icotera.com"

    DESCRIPTION
    "The Icotera management information base SMI definitions"

    REVISION "201703011646Z"
    DESCRIPTION
        "MIBs were adjusted to match all 
		i64xx-series CPE product family."

    REVISION "201702091427Z"
    DESCRIPTION
	"Minor correction of object values"

    REVISION "201701161032Z"
    DESCRIPTION
	"Added support for Multicast Analyser"

    REVISION "201608260924Z"
    DESCRIPTION
	"Minor correction of object names, 
	unnecessary commentary removed"

    REVISION "201608240904Z"
    DESCRIPTION
	"Missing descriptions added,
	Some MODULE_IDENTITY was changed to correct OBJECT_IDENTITY,
	CATV Filter packages fixed,
	Fixed mib name from 4k to 1k,
	Minor cosmetic corrections,
	Added support for DDM"

    REVISION "201504011357Z"
    DESCRIPTION
        "Created from ICOTERA-MIB.mib"

    ::= { enterprises 29865 }  -- assigned by IANA --

--
-- All SNMP options supported by i6400-series CPE --
--
ictIGW1k OBJECT-IDENTITY
		STATUS current
		DESCRIPTION
		"Device related SNMP options"
		::= { icotera 11 }

ictMgmt		OBJECT IDENTIFIER ::= { ictIGW1k 2 }
ictServices	OBJECT IDENTIFIER ::= { ictIGW1k 3 }
ictReset 	OBJECT IDENTIFIER ::= { ictIGW1k 5 }
ictMcastAnalyzer   OBJECT IDENTIFIER ::= { ictIGW1k 7 }

--
-- CATV detailed status --
--
-- CATV definition --
--

ictServicesMibs OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The MIB module for managing Icotera services"
       ::= { ictServices 1 }

ictCatv OBJECT-IDENTITY
STATUS current
    DESCRIPTION
    "The MIB module for managing Icotera services"
       ::= { ictServicesMibs 1 }

--
-- CATV subtree options --

catvModuleAdminStatus OBJECT-TYPE
    SYNTAX INTEGER {
      disabled(0),
      enabled(1)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "The administrative status of the module, this can be enabled(1) or
    disabled(0)."
    DEFVAL { 0 }
      ::= { ictCatv 1 }

catvModuleFilter OBJECT-TYPE
    SYNTAX INTEGER {
      none(0),
      pkg1(1),
      pkg2(2),
      pkg3(3),
      pkg4(4)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Package filter selected for catv module"
      ::= { ictCatv 2 }

catvModuleRflevel OBJECT-TYPE
    SYNTAX INTEGER {
      auto(0),
      low(1),
      medium(2),
      high(3)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "RF signal amplification on CATV output"
      ::= { ictCatv 3 }

catvModuleLowSignal OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Low signal level of catv led"
      ::= { ictCatv 4 }

catvModuleSignalDetected OBJECT-TYPE
    SYNTAX INTEGER {
      no(0),
      yes(1)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Tells whether CATV signal is detected: yes(1) - detected, no(0) - not detected." 
      ::= { ictCatv 5 }

catvModulePowerLevel OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Current CATV power level. It can have one of the following values:
     - any integer between -1099 and 199 when the power level is higher than -11.00 and lower than 2.00,
       which is the power level in dBm multiplied by 100.
     - a value of -2147483648 when the power level is lower than -11 dBm
     - a value of 2147483647 when the power level is higher than 2 dBm." 
      ::= { ictCatv 6 }

--
-- DDM feature --
--
-- Note: this is supported only by CPE equipped with DDM Transciever
-- 

--ictTransceiver OBJECT-IDENTITY
--    STATUS current
--    DESCRIPTION
--   "The general MIB module for Transciever diagnostic module"
--      ::= { ictServices 1 }

ictTransceiver OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The container for DDM related MIB module"
      ::= { ictServicesMibs 3 }

transceiverDdmTemperature OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Internally measured transceiver temperature.
     Represented in increments of 1/256 degrees Celsius,
     yielding a total range of (minus) 128C to (plus) 128C." 
      ::= { ictTransceiver 1 }

transceiverDdmTxPower OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Measured TX output power.
     Represented in increments of 1/10000 mW." 
      ::= { ictTransceiver 2 }

transceiverDdmRxPower OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Measured RX received optical power.
     Represented in increments of 1/10000 mW." 
      ::= { ictTransceiver 3 }

transceiverDdmVoltage OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Internally measured transceiver supply voltage.
     Represented in increments of 1/10000 V." 
      ::= { ictTransceiver 4 }

transceiverDdmTxBiasCurrent OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Measured TX bias current.
     Represented in increments of 1/500 mA." 
      ::= { ictTransceiver 5 }

transceiverTransceiverType OBJECT-TYPE
    SYNTAX INTEGER {
      unknown(0),
      gbic(1),
      moduleSolderedToMotherboard(2),
      sfp(3),
      type300pinXbi(4),
      xenpak(5),
      xfp(6),
      xff(7),
      xfpE(8),
      xPak(9),
      x2(10),
      dWdmSfp(11),
      qSfp(12)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Type of serial transceiver." 
      ::= { ictTransceiver 6 }

transceiverLaserWavelength OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "TX Laser Wavelength, units of nm." 
      ::= { ictTransceiver 7 }

transceiverConnectorType OBJECT-TYPE
    SYNTAX INTEGER {
      unknown(0),
      sc(1),
      fibreChannelStyle1CopperConnector(2),
      fibreChannelStyle2CopperConnector(3),
      bncTnc(4),
      fibreChannelCoaxialHeaders(5),
      fiberJack(6),
      lc(7),
      mtRj(8),
      mu(9),
      sg(10),
      opticalPigtail(11),
      mpoParallelOptic(12),
      hssdcII(32),
      copperPigtail(33),
      rj45(34)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Connector type provided." 
      ::= { ictTransceiver 8 }

transceiverEthernetCompliance OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Ethernet compliance. 8-bit bit field:
     Bit 7 - BASE-PX
     Bit 6 - BASE-BX10
     Bit 5 - 100BASE-FX
     Bit 4 - 100BASE-LX/LX10
     Bit 3 - 1000BASE-T
     Bit 2 - 1000BASE-CX
     Bit 1 - 1000BASE-LX
     Bit 0 - 1000BASE-SX." 
      ::= { ictTransceiver 9 }

transceiverLinkLength OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Link length supported for single mode fiber, units of km." 
      ::= { ictTransceiver 10 }

transceiverDiagCapable OBJECT-TYPE
    SYNTAX INTEGER {
      no(0),
      yes(1)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "Digital diagnostic monitoring implemented." 
      ::= { ictTransceiver 11 }

-- END of SERVICEs part --
--
--
-- RESET detailed status --
--
-- Factory reset definition --

ictFacRst OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The MIB parent for CPE reset"
       ::= { ictReset 1 }

ictFacRstMib OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The MIB which makes Factory Reset of CPE"
       ::= { ictFacRst 1 }

--
-- FactoryReset subtree options --

performFactoryReset OBJECT-TYPE
  SYNTAX INTEGER {
    noActionRequested(0),
    makeFactoryreset(1),
    someErrorOccured(3)
  }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION 
     "MIB used to perform Factory Reset."
  DEFVAL { 0 }
    ::= { ictFacRstMib 1 }

-- END of RESET part --

--
-- Management functions --
--
-- Management definition --
--

ictMgmtMib OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The MIB which allows managing the CPE"
       ::= { ictMgmt 1 }

ictFwUpg OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The MIB of firmware upgrade"
       ::= { ictMgmtMib 1 }

ictCfgUpdate OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The MIB of configuration update"
       ::= { ictMgmtMib 2 }

ictReboot OBJECT-IDENTITY
    STATUS current
    DESCRIPTION
    "The MIB responsible for CPE reboot"
       ::= { ictMgmtMib 3 }

--
-- Management subtree options --

upgUrl OBJECT-TYPE
  SYNTAX OCTET STRING  (SIZE(0..255))
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "MIB for firmware file path declaration."
    ::= { ictFwUpg 1 }

upgExecute OBJECT-TYPE
  SYNTAX INTEGER {
    notUpgrading(0),
    startUpgrade(1),
    validatingUpgrade-CheckErrorCodeIfFailed(2),
    someErrorOccured(3)
  }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "MIB for firmware upgrade execution."
    ::= { ictFwUpg 2 }

upgStatus OBJECT-TYPE
  SYNTAX OCTET STRING  (SIZE(0..255))
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "MIB used to check firmware upgrade status."
    ::= { ictFwUpg 3 }

cfgTftpPath OBJECT-TYPE
  SYNTAX OCTET STRING  (SIZE(0..255))
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "MIB for configuration file path stored at TFTP declaration."
    ::= { ictCfgUpdate 1 }

cfgExecute OBJECT-TYPE
  SYNTAX INTEGER {
    notUpdating(0),
    startUpdate(1),
    inProgress(2),
    someErrorOccured(3),
    resultOK(4)
  }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "MIB for configuration upload exectution."
    ::= { ictCfgUpdate 2 }

cfgStatus OBJECT-TYPE
  SYNTAX OCTET STRING  (SIZE(0..255))
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "MIB used to check configuration upload status."
    ::= { ictCfgUpdate 3 }

performCpeReboot OBJECT-TYPE
  SYNTAX INTEGER {
    noActionRequested(0),
    makeReboot(1),
    someErrorOccured(3)
  }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "MIB for CPE reboot execution."
  DEFVAL { 0 }
    ::= { ictReboot 2 }

-- END of MANAGEMENT part -- 
----------------------------

IctTimeStamp ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "The time as the number of seconds since the Epoch." 
    SYNTAX       Counter32

IctPortList ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            "Comma-separated list of LAN ports." 
    SYNTAX       OCTET STRING

IctJitter ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-2"
    STATUS      current
    DESCRIPTION
            "When used in conjunction with the DISPLAY-HINT will show jitter calculated for the last second.
             Without the DISPLAY-HINT the jitter value is multiplied by 100."
    SYNTAX       INTEGER

IctDelta ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-2"
    STATUS      current
    DESCRIPTION
            "Time period between two successive packets expressed in hundredths of a milliseconds.
             When used in conjunction with the DISPLAY-HINT will show milliseconds and fractions of millisecond." 
    SYNTAX       INTEGER

ictMcastAnalyzerCurrent   OBJECT IDENTIFIER ::= { ictMcastAnalyzer 1 }
ictMcastAnalyzerHistory   OBJECT IDENTIFIER ::= { ictMcastAnalyzer 2 }

CurrentListEntry ::=
    SEQUENCE {
        curGroupIndex            INTEGER,
        curGroupAddr             IpAddress    }

currentListEntry OBJECT-TYPE
    SYNTAX      CurrentListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry containing a particular multicast group address." 
    INDEX   { curGroupIndex }
    ::= { ictMcastAnalyzerCurrentList 1 }

ictMcastAnalyzerCurrentList OBJECT-TYPE
    SYNTAX      SEQUENCE OF CurrentListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of currently analyzed multicast groups." 
    ::= { ictMcastAnalyzerCurrent 1 }

curGroupIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Index of the analyzed multicast group." 
    ::= { currentListEntry 1 }

curGroupAddr OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The IPv4 address of this entry's multicast group." 
    ::= { currentListEntry 2 }

ictMcastAnalyzerCurrentMetrics OBJECT-TYPE
    SYNTAX      SEQUENCE OF CurrentMetricsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of currently analyzed multicast groups and their metrics." 
    ::= { ictMcastAnalyzerCurrent 2 }

currentMetricsEntry OBJECT-TYPE
    SYNTAX      CurrentMetricsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry containing metrics concerning a particular multicast group." 
    INDEX   { curMetrGroupAddr }
    ::= { ictMcastAnalyzerCurrentMetrics 1 }

CurrentMetricsEntry ::=
    SEQUENCE {
        curMetrGroupAddr             IpAddress,
        curMetrSourceAddr            IpAddress,
        curMetrDstPort               Integer32,
        curMetrSrcPort               Integer32,
        curMetrTotalBytes            Counter64,
        curMetrTotalPackets          Counter64,
        curMetrKbps                  Gauge32,
        curMetrPps                   Gauge32,
        curMetrAvgKbps               Gauge32,
        curMetrAvgPps                Gauge32,
        curMetrMaxDelta              IctDelta,
        curMetrAvgDelta              IctDelta,
        curMetrTotalMaxDelta         IctDelta,
        curMetrTotalAvgDelta         IctDelta,
        curMetrStartTimestamp        IctTimeStamp,
        curMetrStopTimestamp         IctTimeStamp,
        curMetrMemberPorts           IctPortList,
        curMetrStreamType            OCTET STRING,
        curMetrSkips                 Counter32,
        curMetrDiscontinuities       Counter32,
        curMetrLost                  Counter32,
        curMetrReordered             Counter32,
        curMetrTotalSkips            Counter32,
        curMetrTotalDiscontinuities  Counter32,
        curMetrTotalLost             Counter32,
        curMetrTotalReordered        Counter32,
        curMetrAvgLostPps            Gauge32,
        curMetrJitter                IctJitter
    }

curMetrGroupAddr OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The IPv4 address of this entry's multicast group." 
    ::= { currentMetricsEntry 1 }

curMetrSourceAddr OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The source IPv4 address of this multicast stream." 
    ::= { currentMetricsEntry 2 }

curMetrDstPort OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The destination port number of this multicast stream." 
    ::= { currentMetricsEntry 3 }

curMetrSrcPort OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The source port number of this multicast stream." 
    ::= { currentMetricsEntry 4 }

curMetrTotalBytes OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of bytes transferred within the stream." 
    ::= { currentMetricsEntry 5 }

curMetrTotalPackets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets transferred within the stream." 
    ::= { currentMetricsEntry 6 }

curMetrKbps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Kilobits per second during last second." 
    ::= { currentMetricsEntry 7 }

curMetrPps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Packets per second during last second." 
    ::= { currentMetricsEntry 8 }

curMetrAvgKbps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Average kilobits per second." 
    ::= { currentMetricsEntry 9 }

curMetrAvgPps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Average packets per second." 
    ::= { currentMetricsEntry 10 }

curMetrMaxDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Maximum time period between two successive packets from the last second." 
    ::= { currentMetricsEntry 11 }

curMetrAvgDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Average time period between two successive packets from the last second." 
    ::= { currentMetricsEntry 12 }

curMetrTotalMaxDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Maximum time period between two successive packets." 
    ::= { currentMetricsEntry 13 }

curMetrTotalAvgDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Average time period between two successive packets." 
    ::= { currentMetricsEntry 14 }

curMetrStartTimestamp OBJECT-TYPE
    SYNTAX      IctTimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The time at which the stream started being analyzed." 
    ::= { currentMetricsEntry 15 }

curMetrStopTimestamp OBJECT-TYPE
    SYNTAX      IctTimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The time at which the stream stopped being analyzed." 
    ::= { currentMetricsEntry 16 }

curMetrMemberPorts OBJECT-TYPE
    SYNTAX      IctPortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "LAN ports being members of the multicast group." 
    ::= { currentMetricsEntry 17 }

curMetrStreamType OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Type of the stream: either RTP or UDP." 
    ::= { currentMetricsEntry 18 }

curMetrSkips OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of skipped MPG-TS packets during last second." 
    ::= { currentMetricsEntry 19 }

curMetrDiscontinuities OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of MPG-TS discontinuities during last second." 
    ::= { currentMetricsEntry 20 }

curMetrLost OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of lost RTP packets during last second." 
    ::= { currentMetricsEntry 21 }

curMetrReordered OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of reordered RTP packets during last second." 
    ::= { currentMetricsEntry 22 }

curMetrTotalSkips OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of skipped MPG-TS packets." 
    ::= { currentMetricsEntry 23 }

curMetrTotalDiscontinuities OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of MPG-TS discontinuities." 
    ::= { currentMetricsEntry 24 }

curMetrTotalLost OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of lost RTP packets." 
    ::= { currentMetricsEntry 25 }

curMetrTotalReordered OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of reordered RTP packets." 
    ::= { currentMetricsEntry 26 }

curMetrAvgLostPps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Average number of lost RTP packets per second." 
    ::= { currentMetricsEntry 27 }

curMetrJitter OBJECT-TYPE
    SYNTAX     IctJitter
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Jitter calculated for the last second." 
    ::= { currentMetricsEntry 28 }

HistoryListEntry ::=
    SEQUENCE {
        histGroupIndex            INTEGER,
        histGroupAddr             IpAddress }

historyListEntry OBJECT-TYPE
    SYNTAX      HistoryListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry containing a particular multicast group address." 
    INDEX   { histGroupIndex }
    ::= { ictMcastAnalyzerHistoryList 1 }

ictMcastAnalyzerHistoryList OBJECT-TYPE
    SYNTAX      SEQUENCE OF HistoryListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of formerly analyzed multicast groups." 
    ::= { ictMcastAnalyzerHistory 1 }

histGroupIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Index of the historical multicast group." 
    ::= { historyListEntry 1 }

histGroupAddr OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The IPv4 address of this entry's multicast group." 
    ::= { historyListEntry 2 }

ictMcastAnalyzerHistoryMetrics OBJECT-TYPE
    SYNTAX      SEQUENCE OF HistoryMetricsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of formerly analyzed multicast groups and their metrics." 
    ::= { ictMcastAnalyzerHistory 2 }

historyMetricsEntry OBJECT-TYPE
    SYNTAX      HistoryMetricsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry containing metrics concerning a particular multicast group." 
    INDEX   { histMetrGroupAddr }
    ::= { ictMcastAnalyzerHistoryMetrics 1 }

HistoryMetricsEntry ::=
    SEQUENCE {
        histMetrGroupAddr             IpAddress,
        histMetrSourceAddr            IpAddress,
        histMetrDstPort               Integer32,
        histMetrSrcPort               Integer32,
        histMetrTotalBytes            Counter64,
        histMetrTotalPackets          Counter64,
        histMetrKbps                  Gauge32,
        histMetrPps                   Gauge32,
        histMetrAvgKbps               Gauge32,
        histMetrAvgPps                Gauge32,
        histMetrMaxDelta              IctDelta,
        histMetrAvgDelta              IctDelta,
        histMetrTotalMaxDelta         IctDelta,
        histMetrTotalAvgDelta         IctDelta,
        histMetrStartTimestamp        IctTimeStamp,
        histMetrStopTimestamp         IctTimeStamp,
        histMetrMemberPorts           IctPortList,
        histMetrStreamType            OCTET STRING,
        histMetrSkips                 Counter32,
        histMetrDiscontinuities       Counter32,
        histMetrLost                  Counter32,
        histMetrReordered             Counter32,
        histMetrTotalSkips            Counter32,
        histMetrTotalDiscontinuities  Counter32,
        histMetrTotalLost             Counter32,
        histMetrTotalReordered        Counter32,
        histMetrAvgLostPps            Gauge32,
        histMetrJitter                IctJitter
    }

histMetrGroupAddr OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The IPv4 address of this entry's multicast group." 
    ::= { historyMetricsEntry 1 }

histMetrSourceAddr OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The source IPv4 address of this multicast stream." 
    ::= { historyMetricsEntry 2 }

histMetrDstPort OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The destination port number of this multicast stream." 
    ::= { historyMetricsEntry 3 }

histMetrSrcPort OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The source port number of this multicast stream." 
    ::= { historyMetricsEntry 4 }

histMetrTotalBytes OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of bytes transferred within the stream." 
    ::= { historyMetricsEntry 5 }

histMetrTotalPackets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets transferred within the stream." 
    ::= { historyMetricsEntry 6 }

histMetrKbps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Kilobits per second during last second." 
    ::= { historyMetricsEntry 7 }

histMetrPps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Packets per second during last second." 
    ::= { historyMetricsEntry 8 }

histMetrAvgKbps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Average kilobits per second." 
    ::= { historyMetricsEntry 9 }

histMetrAvgPps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Average packets per second." 
    ::= { historyMetricsEntry 10 }

histMetrMaxDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Maximum time period between two successive packets from the last second." 
    ::= { historyMetricsEntry 11 }

histMetrAvgDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Average time period between two successive packets from the last second." 
    ::= { historyMetricsEntry 12 }

histMetrTotalMaxDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Maximum time period between two successive packets." 
    ::= { historyMetricsEntry 13 }

histMetrTotalAvgDelta OBJECT-TYPE
    SYNTAX     IctDelta
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Average time period between two successive packets." 
    ::= { historyMetricsEntry 14 }

histMetrStartTimestamp OBJECT-TYPE
    SYNTAX      IctTimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The time at which the stream started being analyzed." 
    ::= { historyMetricsEntry 15 }

histMetrStopTimestamp OBJECT-TYPE
    SYNTAX      IctTimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The time at which the stream stopped being analyzed." 
    ::= { historyMetricsEntry 16 }

histMetrMemberPorts OBJECT-TYPE
    SYNTAX      IctPortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "LAN ports being members of the multicast group." 
    ::= { historyMetricsEntry 17 }

histMetrStreamType OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Type of the stream: either RTP or UDP." 
    ::= { historyMetricsEntry 18 }

histMetrSkips OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of skipped MPG-TS packets during last second." 
    ::= { historyMetricsEntry 19 }

histMetrDiscontinuities OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of MPG-TS discontinuities during last second." 
    ::= { historyMetricsEntry 20 }

histMetrLost OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of lost RTP packets during last second." 
    ::= { historyMetricsEntry 21 }

histMetrReordered OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of reordered RTP packets during last second." 
    ::= { historyMetricsEntry 22 }

histMetrTotalSkips OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of skipped MPG-TS packets." 
    ::= { historyMetricsEntry 23 }

histMetrTotalDiscontinuities OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of MPG-TS discontinuities." 
    ::= { historyMetricsEntry 24 }

histMetrTotalLost OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of lost RTP packets." 
    ::= { historyMetricsEntry 25 }

histMetrTotalReordered OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of reordered RTP packets." 
    ::= { historyMetricsEntry 26 }

histMetrAvgLostPps OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Average number of lost RTP packets per second." 
    ::= { historyMetricsEntry 27 }

histMetrJitter OBJECT-TYPE
    SYNTAX     IctJitter
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "Jitter calculated for the last second." 
    ::= { historyMetricsEntry 28 }

-- End of McastAnalyser part --
------------------------------- 

--
END

