  ALCATEL-IND1-OPENFLOW-MIB DEFINITIONS ::= BEGIN

      IMPORTS
          MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE,
          Integer32, Unsigned32, NOTIFICATION-TYPE
              FROM SNMPv2-SMI

          RowStatus
              FROM SNMPv2-TC

          MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
              FROM SNMPv2-CONF

          InetAddressType, InetAddress
              FROM INET-ADDRESS-MIB

          SnmpAdminString         FROM SNMP-FRAMEWORK-MIB

          softentIND1OpenflowMIB
              FROM ALCATEL-IND1-BASE
      ;


      alcatelIND1OpenflowMIB MODULE-IDENTITY
          LAST-UPDATED  "201403260000Z"
          ORGANIZATION  "Alcatel-Lucent"
          CONTACT-INFO
              "Please consult with Customer Service to ensure the most appropriate
               version of this document is used with the products in question:

                        Alcatel-Lucent, Enterprise Solutions Division
                      (Formerly Alcatel Internetworking, Incorporated)
                                 26801 West Agoura Road
                              Agoura Hills, CA  91301-5122
                                United States Of America

              Telephone:               North America  +1 800 995 2696
                                       Latin America  +1 877 919 9526
                                       Europe         +31 23 556 0100
                                       Asia           +65 394 7933
                                       All Other      +1 818 878 4507

              Electronic Mail:         support@ind.alcatel.com
              World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
              File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

          DESCRIPTION
              "This module describes an authoritative enterprise-specific Simple
               Network Management Protocol (SNMP) Management Information Base (MIB):

               Openflow for OS6900 Product Line.

               The right to make changes in specification and other information
               contained in this document without prior notice is reserved.

               No liability shall be assumed for any incidental, indirect, special, or
               consequential damages whatsoever arising from or related to this
               document or the information contained herein.

               Vendors, end-users, and other interested parties are granted
               non-exclusive license to use this specification in connection with
               management of the products for which it is intended to be used.

                           Copyright (C) 2013 Alcatel-Lucent
                               ALL RIGHTS RESERVED WORLDWIDE"

          REVISION      "201403260000Z"
          DESCRIPTION
              "The latest version of this MIB Module."

          REVISION      "201410080000Z"
          DESCRIPTION
              "alaOpenflowLogicalSwitchLearnedMacUpdate is not limited to OS6900 devices"
          ::= { softentIND1OpenflowMIB 1 }

  -- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
  -- Hook into the Alcatel Tree
  -- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

  alcatelIND1OpenflowMIBNotifications OBJECT IDENTIFIER ::= { alcatelIND1OpenflowMIB 0 }

  alcatelIND1OpenflowMIBObjects OBJECT-IDENTITY
         STATUS current
         DESCRIPTION
           " Alcatel-Lucent Openflow Managed Objects."
         ::= { alcatelIND1OpenflowMIB 1 }

  alcatelIND1OpenflowMIBConformance OBJECT-IDENTITY
       STATUS current
       DESCRIPTION
                  " Alcatel-Lucent Openflow Conformance Information."
       ::= { alcatelIND1OpenflowMIB 2 }


  alaOpenflowGlobalConfigObjects OBJECT IDENTIFIER ::= { alcatelIND1OpenflowMIBObjects 1 }

  alaOpenflowGlobalBackoffMax OBJECT-TYPE
       SYNTAX  Integer32 (1..60)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
          " Alcatel-Lucent Openflow maximum back-off time in seconds for controller connection attempts."
       DEFVAL { 60 }
       ::= { alaOpenflowGlobalConfigObjects 1 }

  alaOpenflowGlobalIdleProbeTimeout OBJECT-TYPE
       SYNTAX  Integer32 (0..60)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
          " Alcatel-Lucent Openflow idle probe timeout value in seconds. If set to 0, idle probing is disabled."
       DEFVAL { 15 }
       ::= { alaOpenflowGlobalConfigObjects 2 }

  -- Openflow LogicalSwitch Table

  alaOpenflowLogicalSwitchTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AlaOpenflowLogicalSwitchEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains one row for each Logical Switch."
    ::= { alcatelIND1OpenflowMIBObjects 2 }

  alaOpenflowLogicalSwitchEntry OBJECT-TYPE
            SYNTAX AlaOpenflowLogicalSwitchEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
              "Information about the Openflow Logical Switches. "
            INDEX { alaOpenflowLogicalSwitch }
    ::= { alaOpenflowLogicalSwitchTable 1 }

  AlaOpenflowLogicalSwitchEntry ::= SEQUENCE
         {
             alaOpenflowLogicalSwitch                 SnmpAdminString,
             alaOpenflowLogicalSwitchAdminState       INTEGER,
             alaOpenflowLogicalSwitchMode             INTEGER,
             alaOpenflowLogicalSwitchVersions         BITS,
             alaOpenflowLogicalSwitchVlan             Integer32,
             alaOpenflowLogicalSwitchControllerCount  Integer32,
             alaOpenflowLogicalSwitchInterfaceCount   Integer32,
             alaOpenflowLogicalSwitchFlowCount        Integer32,
             alaOpenflowLogicalSwitchRowStatus        RowStatus,
             alaOpenflowLogicalSwitchLearnedMacUpdate INTEGER,
             alaOpenflowLogicalSwitchProbeTime 	      Integer32,
             alaOpenflowLogicalSwitchFailureDetectTime Integer32,
             alaOpenflowLogicalSwitchDPID 	      OCTET STRING,

             alaOpenflowLogicalSwitchTableMissAction  INTEGER,
             alaOpenflowLogicalSwitchTCPBufferSizeTx  Unsigned32,
             alaOpenflowLogicalSwitchTCPBufferSizeRx  Unsigned32
         }

  alaOpenflowLogicalSwitch OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(1..31))
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "Openflow Logical Switch Name."
        ::= { alaOpenflowLogicalSwitchEntry 1 }

  alaOpenflowLogicalSwitchAdminState OBJECT-TYPE
        SYNTAX INTEGER {
             enabled(1),
             disabled(2)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "Logical Switch Admin State. Enable or disable the Logical Switch.
          When disabled, all controllers for the Logical Switch will be
          operationally disabled and flows added by those controllers will
          be removed."
        DEFVAL { enabled }
        ::= { alaOpenflowLogicalSwitchEntry 2 }

  alaOpenflowLogicalSwitchMode OBJECT-TYPE
        SYNTAX INTEGER {
             normal(1),
             api(2),
             pfcChannel(3)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "Openflow Logical Switch Mode. Normal is regular Openflow,
         API is for ACL-like flow operation. Only one Logical Switch
         can be in api mode at a time. 
	 PFC-Channel mode is to indicate the Logical Switch 
	 is operating in NEC mode.

	 This object cannot be modified after the Logical Switch has been created."
         DEFVAL { normal }
        ::= { alaOpenflowLogicalSwitchEntry 3 }

  alaOpenflowLogicalSwitchVersions OBJECT-TYPE
        SYNTAX BITS {
             v1dot0 (0),
             v1dot3dot1 (1)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "Openflow Logical Switch Bitmap of enabled Openflow versions.
         At least one version must be enabled."
        DEFVAL { { v1dot0, v1dot3dot1 } }
        ::= { alaOpenflowLogicalSwitchEntry 4 }

  alaOpenflowLogicalSwitchVlan OBJECT-TYPE
       SYNTAX  Integer32 (0|2..4093)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
          "Openflow Logical Switch VLAN. The value 0 indicates that no
          VLAN has been specified, it is not a valid value to write.
          This object is not valid to write when creating/modifying an
          entry with alaOpenflowLogicalSwitchMode api(2)"
       DEFVAL { 0 }
       ::= { alaOpenflowLogicalSwitchEntry 5 }

  alaOpenflowLogicalSwitchControllerCount OBJECT-TYPE
       SYNTAX  Integer32 (0..3)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
          "Count of the configured controllers for the Logical Switch."
       ::= { alaOpenflowLogicalSwitchEntry 6 }

  alaOpenflowLogicalSwitchInterfaceCount OBJECT-TYPE
       SYNTAX  Integer32 (0..5000)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
          "Count of the configured interfaces (ports and link aggregations) for the Logical Switch."
       ::= { alaOpenflowLogicalSwitchEntry 7 }

  alaOpenflowLogicalSwitchFlowCount OBJECT-TYPE
       SYNTAX  Integer32 (0..511)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
          "Count of the flows pushed to the Logical Switch by its controllers."
       ::= { alaOpenflowLogicalSwitchEntry 8 }

  alaOpenflowLogicalSwitchRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS     current
        DESCRIPTION
         "Deleting a row from this table will also remove associated entries from other tables in this mib
         that have a logical switch as part of their index."
        ::= { alaOpenflowLogicalSwitchEntry 9 }

  alaOpenflowLogicalSwitchLearnedMacUpdate OBJECT-TYPE
        SYNTAX INTEGER {
             enabled(1),
             disabled(2)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "This object is only applicable to Logical Switches in api(2) mode.
          When enabled(1), learned MACs will be forwarded to controllers
          via a Packet-In message."
        DEFVAL { disabled }
        ::= { alaOpenflowLogicalSwitchEntry 10 }

  alaOpenflowLogicalSwitchProbeTime OBJECT-TYPE
       SYNTAX  	  	Integer32 (1..60)
       MAX-ACCESS	read-create
       STATUS 	  	current
       DESCRIPTION
          "Probe-time for a logical switch in the pfc-channel mode in seconds,
	  which will override the existing global idle-probe-time for sending 
	  echo-request to the OpenFlow Controller."
       DEFVAL { 5 }
       ::= { alaOpenflowLogicalSwitchEntry 11 }

  alaOpenflowLogicalSwitchFailureDetectTime OBJECT-TYPE
       SYNTAX  		Integer32 (1..60)
       MAX-ACCESS 	read-create
       STATUS 		current
       DESCRIPTION
          "Failure detect time, in seconds, is configured for a logical switch 
	  in the pfc-channel mode for detecting disconnection to the 
	  OpenFlow Controller if there was no echo reply or message from the controller."
       DEFVAL { 4 }
       ::= { alaOpenflowLogicalSwitchEntry 12 }

  alaOpenflowLogicalSwitchDPID OBJECT-TYPE
       SYNTAX           OCTET STRING (SIZE (8))
       MAX-ACCESS 	read-create
       STATUS 		current
       DESCRIPTION
          "An unique 8 bytes DPID for a logical switch."
       ::= { alaOpenflowLogicalSwitchEntry 13 }

  alaOpenflowLogicalSwitchTableMissAction OBJECT-TYPE
        SYNTAX INTEGER {
             drop(1),
             controller(2)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "The action to be taken when an Openflow Table Miss occurs. When set to drop 
	  if any packet has a table miss, it will be dropped. If set to controller
	  it will be forwarded to the controller."        
        DEFVAL { drop }
        ::= { alaOpenflowLogicalSwitchEntry 14 }

  alaOpenflowLogicalSwitchTCPBufferSizeTx OBJECT-TYPE
       SYNTAX  Unsigned32 (2..32)
       UNITS   "Kilo Bytes"
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
          "TCP send buffer size, in Kilo Bytes, for socket connection to OpenFlow controllers 
       in the logical switch."
       DEFVAL { 2 }
       ::= { alaOpenflowLogicalSwitchEntry 15 }

  alaOpenflowLogicalSwitchTCPBufferSizeRx OBJECT-TYPE
       SYNTAX  Unsigned32 (2..32)
       UNITS   "Kilo Bytes"
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
          "TCP receive buffer size, in Kilo Bytes, for socket connection to OpenFlow controllers 
       in the logical switch."
       DEFVAL { 2 }
       ::= { alaOpenflowLogicalSwitchEntry 16 }

  -- Openflow Controller Table

  alaOpenflowControllerTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AlaOpenflowControllerEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains one row for each controller on each logical switch.
           Currently, up to three controllers per logical switch are supported per logical switch."
    ::= { alcatelIND1OpenflowMIBObjects 3 }

  alaOpenflowControllerEntry OBJECT-TYPE
            SYNTAX AlaOpenflowControllerEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
              "Information about the Openflow Controllers attached to Logical Switches. "
            INDEX { alaOpenflowControllerLogicalSwitch, alaOpenflowControllerIpType, alaOpenflowControllerIp, alaOpenflowControllerPort }
    ::= { alaOpenflowControllerTable 1 }

  AlaOpenflowControllerEntry ::= SEQUENCE
         {
             alaOpenflowControllerLogicalSwitch   SnmpAdminString,
             alaOpenflowControllerIpType          InetAddressType,
             alaOpenflowControllerIp              InetAddress,
             alaOpenflowControllerPort            Integer32,
             alaOpenflowControllerRole            INTEGER,
             alaOpenflowControllerAdminState      INTEGER,
             alaOpenflowControllerOperState       INTEGER,
             alaOpenflowControllerRowStatus       RowStatus,
             alaOpenflowControllerPriority        Integer32
         }

  alaOpenflowControllerLogicalSwitch OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(1..31))
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "Openflow Logical Switch Name."
        ::= { alaOpenflowControllerEntry 1 }

  alaOpenflowControllerIpType OBJECT-TYPE
        SYNTAX      InetAddressType(1)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "Openflow Controller IP Address Type. The only type currently supported is ipv4(1)"
        ::= { alaOpenflowControllerEntry 2 }

  alaOpenflowControllerIp OBJECT-TYPE
        SYNTAX      InetAddress(SIZE (4|16))
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "Openflow Controller IP Address. As specified by alaOpenflowControllerIpType,
         only ipv4 is currently supported"
        ::= { alaOpenflowControllerEntry 3 }

  alaOpenflowControllerPort OBJECT-TYPE
        SYNTAX  Integer32 (1..65535)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "Openflow Controller Port."
        ::= { alaOpenflowControllerEntry 4 }

  alaOpenflowControllerRole OBJECT-TYPE
        SYNTAX INTEGER {
             equal(1),
             master(2),
             slave(3)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
         "Role of the Controller for the Logical Switch. The role is negotiated by the
         controllers and the switch is notified of the outcome (1.3.1+). 1.0 controllers
         will always have the role of equal. Only one controller per Logical Switch
         can have the role of master."
        ::= { alaOpenflowControllerEntry 5 }

  alaOpenflowControllerAdminState OBJECT-TYPE
        SYNTAX INTEGER {
             enabled(1),
             disabled(2)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "Controller Admin State. Enable or disable connection to the controller.
          The Logical Switch runs in 'Fail Secure Mode' so all flow aging, etc
          continues unaffected when the controller is administratively disabled."
        DEFVAL { enabled }
        ::= { alaOpenflowControllerEntry 6 }

  alaOpenflowControllerOperState OBJECT-TYPE
        SYNTAX INTEGER {
             invalid(1),
             disabled(2),
             sendError(3),
             init(4),
             connecting(5),
             backoff(6),
             exchangingHello(7),
             active(8),
             idle(9),
             disconnected(10)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
         "State of the Logical Switch connection to the Controller."
        ::= { alaOpenflowControllerEntry 7 }

  alaOpenflowControllerRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS     current
        DESCRIPTION
         "On create, if the specified logical switch does not exist in alaOpenflowLogicalSwitchTable,
          an entry will be created in that table. Delete does not effect alaOpenflowLogicalSwitchTable."
        ::= { alaOpenflowControllerEntry 8 }

  alaOpenflowControllerPriority OBJECT-TYPE
        SYNTAX		Integer32(0..2)
        MAX-ACCESS 	read-create 
        STATUS      	current
        DESCRIPTION
         "Openflow Controller Priority. Priority value of 0 implies highest pririoty and 2 implies lowest."
        DEFVAL { 2 }
        ::= { alaOpenflowControllerEntry 9 }

  -- Openflow Interface Table

  alaOpenflowInterfaceTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AlaOpenflowInterfaceEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains one row for each interface (port or link aggregation) assigned to
           a logical switch. An interface can only belong to one logical switch at a time.
           If a logical switch in API mode exists, interfaces cannot be manually added to/deleted from it;
           instead, interfaces default to the API mode logical switch when not assigned to another Logical Switch.
           Interfaces can be reassigned from the API mode logical switch to a normal mode logical switch
           (by adding it to that normal mode logical switch) but not directly reassigned from one normal mode
           logical switch to another normal mode logical switch."
    ::= { alcatelIND1OpenflowMIBObjects 4 }

  alaOpenflowInterfaceEntry OBJECT-TYPE
            SYNTAX AlaOpenflowInterfaceEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
              "Information about the interfaces assigned to Openflow Logical Switches."
            INDEX { alaOpenflowInterfaceLogicalSwitch, alaOpenflowInterface }
    ::= { alaOpenflowInterfaceTable 1 }

  AlaOpenflowInterfaceEntry ::= SEQUENCE
         {
             alaOpenflowInterfaceLogicalSwitch   SnmpAdminString,
             alaOpenflowInterface                Integer32,
             alaOpenflowInterfaceMode            INTEGER,
             alaOpenflowInterfaceRowStatus       RowStatus,
             alaOpenflowInterfaceType 		 INTEGER,
             alaOpenflowInterfaceNativeVlan      Unsigned32
         }

  alaOpenflowInterfaceLogicalSwitch OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(1..31))
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "Openflow Logical Switch Name."
        ::= { alaOpenflowInterfaceEntry 1 }

  alaOpenflowInterface OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "Openflow Interface attached to a Logical Switch. Port values are dot1dBasePort values,
         Link Aggregations start at 32769."
        ::= { alaOpenflowInterfaceEntry 2 }

  alaOpenflowInterfaceMode OBJECT-TYPE
        SYNTAX INTEGER {
             normal(1),
             api(2),
             pfcChannel(3)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
         "Openflow Interface Mode. Normal is regular Openflow,
         API is for ACL like flow operation and PFC-Channel is for NEC OFC."
        ::= { alaOpenflowInterfaceEntry 3 }

  alaOpenflowInterfaceRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS     current
        DESCRIPTION
         "On create, if the specified logical switch does not exist in alaOpenflowLogicalSwitchTable,
          an entry will be created in that table. Delete does not effect alaOpenflowLogicalSwitchTable."
        ::= { alaOpenflowInterfaceEntry 4 }

  alaOpenflowInterfaceType OBJECT-TYPE
        SYNTAX INTEGER {
             trunk (1),
             access (2)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "Openflow Interface Type."
        ::= { alaOpenflowInterfaceEntry 5 }

  alaOpenflowInterfaceNativeVlan OBJECT-TYPE
        SYNTAX 	    Unsigned32 (2..4093)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "Native VLAN for Openflow Interface."
        ::= { alaOpenflowInterfaceEntry 6 }

  -- Openflow Interface VLAN Table

  alaOpenflowInterfaceVlanTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AlaOpenflowInterfaceVlanEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains a list of Tag VLANs for an OpenFlow Interface (port or link-aggregation) Entry.
           logical switch belongs to."
    ::= { alcatelIND1OpenflowMIBObjects 5 }

  alaOpenflowInterfaceVlanEntry OBJECT-TYPE
            SYNTAX AlaOpenflowInterfaceVlanEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
              "Information about the Tag VLANs associated with an OpenFlow Interface."
            INDEX { alaOpenflowInterfaceLogicalSwitch, alaOpenflowInterface, alaOpenflowInterfaceVlanVlanID }
    ::= { alaOpenflowInterfaceVlanTable 1 }

  AlaOpenflowInterfaceVlanEntry ::= SEQUENCE
         {
             alaOpenflowInterfaceVlanVlanID	Unsigned32,
             alaOpenflowInterfaceVlanRowStatus	RowStatus
         }

  alaOpenflowInterfaceVlanVlanID OBJECT-TYPE
        SYNTAX		    Unsigned32 (0|2..4093)
        MAX-ACCESS  	not-accessible 
        STATUS      	current
        DESCRIPTION
         "Tag VLAN for an Openflow Interface."
        DEFVAL { 0 }
        ::= { alaOpenflowInterfaceVlanEntry 1 }

  alaOpenflowInterfaceVlanRowStatus OBJECT-TYPE
        SYNTAX 		RowStatus
        MAX-ACCESS 	read-create
        STATUS     	current
        DESCRIPTION
         "On create, the specified logical switch interface must exist in alaOpenflowInterfaceTable,
          otherwise an entry creation in this table would not be allowed. Deletion of an interface entry in 
          alaOpenflowInterfaceTable would result in deletion of all entries for that interface in the
          alaOpenflowInterfaceVlanEntry"
        ::= { alaOpenflowInterfaceVlanEntry 2 }

   -- Openflow MIB Conformance and Compliances

  alcatelIND1OpenflowMIBGroups OBJECT-IDENTITY
       STATUS current
       DESCRIPTION
          "Branch For ALU Openflow MIB Subsystem Units Of Conformance."
       ::= { alcatelIND1OpenflowMIBConformance 1 }

  alcatelIND1OpenflowMIBCompliances OBJECT-IDENTITY
       STATUS current
       DESCRIPTION
          "Branch For ALU Openflow MIB Subsystem Compliance Statements."
       ::= { alcatelIND1OpenflowMIBConformance 2 }


  alaOpenflowMIBCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
          "Compliance statement for Openflow."
       MODULE -- This module
           MANDATORY-GROUPS
           {
               alaOpenflowModuleConfigGroup,
               alaOpenflowModuleLogicalSwitchGroup,
               alaOpenflowModuleControllerGroup,
               alaOpenflowModuleInterfaceGroup,
               alaOpenflowModuleInterfaceVlanGroup
           }
       ::= { alcatelIND1OpenflowMIBCompliances 1 }

  alaOpenflowModuleConfigGroup OBJECT-GROUP
       OBJECTS
       {
         alaOpenflowGlobalBackoffMax,
         alaOpenflowGlobalIdleProbeTimeout
       }
       STATUS  current
       DESCRIPTION
          "Openflow Global Configuration Modules Group."
       ::= { alcatelIND1OpenflowMIBGroups 1 }


  alaOpenflowModuleLogicalSwitchGroup OBJECT-GROUP
       OBJECTS
       {
           alaOpenflowLogicalSwitchAdminState,
           alaOpenflowLogicalSwitchMode,
           alaOpenflowLogicalSwitchVersions,
           alaOpenflowLogicalSwitchVlan,
           alaOpenflowLogicalSwitchControllerCount,
           alaOpenflowLogicalSwitchInterfaceCount,
           alaOpenflowLogicalSwitchFlowCount,
           alaOpenflowLogicalSwitchRowStatus,
           alaOpenflowLogicalSwitchLearnedMacUpdate,
           alaOpenflowLogicalSwitchProbeTime,
           alaOpenflowLogicalSwitchFailureDetectTime,
           alaOpenflowLogicalSwitchDPID,
           alaOpenflowLogicalSwitchTableMissAction,
           alaOpenflowLogicalSwitchTCPBufferSizeTx,
           alaOpenflowLogicalSwitchTCPBufferSizeRx
       }
       STATUS  current
       DESCRIPTION
          "Openflow Logical Switch Configuration Modules Group."
       ::= { alcatelIND1OpenflowMIBGroups 2 }

  alaOpenflowModuleControllerGroup OBJECT-GROUP
       OBJECTS
       {
           alaOpenflowControllerRole,
           alaOpenflowControllerAdminState,
           alaOpenflowControllerOperState,
           alaOpenflowControllerRowStatus,
           alaOpenflowControllerPriority
       }
       STATUS  current
       DESCRIPTION
          "Openflow Controller Configuration Modules Group."
       ::= { alcatelIND1OpenflowMIBGroups 3 }

  alaOpenflowModuleInterfaceGroup OBJECT-GROUP
       OBJECTS
       {
           alaOpenflowInterfaceMode,
           alaOpenflowInterfaceRowStatus,
           alaOpenflowInterfaceType,
           alaOpenflowInterfaceNativeVlan
       }
       STATUS  current
       DESCRIPTION
          "Openflow Interface Configuration Modules Group."
       ::= { alcatelIND1OpenflowMIBGroups 4 }

  alaOpenflowModuleInterfaceVlanGroup OBJECT-GROUP
       OBJECTS
       {
           alaOpenflowInterfaceVlanRowStatus
       }
       STATUS  current
       DESCRIPTION
          "Openflow Interface with VLAN Configuration Modules Group."
       ::= { alcatelIND1OpenflowMIBGroups 5 }

  END
