
-- File Name : MwrRadio-MC-MIB.mib
-- Version   : 1.0.0
-- Date      : October 6, 2014
-- Author    : DragonWave Inc.

MWR-RADIO-MC-MIB DEFINITIONS ::= BEGIN

IMPORTS
	MODULE-IDENTITY, NOTIFICATION-TYPE, OBJECT-TYPE, 
	Counter32, Counter64, Integer32
		FROM SNMPv2-SMI
	DisplayString
		FROM SNMPv2-TC
	mwr
		FROM DWI-HARMONY-PRIVATE-MIB
	equipmentTrapInfo, equipmentOutTrapsCounter, equipmentAlarmActiveConditionId, EnableType
		FROM EQUIPMENT-COMMON-MIB
	mwrEventConfigSeverity, RadioInstanceType
		FROM MWR-ETHERNET-MIB;

mwrRadioMcModIdentity MODULE-IDENTITY
	LAST-UPDATED "201406101023Z"
	ORGANIZATION 
		"Dragonwave Inc."
	CONTACT-INFO 
		"http://www.dragonwaveinc.com
		600-411 Legget Drive
		Ottawa, Ontario
		Canada, K2K 3C9
		
		Tel : 613-599-9991
		Fax: 613-599-4265
		Support: 613-271-7010"
	DESCRIPTION 
		"This specifies the contact information and the revision tracking information for the MIB module version."

	REVISION "201406231109Z"
	DESCRIPTION 
		"First release of the Dragonwave Harmony radio Enhanced-multicarrier MIB."

	REVISION "201409231722Z"
	DESCRIPTION 
		"Updated some OIDs Descriptions."
::= { mwr 1003 }

mwrRadio             OBJECT IDENTIFIER ::= { mwr 12 }
mwrEmcRadioConfigurations  OBJECT IDENTIFIER ::= { mwrRadio 201 }
mwrEmcRadioStatus    OBJECT IDENTIFIER ::= { mwrRadio 202 }
mwrEmcRadioPerformance  OBJECT IDENTIFIER ::= { mwrRadio 203 }
mwrEmcRadioNotifications  OBJECT IDENTIFIER ::= { mwrRadio 204 }

mwrEmcRadioConfigurationsTable  OBJECT-TYPE
	SYNTAX SEQUENCE OF MwrEmcRadioConfigurationsEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table containing radio configurations."
	::= { mwrEmcRadioConfigurations 1 }

mwrEmcRadioConfigurationsEntry  OBJECT-TYPE
	SYNTAX 	MwrEmcRadioConfigurationsEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table entry containing radio channel configurations."
	INDEX { mwrEmcRadioConfigIndex }
	::= { mwrEmcRadioConfigurationsTable 1 }

MwrEmcRadioConfigurationsEntry ::= SEQUENCE {
	mwrEmcRadioConfigIndex
		RadioInstanceType,
	mwrEmcRadioTxState
		EnableType,
	mwrEmcRadioTxPower
		Integer32,
	mwrEmcRadioTxDownTime
		Integer32,
	mwrEmcRadioRxFrequency
		Integer32,
	mwrEmcRadioTxFrequency
		Integer32
}

mwrEmcRadioConfigIndex  OBJECT-TYPE
	SYNTAX     RadioInstanceType
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"A unique value for each radio channel if applicable."
	::= { mwrEmcRadioConfigurationsEntry 1 }

mwrEmcRadioTxState  OBJECT-TYPE
	SYNTAX     EnableType
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"Represents the transmit state of the radio channel."
	::= { mwrEmcRadioConfigurationsEntry 2 }

mwrEmcRadioTxPower  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"dB"
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"This defines the programmed transmit level of the radio channel.
		The power you see is divided by 10. e.g. A display of 133 is actually 13.3 dB.
		Notes: 
		- Programmed and Actual transmit power may differ - see mwrEmcRadioActualTxPower."
	::= { mwrEmcRadioConfigurationsEntry 3 }

mwrEmcRadioTxDownTime  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"sec"
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"The amount of time in seconds the radio transmitter is disabled when the mwrEmcRadioTxState is turned off. 
		- Make sure this is set before the mwrEmcRadioTxState is disabled.
		- If the down time is set to 0, the radio will stay disabled until it is re-enabled again."
	::= { mwrEmcRadioConfigurationsEntry 4 }

mwrEmcRadioRxFrequency  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"kHz"
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"Represents the receive Radio frequency in kHz."
	::= { mwrEmcRadioConfigurationsEntry 5 }

mwrEmcRadioTxFrequency  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"kHz"
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"Represents the transmit Radio frequency in kHz."
	::= { mwrEmcRadioConfigurationsEntry 6 }

mwrEmcRadioProfileTable  OBJECT-TYPE
	SYNTAX SEQUENCE OF MwrEmcRadioProfileEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table containing the radio profile configurations."
	::= { mwrEmcRadioConfigurations 2 }

mwrEmcRadioProfileEntry  OBJECT-TYPE
	SYNTAX 	MwrEmcRadioProfileEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table entry containing the radio profile configurations."
	INDEX { mwrEmcRadioStandardMode, 
		mwrEmcRadioChannelBw, 
		mwrEmcRadioStaticTxProfile }
	::= { mwrEmcRadioProfileTable 1 }

MwrEmcRadioProfileEntry ::= SEQUENCE {
	mwrEmcRadioStandardMode
		DisplayString,
	mwrEmcRadioChannelBw
		DisplayString,
	mwrEmcRadioStaticTxProfile
		DisplayString,
	mwrEmcRadioProgrammedProfile
		EnableType
}

mwrEmcRadioStandardMode  OBJECT-TYPE
	SYNTAX     DisplayString
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"An index representing the available standard mode of the radio channel."
	::= { mwrEmcRadioProfileEntry 1 }

mwrEmcRadioChannelBw  OBJECT-TYPE
	SYNTAX     DisplayString
	UNITS 	"MHz"
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"An index representing the available channel bandwidth of the radio channel."
	::= { mwrEmcRadioProfileEntry 2 }

mwrEmcRadioStaticTxProfile  OBJECT-TYPE
	SYNTAX     DisplayString
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"An index representing the available static tx profile of the radio channel."
	::= { mwrEmcRadioProfileEntry 3 }

mwrEmcRadioProgrammedProfile  OBJECT-TYPE
	SYNTAX     EnableType
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"Represents the configured standard mode, channel BW and the TX profile of the radio channel."
	::= { mwrEmcRadioProfileEntry 4 }

mwrEmcRadioThresholdAlarmTable  OBJECT-TYPE
	SYNTAX SEQUENCE OF MwrEmcRadioThresholdAlarmEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table containing the threshold alarm configurations of the radio channel."
	::= { mwrEmcRadioConfigurations 3 }

mwrEmcRadioThresholdAlarmEntry  OBJECT-TYPE
	SYNTAX 	MwrEmcRadioThresholdAlarmEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table entry containing the threshold alarm configurations of the radio channel."
	INDEX { mwrEmcRadioThresholdIndex }
	::= { mwrEmcRadioThresholdAlarmTable 1 }

MwrEmcRadioThresholdAlarmEntry ::= SEQUENCE {
	mwrEmcRadioThresholdIndex
		RadioInstanceType,
	mwrEmcRadioRslBelowThresholdParams
		DisplayString,
	mwrEmcRadioTxAboveThresholdParams
		DisplayString
}

mwrEmcRadioThresholdIndex  OBJECT-TYPE
	SYNTAX     RadioInstanceType
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"A unique value for each radio channel if applicable."
	::= { mwrEmcRadioThresholdAlarmEntry 1 }

mwrEmcRadioRslBelowThresholdParams  OBJECT-TYPE
	SYNTAX     DisplayString
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"Represents the RSL threshold in dB and the number of seconds the RSL should be below the threshold. 
		 An example of the format of the string is as follows: '-75 10'. The first parameter power level in dB, the second is the time in seconds. In this example the threshold -75 dB and the time is set to 10 seconds. The single quote marks are not used in the command."
	::= { mwrEmcRadioThresholdAlarmEntry 2 }

mwrEmcRadioTxAboveThresholdParams  OBJECT-TYPE
	SYNTAX     DisplayString
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"Represents the radio transmit power threshold in dB and the number of seconds threshold must be exceeded. 
		 An example of the format of the string is as follows: '-75 10'. The first parameter power level in dB, the second is the time in seconds. In this example the threshold -75 dB and the time is set to 10 seconds. The single quote marks are not used in the command."
	::= { mwrEmcRadioThresholdAlarmEntry 3 }

mwrEmcRadioChCfgSynchEnable  OBJECT-TYPE
	SYNTAX     EnableType
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION 
		"This object enables or disables synchronization of the radio configuration on multiple carriers."
	::= { mwrEmcRadioConfigurations 4 }

-- 
-- RADIO INFORMATION
-- 

mwrEmcRadioStatusTable  OBJECT-TYPE
	SYNTAX SEQUENCE OF MwrEmcRadioStatusEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table containing the status of the radio channel."
	::= { mwrEmcRadioStatus 1 }

mwrEmcRadioStatusEntry  OBJECT-TYPE
	SYNTAX 	MwrEmcRadioStatusEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table entry containing the status of the radio channel."
	INDEX { mwrEmcRadioStatusIndex }
	::= { mwrEmcRadioStatusTable 1 }

MwrEmcRadioStatusEntry ::= SEQUENCE {
	mwrEmcRadioStatusIndex
		RadioInstanceType,
	mwrEmcRadioOperStatus
		INTEGER,
	mwrEmcRadioTRSpacing
		Integer32,
	mwrEmcRadioActualTxStatus
		EnableType,
	mwrEmcRadioRxFreqMin
		Integer32,
	mwrEmcRadioRxFreqMax
		Integer32,
	mwrEmcRadioTxFreqMin
		Integer32,
	mwrEmcRadioTxFreqMax
		Integer32,
	mwrEmcRadioTxPowerMin
		Integer32,
	mwrEmcRadioTxPowerMax
		Integer32,
	mwrEmcRadioLinkStatus
		INTEGER
}

mwrEmcRadioStatusIndex  OBJECT-TYPE
	SYNTAX     RadioInstanceType
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"A unique value for each radio channel if applicable."
	::= { mwrEmcRadioStatusEntry 1 }

mwrEmcRadioOperStatus  OBJECT-TYPE
	SYNTAX     INTEGER {
		up (1),
		down (2)
	}
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"The current operational state of the Radio. When radio is fully configured and ready to operate the status will be up."
	::= { mwrEmcRadioStatusEntry 2 }

mwrEmcRadioTRSpacing  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"kHz"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Represents the difference between the configured TX/RX center frequency of the radio channel."
	::= { mwrEmcRadioStatusEntry 3 }

mwrEmcRadioActualTxStatus  OBJECT-TYPE
	SYNTAX     EnableType
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"This object defines the actual transmit state of the radio channel."
	::= { mwrEmcRadioStatusEntry 4 }

mwrEmcRadioRxFreqMin  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"kHz"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Represents the minimum radio RX frequency allowed."
	::= { mwrEmcRadioStatusEntry 5 }

mwrEmcRadioRxFreqMax  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"kHz"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Represents the maximum radio RX frequency allowed."
	::= { mwrEmcRadioStatusEntry 6 }

mwrEmcRadioTxFreqMin  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"kHz"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Represents the minimum radio TX frequency allowed."
	::= { mwrEmcRadioStatusEntry 7 }

mwrEmcRadioTxFreqMax  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"kHz"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Represents the maximum radio TX frequency allowed."
	::= { mwrEmcRadioStatusEntry 8 }

mwrEmcRadioTxPowerMin  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"dB"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Represents the minimum radio Transmit Power allowed."
	::= { mwrEmcRadioStatusEntry 9 }

mwrEmcRadioTxPowerMax  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"dB"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Represents the maximum radio Transmit Power allowed."
	::= { mwrEmcRadioStatusEntry 10 }

mwrEmcRadioLinkStatus  OBJECT-TYPE
	SYNTAX     INTEGER {
		up (1),
		down (2)
	}
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"The current operational status of the radio link."
	::= { mwrEmcRadioStatusEntry 11 }

mwrEmcRadioPerfStatsTable  OBJECT-TYPE
	SYNTAX SEQUENCE OF MwrEmcRadioPerfStatsEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table containing the performance of the radio channel."
	::= { mwrEmcRadioPerformance 1 }

mwrEmcRadioPerfStatsEntry  OBJECT-TYPE
	SYNTAX 	MwrEmcRadioPerfStatsEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table entry containing the performance of the radio channel."
	INDEX { mwrEmcRadioStatsIndex }
	::= { mwrEmcRadioPerfStatsTable 1 }

MwrEmcRadioPerfStatsEntry ::= SEQUENCE {
	mwrEmcRadioStatsIndex
		RadioInstanceType,
	mwrEmcRadioTxFrames
		Counter64,
	mwrEmcRadioRxGoodFrames
		Counter64,
	mwrEmcRadioRxErrsFrames
		Counter64,
	mwrEmcRadioRSL
		Integer32,
	mwrEmcRadioEqualizerStress
		Integer32,
	mwrEmcRadioSNR
		Integer32,
	mwrEmcRadioLinkAvailability
		Counter32,
	mwrEmcRadioActualTxPower
		Integer32,
	mwrEmcRadioActualTxProfile
		DisplayString
}

mwrEmcRadioStatsIndex  OBJECT-TYPE
	SYNTAX     RadioInstanceType
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"A unique value for each radio channel if applicable."
	::= { mwrEmcRadioPerfStatsEntry 1 }

mwrEmcRadioTxFrames  OBJECT-TYPE
	SYNTAX     Counter64
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"The current count of radio frames transmitted."
	::= { mwrEmcRadioPerfStatsEntry 2 }

mwrEmcRadioRxGoodFrames  OBJECT-TYPE
	SYNTAX     Counter64
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"The current count of good radio frames received."
	::= { mwrEmcRadioPerfStatsEntry 3 }

mwrEmcRadioRxErrsFrames  OBJECT-TYPE
	SYNTAX     Counter64
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"The current count of radio frames received in error."
	::= { mwrEmcRadioPerfStatsEntry 4 }

mwrEmcRadioRSL  OBJECT-TYPE
	SYNTAX     Integer32
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"An estimate of the radio RSL. Divide the value by 10 to get the actual RSL value. Once this number is divided by 10 the units are dB.  For example -352 is actually -35.2dB"
	::= { mwrEmcRadioPerfStatsEntry 5 }

mwrEmcRadioEqualizerStress  OBJECT-TYPE
	SYNTAX     Integer32
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"Indicates the average magnitude of all the equalizer taps to provide a measure of how hard the equalizer is working."
	::= { mwrEmcRadioPerfStatsEntry 6 }

mwrEmcRadioSNR  OBJECT-TYPE
	SYNTAX     Integer32
	UNITS 	"dB"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"The absolute value of the estimate of the radio SNR. Divide the value by 10 to get the actual SNR."
	::= { mwrEmcRadioPerfStatsEntry 7 }

mwrEmcRadioLinkAvailability  OBJECT-TYPE
	SYNTAX     Counter32
	UNITS 	"sec"
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"The amount of time the radio link is up."
	::= { mwrEmcRadioPerfStatsEntry 8 }

mwrEmcRadioActualTxPower  OBJECT-TYPE
	SYNTAX     Integer32
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"This object indicates the running configuration for tx power."
	::= { mwrEmcRadioPerfStatsEntry 9 }

mwrEmcRadioActualTxProfile  OBJECT-TYPE
	SYNTAX     DisplayString
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"A read-only string specifying the actual value for the TX profile."
	::= { mwrEmcRadioPerfStatsEntry 10 }

mwrEmcRadioPerfStats32BitTable  OBJECT-TYPE
	SYNTAX SEQUENCE OF MwrEmcRadioPerfStats32BitEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table containing 32-bit counters of the radio channel. This table is provided to satisfy snmp v1 users where they can't access 64-bit counters."
	::= { mwrEmcRadioPerformance 2 }

mwrEmcRadioPerfStats32BitEntry  OBJECT-TYPE
	SYNTAX 	MwrEmcRadioPerfStats32BitEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"Table entry containing 32-bit counters of the radio channel."
	INDEX { mwrEmcRadioStats32BitIndex }
	::= { mwrEmcRadioPerfStats32BitTable 1 }

MwrEmcRadioPerfStats32BitEntry ::= SEQUENCE {
	mwrEmcRadioStats32BitIndex
		RadioInstanceType,
	mwrEmcRadioTxFrames32Bit
		Counter32,
	mwrEmcRadioRxGoodFrames32Bit
		Counter32,
	mwrEmcRadioRxErrsFrames32Bit
		Counter32
}

mwrEmcRadioStats32BitIndex  OBJECT-TYPE
	SYNTAX     RadioInstanceType
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION 
		"A unique value for each radio channel if applicable."
	::= { mwrEmcRadioPerfStats32BitEntry 1 }

mwrEmcRadioTxFrames32Bit  OBJECT-TYPE
	SYNTAX     Counter32
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"A low capacity 32-bit counter representing the current count of radio frames transmitted."
	::= { mwrEmcRadioPerfStats32BitEntry 2 }

mwrEmcRadioRxGoodFrames32Bit  OBJECT-TYPE
	SYNTAX     Counter32
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"A low capacity 32-bit counter representing the current count of radio frames received."
	::= { mwrEmcRadioPerfStats32BitEntry 3 }

mwrEmcRadioRxErrsFrames32Bit  OBJECT-TYPE
	SYNTAX     Counter32
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION 
		"A low capacity 32-bit counter representing the current count of radio frames received in error."
	::= { mwrEmcRadioPerfStats32BitEntry 4 }

-- 
-- RADIO NOTIFICATIONS
-- 

mwrEmcRadioRxLossOfSync  NOTIFICATION-TYPE
	OBJECTS { mwrEventConfigSeverity, 
		mwrEmcRadioStatusIndex, 
		equipmentAlarmActiveConditionId, 
		equipmentTrapInfo, 
		equipmentOutTrapsCounter }
	STATUS     current
	DESCRIPTION 
		"This notification is raised when radio link loses synchronization on its receiver. The mwrEmcRadioStatusIndex indicates each radio channel."
	::= { mwrEmcRadioNotifications 1 }

mwrEmcRadioFailure  NOTIFICATION-TYPE
	OBJECTS { mwrEventConfigSeverity, 
		mwrEmcRadioStatusIndex, 
		equipmentAlarmActiveConditionId, 
		equipmentTrapInfo, 
		equipmentOutTrapsCounter }
	STATUS     current
	DESCRIPTION 
		"This notification is raised when fault is detected in radio. The reason could be faulty components or invalid configuration. The mwrEmcRadioStatusIndex indicates each radio channel."
	::= { mwrEmcRadioNotifications 2 }

mwrEmcRadioCalUnavailable  NOTIFICATION-TYPE
	OBJECTS { mwrEventConfigSeverity, 
		equipmentAlarmActiveConditionId, 
		equipmentTrapInfo, 
		equipmentOutTrapsCounter }
	STATUS     current
	DESCRIPTION 
		"This notification is raised when the calibration information is not available in the system."
	::= { mwrEmcRadioNotifications 3 }

mwrEmcRadioRslBelowThreshold  NOTIFICATION-TYPE
	OBJECTS { mwrEventConfigSeverity, 
		mwrEmcRadioStatusIndex, 
		equipmentAlarmActiveConditionId, 
		equipmentTrapInfo, 
		equipmentOutTrapsCounter }
	STATUS     current
	DESCRIPTION 
		"This notification is raised when the receive signal level of the radio link is below the user configured limit. The mwrEmcRadioStatusIndex indicates each radio channel."
	::= { mwrEmcRadioNotifications 4 }

mwrEmcRadioTxlAboveThreshold  NOTIFICATION-TYPE
	OBJECTS { mwrEventConfigSeverity, 
		mwrEmcRadioStatusIndex, 
		equipmentAlarmActiveConditionId, 
		equipmentTrapInfo, 
		equipmentOutTrapsCounter }
	STATUS     current
	DESCRIPTION 
		"This notification is raised when the radio transmit power level exceeds the user set limit.  The mwrEmcRadioStatusIndex indicates each radio channel."
	::= { mwrEmcRadioNotifications 5 }

mwrEmcRadioConfigMismatch  NOTIFICATION-TYPE
	OBJECTS { mwrEventConfigSeverity, 
		mwrEmcRadioStatusIndex, 
		equipmentAlarmActiveConditionId, 
		equipmentTrapInfo, 
		equipmentOutTrapsCounter }
	STATUS     current
	DESCRIPTION 
		"This notification is raised when the radio configuration between the peers is mismatched."
	::= { mwrEmcRadioNotifications 6 }
END

