ALCATEL-IND1-DVMRP-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        Integer32, Unsigned32
            FROM SNMPv2-SMI
        TruthValue
            FROM SNMPv2-TC
        MODULE-COMPLIANCE, OBJECT-GROUP
            FROM SNMPv2-CONF
        dvmrpInterfaceEntry
            FROM DVMRP-STD-MIB
        routingIND1Dvmrp
            FROM ALCATEL-IND1-BASE;

alcatelIND1DVMRPMIB MODULE-IDENTITY
    LAST-UPDATED  "200704030000Z"
    ORGANIZATION  "Alcatel-Lucent"
    CONTACT-INFO
        "Please consult with Customer Service to ensure the most appropriate
         version of this document is used with the products in question:

                    Alcatel-Lucent, Enterprise Solutions Division
                   (Formerly Alcatel Internetworking, Incorporated)
                           26801 West Agoura Road
                        Agoura Hills, CA  91301-5122
                          United States Of America

        Telephone:               North America  +1 800 995 2696
                                 Latin America  +1 877 919 9526
                                 Europe         +31 23 556 0100
                                 Asia           +65 394 7933
                                 All Other      +1 818 878 4507

        Electronic Mail:         support@ind.alcatel.com
        World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
        File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

    DESCRIPTION
        "This module describes an authoritative enterprise-specific Simple
         Network Management Protocol (SNMP) Management Information Base (MIB):

             This MIB contains management information for Coronado Layer
             3 Hardware Routing Engine (HRE) management.

         The right to make changes in specification and other information
         contained in this document without prior notice is reserved.

         No liability shall be assumed for any incidental, indirect, special, or
         consequential damages whatsoever arising from or related to this
         document or the information contained herein.

         Vendors, end-users, and other interested parties are granted
         non-exclusive license to use this specification in connection with
         management of the products for which it is intended to be used.

                     Copyright (C) 1995-2007 Alcatel-Lucent
                         ALL RIGHTS RESERVED WORLDWIDE"

    REVISION      "200704030000Z"
    DESCRIPTION
        "The latest version of this MIB Module."

    ::= { routingIND1Dvmrp 1 }

alcatelIND1DVMRPMIBObjects OBJECT IDENTIFIER ::= { alcatelIND1DVMRPMIB 1 }

alaDvmrpGlobalConfig    OBJECT IDENTIFIER ::= { alcatelIND1DVMRPMIBObjects 1 }
alaDvmrpTunnelXIfTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF AlaDvmrpTunnelXIfEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of attributes that are associated with the internal
        assigned tunnel index when a DVMRP tunnel is created.  This table
        contains additional objects that are not present in the tunnelMIB
        tunnelIfTable."
        ::= { alcatelIND1DVMRPMIBObjects 2 }


-- ***************************************************************************
-- Global DVMRP Configuration
-- ***************************************************************************

alaDvmrpAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                 enable(1),
                 disable(2),
                 unrestrictedEnable(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "Administratively enables/disables the
                 DVMRP protocol on this router."
    DEFVAL      { disable }
    ::= { alaDvmrpGlobalConfig 1}

alaDvmrpRouteReportInterval OBJECT-TYPE
    SYNTAX      Integer32 (10..2000)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The Route Report Interval determines how often
                 a router will send its complete routing tables to
                 neighboring routers running DVMRP."
    DEFVAL      { 60 }
    ::= { alaDvmrpGlobalConfig 2}

alaDvmrpFlashUpdateInterval OBJECT-TYPE
    SYNTAX      Integer32 (5..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The minimum Flash Update Interval defines how often
                 routing table change messages are sent to
                 neighboring DVMRP routers.  Since these messages
                 are sent between the transmission of complete
                 routing tables, the flash update interval value
                 must be shorter than that of the route report
                 interval."
    DEFVAL      { 5 }
    ::= { alaDvmrpGlobalConfig 3}

alaDvmrpNeighborTimeout OBJECT-TYPE
    SYNTAX      Integer32 (5..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The Neighbor Timeout value specifies how long, without
                 any activity from a neighboring DVMRP router, the
                 router will wait before assuming that the inactive
                 router is down."
    DEFVAL      { 35 }
    ::= { alaDvmrpGlobalConfig 4}

alaDvmrpRouteExpirationTimeout OBJECT-TYPE
    SYNTAX      Integer32 (20..4000)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The Route Expiration Timeout value specifies how
                 long the router will wait before aging out a route.
                 When this value expires, the route is advertised as
                 inactive until either it's activity resumes or it is
                 deleted."
    DEFVAL      { 140 }
    ::= { alaDvmrpGlobalConfig 5}

alaDvmrpRouteHoldDown OBJECT-TYPE
    SYNTAX      Integer32 (1..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "Specifies the time during which DVMRP routes are kept
                 in a hold-down state.  A hold-down state refers to
                 the time that a route to an inactive network continues
                 to be advertised."
    DEFVAL      { 120 }
    ::= { alaDvmrpGlobalConfig 6}

alaDvmrpNeighborProbeInterval OBJECT-TYPE
    SYNTAX      Integer32 (5..30)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The Neighbor Probe Interval value specifies how often
                 probes will be transmitted to those interfaces
                 with attached DVMRP neighbors."
    DEFVAL      { 10 }
    ::= { alaDvmrpGlobalConfig 7}

alaDvmrpPruneLifetime OBJECT-TYPE
    SYNTAX      Integer32 (180..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The Prune Lifetime value defines the value
                 whereby a source-rooted multicast tree will be
                 pruned."
    DEFVAL      { 7200 }
    ::= { alaDvmrpGlobalConfig 8}

alaDvmrpPruneRetransmission OBJECT-TYPE
    SYNTAX      Integer32 (30..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The Prune Packet Retransmission value is the duration
                 of time that the router will wait, if it continues
                 to receive unwanted multicast traffic, before
                 retransmitting a prune message."
    DEFVAL      { 30 }
    ::= { alaDvmrpGlobalConfig 9}

alaDvmrpGraftRetransmission OBJECT-TYPE
    SYNTAX      Integer32 (5..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The Graft message Retransmission value defines
                 the duration of time that the router will wait
                 before retransmitting a graft message, if it has
                 not already received an acknowledgement from its
                 neighbor."
    DEFVAL      { 5 }
    ::= { alaDvmrpGlobalConfig 10}

alaDvmrpInitNbrAsSubord OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
                "The value true(1) indicates neighbors, on initial discovery,
                are considered subordinate.  This means traffic may be resumed
                slightly quicker on network disruptions.  But, if the neighbor
                has trouble handling huge initial blasts of traffic, it may be
                wise to wait until route reports have been exchanged and the
                neighbor has requested dependency, before forwarding traffic."
    DEFVAL      { true }
    ::= { alaDvmrpGlobalConfig 11}

 alaDvmrpBfdStatus    OBJECT-TYPE
	SYNTAX	INTEGER
			{
			enable(1),
			disable(2)
			}
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	"Enables/Disables Bfd for DVMRP Protocol."
	DEFVAL      {disable}
	::= { alaDvmrpGlobalConfig 12}

 alaDvmrpBfdAllInterfaceStatus   OBJECT-TYPE
	SYNTAX	INTEGER
			{
			enable(1),
			disable(2)
			}
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	"Enables/Disables Bfd for all DVMRP interfaces."
	DEFVAL      {disable}
	::= { alaDvmrpGlobalConfig 13}

 alaDvmrpMbrOperStatus   OBJECT-TYPE
	SYNTAX	INTEGER
			{
			enable(1),
			disable(2)
			}
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	"Whether MBR is currently enabled/disabled for DVMRP."
	::= { alaDvmrpGlobalConfig 14}

-- ************************************************************************
--  DVMRP Tunnel Config Extension Table
-- ************************************************************************
alaDvmrpTunnelXIfEntry  OBJECT-TYPE
    SYNTAX      AlaDvmrpTunnelXIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing additional attributes associated with a DVMRP
        tunnel."
    INDEX { alaDvmrpTunnelIndex }
    ::= { alaDvmrpTunnelXIfTable 1 }

AlaDvmrpTunnelXIfEntry ::=
    SEQUENCE {
        alaDvmrpTunnelIndex     Unsigned32,
        alaDvmrpLocalIfIndex    Unsigned32
    }

alaDvmrpTunnelIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tunnel index of the DVMRP tunnel."
    ::= { alaDvmrpTunnelXIfEntry 1 }

alaDvmrpLocalIfIndex        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interface index of the local end-point of the DVMRP tunnel."

    ::= { alaDvmrpTunnelXIfEntry 2 }

 alaDvmrpIfAugTable OBJECT-TYPE
	SYNTAX     SEQUENCE OF AlaDvmrpIfAugEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"Expansion for Dvmrp Intf table."
		::= { alcatelIND1DVMRPMIBObjects 4 }

 alaDvmrpIfAugEntry OBJECT-TYPE
	SYNTAX       AlaDvmrpIfAugEntry
	MAX-ACCESS   not-accessible
	STATUS       current
	DESCRIPTION
		"An entry of alaDvmrpIfAugEntry."
    	AUGMENTS { dvmrpInterfaceEntry } 
		::= { alaDvmrpIfAugTable 1 }

 AlaDvmrpIfAugEntry ::=
	SEQUENCE {
			alaDvmrpIfBfdStatus		       INTEGER, 
			alaDvmrpIfMbrDefaultInfoStatus INTEGER 
           	 }

 alaDvmrpIfBfdStatus		OBJECT-TYPE
	SYNTAX		INTEGER
			{
			enable(1),
			disable(2)
			}
	MAX-ACCESS	read-only
	STATUS   current
	DESCRIPTION
		"This object enables/disables BFD for this DVMRP interface."
		::= { alaDvmrpIfAugEntry 1 }

 alaDvmrpIfMbrDefaultInfoStatus	OBJECT-TYPE
	SYNTAX		INTEGER
			{
			enable(1),
			disable(2)
			}
	MAX-ACCESS	read-create
	STATUS   current
	DESCRIPTION
		"This object enables/disables DVMRP to advertise the default route 
        on this interface.  This object is only applicable if the router
        is operating as a Multicast Border Router."
	DEFVAL { disable }
		::= { alaDvmrpIfAugEntry 2 }

-- conformance information

alcatelIND1DVMRPMIBConformance OBJECT IDENTIFIER ::= { alcatelIND1DVMRPMIB 2 }
alcatelIND1DVMRPMIBCompliances OBJECT IDENTIFIER ::=
                                          { alcatelIND1DVMRPMIBConformance 1 }
alcatelIND1DVMRPMIBGroups      OBJECT IDENTIFIER ::=
                                          { alcatelIND1DVMRPMIBConformance 2 }

-- compliance statements

alaDvmrpCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for routers running DVMRP
            and implementing the ALCATEL-IND1-DVMRP MIB."
    MODULE  -- this module
        MANDATORY-GROUPS { alaDvmrpConfigMIBGroup, 
                           alaDvmrpTunnelXIfMIBGroup,alaDvmrpIfConfigGroup }

    ::= { alcatelIND1DVMRPMIBCompliances 1 }

-- units of conformance

alaDvmrpConfigMIBGroup OBJECT-GROUP
    OBJECTS { alaDvmrpAdminStatus, alaDvmrpRouteReportInterval,
              alaDvmrpFlashUpdateInterval, alaDvmrpNeighborTimeout,
              alaDvmrpRouteExpirationTimeout, alaDvmrpRouteHoldDown,
              alaDvmrpNeighborProbeInterval, alaDvmrpPruneLifetime,
              alaDvmrpPruneRetransmission, alaDvmrpGraftRetransmission,
              alaDvmrpInitNbrAsSubord,alaDvmrpBfdStatus,alaDvmrpBfdAllInterfaceStatus,
              alaDvmrpMbrOperStatus
            }
    STATUS  current
    DESCRIPTION
            "A collection of objects to support the management of global
            configuration parameters on DVMRP routers."
    ::= { alcatelIND1DVMRPMIBGroups 1 }

alaDvmrpTunnelXIfMIBGroup OBJECT-GROUP
    OBJECTS { alaDvmrpLocalIfIndex }
    STATUS  current
    DESCRIPTION
            "These objects are required to provide additional information 
            about configured DVMRP tunnels not found in the standard tunnel
            MIB."
    ::= { alcatelIND1DVMRPMIBGroups 2 }
alaDvmrpIfConfigGroup    OBJECT-GROUP
   OBJECTS { alaDvmrpIfBfdStatus, alaDvmrpIfMbrDefaultInfoStatus }
    STATUS  current
    DESCRIPTION
            "These objects are required to provide additional information
            about configured DVMRP interfaces not found in the standard tunnel
            MIB."
    ::= { alcatelIND1DVMRPMIBGroups 3 }


END

