-- **************************************************************************
-- **************************************************************************
--
-- File         : mmalert.mib
-- Description  : IBM Management Module traps
--                MIB for traps(Alerts)
-- Version      : 6.0
-- Date         : August 2014
--
--
-- Copyright (c) 2002 - 2014 IBM  All Rights Reserved.
--
--
-- Contains trap descriptions for:
--  (1) Bladecenter Management Module
--
-- This MIB is used by the Management Module to describe
-- traps for alert conditions detected by the MM/Blades on Bladecenter hardware.
--
-- The CMM alert MIB (mmalert.mib) is written in SNMPv1 SMI format,
-- which does not include a SYNTAX definition for an unsigned data type.
-- This data type, however, is important and is used for event identifiers
-- in this MIB.
--
-- Some management tools, MIB browsers, and MIB compiler tools will raise
-- errors when encountering this Unsigned32 SYNTAX. To alleviate these
-- errors, the mmalert.mib file may be updated using one of these methods:
--
-- 1) Define the Unsigned32 TEXTUAL-CONVENTION
--
--          Unsigned32 ::= TEXTUAL-CONVENTION
--                         STATUS       current
--                         DESCRIPTION
--                         Unsigned integer data type
--                         SYNTAX       INTEGER (0..4294967295)
--
-- 2) Define an Unsigned32 integer range
--
--          Unsigned32 ::=  INTEGER (0..4294967295)
--
-- 3) Define an alias for Unsigned32 integer range and then update the
--    usage of it in the mmalert.mib file:
--
--          AliasUnsigned32 ::=  INTEGER (0..4294967295)
--
--          SYNTAX  AliasUnsigned32   // For example
--
-- 4) Add the Unsigned32 line to the IMPORTS list:
--
--     IMPORTS                                                                  
--        OBJECT-TYPE        FROM RFC-1212                                
--        enterprises        FROM RFC1155-SMI                              
--        DisplayString      FROM RFC1213-MIB                              
--        Unsigned32         FROM SNMPv2-SMI
--        TRAP-TYPE          FROM RFC-1215;
-- 
-- **************************************************************************
-- **************************************************************************

        BLADESPPALT-MIB DEFINITIONS ::= BEGIN


        IMPORTS
            OBJECT-TYPE                          FROM RFC-1212
            enterprises                          FROM RFC1155-SMI
            DisplayString                        FROM RFC1213-MIB
            TRAP-TYPE                            FROM RFC-1215;


        ibm            OBJECT IDENTIFIER ::=   { enterprises 2 }

        -- IBM products group

        ibmProd        OBJECT IDENTIFIER ::=   { ibm 6 }

        -- IBM Netfinity SP

        supportProcessor OBJECT IDENTIFIER ::= { ibmProd 158 }

        -- IBM Netfinity SP Alert

        mmRemoteSupTrapMIB     OBJECT IDENTIFIER ::= { supportProcessor 3 }

-- **************************************************************************
-- Start: Management Module Adapter SP Alerts
-- **************************************************************************

        -- the rsspalt generic trap generator group

        remoteSupTrapMibObjects OBJECT IDENTIFIER ::= { mmRemoteSupTrapMIB 1 }


        spTrapInfo OBJECT IDENTIFIER ::= { remoteSupTrapMibObjects 1 }

        spTrapDateTime  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Timestamp of Local Date and Time when alert was generated
                        NOTE: the format is changeable by a setting on the Management Module (Flex System only)"
                       ::= { spTrapInfo 1 }

        spTrapAppId    OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Platform ID, either 'IBM Flex Chassis Management Module' (Flex System)
                                     or 'BladeCenter Management Module' (BladeCenter)"
                       ::= { spTrapInfo 2 }

        spTrapSpTxtId  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "SP System Identification - Text Identification"
                       ::= { spTrapInfo 3 }

        spTrapSysUuid  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Host System UUID(Universal Unique ID)"
                       ::= { spTrapInfo 4 }

        spTrapSysSern  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "'Chassis Serial Number'(Flex System) or 'AMM Serial Number' (BladeCenter)" 
                       ::= { spTrapInfo 5 }

        spTrapAppType  OBJECT-TYPE
                       SYNTAX  INTEGER (1..65535)
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Application Alert Type - Trap Type ID"
                       ::= { spTrapInfo 6 }

        spTrapPriority  OBJECT-TYPE
                       SYNTAX  INTEGER (1..65535)
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Alert Severity Value
                          - Critical Alert(0)
                          - Major(1)
                          - Non-Critical Alert(2)
                          - System Alert(4)
                          - Recovery Alert(8)
                          - Informational Only Alert(255)"
                       ::= { spTrapInfo 7 }

        spTrapMsgText  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Alert Message Text"
                       ::= { spTrapInfo 8 }

        spTrapHostContact  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Host Contact"
                       ::= { spTrapInfo 9 }

        spTrapHostLocation  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Host Location"
                       ::= { spTrapInfo 10 }

        spTrapBladeName  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Server Name
                        NOTE: This will only be populated if a server event triggered this trap."
                       ::= { spTrapInfo 11 }

        spTrapBladeSern  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Server Serial Number
                        NOTE: This will only be populated if a server event triggered this trap."
                       ::= { spTrapInfo 12 }

        spTrapBladeUuid  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Server UUID(Universal Unique ID)
                        NOTE: This will only be populated if a server event triggered this trap."
                       ::= { spTrapInfo 13 }

        spTrapEvtName  OBJECT-TYPE
                       SYNTAX Unsigned32 (1..4294967295)
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "The event ID in decimal (hexidecimal format may be cross referenced in InfoCenter)."
                       ::= { spTrapInfo 14 }                       

        spTrapSourceId  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "The source identifier associated with the event that caused the trap
                        - SERVPROC : event associated with the service processor
                        - Audit    : audit event (in audit log)
                        - Stor_X   : event associated with storage element X
                        - IOMod_X  : event associated with switch X
                        - Cool_X   : event associated with fan X
                        - Power_X  : event associated with power supply X
                        - Blade_X  : event associated with server X"
                       ::= { spTrapInfo 15 }

        spTrapCallHomeFlag  OBJECT-TYPE
                       SYNTAX  Unsigned32 (1..4294967295)
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "The call home flag associated with the event that caused the trap
                         - No Call Home generated with this event (0)
                         - Call Home generated with this event if call home is enabled (1)"
                       ::= { spTrapInfo 16 }

        spTrapSysIPAddress  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "The chassis Management Module IP Address.
                       
                        NOTE: In some very rare cases, the IP address will indicate 0.0.0.0 
                              instead of the proper configured IP address. This can happen
                              on the initial trap that leaves the chassis Management Module
                              if the associated event happens extremely early in the boot up cycle."
                       ::= { spTrapInfo 17 }

        spTrapSysMachineModel  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Chassis Machine Type/Model"
                       ::= { spTrapInfo 18 }

        spTrapBladeMachineModel  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Server Machine Type/Model
                        NOTE: This will only be populated if a server event triggered this trap."
                       ::= { spTrapInfo 19 }

        spTrapBladeFRUSerialNumber  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Server Field Replaceable Unit (FRU) Serial Number
                        NOTE: This will only be populated if a server event triggered this trap.
                              spTrapBladeFRUSerialNumber is only available on Flex System."
                       ::= { spTrapInfo 20 }

        spTrapBladeEvtName  OBJECT-TYPE
                       SYNTAX  DisplayString 
		       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "The server event ID. This ID can be cross referenced in the InfoCenter.
                        NOTE: This will only be populated if a server event triggered this trap.
                              spTrapBladeEvtName is only available on Flex System."
                       ::= { spTrapInfo 21 }

        spBladeEventDataSource  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "The 5 bytes are values from the IPMI standard SEL (System Event Log) entry received for from server.
                        Byte 1 (SEL Byte 11) - IPMI Standard Sensor Type
                        Byte 2 (SEL Byte 13) - IPMI Standard Event/Reading Type Code
                        Byte 3 (SEL Byte 14) - Event Data 1
                        Byte 4 (SEL Byte 15) - Event Data 2
                        Byte 5 (SEL Byte 16) - Event Data 3
                        NOTE: This will only be populated if a server event triggered this trap.
                              spBladeEventDataSource is only available on Flex System"
                       ::= { spTrapInfo 22 }

        spTrapAuxData  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Auxiliary data associated with the event. Truncated if more than 127 characters.
                        NOTE: spTrapAuxData is only available on Flex System."
                       ::= { spTrapInfo 23 }

        spTrapComponentID  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Component ID to associate the trap with the location in the chassis and, if applicable, the node enclosure.
                        NOTE: spTrapComponentID is only available on Flex System."
                       ::= { spTrapInfo 24 }

        spTrapComponentFRUInfo  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Field Replaceable Unit (FRU) of the component that caused the trap.
                        NOTE: spTrapComponentFRUInfo is only available on Flex System."
                       ::= { spTrapInfo 25 }

        spTrapChassisName  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Chassis Name
                        NOTE: This will only populate if the Chassis Name has been set.
                              spTrapChassisName is only available on Flex System."
                       ::= { spTrapInfo 26 }

        spTrapSysRoomId  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Chassis Room ID
                        NOTE: This will only populate if the Chassis Room ID has been set.
                              spTrapSysRoomId is only available on Flex System."
                       ::= { spTrapInfo 27 }

        spTrapSysRackId  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Chassis Rack ID
                        NOTE: This will only populate if the Chassis Rack ID has been set.
                              spTrapSysRackId is only available on Flex System."
                       ::= { spTrapInfo 28 }

        spTrapSysRackU  OBJECT-TYPE
                       SYNTAX  Unsigned32 (1..4294967295) 
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Chassis anchor (lowest) Rack U location
                        NOTE: This will only populate if the Chassis lowest Rack U has been set (otherwise it will be '0').
                              spTrapSysRackU is only available on Flex System."
                       ::= { spTrapInfo 29 }

        spTrapServiceableEventFlag  OBJECT-TYPE
                       SYNTAX  Unsigned32 (1..4294967295) 
		       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "The serviceable event flag associated with the event that caused the trap
                        - the event requires no user action (0)
                        - the event is serviceable and requires user attention (1)
                        NOTE: spTrapServiceableEventFlag is only available on Flex System."
                       ::= { spTrapInfo 30 }

        spLogSequenceNum  OBJECT-TYPE
                       SYNTAX  Unsigned32 (1..4294967295)
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "Sequence number from the chassis event log or audit log.
                        NOTE: Audit logs are stored separately internally.
                              spLogSequenceNum is only available on Flex System."
                       ::= { spTrapInfo 31 }

        spCimMsgID  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "CIM Indication Message ID
                        NOTE: spCimMsgID is only available on Flex System."
                       ::= { spTrapInfo 32 }

        spCimMsgPrefix  OBJECT-TYPE
                       SYNTAX  DisplayString
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "CIM Indication Message ID name space, one of the following:
                        - PLAT : DMTF platform registry
                        - CMM  : CMM message registry
                        NOTE: spCimMsgPrefix is only available on Flex System."
                       ::= { spTrapInfo 33 }

        spEventCorrelator  OBJECT-TYPE
                       SYNTAX  Unsigned32 (0..4294967295)
                       ACCESS  read-only
                       STATUS  mandatory
                       DESCRIPTION
                       "For events originated by the CMM:
                       If this event is part of a event group, this will be the unique
                       identifier from 1 - 255 for the event group. Zero means no group.
                       An alert in the same event group replaces an active alert from the
                       group.  The recovery event in the group clears the active alert
                       in the group.

                       For events created by the node system-management processor that are 
                       logged by CMM:
                       This field is a correlator from 0 - 254 that is the same for a node alert
                       and the node recovery event for the alert.  A node recovery event clears 
                       an existing node alert if all of the following fields from the node alert 
                       and the node recovery event match: the event correlator (spEventCorrelator) 
                       value, the Blade UUID (spTrapBladeUuid), and the Blade Event Data Source 
                       (spBladeEventDataSource).
                       NOTE: spEventCorrelator is only available on Flex System."
                       ::= { spTrapInfo 34 }

              
-- **************************************************************************
-- Critical Traps
-- **************************************************************************
        mmTrapTempC          TRAP-TYPE
                                ENTERPRISE  mmRemoteSupTrapMIB
                                VARIABLES
                                  {
                                  spTrapDateTime,
                                  spTrapAppId,
                                  spTrapSpTxtId,
                                  spTrapSysUuid,
                                  spTrapSysSern,
                                  spTrapAppType,
                                  spTrapPriority,
                                  spTrapMsgText,
                                  spTrapHostContact,
                                  spTrapHostLocation,
                                  spTrapBladeName,
                                  spTrapBladeSern,
                                  spTrapBladeUuid,
                                  spTrapEvtName,
                                  spTrapSourceId,
                                  spTrapCallHomeFlag,
                                  spTrapSysIPAddress,
                                  spTrapSysMachineModel,  
                                  spTrapBladeMachineModel,
                                  spEventCorrelator
                                  }
                                  DESCRIPTION
                                    "Critical Alert: Temperature threshold exceeded.
                                    Note: This mib object will be replaced in a future release."
                                  ::= 0

        mmTrapVoltC        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Voltage threshold exceeded.
                                  Note: This mib object will be replaced in a future release."
                                ::= 1

        mmTrapTampC        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Physical intrusion of system has occurred.
                                  Note: This mib object will be replaced in a future release."
                                ::= 2

        mmTrapMffC         TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Multiple fan failure.
                                  Note: This mib object will be replaced in a future release."
                                ::= 3

        mmTrapPsC          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Power supply failure."
                                ::= 4

        mTrapHdC          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Hard disk drive failure.
                                  Note: This mib object will be replaced in a future release."
                                ::= 5

        mmTrapVrmC         TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Voltage Regulator Module(VRM) failure.
                                  Note: This mib object will be replaced in a future release."
                                ::= 6

        mmTrapSffC         TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel ,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Single Fan failure.
                                  Note: This mib object will be replaced in a future release."
                                ::= 11


        mmTrapMsC          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel ,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Multiple switch module failure.
                                  Note: This mib object will be replaced in a future release."
                                ::= 31

        mmTrapIhcC         TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Incompatible hardware configuration.
                                  Note: This mib object will be replaced in a future release."
                                ::= 36

        mmTrapBladeC          TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Blade."
                                ::= 128

        mmTrapIOC          TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: I/O Module."
                                ::= 129

        mmTrapStorageC      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Storage Module."
                                ::= 131

        mmTrapChassisC      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
		                }
                                DESCRIPTION
                                  "Critical Alert: Chassis Module."
                                ::= 130

        mmTrapFanC      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Critical Alert: Cooling Devices."
                                ::= 133

-- **************************************************************************
-- Non-Critical Traps
-- **************************************************************************

        mmTrapRdpsN          TRAP-TYPE
                                ENTERPRISE  mmRemoteSupTrapMIB
                                VARIABLES
                                  {
                                  spTrapDateTime,
                                  spTrapAppId,
                                  spTrapSpTxtId,
                                  spTrapSysUuid,
                                  spTrapSysSern,
                                  spTrapAppType,
                                  spTrapPriority,
                                  spTrapMsgText,
                                  spTrapHostContact,
                                  spTrapHostLocation,
                                  spTrapBladeName,
                                  spTrapBladeSern,
                                  spTrapBladeUuid,
                                  spTrapEvtName,
                                  spTrapSourceId,
                                  spTrapCallHomeFlag,
                                  spTrapSysIPAddress,
                                  spTrapSysMachineModel,  
                                  spTrapBladeMachineModel,
                                  spEventCorrelator
                                  }
                                  DESCRIPTION
                                    "Non-Critical Alert: Redundant Power Supply failure.
                                  Note: This mib object will be replaced in a future release."
                                  ::= 10

        mmTrapTempN        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Temperature threshold exceeded.
                                  Note: This mib object will be replaced in a future release."
                                ::= 12

        mmTrapVoltN        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel 
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Voltage threshold exceeded.
                                  Note: This mib object will be replaced in a future release."
                                ::= 13

        mmTrapRmN          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Redundant module.
                                  Note: This mib object will be replaced in a future release."
                                ::= 32
                                
       mmTrapBladeN          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Blade "
                                ::= 160

       mmTrapION          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: I/O Module"
                                ::= 161


        mmTrapLogFullN          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Event Log 100% Full."
                                ::= 7

        mmTrapStorageN       TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel, 
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Storage Module"
                                ::= 163

        mmTrapPowerN      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Power Module."
                                ::= 164

        mmTrapChassisN      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Chassis Module."
                                ::= 162

        mmTrapFanN      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "Non-Critical Alert: Cooling Devices."
                                ::= 165

-- **************************************************************************
-- System Traps
-- **************************************************************************

        mmTrapSecDvS       TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Secondary Device warning.
                                  Note: This mib object will be replaced in a future release."
                                ::= 15

        mmTrapPostToS      TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Post Timeout value exceeded.
                                  Note: This mib object will be replaced in a future release."
                                ::= 20

        mmTrapOsToS        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: OS Timeout value exceeded.
                                  Note: This mib object will be replaced in a future release."
                                ::= 21

        mmTrapAppS         TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
				spTrapBladeFRUSerialNumber,
				spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
				spTrapComponentID,
				spTrapComponentFRUInfo,
                                spTrapChassisName,
				spTrapSysRoomId,
				spTrapSysRackId,
				spTrapSysRackU,
				spTrapServiceableEventFlag,
				spLogSequenceNum,
				spCimMsgID,
				spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Application Alert."
                                ::= 22
                                
        mmTrapPoffS        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Power Off.
                                  Note: This mib object will be replaced in a future release."
                                ::= 23

        mmTrapPonS         TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Power On.
                                  Note: This mib object will be replaced in a future release."
                                ::= 24

        mmTrapBootS        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: System Boot Failure.
                                  Note: This mib object will be replaced in a future release."
                                ::= 25

        mmTrapLdrToS       TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: OS Loader Timeout.
                                  Note: This mib object will be replaced in a future release."
                                ::= 26

        mmTrapPFAS         TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Predictive Failure Analysis(PFA) information.
                                  Note: This mib object will be replaced in a future release."
                                ::= 27

        mmTrapRemoteLoginS    TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Remote Login"
                                ::= 30


        mmTrapKVMSwitchS   TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Keyboard/Video/Mouse(KVM) or Medial Tray(MT) switching failure.  
                                  Note: This mib object will be replaced in a future release."
                                ::= 33

        mmTrapSysInvS      TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Inventory."
                                ::= 34

        mmTrapSysLogS      TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: System Log 75% full."
                                ::= 35

        mmTrapNwChangeS    TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Network change notification."
                                ::= 37

        mmTrapBlThrS          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Blade Throttle.
                                  Note: This mib object will be replaced in a future release."
                                ::= 39

        mmTrapPwrMgntS          TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Power Management.
                                  Note: This mib object will be replaced in a future release."
                                ::= 40

        mmTrapBladeS        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Blade"
                                ::= 176

        mmTrapIOS        TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: I/O Module"
                                ::= 177

        mmTrapStorageS      TRAP-TYPE
                              ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Storage Module"
                                ::= 179

        mmTrapPowerS      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Power Module."
                                ::= 180

        mmTrapChassisS      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Chassis Module."
                                ::= 178

        mmTrapFanS      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Cooling Devices."
                                ::= 181

        mmTrapPwrDOS      TRAP-TYPE 
                             ENTERPRISE  mmRemoteSupTrapMIB
                              VARIABLES
                                {
                                spTrapDateTime,
                                spTrapAppId,
                                spTrapSpTxtId,
                                spTrapSysUuid,
                                spTrapSysSern,
                                spTrapAppType,
                                spTrapPriority,
                                spTrapMsgText,
                                spTrapHostContact,
                                spTrapHostLocation,
                                spTrapBladeName,
                                spTrapBladeSern,
                                spTrapBladeUuid,
                                spTrapEvtName,
                                spTrapSourceId,
                                spTrapCallHomeFlag,
                                spTrapSysIPAddress,
                                spTrapSysMachineModel,  
                                spTrapBladeMachineModel,
                                spTrapBladeFRUSerialNumber,
                                spTrapBladeEvtName,
                                spBladeEventDataSource,
                                spTrapAuxData,
                                spTrapComponentID,
                                spTrapComponentFRUInfo,
                                spTrapChassisName,
                                spTrapSysRoomId,
                                spTrapSysRackId,
                                spTrapSysRackU,
                                spTrapServiceableEventFlag,
                                spLogSequenceNum,
                                spCimMsgID,
                                spCimMsgPrefix,
                                spEventCorrelator
                                }
                                DESCRIPTION
                                  "System Alert: Power down or on."
                                ::= 182

END

