-- This module defines enterprise MIBs for Global, Global-Pro and NSM setting
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-SET-GLB-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenSetting, netscreenSettingMibModule
        FROM NETSCREEN-SMI
    Integer32, IpAddress, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    ;

netscreenSetGlbMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines the object that are used to monitor 
         Global, Global-Pro and NSM setting"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "No Comment"
    REVISION      "200105270000Z" -- May 27, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenSettingMibModule 10 }

nsSetGlbMng OBJECT IDENTIFIER ::= { netscreenSetting 10 }

nsSetGlbMngVPNEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Secure NS Global Manager/PRO traffic via VPN encryption."
    ::= { nsSetGlbMng 1 }

nsSetGlbMngEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Global Manager service on NetScreen device."
    ::= { nsSetGlbMng 2 }

nsSetGlbProEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Global Pro Management service on NetScreen device."
    ::= { nsSetGlbMng 3 }

nsSetGlbManagerSetting OBJECT IDENTIFIER ::= { nsSetGlbMng 4 }

nsSetGlbMngSerName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Server Name of Global Manager service."
    ::= { nsSetGlbManagerSetting 1 }

nsSetGlbMngSerTCP OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "TCP port number of Global Manager service."
    ::= { nsSetGlbManagerSetting 2 }

nsSetGlbMngSerUDP OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "UDP port number of Global Manager service."
    ::= { nsSetGlbManagerSetting 3 }

nsSetGlbMngLocal OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Global Manager service listening port number(NS device
         side)."
    ::= { nsSetGlbManagerSetting 4 }

nsSetGlbProManagerSetting OBJECT IDENTIFIER ::= { nsSetGlbMng 5 }

nsSetGlbProPriSer OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Primary IP Address of Global PRO Server."
    ::= { nsSetGlbProManagerSetting 1 }

nsSetGlbProSecSer OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Secondary IP Address of Global PRO Server"
    ::= { nsSetGlbProManagerSetting 2 }

nsSetGlbMngSetting OBJECT IDENTIFIER ::= { nsSetGlbMng 6 }

nsSetGlbMngProtDist OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Protocol Distribution in global management service."
    ::= { nsSetGlbMngSetting 1 }

nsSetGlbMngEthStatis OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Ethernet Statistics in global management service."
    ::= { nsSetGlbMngSetting 2 }

nsSetGlbMngAttStatis OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Attack Statistics in global management service."
    ::= { nsSetGlbMngSetting 3 }

nsSetGlbMngPlyStatis OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Policy Statistics in global management service."
    ::= { nsSetGlbMngSetting 4 }

nsSetGlbMngFlowStatis OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Flow Statistics in global management service."
    ::= { nsSetGlbMngSetting 5 }

nsSetGlbMngTrafAlm OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Traffic Alarms in global management service."
    ::= { nsSetGlbMngSetting 6 }

nsSetGlbMngAttAlm OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Attack Alarms in global management service."
    ::= { nsSetGlbMngSetting 7 }

nsSetGlbMngEvtAlm OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Event Alarms in global management service."
    ::= { nsSetGlbMngSetting 8 }

nsSetGlbMngCfgLog OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Configuration Logs in global management service."
    ::= { nsSetGlbMngSetting 9 }

nsSetGlbMngTrafLog OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Traffic Logs in global management service."
    ::= { nsSetGlbMngSetting 10 }

nsSetGlbMngInfoLog OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Information Logs in global management service."
    ::= { nsSetGlbMngSetting 11 }

nsSetGlbMngSelfLog OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Self Logs in global management service."
    ::= { nsSetGlbMngSetting 12 }

END


