
-- *****************************************************************************
-- Juniper-ATM-CONF
--
-- SNMP Agent Capabilities definitions for the ATM MIBs.
--
-- Copyright (c) 2001, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002-2005 Juniper Networks, Inc.
--   All rights reserved.
-- *****************************************************************************

Juniper-ATM-CONF  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    juniAgents
        FROM Juniper-Agents;

juniAtmAgent  MODULE-IDENTITY
    LAST-UPDATED "200508171726Z"  -- 17-Aug-05 01:26 PM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        E-mail: mib@Juniper.net"
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         The agent capabilities definitions for the ATM component of the SNMP
         agent in the Juniper E-series family of products."
    -- Revision History
    REVISION    "200508171726Z"  -- 17-Aug-05 01:26 PM EDT  - JUNOSe 7.3
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         Removed SVC support.
         ATM2-MIB:
         Removed SVC support."
    REVISION    "200502172315Z"  -- 17-Feb-05 06:15 PM EST  - JUNOSe 7.1
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         Added circuit OAM support to the ATM VCC end point agent capabilities."
    REVISION    "200401061953Z"  -- 06-Jan-04 02:53 PM EST  - JUNOSe 5.3
    DESCRIPTION
        "Added support to export the subinterface description to the line
         cards."
    REVISION    "200311071457Z"  -- 07-Nov-03 09:57 AM EST  - JUNOSe 5.2
    DESCRIPTION
        "ATM2-MIB:
         Updated from an Internet Draft to a Proposed Standard (RFC 3606).
         Juniper-UNI-ATM-MIB:
         Added ATM sub-interface location support."
    REVISION    "200305081757Z"  -- 08-May-03 01:57 PM EDT  - JUNOSe 5.1
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         Added ATM F4 OAM circuits management and ATM VP description support."
    REVISION    "200209061654Z"  -- 06-Sep-02 12:54 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         Replaced Unisphere names with Juniper names."
    REVISION    "200208091415Z"  -- 09-Aug-02 10:15 AM EDT  - JUNOSe 4.1
    DESCRIPTION
        "ATM2-MIB:
         Added support for the atmSigStatTable, the atmAal5VclStatTable and the
         atmInterfaceExtTable.
         Juniper-UNI-ATM-MIB:
         Added receive bandwith support to CAC.
         Added E164 public addressing support."
    REVISION    "200201291518Z"  -- 29-Jan-02 10:18 AM EST  - JUNOSe 4.0
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         Added ATM switched virtual connection (SVC) support to the VCC end
         point capabilities."
    REVISION    "200201241416Z"  -- 24-Jan-02 09:16 AM EST  - JUNOSe 3.4
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         Added support for ATM connection admission control (CAC) to the VCC end
         point capabilities."
    REVISION    "200112141951Z"  -- 14-Dec-01 02:51 PM EST  - JUNOSe 3.3
    DESCRIPTION
        "Juniper-UNI-ATM-MIB:
         Added ATM traffic shaping capabilities."
    REVISION    "200105231612Z"  -- 23-May-01 12:12 PM EDT  - JUNOSe 3.2
    DESCRIPTION
        "The initial release of this management information module."
    ::= { juniAgents 3 }


-- *****************************************************************************
-- ATM VCC end point agent capabilities
-- *****************************************************************************
juniAtmVccEndPointAgent  OBJECT IDENTIFIER ::= { juniAtmAgent 1 }

juniAtmVccEndPointAgentV1  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 1 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was
        supported in JUNOSe 3.0 and 3.1 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in JUNOSe.
        These capabilities became obsolete when new objects were added to the
        juniAtmSubIfGroup and support for the atmfM4IfLoopbackLocationCode
        object was added."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup,
            juniAtmAal5Group,
            juniAtmSubIfGroup }
    ::= { juniAtmVccEndPointAgent 1 }

juniAtmVccEndPointAgentV2  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 2 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was
        supported in JUNOSe 3.2 and JUNOSe 3.3 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in JUNOSe.
        These capabilities became obsolete when support was added to the
        Juniper-UNI-ATM-MIB for connection admission control (CAC)."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup2,
            juniAtmAal5Group,
            juniAtmSubIfGroup2,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup }
    ::= { juniAtmVccEndPointAgent 2 }

juniAtmVccEndPointAgentV3  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 3 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was
        supported in JUNOSe 3.4 and subsequent 3.x system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in JUNOSe.
        These capabilities became obsolete when support was added to the
        Juniper-UNI-ATM-MIB for switched virtual connection (SVC)."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup3,
            juniAtmAal5Group,
            juniAtmSubIfGroup2,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup }
    ::= { juniAtmVccEndPointAgent 3 }

juniAtmVccEndPointAgentV4  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 4 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was
        supported in JUNOSe 4.0 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in JUNOSe.
        These capabilitie became obsolete when CAC recieve bandwith and E164
        public addressing objects were added."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup4,
            juniAtmAal5Group,
            juniAtmSubIfGroup3,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup }
    ::= { juniAtmVccEndPointAgent 4 }

juniAtmVccEndPointAgentV5  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 5 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was
        supported in JUNOSe 4.1 thru 5.0 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in JUNOSe.
        These capabilitie became obsolete when F4 flow OAM circuits and ATM VP
        description objects were added to the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup5,
            juniAtmAal5Group,
            juniAtmSubIfGroup4,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2 }
    ::= { juniAtmVccEndPointAgent 5 }

juniAtmVccEndPointAgentV6  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 6 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was
        supported in JUNOSe 5.1 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in JUNOSe.
        These capabilitie became obsolete when ATM sub-interface location
        support was added to the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup6,
            juniAtmAal5Group,
            juniAtmSubIfGroup4,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2,
            juniAtmF4OamCircuitGroup }
    ::= { juniAtmVccEndPointAgent 6 }

juniAtmVccEndPointAgentV7  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 7 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was supported
        in JUNOSe 5.2 system release."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in JUNOSe.
        These capabilitie became obsolete when support was added to export
        ATM sub-interface descriptions to the line cards."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup6,
            juniAtmAal5Group,
            juniAtmSubIfGroup4,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2,
            juniAtmF4OamCircuitGroup,
            juniAtmLocationGroup }
    ::= { juniAtmVccEndPointAgent 7 }

juniAtmVccEndPointAgentV8  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 8 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was supported
        in JUNOSe 5.3 and 6.0 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in
        JUNOSe.  These capabilities became obsolete when ATM bulk configuration
        profile override was introduced."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup6,
            juniAtmAal5Group,
            juniAtmSubIfGroup5,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2,
            juniAtmF4OamCircuitGroup,
            juniAtmLocationGroup }
    ::= { juniAtmVccEndPointAgent 8 }

juniAtmVccEndPointAgentV9  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 9 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent was supported
        in JUNOSe 6.1 system release."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in
        JUNOSe.  These capabilities became obsolete when ATM bulk configuration
        profile override was introduced."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup7,
            juniAtmAal5Group,
            juniAtmSubIfGroup5,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2,
            juniAtmF4OamCircuitGroup,
            juniAtmLocationGroup }
    ::= { juniAtmVccEndPointAgent 9 }

juniAtmVccEndPointAgentV10  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 10 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent is supported
        in JUNOSe 7.0 and subsequent system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in
        JUNOSe.These capabilities became obsolete when ATM VP Statistics
        was introduced."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup8,
            juniAtmAal5Group,
            juniAtmSubIfGroup5,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2,
            juniAtmF4OamCircuitGroup,
            juniAtmLocationGroup }
    ::= { juniAtmVccEndPointAgent 10 }

juniAtmVccEndPointAgentV11  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 11 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent is supported
        in JUNOSe 7.1 and 7.2 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in
        JUNOSe. These capabilities became obsolete when SVC support
        was removed."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup8,
            juniAtmAal5Group,
            juniAtmSubIfGroup6,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2,
            juniAtmF4OamCircuitGroup2,
            juniAtmLocationGroup,
            juniAtmVpStatsGroup }
    ::= { juniAtmVccEndPointAgent 11 }

juniAtmVccEndPointAgentV12  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 12 of the ATM VCC end point agent subcomponent of the JUNOSe
        SNMP agent.  This version of the ATM end point subcomponent is supported
        in JUNOSe 7.3 and subsequent system releases."
    STATUS      current
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the ATM application in
        JUNOSe."
    SUPPORTS    ATM-MIB
        INCLUDES {
            atmInterfaceTCGroup,
            aal5VccGroup,
            atmInterfaceConfGroup2,
            atmVccTerminationGroup2 }
        VARIATION   atmVclAdminStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclReceiveTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclTransmitTrafficDescrIndex
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVccAalType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclRowStatus
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclCastType
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
        VARIATION   atmVclConnKind
            ACCESS      read-only
            DESCRIPTION
                "The atmVccTerminationGroup2 is not used for configuring VCCs.
                Use the Juniper-UNI-ATM-MIB."
    SUPPORTS    ATM2-MIB
        INCLUDES {
            atmCommonGroup,
            atmHostGroup }
        VARIATION   atmSigSSCOPConEvents
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigSSCOPErrdPdus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectSetupAttempts
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitSetupAttempts
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectUnavailRoutes
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitUnavailRoutes
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectUnavailResrcs
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitUnavailResrcs
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectCldPtyEvents
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitCldPtyEvents
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectMsgErrors
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitMsgErrors
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectClgPtyEvents
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitClgPtyEvents
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectTimerExpireds
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitTimerExpireds
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigDetectRestarts
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigEmitRestarts
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigInEstabls
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmSigOutEstabls
            ACCESS      not-implemented
            DESCRIPTION
                "The atmSigStatTable is not supported."
        VARIATION   atmVplLogicalPortDef
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmVplLogicalPortIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVplLogicalPortTable is not supported."
        VARIATION   atmInterfaceConfMaxSvpcVpi
            ACCESS      not-implemented
            DESCRIPTION
                "The atmInterfaceConfMaxSvpcVpi is not supported."
        VARIATION   atmInterfaceCurrentMaxSvpcVpi
            ACCESS      not-implemented
            DESCRIPTION
                "The atmInterfaceCurrentMaxSvpcVpi is not supported."
        VARIATION   atmInterfaceConfMaxSvccVpi
            ACCESS      not-implemented
            DESCRIPTION
                "The atmInterfaceConfMaxSvccVpi is not supported."
        VARIATION   atmInterfaceCurrentMaxSvccVpi
            ACCESS      not-implemented
            DESCRIPTION
                "The atmInterfaceCurrentMaxSvccVpi is not supported."
        VARIATION   atmInterfaceConfMinSvccVci
            ACCESS      not-implemented
            DESCRIPTION
                "The atmInterfaceConfMinSvccVci is not supported."
        VARIATION   atmInterfaceCurrentMinSvccVci
            ACCESS      not-implemented
            DESCRIPTION
                "The atmInterfaceCurrentMinSvccVci is not supported."
        VARIATION   atmIntfSigVccRxTrafficDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmIntfSigVccRxTrafficDescrIndex is not supported."
        VARIATION   atmIntfSigVccTxTrafficDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmIntfSigVccTxTrafficDescrIndex is not supported."
        VARIATION   atmIntfLeafSetupFailures
            ACCESS      not-implemented
            DESCRIPTION
                "The atmIntfLeafSetupFailures is not supported."
        VARIATION   atmIntfLeafSetupRequests
            ACCESS      not-implemented
            DESCRIPTION
                "The atmIntfLeafSetupRequests is not supported."
        VARIATION   atmCurrentlyFailingPVplTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVplTable is not supported."
        VARIATION   atmCurrentlyFailingPVclTimeStamp
            ACCESS      not-implemented
            DESCRIPTION
                "The atmCurrentlyFailingPVclTable is not supported."
        VARIATION   atmVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmVclAddrRowStatus
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclAddrTable is not supported."
        VARIATION   atmAddrVclAddrType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmAddrVclTable is not supported."
        VARIATION   atmVclGenSigDescrIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmVclGenTable is not supported."
    SUPPORTS    ATM-FORUM-SNMP-M4-MIB
        INCLUDES {
            atmfM4General,
            atmfM4AtmLayerGroup,
            atmfM4VpTestGroup,
            atmfM4VcTestGroup }
        VARIATION   atmfM4NeVersion
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeVersion object is not supported."
        VARIATION   atmfM4NeStartTime
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeStartTime object is not supported."
        VARIATION   atmfM4NeAlarmSeverityIndex
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeAlarmSeverityIndex is not supported."
        VARIATION   atmfM4NeSuppressZeroStats
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4NeSuppressZeroStats object is not supported."
        VARIATION   atmfM4IfType
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfType object is not supported."
        VARIATION   atmfM4IfSubscriberAddress
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfSubscriberAddress object is not supported."
        VARIATION   atmfM4IfPreferredCarrier
            ACCESS      not-implemented
            DESCRIPTION
                "The atmfM4IfPreferredCarrier object is not supported."
        VARIATION   atmfM4IfFarEndCarrierNetwork
            ACCESS      not-implemented
            DESCRIPTION
                "The IfFarEndCarrierNetwork object is not supported."
        VARIATION   atmfM4VclSegEndPt
            ACCESS      read-only
            DESCRIPTION
                "An atmfM4VclEntry cannot be created/modified via SNMP."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmGroup8,
            juniAtmAal5Group,
            juniAtmSubIfGroup7,
            juniAtmVpPingControlGroup,
            juniAtmVcPingControlGroup,
            juniAtmPingTrapGroup,
            juniAtmSvcGroup2,
            juniAtmF4OamCircuitGroup2,
            juniAtmLocationGroup,
            juniAtmVpStatsGroup }
    ::= { juniAtmVccEndPointAgent 12 }

-- *****************************************************************************
-- ATM VP tunnel agent capabilities
-- *****************************************************************************
juniAtmVpTunnelAgent  OBJECT IDENTIFIER ::= { juniAtmAgent 2 }

juniAtmVpTunnelAgentV1  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 1 of the ATM VP tunnel subcomponent of the JUNOSe SNMP agent.
        This version of the ATM tunnel subcomponent is supported in JUNOSe 3.0
        and subsequent system releases."
    STATUS      current
    DESCRIPTION
        "The MIB supported by the SNMP agent for the ATM application in JUNOSe."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmVpTunnelGroup }
    ::= { juniAtmVpTunnelAgent 1 }


-- *****************************************************************************
-- ATM NBMA interface agent capabilities
-- *****************************************************************************
juniAtmNbmaAgent  OBJECT IDENTIFIER ::= { juniAtmAgent 3 }

juniAtmNbmaAgentV1  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 1 of the ATM NBMA interface subcomponent of the JUNOSe SNMP
        agent.  This version of the ATM NBMA subcomponent is supported in JUNOSe
        3.2 and subsequent system releases."
    STATUS      current
    DESCRIPTION
        "The MIB supported by the SNMP agent for the ATM application in JUNOSe."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmNbmaMapGroup }
    ::= { juniAtmNbmaAgent 1 }


-- *****************************************************************************
-- ATM Switch agent capabilities
--
-- This is a placeholder for the agent capabilities for the ATM switch (cross
-- connect) subcomponent of the JUNOSe SNMP agent.
-- The ATM switch subcomponent has not been supported in a released product.
-- *****************************************************************************
juniAtmSwitchAgent    OBJECT IDENTIFIER ::= { juniAtmAgent 4 }
juniAtmSwitchAgentV1  OBJECT IDENTIFIER ::= { juniAtmSwitchAgent 1 } -- Obsolete
juniAtmSwitchAgentV2  OBJECT IDENTIFIER ::= { juniAtmSwitchAgent 2 } -- Obsolete


-- *****************************************************************************
-- ATM traffic shaping agent capabilities
-- *****************************************************************************
juniAtmTrafficShapingAgent  OBJECT IDENTIFIER ::= { juniAtmAgent 5 }

juniAtmTrafficShapingAgentV1  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 1 of the ATM traffic shaping subcomponent of the JUNOSe SNMP
        agent.  This version of the ATM traffic shaping subcomponent is
        supported in JUNOSe 3.3 and subsequent system releases."
    STATUS      current
    DESCRIPTION
        "The MIB supported by the SNMP agent for the ATM application in JUNOSe."
    SUPPORTS    Juniper-UNI-ATM-MIB
        INCLUDES {
            juniAtmTrafficShapingGroup }
    ::= { juniAtmTrafficShapingAgent 1 }

END
