-- file: ORION-BASE-MIB.mib

ORION-BASE-MIB DEFINITIONS ::= BEGIN

IMPORTS
        DisplayString
                FROM SNMPv2-TC
        OBJECT-GROUP,
        NOTIFICATION-GROUP,
        MODULE-COMPLIANCE
                FROM SNMPv2-CONF
        modules,
        orion
                FROM GLOBAL-REG
        enterprises,
        MODULE-IDENTITY,
        OBJECT-TYPE,
        NOTIFICATION-TYPE,
        Gauge32,
        Integer32,
        IpAddress
                FROM SNMPv2-SMI;

orionBaseMibModule MODULE-IDENTITY
        LAST-UPDATED "200802211439Z"
        ORGANIZATION "Delta Energy Systems (Switzerland) AG"
        CONTACT-INFO
                "postal: Delta Energy Systems (Switzerland) AG
                         Freiburgstrasse 251,
                         CH-3018 Bern-Buempliz
                 web:    www.deltapowersolutions.com
                 email:  patrick.camina@delta-es.com"
        DESCRIPTION
                "MIB for managing a DC power system with PSC 3."

                                REVISION "201204271200Z"
        DESCRIPTION
                "Rev V5.0 - ORION V5.10
                - Add Multi-Stage temperature compensation
                - Add dcBoD and dcEnableUsTempComp"
                
        REVISION "201201261415Z"
        DESCRIPTION
                "Rev V2.1 - ORION V5.0
                - changed product name from PSC3 to Orion"

        REVISION "201106200734Z"
        DESCRIPTION
                "Rev V2.0 - PSC 3 V3.20
                - hour meter functionality added"
                           
        REVISION "201102100901Z"
        DESCRIPTION
                "Rev V1.9 - PSC 3 V3.10
                - dcPowerSystem can be negativ now
                - added limits for DefaultLog and EventProcessing table
                - added dcResendActiveAlarmTraps in deschMiscGroup"
                           
        REVISION "201006161027Z"
        DESCRIPTION
                "Rev V1.8 - PSC 3 V2.70
                - new rectifier types added
                - resend active alarm traps feature added
                - measurement table added
                - battery test result enum extended"
                           
        REVISION "201002241046Z"
        DESCRIPTION
                "Rev V1.7 - PSC 3 V2.60
                - Critical alarm trap added
                - Float Charge, Battery Test, Equalize, Boost Charge,
                  ,System Voltage Supervision and Event Control Charge 
                  parameter added
                - Rectifier Group table added
                - Rectifier power limitation and efficiency cycling
                  parameter added
                - LVD table added
                - Default Log event configuration table added
                - Event Processing event configuration table added
                - Loss of Backup time parameter added"
 
        REVISION "200909040952Z"
        DESCRIPTION
                "Rev V1.6 - PSC 3 V2.50
                - Generic Alarm table added
                - Trap Destination table added"
                
        REVISION "200802211439Z"
        DESCRIPTION
                "Rev V1.5 - PSC  V2.20
                - support of write access
                - added battery parameters"
                
        REVISION "200801180835Z"
        DESCRIPTION
                "Rev V1.4 - PSC 3 V2.10
                - added event controlled charge state"

        REVISION "200607271026Z"
        DESCRIPTION
                "Rev V1.3 - PSC 3 V1.70
                - corrected Oid comment for dcStartTemp, dcStopTemp 
          and dcTotalBatteryCapacity"

        REVISION "200603020855Z"
        DESCRIPTION
                "Rev V1.2
                - added various parameters.
                - added additional TRAP parameter."

        REVISION "200602230932Z"
        DESCRIPTION
                "Rev V1.1 - PSC 3 V1.60
                - extended dcChargeState with new sepCharge state."

        REVISION "200506031107Z"
        DESCRIPTION
                "Rev V1.0 - PSC 3 V1.5 and older
                - added dcCurrentLimit parameter.
                - renamed module.
                - increased dcSoftwareVersion string size.
                - added recharge state to dcChargeState parameter.
                - added max. number of entries in comment for event history."

 -- 1.3.6.1.4.1.20246.2.1.1.2 --  
 ::= { modules 2 }


-- root for items in the controller MIB module

orionBaseMib OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1 --  
 ::= { orion 1 }

-- conformance area, containing groups and compliance specifications

controllerConfs OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1 --  
 ::= { orionBaseMib 1 }

controllerGroups OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1 --  
 ::= { controllerConfs 1 }

controllerCompl OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.2 --  
 ::= { controllerConfs 2 }

-- sub-tree for objects, and for each functional area

controllerObjects OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2 --  
 ::= { orionBaseMib 2 }

dcSystemInfo OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.1 --  
 ::= { controllerObjects 1 }

dcSystemAlarms OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2 --  
 ::= { controllerObjects 2 }

dcSystemMonitor OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3 --  
 ::= { controllerObjects 3 }

dcRectifier OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4 --  
 ::= { controllerObjects 4 }

dcRectifierFunctions OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6 --  
 ::= { dcRectifier 6 }  
 
  dcEfficiencyCycling OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.1 --  
   ::= { dcRectifierFunctions 1 } 

  dcPowerLimitation OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2 --  
   ::= { dcRectifierFunctions 2 } 

dcBattery OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5 --  
 ::= { controllerObjects 5 }

  dcFloatCharge OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.1 --  
   ::= { dcBattery 1 }

  dcBatteryTest OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2 --  
   ::= { dcBattery 2 }

    dcBatteryTestParameter OBJECT IDENTIFIER 
     -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1 --  
     ::= { dcBatteryTest 1 }
     
    dcBatteryTestResults OBJECT IDENTIFIER 
     -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.2 --  
     ::= { dcBatteryTest 2 }

  dcBatteryParameter OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3 --  
   ::= { dcBattery 3 }   
   
     dcLossOfBackupTime OBJECT IDENTIFIER 
     -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.3 --  
     ::= { dcBatteryParameter 3 }

  dcEqualize OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4 --  
   ::= { dcBattery 4 }

    dcEqualizeParameter OBJECT IDENTIFIER 
     -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4 --  
     ::= { dcEqualize 4 }
                          
  dcBoostCharge OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5 --  
   ::= { dcBattery 5 }

    dcBoostChargeParameter OBJECT IDENTIFIER 
     -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.4 --  
     ::= { dcBoostCharge 4 }
 
  dcSystemVoltageSupervision OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6 --  
   ::= { dcBattery 6 }  
   
  dcEvtCtrlCharge OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.7 --  
   ::= { dcBattery 7 }   

    dcEvtCtrlChargeParameter OBJECT IDENTIFIER 
     -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.7.3 --  
     ::= { dcEvtCtrlCharge 3 }  
     
  dcTempComp OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8 --  
   ::= { dcBattery 8 }   
   
  dcTempSupervision OBJECT IDENTIFIER 
   -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.9 --  
   ::= { dcBattery 9 }   
      
dcInputOutput OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.6 --  
 ::= { controllerObjects 6 }
                                    
dcMisc OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7 --  
 ::= { controllerObjects 7 }

dcConfig OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8 --  
 ::= { controllerObjects 8 }
                                    
dcMeasurement OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9 --  
 ::= { controllerObjects 9 }

dcMeterPanel OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.10 --  
 ::= { controllerObjects 10 }
                                    
-- sub-tree for notifications
controllerEvents OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.3 --  
 ::= { orionBaseMib 3 }

controllerEventObjects OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.3.1 --  
 ::= { controllerEvents 1 }

-- The following OBJECT IDENTIFIER is used to define SNMPv2 notifications
-- that are backward compatible with SNMPv1 traps
controllerEventsV2 OBJECT IDENTIFIER 
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.3.1.0 --  
 ::= { controllerEventObjects 0 }

-- ================================
-- Scalar objects
-- ================================
dcSiteName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..16))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "An administratively-assigned site name for this
                DC-power system."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.1.1 --  
 ::= { dcSystemInfo 1 }

dcSystemName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..16))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "An administratively-assigned system name for this
                DC-power system."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.1.2 --  
 ::= { dcSystemInfo 2 }

dcSystemDateTime OBJECT-TYPE
        SYNTAX DisplayString (SIZE (19))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "ISO 8601 representation of controllerīs local date/time. 
                The value is in the format YYYY-MM-DDThh:mm:ss. 
                An example of a valid string is: '2004-10-04T13:45:00'."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.1.3 --  
 ::= { dcSystemInfo 3 }

dcSoftwareVersion OBJECT-TYPE
        SYNTAX DisplayString (SIZE (10..12))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The controllerīs software version e.g V2.50Build1."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.1.4 --  
 ::= { dcSystemInfo 4 }

dcNumberUrgentAlarms OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Number of currently active urgent alarm sources. A zero 
                value indicates that urgent alarm is not active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.3 --  
 ::= { dcSystemAlarms 3 }

dcNumberNonUrgentAlarms OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Number of currently active non urgent alarm sources. A zero 
                value indicates that non urgent alarm is not active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.4 --  
 ::= { dcSystemAlarms 4 }

dcMainsFailureAlarm OBJECT-TYPE
        SYNTAX INTEGER {
                inactive(1),
                active(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Mains failure alarm."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.5 --  
 ::= { dcSystemAlarms 5 }

dcUrgentAlarmIdentifier OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current unique urgent alarm event identifier. A zero value 
                indicates that urgent alarm is not active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.6 --  
 ::= { dcSystemAlarms 6 }

dcUrgentAlarmValue OBJECT-TYPE
        SYNTAX INTEGER {
                false(1),
                indeterminate(2),  -- deprecated, not used anymore
                true(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current urgent alarm event status that corresponds to the 
                urgent alarm identifier. If the urgent alarm identifier is zero 
                then the alarm value is false."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.7 --  
 ::= { dcSystemAlarms 7 }

dcNonUrgentAlarmIdentifier OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current unique non urgent alarm event identifier. A zero value 
                indicates that non urgent alarm is not active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.8 --  
 ::= { dcSystemAlarms 8 }

dcNonUrgentAlarmValue OBJECT-TYPE
        SYNTAX INTEGER {
                false(1),
                indeterminate(2),  -- deprecated, not used anymore
                true(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current non urgent alarm event status that corresponds to non urgent 
                alarm identifier. If the non urgent alarm identifier is zero then 
                the alarm value is false."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.9 --  
 ::= { dcSystemAlarms 9 }

dcUrgentAlarmName OBJECT-TYPE
    SYNTAX DisplayString (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current alarm name for urgent alarm that corresponds to urgent 
                alarm identifier."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.10 --  
 ::= { dcSystemAlarms 10 }

dcNonUrgentAlarmName OBJECT-TYPE
    SYNTAX DisplayString (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current alarm name for active non urgent alarm that corresponds 
                to non urgent alarm identifier."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.11 --  
 ::= { dcSystemAlarms 11 }

dcNumberCriticalAlarms OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Number of currently active critical alarm sources. A zero 
                value indicates that critical alarm is not active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.13 --  
 ::= { dcSystemAlarms 13 }
 
dcCriticalAlarmIdentifier OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current unique critical alarm event identifier. A zero value 
                indicates that critical alarm is not active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.14 --  
 ::= { dcSystemAlarms 14 }

dcCriticalAlarmValue OBJECT-TYPE
        SYNTAX INTEGER {
                false(1),
                indeterminate(2),  -- deprecated, not used anymore
                true(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current critical alarm event status that corresponds to the 
                critical alarm identifier. If the critical alarm identifier is zero 
                then the alarm value is false."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.15 --  
 ::= { dcSystemAlarms 15 }

dcCriticalAlarmName OBJECT-TYPE
    SYNTAX DisplayString (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current alarm name for active critical alarm that corresponds 
        to critical alarm identifier."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.16 --  
 ::= { dcSystemAlarms 16 }

dcSystemVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The measured system voltage. The max. value 2147483647 
                is used to indicate an invalid value."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.1 --  
 ::= { dcSystemMonitor 1 }

dcLoadCurrent OBJECT-TYPE
        SYNTAX Integer32
        UNITS "100 mA"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The measured load current. The max. value 2147483647 
                is used to indicate an invalid value."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.2 --  
 ::= { dcSystemMonitor 2 }

dcBatteryCurrent OBJECT-TYPE
        SYNTAX Integer32
        UNITS "100 mA"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION           
                "The measured battery current. The max. value 2147483647 
                is used to indicate an invalid value."  
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.3 --  
 ::= { dcSystemMonitor 3 }

dcBatteryTemperature OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The measured battery temperature. The max. value 2147483647 
                is used to indicate an invalid value."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.4 --  
 ::= { dcSystemMonitor 4 }

dcChargeState OBJECT-TYPE
        SYNTAX INTEGER {
                float(1),
                discharge(2),
                equalize(3),
                boost(4),
                battTest(5), 
                recharge(6),
                sepCharge(7),
                evCtrlCharge(8) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Battery charge state."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.5 --  
 ::= { dcSystemMonitor 5 }

dcCurrentLimit OBJECT-TYPE
        SYNTAX INTEGER {
                inactive(1),
                active(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Battery current limit."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.6 --  
 ::= { dcSystemMonitor 6 }

dcRectifierCurrent OBJECT-TYPE
        SYNTAX Integer32
        UNITS "100 mA"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION           
                "Total current of all working rectifier modules.
                The maximum value 2147483647 is used to indicate
                an invalid value."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.7 --  
 ::= { dcSystemMonitor 7 }

dcSystemPower OBJECT-TYPE
        SYNTAX Integer32
        UNITS "1 W"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION           
                "Calculated system power. The maximum value 
                2147483647 is used to indicate an invalid value."       
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.3.8 --  
 ::= { dcSystemMonitor 8 }

-- Rectifier
dcNumberRectifiers OBJECT-TYPE
        SYNTAX Gauge32 (0..128)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The configured number of rectifiers plugged into
                the system. The maximum number of rectifiersi is 128."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.1 --  
 ::= { dcRectifier 1 }

dcNumberRectifiersFailure OBJECT-TYPE
        SYNTAX Gauge32 (0..128)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Number of rectifiers that are not properly working."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.2 --  
 ::= { dcRectifier 2 }

dcNumberRectifiersOkay OBJECT-TYPE
        SYNTAX Gauge32 (0..128)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Number of rectifiers that are properly working."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.3 --  
 ::= { dcRectifier 3 }
                      
-- Rectifier - RectifierFunctions - EfficiencyCycling
dcEfficiencyCyclingEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable efficiency cycling."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.1.1 --  
 ::= { dcEfficiencyCycling 1 } 

dcLimitSwitchingTimes OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable limit switching times."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.1.2 --  
 ::= { dcEfficiencyCycling 2 }
 
dcForceSwitchingOncePerMonth OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable force switching once per month."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.1.3 --  
 ::= { dcEfficiencyCycling 3 } 
 
dcMaximumLoadStep OBJECT-TYPE
        SYNTAX Integer32
        UNITS "1 W"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Maximum load setup."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.1.4 --  
 ::= { dcEfficiencyCycling 4 }
 
dcMinimumLoadStep OBJECT-TYPE
        SYNTAX Integer32
        UNITS "1 W"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Minimum load setup."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.1.5 --  
 ::= { dcEfficiencyCycling 5 } 

-- Battery - FloatCharge                      
dcUsys20 OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Voltage to regulate to at 20°C. If temperature compensation 
                is used, this voltage will vary."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.1.1 --  
 ::= { dcFloatCharge 1 }      
 
                                      
-- Battery - BatteryTest - BatteryTestParameter
dcBatteryTestUsupport OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Support charge voltage for the battery."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.1 --  
 ::= { dcBatteryTestParameter 1 }      

dcBatteryTestDuration OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "minute"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Battery test duration."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.2 --  
 ::= { dcBatteryTestParameter 2 }      
               
dcBatteryTestInterval OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "days"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Minimal time between programmed battery tests as start 
                condition."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.3 --  
 ::= { dcBatteryTestParameter 3 }      
               
dcBatteryTestDischargeCurrent OBJECT-TYPE
        SYNTAX Integer32
        UNITS "100 mA"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Battery discharge current. The maximum value 2147483647 
                is used to indicate an invalid value."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.4 --  
 ::= { dcBatteryTestParameter 4 }      
                               
dcBatteryTestMinDuration OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "minutes"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Minimum battery test duration during which time a battery test 
                is not stopped in case of a voltage below the support voltage or 
                a current difference higher than the specified value defined in 
                Idiff measurement is detected."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.5 --  
 ::= { dcBatteryTestParameter 5 }                              

dcBatteryTestVoltageWithinUfloat OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Battery voltage must be within Ufloat +/- set voltage for a 
                given time (see also dcBatteryTestVoltageWithinUfloatPeriod)
                in order to start a battery test."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.6 --  
 ::= { dcBatteryTestParameter 6 }
 
dcBatteryTestVoltageWithinUfloatPeriod OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "days"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcBatteryTestVoltageWithinUfloat parameter."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.7 --  
 ::= { dcBatteryTestParameter 7 }

dcBatteryTestTempFrom OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Battery temperature must be within temperature range given by
                dcBatteryTestTempFrom and dcBatteryTestTempTo, so that a battery
                test can be started."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.8 --  
 ::= { dcBatteryTestParameter 8 }

dcBatteryTestTempTo OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcBatteryTestTempFrom parameter."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.9 --  
 ::= { dcBatteryTestParameter 9 }

dcBatteryTestIntervalEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable interval. For more details see dcBatteryTestInterval."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.1.10 --  
 ::= { dcBatteryTestParameter 10 } 

dcBatteryTestStartTimeFrom OBJECT-TYPE
        SYNTAX DisplayString (SIZE (8))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Defines start time window for battery test. The possible time window 
                is defined as the range between dcBatteryTestStartTimeFrom and 
                dcBatteryTestStartTimeTo. The value is in the format 'hh:mm:ss'."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.11 --  
 ::= { dcBatteryTestParameter 11 }  
  
dcBatteryTestStartTimeTo OBJECT-TYPE
        SYNTAX DisplayString (SIZE (8))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcBatteryTestStartTimeFrom."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.1.12 --  
 ::= { dcBatteryTestParameter 12 }   
       
-- Battery - BatteryTest - BatteryTestResults
dcBatteryTestDateTime OBJECT-TYPE
        SYNTAX DisplayString (SIZE (19))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "ISO 8601 representation of the last performed battery test. 
                The value is in the format YYYY-MM-DDThh:mm:ss. This parameter 
                is valid only if there is a test result available."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.2.1 --  
 ::= { dcBatteryTestResults 1 }      

dcBatteryTestResult OBJECT-TYPE
        SYNTAX INTEGER {
                none(1),
                failed(2),
                aborted(3),
                loadFailure(4),
                okay(5),
                abortedManual(6),
                abortedEvCtrlCharge(7),
                abortedInhibitEv(8) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Result of last performed battery test."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.2.2 --  
 ::= { dcBatteryTestResults 2 }      

dcBatteryTestEndVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "System voltage at the end of the last performed battery test. 
                The maximum value 2147483647 is used to indicate an invalid 
                value."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.2.3 --  
 ::= { dcBatteryTestResults 3 } 

dcBatteryTestControl OBJECT-TYPE
        SYNTAX INTEGER {
                start(1),
                stop(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Start/stop of battery test. This special charge mode is used 
                to check the capacity of a battery. Please note that a battery 
                test can be started even if the battery is not fully charged. 
                In this case the test result is ambiguous and the set failure 
                event will become active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.3 --  
 ::= { dcBatteryTest 3 } 

dcBatteryTestStatus OBJECT-TYPE
        SYNTAX INTEGER {
                inactive(1),
                starting(2),
                stopping(3),
                constantCurrent(4),
                timeBased(5),
                energyBased(6),
                recovery(7),
                realLoad(8),
                stop(9) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Status of battery test."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.4 --  
 ::= { dcBatteryTest 4 }

dcBatteryTestFailureEvent OBJECT-TYPE
        SYNTAX INTEGER {
                reset(1) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Reset battery test failure event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.5 --  
 ::= { dcBatteryTest 5 }
 
dcBatteryTestType OBJECT-TYPE
        SYNTAX INTEGER {
                none(1),
                constantCurrent(2),
                --timeBased(3),   deprecated --
                --energyBased(4), deprecated --
                realLoad(5) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Battery test type used."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.2.6 --  
 ::= { dcBatteryTest 6 } 
 
-- Battery - BatteryParameter
dcTotalBatteryCapacity OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "100 mAh"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Total battery capacity for all available batteries."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.1 --  
 ::= { dcBatteryParameter 1 }      

-- Battery - BatteryParameter - LossOfBackupTime
dcLossOfBackupTimeEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable loss of backup time functionality."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.3.1 --
 ::= { dcLossOfBackupTime 1 }

dcLossOfBackupTimeStatus OBJECT-TYPE
        SYNTAX INTEGER {
                inactive(1), 
                ok(2), 
                occured(3), 
                fail(4) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Status of loss of backup time functionality."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.3.2 --  
 ::= { dcLossOfBackupTime 2 }
 
dcExpectedBackupTime OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "minutes"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Expected backup time value. Based on the given value for 
                the parameter expected backup time, the corresponding 
                maximum discharge current is calculated."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.3.3 --  
 ::= { dcLossOfBackupTime 3 }
 
-- Battery - Equalize
dcEqualizeControl OBJECT-TYPE
        SYNTAX INTEGER {
                start(1),
                stop(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Start/stop of battery equalize which is a special charge 
                mode that applies a higher voltage to the batteries than 
                the float charge. This ensures that the cells are all 
                equally charged."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.1 --  
 ::= { dcEqualize 1 } 

dcEqualizeStatus OBJECT-TYPE
        SYNTAX INTEGER {
                inactive(1),
                starting(2),
                stopping(3),
                preparing(4),
                cooking(5),
                recovering(6) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current status of battery equalize."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.2 -- 
 ::= { dcEqualize 2 }
    
dcEqualizeEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable equalize."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.3 --  
 ::= { dcEqualize 3 }

-- Equalize - EqualizeParameter
dcEqualizeVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Voltage used for equalize."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.1 --  
 ::= { dcEqualizeParameter 1 }
 
dcEqualizeDuration OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "minutes"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Duration of equalize."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.2 --  
 ::= { dcEqualizeParameter 2 }

dcEqualizeUseBattRoomFanEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable battery room fan during equalize."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.3 --  
 ::= { dcEqualizeParameter 3 }

dcEqualizeLeadTime OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "minutes"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Lead time for equalize."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.4 --  
 ::= { dcEqualizeParameter 4 }

dcEqualizeTimeLag OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "minutes"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Time lag for equalize."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.5 --  
 ::= { dcEqualizeParameter 5 }

dcEqualizeInterval OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "days"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Interval for equalize as start condition."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.6 --  
 ::= { dcEqualizeParameter 6 }

dcEqualizeStartTimeIntervalFrom OBJECT-TYPE
        SYNTAX DisplayString (SIZE (8))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION  
                "Defines start time window for equqlize. The possible time window 
                is defined as the range between dcEqualizeStartTimeIntervalFrom and 
                dcEqualizeStartTimeIntervalTo. The value is in the format 'hh:mm:ss'."               
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.7 --  
 ::= { dcEqualizeParameter 7 }

dcEqualizeStartTimeIntervalTo OBJECT-TYPE
        SYNTAX DisplayString (SIZE (8))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For detail see dcEqualizeStartTimeIntervalFrom."               
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.8 --  
 ::= { dcEqualizeParameter 8 }

dcEqualizeInhibitAfterBoost OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "hours"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Inhibit after boost as start condition."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.4.4.9 --   
 ::= { dcEqualizeParameter 9 }

-- Battery - BoostCharge
dcBoostChargeControl OBJECT-TYPE
        SYNTAX INTEGER {
                start(1),
                stop(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Start/stop of boost charge which is a special charge mode 
                that applies a higher voltage to the batteries than the float 
                charge. This mode is started after a discharge phase to 
                recharge the batteries faster."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.1 --  
 ::= { dcBoostCharge 1 } 

dcBoostChargeStatus OBJECT-TYPE
        SYNTAX INTEGER {
                inactive(1),
                starting(2),
                stopping(3),
                cooking(4),
                recovering(5) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current status of boost charge."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2 -- 
 ::= { dcBoostCharge 2 }

dcBoostChargeType OBJECT-TYPE
        SYNTAX INTEGER {
                none(1),
                currentBased(2),
                timeBased(3),
                energyBased(4) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Boost charge type."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.3 -- 
 ::= { dcBoostCharge 3 }

-- Battery - BoostCharge - BoostChargeParameter
dcBoostChargeVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Voltage used for boost charge."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2.1 --  
 ::= { dcBoostChargeParameter 1 }

dcBoostChargeMaxDuration OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "hours"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Defines the maximum allowed time for boost charge to 
                prevent that the battery is charged forever."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2.2 --  
 ::= { dcBoostChargeParameter 2 }

dcBoostChargeUseBattRoomFanEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable battery room fan during boost charge."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2.3 --  
 ::= { dcBoostChargeParameter 3 }

dcBoostChargeTimeLag OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "minutes"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Time lag used for boost charge."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2.4 --  
 ::= { dcBoostChargeParameter 4 }

dcBoostChargeIstart OBJECT-TYPE
        SYNTAX Integer32
        UNITS "100 mA"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For current based boost charge, the parameters Istart 
                and Istop are the battery current values at which boost charge 
                starts or stops."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2.5 --  
 ::= { dcBoostChargeParameter 5 }

dcBoostChargeIstop OBJECT-TYPE
        SYNTAX Integer32
        UNITS "100 mA"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcBoostChargeIstart."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2.6 --  
 ::= { dcBoostChargeParameter 6 }

dcBoostChargeInhibitTime OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "hours"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "A start condition for all types of boost charge. It defines 
                the time from last boost charge stop to the next acceptable boost 
                charge start."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.5.2.7 --  
 ::= { dcBoostChargeParameter 7 }
     
-- Battery - SystemVoltageSupervision
dcUaMax OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "If the system voltage is outside the range specified by the values 
                UaMin (lower alarm voltage)/UaMax (upper alarm voltage), the 
                system event 'S Ua low'/'S Ua high' is activated. The values for the 
                parameters UaMin and UaMax are not temperature compensated."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.1 --  
 ::= { dcSystemVoltageSupervision 1 }     
     
dcUaMin OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcUaMax."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.2 --  
 ::= { dcSystemVoltageSupervision 2 }

dcUsMax OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "If the voltage is outside the range defined by the parameters UsMin (lower 
                safety voltage)/UsMax (upper safety voltage), the system event 
                'S Us low'/'S Us high' is activated. If temperature compensation is enabled,
                the levels for Us min and / Us max are automatically temperature compensated 
                to correspond to the required system voltage. The parameters are defined 
                at 20°C."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.3 --  
 ::= { dcSystemVoltageSupervision 3 }

dcUsMin OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcUsMax."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.4 --  
 ::= { dcSystemVoltageSupervision 4 }
 
dcBoD OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Voltage threshold for Battery on Discharge alarm."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.5 --  
 ::= { dcSystemVoltageSupervision 5 }

dcHysteresis OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Hysteresis used for Ua and Us."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.6 --  
 ::= { dcSystemVoltageSupervision 6 }

dcSuppressUaLowEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Suppress Ua Low alarm during mains failure."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.7 --  
 ::= { dcSystemVoltageSupervision 7 }

dcSuppressUsLowEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Suppress Us Low alarm during mains failure."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.8 --  
 ::= { dcSystemVoltageSupervision 8 }
 
dcEnableUsTempComp OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Checkbox to enable the automatic temperature compensation for the Us thresholds (Us min, Us max)."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.6.9 --  
 ::= { dcSystemVoltageSupervision 9 }
       
-- Battery - EvtCtrlCharge
dcEvtCtrlChargeStatus OBJECT-TYPE
        SYNTAX INTEGER {
                inactive(1),
                voltageControlled(2),
                noBatteryCharge(3),
                currentLimitation(4) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Event control charge status."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.7.1 --  
 ::= { dcEvtCtrlCharge 1 }

dcEvtCtrlChargeType OBJECT-TYPE
        SYNTAX INTEGER {
                none(1),
                voltageControlled(2),
                noBatteryCharge(3),
                currentLimitation(4) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Selected event control charge type."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.7.2 --  
 ::= { dcEvtCtrlCharge 2 }

dcEvtCtrlChargeVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Voltage used for event control charge."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.7.1.1 --  
 ::= { dcEvtCtrlChargeParameter 1}

dcEvtCtrlChargeTempCompEnabled OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable temperature compensation during event 
                control charge."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.7.1.2 --  
 ::= { dcEvtCtrlChargeParameter 2 }

dcEvtCtrlChargeMaxIBatt OBJECT-TYPE
        SYNTAX Integer32
        UNITS "100 mA"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Max. IBatt used for event control charge."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.7.1.3 --  
 ::= { dcEvtCtrlChargeParameter 3}
 
dcTempCompType OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                linear(2),
                multi-stage(3) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable battery temperature compensation."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.1 --  
 ::= { dcTempComp 1 }  
 
dcSlope OBJECT-TYPE
        SYNTAX Integer32
        UNITS "-1 mV/°C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Temperature compensation coefficient for system voltage."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.2 --  
 ::= { dcTempComp 2 } 
 
dcStartTemp OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Lower limit for the area in which the temperature compensation 
                is active."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.3 --  
 ::= { dcTempComp 3 }  

dcStopTemp OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Upper limit for the area in which the temperature compensation 
                is active."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.4 --  
 ::= { dcTempComp 4 }  
                    
dcMaxVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Upper limit for the area in which the temperature compensation 
                is not controlling the system voltage."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.5 --  
 ::= { dcTempComp 5 }
 
dcLowStopVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The temperature compensation will not control the charging voltage above this parameter at low temperatures."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.6 --  
 ::= { dcTempComp 6 }
 
dcLowStartTemp OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "High temperature limit of the lower range."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.7 --  
 ::= { dcTempComp 7 }  
 
dcLowTempSlope OBJECT-TYPE
        SYNTAX Integer32
        UNITS "-1 mV/°C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Compensation factor applied inside the low range."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.8 --  
 ::= { dcTempComp 8 } 
 
dcHighStartTemp OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The low temperature limit of the higher range."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.9 --  
 ::= { dcTempComp 9 } 
 
dcHighTempSlope OBJECT-TYPE
        SYNTAX Integer32
        UNITS "-1 mV/°C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Compensation factor applied inside the high range."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.10 --  
 ::= { dcTempComp 10 } 
 
dcHighStopVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The temperature compensation will not control the charging voltage below this parameter at high temperatures."      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.11 --  
 ::= { dcTempComp 11 }
 
dcRunawayTemp OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "A threshold for detecting thermal runaway of the battery."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.12 --  
 ::= { dcTempComp 12 } 
 
dcRunawayVoltage OBJECT-TYPE
        SYNTAX Integer32
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Charging voltage while Runaway Temp has been exceeded."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.8.13 --  
 ::= { dcTempComp 13 } 
 
 dcHighTemp OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Temperature threshold for high battery temperature alarm 10°C ... 70°C"
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.9.1 --  
 ::= { dcTempSupervision 1 }  
 
 dcHighTempHyst OBJECT-TYPE
        SYNTAX Integer32
        UNITS "0.1 °C"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Hysteresis for the High Temp 1°C ... 70°C"      
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.9.2 --  
 ::= { dcTempSupervision 2 }  

-- Misc
dcFileProcessingStatus OBJECT-TYPE
        SYNTAX INTEGER {
                idle(1),
                inProgress(2),
                successful(3),
                error(4),
                unknown(5) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "File processing status for software and setup up/downloads."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7.2 -- 
 ::= { dcMisc 2 }
 
dcResendActiveAlarmTraps OBJECT-TYPE
        SYNTAX INTEGER {
                resend(1) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Resend all active Urgent, Non Urgent, and Critical Alarm Traps."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7.4 --  
 ::= { dcMisc 4 }

-- Event Processing Table 
dcEventProcessingEventSelected OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Reference to dcEventProcessingEventIndex in order to select
                a specific event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.3 --  
 ::= { dcConfig 3 }
                                                   
-- ====================================================================
-- Event History table
-- ====================================================================
dcEventHistoryTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcEventHistoryEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Controllerīs event history table that shows the content of the
                default log file."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.1 --  
 ::= { dcSystemAlarms 1 }

dcEventHistoryEntry OBJECT-TYPE
        SYNTAX DcEventHistoryEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular Event History entry."
        INDEX { dcEventHistoryIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.1.1 --  
 ::= { dcEventHistoryTable 1 }

DcEventHistoryEntry ::= SEQUENCE {

        dcEventHistoryIndex     Integer32,
        dcEventHistoryTimestamp DisplayString,
        dcEventHistoryMessage   DisplayString }

dcEventHistoryIndex OBJECT-TYPE
        SYNTAX Integer32 (1..10000)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.1.1.1 --  
 ::= { dcEventHistoryEntry 1 }

dcEventHistoryTimestamp OBJECT-TYPE
        SYNTAX DisplayString (SIZE (19))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "ISO8601 timestamp representation of a particular entry
                in the form YYYY-MM-DDThh:mm:ss."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.1.1.2 --  
 ::= { dcEventHistoryEntry 2 }

dcEventHistoryMessage OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Event message of a particular entry."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.1.1.3 --  
 ::= { dcEventHistoryEntry 3 }


-- ====================================================================
-- Active Alarm table
-- ====================================================================
dcAlarmTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcAlarmEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table that shows all currently active alarm sources 
                causing urgent or non-urgent alarm(s)."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.2 --  
 ::= { dcSystemAlarms 2 }

dcAlarmEntry OBJECT-TYPE
        SYNTAX DcAlarmEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular active alarm source entry."
        INDEX { dcAlarmIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.2.1 --  
 ::= { dcAlarmTable 1 }

DcAlarmEntry ::= SEQUENCE {
        dcAlarmIndex           Integer32,
        dcAlarmEventCategory   INTEGER,
        dcAlarmEventName       DisplayString,
        dcAlarmEventIdentifier Gauge32, 
        dcAlarmEventValue      INTEGER }

dcAlarmIndex OBJECT-TYPE
        SYNTAX Integer32 (1..16)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.2.1.1 --  
 ::= { dcAlarmEntry 1 }

dcAlarmEventCategory OBJECT-TYPE
        SYNTAX INTEGER {
                unknown(1),
                urgent(2),
                nonUrgent(3),
                critical(4) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Specifies the type of alarm source."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.2.1.2 --  
 ::= { dcAlarmEntry 2 }

dcAlarmEventName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Name of a particular alarm source entry."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.2.1.3 --  
 ::= { dcAlarmEntry 3 }

dcAlarmEventIdentifier OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unique alarm event identifier."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.2.1.4 --  
 ::= {  dcAlarmEntry 4 }

dcAlarmEventValue OBJECT-TYPE
        SYNTAX INTEGER {
                false(1),
                -- indeterminate(2),   deprecated --
                true(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Event status that corresponds to alarm event identifier."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.2.1.5 --  
 ::= {  dcAlarmEntry 5 }

-- ====================================================================
-- Generic Alarm table
-- ====================================================================
dcGenericAlarmTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcGenericAlarmEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table that shows ten alarm event assignments that can be 
                 configured via WEB interface."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.12 --  
 ::= { dcSystemAlarms 12 }

dcGenericAlarmEntry OBJECT-TYPE
        SYNTAX DcGenericAlarmEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular generic alarm entry."
        INDEX { dcGenericAlarmIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.12.1 --  
 ::= { dcGenericAlarmTable 1 }

DcGenericAlarmEntry ::= SEQUENCE {
        dcGenericAlarmIndex           Integer32,
        dcGenericAlarmEventName       DisplayString,
        dcGenericAlarmEventIdentifier Gauge32, 
        dcGenericAlarmEventValue      INTEGER }

dcGenericAlarmIndex OBJECT-TYPE
        SYNTAX Integer32 (1..16)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.12.1.1 --  
 ::= { dcGenericAlarmEntry 1 }
                                                
dcGenericAlarmEventName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Plain text name of the assigned alarm event. Empty if not
                configured."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.12.1.2 --  
 ::= { dcGenericAlarmEntry 2 }

dcGenericAlarmEventIdentifier OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unique numeric identifier of the assigned alarm event. Zero
                if not configured."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.12.1.3 --  
 ::= {  dcGenericAlarmEntry 3 }

dcGenericAlarmEventValue OBJECT-TYPE
        SYNTAX INTEGER {
                false(1),
                true(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Current value of the assigned alarm event. Value is false if
                not configured."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.2.12.1.4 --  
 ::= {  dcGenericAlarmEntry 4 }      

-- ====================================================================
-- Rectifier table
-- ====================================================================
dcRectifierTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcRectifierEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table that shows all currently active rectifier modules."
-- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.4 -- 
 ::= { dcRectifier 4 }

dcRectifierEntry OBJECT-TYPE
        SYNTAX DcRectifierEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular rectifier entry."
        INDEX { dcRectifierIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.4.1 --  
 ::= { dcRectifierTable 1 }

DcRectifierEntry ::= SEQUENCE {
        dcRectifierIndex        Integer32, 
        dcRectifierIdentifier   DisplayString, 
        dcRectifierStatus       INTEGER }

dcRectifierIndex OBJECT-TYPE
        SYNTAX Integer32 (1..128)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.4.1.1 --  
 ::= { dcRectifierEntry 1 }
                               
dcRectifierIdentifier OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..16))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unique rectifier identifier. If positioning active the 
                position number scheme is used otherwise the rectifier 
                instance is used to identify a rectifier."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.4.1.2 --  
 ::= { dcRectifierEntry 2 }

dcRectifierStatus OBJECT-TYPE
        SYNTAX INTEGER {
                unknown(1),
                off(2),
                on(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Specifies status of rectifiers."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.4.1.3 --  
 ::= { dcRectifierEntry 3 }
    
-- ====================================================================
-- Rectifier Group table
-- ====================================================================
dcRectifierGroupTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcRectifierGroupEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table that shows all available rectifier groups."
-- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5 -- 
 ::= { dcRectifier 5 }

dcRectifierGroupEntry OBJECT-TYPE
        SYNTAX DcRectifierGroupEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular rectifier group entry."
        INDEX { dcRectifierGroupIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1 --  
 ::= { dcRectifierGroupTable 1 }

DcRectifierGroupEntry ::= SEQUENCE {
        dcRectifierGroupIndex Integer32, 
        dcRectifierGroupName DisplayString, 
        dcRectifierGroupRectifierType INTEGER,
        dcRectifierGroupDefaultVoltage Integer32,
        dcRectifierGroupDefaultCurrentLimit Integer32,
        dcRectifierGroupDefaultPowerLimit Integer32,
        dcRectifierGroupInputLowOff Integer32,
        dcRectifierGroupInputLowOn Integer32,
        dcRectifierGroupStartupVoltage Integer32,
        dcRectifierGroupStartupCurrentLimit Integer32,
        dcRectifierGroupStartupPowerLimit Integer32,
        dcRectifierGroupStartupTimeLimit Gauge32,
        dcRectifierGroupPowerupDelay Gauge32,
        dcRectifierGroupPowerupTime Gauge32,
        dcRectifierGroupUmaxOff Integer32 }

dcRectifierGroupIndex OBJECT-TYPE
        SYNTAX Integer32 (1..1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.1 --  
 ::= { dcRectifierGroupEntry 1 }
                               
dcRectifierGroupName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..16))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Rectifier group name to identify an individual device 
                parameter set."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.2 --  
 ::= { dcRectifierGroupEntry 2 }

dcRectifierGroupRectifierType OBJECT-TYPE
        SYNTAX INTEGER {
                unknown48V(1), 
                fR48V2000W(2), 
                dPR1200B48(3), 
                dPR1500B48(4), 
                dPR600B48(5),
                dPR7200B48(6),
                fR48to60V2000W(7),
                unknown24V(8),
                unknown60V(9),
                dPR600B60(10),
                dPR3500B48(11),
                dPR3500B24(12),
                dPR300B48(13),
                dPR1600B48(14),
                dPR2700B48(15),
                dPR2400B48(16),
                dPR4000B48(17),
                dPR2900B48(18),
                dPR4000B48to60(19),
                dPR850B48(20),
                dPR2000B48(21) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Rectifier type defined for this group."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.3 --  
 ::= { dcRectifierGroupEntry 3 }

dcRectifierGroupDefaultVoltage OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "This default voltage is used by rectifiers when there 
                is no connection to PSC 3."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.4 --  
 ::= { dcRectifierGroupEntry 4 }
 
dcRectifierGroupDefaultCurrentLimit OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "100 mA"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "This default current limit is used by rectifiers when there 
                is no connection to PSC 3."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.5 --  
 ::= { dcRectifierGroupEntry 5 }

dcRectifierGroupDefaultPowerLimit OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "1 W"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "This default power limit is used by rectifiers when there 
                is no connection to PSC 3."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.6 --  
 ::= { dcRectifierGroupEntry 6 }
 
dcRectifierGroupInputLowOff OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Threshold for low AC input voltage. It can is used to 
                adjust the behaviour of the power system to the available 
                AC network limitation."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.7 --  
 ::= { dcRectifierGroupEntry 7 }
    
dcRectifierGroupInputLowOn OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcRectifierGroupInputLowOff."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.8 --  
 ::= { dcRectifierGroupEntry 8 }

dcRectifierGroupStartupVoltage OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Startup parameters are the values that rectifiers use 
                during the start-up phase. These parameters allow starting 
                the system smoothly after a mains failure even on a 
                discharged battery and even without PSC 3."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.9 --  
 ::= { dcRectifierGroupEntry 9 }

dcRectifierGroupStartupCurrentLimit OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "100 mA"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcRectifierGroupStartupVoltage."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.10 --  
 ::= { dcRectifierGroupEntry 10 }

dcRectifierGroupStartupPowerLimit OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "1 W"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcRectifierGroupStartupVoltage."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.11 --  
 ::= { dcRectifierGroupEntry 11 }
 
dcRectifierGroupStartupTimeLimit OBJECT-TYPE
        SYNTAX Gauge32 
        UNITS "10 ms"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "For details see dcRectifierGroupStartupVoltage."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.12 --  
 ::= { dcRectifierGroupEntry 12 }
 
dcRectifierGroupPowerupDelay OBJECT-TYPE
        SYNTAX Gauge32 
        UNITS "10 ms"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "This parameter is used after a mains failure to 
                delay the start-up of all rectifiers."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.13 --  
 ::= { dcRectifierGroupEntry 13 }

dcRectifierGroupPowerupTime OBJECT-TYPE
        SYNTAX Gauge32 
        UNITS "10 ms"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "This parameter used after a mains failure and allows 
                defining a time within all rectifiers needs to start-up 
                one after another."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.14 -- 
 ::= { dcRectifierGroupEntry 14 }      
 
dcRectifierGroupUmaxOff OBJECT-TYPE
        SYNTAX Integer32 
        UNITS "10 mV"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Overvoltage protection value."
                
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.5.1.15 -- 
 ::= { dcRectifierGroupEntry 15 }

-- ====================================================================
-- Rectifier Power Limitation table
-- ====================================================================
dcPowerLimitationTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcPowerLimitationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table that shows parameters of the available power limitation
                 functions."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2 --   
 ::= { dcPowerLimitation 1 }

dcPowerLimitationEntry OBJECT-TYPE
        SYNTAX DcPowerLimitationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular power limitation entry."
        INDEX { dcPowerLimitationIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2.1 --  
 ::= { dcPowerLimitationTable 1 }
 
DcPowerLimitationEntry ::= SEQUENCE {
        dcPowerLimitationIndex     Integer32,
        dcPowerLimitationEventName DisplayString,
        dcPowerLimitationStatus    INTEGER,
        dcPowerLimitationType      INTEGER,
        dcPowerLimitationLimit     Integer32,
        dcPowerLimitationNoBatteryDischarge INTEGER }

dcPowerLimitationIndex OBJECT-TYPE
        SYNTAX Integer32 (1..16)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2.1.1 --  
 ::= { dcPowerLimitationEntry 1 }

dcPowerLimitationEventName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..35))        
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Name of the power limitation event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2.1.2 --
 ::= { dcPowerLimitationEntry 2 }

dcPowerLimitationStatus OBJECT-TYPE
        SYNTAX INTEGER {
                disabled(1), 
                inactive(2), 
                powerLimit(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Status of power limitation."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2.1.3 --  
 ::= { dcPowerLimitationEntry 3 } 

dcPowerLimitationType OBJECT-TYPE
        SYNTAX INTEGER {
                dynamic(1), 
                fixedLimit(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Power limitation type."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2.1.4 --  
 ::= { dcPowerLimitationEntry 4 } 
 
dcPowerLimitationLimit OBJECT-TYPE
        SYNTAX Integer32        
        UNITS "1 W"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Limit used for power limitation."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2.1.5 --  
 ::= { dcPowerLimitationEntry 5 }
 
dcPowerLimitationNoBatteryDischarge OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Enable/disable no battery discharge during power limitation."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.4.6.2.1.6 --  
 ::= { dcPowerLimitationEntry 6 }
 
-- ====================================================================
-- BatteryString table
-- ====================================================================
dcBatteryStringTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcBatteryStringEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table that shows parameters of the available battery strings."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.2 --   
 ::= { dcBatteryParameter 2 }

dcBatteryStringEntry OBJECT-TYPE
        SYNTAX DcBatteryStringEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular battery string entry."
        INDEX { dcBatteryStringIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.2.1 --  
 ::= { dcBatteryStringTable 1 }

DcBatteryStringEntry ::= SEQUENCE {
        dcBatteryStringIndex    Integer32,
        dcBatteryStringName     DisplayString,
        dcBatteryStringMaxIBatt Integer32,
        dcBatteryStringCapacity Gauge32 }

dcBatteryStringIndex OBJECT-TYPE
        SYNTAX Integer32 (1..16)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.2.1.1 --  
 ::= { dcBatteryStringEntry 1 }
 
dcBatteryStringName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..16))        
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Name of the battery string."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.2.1.2 --
 ::= { dcBatteryStringEntry 2 }

dcBatteryStringMaxIBatt OBJECT-TYPE
        SYNTAX Integer32        
        UNITS "100 mA"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Maximum battery charging current for this string. This 
                parameter can be set individually for each battery. 
                PSC 3 then regulates the system voltage such that the maximum 
                battery charging current of each battery is respected."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.2.1.3 --  
 ::= { dcBatteryStringEntry 3 }

dcBatteryStringCapacity OBJECT-TYPE
        SYNTAX Gauge32        
        UNITS "100 mAh"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Capacity of battery can be defined individually. It is used 
                to calculate the expected backup time of the system."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.5.3.2.1.4 --  
 ::= { dcBatteryStringEntry 4 }
                  
-- ====================================================================
-- Control Event table
-- ====================================================================
dcControlEventTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcControlEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table that shows ten output event assignments that can be 
                 configured via WEB interface."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.6.1 --   
 ::= { dcInputOutput 1 }

dcControlEventEntry OBJECT-TYPE
        SYNTAX DcControlEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular generic output entry."
        INDEX { dcControlEventIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.6.1.1 --  
 ::= { dcControlEventTable 1 }

DcControlEventEntry ::= SEQUENCE {
        dcControlEventIndex      Integer32,
        dcControlEventName       DisplayString,
        dcControlEventIdentifier Gauge32, 
        dcControlEventValue      INTEGER }

dcControlEventIndex OBJECT-TYPE
        SYNTAX Integer32 (1..16)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.6.1.1.1 --  
 ::= { dcControlEventEntry 1 }

dcControlEventName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Plain text name of the assigned control event. Empty if not 
                configure."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.6.1.1.2 --  
 ::= { dcControlEventEntry 2 }

dcControlEventIdentifier OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unique numeric identifier of the assigned control event. Zero
                if not configured."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.6.1.1.3 --  
 ::= {  dcControlEventEntry 3 }

dcControlEventValue OBJECT-TYPE
        SYNTAX INTEGER {
                false(1),
                true(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Current value of the assigned control event. Value is false if
                not configured."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.6.1.1.4 --  
 ::= {  dcControlEventEntry 4 }      
        
-- ====================================================================
-- Trap Destinations table
-- ====================================================================
dcTrapDestinationTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcTrapDestinationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Trap table that shows all configured trap destinations."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7.1 --  
 ::= { dcMisc 1 }

dcTrapDestinationEntry OBJECT-TYPE
        SYNTAX DcTrapDestinationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular trap destination entry."
        INDEX { dcTrapDestinationIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7.1.1 --  
 ::= { dcTrapDestinationTable 1 }

DcTrapDestinationEntry ::= SEQUENCE {
        dcTrapDestinationIndex      Integer32,
        dcTrapDestinationIp         IpAddress,   
        dcTrapDestinationPort       Gauge32 }

dcTrapDestinationIndex OBJECT-TYPE
        SYNTAX Integer32 (1..10)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7.1.1.1 --  
 ::= { dcTrapDestinationEntry 1 }

dcTrapDestinationIp OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "IP address of the trap destination. Value is 0.0.0.0 if IP
                address is not configured."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7.1.1.2 --  
 ::= { dcTrapDestinationEntry 2 }

dcTrapDestinationPort OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Port number of the trap destination. By default port 162
                is used."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.7.1.1.3 --  
 ::= {  dcTrapDestinationEntry 3 }
   
-- ====================================================================
-- Default Log Config table
-- ====================================================================
dcDefaultLogEventTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcDefaultLogEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Event config table for default log."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.1 --  
 ::= { dcConfig 1 }

dcDefaultLogEventEntry OBJECT-TYPE
        SYNTAX DcDefaultLogEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular event entry."
        INDEX { dcDefaultLogEventIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.1.1 --  
 ::= { dcDefaultLogEventTable 1 }

DcDefaultLogEventEntry ::= SEQUENCE {
        dcDefaultLogEventIndex  Integer32,
        dcDefaultLogEventName   DisplayString,   
        dcDefaultLogEventLogged INTEGER }

dcDefaultLogEventIndex OBJECT-TYPE
        SYNTAX Integer32 (0..1000)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.1.1.1 --  
 ::= { dcDefaultLogEventEntry 1 }

dcDefaultLogEventName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Plain text name of the event that can be logged."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.1.1.2 --  
 ::= { dcDefaultLogEventEntry 2 }

dcDefaultLogEventLogged OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "If yes then this event is logged otherwise not."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.1.1.3 --  
 ::= {  dcDefaultLogEventEntry 3 }

-- ====================================================================
-- Event Processing Config table
-- ====================================================================
dcEventProcessingEventTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcEventProcessingEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Event config table for event ORs."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.2 --  
 ::= { dcConfig 2 }

dcEventProcessingEventEntry OBJECT-TYPE
        SYNTAX DcEventProcessingEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular event entry."
        INDEX { dcEventProcessingEventIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.2.1 --  
 ::= { dcEventProcessingEventTable 1 }

DcEventProcessingEventEntry ::= SEQUENCE {
        dcEventProcessingEventIndex  Integer32,
        dcEventProcessingEventName   DisplayString,   
        dcEventProcessingEventAssigned INTEGER,
        dcEventProcessingEventType INTEGER }

dcEventProcessingEventIndex OBJECT-TYPE
        SYNTAX Integer32 (0..1000)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.2.1.1 --  
 ::= { dcEventProcessingEventEntry 1 }

dcEventProcessingEventName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..35))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Plain text name of the input event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.2.1.2 --  
 ::= { dcEventProcessingEventEntry 2 }

dcEventProcessingEventAssigned OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "If yes then the input event is assigned to the selected 
                event. Please note, that it is only possible to change 
                assignment of event ORs."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.2.1.3 --  
 ::= {  dcEventProcessingEventEntry 3 }

dcEventProcessingEventType OBJECT-TYPE
        SYNTAX INTEGER {
                unknown(1),
                eventOR(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Type of the input event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.2.1.4 --  
 ::= {  dcEventProcessingEventEntry 4 }

-- ====================================================================
-- LVD Config table
-- ====================================================================
dcLvdTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcLvdEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table lists all available LVDs."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.4 --  
 ::= { dcConfig 4 }

dcLvdEntry OBJECT-TYPE
        SYNTAX DcLvdEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular LVD entry."
        INDEX { dcLvdIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.4.1 --  
 ::= { dcLvdTable 1 }

DcLvdEntry ::= SEQUENCE {
        dcLvdIndex Integer32,
        dcLvdName DisplayString,   
        dcLvdDisconnectDelay DisplayString }

dcLvdIndex OBJECT-TYPE
        SYNTAX Integer32 (1..96)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.4.1.1 --  
 ::= { dcLvdEntry 1 }

dcLvdName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..16))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Name of the LVD."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.4.1.2 --  
 ::= { dcLvdEntry 2 }

dcLvdDisconnectDelay OBJECT-TYPE
        SYNTAX DisplayString (SIZE (8))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Time delay from the activation of the source event, after 
                which the LVD event is switched. The value is in the format 
                'hh:mm:ss'."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.8.4.1.3 -- 
 ::= {  dcLvdEntry 3 }

-- ====================================================================
-- Measurement table
-- ====================================================================
dcMeasurementTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcMeasurementEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table lists all available measurements."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9.1 --    
 ::= { dcMeasurement 1 }

dcMeasurementEntry OBJECT-TYPE
        SYNTAX DcMeasurementEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular measurement entry."
        INDEX { dcMeasurementIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9.1.1 -- 
 ::= { dcMeasurementTable 1 }

DcMeasurementEntry ::= SEQUENCE {
        dcMeasurementIndex Integer32,
        dcMeasurementName DisplayString,
        dcMeasurementValue Integer32, 
        dcMeasurementScaleFactor Integer32,
        dcMeasurementUnit INTEGER }

dcMeasurementIndex OBJECT-TYPE
        SYNTAX Integer32 (1..500)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9.1.1.1 --  
 ::= { dcMeasurementEntry 1 }

dcMeasurementName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..16))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Name of the measurement."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9.1.1.2 --  
 ::= { dcMeasurementEntry 2 }

dcMeasurementValue OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unscaled calibrated value of the measurement."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9.1.1.3 --  
 ::= { dcMeasurementEntry 3 }     
 
dcMeasurementScaleFactor OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Scale factor as power of 10 to be multiplied with measurement value."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9.1.1.4 --  
 ::= { dcMeasurementEntry 4 }
 
dcMeasurementUnit OBJECT-TYPE
        SYNTAX INTEGER {
                unknown(1), 
                none(2),
                voltDC(3),
                voltAC(4),
                ampere(5),
                ampereHour(6),
                degreeCelsius(7),
                temperatureCoefficient(8),
                watt(9),
                wattHour(10),
                seconds(11),
                percent(12),
                hertz(13),
                voltAmpere(14),
                voltAmpereReactive(15), 
                voltAmpereReactiveHour(16) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unit of the measurement."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.9.1.1.5 --  
 ::= { dcMeasurementEntry 5 }

-- ====================================================================
-- Meter Panel Event table
-- ====================================================================
dcMeterPanelEventTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DcMeterPanelEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table lists all available meter panel events."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.10.1 --    
 ::= { dcMeterPanel 1 }

dcMeterPanelEventEntry OBJECT-TYPE
        SYNTAX DcMeterPanelEventEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "A particular meter panel event entry."
        INDEX { dcMeterPanelEventIndex }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.10.1.1 -- 
 ::= { dcMeterPanelEventTable 1 }

DcMeterPanelEventEntry ::= SEQUENCE {
        dcMeterPanelEventIndex Integer32,
        dcMeterPanelEventName DisplayString,
        dcMeterPanelEventValue INTEGER,
        dcMeterPanelEventHourMeterValue Gauge32 }

dcMeterPanelEventIndex OBJECT-TYPE
        SYNTAX Integer32 (1..128)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Table index."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.10.1.1.1 --  
 ::= { dcMeterPanelEventEntry 1 }

dcMeterPanelEventName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..16))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Name of the event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.10.1.1.2 --  
 ::= { dcMeterPanelEventEntry 2 }
                                       
dcMeterPanelEventValue OBJECT-TYPE
        SYNTAX INTEGER {
                false(1),
                indeterminate(2),
                true(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Value of the event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.10.1.1.3 --  
 ::= { dcMeterPanelEventEntry 3 }     

dcMeterPanelEventHourMeterValue OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "hours"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Value of the hour meter event."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.2.10.1.1.4 --  
 ::= { dcMeterPanelEventEntry 4 } 

-- ====================================================================
-- Notifications
-- ====================================================================
systemNonUrgentAlarm NOTIFICATION-TYPE
        OBJECTS {
                dcSystemDateTime,
                dcNumberNonUrgentAlarms,
                dcNonUrgentAlarmIdentifier,
                dcNonUrgentAlarmValue,
                dcNonUrgentAlarmName }
        STATUS current
        DESCRIPTION
                "The controller reports that one or more elements have changed
                into none urgent alarm state."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.3.1.0.1 --  
 ::= { controllerEventsV2 1 }

systemUrgentAlarm NOTIFICATION-TYPE
        OBJECTS {                        
                dcSystemDateTime,
                dcNumberUrgentAlarms,
                dcUrgentAlarmIdentifier,
                dcUrgentAlarmValue,
                dcUrgentAlarmName }
        STATUS current
        DESCRIPTION
                "The controller reports that one or more elements have changed
                into urgent alarm state."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.3.1.0.2 --  
 ::= { controllerEventsV2 2 }

systemCriticalAlarm NOTIFICATION-TYPE
        OBJECTS {
                dcSystemDateTime,
                dcNumberCriticalAlarms,
                dcCriticalAlarmIdentifier,
                dcCriticalAlarmValue,
                dcCriticalAlarmName }
        STATUS current
        DESCRIPTION
                "The controller reports that one or more elements have changed
                into critical alarm state."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.3.1.0.3 --  
 ::= { controllerEventsV2 3 }
                                        
-- ====================================================================
-- Conformance area, containing groups and compliance specifications
-- ====================================================================
systemInfoGroup OBJECT-GROUP
        OBJECTS {
                dcSiteName,
                dcSystemName,
                dcSystemDateTime,
                dcSoftwareVersion }
        STATUS current
        DESCRIPTION
                "The collection of system info scalar objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.1 --  
 ::= { controllerGroups 1 }

systemAlarmGroup OBJECT-GROUP
        OBJECTS {
                dcNumberUrgentAlarms,
                dcNumberNonUrgentAlarms,
                dcMainsFailureAlarm,
                dcUrgentAlarmIdentifier,
                dcUrgentAlarmValue,
                dcNonUrgentAlarmIdentifier,
                dcNonUrgentAlarmValue,
                dcUrgentAlarmName,
                dcNonUrgentAlarmName,
                dcNumberCriticalAlarms,
                dcCriticalAlarmIdentifier,
                dcCriticalAlarmValue,
                dcCriticalAlarmName }
        STATUS current
        DESCRIPTION
                "The collection of system alarm scalar objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.2 --  
 ::= { controllerGroups 2 }

systemMonitorGroup OBJECT-GROUP
        OBJECTS {
                dcSystemVoltage,
                dcLoadCurrent,
                dcBatteryCurrent,
                dcBatteryTemperature,
                dcChargeState,
                dcCurrentLimit,
                dcRectifierCurrent,
                dcSystemPower }
        STATUS current
        DESCRIPTION
                "The collection of system monitor scalar objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.3 --  
 ::= { controllerGroups 3 }

rectifierGroup OBJECT-GROUP
        OBJECTS {
                dcNumberRectifiers,
                dcNumberRectifiersFailure,
                dcNumberRectifiersOkay,
                dcEfficiencyCyclingEnabled,
                dcLimitSwitchingTimes,
                dcForceSwitchingOncePerMonth,
                dcMaximumLoadStep,
                dcMinimumLoadStep }
        STATUS current
        DESCRIPTION
                "The collection of rectifier scalar objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.4 --  
 ::= { controllerGroups 4 }

eventHistoryTableGroup OBJECT-GROUP
        OBJECTS {
                dcEventHistoryTimestamp,
                dcEventHistoryMessage }
        STATUS current
        DESCRIPTION
                "The collection of event history table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.5 --  
 ::= { controllerGroups 5 }

alarmTableGroup OBJECT-GROUP
        OBJECTS {
                dcAlarmEventCategory,
                dcAlarmEventName,
                dcAlarmEventIdentifier,
                dcAlarmEventValue }
        STATUS current
        DESCRIPTION
                "The collection of alarm table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.6 --  
 ::= { controllerGroups 6 }

rectifierTableGroup OBJECT-GROUP
        OBJECTS {
                dcRectifierIdentifier,
                dcRectifierStatus }
        STATUS current
        DESCRIPTION
                "The collection of rectifier table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.7 --  
 ::= { controllerGroups 7 }

notificationsGroup NOTIFICATION-GROUP
        NOTIFICATIONS {
                systemNonUrgentAlarm,
                systemUrgentAlarm,
                systemCriticalAlarm }
        STATUS current
        DESCRIPTION
                "The group of all controller notifications."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.8 --  
 ::= { controllerGroups 8 }   
 
genericAlarmTableGroup OBJECT-GROUP
        OBJECTS {
                dcGenericAlarmEventIdentifier,
                dcGenericAlarmEventName,
                dcGenericAlarmEventValue }
        STATUS current
        DESCRIPTION
                "Assignment of events to alarm table entries."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.9 --  
 ::= { controllerGroups 9 }        
 
batteryGroup OBJECT-GROUP
        OBJECTS {
            dcUsys20,
            dcTempCompType,
            dcSlope,
            dcStartTemp,
            dcStopTemp,
            dcMaxVoltage,
            dcLowStopVoltage,
            dcLowStartTemp,
            dcLowTempSlope,
            dcHighStartTemp,
            dcHighTempSlope,
            dcHighStopVoltage,
            dcRunawayTemp,
            dcRunawayVoltage,
            dcBatteryTestUsupport,
            dcBatteryTestDuration,
            dcBatteryTestInterval,
            dcBatteryTestDischargeCurrent,
            dcBatteryTestMinDuration,
            dcBatteryTestVoltageWithinUfloat,
            dcBatteryTestVoltageWithinUfloatPeriod,
            dcBatteryTestTempFrom,
            dcBatteryTestTempTo,
            dcBatteryTestIntervalEnabled,
            dcBatteryTestStartTimeFrom,
            dcBatteryTestStartTimeTo,
            dcBatteryTestDateTime,
            dcBatteryTestResult,
            dcBatteryTestEndVoltage,
            dcBatteryTestControl,
            dcBatteryTestStatus,
            dcBatteryTestFailureEvent,
            dcBatteryTestType,
            dcTotalBatteryCapacity, 
            dcLossOfBackupTimeEnabled,
            dcLossOfBackupTimeStatus,
            dcExpectedBackupTime,
            dcEqualizeControl,
            dcEqualizeStatus,
            dcEqualizeEnabled,
            dcEqualizeVoltage,
            dcEqualizeDuration,
            dcEqualizeUseBattRoomFanEnabled,
            dcEqualizeLeadTime,
            dcEqualizeTimeLag,
            dcEqualizeInterval,
            dcEqualizeStartTimeIntervalFrom,
            dcEqualizeStartTimeIntervalTo,
            dcEqualizeInhibitAfterBoost,
            dcBoostChargeControl,
            dcBoostChargeStatus,
            dcBoostChargeType,
            dcBoostChargeVoltage,
            dcBoostChargeMaxDuration,
            dcBoostChargeUseBattRoomFanEnabled,
            dcBoostChargeTimeLag,
            dcBoostChargeIstart,
            dcBoostChargeIstop,
            dcBoostChargeInhibitTime,
            dcUaMax,
            dcUaMin,
            dcUsMax,
            dcUsMin,
            dcBoD,
            dcHysteresis,
            dcSuppressUaLowEnabled,
            dcSuppressUsLowEnabled,
            dcEnableUsTempComp,
            dcEvtCtrlChargeStatus,
            dcEvtCtrlChargeType,
            dcEvtCtrlChargeVoltage,
            dcEvtCtrlChargeTempCompEnabled,
            dcEvtCtrlChargeMaxIBatt,
            dcHighTemp,
            dcHighTempHyst }
        STATUS current
        DESCRIPTION
                "The collection of battery scalar objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.10 --  
 ::= { controllerGroups 10 }
                                      
controlEventTableGroup
  OBJECT-GROUP
        OBJECTS {
                dcControlEventName,
                dcControlEventIdentifier,
                dcControlEventValue }
        STATUS current
        DESCRIPTION
                "Assignment of control events to table entries."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.11 --  
 ::= { controllerGroups 11 }
                                   
trapDestinationTableGroup  
  OBJECT-GROUP
        OBJECTS {
                dcTrapDestinationIp,
                dcTrapDestinationPort }
        STATUS current
        DESCRIPTION
                "Trap destionation table."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.12 --  
 ::= { controllerGroups 12 }
       
miscGroup OBJECT-GROUP
        OBJECTS {
                dcFileProcessingStatus,
                dcResendActiveAlarmTraps }
        STATUS current
        DESCRIPTION
                "The collection of miscellaneous objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.13 --  
 ::= { controllerGroups 13 }
     
rectifierGroupTableGroup OBJECT-GROUP
        OBJECTS {
                dcRectifierGroupName,
                dcRectifierGroupRectifierType,
                dcRectifierGroupDefaultVoltage,
                dcRectifierGroupDefaultCurrentLimit,
                dcRectifierGroupDefaultPowerLimit,
                dcRectifierGroupInputLowOff,
                dcRectifierGroupInputLowOn,
                dcRectifierGroupStartupVoltage,
                dcRectifierGroupStartupCurrentLimit,
                dcRectifierGroupStartupPowerLimit,
                dcRectifierGroupStartupTimeLimit,
                dcRectifierGroupPowerupDelay,
                dcRectifierGroupPowerupTime,
                dcRectifierGroupUmaxOff }
        STATUS current
        DESCRIPTION
                "The collection of rectifier group table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.14 --  
 ::= { controllerGroups 14 }

batteryStringTableGroup OBJECT-GROUP
        OBJECTS {
                dcBatteryStringName,
                dcBatteryStringMaxIBatt,
                dcBatteryStringCapacity }
        STATUS current
        DESCRIPTION
                "The collection of battery string table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.15 --  
 ::= { controllerGroups 15 }

defaultLogEventTableGroup OBJECT-GROUP
        OBJECTS {
                dcDefaultLogEventName,
                dcDefaultLogEventLogged }
        STATUS current
        DESCRIPTION
                "The collection of default log event table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.16 --  
 ::= { controllerGroups 16 }

eventProcessingEventTableGroup OBJECT-GROUP
        OBJECTS {
                dcEventProcessingEventName,
                dcEventProcessingEventAssigned,
                dcEventProcessingEventType,
                dcEventProcessingEventSelected }
        STATUS current
        DESCRIPTION
                "The collection of event processing event table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.17 --  
 ::= { controllerGroups 17 }

lvdTableGroup OBJECT-GROUP
        OBJECTS {
                dcLvdName,
                dcLvdDisconnectDelay }
        STATUS current
        DESCRIPTION
                "The collection of LVD table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.18 --  
 ::= { controllerGroups 18 }   
 
powerLimitationTableGroup OBJECT-GROUP
        OBJECTS {
                dcPowerLimitationEventName,
                dcPowerLimitationStatus,
                dcPowerLimitationType,
                dcPowerLimitationLimit,
                dcPowerLimitationNoBatteryDischarge }
        STATUS current
        DESCRIPTION
                "The collection of power limitation table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.19 --  
 ::= { controllerGroups 19 }   

measurementTableGroup OBJECT-GROUP
        OBJECTS {
                dcMeasurementName,
                dcMeasurementValue,
                dcMeasurementScaleFactor,
                dcMeasurementUnit }      
        STATUS current
        DESCRIPTION
                "The collection of measurement table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.20 --  
 ::= { controllerGroups 20 }   

meterPanelEventTableGroup OBJECT-GROUP
        OBJECTS {
                dcMeterPanelEventName,
                dcMeterPanelEventValue,
                dcMeterPanelEventHourMeterValue }      
        STATUS current
        DESCRIPTION
                "The collection of meter panel event table objects."
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.1.21 --  
 ::= { controllerGroups 21 }    
                                      
controllerBasicCompl MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION
                "The basic implementation requirements for the controller MIB."
        MODULE 
        MANDATORY-GROUPS {
                systemInfoGroup,
                systemAlarmGroup,
                systemMonitorGroup,
                alarmTableGroup,
                notificationsGroup }
 -- 1.3.6.1.4.1.20246.2.3.1.1.1.1.2.1 --
 ::= { controllerCompl 1 }

END
