--  *****************************************************************
--  DLINKSW-DHCP6-CLIENT-MIB.mib : DHCPv6 Client MIB
-- 
--  Copyright (c) 2013 D-Link Corporation, all rights reserved.
--   
--  *****************************************************************
DLINKSW-DHCP6-CLIENT-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY,
        OBJECT-TYPE,
        Integer32,
        Unsigned32        
                FROM SNMPv2-SMI
        DisplayString,
        TruthValue,
        RowStatus
            FROM SNMPv2-TC
        MODULE-COMPLIANCE, OBJECT-GROUP
		    FROM SNMPv2-CONF 
        InterfaceIndex,
        InterfaceIndexOrZero
            FROM IF-MIB
        InetAddressPrefixLength, InetAddressIPv6
            FROM INET-ADDRESS-MIB
        dlinkIndustrialCommon			
			FROM DLINK-ID-REC-MIB;


    dlinkSwDhcp6ClientMIB MODULE-IDENTITY
        LAST-UPDATED "201301180000Z"
        ORGANIZATION "D-Link Corp."
        CONTACT-INFO
            "         D-Link Corporation
             Postal: No. 289, Sinhu 3rd Rd., Neihu District,
                     Taipei City 114, Taiwan, R.O.C
             Tel:    +886-2-66000123
             E-mail: tsd@dlink.com.tw
            "
        DESCRIPTION
            "This MIB module defines objects for DHCPv6 Client."
        REVISION     "201301180000Z"
        DESCRIPTION
            "This is the first version of the MIB file for 'DHCPv6 Client'
            functionality."
        ::= { dlinkIndustrialCommon 222 }

-- -----------------------------------------------------------------------------
    dDhcp6ClientNotifications    OBJECT IDENTIFIER ::= { dlinkSwDhcp6ClientMIB 0 }
    dDhcp6ClientObjects          OBJECT IDENTIFIER ::= { dlinkSwDhcp6ClientMIB 1 }
    dDhcp6ClientConformance      OBJECT IDENTIFIER ::= { dlinkSwDhcp6ClientMIB 2 }

-- -----------------------------------------------------------------------------
    dDhcp6ClientGeneral          OBJECT IDENTIFIER ::= { dDhcp6ClientObjects 1 }

    dDhcp6ClientDuid OBJECT-TYPE
        SYNTAX      OCTET STRING
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The DHCP Unique Identity (DUID) of DHCPv6 Client."
        ::= { dDhcp6ClientGeneral 1 }
 
    dhcp6ClientRestartIf OBJECT-TYPE
        SYNTAX      InterfaceIndexOrZero
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "Specifies the ifIndex of the interface on which DHCPv6 client will
            be restart.
            The agent will return an inconsistentValue error on sets if DHCPv6
            client is not enabled on the interface.         	            
            The special value 0 is return when read."
        ::= { dDhcp6ClientGeneral 2 }


-- -----------------------------------------------------------------------------
    dDhcp6ClientIfObjects          OBJECT IDENTIFIER ::= { dDhcp6ClientObjects 2 }
    dDhcp6CIfTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF DDhcp6CIfEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
             "A table contains all DHCPv6 client entries which consists of
             DHCPv6 client related configuration. An entry is created to set a
             value different from the default on an interface. If an entry is
             deleted, all configurations are reverted to default."
        ::= { dDhcp6ClientIfObjects 1 }

    dDhcp6CIfEntry OBJECT-TYPE
        SYNTAX          DDhcp6CIfEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Defines an entry in the dDhcp6CIfTable."
        INDEX  { dDhcp6CIfIndex }
        ::= { dDhcp6CIfTable 1 }

    DDhcp6CIfEntry ::= SEQUENCE {
        dDhcp6CIfIndex                  InterfaceIndex, 
        dDhcp6CIfAcquireAddrEnabled     TruthValue,   
        dDhcp6CIfAcqAddrRapidCommit     TruthValue, 
        dDhcp6CIfMinRefresh             Unsigned32,
        dDhcp6CIfRowStatus              RowStatus
    }

    dDhcp6CIfIndex  OBJECT-TYPE
        SYNTAX          InterfaceIndex
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "The ifIndex value of the interface.
            Only VLAN interfaces are valid interfaces."
        ::= { dDhcp6CIfEntry 1 }
        
    dDhcp6CIfAcquireAddrEnabled OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
            "This object indicates whether acquires an IPv6 address on an
            interface from the DHCPv6 server." 
        DEFVAL      { false }    
        ::= { dDhcp6CIfEntry 2 }
           
    dDhcp6CIfAcqAddrRapidCommit OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
            "This object indicates whether the two-message
            exchange for address allocation and other configuration is used.
            When dDhcp6CIfAcquireAddrEnabled is 'false', dDhcp6CIfRapidCommit
            cannot be set to 'true'." 
        DEFVAL      { false }    
        ::= { dDhcp6CIfEntry 3 }
     
    dDhcp6CIfMinRefresh OBJECT-TYPE
        SYNTAX          Unsigned32 (600..4294967295)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
            "This object specifies the minimum acceptable information refresh 
            time in seconds. If the client receives a information refresh time
            less than the configured minimum refresh time, the configured 
            minimum refresh time will be used."
        DEFVAL      { 86400 }
        ::= { dDhcp6CIfEntry 4 }
                    
     dDhcp6CIfRowStatus OBJECT-TYPE
        SYNTAX          RowStatus
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
           "The status of this conceptual row." 
        ::= { dDhcp6CIfEntry 5 } 
                 
-- -----------------------------------------------------------------------------   	
   	 dDhcp6CIfPrefixDeleCfgTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF DDhcp6CIfPrefixDeleCfgEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
             "The table contains information about prefix delegation request 
             of DHCPv6 client. An entry is created/removed when enable/disable
             request for prefix delegation through a specified interface."
        ::= { dDhcp6ClientIfObjects 3 }

    dDhcp6CIfPrefixDeleCfgEntry OBJECT-TYPE
        SYNTAX          DDhcp6CIfPrefixDeleCfgEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Defines an entry in the dDhcp6CIfPrefixDeleCfgTable."
        INDEX  { dDhcp6CIfPdCfgIfIndex }
        ::= { dDhcp6CIfPrefixDeleCfgTable 1 }

    DDhcp6CIfPrefixDeleCfgEntry ::= SEQUENCE {
        dDhcp6CIfPdCfgIfIndex      InterfaceIndex,              
        dDhcp6CIfPdCfgPrefixName   DisplayString,
        dDhcp6CIfPdCfgHintAddr     InetAddressIPv6,
        dDhcp6CIfPdCfgHintLen      InetAddressPrefixLength,
        dDhcp6CIfPdCfgRapidCommit  TruthValue,
        dDhcp6CIfPdCfgRowStatus    RowStatus
    }
    
    dDhcp6CIfPdCfgIfIndex  OBJECT-TYPE
        SYNTAX          InterfaceIndex
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "The ifIndex value of the interface.
             Only VLAN interfaces are valid interfaces."
        ::= { dDhcp6CIfPrefixDeleCfgEntry 1 }
        
    dDhcp6CIfPdCfgPrefixName OBJECT-TYPE
        SYNTAX          DisplayString (SIZE (0..32))
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
            "This object indicates a IPv6 general prefix name.           
            The prefix acquired from the server will be stored in the IPv6
            general prefix pool represented by this object, which will be in
            turn used in configuration of IPv6 addresses.
            The zero length indicates the general prefix name is not configured.
            Either dDhcp6CIfPdCfgPrefixName or dDhcp6CIfPdCfgHintAddr can be configured
            on an interface.
            If neither dDhcp6CIfPdCfgPrefixName nor dDhcp6CIfPdCfgHintAddr is 
            configured, this indicates the request for prefix delegation
            through a specified interface is disabled and the entry will be
            deleted."
        ::= { dDhcp6CIfPrefixDeleCfgEntry 2 }
        
    dDhcp6CIfPdCfgHintAddr OBJECT-TYPE
        SYNTAX          InetAddressIPv6
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
            "This object indicates an IPv6 prefix to be sent in the prefix
            delegation request message as a hint.
            The special value of all '00'Hs indicates that hint IPv6 prefix is 
            not configured.
            Either dDhcp6CIfPdCfgPrefixName or dDhcp6CIfPdCfgHintAddr can be configured
            on an interface.
            If neither dDhcp6CIfPdCfgPrefixName nor dDhcp6CIfPdCfgHintAddr is  
            configured, this indicates the request for prefix delegation
            through a specified interface is disabled and the entry will be
            deleted."           
        ::= { dDhcp6CIfPrefixDeleCfgEntry 3 }

    dDhcp6CIfPdCfgHintLen OBJECT-TYPE
        SYNTAX          InetAddressPrefixLength 
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
            "The length of the prefix (in bits).
             It indicates the length of hint prefix."
        ::= { dDhcp6CIfPrefixDeleCfgEntry 4 }
 
    dDhcp6CIfPdCfgRapidCommit OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
            "This object indicates that whether proceed with two-message
            exchange for prefix delegation.  The rapid-commit option will be
            filled in the Solicit message to request two messages handshake." 
        ::= { dDhcp6CIfPrefixDeleCfgEntry 5 }
   	
   	 dDhcp6CIfPdCfgRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
           "The status of this conceptual row." 
        ::= { dDhcp6CIfPrefixDeleCfgEntry 6 }
        		
-- -----------------------------------------------------------------------------
    dDhcp6ClientStatusObjects    OBJECT IDENTIFIER ::= { dDhcp6ClientObjects 3 }
    
    dDhcp6CIfStateTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF DDhcp6CIfStateEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
             "The table contains per-interface DHCPv6 client state information."
        ::= { dDhcp6ClientStatusObjects 1 }

    dDhcp6CIfStateEntry OBJECT-TYPE
        SYNTAX      DDhcp6CIfStateEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "Defines an entry in the dDhcp6CIfStateTable."
        INDEX  { dDhcp6CIfStateIfIndex }
        ::= { dDhcp6CIfStateTable 1 }

    DDhcp6CIfStateEntry ::= SEQUENCE {
            dDhcp6CIfStateIfIndex       InterfaceIndex,
            dDhcp6CIfStateCode          INTEGER,
            dDhcp6CIfStatusEventExpire  Unsigned32              
        }
        
    dDhcp6CIfStateIfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The ifIndex value of the interface.
             Only VLAN interfaces are valid interfaces."
        ::= { dDhcp6CIfStateEntry 1 }
        
    dDhcp6CIfStateCode OBJECT-TYPE
        SYNTAX      INTEGER { invalid(0), init(1), request(2),
                              release(3), active(4), renew(5), rebind(6) }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "DHCPv6 Client running state."
        ::= { dDhcp6CIfStateEntry 2 }
     
    dDhcp6CIfStatusEventExpire OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Next event expire time of DHCPv6 Client.
             It is valid when DHCPv6 Client in 
             REQUEST and REBIND state."
        ::= { dDhcp6CIfStateEntry 3 }
        
-- -----------------------------------------------------------------------------    
    dDhcp6CIfAcquiredIaTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF DDhcp6CIfAcquiredIaEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
             "The table contains the list of the known DHCPv6 servers."
        ::= { dDhcp6ClientStatusObjects 2 }

    dDhcp6CIfAcquiredIaEntry OBJECT-TYPE
        SYNTAX      DDhcp6CIfAcquiredIaEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "Defines an entry in the dDhcp6CIfAcquiredIaTable."
        INDEX  { 
            dDhcp6CIfAcquiredIaType,
            dDhcp6CIfAcquiredIaId,
            dDhcp6CIfAcquiredIaIfIndex }
        ::= { dDhcp6CIfAcquiredIaTable 1 }

    DDhcp6CIfAcquiredIaEntry ::= SEQUENCE {                  
            dDhcp6CIfAcquiredIaType             INTEGER,
            dDhcp6CIfAcquiredIaId               Unsigned32,
            dDhcp6CIfAcquiredIaIfIndex          InterfaceIndex,      
            dDhcp6CIfAcquiredIaServerAddr       InetAddressIPv6,
            dDhcp6CIfAcquiredIaServerDUID       OCTET STRING,
            dDhcp6CIfAcquiredIaServerPref       Unsigned32,                  
            dDhcp6CIfAcquiredIaT1               Unsigned32,
            dDhcp6CIfAcquiredIaT2               Unsigned32,            
            dDhcp6CIfAcquiredIaExpireTime       Unsigned32         
        }
   
    dDhcp6CIfAcquiredIaType OBJECT-TYPE
        SYNTAX          INTEGER { other(0), iapd(1), iana(2) }
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "The acquired IA type.
             other(0) - none of the following.
             iapd(1)  - the type of the IA is Prefix Delegation.
             iana(2)  - the type of the IA is non-temporary addresses."             
        ::= { dDhcp6CIfAcquiredIaEntry 1 }

    dDhcp6CIfAcquiredIaId OBJECT-TYPE
        SYNTAX          Unsigned32 (0..4294967295)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "The acquired IA identify."
        ::= { dDhcp6CIfAcquiredIaEntry 2 }

     dDhcp6CIfAcquiredIaIfIndex OBJECT-TYPE
        SYNTAX          InterfaceIndex
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "The ifIndex value of the interface.
            Only VLAN interfaces are valid interfaces."
        ::= { dDhcp6CIfAcquiredIaEntry 3 }
      
    dDhcp6CIfAcquiredIaServerAddr OBJECT-TYPE
        SYNTAX          InetAddressIPv6
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The address of DHCPv6 server."
        ::= { dDhcp6CIfAcquiredIaEntry 4 }
                
    dDhcp6CIfAcquiredIaServerDUID OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The DUID of the corresponding DHCPv6 server."
        ::= { dDhcp6CIfAcquiredIaEntry 5 }

    dDhcp6CIfAcquiredIaServerPref OBJECT-TYPE
        SYNTAX          Unsigned32 (0..4294967295)
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The preference of the corresponding DHCPv6 server."
        ::= { dDhcp6CIfAcquiredIaEntry 6 }
   
    dDhcp6CIfAcquiredIaT1 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The T1 timer of the acquired IA."             
        ::= { dDhcp6CIfAcquiredIaEntry 7 }

    dDhcp6CIfAcquiredIaT2 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The T2 timer of the acquired IA."  
        ::= { dDhcp6CIfAcquiredIaEntry 8 }
 
    dDhcp6CIfAcquiredIaExpireTime OBJECT-TYPE        
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The expire time of acquired IA."            
        ::= { dDhcp6CIfAcquiredIaEntry 9 }
               
-- -----------------------------------------------------------------------------
    dDhcp6CIfAddrTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF DDhcp6CIfAddrEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
             "The table contains per-interface DHCPv6 address acquired from DHCPv6
             server."
        ::= { dDhcp6ClientStatusObjects 3 }

    dDhcp6CIfAddrEntry OBJECT-TYPE
        SYNTAX          DDhcp6CIfAddrEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Defines an entry in the dDhcp6CIfAddrTable."
        INDEX  { 
            dDhcp6CIfAcquiredIaId,
            dDhcp6CIfAddrInetAddr
        }
        ::= { dDhcp6CIfAddrTable 1 }

    DDhcp6CIfAddrEntry ::= SEQUENCE {           
            dDhcp6CIfAddrInetAddr           InetAddressIPv6,           
            dDhcp6CIfAddrPreferLifeTime     Unsigned32,
            dDhcp6CIfAddrValidLifeTime      Unsigned32,                  
            dDhcp6CIfAddrExpireTime         Unsigned32
    }

    dDhcp6CIfAddrInetAddr OBJECT-TYPE
        SYNTAX         InetAddressIPv6
        MAX-ACCESS     not-accessible
        STATUS         current
        DESCRIPTION
            "The acquired address from DHCPv6 server."            
        ::= { dDhcp6CIfAddrEntry 1 }
   
    dDhcp6CIfAddrPreferLifeTime OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The prefer lifetime of the acquired address."             
        ::= { dDhcp6CIfAddrEntry 2 }
      
    dDhcp6CIfAddrValidLifeTime OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The valid lifetime of the acquired address."
        ::= { dDhcp6CIfAddrEntry 3 } 
                          
    dDhcp6CIfAddrExpireTime OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The expire time of the acquired address."           
        ::= { dDhcp6CIfAddrEntry 4 }  
  
-- -----------------------------------------------------------------------------
    dDhcp6CIfPrefixTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF DDhcp6CIfPrefixEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
             "The table contains all acquired prefixes from DHCPv6 server(s)."
        ::= { dDhcp6ClientStatusObjects 4 }

    dDhcp6CIfPrefixEntry OBJECT-TYPE
        SYNTAX          DDhcp6CIfPrefixEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Defines an entry in the dDhcp6CIfPrefixTable."
        INDEX  { 
              dDhcp6CIfAcquiredIaId,
              dDhcp6CIfPrefixAddr,
              dDhcp6CIfPrefixAddrLen }
        ::= { dDhcp6CIfPrefixTable 1 }

    DDhcp6CIfPrefixEntry ::= SEQUENCE {          
            dDhcp6CIfPrefixAddr             InetAddressIPv6,
            dDhcp6CIfPrefixAddrLen          InetAddressPrefixLength,
            dDhcp6CIfPrefixPreferLifeTime   Unsigned32,
            dDhcp6CIfPrefixValidLifeTime    Unsigned32,                  
            dDhcp6CIfPrefixExpireTime       Unsigned32
        }
    
    dDhcp6CIfPrefixAddr OBJECT-TYPE
        SYNTAX          InetAddressIPv6
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "The address of the acquired prefix."
        ::= { dDhcp6CIfPrefixEntry 1 }

    dDhcp6CIfPrefixAddrLen OBJECT-TYPE
        SYNTAX          InetAddressPrefixLength
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "The prefix length of the acquired prefix."
           
        ::= { dDhcp6CIfPrefixEntry 2 }
        
    dDhcp6CIfPrefixPreferLifeTime OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "The prefer lifetime of the acquired prefix."             
        ::= { dDhcp6CIfPrefixEntry 3 }

    dDhcp6CIfPrefixValidLifeTime OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The valid lifetime of the acquired prefix."             
        ::= { dDhcp6CIfPrefixEntry 4 }

    dDhcp6CIfPrefixExpireTime OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The expire time of the acquired prefix"
        ::= { dDhcp6CIfPrefixEntry 5 }
        
--  ***************************************************************************	
--  Conformance
--  ***************************************************************************
    dDhcp6ClientCompliances OBJECT IDENTIFIER ::= { dDhcp6ClientConformance 1 }
		
	dDhcp6ClientCompliance MODULE-COMPLIANCE
		STATUS          current
		DESCRIPTION 
			"The compliance statement for entities which implement the 
			DLINKSW-DHCP6-CLIENT-MIB."
		MODULE -- this module
		MANDATORY-GROUPS { 
		    dDhcp6CBasicGroup,
		    dDhcp6CBasicStatusGroup
		}	
		
		OBJECT dDhcp6CIfMinRefresh
        MIN-ACCESS      read-only
        DESCRIPTION
            "It is complaint to support read only if the implementation doesn't
            support setting acceptable information refresh time."
        
        OBJECT dDhcp6CIfAcqAddrRapidCommit
        MIN-ACCESS      read-only
        DESCRIPTION
            "It is complaint to support read only if the implementation doesn't
            support rapid-commit for acquiring address."  
                     
		GROUP       dDhcp6CPrefixDelegationGroup
        DESCRIPTION
              "This group is required only if the agent supports requesting
              for prefix delegation through a specified interface."
                
		GROUP       dDhcp6CPrefixDelegStatusGroup
        DESCRIPTION
              "This group is required only if the agent supports requesting
              for prefix delegation through a specified interface."
        
        OBJECT dDhcp6CIfPdCfgRapidCommit
        MIN-ACCESS      read-only
        DESCRIPTION
            "It is complaint to support read only if the implementation doesn't
            support rapid-commit for requesting the prefix delegation."
                        
	    ::= { dDhcp6ClientCompliances 1 }
		
	dDhcp6ClientGroups OBJECT IDENTIFIER ::= { dDhcp6ClientCompliances 2 }
		
    dDhcp6CBasicGroup OBJECT-GROUP
		OBJECTS { 
		    dDhcp6ClientDuid, 
		    dhcp6ClientRestartIf, 
		    dDhcp6CIfAcquireAddrEnabled, 
		    dDhcp6CIfAcqAddrRapidCommit, 
		    dDhcp6CIfMinRefresh, 
			dDhcp6CIfRowStatus 
		}
		STATUS current
		DESCRIPTION 
			"This group contains the collection of objects related to  
			acquiring IPv6 address on an interface from DHCPv6 server."						
		::= { dDhcp6ClientGroups 1 }

		
	dDhcp6CBasicStatusGroup OBJECT-GROUP
		OBJECTS { 
		    dDhcp6CIfStateCode, 
		    dDhcp6CIfStatusEventExpire, 		   
		    dDhcp6CIfAcquiredIaServerAddr, 
		    dDhcp6CIfAcquiredIaServerDUID, 
		    dDhcp6CIfAcquiredIaServerPref, 
		    dDhcp6CIfAcquiredIaT1, 
		    dDhcp6CIfAcquiredIaT2, 
			dDhcp6CIfAcquiredIaExpireTime, 
			dDhcp6CIfAddrPreferLifeTime, 
			dDhcp6CIfAddrValidLifeTime, 
			dDhcp6CIfAddrExpireTime
		}
		STATUS current
		DESCRIPTION 
			"This group contains the collection of objects about the status 
			of acquired IPv6 address and the information about DHCPv6 server."
		::= { dDhcp6ClientGroups 2 }

		
	dDhcp6CPrefixDelegationGroup OBJECT-GROUP
		OBJECTS { 
		    dDhcp6CIfPdCfgPrefixName, 
		    dDhcp6CIfPdCfgHintAddr, 
		    dDhcp6CIfPdCfgHintLen, 
		    dDhcp6CIfPdCfgRapidCommit, 
		    dDhcp6CIfPdCfgRowStatus
		}
		STATUS current
		DESCRIPTION 
			"This group contains the collection of objects related to  
			acquiring IPv6 prefix on an interface from DHCPv6 server."
		::= { dDhcp6ClientGroups 3 }
		
	dDhcp6CPrefixDelegStatusGroup OBJECT-GROUP
		OBJECTS { 		 
		    dDhcp6CIfPrefixPreferLifeTime, 
		    dDhcp6CIfPrefixValidLifeTime, 
		    dDhcp6CIfPrefixExpireTime
		}
		STATUS current
		DESCRIPTION 
			"This group contains the collection of objects about the status 
			of the acquired prefixes."
		::= { dDhcp6ClientGroups 4 }

END

