    HIMOINSAv14-MIB DEFINITIONS ::= BEGIN

	IMPORTS
     enterprises
         FROM RFC1155-SMI
     OBJECT-TYPE
         FROM RFC-1212
     TRAP-TYPE
         FROM RFC-1215
	 DisplayString
		 FROM RFC1213-MIB
	 Gauge, Counter, IpAddress
		FROM RFC1155-SMI;


	InterfaceIndex ::= INTEGER

        himoinsa       OBJECT IDENTIFIER ::= { enterprises 41809 }

        measures        OBJECT IDENTIFIER ::= { himoinsa 1 }

        parameters      OBJECT IDENTIFIER ::= { himoinsa 2 }

        traps           OBJECT IDENTIFIER ::= { himoinsa 3 }

        mainsFreq OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 1 }

        mainsVL12 OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 2 }

        mainsVL23 OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 3 }

        mainsVL13 OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 4 }

        mainsVL1N OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 5 }

        mainsVL2N OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 6 }

        mainsVL3N OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 7 }

        genFreq OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 8 }

        genVL12 OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 9 }

        genVL23 OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 10 }

        genVL13 OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 11 }

        genVL1N OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 12 }

        genVL2N OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 13 }

        genVL3N OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 14 }

        ph1Amp OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 15 }

        ph2Amp OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 16 }

        ph3Amp OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 17 }

        flagsCurrent OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 18 }

		pFCTotal OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measures 19 }

		pFC1 OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measures 20 }

		pFC2 OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measures 21 }

		pFC3 OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measures 22 }

        realPow OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 23 }

        appPow OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 24 }

        reactivePow OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 25 }

        speed OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 26 }

        fuelLevel OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 27 }

        altenatorVolt OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 28 }

        batteryVolt OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 29 }

        waterTemp OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 30 }

        oilPress OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 31 }

        oilTemp OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 32 }

        sensorDet OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 33 }

        units OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 34 }

        totalInstantPower OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 35 }

		partialInstantPower OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 36 }

        powerPerDay OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 37 }

        powerPerMonth OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 38 }

        powerPerYear OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 39 }

        totalRunningTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 40 }

        partialRunningTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 41 }

        successfulStarts OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 42 }

        unsuccessfulStarts OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 43 }

        switchPanelCount OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 44 }

        secondaryBatteryVoltage OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 45 }

        status OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 46 }

        alarmBitMapHigh OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 47 }

        alarmBitMapLow OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 48 }

        alarmBitMapHigh1 OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 49 }

		falloArranqueMeasure OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 50 }

		nivelCombustibleMeasure OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 51 }

		caidaGrupoMeasure OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 52 }

		caidaRedMeasure OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 53 }

		caidaGrupoConmMeasure OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 54 }

        measuresConmTable OBJECT-TYPE
                SYNTAX SEQUENCE OF MeasuresConmEntry
                ACCESS not-accessible
                STATUS current
                DESCRIPTION
                        ""
                ::= { measures 55 }


        measuresConmEntry OBJECT-TYPE
                SYNTAX MeasuresConmEntry
                ACCESS not-accessible
                STATUS current
                DESCRIPTION
                        ""
                INDEX { measuresConmIndex }
                ::= { measuresConmTable 1 }

        MeasuresConmEntry ::= SEQUENCE {
		measuresConmIndex
			InterfaceIndex,
        mainsFreqConm
            INTEGER,
        mainsVL12Conm
            INTEGER,
		mainsVL23Conm
		    INTEGER,
		mainsVL13Conm
		    INTEGER,
		mainsVL1NConm
		    INTEGER,
		mainsVL2NConm
		    INTEGER,
		mainsVL3NConm
		    INTEGER,
		genFreqConm
            INTEGER,
        genVL12Conm
            INTEGER,
		genVL23Conm
		    INTEGER,
		genVL13Conm
		    INTEGER,
		genVL1NConm
		    INTEGER,
		genVL2NConm
		    INTEGER,
		genVL3NConm
		    INTEGER,
		ph1AmpConm
		    INTEGER,
		ph2AmpConm
		    INTEGER,
		ph3AmpConm
		    INTEGER,
		flagsCurrentConm
		    Gauge,
		pFCTotalConm
		    INTEGER,
		pFC1Conm
		    INTEGER,
		pFC2Conm
		    INTEGER,
		pFC3Conm
		    INTEGER,
		realPowConm
		    INTEGER,
		appPowConm
		    INTEGER,
		reactPowConm
			INTEGER,
		mainsControlType
		    INTEGER,
		statusConm
			Gauge,
		alarmBitMapConm
			Gauge
        }

        measuresConmIndex OBJECT-TYPE
                SYNTAX InterfaceIndex
                ACCESS not-accessible
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 1 }

        mainsFreqConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 2 }

        mainsVL12Conm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 3 }

        mainsVL23Conm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 4 }

        mainsVL13Conm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 5 }

        mainsVL1NConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 6 }

        mainsVL2NConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 7 }

        mainsVL3NConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 8 }

        genFreqConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 9 }

        genVL12Conm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 10 }

        genVL23Conm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 11 }

        genVL13Conm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 12 }

        genVL1NConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 13 }

        genVL2NConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 14 }

        genVL3NConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 15 }

        ph1AmpConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 16 }

        ph2AmpConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 17 }

        ph3AmpConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 18 }

        flagsCurrentConm OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 19 }

		pFCTotalConm OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measuresConmEntry 20 }
		pFC1Conm OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measuresConmEntry 21 }

		pFC2Conm OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measuresConmEntry 22 }

		pFC3Conm OBJECT-TYPE
				SYNTAX INTEGER
				ACCESS read-only
				STATUS current
				DESCRIPTION
						""
				::= { measuresConmEntry 23 }

        realPowConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 24 }

        appPowConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 25 }

        reactPowConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 26 }

        mainsControlType OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 27 }

        statusConm OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 28 }

        alarmBitMapConm OBJECT-TYPE
                SYNTAX Gauge
                ACCESS read-only
                STATUS current
                DESCRIPTION
                        ""
                ::= { measuresConmEntry 29 }

        startsCount OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 1 }

        timeBetweenStarts OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 2 }

        startDelay OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 3 }

        preheatingTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 4 }

        startupTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 5 }

        loadActivationTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 6 }

        nominalConditionTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 7 }

        dplusActivationTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 8 }

		eJP1ActivationDelayTime  OBJECT-TYPE
				SYNTAX  	INTEGER
				ACCESS		read-write
				STATUS		current
				DESCRIPTION
						""
				::= { parameters 9 }

        mainsActivationDelay OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 10 }

        coolingTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 11 }

		pEActivationTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 12 }

        counterDetectionTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 13 }

        maximumAlarmActivationTime OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 14 }

        phaseNumber OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 15 }

        maxGensetVoltage OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 16 }

        minGensetVoltage OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 17 }

        maxGensetAsymetryValue OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 18 }

        maxGensetFrequency OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 19 }

        minGensetFrequency OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 20 }

        maxGensetCurrent OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 21 }

        shortCircuitDetection OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 22 }

        gensetNominalPower OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 23 }

        maxReversePower OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 24 }

        maxPickupSpeed OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 25 }

        minPickupSpeed OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 26 }

        maxMainsVoltage OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 27 }

        minMainsVoltage OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 28 }

        maxMainsFrequency OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 29 }

        minMainsFrequency OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 30 }

        minBatteryVoltage OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 31 }

        transferPumpMinLevel OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 32 }

        transferPumpMaxLevel OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 33 }

        startingVoltageGensetSignal OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 34 }

        startingVoltageAlternator OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 35 }

        startingSpeed OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 36 }

        engineFlywheelTeeth OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 37 }

        fuelReserveLevel OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 38 }

        lowOilPressure OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 39 }

        highWaterTemperatureThreshold OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 40 }

        lowEngineTemperature OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 41 }

        minPreheatingTemp OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 42 }

        maxPreheatingTemp OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 43 }

        deviceIpAddress OBJECT-TYPE
                SYNTAX IpAddress
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 44 }

        deviceMaskSubnet OBJECT-TYPE
                SYNTAX IpAddress
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 45 }

        deviceGateway OBJECT-TYPE
                SYNTAX IpAddress
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 46 }

        managerAddress OBJECT-TYPE
                SYNTAX IpAddress
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 47 }

        agentSNMPPort OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 48 }

        managertrapsPort OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 49 }

        reset OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 50 }

		version  OBJECT-TYPE
				SYNTAX  	INTEGER
				ACCESS		read-only
				STATUS		current
				DESCRIPTION
						""
				::= { parameters 51 }

		gensetStartStop  OBJECT-TYPE
				SYNTAX  	INTEGER
				ACCESS		read-write
				STATUS		current
				DESCRIPTION
						""
				::= { parameters 52 }

		gensetMode  OBJECT-TYPE
				SYNTAX  	INTEGER
				ACCESS		read-write
				STATUS		current
				DESCRIPTION
						""
				::= { parameters 53 }

		mainsBreakerStatus  OBJECT-TYPE
				SYNTAX  	INTEGER
				ACCESS		read-write
				STATUS		current
				DESCRIPTION
						""
				::= { parameters 54 }

		gensetBreakerStatus  OBJECT-TYPE
				SYNTAX  	INTEGER
				ACCESS		read-write
				STATUS		current
				DESCRIPTION
						""
				::= { parameters 55 }

        parametersConmTable OBJECT-TYPE
                SYNTAX SEQUENCE OF ParametersConmEntry
                ACCESS not-accessible
                STATUS current
                DESCRIPTION
                        ""
                ::= { parameters 56 }

        parametersConmEntry OBJECT-TYPE
                SYNTAX ParametersConmEntry
                ACCESS not-accessible
                STATUS current
                DESCRIPTION
                        ""
                INDEX { parametersConmIndex }
                ::= { parametersConmTable 1 }

        ParametersConmEntry ::= SEQUENCE {
            parametersConmIndex InterfaceIndex,
            phaseNumberConm INTEGER,
            maxGensetVoltageConm INTEGER,
            minGensetVoltageConm INTEGER,
            maxGensetAsymetryValueConm INTEGER,
            maxGensetFrequencyConm INTEGER,
            minGensetFrequencyConm INTEGER,
            maxGensetCurrentConm INTEGER,
            shortCircuitDetectionConm INTEGER,
            gensetNominalPowerConm INTEGER,
            maxReversePowerConm INTEGER,
            maxPickupSpeedConm INTEGER,
            minPickupSpeedConm INTEGER,
            maxMainsVoltageConm INTEGER,
            minMainsVoltageConm INTEGER,
            maxMainsFrequencyConm INTEGER,
            minMainsFrequencyConm INTEGER,
            startingVoltageValueConm INTEGER
        }

        parametersConmIndex OBJECT-TYPE
                SYNTAX InterfaceIndex
                ACCESS not-accessible
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 1 }

        phaseNumberConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 2 }

        maxGensetVoltageConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 3 }

        minGensetVoltageConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 4 }

        maxGensetAsymetryValueConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 5 }

        maxGensetFrequencyConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 6 }

        minGensetFrequencyConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 7 }

        maxGensetCurrentConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 8 }

        shortCircuitDetectionConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 9 }

        gensetNominalPowerConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 10 }

        maxReversePowerConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 11 }

        maxPickupSpeedConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 12 }

        minPickupSpeedConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 13 }

        maxMainsVoltageConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 14 }

        minMainsVoltageConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 15 }

        maxMainsFrequencyConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 16 }

        minMainsFrequencyConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 17 }

        startingVoltageValueConm OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-write
                STATUS current
                DESCRIPTION
                        ""
                ::= { parametersConmEntry 18 }

		alarmString OBJECT-TYPE
                SYNTAX DisplayString
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION
                        ""
                ::= { traps 1 }

		falloArranque OBJECT-TYPE
                SYNTAX DisplayString
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION
                        ""
                ::= { traps 2 }

		nivelCombustible OBJECT-TYPE
                SYNTAX DisplayString
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION
                        ""
                ::= { traps 4 }

		caidaGrupo OBJECT-TYPE
                SYNTAX DisplayString
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION
                        ""
                ::= { traps 6 }

		caidaRed OBJECT-TYPE
                SYNTAX DisplayString
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION
                        ""
                ::= { traps 8 }

		caidaGrupoConm OBJECT-TYPE
                SYNTAX DisplayString
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION
                        ""
                ::= { traps 10 }

    END
