   TPLINK-DDMTXPOWTHRESHOLD-MIB DEFINITIONS ::= BEGIN

         IMPORTS
            MODULE-IDENTITY, OBJECT-TYPE
          	  	        FROM SNMPv2-SMI
          	ifIndex
						FROM RFC1213-MIB
			DisplayString
						FROM SNMPv2-TC
			tplinkDdmManageMIBObjects
						FROM TPLINK-DDMMANAGE-MIB;
						
		   		ddmTxPowThreshold MODULE-IDENTITY  
				    LAST-UPDATED    "200908270000Z"
				    ORGANIZATION    "TPLINK"
				    CONTACT-INFO		"www.tplink.com"
				    DESCRIPTION			"The config of DDM Tx Power threshold."
				    REVISION        "200908270000Z"
				    DESCRIPTION			"Initial version of this MIB module."
				    ::= { tplinkDdmManageMIBObjects 5 } 
			 												
				ddmTxPowThresholdTable OBJECT-TYPE
					SYNTAX SEQUENCE OF DDMTxPowThresholdEntry
					MAX-ACCESS	not-accessible
					STATUS			current
					DESCRIPTION 
					"A table that is used to configure the DDM Tx Power Threshold for specific ports on the Switch."
					::= { ddmTxPowThreshold 1 }
				
				ddmTxPowThresholdEntry OBJECT-TYPE
					SYNTAX			DDMTxPowThresholdEntry
					MAX-ACCESS	not-accessible
					STATUS			current
					DESCRIPTION 
					"A list of information for every port."	
					INDEX { ifIndex }
					::= { ddmTxPowThresholdTable 1 }
					
				DDMTxPowThresholdEntry ::=
				SEQUENCE
				{
                    ddmTxPowThresholdPort			DisplayString(SIZE(0..255)),
					ddmTxPowThresholdHighAlarm		OCTET STRING(SIZE(0..30)),
					ddmTxPowThresholdLowAlarm		OCTET STRING(SIZE(0..30)),
					ddmTxPowThresholdHighWarn		OCTET STRING(SIZE(0..30)),
					ddmTxPowThresholdLowWarn		OCTET STRING(SIZE(0..30)),
					ddmTxPowThresholdPortLAG		OCTET STRING(SIZE(0..30))
				}
				         
				ddmTxPowThresholdPort OBJECT-TYPE
					SYNTAX				DisplayString(SIZE(0..255))
					MAX-ACCESS			read-only
					STATUS				current
					DESCRIPTION
					"This object indicates the port number."
					::= { ddmTxPowThresholdEntry 1 }

				ddmTxPowThresholdHighAlarm OBJECT-TYPE
					SYNTAX 				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the highest threshold for the alarm."
					::= { ddmTxPowThresholdEntry 2 }
				
				ddmTxPowThresholdLowAlarm OBJECT-TYPE
					SYNTAX				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the lowest threshold for the alarm."
					::=	{ ddmTxPowThresholdEntry 3 }
		        
				ddmTxPowThresholdHighWarn OBJECT-TYPE
					SYNTAX 				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the highest threshold for the warning."
					::= { ddmTxPowThresholdEntry 4 }
				
				ddmTxPowThresholdLowWarn OBJECT-TYPE
					SYNTAX				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the lowest threshold for the warning."
					::=	{ ddmTxPowThresholdEntry 5 }

				ddmTxPowThresholdPortLAG OBJECT-TYPE
					SYNTAX				OCTET STRING(SIZE(0..30))
					MAX-ACCESS			read-only
					STATUS				current
					DESCRIPTION
					"This object indicates the lag number of the port."
					::= { ddmTxPowThresholdEntry 6 }
																			
END
					