-- ============================================================================
-- Copyright (C) 2020 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- Description:  The mib is used for config the ac in global view.
-- Reference: 
-- Version: V1.15
-- ============================================================================
-- Module definition

	HUAWEI-WLAN-GLOBAL-MIB DEFINITIONS ::= BEGIN

		IMPORTS
			hwWlan
				FROM HUAWEI-WLAN-MIB
			OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP
				FROM SNMPv2-CONF
			IpAddress, Integer32, Unsigned32, Counter64, OBJECT-TYPE,
			MODULE-IDENTITY, NOTIFICATION-TYPE
				FROM SNMPv2-SMI
			MacAddress, RowStatus, DateAndTime
				FROM SNMPv2-TC;
		--1.3.6.1.4.1.2011.6.139.12
		hwWlanGlobalManagement MODULE-IDENTITY
			LAST-UPDATED "202001181237Z"		-- Aug 10, 2019 at 23:37 GMT  
			ORGANIZATION 
				"Huawei Technologies Co.,Ltd."
			CONTACT-INFO 
                                  "Huawei Industrial Base
				   Bantian, Longgang
				   Shenzhen 518129
				   People's Republic of China
				   Website: http://www.huawei.com
				   Email: support@huawei.com

				  "
			DESCRIPTION
                             "V1.15 Modify the node hwWlanUpSpeedHistory."
                        REVISION "202001181237Z"		-- Aug 10, 2019 at 23:37 GMT  	
		                   
                                                         DESCRIPTION
                             "V1.14, Add the node for global trap."
                        REVISION "201908192337Z"		-- Aug 10, 2019 at 23:37 GMT  
			
			DESCRIPTION
                             "V1.13, Add the node for global trap."
                        REVISION "201907162130Z"		-- Jun 16, 2019 at 21:30 GMT  	        

			DESCRIPTION
                             "V1.12, Add the node for global statistics."
                        REVISION "201902181830Z"		-- Feb 18, 2019 at 18:30 GMT  	        
			DESCRIPTION
                             "V1.11, Add the node for global trap."
                        REVISION "201901151950Z"		-- Jan 15, 2019 at 19:50 GMT 
						
                        DESCRIPTION
                             "V1.10, Add the node for global trap."
                        REVISION "201810311440Z"		-- October 31, 2018 at 14:40 GMT                       
                        DESCRIPTION
                             "V1.08, Add the node for global statistics."
                        REVISION "201805091530Z"		-- May 9, 2018 at 15:30 GMT				  
                        DESCRIPTION
                             "V1.08, Add the node for global statistics."
                        REVISION "201803121530Z"		-- March 12, 2018 at 15:30 GMT
			
			DESCRIPTION
                             "V1.07, Modify the node of hwStaGlobalAccessExperience."
                        REVISION "201705020930Z"		-- May 2, 2017 at 09:30 GMT

                        DESCRIPTION
                             "V1.06, Add the node for station DFX."
                        REVISION "201703271415Z"		-- March 27, 2017 at 14:15 GMT
                        DESCRIPTION
                             "V1.05, Add the hwWlanCurrentL3RoamStaCnt info node"
                        REVISION "201602161615Z"		-- Feb 16, 2016 at 16:15 GMT
			DESCRIPTION 
				"The MIB module defines the ap update operation."
			REVISION "201508251550Z"		-- Aug 25, 2015 at 15:50 GMT
			DESCRIPTION 
				"V1.04, Add the ApGroup Statistics  info nodes."	
			REVISION "201506271150Z"		-- June 27, 2015 at 11:50 GMT
			DESCRIPTION 
				"V1.03, Add the hwWlanServiceNormalAPCount and hwWlanApCount  info nodes."
			REVISION "201506211020Z"		-- June 21, 2015 at 10:20 GMT
			DESCRIPTION 
				"V1.02, Add the backup license info nodes."
				
			REVISION "201502021445Z"		-- May 11, 2015 at 14:40 GMT
			DESCRIPTION 
				"V1.01, Add the description of mib nodes."
	                REVISION "201502021445Z"		-- February 2, 2015 at 14:40 GMT
			DESCRIPTION 
				"
				V1.00, Inital version.
				"
			::= { hwWlan 12 }

--
--Node definitions
--

		-- 1.3.6.1.4.1.2011.6.139.12.1
		hwWlanGlobalObjects OBJECT IDENTIFIER ::= { hwWlanGlobalManagement 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.1
		hwWlanGlobalPara OBJECT IDENTIFIER ::= { hwWlanGlobalObjects 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.1.1
		hwWlanGlobalWorkMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				ac(1) ,
				ap(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalPara 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.1.2
		hwWlanAccessMaxApNumber OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the maximum number of APs."
			::= { hwWlanGlobalPara 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.1.3
		hwWlanAccessMaxStaNumber OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the maximum number of STAs connected to an AC."
			::= { hwWlanGlobalPara 3 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.1.4
		hwBranchGroupFileLoadFailGroupNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of branch groups that failed to load the certificate."
			::= { hwWlanGlobalPara 4 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.2
		hwWlanGlobalAcStatistics OBJECT IDENTIFIER ::= { hwWlanGlobalObjects 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.1
		hwWlanCurJointApNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of APs currently connected to an AC."
			::= { hwWlanGlobalAcStatistics 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.2
		hwWlanCurAssocStaNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of associated users on an AC."
			::= { hwWlanGlobalAcStatistics 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.3
		hwWlanCurAuthSuccessStaNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of online STAs on an AC."
			::= { hwWlanGlobalAcStatistics 3 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.4
		hwWlanReassocSuccessTimes OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of successful roaming times on an AC."
			::= { hwWlanGlobalAcStatistics 4 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.5
		hwWlanCurAssoc2gStaNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of 2.4G users on an AC."
			::= { hwWlanGlobalAcStatistics 5 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.6
		hwWlanCurAssoc5gStaNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of 5G users on an AC."
			::= { hwWlanGlobalAcStatistics 6 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.7
		hwWlanDualBandStaNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of dual-band STAs."
			::= { hwWlanGlobalAcStatistics 7 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.8
		hwWlanGlobalUpSpeed OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the upstream rate of the system (uplink throughput)."
			::= { hwWlanGlobalAcStatistics 8 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.2.9
		hwWlanGlobalDownSpeed OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the downstream rate of the system (downlink throughput)."
			::= { hwWlanGlobalAcStatistics 9 }

        -- 1.3.6.1.4.1.2011.6.139.12.1.2.10
		hwWlanCurrentL3RoamStaCnt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the count of current L3 roam stations."
			::= { hwWlanGlobalAcStatistics 10 }

        -- 1.3.6.1.4.1.2011.6.139.12.1.2.11
		hwWlanCurAssoc2gStaType OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the numbers of 2.4G users with different rfmodes on an AC."
			::= { hwWlanGlobalAcStatistics 11 }

        -- 1.3.6.1.4.1.2011.6.139.12.1.2.12
		hwWlanCurAssoc5gStaType OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the numbers of 5G users with different rfmodes on an AC."
			::= { hwWlanGlobalAcStatistics 12 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.3
		hwWlanGlobalStaStatistics OBJECT IDENTIFIER ::= { hwWlanGlobalObjects 3 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.1
		hwWlanStaRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the STA rate.
Unit: 0.01 Compliance standard: Rate > x (x = proportion of 12 Mbps STAs to the total number of STAs)."
			::= { hwWlanGlobalStaStatistics 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.2
		hwWlanStaSnrComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of STA signal-to-noise ratio (SNR).
Unit: 0.01 Compliance standard: SNR > x (x = 20 dB)."
			::= { hwWlanGlobalStaStatistics 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.3
		hwWlanStaResendRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the STA retransmission rate (RR).
Unit: 0.01 Compliance standard: RR < x (x = 50%)."
			::= { hwWlanGlobalStaStatistics 3 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.4
		hwWlanStaDropRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the STA packet loss rate (PLR).
Unit: 0.01 Compliance standard: PLR < x (x = 5%)."
			::= { hwWlanGlobalStaStatistics 4 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.5
		hwWlanStaComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total STA compliance ratio."
			::= { hwWlanGlobalStaStatistics 5 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.6
		hwStaSnrNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 2.4G SNR fails to meet the compliance standard.
Compliance standard: SNR > x (x = 20 dB)."
			::= { hwWlanGlobalStaStatistics 6 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.7
		hwStaRateNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 2.4G rate fails to meet the compliance standard.
Compliance standard: Rate > x (x = 12 Mbps)."
			::= { hwWlanGlobalStaStatistics 7 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.8
		hwStaResendRateNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 2.4G retransmission rate (RR) fails to meet the compliance standard.
Compliance standard: RR < x (x = 50%)."
			::= { hwWlanGlobalStaStatistics 8 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.9
		hwStaDropRateNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 2.4G packet loss rate (PLR) fails to meet the compliance standard.
Compliance standard: PLR < x (x = 5%)."
			::= { hwWlanGlobalStaStatistics 9 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.10
		hwStaThruputNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 2.4G throughput fails to meet the compliance standard. (Here the throughput refers to a sum of the uplink and the downlink throughput.)
Compliance standard: Throughput > x (x = 12 Mbps)."
			::= { hwWlanGlobalStaStatistics 10 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.11
		hwStaSnrNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 5G SNR fails to meet the compliance standard.
Compliance standard: SNR > x (x = 20 dB)."
			::= { hwWlanGlobalStaStatistics 11 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.12
		hwStaRateNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 5G rate fails to meet the compliance standard.
Compliance standard: Rate > x (x = 12 Mbps)."
			::= { hwWlanGlobalStaStatistics 12 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.13
		hwStaResendRateNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 5G retransmission rate (RR) fails to meet the compliance standard.
Compliance standard: RR < x (x = 50%)."
			::= { hwWlanGlobalStaStatistics 13 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.14
		hwStaDropRateNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 5G packet loss rate (PLR) fails to meet the compliance standard.
Compliance standard: PLR < x (x = 5%)."
			::= { hwWlanGlobalStaStatistics 14 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.3.15
		hwStaThruputNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs whose 5G throughput fails to meet the compliance standard. (Here the throughput refers to a sum of the uplink and the downlink throughput.)
Compliance standard: Throughput > x (x = 12 Mbps)."
			::= { hwWlanGlobalStaStatistics 15 }


					
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.16
		hwStaGlobalWirelessPacketDelay OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the average packet delay of the stations."
			::= { hwWlanGlobalStaStatistics 16 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.3.17
		hwStaGlobalWirelessPacketDropRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the average packet drop rate of the stations."
			::= { hwWlanGlobalStaStatistics 17 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.3.18
		hwStaGlobalTotalAccessTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the average online time of the stations."
			::= { hwWlanGlobalStaStatistics 18 }
			
	
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.19
		hwStaGlobalAccessExperience OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the access experience of the stations."
			::= { hwWlanGlobalStaStatistics 19 }
			
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.20
		hwStaGlobalAssocRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the associate rate of station."
			::= { hwWlanGlobalStaStatistics 20 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.21
		hwStaGlobalAuthRateDot1x OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the Dot1x authentication rate of station."
			::= { hwWlanGlobalStaStatistics 21 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.22
		hwStaGlobalAuthRatePortal OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the Portal authentication rate of station."
			::= { hwWlanGlobalStaStatistics 22 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.1.3.23
		hwStaGlobalAuthRateMac OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the Mac authentication rate of station."
			::= { hwWlanGlobalStaStatistics 23 }
			
		-- 1.3.6.1.4.1.2011.6.139.12.1.4
		hwWlanGlobalRfStatistics OBJECT IDENTIFIER ::= { hwWlanGlobalObjects 4 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.1
		hwWlanRfChannelUtilRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the RF channel utilization.
Unit: 0.01 Compliance standard: Channel utilization < x (x = 70%)."
			::= { hwWlanGlobalRfStatistics 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.2
		hwWlanRfNoiseComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the RF noise intensity.
Unit: 0.01 Compliance standard: Noise intensity < x (x = -80 dBm)."
			::= { hwWlanGlobalRfStatistics 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.3
		hwWlanRfChannelJamRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This objects indicates compliance ratio of the RF interference ratio.
Unit: 0.01 Compliance standard: Interference ratio < x (x = 40%)."
			::= { hwWlanGlobalRfStatistics 3 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.4
		hwWlanRfResendRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This objects indicate compliance ratio of the RF retransmission rate (RR).
Unit: 0.01 Compliance standard: RR < x (x = 50%)."
			::= { hwWlanGlobalRfStatistics 4 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.5
		hwWlanRfDropRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This objects indicates compliance ratio of the RF packet loss rate (PLR).
Unit: 0.01 Compliance standard: PLR < x (x = 5%)."
			::= { hwWlanGlobalRfStatistics 5 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.6
		hwWlanRfComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total RF compliance ratio."
			::= { hwWlanGlobalRfStatistics 6 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.7
		hwWlanRfNoiseNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 2.4G noise intensity fails to meet the compliance standard.
Compliance standard: Noise intensity < x (x = -80 dBm)."
			::= { hwWlanGlobalRfStatistics 7 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.8
		hwWlanRfChannelUtilRateNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 2.4G channel utilization fails to meet the compliance standard.
Compliance standard: Channel utilization < x (x = 70%)."
			::= { hwWlanGlobalRfStatistics 8 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.4.9
		hwWlanRfLoadNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 2.4G load fails to meet the compliance standard.
Compliance standard: Number of online users < x (x = 40)."
			::= { hwWlanGlobalRfStatistics 9 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.10
		hwWlanRfChannelJamRateNoncompliance2gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 2.4G interference ratio fails to meet the compliance standard.
Compliance standard: Interference ratio < x (x = 40%)."
			::= { hwWlanGlobalRfStatistics 10 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.11
		hwWlanRfNoiseNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 5G noise intensity fails to meet the compliance standard.
Compliance standard: Noise intensity < x (x = -80 dBm)."
			::= { hwWlanGlobalRfStatistics 11 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.12
		hwWlanRfChannelUtilRateNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 5G channel utilization fails to meet the compliance standard.
Compliance standard: Channel utilization < x (x = 70%)."
			::= { hwWlanGlobalRfStatistics 12 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.13
		hwWlanRfLoadNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 5G load fails to meet the compliance standard.
Compliance standard: Number of online users < x (x = 40)."
			::= { hwWlanGlobalRfStatistics 13 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.4.14
		hwWlanRfChannelJamRateNoncompliance5gCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of radios on which the 5G interference ratio fails to meet the compliance standard.
Compliance standard: Interference ratio < x (x = 40%)."
			::= { hwWlanGlobalRfStatistics 14 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.5
		hwWlanGlobalApStatistics OBJECT IDENTIFIER ::= { hwWlanGlobalObjects 5 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.5.1
		hwWlanApNormalRatio OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the proportion of APs in normal and commit states to all APs.
Unit: 0.01."
			::= { hwWlanGlobalApStatistics 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.5.2
		hwWlanApStaOnlineFailRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the AP's STA access failure rate.
Unit: 0.01 Compliance standard: STA access failure rate < x (x = 20%) Access failure rate = (hwStaAccessRequestFailedCount+hwStaAuthenRequestFailedCount)/(hwStaAssocAndReAssocRequestCount+hwStaAuthenRequestCount)."
			::= { hwWlanGlobalApStatistics 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.5.3
		hwWlanApStaOfflineRateComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the AP's STA offline rate.
Unit: 0.01 Compliance standard: STA offline rate x (x = 20%) Offline rate = hwStaExceptionalOfflineCnt/hwStaAuthenRequestSuccessCount. Abnormal APs are those in fault, version mismatch, and type mismatch."
			::= { hwWlanGlobalApStatistics 3 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.5.4
		hwWlanApStaOnlineCntComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates compliance ratio of the number of access STAs on an AP.
Unit: 0.01 Compliance standard: Access STAs < x (x = 40). Access STAs refer to online STAs. Abnormal APs are those in fault, version mismatch, and type mismatch."
			::= { hwWlanGlobalApStatistics 4 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.5.5
		hwWlanApComplianceRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total AP compliance ratio."
			::= { hwWlanGlobalApStatistics 5 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.5.6
		hwWlanServiceNormalAPCount OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the total of AP in service normal states."
			::= { hwWlanGlobalApStatistics 6 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.5.7
		hwWlanApCount OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the total of AP."
			::= { hwWlanGlobalApStatistics 7 }

		
--  1.3.6.1.4.1.2011.6.139.12.1.6
		-- 1.3.6.1.4.1.2011.6.139.12.1.6
		hwWlanOnlineStaCntHistoryTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanOnlineStaCntHistoryEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table describes historical number of access users, which is counted every 1 min. The AC stores data in the latest 15 min."
			::= { hwWlanGlobalObjects 6 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.6.1
		hwWlanOnlineStaCntHistoryEntry OBJECT-TYPE
			SYNTAX HwWlanOnlineStaCntHistoryEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The index of this table is hwWlanOnlineStaCntTime."
			INDEX { hwWlanOnlineStaCntTime }
			::= { hwWlanOnlineStaCntHistoryTable 1 }


		HwWlanOnlineStaCntHistoryEntry ::=
			SEQUENCE {				
				hwWlanOnlineStaCntTime
					Unsigned32,
				hwWlanOnlineStaCnt
					Integer32,
				hwWlan2gOnlineStaCnt
					Integer32,
				hwWlan5gOnlineStaCnt
					Integer32 
			 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.6.1.1
		hwWlanOnlineStaCntTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the count time. It is the index of the table."
			::= { hwWlanOnlineStaCntHistoryEntry 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.6.1.2
		hwWlanOnlineStaCnt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of access users."
			::= { hwWlanOnlineStaCntHistoryEntry 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.6.1.3
		hwWlan2gOnlineStaCnt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of users connected to the 2.4G radio."
			::= { hwWlanOnlineStaCntHistoryEntry 3 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.6.1.4
		hwWlan5gOnlineStaCnt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of users connected to the 5G radio."
			::= { hwWlanOnlineStaCntHistoryEntry 4 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.7
		hwWlanSpeedHistoryTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanSpeedHistoryEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table describes the historical effective throughput statistics, which is collected every 1 min. The AC stores data in the latest 15 min."
			::= { hwWlanGlobalObjects 7 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.7.1
		hwWlanSpeedHistoryEntry OBJECT-TYPE
			SYNTAX HwWlanSpeedHistoryEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The index of this table is hwWlanSpeedHistoryTime."
			INDEX { hwWlanSpeedHistoryTime }
			::= { hwWlanSpeedHistoryTable 1 }


		HwWlanSpeedHistoryEntry ::=
			SEQUENCE {				
				hwWlanSpeedHistoryTime
					Unsigned32,
				hwWlanUpSpeedHistory
					Integer32,
				hwWlanDownSpeedHistory
					Integer32 
			 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.7.1.1
		hwWlanSpeedHistoryTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the statistics collection time. It is the index of the table."
			::= { hwWlanSpeedHistoryEntry 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.7.1.2
		hwWlanUpSpeedHistory OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates uplink effective throughput of the AC. Unit: Kbps."
			::= { hwWlanSpeedHistoryEntry 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.1.7.1.3
		hwWlanDownSpeedHistory OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates downlink effective throughput of the AC.Unit: Kbps."
			::= { hwWlanSpeedHistoryEntry 3 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.8
		hwWlanBackupLicenseTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanBackupLicenseEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwWlanGlobalObjects 8 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.8.1
		hwWlanBackupLicenseEntry OBJECT-TYPE
			SYNTAX HwWlanBackupLicenseEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwWlanMainAcMac }
			::= { hwWlanBackupLicenseTable 1 }

		
		HwWlanBackupLicenseEntry ::=
			SEQUENCE { 
				hwWlanMainAcMac
					MacAddress,
				hwWlanBackupLicense
					Integer32,
				hwWlanLicenseOrigin
					Integer32,
				hwWlanLicenseBackupTime
					OCTET STRING,
				hwWlanLicenseBackType
					OCTET STRING
			 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.8.1.1
		hwWlanMainAcMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwWlanBackupLicenseEntry 1 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.8.1.2
		hwWlanBackupLicense OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwWlanBackupLicenseEntry 2 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.8.1.3
		hwWlanLicenseOrigin OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwWlanBackupLicenseEntry 3 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.8.1.4
		hwWlanLicenseBackupTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwWlanBackupLicenseEntry 4 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.8.1.5
		hwWlanLicenseBackType OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Backup license source type."
			::= { hwWlanBackupLicenseEntry 5 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.9
		hwWlanApGroupStatisticsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanApGroupStatisticsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table  collects statistics about 2G and 5G users in AP groups."
			::= { hwWlanGlobalObjects 9 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.9.1
		hwWlanApGroupStatisticsEntry OBJECT-TYPE
			SYNTAX HwWlanApGroupStatisticsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"The index of this table is hwWlanApGpStatAPGroupName."
			INDEX { hwWlanApGpStatAPGroupName }
			::= { hwWlanApGroupStatisticsTable 1 }

		
		HwWlanApGroupStatisticsEntry ::=
			SEQUENCE { 
				hwWlanApGpStatAPGroupName
					OCTET STRING,
				hwWlanApGpStatCurAssoc2gStaNum
					Unsigned32,
				hwWlanApGpStatCurAssoc5gStaNum
					Unsigned32
			 }

		-- 1.3.6.1.4.1.2011.6.139.12.1.9.1.1
		hwWlanApGpStatAPGroupName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the name of an AP group. It is the index of the table."
			::= { hwWlanApGroupStatisticsEntry 1 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.9.1.2
		hwWlanApGpStatCurAssoc2gStaNum OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of 2G users in an AP group."
			::= { hwWlanApGroupStatisticsEntry 2 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.1.9.1.3
		hwWlanApGpStatCurAssoc5gStaNum OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of 5G users in an AP group."
			::= { hwWlanApGroupStatisticsEntry 3 }

		
--    1.3.6.1.4.1.2011.6.139.12.2
-- 1.3.6.1.4.1.2011.6.139.12.2
		-- 1.3.6.1.4.1.2011.6.139.12.2
		hwWlanGlobalManagementConformance OBJECT IDENTIFIER ::= { hwWlanGlobalManagement 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.1
		hwWlanGlobalManagementCompliances OBJECT IDENTIFIER ::= { hwWlanGlobalManagementConformance 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.1.1
		hwWlanGlobalManagementCompliance MODULE-COMPLIANCE
			STATUS current
			DESCRIPTION 
				"Description."
			MODULE
					MANDATORY-GROUPS { hwWlanGlobalParaGroup, hwWlanGlobalStatisticsGroup, hwWlanGlobalStaStatisticsGroup, hwWlanGlobalRfStatisticsGroup, hwWlanGlobalApStatisticsGroup, 
			hwWlanOnlineStaCntHistoryGroup, hwWlanSpeedHistoryGroup }
			::= { hwWlanGlobalManagementCompliances 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2
		hwWlanGlobalManagementObjectGroups OBJECT IDENTIFIER ::= { hwWlanGlobalManagementConformance 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2.1
		hwWlanGlobalParaGroup OBJECT-GROUP
			OBJECTS { hwWlanGlobalWorkMode, hwWlanAccessMaxApNumber, hwWlanAccessMaxStaNumber, hwBranchGroupFileLoadFailGroupNum }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 1 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2.2
		hwWlanGlobalStatisticsGroup OBJECT-GROUP
			OBJECTS { hwWlanCurJointApNum, hwWlanCurAssocStaNum, hwWlanCurAuthSuccessStaNum, hwWlanReassocSuccessTimes, hwWlanCurAssoc2gStaNum, 
			hwWlanCurAssoc5gStaNum, hwWlanDualBandStaNum, hwWlanGlobalUpSpeed, hwWlanGlobalDownSpeed }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 2 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2.3
		hwWlanGlobalStaStatisticsGroup OBJECT-GROUP
			OBJECTS { hwWlanStaRateComplianceRate, hwWlanStaSnrComplianceRate, hwWlanStaResendRateComplianceRate, hwWlanStaDropRateComplianceRate, hwWlanStaComplianceRate, 
			hwStaSnrNoncompliance2gCnt, hwStaRateNoncompliance2gCnt, hwStaResendRateNoncompliance2gCnt, hwStaDropRateNoncompliance2gCnt, hwStaThruputNoncompliance2gCnt, 
			hwStaSnrNoncompliance5gCnt, hwStaRateNoncompliance5gCnt, hwStaResendRateNoncompliance5gCnt, hwStaDropRateNoncompliance5gCnt, hwStaThruputNoncompliance5gCnt,
			hwStaGlobalWirelessPacketDelay, hwStaGlobalWirelessPacketDropRate, hwStaGlobalTotalAccessTime, hwStaGlobalAccessExperience, hwStaGlobalAssocRate, hwStaGlobalAuthRateDot1x, 
			hwStaGlobalAuthRatePortal, hwStaGlobalAuthRateMac}
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 3 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2.4
		hwWlanGlobalRfStatisticsGroup OBJECT-GROUP
			OBJECTS { hwWlanRfChannelUtilRateComplianceRate, hwWlanRfNoiseComplianceRate, hwWlanRfChannelJamRateComplianceRate, hwWlanRfResendRateComplianceRate, hwWlanRfDropRateComplianceRate, 
			hwWlanRfComplianceRate, hwWlanRfNoiseNoncompliance2gCnt, hwWlanRfChannelUtilRateNoncompliance2gCnt, hwWlanRfLoadNoncompliance2gCnt, hwWlanRfChannelJamRateNoncompliance2gCnt, 
			hwWlanRfNoiseNoncompliance5gCnt, hwWlanRfChannelUtilRateNoncompliance5gCnt, hwWlanRfLoadNoncompliance5gCnt, hwWlanRfChannelJamRateNoncompliance5gCnt }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 4 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2.5
		hwWlanGlobalApStatisticsGroup OBJECT-GROUP
			OBJECTS { hwWlanApNormalRatio, hwWlanApStaOnlineFailRateComplianceRate, hwWlanApStaOfflineRateComplianceRate, hwWlanApStaOnlineCntComplianceRate, hwWlanApComplianceRate, 
			hwWlanServiceNormalAPCount, hwWlanApCount }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 5 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2.6
		hwWlanOnlineStaCntHistoryGroup OBJECT-GROUP
			OBJECTS { hwWlanOnlineStaCnt, hwWlan2gOnlineStaCnt, hwWlan5gOnlineStaCnt }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 6 }


		-- 1.3.6.1.4.1.2011.6.139.12.2.2.7
		hwWlanSpeedHistoryGroup OBJECT-GROUP
			OBJECTS { hwWlanUpSpeedHistory, hwWlanDownSpeedHistory }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 7 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.2.2.8
		hwWlanBackupLicenseGroup OBJECT-GROUP
			OBJECTS { hwWlanMainAcMac, hwWlanBackupLicense, hwWlanLicenseOrigin, hwWlanLicenseBackupTime }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 8 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.2.2.9
		hwWlanApGroupStatisticsGroup OBJECT-GROUP
			OBJECTS { hwWlanApGpStatCurAssoc2gStaNum, hwWlanApGpStatCurAssoc5gStaNum }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanGlobalManagementObjectGroups 9 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.3
		hwWlanGlobalTrapInfo OBJECT IDENTIFIER ::= { hwWlanGlobalManagement 3 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.3.1
		hwWlanGlobalTrap OBJECT IDENTIFIER ::= { hwWlanGlobalTrapInfo 1 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.1
		hwWlanBackLicAgeTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanMainAcMac, hwWlanBackupLicense, hwWlanLicenseBackType, hwWlanLicenseBackupTime }
			STATUS current
			DESCRIPTION 
				"Backup license aging alarm."
			::= { hwWlanGlobalTrap 1 }

		
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.2
		hwWlanBackLicAgeRestoreTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanMainAcMac, hwWlanBackupLicense, hwWlanLicenseBackType, hwWlanLicenseBackupTime }
			STATUS current
			DESCRIPTION 
				"The backup license stops aging."
			::= { hwWlanGlobalTrap 2 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.3
		hwWlanShareLicAgeTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanShareLicAcMac, hwWlanShareLicNum }
			STATUS current
			DESCRIPTION 
				"Shared license aging."
			::= { hwWlanGlobalTrap 3 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.4
		hwWlanShareLicAgeRestoreTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanShareLicAcMac, hwWlanShareLicNum }
			STATUS current
			DESCRIPTION 
				"Shared license aging restore."
			::= { hwWlanGlobalTrap 4 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.5
		hwWlanPoolLicAgeTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanPoolTotalLicNum, hwWlanPoolSelfShareLicNum }
			STATUS current
			DESCRIPTION 
				"License resource pool aging."
			::= { hwWlanGlobalTrap 5 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.6
		hwWlanPoolLicAgeRestoreTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanPoolTotalLicNum, hwWlanPoolSelfShareLicNum }
			STATUS current
			DESCRIPTION 
				"License resource pool aging restore."
			::= { hwWlanGlobalTrap 6 }

		-- 1.3.6.1.4.1.2011.6.139.12.3.1.7
		hwWlanStaNumReachWarningTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanStaMaxNum, hwWlanStaCurNum }
			STATUS current
			DESCRIPTION 
				"The number of stations reaches 80% of the maximum specifications."
			::= { hwWlanGlobalTrap 7 }
            
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.8
		hwWlanStaNumReachWarningRestoreTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanStaMaxNum, hwWlanStaCurNum }
			STATUS current
			DESCRIPTION 
				"The number of stations is less than 80% of the maximum specifications."
			::= { hwWlanGlobalTrap 8 }

		-- 1.3.6.1.4.1.2011.6.139.12.3.1.9
		hwWlanStaNumReachMaxTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanStaMaxNum, hwWlanStaCurNum }
			STATUS current
			DESCRIPTION 
				"The number of stations reaches the maximum specifications."
			::= { hwWlanGlobalTrap 9 }
            
		-- 1.3.6.1.4.1.2011.6.139.12.3.1.10
		hwWlanStaNumReachMaxRestoreTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanStaMaxNum, hwWlanStaCurNum }
			STATUS current
			DESCRIPTION 
				"The number of stations is less than the maximum specifications."
			::= { hwWlanGlobalTrap 10 }

		-- 1.3.6.1.4.1.2011.6.139.12.3.1.11
		hwWlanWapiCertificateNearlyExpiredTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanWapiSecurityProfileName, hwWlanWapiCertType, hwWlanWapiCertFileName, hwWlanWapiCertStartTime, hwWlanWapiCertEndTime }
			STATUS current
			DESCRIPTION 
				"The WAPI certificate is nearly expired."
			::= { hwWlanGlobalTrap 11 }            

		-- 1.3.6.1.4.1.2011.6.139.12.3.1.12            
		hwWlanWapiCertificateNearlyExpiredTrapRestore NOTIFICATION-TYPE
			OBJECTS { hwWlanWapiSecurityProfileName, hwWlanWapiCertType }
			STATUS current
			DESCRIPTION 
				"The alarm of the WAPI certificate reaching expiration is cleared."
			::= { hwWlanGlobalTrap 12 }    
            
 		-- 1.3.6.1.4.1.2011.6.139.12.3.1.13
		hwWlanWapiCertificateInvalidTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanWapiSecurityProfileName, hwWlanWapiCertType, hwWlanWapiCertFileName, hwWlanWapiCertStartTime, hwWlanWapiCertEndTime }
			STATUS current
			DESCRIPTION 
				"The WAPI certificate is invalid."
			::= { hwWlanGlobalTrap 13 }       

 		-- 1.3.6.1.4.1.2011.6.139.12.3.1.14
		hwWlanWapiCertificateInvalidTrapRestore NOTIFICATION-TYPE
			OBJECTS { hwWlanWapiSecurityProfileName, hwWlanWapiCertType }
			STATUS current
			DESCRIPTION 
				"The alarm of the WAPI certificate out of the invalidity period is cleared."
			::= { hwWlanGlobalTrap 14 }  
            
		-- 1.3.6.1.4.1.2011.6.139.12.3.2
		hwWlanGlobalTrapObjects OBJECT IDENTIFIER ::= { hwWlanGlobalTrapInfo 2 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.2.1
		hwWlanShareLicAcMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The mac address of the shared AC"
			::= { hwWlanGlobalTrapObjects 1 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.2.2
		hwWlanShareLicNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The number of shared license."
			::= { hwWlanGlobalTrapObjects 2 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.2.3
		hwWlanPoolTotalLicNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The total number in license pool."
			::= { hwWlanGlobalTrapObjects 3 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.2.4
		hwWlanPoolSelfShareLicNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The total number of self shared in license pool ."
			::= { hwWlanGlobalTrapObjects 4 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.2.5
		hwWlanStaMaxNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the maximum specifications of stations."
			::= { hwWlanGlobalTrapObjects 5 }
		
		-- 1.3.6.1.4.1.2011.6.139.12.3.2.6
		hwWlanStaCurNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of associated stations."
			::= { hwWlanGlobalTrapObjects 6 }

		-- 1.3.6.1.4.1.2011.6.139.12.3.2.7
		hwWlanWapiSecurityProfileName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the name of security profile."
			::= { hwWlanGlobalTrapObjects 7 }	

		-- 1.3.6.1.4.1.2011.6.139.12.3.2.8
		hwWlanWapiCertType OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the type of WAPI certificate."
			::= { hwWlanGlobalTrapObjects 8 }	

		-- 1.3.6.1.4.1.2011.6.139.12.3.2.9
		hwWlanWapiCertFileName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the file name of WAPI certificate."
			::= { hwWlanGlobalTrapObjects 9 }

		-- 1.3.6.1.4.1.2011.6.139.12.3.2.10
		hwWlanWapiCertStartTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the start time of WAPI certificate validity."
			::= { hwWlanGlobalTrapObjects 10 }     

		-- 1.3.6.1.4.1.2011.6.139.12.3.2.11
		hwWlanWapiCertEndTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the end time of WAPI certificate validity."
			::= { hwWlanGlobalTrapObjects 11 }              
	END
--
-- HUAWEI-WLAN-GLOBAL-MIB.mib
--












