       ADTRAN-AOS-VQM DEFINITIONS ::= BEGIN

       IMPORTS
           TimeTicks, IpAddress, Integer32, Gauge32, Unsigned32, Counter32,
           Counter64, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE
               FROM SNMPv2-SMI
           DisplayString, TruthValue, DateAndTime, TEXTUAL-CONVENTION
               FROM SNMPv2-TC
           MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
               FROM SNMPv2-CONF
           ifIndex
                FROM IF-MIB
           adIdentity
               FROM ADTRAN-MIB
           adGenAOSConformance, adGenAOSVoice
               FROM ADTRAN-AOS;

       adGenAOSVQMMib MODULE-IDENTITY
        LAST-UPDATED "200901060000Z"  -- Jan 6, 2009 / YYYYMMDDHHMMZ
        ORGANIZATION "ADTRAN, Inc."
        CONTACT-INFO
               "Technical Support Dept.
                Postal: ADTRAN, Inc.
                901 Explorer Blvd.
                Huntsville, AL 35806

                Tel: +1 800 726-8663
                Fax: +1 256 963 6217
                E-mail: support@adtran.com"

            DESCRIPTION
                "ADTRAN-AOS-VQM MIB module."

       ::= { adIdentity 10000 53 5 3 }

        adVQM                   OBJECT IDENTIFIER ::= { adGenAOSVoice 3 }
        adVQMTrap               OBJECT IDENTIFIER ::= { adVQM 0 }
        adVQMTrapControl        OBJECT IDENTIFIER ::= { adVQM 1 }
        adVQMCfg                OBJECT IDENTIFIER ::= { adVQM 2 }
        adVQMThreshold          OBJECT IDENTIFIER ::= { adVQM 3 }
        adVQMSysPerf            OBJECT IDENTIFIER ::= { adVQM 4 }
        adVQMInterface          OBJECT IDENTIFIER ::= { adVQM 5 }
        adVQMEndPoint           OBJECT IDENTIFIER ::= { adVQM 6 }
        adVQMHistory            OBJECT IDENTIFIER ::= { adVQM 7 }
        adVQMActive             OBJECT IDENTIFIER ::= { adVQM 8 }

-- ========================================================================
        MOSvalue ::= TEXTUAL-CONVENTION
                DISPLAY-HINT "d"
                STATUS  current
                DESCRIPTION
                        "MOS values typically are represented as a value from
                        1.00-5.00. In this representation the MOS score will be
                        scaled by 100.  Hence a value of 3.25 will be
                        represented as 325. A value of 65535 shall be
                        interpreted as NULL or unsupported."
                SYNTAX  Integer32 (100..1000|65535)

        Percentage ::= TEXTUAL-CONVENTION
                DISPLAY-HINT "d"
                STATUS  current
                DESCRIPTION
                        "Percentages typically are represented as a value from
                        0.00%-100.00%. In this representation the percentage
                        will be scaled by 100.  Hence a value of 0.45 will be
                        represented as 45 and a value of 100.00 will be
                        represented as 1000. A value of 65535 shall be
                        interpreted as NULL or unsupported."
                SYNTAX  Integer32 (0..1000|65535)

        MsecValue ::= TEXTUAL-CONVENTION
                DISPLAY-HINT "d"
                STATUS  current
                DESCRIPTION
                        "Millisecond values typically are represented as a
                        value with a decimal place.
                        In this representation th value will be
                        scaled by 10.  Hence a value of 1.5 will be represented
                        as 15."
                SYNTAX  Integer32



     adVQMEndOfCallTrap NOTIFICATION-TYPE
         OBJECTS  {
                adVqmTrapEventType,
                adVqmCallHistMosLq,
                adVqmCallHistMosPq,
                adVqmCallHistPktsLostTotal,
                adVqmCallHistOutOfOrder,
                adVqmCallHistPdvAverageMs
         }
         STATUS      current
         DESCRIPTION
            "This trap indicates that the severity level has been met at the
            end of a call to generate a trap. Enable this trap using
            adVqmTrapState. The severity level, by default, is set to warning.
            Use adVqmTrapCfgSeverityLevel to change the severity level setting."
     ::= { adVQMTrap 1 }


     adVqmTrapState OBJECT-TYPE
         SYNTAX  INTEGER     { enabled(1), disabled(2) }
         MAX-ACCESS   read-write
         STATUS   current
         DESCRIPTION
            "This variable indicates whether the system produces
            the vqmEndOfCall trap."
         DEFVAL { disabled }
         ::= { adVQMTrapControl 1 }

     adVqmTrapCfgSeverityLevel OBJECT-TYPE
         SYNTAX  INTEGER     {
                        error(1),
                        warning(2),
                        notice(3),
                        info(4)
                         }
         MAX-ACCESS   read-write
         STATUS   current
         DESCRIPTION
            "This read-write variable indicates the severity level that will
            generate an adVqmEndOfCallTrap. If traps are enabled, a trap will be
            generated at the end of a call for all calls that have a numerical
            severity level equal to or less than the configured
            severity level."
         DEFVAL { warning }
         ::= { adVQMTrapControl 2 }

     adVqmTrapEventType OBJECT-TYPE
        SYNTAX  BITS {
                        lQMos(0),
                        pQMos(1),
                        loss(2),
                        outOfOrder(3),
                        jitter(4)
        }
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "This variable indicates the event that generated the most
                recent trap. The vqmTrapEventType is a bitmap and can represent
                multiple failures simultaneously.
                The various bit positions are:
                BIT   EVENT      DESCRIPTION
                0     LQMos      LQ-MOS threshold exceeded
                1     PQMos      PQ-MOS threshold exceeded
                2     Loss       Loss threshold exceeded
                3     OutOfOrder Out-of-Order threshold exceeded
                4     Jitter     Jitter threshold exceeded
                "
         ::= { adVQMTrapControl 3 }

     -- adVQMCfg Group
     adVqmCfgEnable OBJECT-TYPE
        SYNTAX  INTEGER {
                enabled (1),
                disabled (2)
                }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "VQM feature global enable/disable."
         ::= { adVQMCfg 1 }

     adVqmCfgSipEnable OBJECT-TYPE
        SYNTAX  INTEGER {
                enabled (1),
                disabled (2)
                }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "VQM uses SIP signaling to monitor for RTP traffic."
         ::= { adVQMCfg 2 }

     adVqmCfgUdpEnable OBJECT-TYPE
        SYNTAX  INTEGER {
                enabled (1),
                disabled (2)
                }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "VQM uses UDP packet inspection to monitor for RTP
                traffic."
         ::= { adVQMCfg 3 }

     adVqmCfgInternationalCode OBJECT-TYPE
        SYNTAX  INTEGER {
                none (1),
                japan (5)
                }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Regional scoring adjustment for VQM calculations."
         ::= { adVQMCfg 4 }

     adVqmCfgJitterBufferType OBJECT-TYPE
        SYNTAX  INTEGER {
                jitterBufferFixed (1),
                jitterBufferAdaptive (2),
                jitterBufferUnknown (3)
                }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Regional scoring adjustment for VQM calculations."
         ::= { adVQMCfg 5 }

     adVqmCfgJitterBufferAdaptiveMin OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Minimum adaptive jitter buffer delay (10-240 ms)."
         ::= { adVQMCfg 6 }

     adVqmCfgJitterBufferAdaptiveNominal OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Adaptive starting delay applied to packets (10-240 ms)."
         ::= { adVQMCfg 7 }

     adVqmCfgJitterBufferAdaptiveMax OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Adaptive maximum jitter buffer delay (40-320 ms)."
         ::= { adVQMCfg 8 }

     adVqmCfgJitterBufferFixedNominal OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Fixed jitter buffer constant delay applied to packets
                (4-250 ms)."
         ::= { adVQMCfg 9 }

     adVqmCfgJitterBufferFixedSize OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Number packets fixed jitter buffer can hold (10-500 pkts)."
         ::= { adVQMCfg 10 }

     adVqmCfgJitterBufferThresholdEarlyMs OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Jitter buffer threshold for early arriving packets."
         ::= { adVQMCfg 11 }

     adVqmCfgJitterBufferThresholdLateMs OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Jitter buffer threshold for late arriving packets."
         ::= { adVQMCfg 12 }

     adVqmCfgRoundTripPingEnabled OBJECT-TYPE
        SYNTAX  INTEGER {
                enabled (1),
                disabled (2)
                }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Ping use for measuring round-trip delay between
                end-points."
         ::= { adVQMCfg 13 }

     adVqmCfgRoundTripPingType OBJECT-TYPE
        SYNTAX  INTEGER {
                ping (1),
                timestamp (2)
                }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "ICMP Ping or ICMP Timestamp used for delay measurements."
         ::= { adVQMCfg 14 }

     adVqmCfgCallHistorySize OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Size of Call History buffer."
         ::= { adVQMCfg 15 }

     adVqmCfgHistoryThresholdLqmos OBJECT-TYPE
        SYNTAX          MOSvalue
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Store history statistics if below LQ MOS threshold value."
         ::= { adVQMCfg 16 }

     adVqmCfgHistoryThresholdCqmos OBJECT-TYPE
        SYNTAX          MOSvalue
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Store history statistics if below CQ MOS threshold value."
         ::= { adVQMCfg 17 }

     adVqmCfgHistoryThresholdPqmos OBJECT-TYPE
        SYNTAX          MOSvalue
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Store history statistics if below PESQ MOS threshold
                value."
         ::= { adVQMCfg 18 }

     adVqmCfgHistoryThresholdLoss OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Store history statistics if loss packets are greater than
                threshold value."
         ::= { adVQMCfg 19 }

     adVqmCfgHistoryThresholdOutOfOrder OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Store history statistics if Out of Order packets are greater
                than threshold value."
         ::= { adVQMCfg 20 }

     adVqmCfgHistoryThresholdJitter OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Store history statistics if Jitter exceeds threshold value."
         ::= { adVQMCfg 21 }

     adVqmCfgClear OBJECT-TYPE
        SYNTAX INTEGER {
                clear (1)
        }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
            "Clear all VQM statistics.
            This is a write-only variable. A read will result in no action
            being taken."
         ::= { adVQMCfg 22 }

     adVqmCfgClearCallHistory OBJECT-TYPE
        SYNTAX INTEGER {
                clear (1)
        }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
            "Clear only call history buffer.
            This is a write-only variable. A read will result in no action
            being taken."
         ::= { adVQMCfg 23 }



     --
     -- adVQMThreshold Group
     --

     adVqmThresholdLqmosInfo OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening Quality MOS threshold value for info event."
         ::= { adVQMThreshold 1 }

     adVqmThresholdLqmosNotice OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening Quality MOS threshold value for notice event."
         ::= { adVQMThreshold 2 }

     adVqmThresholdLqmosWarning OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening Quality MOS threshold value for warning event."
         ::= { adVQMThreshold 3 }

     adVqmThresholdLqmosError OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening Quality MOS threshold value for error event."
         ::= { adVQMThreshold 4 }

     adVqmThresholdPqmosInfo OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Normalized PESQ MOS threshold value for info event."
         ::= { adVQMThreshold 5 }

     adVqmThresholdPqmosNotice OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Normalized PESQ MOS threshold value for notice event."
         ::= { adVQMThreshold 6 }

     adVqmThresholdPqmosWarning OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Normalized PESQ MOS threshold value for warning event."
         ::= { adVQMThreshold 7 }

     adVqmThresholdPqmosError OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Normalized PESQ MOS threshold value for error event."
         ::= { adVQMThreshold 8 }

     adVqmThresholdOutOfOrderInfo OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Out of order packet threshold value for info event."
         ::= { adVQMThreshold 9 }

     adVqmThresholdOutOfOrderNotice OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Out of order packet threshold value for notice event."
         ::= { adVQMThreshold 10 }

     adVqmThresholdOutOfOrderWarning OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Out of order packet threshold value for warning event."
         ::= { adVQMThreshold 11 }

     adVqmThresholdOutOfOrderError OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Out of order packet threshold value for error event."
         ::= { adVQMThreshold 12 }

     adVqmThresholdLossInfo OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Loss of packet threshold value for info event."
         ::= { adVQMThreshold 13 }

     adVqmThresholdLossNotice OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Loss of packet threshold value for notice event."
         ::= { adVQMThreshold 14 }

     adVqmThresholdLossWarning OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Loss of packet threshold value for warning event."
         ::= { adVQMThreshold 15 }

     adVqmThresholdLossError OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Loss of packet threshold value for error event."
         ::= { adVQMThreshold 16 }

     adVqmThresholdJitterInfo OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Jitter threshold value for info event."
         ::= { adVQMThreshold 17 }

     adVqmThresholdJitterNotice OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Jitter threshold value for notice event."
         ::= { adVQMThreshold 18 }

     adVqmThresholdJitterWarning OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Jitter threshold value for warning event."
         ::= { adVQMThreshold 19 }

     adVqmThresholdJitterError OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Jitter threshold value for error event."
         ::= { adVQMThreshold 20 }



        --
        -- adVQMSysPerf Group
        --

     adVqmSysActiveCalls OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of active calls."
         ::= { adVQMSysPerf 1 }

     adVqmSysActiveExcellent OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Active calls in excellent MOS range (4.400 - 4.000)."
         ::= { adVQMSysPerf 2 }

     adVqmSysActiveGood OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Active calls in good MOS range (3.999 - 3.600)."
         ::= { adVQMSysPerf 3 }

     adVqmSysActiveFair OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Active calls in fair MOS range (3.599 - 2.600)."
         ::= { adVQMSysPerf 4 }

     adVqmSysActivePoor OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Active calls in poor MOS range (2.599 - 0.000)."
         ::= { adVQMSysPerf 5 }

     adVqmSysCallHistoryCalls OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of calls in history buffer."
         ::= { adVQMSysPerf 6 }

     adVqmSysCallHistoryExcellent OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "History calls in excellent MOS range."
         ::= { adVQMSysPerf 7 }

     adVqmSysCallHistoryGood OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "History calls in good MOS range."
         ::= { adVQMSysPerf 8 }

     adVqmSysCallHistoryFair OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "History calls in fair MOS range."
         ::= { adVQMSysPerf 9 }

     adVqmSysCallHistoryPoor OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "History calls in poor MOS range."
         ::= { adVQMSysPerf 10 }

     adVqmSysAllCallsExcellent OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total calls in excellent MOS range."
         ::= { adVQMSysPerf 11 }

     adVqmSysAllCallsGood OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total calls in good MOS range."
         ::= { adVQMSysPerf 12 }

     adVqmSysAllCallsFair OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total calls in fair MOS range."
         ::= { adVQMSysPerf 13 }

     adVqmSysAllCallsPoor OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total calls in poor MOS range."
         ::= { adVQMSysPerf 14 }

     --
     -- adVQMInterfaceTable
     --

     adVQMInterfaceTable OBJECT-TYPE
         SYNTAX         SEQUENCE OF AdVQMInterfaceEntry
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
            "The adVqmInterface table provides aggregate statistics for each
            system interface.  VQM processes RTP stream packets as received by
            the interface (inbound direction).  The user can enable or disable
            each system interface for VQM using the CLI/GUI.  The VQM interface
            table objects include enable/disable, packet statistics for number
            received, lost, out-of-order, discarded, number of active and
            completed calls, MOS scores, delay measurements, and quality
            analysis counts."
         ::= { adVQMInterface 1 }

     adVQMInterfaceEntry OBJECT-TYPE
         SYNTAX   AdVQMInterfaceEntry
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "The statistics for a particular interface."
         INDEX { adVqmIfcId }
         ::= { adVQMInterfaceTable 1 }


     AdVQMInterfaceEntry ::=
        SEQUENCE {
                adVqmIfcId                      Unsigned32,
                adVqmIfcName                    DisplayString,
                adVqmIfcPktsRx                  Counter64,
                adVqmIfcPktsLost                Counter64,
                adVqmIfcPktsOoo                 Counter64,
                adVqmIfcPktsDiscarded           Counter64,
                adVqmIfcNumberActiveCalls       Counter32,
                adVqmIfcTerminatedCalls         Counter32,
                adVqmIfcRLqMinimum              Unsigned32,
                adVqmIfcRLqAverage              Unsigned32,
                adVqmIfcRLqMaximum              Unsigned32,
                adVqmIfcRCqMinimum              Unsigned32,
                adVqmIfcRCqAverage              Unsigned32,
                adVqmIfcRCqMaximum              Unsigned32,
                adVqmIfcRG107Minimum            Unsigned32,
                adVqmIfcRG107Average            Unsigned32,
                adVqmIfcRG107Maximum            Unsigned32,
                adVqmIfcMosLqMinimum            MOSvalue,
                adVqmIfcMosLqAverage            MOSvalue,
                adVqmIfcMosLqMaximum            MOSvalue,
                adVqmIfcMosCqMinimum            MOSvalue,
                adVqmIfcMosCqAverage            MOSvalue,
                adVqmIfcMosCqMaximum            MOSvalue,
                adVqmIfcMosPqMinimum            MOSvalue,
                adVqmIfcMosPqAverage            MOSvalue,
                adVqmIfcMosPqMaximum            MOSvalue,
                adVqmIfcLossMinimum             Unsigned32,
                adVqmIfcLossAverage             Unsigned32,
                adVqmIfcLossMaximum             Unsigned32,
                adVqmIfcDiscardsMinimum         Unsigned32,
                adVqmIfcDiscardsAverage         Unsigned32,
                adVqmIfcDiscardsMaximum         Unsigned32,
                adVqmIfcPdvAverageMs            INTEGER,
                adVqmIfcPdvMaximumMs            INTEGER,
                adVqmIfcDelayMinMsec            Unsigned32,
                adVqmIfcDelayAvgMsec            Unsigned32,
                adVqmIfcDelayMaxMsec            Unsigned32,
                adVqmIfcNumberStreamsExcellent  Counter32,
                adVqmIfcNumberStreamsGood       Counter32,
                adVqmIfcNumberStreamsFair       Counter32,
                adVqmIfcNumberStreamsPoor       Counter32,
                adVqmIfcClear                   INTEGER
     }

     adVqmIfcId OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "VQM interface index number. This number is unique to the VQM MIB."
         ::= { adVQMInterfaceEntry 1 }


     adVqmIfcName OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Interface name."
         ::= { adVQMInterfaceEntry 2 }

     adVqmIfcPktsRx OBJECT-TYPE
         SYNTAX         Counter64
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Packets received."
         ::= { adVQMInterfaceEntry 3 }

     adVqmIfcPktsLost OBJECT-TYPE
         SYNTAX         Counter64
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Packets lost."
         ::= { adVQMInterfaceEntry 4 }

     adVqmIfcPktsOoo OBJECT-TYPE
         SYNTAX         Counter64
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Packets received out-of-order."
         ::= { adVQMInterfaceEntry 5 }

     adVqmIfcPktsDiscarded OBJECT-TYPE
         SYNTAX         Counter64
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Packets discarded."
         ::= { adVQMInterfaceEntry 6 }

     adVqmIfcNumberActiveCalls OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of active calls."
         ::= { adVQMInterfaceEntry 7 }

     adVqmIfcTerminatedCalls OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of terminated calls."
         ::= { adVQMInterfaceEntry 8 }

     adVqmIfcRLqMinimum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum listening quality R Factor."
         ::= { adVQMInterfaceEntry 9 }

     adVqmIfcRLqAverage OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average listening quality R Factor."
         ::= { adVQMInterfaceEntry 10 }

     adVqmIfcRLqMaximum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum listening quality R Factor."
         ::= { adVQMInterfaceEntry 11 }

     adVqmIfcRCqMinimum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum conversation quality R Factor."
         ::= { adVQMInterfaceEntry 12 }

     adVqmIfcRCqAverage OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average conversation quality R Factor."
         ::= { adVQMInterfaceEntry 13 }

     adVqmIfcRCqMaximum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum conversation quality R Factor."
         ::= { adVQMInterfaceEntry 14 }

     adVqmIfcRG107Minimum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum G.107 R Factor."
         ::= { adVQMInterfaceEntry 15 }

     adVqmIfcRG107Average OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average G.107 R Factor."
         ::= { adVQMInterfaceEntry 16 }

     adVqmIfcRG107Maximum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum G.107 R Factor."
         ::= { adVQMInterfaceEntry 17 }

     adVqmIfcMosLqMinimum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum listening quality MOS score."
         ::= { adVQMInterfaceEntry 18 }

     adVqmIfcMosLqAverage OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average listening quality MOS score."
         ::= { adVQMInterfaceEntry 19 }

     adVqmIfcMosLqMaximum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum listening quality MOS score."
         ::= { adVQMInterfaceEntry 20 }

     adVqmIfcMosCqMinimum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum conversation quality MOS score."
         ::= { adVQMInterfaceEntry 21 }

     adVqmIfcMosCqAverage OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average conversation quality MOS score."
         ::= { adVQMInterfaceEntry 22 }

     adVqmIfcMosCqMaximum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum conversation quality MOS score."
         ::= { adVQMInterfaceEntry 23 }

     adVqmIfcMosPqMinimum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum PESQ, P.862 raw MOS score."
         ::= { adVQMInterfaceEntry 24 }

     adVqmIfcMosPqAverage OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average PESQ, P.862 raw MOS score."
         ::= { adVQMInterfaceEntry 25 }

     adVqmIfcMosPqMaximum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum PESQ, P.862 raw MOS score."
         ::= { adVQMInterfaceEntry 26 }

     adVqmIfcLossMinimum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum network lost packets for all calls completed."
         ::= { adVQMInterfaceEntry 27 }

     adVqmIfcLossAverage OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average network lost packets for all calls completed."
         ::= { adVQMInterfaceEntry 28 }

     adVqmIfcLossMaximum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum network lost packets for all calls completed."
         ::= { adVQMInterfaceEntry 29 }

     adVqmIfcDiscardsMinimum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum packets discarded due to late or early arrival."
         ::= { adVQMInterfaceEntry 30 }

     adVqmIfcDiscardsAverage OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average packets discarded due to late or early arrival."
         ::= { adVQMInterfaceEntry 31 }

     adVqmIfcDiscardsMaximum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum packets discarded due to late or early arrival."
         ::= { adVQMInterfaceEntry 32 }

     adVqmIfcPdvAverageMs OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Mean of Average packet delay variation for packets."
         ::= { adVQMInterfaceEntry 33 }

     adVqmIfcPdvMaximumMs OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum of reported average packet delay variation."
         ::= { adVQMInterfaceEntry 34 }

     adVqmIfcDelayMinMsec OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum packet delay in ms."
         ::= { adVQMInterfaceEntry 35 }

     adVqmIfcDelayAvgMsec OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average packet delay in ms."
         ::= { adVQMInterfaceEntry 36 }

     adVqmIfcDelayMaxMsec OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum packet delay in ms."
         ::= { adVQMInterfaceEntry 37 }

     adVqmIfcNumberStreamsExcellent OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with excellent MOS score."
         ::= { adVQMInterfaceEntry 38 }

     adVqmIfcNumberStreamsGood OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with good MOS score."
         ::= { adVQMInterfaceEntry 39 }

     adVqmIfcNumberStreamsFair OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with fair MOS score."
         ::= { adVQMInterfaceEntry 40 }

     adVqmIfcNumberStreamsPoor OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with poor MOS score."
         ::= { adVQMInterfaceEntry 41 }

     adVqmIfcClear OBJECT-TYPE
        SYNTAX INTEGER {
                clear (1)
        }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
            "Clear all VQM statistics.
            This is a write-only variable. A read will result in no action
            being taken."
         ::= { adVQMInterfaceEntry 42 }

     --
     -- adVqmEndPoint
     --

     adVQMEndPointTable OBJECT-TYPE
         SYNTAX         SEQUENCE OF AdVQMEndPointEntry
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
            "The adVqmEndPoint table provides aggregate statistics for each
            VoIP end-point device.  The RTP Source IP address,
            adVqmEndPointRtpSourceIp, provides a unique table index.
            The VQM End-point table provides summary statistics for MOS scores,
            packets lost, out-of-order, jitter, delay and quality analysis
            counts."
         ::= { adVQMEndPoint 1 }

     adVQMEndPointEntry OBJECT-TYPE
         SYNTAX   AdVQMEndPointEntry
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "The statistics for a particular VoIP end-point device."
         INDEX { adVqmEndPointRtpSourceIp }
         ::= { adVQMEndPointTable 1 }


     AdVQMEndPointEntry ::=
        SEQUENCE {
                adVqmEndPointRtpSourceIp                IpAddress,
                adVqmEndPointNumberCompletedCalls       Counter32,
                adVqmEndPointInterfaceId                Unsigned32,
                adVqmEndPointInterfaceName              DisplayString,
                adVqmEndPointMosLqMinimum               MOSvalue,
                adVqmEndPointMosLqAverage               MOSvalue,
                adVqmEndPointMosLqMaximum               MOSvalue,
                adVqmEndPointMosPqMinimum               MOSvalue,
                adVqmEndPointMosPqAverage               MOSvalue,
                adVqmEndPointMosPqMaximum               MOSvalue,
                adVqmEndPointPktsLostTotal              Counter32,
                adVqmEndPointPktsOutOfOrder             Counter32,
                adVqmEndPointJitterMaximum              Unsigned32,
                adVqmEndPointNumberStreamsExcellent     Counter32,
                adVqmEndPointNumberStreamsGood          Counter32,
                adVqmEndPointNumberStreamsFair          Counter32,
                adVqmEndPointNumberStreamsPoor          Counter32
     }

     adVqmEndPointRtpSourceIp OBJECT-TYPE
         SYNTAX         IpAddress
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source IP Address of RTP stream from this end-point."
         ::= { adVQMEndPointEntry 1 }

     adVqmEndPointNumberCompletedCalls OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of completed calls on this end-point."
         ::= { adVQMEndPointEntry 2 }

     adVqmEndPointInterfaceId OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Interface index that received RTP stream from this end-point."
         ::= { adVQMEndPointEntry 3 }

     adVqmEndPointInterfaceName OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Interface name that received RTP stream from this end-point."
         ::= { adVQMEndPointEntry 4 }

     adVqmEndPointMosLqMinimum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum listening quality MOS score."
         ::= { adVQMEndPointEntry 5 }

     adVqmEndPointMosLqAverage OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average listening quality MOS score."
         ::= { adVQMEndPointEntry 6 }

     adVqmEndPointMosLqMaximum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum listening quality MOS score."
         ::= { adVQMEndPointEntry 7 }

     adVqmEndPointMosPqMinimum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Minimum PESQ MOS score."
         ::= { adVQMEndPointEntry 8 }

     adVqmEndPointMosPqAverage OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average PESQ MOS score."
         ::= { adVQMEndPointEntry 9 }

     adVqmEndPointMosPqMaximum OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum PESQ MOS score."
         ::= { adVQMEndPointEntry 10 }

     adVqmEndPointPktsLostTotal OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total packets lost."
         ::= { adVQMEndPointEntry 11 }

     adVqmEndPointPktsOutOfOrder OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total out-of-order packets."
         ::= { adVQMEndPointEntry 12 }

     adVqmEndPointJitterMaximum OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum jitter."
         ::= { adVQMEndPointEntry 13 }

     adVqmEndPointNumberStreamsExcellent OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with excellent MOS score."
         ::= { adVQMEndPointEntry 14 }

     adVqmEndPointNumberStreamsGood OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with good MOS score."
         ::= { adVQMEndPointEntry 15 }

     adVqmEndPointNumberStreamsFair OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with fair MOS score."
         ::= { adVQMEndPointEntry 16 }

     adVqmEndPointNumberStreamsPoor OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number voice streams with poor MOS score."
         ::= { adVQMEndPointEntry 17 }

     --
     -- adVqmCallHistory
     --

     adVQMCallHistoryTable OBJECT-TYPE
         SYNTAX         SEQUENCE OF AdVQMCallHistoryEntry
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
            "The adVqmCallHistory table provides detail voice quality statistics
            on completed RTP voice streams.  A voice call will typically have
            two entries in this table one for each RTP stream.  A combination
            of Source IP Address and Port, Destination IP Address and Port,
            and SSRC (synchronization source ID) are necessary to uniquely
            identify the call session.
            One management option is to configure VQM to only save call history
            information for poor quality calls that exceed threshold limits.
            Threshold limit settings are available for MOS scores and packet
            statistics for loss, out-of-order, and jitter.  Setting the maximum
            call history buffer size to a lower value (default is 100 streams)
            can reduce the amount of data transfer to the NMS during a
            SNMP query."
         ::= { adVQMHistory 1 }

     adVQMCallHistoryEntry OBJECT-TYPE
         SYNTAX   AdVQMCallHistoryEntry
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "The statistics for a particular VoIP end-point device."
         INDEX { adVqmCallHistRtpSourceIp, adVqmCallHistRtpSourcePort,
                adVqmCallHistRtpDestIp, adVqmCallHistRtpDestPort,
                adVqmCallHistSsrcid }
         ::= { adVQMCallHistoryTable 1 }

     AdVQMCallHistoryEntry ::=
        SEQUENCE {
                adVqmCallHistRtpSourceIp                IpAddress,
                adVqmCallHistRtpSourcePort              Unsigned32,
                adVqmCallHistRtpDestIp                  IpAddress,
                adVqmCallHistRtpDestPort                Unsigned32,
                adVqmCallHistSsrcid                     Unsigned32,
                adVqmCallHistTo                         DisplayString,
                adVqmCallHistFrom                       DisplayString,
                adVqmCallHistRtpSourceUri               DisplayString,
                adVqmCallHistCallid                     DisplayString,
                adVqmCallHistCcmid                      Unsigned32,
                adVqmCallHistSourceIntName              DisplayString,
                adVqmCallHistDestIntName                DisplayString,
                adVqmCallHistSourceIntDescription       DisplayString,
                adVqmCallHistDestIntDescription         DisplayString,
                adVqmCallHistCallStart                  DisplayString,
                adVqmCallHistCallDurationMs             Unsigned32,
                adVqmCallHistCodec                      INTEGER,
                adVqmCallHistCodecClass                 INTEGER,
                adVqmCallHistDscp                       Unsigned32,
                adVqmCallHistPktsRcvdTotal              Counter32,
                adVqmCallHistPktsLostTotal              Counter32,
                adVqmCallHistPktsDiscardedTotal         Counter32,
                adVqmCallHistOutOfOrder                 Counter32,
                adVqmCallHistPdvAverageMs               Unsigned32,
                adVqmCallHistPdvMaximumMs               Unsigned32,
                adVqmCallHistRtDelayInst                INTEGER,
                adVqmCallHistRtDelayAverage             INTEGER,
                adVqmCallHistRtDelayMaximum             INTEGER,
                adVqmCallHistOnewayDelayInst            INTEGER,
                adVqmCallHistOnewayDelayAverage         INTEGER,
                adVqmCallHistOnewayDelayMaximum         INTEGER,
                adVqmCallHistOrigDelayInst              INTEGER,
                adVqmCallHistOrigDelayAverage           INTEGER,
                adVqmCallHistOrigDelayMaximum           INTEGER,
                adVqmCallHistTermDelayMinimum           INTEGER,
                adVqmCallHistTermDelayAverage           INTEGER,
                adVqmCallHistTermDelayMaximum           INTEGER,
                adVqmCallHistRLq                        Unsigned32,
                adVqmCallHistRCq                        Unsigned32,
                adVqmCallHistRNominal                   Unsigned32,
                adVqmCallHistRG107                      Unsigned32,
                adVqmCallHistMosLq                      MOSvalue,
                adVqmCallHistMosCq                      MOSvalue,
                adVqmCallHistMosPq                      MOSvalue,
                adVqmCallHistMosNominal                 MOSvalue,
                adVqmCallHistDegLoss                    Percentage,
                adVqmCallHistDegDiscard                 Percentage,
                adVqmCallHistDegVocoder                 Percentage,
                adVqmCallHistDegRecency                 Percentage,
                adVqmCallHistDegDelay                   Percentage,
                adVqmCallHistDegSiglvl                  Percentage,
                adVqmCallHistDegNoiselvl                Percentage,
                adVqmCallHistDegEcholvl                 Percentage,
                adVqmCallHistBurstRLq                   Unsigned32,
                adVqmCallHistBurstCount                 Counter32,
                adVqmCallHistBurstRateAvg               Percentage,
                adVqmCallHistBurstLenAvgPkts            Unsigned32,
                adVqmCallHistBurstLenAvgMsec            Unsigned32,
                adVqmCallHistGapR                       Unsigned32,
                adVqmCallHistGapCount                   Counter32,
                adVqmCallHistGapLossRateAvg             Percentage,
                adVqmCallHistGapLenPkts                 Unsigned32,
                adVqmCallHistGapLenMsec                 Unsigned32,
                adVqmCallHistLossRateAvg                Percentage,
                adVqmCallHistNetworkLossAvg             Percentage,
                adVqmCallHistDiscardRateAvg             Percentage,
                adVqmCallHistExcessBurst                Unsigned32,
                adVqmCallHistExcessGap                  Unsigned32,
                adVqmCallHistPpdvMsec                   MsecValue,
                adVqmCallHistLateThresholdMs            MsecValue,
                adVqmCallHistLateThresholdPc            Percentage,
                adVqmCallHistLateUnderThresh            Counter32,
                adVqmCallHistLateTotalCount             Counter32,
                adVqmCallHistLatePeakJitterMs           MsecValue,
                adVqmCallHistEarlyThreshMs              MsecValue,
                adVqmCallHistEarlyThreshPc              Percentage,
                adVqmCallHistEarlyUnderThresh           Counter32,
                adVqmCallHistEarlyTotalCount            Counter32,
                adVqmCallHistEarlyPeakJitterMs          MsecValue,
                adVqmCallHistDelayIncreaseCount         Counter32,
                adVqmCallHistDelayDecreaseCount         Counter32,
                adVqmCallHistResyncCount                Counter32,
                adVqmCallHistJitterBufferType           INTEGER,
                adVqmCallHistJbCfgMin                   Unsigned32,
                adVqmCallHistJbCfgNom                   Unsigned32,
                adVqmCallHistJbCfgMax                   Unsigned32,
                adVqmCallHistDuplicatePkts              Counter32,
                adVqmCallHistEarlyPkts                  Counter32,
                adVqmCallHistLatePkts                   Counter32,
                adVqmCallHistOverrunDiscardPkts         Counter32,
                adVqmCallHistUnderrunDiscardPkts        Counter32,
                adVqmCallHistDelayMinMsec               Unsigned32,
                adVqmCallHistDelayAvgMsec               Unsigned32,
                adVqmCallHistDelayMaxMsec               Unsigned32,
                adVqmCallHistDelayCurrentMsec           Unsigned32,
                adVqmCallHistExtRLqIn                   INTEGER,
                adVqmCallHistExtRLqOut                  INTEGER,
                adVqmCallHistExtRCqIn                   INTEGER,
                adVqmCallHistExtRCqOut                  INTEGER,
                adVqmCallHistThroughPutIndex            Unsigned32,
                adVqmCallHistReliabilityIndex           Unsigned32,
                adVqmCallHistBitrate                    Unsigned32
     }

     adVqmCallHistRtpSourceIp OBJECT-TYPE
         SYNTAX         IpAddress
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source IP Address of RTP stream."
         ::= { adVQMCallHistoryEntry 1 }

     adVqmCallHistRtpSourcePort OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source port number."
         ::= { adVQMCallHistoryEntry 2 }

     adVqmCallHistRtpDestIp OBJECT-TYPE
         SYNTAX         IpAddress
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination IP address of RTP stream."
         ::= { adVQMCallHistoryEntry 3 }

     adVqmCallHistRtpDestPort OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination port number."
         ::= { adVQMCallHistoryEntry 4 }

     adVqmCallHistSsrcid OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "SSRC (synchronization source ID) for this stream per RFC3550."
         ::= { adVQMCallHistoryEntry 5 }

     adVqmCallHistTo OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "To URI (dialed) from monitored SIP call signaling."
         ::= { adVQMCallHistoryEntry 6 }

     adVqmCallHistFrom OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "From URI (originating caller) from monitored SIP call signaling."
         ::= { adVQMCallHistoryEntry 7 }

     adVqmCallHistRtpSourceUri OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "URI of sender RTP, either To URI or From URI."
         ::= { adVQMCallHistoryEntry 8 }

     adVqmCallHistCallid OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "SIP call-ID from monitored SIP call signaling."
         ::= { adVQMCallHistoryEntry 9 }

     adVqmCallHistCcmid OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Internal generated call-ID."
         ::= { adVQMCallHistoryEntry 10 }

     adVqmCallHistSourceIntName OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source interface name that RTP arrived inbound to unit."
         ::= { adVQMCallHistoryEntry 11 }

     adVqmCallHistDestIntName OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination interface name for RTP."
         ::= { adVQMCallHistoryEntry 12 }

     adVqmCallHistSourceIntDescription OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source interface description as defined in CLI or GUI."
         ::= { adVQMCallHistoryEntry 13 }

     adVqmCallHistDestIntDescription OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination interface description as defined in CLI or GUI."
         ::= { adVQMCallHistoryEntry 14 }

     adVqmCallHistCallStart OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Time at which monitoring began on this RTP stream."
         ::= { adVQMCallHistoryEntry 15 }

     adVqmCallHistCallDurationMs OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Elapsed time from start to last RTP packet on this stream."
         ::= { adVQMCallHistoryEntry 16 }

     adVqmCallHistCodec OBJECT-TYPE
         SYNTAX         INTEGER
                        {
                        -- -1
                        unknown         (1),
                        -- 0
                        g711U           (2),
                        g711UPLC        (3),
                        g723153K        (4),
                        deprecated1     (5),
                        g723163K        (6),
                        deprecated2     (7),
                        g728            (8),
                        deprecated3     (9),
                        g729            (10),
                        deprecated4     (11),
                        g729A           (12),
                        deprecated5     (13),
                        user1           (14),
                        user2           (15),
                        user3           (16),
                        user4           (17),
                        gsmfr           (18),
                        reservedgsmhr   (19),
                        gsmefr          (20),
                        sx7300          (21),
                        sx9600          (22),
                        g711A           (23),
                        g711APLC        (24),
                        deprecated6     (25),
                        g72616K         (26),
                        g72624K         (27),
                        g72632K         (28),
                        g72640K         (29),
                        gipse711U       (30),
                        gipse711A       (31),
                        gipsilbc        (32),
                        gipsisac        (33),
                        gipsipcmwb      (34),
                        g729E8K0        (35),
                        g729E11k8       (36),
                        wblinearpcm     (37),
                        wblinearpcmPlc  (38),
                        g722at64k       (39),
                        g722at56k       (40),
                        g722at48k       (41),
                        g7221at32k      (42),
                        g7221at24k      (43),
                        g7222at23k85    (44),
                        g7222at23k05    (45),
                        g7222at19k85    (46),
                        g7222at18k25    (47),
                        g7222at15k85    (48),
                        g7222at14k25    (49),
                        g7222at12k85    (50),
                        g7222at8k85     (51),
                        g7222at6k6      (52),
                        qcelp8          (53),
                        qcelp13         (54),
                        evrc            (55),
                        smv812          (56),
                        smv579          (57),
                        smv444          (58),
                        smv395          (59),
                        amrnb12k2       (60),
                        amrnb10k2       (61),
                        amrnb7k95       (62),
                        amrnb7k4        (63),
                        amrnb6k7        (64),
                        amrnb5k9        (65),
                        amrnb5k15       (66),
                        amrnb4k75       (67),
                        ilbc13k3        (68),
                        ilbc15k2        (69),
                        g711u56k        (70),
                        g711uPLC56k     (71),
                        g711A56k        (72),
                        g711APLC56k     (73),
                        g7231C          (74),
                        speex2k15       (75),
                        speex5k95       (76),
                        speeX8k         (77),
                        speeX11k        (78),
                        speeX15k        (79),
                        speeX18k2       (80),
                        speeX24k6       (81),
                        speeX3k95       (82),
                        speeX12k8       (83),
                        speeX16k8       (84),
                        speeX20k6       (85),
                        speeX23k8       (86),
                        speeX27k8       (87),
                        speeX34k2       (88),
                        speeX42k2       (89)
         }
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Last voice CODEC detected on this stream."
         ::= { adVQMCallHistoryEntry 17 }

     adVqmCallHistCodecClass OBJECT-TYPE
         SYNTAX         INTEGER {
                wideband        (1),
                other           (2)
         }
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Class to which CODEC vocoder belongs."
         ::= { adVQMCallHistoryEntry 18 }

     adVqmCallHistDscp OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Differentiated Services Code Point (DSCP) in RTP packet IP header."
         ::= { adVQMCallHistoryEntry 19 }

     adVqmCallHistPktsRcvdTotal OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total received RTP packets in this stream."
         ::= { adVQMCallHistoryEntry 20 }

     adVqmCallHistPktsLostTotal OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total packets determined to be lost in network by simulated jitter
            buffer."
         ::= { adVQMCallHistoryEntry 21 }

     adVqmCallHistPktsDiscardedTotal OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total packets discarded by simulated jitter buffer."
         ::= { adVQMCallHistoryEntry 22 }

     adVqmCallHistOutOfOrder OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total packets received out of order at simulated jitter buffer."
         ::= { adVQMCallHistoryEntry 23 }

     adVqmCallHistPdvAverageMs OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average Packet Delay Variation (PDV) in RTP stream in
            milliseconds."
         ::= { adVQMCallHistoryEntry 24 }

     adVqmCallHistPdvMaximumMs OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum Packet Delay Variation (PDV) in RTP stream in
            milliseconds."
         ::= { adVQMCallHistoryEntry 25 }

     adVqmCallHistRtDelayInst OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous round-trip delay obtained from RTCP or RTCP XR
            reports."
         ::= { adVQMCallHistoryEntry 26 }

     adVqmCallHistRtDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average round-trip delay obtained from RTCP or RTCP XR reports."
         ::= { adVQMCallHistoryEntry 27 }

     adVqmCallHistRtDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum round-trip delay obtained from RTCP or RTCP XR reports."
         ::= { adVQMCallHistoryEntry 28 }

     adVqmCallHistOnewayDelayInst OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous one-way delay including simulated jitter buffer (SJB)
            delay."
         ::= { adVQMCallHistoryEntry 29 }

     adVqmCallHistOnewayDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average one-way delay including SJB delay."
         ::= { adVQMCallHistoryEntry 30 }

     adVqmCallHistOnewayDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum one-way delay including SJB delay."
         ::= { adVQMCallHistoryEntry 31 }

     adVqmCallHistOrigDelayInst OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous origination end-point delay from RTCP XR reports."
         ::= { adVQMCallHistoryEntry 32 }

     adVqmCallHistOrigDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average origination end-point delay from RTCP XR reports."
         ::= { adVQMCallHistoryEntry 33 }

     adVqmCallHistOrigDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum origination end-point delay from RTCP XR reports."
         ::= { adVQMCallHistoryEntry 34 }

     adVqmCallHistTermDelayMinimum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous termination end-point delay, simulated jitter
            buffer + codec."
         ::= { adVQMCallHistoryEntry 35 }

     adVqmCallHistTermDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average termination end-point delay, simulated jitter
            buffer + codec."
         ::= { adVQMCallHistoryEntry 36 }

     adVqmCallHistTermDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum termination end-point delay, simulated jitter
            buffer + codec."
         ::= { adVQMCallHistoryEntry 37 }

     adVqmCallHistRLq OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening quality R factor."
         ::= { adVQMCallHistoryEntry 38 }

     adVqmCallHistRCq OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Conversational quality R factor."
         ::= { adVQMCallHistoryEntry 39 }

     adVqmCallHistRNominal OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Nominal or generally accepted maximum R factor for this stream."
         ::= { adVQMCallHistoryEntry 40 }

     adVqmCallHistRG107 OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "R factor based on ITU G.107 E Model for this stream."
         ::= { adVQMCallHistoryEntry 41 }

     adVqmCallHistMosLq OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening quality MOS score."
         ::= { adVQMCallHistoryEntry 42 }

     adVqmCallHistMosCq OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Conversational quality MOS score."
         ::= { adVQMCallHistoryEntry 43 }

     adVqmCallHistMosPq OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening quality MOS score normalized to the PESQ scale."
         ::= { adVQMCallHistoryEntry 44 }

     adVqmCallHistMosNominal OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Nominal or generally accepted maximum MOS score for this stream."
         ::= { adVQMCallHistoryEntry 45 }

     adVqmCallHistDegLoss OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to packet loss."
         ::= { adVQMCallHistoryEntry 46 }

     adVqmCallHistDegDiscard OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to packet discard."
         ::= { adVQMCallHistoryEntry 47 }

     adVqmCallHistDegVocoder OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to voice CODEC selection."
         ::= { adVQMCallHistoryEntry 48 }

     adVqmCallHistDegRecency OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to loss or discard recency in
            call."
         ::= { adVQMCallHistoryEntry 49 }

     adVqmCallHistDegDelay OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to delay."
         ::= { adVQMCallHistoryEntry 50 }

     adVqmCallHistDegSiglvl OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to low speech energy signal
            level."
         ::= { adVQMCallHistoryEntry 51 }

     adVqmCallHistDegNoiselvl OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to high noise levels."
         ::= { adVQMCallHistoryEntry 52 }

     adVqmCallHistDegEcholvl OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to high echo levels."
         ::= { adVQMCallHistoryEntry 53 }

     adVqmCallHistBurstRLq OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average listening quality R factor during burst condition."
         ::= { adVQMCallHistoryEntry 54 }

     adVqmCallHistBurstCount OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of times the stream was in a burst condition."
         ::= { adVQMCallHistoryEntry 55 }

     adVqmCallHistBurstRateAvg OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost or discarded while in
            burst condition."
         ::= { adVQMCallHistoryEntry 56 }

     adVqmCallHistBurstLenAvgPkts OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average burst length in packets."
         ::= { adVQMCallHistoryEntry 57 }

     adVqmCallHistBurstLenAvgMsec OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average burst length in miliseconds."
         ::= { adVQMCallHistoryEntry 58 }

     adVqmCallHistGapR OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average listening quality R factor while stream is in a gap
            condition."
         ::= { adVQMCallHistoryEntry 59 }

     adVqmCallHistGapCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of times the stream is in gap condition."
         ::= { adVQMCallHistoryEntry 60 }

     adVqmCallHistGapLossRateAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost or discarded while in
            gap condition."
         ::= { adVQMCallHistoryEntry 61 }

     adVqmCallHistGapLenPkts  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average gap length in packets."
         ::= { adVQMCallHistoryEntry 62 }

     adVqmCallHistGapLenMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average gap length in milliseconds."
         ::= { adVQMCallHistoryEntry 63 }

     adVqmCallHistLossRateAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost or discarded."
         ::= { adVQMCallHistoryEntry 64 }

     adVqmCallHistNetworkLossAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost in network, excludes
            SJB discards."
         ::= { adVQMCallHistoryEntry 65 }

     adVqmCallHistDiscardRateAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames discarded by SJB."
         ::= { adVQMCallHistoryEntry 66 }

     adVqmCallHistExcessBurst  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total length of speech lost during burst conditions not handled
            effectively by packet loss-concealment."
         ::= { adVQMCallHistoryEntry 67 }

     adVqmCallHistExcessGap  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total length of speech lost during gap conditions not handled
            effectively by packet loss-concealment."
         ::= { adVQMCallHistoryEntry 68 }

     adVqmCallHistPpdvMsec  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Packet to packed delay variation (jitter) in ms, as defined in
            RFC3550."
         ::= { adVQMCallHistoryEntry 69 }

     adVqmCallHistLateThresholdMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Late threshold for SJB, packets arriving under this threshold are
            not discarded."
         ::= { adVQMCallHistoryEntry 70 }

     adVqmCallHistLateThresholdPc  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage of total packets (including both early and late packets)
            not judged as being under the late jitter threshold."
         ::= { adVQMCallHistoryEntry 71 }

     adVqmCallHistLateUnderThresh  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Count of late packets which arrived under the late jitter
            threshold."
         ::= { adVQMCallHistoryEntry 72 }

     adVqmCallHistLateTotalCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total count of late packets arriving after the expected delay."
         ::= { adVQMCallHistoryEntry 73 }

     adVqmCallHistLatePeakJitterMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Largest jitter encountered among packets counted as late."
         ::= { adVQMCallHistoryEntry 74 }

     adVqmCallHistEarlyThreshMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Early threshold for SJB, packets arriving under this threshold
            will not be discarded by SJB as early."
         ::= { adVQMCallHistoryEntry 75 }

     adVqmCallHistEarlyThreshPc  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage of total packets (including both early and late packets)
            not judged as being under the early jitter threshold."
         ::= { adVQMCallHistoryEntry 76 }

     adVqmCallHistEarlyUnderThresh  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Count of early packets which arrived under the early jitter
            threshold."
         ::= { adVQMCallHistoryEntry 77 }

     adVqmCallHistEarlyTotalCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total count of early packets arriving before the expected delay."
         ::= { adVQMCallHistoryEntry 78 }

     adVqmCallHistEarlyPeakJitterMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Largest jitter encountered among packets counted as early."
         ::= { adVQMCallHistoryEntry 79 }

     adVqmCallHistDelayIncreaseCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of SJB delay increases (adaptive mode only)."
         ::= { adVQMCallHistoryEntry 80 }

     adVqmCallHistDelayDecreaseCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of SJB delay decreases (adaptive mode only)."
         ::= { adVQMCallHistoryEntry 81 }

     adVqmCallHistResyncCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of  SJB resynchronizations caused by discontinuous
            transmission (DTX), voice activity detection (VAD), or silence
            suppression."
         ::= { adVQMCallHistoryEntry 82 }

     adVqmCallHistJitterBufferType  OBJECT-TYPE
         SYNTAX         INTEGER {
                        fixed     (1),
                        adaptive  (2),
                        unknown   (3)
         }
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Configured SJB type either adaptive or fixed for this stream."
         ::= { adVQMCallHistoryEntry 83 }

     adVqmCallHistJbCfgMin  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Adaptive jitter buffer minimum delay applied to packets received."
         ::= { adVQMCallHistoryEntry 84 }

     adVqmCallHistJbCfgNom  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Adaptive jitter buffer inital delay applied to packets received,
            or fixed jitter buffer delay applied to each packet."
         ::= { adVQMCallHistoryEntry 85 }

     adVqmCallHistJbCfgMax  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Adaptive jitter buffer upper bound on delay applied to packets
            received, or fixed jitter buffer maximum number of packets that will
            be inserted in buffer."
         ::= { adVQMCallHistoryEntry 86 }

     adVqmCallHistDuplicatePkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of duplicated packets discarded by SJB."
         ::= { adVQMCallHistoryEntry 87 }

     adVqmCallHistEarlyPkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets arriving early."
         ::= { adVQMCallHistoryEntry 88 }

     adVqmCallHistLatePkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets arriving late."
         ::= { adVQMCallHistoryEntry 89 }

     adVqmCallHistOverrunDiscardPkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets discarded by SJB due to jitter buffer
            overrun."
         ::= { adVQMCallHistoryEntry 90 }

     adVqmCallHistUnderrunDiscardPkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets discarded by SJB due to jitter buffer
            underrun."
         ::= { adVQMCallHistoryEntry 91 }

     adVqmCallHistDelayMinMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay minimum value."
         ::= { adVQMCallHistoryEntry 92 }

     adVqmCallHistDelayAvgMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay average value."
         ::= { adVQMCallHistoryEntry 93 }

     adVqmCallHistDelayMaxMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay maximum value."
         ::= { adVQMCallHistoryEntry 94 }

     adVqmCallHistDelayCurrentMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay current value."
         ::= { adVQMCallHistoryEntry 95 }

     adVqmCallHistExtRLqIn  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External listening quality R factor (in), from RTCP XR report
            (RFC3611)."
         ::= { adVQMCallHistoryEntry 96 }

     adVqmCallHistExtRLqOut  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External listening quality R factor (out), from RTCP XR report
            (RFC3611)."
         ::= { adVQMCallHistoryEntry 97 }

     adVqmCallHistExtRCqIn  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External conversational quality R factor (in), from RTCP XR report
            (RFC3611)."
         ::= { adVQMCallHistoryEntry 98 }

     adVqmCallHistExtRCqOut  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External conversational quality R factor (out), from RTCP XR report
            (RFC3611)."
         ::= { adVQMCallHistoryEntry 99 }

     adVqmCallHistThroughPutIndex  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Estimated throughput for fax or data call; bitrate range from 0 to
            35000 bps, calculated based on gap/burst conditions and loss/discard
            rates."
         ::= { adVQMCallHistoryEntry 100 }

     adVqmCallHistReliabilityIndex  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Reliability index for a fax or data call ranging from 0 least to
            100 most reliable."
         ::= { adVQMCallHistoryEntry 101 }

     adVqmCallHistBitrate  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Actual bitrate of RTP stream, calculated using size of each RTP
            packet in bits and duration of audio represented in each packet,
            indication of required bandwidth."
         ::= { adVQMCallHistoryEntry 102 }

     --
     -- adVqmActiveCall
     --

     adVQMActiveCallTable OBJECT-TYPE
         SYNTAX         SEQUENCE OF AdVQMActiveCallEntry
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
                "The adVqmActiveCall table provides detail voice quality
                statistics on currently active RTP voice streams.  A voice call
                will have two entries in this table one for each active RTP
                stream.  A combination of Source IP Address and Port,
                Destination IP Address and Port, and SSRC
                (synchronization source ID) are necessary to uniquely identify
                the call session.
                The VQM Active Call table shares the same type of information
                as found in the Call History table.  The VQM Manager transfers
                the active call statistics into the call history table database
                when the call completes."
         ::= { adVQMActive 1 }

     adVQMActiveCallEntry OBJECT-TYPE
         SYNTAX   AdVQMActiveCallEntry
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "The statistics for a particular VoIP end-point device."
         INDEX { adVqmActCallRtpSourceIp, adVqmActCallRtpSourcePort,
                adVqmActCallRtpDestIp, adVqmActCallRtpDestPort,
                adVqmActCallSsrcid }
         ::= { adVQMActiveCallTable 1 }

     AdVQMActiveCallEntry ::=
        SEQUENCE {
                adVqmActCallRtpSourceIp                IpAddress,
                adVqmActCallRtpSourcePort              Unsigned32,
                adVqmActCallRtpDestIp                  IpAddress,
                adVqmActCallRtpDestPort                Unsigned32,
                adVqmActCallSsrcid                     Unsigned32,
                adVqmActCallTo                         DisplayString,
                adVqmActCallFrom                       DisplayString,
                adVqmActCallRtpSourceUri               DisplayString,
                adVqmActCallCallid                     DisplayString,
                adVqmActCallCcmid                      Unsigned32,
                adVqmActCallSourceIntName              DisplayString,
                adVqmActCallDestIntName                DisplayString,
                adVqmActCallSourceIntDescription       DisplayString,
                adVqmActCallDestIntDescription         DisplayString,
                adVqmActCallCallStart                  DisplayString,
                adVqmActCallCallDurationMs             Unsigned32,
                adVqmActCallCodec                      INTEGER,
                adVqmActCallCodecClass                 INTEGER,
                adVqmActCallDscp                       Unsigned32,
                adVqmActCallPktsRcvdTotal              Counter32,
                adVqmActCallPktsLostTotal              Counter32,
                adVqmActCallPktsDiscardedTotal         Counter32,
                adVqmActCallOutOfOrder                 Counter32,
                adVqmActCallPdvAverageMs               Unsigned32,
                adVqmActCallPdvMaximumMs               Unsigned32,
                adVqmActCallRtDelayInst                INTEGER,
                adVqmActCallRtDelayAverage             INTEGER,
                adVqmActCallRtDelayMaximum             INTEGER,
                adVqmActCallOnewayDelayInst            INTEGER,
                adVqmActCallOnewayDelayAverage         INTEGER,
                adVqmActCallOnewayDelayMaximum         INTEGER,
                adVqmActCallOrigDelayInst              INTEGER,
                adVqmActCallOrigDelayAverage           INTEGER,
                adVqmActCallOrigDelayMaximum           INTEGER,
                adVqmActCallTermDelayMinimum           INTEGER,
                adVqmActCallTermDelayAverage           INTEGER,
                adVqmActCallTermDelayMaximum           INTEGER,
                adVqmActCallRLq                        Unsigned32,
                adVqmActCallRCq                        Unsigned32,
                adVqmActCallRNominal                   Unsigned32,
                adVqmActCallRG107                      Unsigned32,
                adVqmActCallMosLq                      MOSvalue,
                adVqmActCallMosCq                      MOSvalue,
                adVqmActCallMosPq                      MOSvalue,
                adVqmActCallMosNominal                 MOSvalue,
                adVqmActCallDegLoss                    Percentage,
                adVqmActCallDegDiscard                 Percentage,
                adVqmActCallDegVocoder                 Percentage,
                adVqmActCallDegRecency                 Percentage,
                adVqmActCallDegDelay                   Percentage,
                adVqmActCallDegSiglvl                  Percentage,
                adVqmActCallDegNoiselvl                Percentage,
                adVqmActCallDegEcholvl                 Percentage,
                adVqmActCallBurstRLq                   Unsigned32,
                adVqmActCallBurstCount                 Counter32,
                adVqmActCallBurstRateAvg               Percentage,
                adVqmActCallBurstLenAvgPkts            Unsigned32,
                adVqmActCallBurstLenAvgMsec            Unsigned32,
                adVqmActCallGapR                       Unsigned32,
                adVqmActCallGapCount                   Counter32,
                adVqmActCallGapLossRateAvg             Percentage,
                adVqmActCallGapLenPkts                 Unsigned32,
                adVqmActCallGapLenMsec                 Unsigned32,
                adVqmActCallLossRateAvg                Percentage,
                adVqmActCallNetworkLossAvg             Percentage,
                adVqmActCallDiscardRateAvg             Percentage,
                adVqmActCallExcessBurst                Unsigned32,
                adVqmActCallExcessGap                  Unsigned32,
                adVqmActCallPpdvMsec                   MsecValue,
                adVqmActCallLateThresholdMs            MsecValue,
                adVqmActCallLateThresholdPc            Percentage,
                adVqmActCallLateUnderThresh            Counter32,
                adVqmActCallLateTotalCount             Counter32,
                adVqmActCallLatePeakJitterMs           MsecValue,
                adVqmActCallEarlyThreshMs              MsecValue,
                adVqmActCallEarlyThreshPc              Percentage,
                adVqmActCallEarlyUnderThresh           Counter32,
                adVqmActCallEarlyTotalCount            Counter32,
                adVqmActCallEarlyPeakJitterMs          MsecValue,
                adVqmActCallDelayIncreaseCount         Counter32,
                adVqmActCallDelayDecreaseCount         Counter32,
                adVqmActCallResyncCount                Counter32,
                adVqmActCallJitterBufferType           INTEGER,
                adVqmActCallJbCfgMin                   Unsigned32,
                adVqmActCallJbCfgNom                   Unsigned32,
                adVqmActCallJbCfgMax                   Unsigned32,
                adVqmActCallDuplicatePkts              Counter32,
                adVqmActCallEarlyPkts                  Counter32,
                adVqmActCallLatePkts                   Counter32,
                adVqmActCallOverrunDiscardPkts         Counter32,
                adVqmActCallUnderrunDiscardPkts        Counter32,
                adVqmActCallDelayMinMsec               Unsigned32,
                adVqmActCallDelayAvgMsec               Unsigned32,
                adVqmActCallDelayMaxMsec               Unsigned32,
                adVqmActCallDelayCurrentMsec           Unsigned32,
                adVqmActCallExtRLqIn                   INTEGER,
                adVqmActCallExtRLqOut                  INTEGER,
                adVqmActCallExtRCqIn                   INTEGER,
                adVqmActCallExtRCqOut                  INTEGER,
                adVqmActCallThroughPutIndex            Unsigned32,
                adVqmActCallReliabilityIndex           Unsigned32,
                adVqmActCallBitrate                    Unsigned32
     }

     adVqmActCallRtpSourceIp OBJECT-TYPE
         SYNTAX         IpAddress
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source IP Address of RTP stream."
         ::= { adVQMActiveCallEntry 1 }

     adVqmActCallRtpSourcePort OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source port number."
         ::= { adVQMActiveCallEntry 2 }

     adVqmActCallRtpDestIp OBJECT-TYPE
         SYNTAX         IpAddress
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination IP address of RTP stream."
         ::= { adVQMActiveCallEntry 3 }

     adVqmActCallRtpDestPort OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination port number."
         ::= { adVQMActiveCallEntry 4 }

     adVqmActCallSsrcid OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "SSRC (synchronization source ID) for this stream per RFC3550."
         ::= { adVQMActiveCallEntry 5 }

     adVqmActCallTo OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "To URI (dialed) from monitored SIP call signaling."
         ::= { adVQMActiveCallEntry 6 }

     adVqmActCallFrom OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "From URI (originating caller) from monitored SIP call signaling."
         ::= { adVQMActiveCallEntry 7 }

     adVqmActCallRtpSourceUri OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "URI of sender RTP, either To URI or From URI."
         ::= { adVQMActiveCallEntry 8 }

     adVqmActCallCallid OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "SIP call-ID from monitored SIP call signaling."
         ::= { adVQMActiveCallEntry 9 }

     adVqmActCallCcmid OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Internal generated call-ID."
         ::= { adVQMActiveCallEntry 10 }

     adVqmActCallSourceIntName OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source interface name that RTP arrived inbound to unit."
         ::= { adVQMActiveCallEntry 11 }

     adVqmActCallDestIntName OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination interface name for RTP."
         ::= { adVQMActiveCallEntry 12 }

     adVqmActCallSourceIntDescription OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Source interface description as defined in CLI or GUI."
         ::= { adVQMActiveCallEntry 13 }

     adVqmActCallDestIntDescription OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Destination interface description as defined in CLI or GUI."
         ::= { adVQMActiveCallEntry 14 }

     adVqmActCallCallStart OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Time at which monitoring began on this RTP stream."
         ::= { adVQMActiveCallEntry 15 }

     adVqmActCallCallDurationMs OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Elapsed time from start to last RTP packet on this stream."
         ::= { adVQMActiveCallEntry 16 }

     adVqmActCallCodec OBJECT-TYPE
         SYNTAX         INTEGER
                        {
                        -- -1
                        unknown         (1),
                        -- 0
                        g711U           (2),
                        g711UPLC        (3),
                        g723153K        (4),
                        deprecated1     (5),
                        g723163K        (6),
                        deprecated2     (7),
                        g728            (8),
                        deprecated3     (9),
                        g729            (10),
                        deprecated4     (11),
                        g729A           (12),
                        deprecated5     (13),
                        user1           (14),
                        user2           (15),
                        user3           (16),
                        user4           (17),
                        gsmfr           (18),
                        reservedgsmhr   (19),
                        gsmefr          (20),
                        sx7300          (21),
                        sx9600          (22),
                        g711A           (23),
                        g711APLC        (24),
                        deprecated6     (25),
                        g72616K         (26),
                        g72624K         (27),
                        g72632K         (28),
                        g72640K         (29),
                        gipse711U       (30),
                        gipse711A       (31),
                        gipsilbc        (32),
                        gipsisac        (33),
                        gipsipcmwb      (34),
                        g729E8K0        (35),
                        g729E11k8       (36),
                        wblinearpcm     (37),
                        wblinearpcmPlc  (38),
                        g722at64k       (39),
                        g722at56k       (40),
                        g722at48k       (41),
                        g7221at32k      (42),
                        g7221at24k      (43),
                        g7222at23k85    (44),
                        g7222at23k05    (45),
                        g7222at19k85    (46),
                        g7222at18k25    (47),
                        g7222at15k85    (48),
                        g7222at14k25    (49),
                        g7222at12k85    (50),
                        g7222at8k85     (51),
                        g7222at6k6      (52),
                        qcelp8          (53),
                        qcelp13         (54),
                        evrc            (55),
                        smv812          (56),
                        smv579          (57),
                        smv444          (58),
                        smv395          (59),
                        amrnb12k2       (60),
                        amrnb10k2       (61),
                        amrnb7k95       (62),
                        amrnb7k4        (63),
                        amrnb6k7        (64),
                        amrnb5k9        (65),
                        amrnb5k15       (66),
                        amrnb4k75       (67),
                        ilbc13k3        (68),
                        ilbc15k2        (69),
                        g711u56k        (70),
                        g711uPLC56k     (71),
                        g711A56k        (72),
                        g711APLC56k     (73),
                        g7231C          (74),
                        speex2k15       (75),
                        speex5k95       (76),
                        speeX8k         (77),
                        speeX11k        (78),
                        speeX15k        (79),
                        speeX18k2       (80),
                        speeX24k6       (81),
                        speeX3k95       (82),
                        speeX12k8       (83),
                        speeX16k8       (84),
                        speeX20k6       (85),
                        speeX23k8       (86),
                        speeX27k8       (87),
                        speeX34k2       (88),
                        speeX42k2       (89)
         }
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Last voice CODEC detected on this stream."
         ::= { adVQMActiveCallEntry 17 }

     adVqmActCallCodecClass OBJECT-TYPE
         SYNTAX         INTEGER {
                wideband        (1),
                other           (2)
         }
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Class to which CODEC vocoder belongs."
         ::= { adVQMActiveCallEntry 18 }

     adVqmActCallDscp OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Differentiated Services Code Point (DSCP) in RTP packet IP header."
         ::= { adVQMActiveCallEntry 19 }

     adVqmActCallPktsRcvdTotal OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total received RTP packets in this stream."
         ::= { adVQMActiveCallEntry 20 }

     adVqmActCallPktsLostTotal OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total packets determined to be lost in network by simulated jitter
            buffer."
         ::= { adVQMActiveCallEntry 21 }

     adVqmActCallPktsDiscardedTotal OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total packets discarded by simulated jitter buffer."
         ::= { adVQMActiveCallEntry 22 }

     adVqmActCallOutOfOrder OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total packets received out of order at simulated jitter buffer."
         ::= { adVQMActiveCallEntry 23 }

     adVqmActCallPdvAverageMs OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average Packet Delay Variation (PDV) in RTP stream in
            milliseconds."
         ::= { adVQMActiveCallEntry 24 }

     adVqmActCallPdvMaximumMs OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum Packet Delay Variation (PDV) in RTP stream in
            milliseconds."
         ::= { adVQMActiveCallEntry 25 }

     adVqmActCallRtDelayInst OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous round-trip delay obtained from RTCP or RTCP XR
            reports."
         ::= { adVQMActiveCallEntry 26 }

     adVqmActCallRtDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average round-trip delay obtained from RTCP or RTCP XR reports."
         ::= { adVQMActiveCallEntry 27 }

     adVqmActCallRtDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum round-trip delay obtained from RTCP or RTCP XR reports."
         ::= { adVQMActiveCallEntry 28 }

     adVqmActCallOnewayDelayInst OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous one-way delay including simulated jitter buffer (SJB)
            delay."
         ::= { adVQMActiveCallEntry 29 }

     adVqmActCallOnewayDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average one-way delay including SJB delay."
         ::= { adVQMActiveCallEntry 30 }

     adVqmActCallOnewayDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum one-way delay including SJB delay."
         ::= { adVQMActiveCallEntry 31 }

     adVqmActCallOrigDelayInst OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous origination end-point delay from RTCP XR reports."
         ::= { adVQMActiveCallEntry 32 }

     adVqmActCallOrigDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average origination end-point delay from RTCP XR reports."
         ::= { adVQMActiveCallEntry 33 }

     adVqmActCallOrigDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum origination end-point delay from RTCP XR reports."
         ::= { adVQMActiveCallEntry 34 }

     adVqmActCallTermDelayMinimum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Instantaneous termination end-point delay, simulated jitter
            buffer + codec."
         ::= { adVQMActiveCallEntry 35 }

     adVqmActCallTermDelayAverage OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average termination end-point delay, simulated jitter
            buffer + codec."
         ::= { adVQMActiveCallEntry 36 }

     adVqmActCallTermDelayMaximum OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Maximum termination end-point delay, simulated jitter
            buffer + codec."
         ::= { adVQMActiveCallEntry 37 }

     adVqmActCallRLq OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening quality R factor."
         ::= { adVQMActiveCallEntry 38 }

     adVqmActCallRCq OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Conversational quality R factor."
         ::= { adVQMActiveCallEntry 39 }

     adVqmActCallRNominal OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Nominal or generally accepted maximum R factor for this stream."
         ::= { adVQMActiveCallEntry 40 }

     adVqmActCallRG107 OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "R factor based on ITU G.107 E Model for this stream."
         ::= { adVQMActiveCallEntry 41 }

     adVqmActCallMosLq OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening quality MOS score."
         ::= { adVQMActiveCallEntry 42 }

     adVqmActCallMosCq OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Conversational quality MOS score."
         ::= { adVQMActiveCallEntry 43 }

     adVqmActCallMosPq OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Listening quality MOS score normalized to the PESQ scale."
         ::= { adVQMActiveCallEntry 44 }

     adVqmActCallMosNominal OBJECT-TYPE
         SYNTAX         MOSvalue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Nominal or generally accepted maximum MOS score for this stream."
         ::= { adVQMActiveCallEntry 45 }

     adVqmActCallDegLoss OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to packet loss."
         ::= { adVQMActiveCallEntry 46 }

     adVqmActCallDegDiscard OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to packet discard."
         ::= { adVQMActiveCallEntry 47 }

     adVqmActCallDegVocoder OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to voice CODEC selection."
         ::= { adVQMActiveCallEntry 48 }

     adVqmActCallDegRecency OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to loss or discard recency in
            call."
         ::= { adVQMActiveCallEntry 49 }

     adVqmActCallDegDelay OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to delay."
         ::= { adVQMActiveCallEntry 50 }

     adVqmActCallDegSiglvl OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to low speech energy signal
            level."
         ::= { adVQMActiveCallEntry 51 }

     adVqmActCallDegNoiselvl OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to high noise levels."
         ::= { adVQMActiveCallEntry 52 }

     adVqmActCallDegEcholvl OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage quality degradation due to high echo levels."
         ::= { adVQMActiveCallEntry 53 }

     adVqmActCallBurstRLq OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average listening quality R factor during burst condition."
         ::= { adVQMActiveCallEntry 54 }

     adVqmActCallBurstCount OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of times the stream was in a burst condition."
         ::= { adVQMActiveCallEntry 55 }

     adVqmActCallBurstRateAvg OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost or discarded while in
            burst condition."
         ::= { adVQMActiveCallEntry 56 }

     adVqmActCallBurstLenAvgPkts OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average burst length in packets."
         ::= { adVQMActiveCallEntry 57 }

     adVqmActCallBurstLenAvgMsec OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average burst length in miliseconds."
         ::= { adVQMActiveCallEntry 58 }

     adVqmActCallGapR OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average listening quality R factor while stream is in a gap
            condition."
         ::= { adVQMActiveCallEntry 59 }

     adVqmActCallGapCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Number of times the stream is in gap condition."
         ::= { adVQMActiveCallEntry 60 }

     adVqmActCallGapLossRateAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost or discarded while in
            gap condition."
         ::= { adVQMActiveCallEntry 61 }

     adVqmActCallGapLenPkts  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average gap length in packets."
         ::= { adVQMActiveCallEntry 62 }

     adVqmActCallGapLenMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Average gap length in milliseconds."
         ::= { adVQMActiveCallEntry 63 }

     adVqmActCallLossRateAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost or discarded."
         ::= { adVQMActiveCallEntry 64 }

     adVqmActCallNetworkLossAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames lost in network, excludes
            SJB discards."
         ::= { adVQMActiveCallEntry 65 }

     adVqmActCallDiscardRateAvg  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total average percentage of frames discarded by SJB."
         ::= { adVQMActiveCallEntry 66 }

     adVqmActCallExcessBurst  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total length of speech lost during burst conditions not handled
            effectively by packet loss-concealment."
         ::= { adVQMActiveCallEntry 67 }

     adVqmActCallExcessGap  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total length of speech lost during gap conditions not handled
            effectively by packet loss-concealment."
         ::= { adVQMActiveCallEntry 68 }

     adVqmActCallPpdvMsec  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Packet to packed delay variation (jitter) in ms, as defined in
            RFC3550."
         ::= { adVQMActiveCallEntry 69 }

     adVqmActCallLateThresholdMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Late threshold for SJB, packets arriving under this threshold are
            not discarded."
         ::= { adVQMActiveCallEntry 70 }

     adVqmActCallLateThresholdPc  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage of total packets (including both early and late packets)
            not judged as being under the late jitter threshold."
         ::= { adVQMActiveCallEntry 71 }

     adVqmActCallLateUnderThresh  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Count of late packets which arrived under the late jitter
            threshold."
         ::= { adVQMActiveCallEntry 72 }

     adVqmActCallLateTotalCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total count of late packets arriving after the expected delay."
         ::= { adVQMActiveCallEntry 73 }

     adVqmActCallLatePeakJitterMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Largest jitter encountered among packets counted as late."
         ::= { adVQMActiveCallEntry 74 }

     adVqmActCallEarlyThreshMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Early threshold for SJB, packets arriving under this threshold
            will not be discarded by SJB as early."
         ::= { adVQMActiveCallEntry 75 }

     adVqmActCallEarlyThreshPc  OBJECT-TYPE
         SYNTAX         Percentage
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Percentage of total packets (including both early and late packets)
            not judged as being under the early jitter threshold."
         ::= { adVQMActiveCallEntry 76 }

     adVqmActCallEarlyUnderThresh  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Count of early packets which arrived under the early jitter
            threshold."
         ::= { adVQMActiveCallEntry 77 }

     adVqmActCallEarlyTotalCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total count of early packets arriving before the expected delay."
         ::= { adVQMActiveCallEntry 78 }

     adVqmActCallEarlyPeakJitterMs  OBJECT-TYPE
         SYNTAX         MsecValue
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Largest jitter encountered among packets counted as early."
         ::= { adVQMActiveCallEntry 79 }

     adVqmActCallDelayIncreaseCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of SJB delay increases (adaptive mode only)."
         ::= { adVQMActiveCallEntry 80 }

     adVqmActCallDelayDecreaseCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of SJB delay decreases (adaptive mode only)."
         ::= { adVQMActiveCallEntry 81 }

     adVqmActCallResyncCount  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of  SJB resynchronizations caused by discontinuous
            transmission (DTX), voice activity detection (VAD), or silence
            suppression."
         ::= { adVQMActiveCallEntry 82 }

     adVqmActCallJitterBufferType  OBJECT-TYPE
         SYNTAX         INTEGER {
                        fixed     (1),
                        adaptive  (2),
                        unknown   (3)
         }
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Configured SJB type either adaptive or fixed for this stream."
         ::= { adVQMActiveCallEntry 83 }

     adVqmActCallJbCfgMin  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Adaptive jitter buffer minimum delay applied to packets received."
         ::= { adVQMActiveCallEntry 84 }

     adVqmActCallJbCfgNom  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Adaptive jitter buffer inital delay applied to packets received,
            or fixed jitter buffer delay applied to each packet."
         ::= { adVQMActiveCallEntry 85 }

     adVqmActCallJbCfgMax  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Adaptive jitter buffer upper bound on delay applied to packets
            received, or fixed jitter buffer maximum number of packets that will
            be inserted in buffer."
         ::= { adVQMActiveCallEntry 86 }

     adVqmActCallDuplicatePkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of duplicated packets discarded by SJB."
         ::= { adVQMActiveCallEntry 87 }

     adVqmActCallEarlyPkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets arriving early."
         ::= { adVQMActiveCallEntry 88 }

     adVqmActCallLatePkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets arriving late."
         ::= { adVQMActiveCallEntry 89 }

     adVqmActCallOverrunDiscardPkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets discarded by SJB due to jitter buffer
            overrun."
         ::= { adVQMActiveCallEntry 90 }

     adVqmActCallUnderrunDiscardPkts  OBJECT-TYPE
         SYNTAX         Counter32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Total number of packets discarded by SJB due to jitter buffer
            underrun."
         ::= { adVQMActiveCallEntry 91 }

     adVqmActCallDelayMinMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay minimum value."
         ::= { adVQMActiveCallEntry 92 }

     adVqmActCallDelayAvgMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay average value."
         ::= { adVQMActiveCallEntry 93 }

     adVqmActCallDelayMaxMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay maximum value."
         ::= { adVQMActiveCallEntry 94 }

     adVqmActCallDelayCurrentMsec  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Simulated jitter buffer delay current value."
         ::= { adVQMActiveCallEntry 95 }

     adVqmActCallExtRLqIn  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External listening quality R factor (in), from RTCP XR report
            (RFC3611)."
         ::= { adVQMActiveCallEntry 96 }

     adVqmActCallExtRLqOut  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External listening quality R factor (out), from RTCP XR report
            (RFC3611)."
         ::= { adVQMActiveCallEntry 97 }

     adVqmActCallExtRCqIn  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External conversational quality R factor (in), from RTCP XR report
            (RFC3611)."
         ::= { adVQMActiveCallEntry 98 }

     adVqmActCallExtRCqOut  OBJECT-TYPE
         SYNTAX         INTEGER
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "External conversational quality R factor (out), from RTCP XR report
            (RFC3611)."
         ::= { adVQMActiveCallEntry 99 }

     adVqmActCallThroughPutIndex  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Estimated throughput for fax or data call; bitrate range from 0 to
            35000 bps, calculated based on gap/burst conditions and loss/discard
            rates."
         ::= { adVQMActiveCallEntry 100 }

     adVqmActCallReliabilityIndex  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Reliability index for a fax or data call ranging from 0 least to
            100 most reliable."
         ::= { adVQMActiveCallEntry 101 }

     adVqmActCallBitrate  OBJECT-TYPE
         SYNTAX         Unsigned32
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "Actual bitrate of RTP stream, calculated using size of each RTP
            packet in bits and duration of audio represented in each packet,
            indication of required bandwidth."
         ::= { adVQMActiveCallEntry 102 }


     -- conformance information

     adGenAOSVqmConformance OBJECT IDENTIFIER ::= { adGenAOSConformance 10 }
     adGenAOSVqmGroups      OBJECT IDENTIFIER ::= { adGenAOSVqmConformance 1 }
     adGenAOSVqmCompliances OBJECT IDENTIFIER ::= { adGenAOSVqmConformance 2 }

--
-- MIB Compliance statements.
--

-- Full compliance statement
     adGenAOSVqmFullCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
        "The compliance statement for SNMP entities which implement
        version 1 of the adGenAosVQM MIB. When this MIB is implemented
        with support for read-only, then such an implementation can claim
        full compliance. "

         MODULE  -- this module

         GROUP adVQMCfgGroup
         DESCRIPTION
            "A collection of objects providing global configuration information
            of a VQM entity."

         GROUP adVQMThresholdGroup
         DESCRIPTION
            "A collection of objects providing global threshold configuration
            information of a VQM entity."

         GROUP adVQMSysPerfGroup
         DESCRIPTION
            "A collection of objects providing global system performance
            information of a VQM entity."

         GROUP adVQMInterfaceGroup
         DESCRIPTION
            "A collection of VQM aggregate statistics for each
            system interface."

         GROUP adVQMEndPointGroup
         DESCRIPTION
            "A collection of VQM aggregate statistics for each
            end-point device."

         GROUP adVQMCallHistoryGroup
         DESCRIPTION
            "A collection of detailed voice quality statistics
            on completed RTP voice streams."

         GROUP adVQMActiveCallGroup
         DESCRIPTION
            "A collection of detailed voice quality statistics
            on currently active RTP voice streams."

         GROUP adVQMTrapGroup
         DESCRIPTION
            "This optional group is used for the management of
            asynchronous notifications by Voice Quality Monitoring."

         GROUP  adVQMNotificationGroup
         DESCRIPTION
            "This optional group defines the asynchronous
            notifications generated by Voice Quality Monitoring."

         ::= { adGenAOSVqmCompliances 1 }

     -- units of conformance

     adVQMCfgGroup    OBJECT-GROUP
         OBJECTS {
                adVqmCfgEnable,
                adVqmCfgSipEnable,
                adVqmCfgUdpEnable,
                adVqmCfgInternationalCode,
                adVqmCfgJitterBufferType,
                adVqmCfgJitterBufferAdaptiveMin,
                adVqmCfgJitterBufferAdaptiveNominal,
                adVqmCfgJitterBufferAdaptiveMax,
                adVqmCfgJitterBufferFixedNominal,
                adVqmCfgJitterBufferFixedSize,
                adVqmCfgJitterBufferThresholdEarlyMs,
                adVqmCfgJitterBufferThresholdLateMs,
                adVqmCfgRoundTripPingEnabled,
                adVqmCfgRoundTripPingType,
                adVqmCfgCallHistorySize,
                adVqmCfgHistoryThresholdLqmos,
                adVqmCfgHistoryThresholdCqmos,
                adVqmCfgHistoryThresholdPqmos,
                adVqmCfgHistoryThresholdLoss,
                adVqmCfgHistoryThresholdOutOfOrder,
                adVqmCfgHistoryThresholdJitter,
                adVqmCfgClear,
                adVqmCfgClearCallHistory
            -- ????adVqmCfgTrapPriority                    INTEGER ( We do not currently have a column to support this OID.)
         }
         STATUS  current
         DESCRIPTION
            "The adVQMCfg group contains read-only VQM system configuration
            information for global enable/disable, type of RTP stream detection,
            jitter buffer emulator settings, ping settings for measuring delay,
            and call history buffer filter threshold values.  Network Management
            System may read these values to augment their charts and graphs of
            VQM performance statistics.  Clear write-only controls provide the
            NMS the ability to clear VQM performance statistics."
         ::= { adGenAOSVqmGroups 1 }

     adVQMThresholdGroup    OBJECT-GROUP
         OBJECTS {
                adVqmThresholdLqmosInfo,
                adVqmThresholdLqmosNotice,
                adVqmThresholdLqmosWarning,
                adVqmThresholdLqmosError,
                adVqmThresholdPqmosInfo,
                adVqmThresholdPqmosNotice,
                adVqmThresholdPqmosWarning,
                adVqmThresholdPqmosError,
                adVqmThresholdOutOfOrderInfo,
                adVqmThresholdOutOfOrderNotice,
                adVqmThresholdOutOfOrderWarning,
                adVqmThresholdOutOfOrderError,
                adVqmThresholdLossInfo,
                adVqmThresholdLossNotice,
                adVqmThresholdLossWarning,
                adVqmThresholdLossError,
                adVqmThresholdJitterInfo,
                adVqmThresholdJitterNotice,
                adVqmThresholdJitterWarning,
                adVqmThresholdJitterError
         }
         STATUS  current
         DESCRIPTION
                "The adVQMThreshold group contains read-only configuration
                threshold setting values for VQM event messages.  Threshold
                values include Information, Notice, Warning, and Error events
                for MOS scores, packet loss, out-of-order, and jitter."
         ::= { adGenAOSVqmGroups 2 }

     adVQMSysPerfGroup    OBJECT-GROUP
         OBJECTS {
                adVqmSysActiveCalls,
                adVqmSysActiveExcellent,
                adVqmSysActiveGood,
                adVqmSysActiveFair,
                adVqmSysActivePoor,
                adVqmSysCallHistoryCalls,
                adVqmSysCallHistoryExcellent,
                adVqmSysCallHistoryGood,
                adVqmSysCallHistoryFair,
                adVqmSysCallHistoryPoor,
                adVqmSysAllCallsExcellent,
                adVqmSysAllCallsGood,
                adVqmSysAllCallsFair,
                adVqmSysAllCallsPoor
         }
         STATUS  current
         DESCRIPTION
                "The adVQMSysPerfGroup group provides an overall
                summary view of the quality of voice streams flowing through
                the system. VQM voice call analysis rates the quality of RTP
                voice streams as Excellent, Good, Fair or Poor.  The numbers of
                calls for each quality rating are available for currently active
                calls, completed calls (history), and all calls (totals).  The
                total number of calls monitored by VQM is the sum of active
                calls adVqmSysActiveCalls) and history calls
                (adVqmSysCallHistoryCalls)."
         ::= { adGenAOSVqmGroups 3 }

     adVQMInterfaceGroup    OBJECT-GROUP
         OBJECTS {
                adVqmIfcId,
                adVqmIfcName,
                adVqmIfcPktsRx,
                adVqmIfcPktsLost,
                adVqmIfcPktsOoo,
                adVqmIfcPktsDiscarded,
                adVqmIfcNumberActiveCalls,
                adVqmIfcTerminatedCalls,
                adVqmIfcRLqMinimum,
                adVqmIfcRLqAverage,
                adVqmIfcRLqMaximum,
                adVqmIfcRCqMinimum,
                adVqmIfcRCqAverage,
                adVqmIfcRCqMaximum,
                adVqmIfcRG107Minimum,
                adVqmIfcRG107Average,
                adVqmIfcRG107Maximum,
                adVqmIfcMosLqMinimum,
                adVqmIfcMosLqAverage,
                adVqmIfcMosLqMaximum,
                adVqmIfcMosCqMinimum,
                adVqmIfcMosCqAverage,
                adVqmIfcMosCqMaximum,
                adVqmIfcMosPqMinimum,
                adVqmIfcMosPqAverage,
                adVqmIfcMosPqMaximum,
                adVqmIfcLossMinimum,
                adVqmIfcLossAverage,
                adVqmIfcLossMaximum,
                adVqmIfcDiscardsMinimum,
                adVqmIfcDiscardsAverage,
                adVqmIfcDiscardsMaximum,
                adVqmIfcPdvAverageMs,
                adVqmIfcPdvMaximumMs,
                adVqmIfcDelayMinMsec,
                adVqmIfcDelayAvgMsec,
                adVqmIfcDelayMaxMsec,
                adVqmIfcNumberStreamsExcellent,
                adVqmIfcNumberStreamsGood,
                adVqmIfcNumberStreamsFair,
                adVqmIfcNumberStreamsPoor,
                adVqmIfcClear
         }
         STATUS  current
         DESCRIPTION
            "The adVQMInterface group defines aggregate statistics for each
            system interface."
         ::= { adGenAOSVqmGroups 4 }


     adVQMEndPointGroup    OBJECT-GROUP
         OBJECTS {
                adVqmEndPointRtpSourceIp,
                adVqmEndPointNumberCompletedCalls,
                adVqmEndPointInterfaceId,
                adVqmEndPointInterfaceName,
                adVqmEndPointMosLqMinimum,
                adVqmEndPointMosLqAverage,
                adVqmEndPointMosLqMaximum,
                adVqmEndPointMosPqMinimum,
                adVqmEndPointMosPqAverage,
                adVqmEndPointMosPqMaximum,
                adVqmEndPointPktsLostTotal,
                adVqmEndPointPktsOutOfOrder,
                adVqmEndPointJitterMaximum,
                adVqmEndPointNumberStreamsExcellent,
                adVqmEndPointNumberStreamsGood,
                adVqmEndPointNumberStreamsFair,
                adVqmEndPointNumberStreamsPoor
         }
         STATUS  current
         DESCRIPTION
            "The adVQMEndPoint group defines aggregate statistics for each
            VoIP end-point entity."
         ::= { adGenAOSVqmGroups 5 }

     adVQMCallHistoryGroup    OBJECT-GROUP
         OBJECTS {
                adVqmCallHistRtpSourceIp,
                adVqmCallHistRtpSourcePort,
                adVqmCallHistRtpDestIp,
                adVqmCallHistRtpDestPort,
                adVqmCallHistSsrcid,
                adVqmCallHistTo,
                adVqmCallHistFrom,
                adVqmCallHistRtpSourceUri,
                adVqmCallHistCallid,
                adVqmCallHistCcmid,
                adVqmCallHistSourceIntName,
                adVqmCallHistDestIntName,
                adVqmCallHistSourceIntDescription,
                adVqmCallHistDestIntDescription,
                adVqmCallHistCallStart,
                adVqmCallHistCallDurationMs,
                adVqmCallHistCodec,
                adVqmCallHistCodecClass,
                adVqmCallHistDscp,
                adVqmCallHistPktsRcvdTotal,
                adVqmCallHistPktsLostTotal,
                adVqmCallHistPktsDiscardedTotal,
                adVqmCallHistOutOfOrder,
                adVqmCallHistPdvAverageMs,
                adVqmCallHistPdvMaximumMs,
                adVqmCallHistRtDelayInst,
                adVqmCallHistRtDelayAverage,
                adVqmCallHistRtDelayMaximum,
                adVqmCallHistOnewayDelayInst,
                adVqmCallHistOnewayDelayAverage,
                adVqmCallHistOnewayDelayMaximum,
                adVqmCallHistOrigDelayInst,
                adVqmCallHistOrigDelayAverage,
                adVqmCallHistOrigDelayMaximum,
                adVqmCallHistTermDelayMinimum,
                adVqmCallHistTermDelayAverage,
                adVqmCallHistTermDelayMaximum,
                adVqmCallHistRLq,
                adVqmCallHistRCq,
                adVqmCallHistRNominal,
                adVqmCallHistRG107,
                adVqmCallHistMosLq,
                adVqmCallHistMosCq,
                adVqmCallHistMosPq,
                adVqmCallHistMosNominal,
                adVqmCallHistDegLoss,
                adVqmCallHistDegDiscard,
                adVqmCallHistDegVocoder,
                adVqmCallHistDegRecency,
                adVqmCallHistDegDelay,
                adVqmCallHistDegSiglvl,
                adVqmCallHistDegNoiselvl,
                adVqmCallHistDegEcholvl,
                adVqmCallHistBurstRLq,
                adVqmCallHistBurstCount,
                adVqmCallHistBurstRateAvg,
                adVqmCallHistBurstLenAvgPkts,
                adVqmCallHistBurstLenAvgMsec,
                adVqmCallHistGapR,
                adVqmCallHistGapCount,
                adVqmCallHistGapLossRateAvg,
                adVqmCallHistGapLenPkts,
                adVqmCallHistGapLenMsec,
                adVqmCallHistLossRateAvg,
                adVqmCallHistNetworkLossAvg,
                adVqmCallHistDiscardRateAvg,
                adVqmCallHistExcessBurst,
                adVqmCallHistExcessGap,
                adVqmCallHistPpdvMsec,
                adVqmCallHistLateThresholdMs,
                adVqmCallHistLateThresholdPc,
                adVqmCallHistLateUnderThresh,
                adVqmCallHistLateTotalCount,
                adVqmCallHistLatePeakJitterMs,
                adVqmCallHistEarlyThreshMs,
                adVqmCallHistEarlyThreshPc,
                adVqmCallHistEarlyUnderThresh,
                adVqmCallHistEarlyTotalCount,
                adVqmCallHistEarlyPeakJitterMs,
                adVqmCallHistDelayIncreaseCount,
                adVqmCallHistDelayDecreaseCount,
                adVqmCallHistResyncCount,
                adVqmCallHistJitterBufferType,
                adVqmCallHistJbCfgMin,
                adVqmCallHistJbCfgNom,
                adVqmCallHistJbCfgMax,
                adVqmCallHistDuplicatePkts,
                adVqmCallHistEarlyPkts,
                adVqmCallHistLatePkts,
                adVqmCallHistOverrunDiscardPkts,
                adVqmCallHistUnderrunDiscardPkts,
                adVqmCallHistDelayMinMsec,
                adVqmCallHistDelayAvgMsec,
                adVqmCallHistDelayMaxMsec,
                adVqmCallHistDelayCurrentMsec,
                adVqmCallHistExtRLqIn,
                adVqmCallHistExtRLqOut,
                adVqmCallHistExtRCqIn,
                adVqmCallHistExtRCqOut,
                adVqmCallHistThroughPutIndex,
                adVqmCallHistReliabilityIndex,
                adVqmCallHistBitrate
         }
         STATUS  current
         DESCRIPTION
            "The adVQMCallHistory group defines provides detail voice quality
            statistics on 'completed' RTP voice streams."
         ::= { adGenAOSVqmGroups 6 }

     adVQMActiveCallGroup    OBJECT-GROUP
         OBJECTS {
                adVqmActCallRtpSourceIp,
                adVqmActCallRtpSourcePort,
                adVqmActCallRtpDestIp,
                adVqmActCallRtpDestPort,
                adVqmActCallSsrcid,
                adVqmActCallTo,
                adVqmActCallFrom,
                adVqmActCallRtpSourceUri,
                adVqmActCallCallid,
                adVqmActCallCcmid,
                adVqmActCallSourceIntName,
                adVqmActCallDestIntName,
                adVqmActCallSourceIntDescription,
                adVqmActCallDestIntDescription,
                adVqmActCallCallStart,
                adVqmActCallCallDurationMs,
                adVqmActCallCodec,
                adVqmActCallCodecClass,
                adVqmActCallDscp,
                adVqmActCallPktsRcvdTotal,
                adVqmActCallPktsLostTotal,
                adVqmActCallPktsDiscardedTotal,
                adVqmActCallOutOfOrder,
                adVqmActCallPdvAverageMs,
                adVqmActCallPdvMaximumMs,
                adVqmActCallRtDelayInst,
                adVqmActCallRtDelayAverage,
                adVqmActCallRtDelayMaximum,
                adVqmActCallOnewayDelayInst,
                adVqmActCallOnewayDelayAverage,
                adVqmActCallOnewayDelayMaximum,
                adVqmActCallOrigDelayInst,
                adVqmActCallOrigDelayAverage,
                adVqmActCallOrigDelayMaximum,
                adVqmActCallTermDelayMinimum,
                adVqmActCallTermDelayAverage,
                adVqmActCallTermDelayMaximum,
                adVqmActCallRLq,
                adVqmActCallRCq,
                adVqmActCallRNominal,
                adVqmActCallRG107,
                adVqmActCallMosLq,
                adVqmActCallMosCq,
                adVqmActCallMosPq,
                adVqmActCallMosNominal,
                adVqmActCallDegLoss,
                adVqmActCallDegDiscard,
                adVqmActCallDegVocoder,
                adVqmActCallDegRecency,
                adVqmActCallDegDelay,
                adVqmActCallDegSiglvl,
                adVqmActCallDegNoiselvl,
                adVqmActCallDegEcholvl,
                adVqmActCallBurstRLq,
                adVqmActCallBurstCount,
                adVqmActCallBurstRateAvg,
                adVqmActCallBurstLenAvgPkts,
                adVqmActCallBurstLenAvgMsec,
                adVqmActCallGapR,
                adVqmActCallGapCount,
                adVqmActCallGapLossRateAvg,
                adVqmActCallGapLenPkts,
                adVqmActCallGapLenMsec,
                adVqmActCallLossRateAvg,
                adVqmActCallNetworkLossAvg,
                adVqmActCallDiscardRateAvg,
                adVqmActCallExcessBurst,
                adVqmActCallExcessGap,
                adVqmActCallPpdvMsec,
                adVqmActCallLateThresholdMs,
                adVqmActCallLateThresholdPc,
                adVqmActCallLateUnderThresh,
                adVqmActCallLateTotalCount,
                adVqmActCallLatePeakJitterMs,
                adVqmActCallEarlyThreshMs,
                adVqmActCallEarlyThreshPc,
                adVqmActCallEarlyUnderThresh,
                adVqmActCallEarlyTotalCount,
                adVqmActCallEarlyPeakJitterMs,
                adVqmActCallDelayIncreaseCount,
                adVqmActCallDelayDecreaseCount,
                adVqmActCallResyncCount,
                adVqmActCallJitterBufferType,
                adVqmActCallJbCfgMin,
                adVqmActCallJbCfgNom,
                adVqmActCallJbCfgMax,
                adVqmActCallDuplicatePkts,
                adVqmActCallEarlyPkts,
                adVqmActCallLatePkts,
                adVqmActCallOverrunDiscardPkts,
                adVqmActCallUnderrunDiscardPkts,
                adVqmActCallDelayMinMsec,
                adVqmActCallDelayAvgMsec,
                adVqmActCallDelayMaxMsec,
                adVqmActCallDelayCurrentMsec,
                adVqmActCallExtRLqIn,
                adVqmActCallExtRLqOut,
                adVqmActCallExtRCqIn,
                adVqmActCallExtRCqOut,
                adVqmActCallThroughPutIndex,
                adVqmActCallReliabilityIndex,
                adVqmActCallBitrate
         }
         STATUS  current
         DESCRIPTION
            "The adVQMActiveCall group defines provides detail voice quality
            statistics on 'current' RTP voice streams."
         ::= { adGenAOSVqmGroups 7 }

     adVQMTrapGroup    OBJECT-GROUP
         OBJECTS {
                        adVqmTrapState,
                        adVqmTrapCfgSeverityLevel,
                        adVqmTrapEventType
                  }
         STATUS  current
         DESCRIPTION
            "The objects necessary to control VQM notification messages."
         ::= { adGenAOSVqmGroups 8 }

     adVQMNotificationGroup NOTIFICATION-GROUP
         NOTIFICATIONS { adVQMEndOfCallTrap }
         STATUS  current
         DESCRIPTION
            "Traps which may be used to enhance event driven
            management of VQM."
         ::= { adGenAOSVqmGroups 9 }

     END



