   TPLINK-DDMTEMPTHRESHOLD-MIB DEFINITIONS ::= BEGIN

         IMPORTS
            MODULE-IDENTITY, OBJECT-TYPE
          	  	        FROM SNMPv2-SMI
          	ifIndex
						FROM RFC1213-MIB
			DisplayString
						FROM SNMPv2-TC
			tplinkDdmManageMIBObjects
						FROM TPLINK-DDMMANAGE-MIB;
						
		   		ddmTempThreshold MODULE-IDENTITY  
				    LAST-UPDATED    "200908270000Z"
				    ORGANIZATION    "TPLINK"
				    CONTACT-INFO		"www.tplink.com"
				    DESCRIPTION			"The config of DDM temperature threshold."
				    REVISION        "200908270000Z"
				    DESCRIPTION			"Initial version of this MIB module."
				    ::= { tplinkDdmManageMIBObjects 2 } 
			 												
				ddmTempThresholdTable OBJECT-TYPE
					SYNTAX SEQUENCE OF DDMTempThresholdEntry
					MAX-ACCESS	not-accessible
					STATUS			current
					DESCRIPTION 
					"A table that is used to configure the DDM Temperature Threshold for specific ports on the Switch."
					::= { ddmTempThreshold 1 }
				
				ddmTempThresholdEntry OBJECT-TYPE
					SYNTAX			DDMTempThresholdEntry
					MAX-ACCESS	not-accessible
					STATUS			current
					DESCRIPTION 
					"A list of information for every port."	
					INDEX { ifIndex }
					::= { ddmTempThresholdTable 1 }
					
				DDMTempThresholdEntry ::=
				SEQUENCE
				{
                    ddmTempThresholdPort			DisplayString(SIZE(0..255)),
					ddmTempThresholdHighAlarm		OCTET STRING(SIZE(0..30)),
					ddmTempThresholdLowAlarm		OCTET STRING(SIZE(0..30)),
					ddmTempThresholdHighWarn		OCTET STRING(SIZE(0..30)),
					ddmTempThresholdLowWarn			OCTET STRING(SIZE(0..30)),
					ddmTempThresholdPortLAG			OCTET STRING(SIZE(0..30))
				}
				         
				ddmTempThresholdPort OBJECT-TYPE
					SYNTAX				DisplayString(SIZE(0..255))
					MAX-ACCESS			read-only
					STATUS				current
					DESCRIPTION
					"This object indicates the port number."
					::= { ddmTempThresholdEntry 1 }

				ddmTempThresholdHighAlarm OBJECT-TYPE
					SYNTAX 				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the highest threshold for the alarm."
					::= { ddmTempThresholdEntry 2 }
				
				ddmTempThresholdLowAlarm OBJECT-TYPE
					SYNTAX				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the lowest threshold for the alarm."
					::=	{ ddmTempThresholdEntry 3 }
		        
				ddmTempThresholdHighWarn OBJECT-TYPE
					SYNTAX 				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the highest threshold for the warning."
					::= { ddmTempThresholdEntry 4 }
				
				ddmTempThresholdLowWarn OBJECT-TYPE
					SYNTAX				OCTET STRING(SIZE(0..30)) 
					MAX-ACCESS			read-write
					STATUS				current
					DESCRIPTION		
					"This object indicates the lowest threshold for the warning."
					::=	{ ddmTempThresholdEntry 5 }

				ddmTempThresholdPortLAG OBJECT-TYPE
					SYNTAX				OCTET STRING(SIZE(0..30))
					MAX-ACCESS			read-only
					STATUS				current
					DESCRIPTION
					"This object indicates the lag number of the port."
					::= { ddmTempThresholdEntry 6 }
																			
END
					