-- This module defines enterprise MIBs for NS web setting
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-SET-WEB-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenSetting, netscreenSettingMibModule
        FROM NETSCREEN-SMI
    Integer32, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    ;

netscreenSetWebMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines the object that are used to monitor 
         NS web setting"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311120000Z" -- November 12, 2003
    DESCRIPTION
        "Correct spelling mistake"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "No comment"
    REVISION      "200105270000Z" -- May 27, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenSettingMibModule 12 }

NsSetWebUICfgEntry ::= SEQUENCE
{
    nsSetWebVsys           Integer32,
    nsSetWebIdleTimeout    INTEGER,
    nsSetWebTimeout        Integer32,
    nsSetWebPort           Integer32,
    nsSetWebSSLPort        Integer32,
    nsSetWebSSLCertificate DisplayString,
    nsSetWebSSLCipher      INTEGER
}

nsSetWebUI OBJECT IDENTIFIER ::= { netscreenSetting 12 }

nsSetWebUICfgTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsSetWebUICfgEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "NetScreen devices provide WebUI for easy administration. This
         table collects admin settings relating to WebUI."
    ::= { nsSetWebUI 1 }

nsSetWebUICfgEntry OBJECT-TYPE
    SYNTAX        NsSetWebUICfgEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry containing WebUI admin configuration."
    INDEX
        { nsSetWebVsys }
    ::= { nsSetWebUICfgTable 1 }

nsSetWebVsys OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Virtual system name the configuration belongs to. Also used as
         table index."
    ::= { nsSetWebUICfgEntry 1 }

nsSetWebIdleTimeout OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable Web Management Idle Timeout"
    ::= { nsSetWebUICfgEntry 2 }

nsSetWebTimeout OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Web Management Idle Timeout Setting"
    ::= { nsSetWebUICfgEntry 3 }

nsSetWebPort OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Web Management Http port number setting."
    ::= { nsSetWebUICfgEntry 4 }

nsSetWebSSLPort OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Web Management http ssl port number setting."
    ::= { nsSetWebUICfgEntry 5 }

nsSetWebSSLCertificate OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SSL certificate web management."
    ::= { nsSetWebUICfgEntry 6 }

nsSetWebSSLCipher OBJECT-TYPE
    SYNTAX        INTEGER {
        rc4-md5(0),
        rc4-40-md5(1),
        des-sha(2),
        triple-des-sha(3)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Web Management via SSL cipher algorithm"
    ::= { nsSetWebUICfgEntry 7 }

END


