--***************************************************************************
-- CXR-TS-MIB - Version 1.14 - April 21 2004
--***************************************************************************

  CXR-TS-MIB
  
  DEFINITIONS ::= BEGIN


   IMPORTS
    IpAddress, enterprises 	FROM RFC1155-SMI
    OBJECT-TYPE	FROM RFC-1212
    DisplayString FROM RFC-1213
    TRAP-TYPE FROM RFC-1215;

  --*************************************************************************
  -- Define the enterprise number as allocated by the internet authority
  cxr OBJECT IDENTIFIER ::= { enterprises 1425 }

  --*************************************************************************
  --*************************************************************************
  -- the overall structure of the MIB
  --*************************************************************************
  --*************************************************************************

  ts		OBJECT IDENTIFIER ::= { cxr 1040 }


  --*************************************************************************
	-- First Group: system
	
  system      OBJECT IDENTIFIER ::= { ts  1 }

  --*************************************************************************

  productName     OBJECT-TYPE
    SYNTAX          DisplayString
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "Product Name"
    ::= { system 1 }

  version     OBJECT-TYPE
    SYNTAX          DisplayString
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "Revision"
    ::= { system 2 }

  bootp     OBJECT-TYPE
    SYNTAX          INTEGER {
			enable(1),
			disable(2)
	}
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Bootp"
    ::= { system 3 }

  mainIpAddress     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "IP address"
    ::= { system 4 }

  ipNetmask     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "IP Netmask"
    ::= { system 5 }

  ipGateway     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "IP Gateway"
    ::= { system 6 }

  ethernetAddress     OBJECT-TYPE
    SYNTAX      OCTET STRING
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "Mac Address"
    ::= { system 7 }

  ftpdService     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "FTPD Service"
    ::= { system  8 }

  httpdService     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "HTTPD Service"
    ::= { system  9 }

  telnetdService     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "TELNETD Service"
    ::= { system  10 }

  snmpdService     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "SNMPD Service"
    ::= { system  11 }

  snmpTrap	     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "SNMP Traps"


    ::= { system  12 }

  snmpTrapAddr1     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Trap IP Address"
    ::= { system  13 }

	snmpTrapAddr2     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Trap IP Address"
    ::= { system  14 }

  nameResolution	OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Names Resolution"
    ::= { system  15 }

  nameServer1     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Names Server 1"
    ::= { system  16 }

	nameServer2     OBJECT-TYPE
    SYNTAX	  IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Names Server 1"
    ::= { system  17 }

	radiusServer1     OBJECT-TYPE
    SYNTAX	  IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Radius Server 1"
    ::= { system  18 }

  radiusSecret1     OBJECT-TYPE
    SYNTAX      		DisplayString
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Secret for Radius Server 1"
    ::= { system  19 }

 	radiusServer2     OBJECT-TYPE
    SYNTAX	  IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Radius Server 2"
    ::= { system  20 }

  radiusSecret2     OBJECT-TYPE
    SYNTAX      		DisplayString
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Secret for Radius Server 2"
    ::= { system  21 }

  siteName     			OBJECT-TYPE
    SYNTAX      		DisplayString
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "String indetifier for TS"
    ::= { system  22 }

  resetByButton	OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Reset by button Enable ot Disable"
    ::= { system  23 }

  reset     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Reset the TS"
    ::= { system  24 }

  --*************************************************************************
	-- Second Group: port
	
  portTable OBJECT-TYPE
    			     	SYNTAX SEQUENCE OF PortEntry
         				ACCESS not-accessible
				        STATUS mandatory
                DESCRIPTION
				"A table containing all the ports"
        ::= { ts  2 }

	portEntry OBJECT-TYPE
                SYNTAX PortEntry
                ACCESS not-accessible
                STATUS mandatory
    						DESCRIPTION
        				"Port index 1 to 11 possible"
                INDEX { portIndex }
        ::= { portTable 1 }

	PortEntry ::= SEQUENCE {
    portIndex	INTEGER,
    tcpPort  INTEGER,
    aliasIpAddress IpAddress,
    aliasIpNetmask IpAddress,
    timeoutRxTx  INTEGER,
    baudRate INTEGER,
    nbParStop  INTEGER,
    ipServer  INTEGER,
    remoteIpAddress  IpAddress,
    gatewayToRemote  IpAddress,
    remoteTcpPort  INTEGER,
    flowControl  INTEGER,
    mode  INTEGER,
    rxIdle  INTEGER,
    txIdle  INTEGER,
    endMsg  OCTET STRING,
    interFrame INTEGER,
    beforeSend  INTEGER,
    afterSend  INTEGER,
    timeoutPAD  INTEGER,
    terminalType INTEGER,
    multiSession INTEGER,
    authType  INTEGER,
    authRad1  INTEGER,
    authRad2  INTEGER,
    acctRad1  INTEGER,
    acctRad2  INTEGER,
	formFeed  INTEGER,
    secondIpAddress  IpAddress,
    secondGateway  IpAddress,
    secondTcpPort  INTEGER,
    modbusMode INTEGER,
    modbusType INTEGER,
    portReset INTEGER
  }

  --*************************************************************************

  --*************************************************************************
	-- Second Group: port
  --*************************************************************************

  portIndex     OBJECT-TYPE
    SYNTAX      INTEGER (1..11)
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "Port Index"
    ::= { portEntry  1 }

  tcpPort     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "TCP port"
    ::= { portEntry	2 }

  aliasIpAddress     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Alias IP address"
    ::= { portEntry	3 }

  aliasIpNetmask     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Alias IP netmask"
    ::= { portEntry	4 }

  timeoutRxTx     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Timeout No rx/Tx Data(min)"
    ::= { portEntry	5 }

  baudRate     OBJECT-TYPE
    SYNTAX          INTEGER {
	b300(1),
	b600(2),
	b1200(3),
	b2400(4),
	b4800(5),
	b9600(6),
	b19200(7),
	b38400(8),
	b57600(9),
	b115200(10),
	b50(11),
	b200(12)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Baud rate"
    ::= { portEntry	6 }

  nbParStop     OBJECT-TYPE
    SYNTAX      INTEGER {
	p7Odd1(1),
	p7Odd2(2),
	p7Even1(17),
	p7Even2(18),
	p7None1(33),
	p7None2(34),
	p7High1(49),
	p7High2(50),
	p7Low1(65),
	p7Low2(66),
	p8Odd1(129),

	p8Odd2(130),
	p8Even1(145),
	p8Even2(146),
	p8None1(161),
	p8None2(162),
	p8High1(177),
	p8High2(178),
	p8Low1(193),
	p8Low2(194)
     }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Nb bits/Parity/Nb stop bits"
    ::= { portEntry	7 }

  ipServer     OBJECT-TYPE
    SYNTAX      INTEGER {
	active(1),
	passive(2),
	passiveExclusive(3)
    }
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "Server IP"
    ::= { portEntry	8 }

  remoteIpAddress     OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Remote IP address"
    ::= { portEntry	9 }

  gatewayToRemote    OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Gateway to remote"
    ::= { portEntry	10 }

  remoteTcpPort     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "remote TCP port"
    ::= { portEntry	11 }

  flowControl     OBJECT-TYPE
    SYNTAX      INTEGER {
			noFlowControl(1),
			xonXoff(2),
			rtsCts(3)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Flow Control"
    ::= { portEntry	12 }

  mode     OBJECT-TYPE
    SYNTAX      INTEGER {
			rfc2217(1),
			msgFormat(2),
			carrierBreak(3),
			telex(4),
			rlogin(5),
			lpd(6),
			telnet(7),
			rawIp(8),
			rtelnet(9),
			pad(10),
			muxv24(11),
			modbus(12),
			hnzs2(13),
			hnzs5(14),
		}
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Fonctionnement"
    ::= { portEntry  13 }

  rxIdle     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Rx Idle"
    ::= { portEntry  14 }

  txIdle     OBJECT-TYPE
    SYNTAX          INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Tx Idle"
    ::= { portEntry  15 }

  endMsg     OBJECT-TYPE
    SYNTAX      OCTET STRING
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "End msg character"
    ::= { portEntry	16 }

  interFrame     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Time Inter Frame(modem mode)"
    ::= { portEntry  17 }

  beforeSend     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Time Before Send(modem mode)"
    ::= { portEntry  18 }

  afterSend     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "Time After Send(modem mode)"
    ::= { portEntry  19 }

  timeoutPAD     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Timeout PAD(modem PAD)"
    ::= { portEntry  20 }


  terminalType     OBJECT-TYPE
    SYNTAX      INTEGER {
			console(1),
			linux(2),
			aixterm(3),
			dec-vt100(4),
			vt100(5),
			vt200(6),
			vt420(7),
			xterm(8),
			xterms(9),
			xtermc(10)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "Terminal Type"
    ::= { portEntry  21 }

  multiSession     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "multiSession"
    ::= { portEntry  22 }

  authType     OBJECT-TYPE
    SYNTAX      INTEGER {
			remote(1),
			radius(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "Authentication type"
    ::= { portEntry  23 }

  authRad1     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "Use Server Radius 1 for auth."
    ::= { portEntry  24 }

  authRad2     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "Use Server Radius 2 for auth."
    ::= { portEntry  25 }

  acctRad1     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "Use Server Radius 1 for acct."
    ::= { portEntry  26 }

  acctRad2     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
		}
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION    "Use Server Radius 2 for acct."
    ::= { portEntry  27 }

  formFeed     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
		}
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "LPD form Feed"
    ::= { portEntry  28 }

  secondIpAddress   OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Second IP address"
    ::= { portEntry	29 }

  secondGateway	    OBJECT-TYPE
    SYNTAX	    IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Second Gateway"
    ::= { portEntry	30 }

  secondTcpPort     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Second TCP port"
    ::= { portEntry	31 }

  modbusMode     OBJECT-TYPE
    SYNTAX      INTEGER {
			rtu(1),
			ascii(2)
		}
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Modbus Mode"
    ::= { portEntry	32 }

  modbusType     OBJECT-TYPE
    SYNTAX      INTEGER {
			slave(1),
			master(2)
		}
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Modbus Type"
    ::= { portEntry	33 }

  portReset     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Apply changes to port"
    ::= { portEntry  34 }

--*************************************************************************
-- Third Group: port Stats
  portStatsTable OBJECT-TYPE
    			     	SYNTAX SEQUENCE OF PortStatsEntry
         				ACCESS not-accessible
				        STATUS mandatory
                DESCRIPTION
				"A table containing all the statistics ports"
        ::= { ts  3 }
	
	portStatsEntry OBJECT-TYPE
                SYNTAX PortStatsEntry
                ACCESS not-accessible
                STATUS mandatory
    						DESCRIPTION
       					 "Port index 1 to 11 possible"
                INDEX { portIndex }
        ::= { portStatsTable 1 }

	PortStatsEntry ::= SEQUENCE {
    bytesReceiveFromV24 INTEGER,
		bytesSendToV24      INTEGER,
		statusDTR			      INTEGER
  }
	

--*************************************************************************
-- Third Group: port Stats
--*************************************************************************
    bytesReceiveFromV24     OBJECT-TYPE
    SYNTAX      		INTEGER
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "Bytes received from V24"
    ::= { portStatsEntry  1}

    bytesSendToV24     OBJECT-TYPE
    SYNTAX      		INTEGER
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "Bytes send to V24"
    ::= { portStatsEntry  2}

    statusDTR     OBJECT-TYPE
    SYNTAX      INTEGER {
			on(1),
			off(2)
    }
    ACCESS          read-only
    STATUS          mandatory
    DESCRIPTION     "DTR Status"
    ::= { portStatsEntry  3}



--*************************************************************************
-- Fourth Group: modbus Param
  modbusTable OBJECT-TYPE
    			     	SYNTAX SEQUENCE OF ModbusEntry
         				ACCESS not-accessible
				        STATUS mandatory
                DESCRIPTION
	"Master modbus table containing all the slave parameters table"
        ::= { ts  4 }
	
	modbusEntry OBJECT-TYPE
                SYNTAX ModbusEntry
                ACCESS not-accessible
                STATUS mandatory
		DESCRIPTION
	 "Slave index 1 to 16 possible"
                INDEX { portIndex }
        ::= { modbusTable 1 }

	ModbusEntry ::= SEQUENCE {
	    slaveHexaAddress INTEGER,
	    slaveIPaddr IpAddress,
	    slaveIPport INTEGER
  }
	

--*************************************************************************
-- Fourth Group: modbus
--*************************************************************************
    slaveHexaAddress     OBJECT-TYPE
    SYNTAX      		INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Modbus Hexadecimal address"
    ::= { modbusEntry  1}

    slaveIPaddr     OBJECT-TYPE
    SYNTAX      		IpAddress
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Modbus IP address"
    ::= { modbusEntry  2}

    slaveIPport     OBJECT-TYPE
    SYNTAX      INTEGER
    ACCESS          read-write
    STATUS          mandatory
    DESCRIPTION     "Modbus IP Port"
    ::= { modbusEntry  3}


  --*************************************************************************
        -- TRAP : Terminal SERVER
  --*************************************************************************

 sessionStarted TRAP-TYPE
	ENTERPRISE  cxr
  VARIABLES   { portIndex }
  DESCRIPTION "Session Begin"
    	::= 1041

 sessionStopped TRAP-TYPE
	ENTERPRISE  cxr
	VARIABLES   { portIndex }
	DESCRIPTION "Session End"
    	::= 1042

 dtrUp TRAP-TYPE
	ENTERPRISE  cxr

	VARIABLES   { portIndex }
	DESCRIPTION "DTR UP"
    	::= 1043

 dtrDown TRAP-TYPE
	ENTERPRISE  cxr
	VARIABLES   { portIndex }
	DESCRIPTION "DTR DOWN"
    	::= 1044



END

