DKT-FE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    Counter32                   FROM SNMPv2-SMI
    OBJECT-GROUP				FROM SNMPv2-CONF
    dkt                         FROM DKT-MIB;

feMIB MODULE-IDENTITY
    LAST-UPDATED  "200812170000Z"
    ORGANIZATION "DKT A/S"
    CONTACT-INFO
        "postal:  DKT A/S
                  Fanoevej 6
                  DK-4060 Kirke Saaby
                  Denmark

         email:   info@dktcomega.com"
    DESCRIPTION   "DKT Fast Ethernet MIB."
    ::= { dkt 12 }

feSwitchEngine OBJECT IDENTIFIER ::= { feMIB 1 }


feATU OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..20480))
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Dumps the Address Translation Unit (ATU) Switch table in semi colon format" 
    ::= { feSwitchEngine 1 }

feUnicastDelete
 OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Removes a unicast MAC address from the Address Translation Unit (ATU) Switch table."
    ::= { feSwitchEngine 2 }

feMulticastDelete
 OBJECT-TYPE
    SYNTAX	IpAddress
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Removes a multicast IP address from the Address Translation Unit (ATU) Switch table."
    ::= { feSwitchEngine 3 }

feIGMPSnooping OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Starts/stops IGMP snooping, input parameter 0 = stops IGMP snooping, 1 = starts IGMP snooping. Per Default IGMP snooping is enabled, but has to be configured per port"
    ::= { feSwitchEngine 4 }

feVTU OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..9600))
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Dumps the VLAN Table Unit (VTU) Switch table in semi colon format"  
    ::= { feSwitchEngine 5 }

feVLANCreate OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Creates a VLAN, input parameters are: VID:WAN:LAN1:LAN2:LAN3:LAN4:CPU:NRL-ENABLE"
    ::= { feSwitchEngine 6 }

feVLANDelete OBJECT-TYPE
    SYNTAX	INTEGER (0..4095)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Deletes a VLAN, input parameter is VLAN VID: 0 - 4095"
    ::= { feSwitchEngine 7 }

feClearVTU OBJECT-TYPE
    SYNTAX	INTEGER (1)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Clears the VLAN Table Unit (VTU) Switch table, input parameter 1 = clear VTU table"
    ::= { feSwitchEngine 8 }

feDumpPIRLBuckets OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..10))
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Dumps a list of the active buckets."
    ::= { feSwitchEngine 9 }

feDisablePIRLBucket OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Disables an already defined Port Ingress Rate Limitation (PIRL) bucket, input parameter bucket 0 - 11."
    ::= { feSwitchEngine 10 }

feVLANProviderMode OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enable/disable VLAN provider mode, input parameter 0 = disable VLAN provider mode, 1 = enable VLAN provider mode. Per Default VLAN provider mode is disabled. NOTE: Provider VLAN ID should be setup in port default VID for the originating port."
    ::= { feSwitchEngine 11 }

fePorts OBJECT IDENTIFIER ::= { feMIB 2 }

feCPUPort OBJECT IDENTIFIER ::= { fePorts 1 }

feCPUPortAutoNegotiation OBJECT-TYPE
    SYNTAX	INTEGER (0..10)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Enables/disables auto negotiation on the port. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 1 }

feCPUPortSpeedMode OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..10))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Sets/gets the speed and duplex mode on the port. Input parameters are: 100FD|100HD|10FD|10HD|AUTO|FD|HD"
    ::= { feCPUPort 2 }


feCPUPortLinkStatus OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Gets the Link status for the port"
    ::= { feCPUPort 3 }


feCPUPortFlowControl OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables flow control on the port. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 4 }


feCPUPortIEEEQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on there IEEE priority tags. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 5 }


feCPUPortIPQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on their IP4/IP6 priority fields. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 6 }

feCPUPortFramePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(DA) Frame Priority Override on an ATU match. XX_FRAME_PRIO_OVERRIDE=0..1."
    ::= { feCPUPort 7 }


feCPUPortQueuePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(SA) Queue Priority Override on an ATU match. XX_QUEUE_PRIO_OVERRIDE=0..1."
    ::= { feCPUPort 8 }


feCPUPortQueuePriority OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Queue priority, input parameters: PRIO:ENABLE     PRIO: 0 - 7  ENABLE: 0 - 1  "
    ::= { feCPUPort 9 }


feCPUPortQoSPortMapRule OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces queue priority for a port. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 10 }


feCPUPortVIDNRLEnable OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables per port the Non rate limit for VLANs with the NRL bit enabled. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 11 }


feCPUPortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds/maps the port to a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feCPUPort 12 }


feCPUPortDeletePortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Deletes the port from a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feCPUPort 13 }


feCPUPortEgressRateLimitation OBJECT-TYPE
    SYNTAX	Integer32
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the egress limitation rate for the port. Input parameter is value in kbps"
    ::= { feCPUPort 14 }


feCPUPortIngressRateLimitation OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets a Port Input Rate Limit(PIRL) bucket. Input parameters are: bucket:rate:layer:(DROP|FC)"
    ::= { feCPUPort 15 }


feCPUPortDefaultVLAN OBJECT-TYPE
    SYNTAX	INTEGER
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the default VLAN ID(VID) for the port. Input parameter is 0 - 4095"
    ::= { feCPUPort 16 }


feCPUPortForceDefaultVID OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces the tagging of VID on all frames on the port. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 17 }


feCPUPortVLANPortMode OBJECT-TYPE
    SYNTAX	INTEGER (0..3)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the 802.1Q mode for the ingress port.
       Mode either 0=disable,
                   1=fallback,
                   2=check,
                   3=secure"
    ::= { feCPUPort 18 }


feCPUPortBlockAllUnknown OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"This will make sure that all frames received on the port are blocked, unless they are tagged with the correct VID."
    ::= { feCPUPort 19 }


feCPUPortIGMPSnooping OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables IGMP snooping. Set to 1 for enable and 0 for disable."
    ::= { feCPUPort 20 }


feCPUPortAddUnicast OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the unicast mac address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aa:bb:cc:dd:ee:ff"
    ::= { feCPUPort 21 }


feCPUPortAddMulticast OBJECT-TYPE
    SYNTAX	IpAddress
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the IP multicast address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aaa.bbb.ccc.ddd"
    ::= { feCPUPort 22 }




feWANPort OBJECT IDENTIFIER ::= { fePorts 2 }

feWANPortAutoNegotiation OBJECT-TYPE
    SYNTAX	INTEGER (0..10)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Enables/disables auto negotiation on the port. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 1 }

feWANPortSpeedMode OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..10))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Sets/gets the speed and duplex mode on the port. Valid values are (100FD|100HD|10FD|10HD|AUTO|FD|HD)"
    ::= { feWANPort 2 }


feWANPortLinkStatus OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Gets the Link status for the port"
    ::= { feWANPort 3 }


feWANPortFlowControl OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables flow control on the port. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 4 }


feWANPortIEEEQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on there IEEE priority tags. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 5 }


feWANPortIPQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on their IP4/IP6 priority fields. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 6 }

feWANPortFramePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(DA) Frame Priority Override on an ATU match. XX_FRAME_PRIO_OVERRIDE=0..1."
    ::= { feWANPort 7 }


feWANPortQueuePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(SA) Queue Priority Override on an ATU match. XX_QUEUE_PRIO_OVERRIDE=0..1."
    ::= { feWANPort 8 }


feWANPortQueuePriority OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Queue priority, input parameters: PRIO:ENABLE     PRIO: 0 - 7  ENABLE: 0 - 1  "
    ::= { feWANPort 9 }


feWANPortQoSPortMapRule OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces queue priority for a port. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 10 }


feWANPortVIDNRLEnable OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables per port the Non rate limit for VLANs with the NRL bit enabled. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 11 }


feWANPortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds/maps the port to a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feWANPort 12 }


feWANPortDeletePortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Deletes the port from a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feWANPort 13 }


feWANPortEgressRateLimitation OBJECT-TYPE
    SYNTAX	Integer32
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the egress limitation rate for the port. Input parameter is value in kbps"
    ::= { feWANPort 14 }


feWANPortIngressRateLimitation OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Sets a Port Input Rate Limit(PIRL) bucket. Input parameters are: bucket:rate:layer:(DROP|FC)"
    ::= { feWANPort 15 }


feWANPortDefaultVLAN OBJECT-TYPE
    SYNTAX	INTEGER
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the default VLAN ID(VID) for the port. Input parameter is 0 - 4095"
    ::= { feWANPort 16 }


feWANPortForceDefaultVID OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces the tagging of VID on all frames on the port. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 17 }


feWANPortVLANPortMode OBJECT-TYPE
    SYNTAX	INTEGER (0..3)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the 802.1Q mode for the ingress port.
       Mode either 0=disable,
                   1=fallback,
                   2=check,
                   3=secure"
    ::= { feWANPort 18 }


feWANPortBlockAllUnknown OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"This will make sure that all frames received on the port are blocked, unless they are tagged with the correct VID."
    ::= { feWANPort 19 }


feWANPortIGMPSnooping OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables IGMP snooping. Set to 1 for enable and 0 for disable."
    ::= { feWANPort 20 }


feWANPortAddUnicast OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the unicast mac address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aa:bb:cc:dd:ee:ff"
    ::= { feWANPort 21 }


feWANPortAddMulticast OBJECT-TYPE
    SYNTAX	IpAddress
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the IP multicast address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aaa.bbb.ccc.ddd"
    ::= { feWANPort 22 }


feWANPortArpMirroring OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Mirror ARP packets seen on the port to the CPU port."
    ::= { feWANPort 23 }


feLAN1Port OBJECT IDENTIFIER ::= { fePorts 3 }

feLAN1PortAutoNegotiation OBJECT-TYPE
    SYNTAX	INTEGER (0..10)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Enables/disables auto negotiation on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 1 }

feLAN1PortSpeedMode OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..10))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Sets/gets the speed and duplex mode on the port. Valid values are (100FD|100HD|10FD|10HD|AUTO|FD|HD)"
    ::= { feLAN1Port 2 }


feLAN1PortLinkStatus OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Gets the Link status for the port"
    ::= { feLAN1Port 3 }


feLAN1PortFlowControl OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables flow control on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 4 }


feLAN1PortIEEEQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on there IEEE priority tags. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 5 }


feLAN1PortIPQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on their IP4/IP6 priority fields. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 6 }

feLAN1PortFramePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(DA) Frame Priority Override on an ATU match. XX_FRAME_PRIO_OVERRIDE=0..1."
    ::= { feLAN1Port 7 }


feLAN1PortQueuePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(SA) Queue Priority Override on an ATU match. XX_QUEUE_PRIO_OVERRIDE=0..1."
    ::= { feLAN1Port 8 }


feLAN1PortQueuePriority OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Queue priority, input parameters: PRIO:ENABLE     PRIO: 0 - 7  ENABLE: 0 - 1  "
    ::= { feLAN1Port 9 }


feLAN1PortQoSPortMapRule OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces queue priority for a port. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 10 }


feLAN1PortVIDNRLEnable OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables per port the Non rate limit for VLANs with the NRL bit enabled. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 11 }


feLAN1PortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds/maps the port to a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN1Port 12 }


feLAN1PortDeletePortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Deletes the port from a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN1Port 13 }


feLAN1PortEgressRateLimitation OBJECT-TYPE
    SYNTAX	Integer32
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the egress limitation rate for the port. Input parameter is value in kbps"
    ::= { feLAN1Port 14 }


feLAN1PortIngressRateLimitation OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Sets a Port Input Rate Limit(PIRL) bucket. Input parameters are: bucket:rate:layer:(DROP|FC)"
    ::= { feLAN1Port 15 }


feLAN1PortDefaultVLAN OBJECT-TYPE
    SYNTAX	INTEGER
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the default VLAN ID(VID) for the port. Input parameter is 0 - 4095"
    ::= { feLAN1Port 16 }


feLAN1PortForceDefaultVID OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces the tagging of VID on all frames on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 17 }


feLAN1PortVLANPortMode OBJECT-TYPE
    SYNTAX	INTEGER (0..3)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the 802.1Q mode for the ingress port.
       Mode either 0=disable,
                   1=fallback,
                   2=check,
                   3=secure"
    ::= { feLAN1Port 18 }


feLAN1PortBlockAllUnknown OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"This will make sure that all frames received on the port are blocked, unless they are tagged with the correct VID."
    ::= { feLAN1Port 19 }


feLAN1PortIGMPSnooping OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables IGMP snooping. Set to 1 for enable and 0 for disable."
    ::= { feLAN1Port 20 }


feLAN1PortAddUnicast OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the unicast mac address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aa:bb:cc:dd:ee:ff"
    ::= { feLAN1Port 21 }


feLAN1PortAddMulticast OBJECT-TYPE
    SYNTAX	IpAddress
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the IP multicast address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aaa.bbb.ccc.ddd"
    ::= { feLAN1Port 22 }


feLAN1PortArpMirroring OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Mirror ARP packets seen on the port to the CPU port."
    ::= { feLAN1Port 23 }



feLAN2Port OBJECT IDENTIFIER ::= { fePorts 4 }

feLAN2PortAutoNegotiation OBJECT-TYPE
    SYNTAX	INTEGER (0..10)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Enables/disables auto negotiation on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 1 }

feLAN2PortSpeedMode OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..10))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Sets/gets the speed and duplex mode on the port. Valid values are (100FD|100HD|10FD|10HD|AUTO|FD|HD)"
    ::= { feLAN2Port 2 }


feLAN2PortLinkStatus OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Gets the Link status for the port"
    ::= { feLAN2Port 3 }


feLAN2PortFlowControl OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables flow control on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 4 }


feLAN2PortIEEEQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on there IEEE priority tags. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 5 }


feLAN2PortIPQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on their IP4/IP6 priority fields. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 6 }

feLAN2PortFramePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(DA) Frame Priority Override on an ATU match. XX_FRAME_PRIO_OVERRIDE=0..1."
    ::= { feLAN2Port 7 }


feLAN2PortQueuePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(SA) Queue Priority Override on an ATU match. XX_QUEUE_PRIO_OVERRIDE=0..1."
    ::= { feLAN2Port 8 }


feLAN2PortQueuePriority OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Queue priority, input parameters: PRIO:ENABLE     PRIO: 0 - 7  ENABLE: 0 - 1  "
    ::= { feLAN2Port 9 }


feLAN2PortQoSPortMapRule OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces queue priority for a port. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 10 }


feLAN2PortVIDNRLEnable OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables per port the Non rate limit for VLANs with the NRL bit enabled. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 11 }


feLAN2PortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds/maps the port to a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN2Port 12 }


feLAN2PortDeletePortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Deletes the port from a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN2Port 13 }


feLAN2PortEgressRateLimitation OBJECT-TYPE
    SYNTAX	Integer32
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the egress limitation rate for the port. Input parameter is value in kbps"
    ::= { feLAN2Port 14 }


feLAN2PortIngressRateLimitation OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Sets a Port Input Rate Limit(PIRL) bucket. Input parameters are: bucket:rate:layer:(DROP|FC)"
    ::= { feLAN2Port 15 }


feLAN2PortDefaultVLAN OBJECT-TYPE
    SYNTAX	INTEGER
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the default VLAN ID(VID) for the port. Input parameter is 0 - 4095"
    ::= { feLAN2Port 16 }


feLAN2PortForceDefaultVID OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces the tagging of VID on all frames on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 17 }


feLAN2PortVLANPortMode OBJECT-TYPE
    SYNTAX	INTEGER (0..3)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the 802.1Q mode for the ingress port.
       Mode either 0=disable,
                   1=fallback,
                   2=check,
                   3=secure"
    ::= { feLAN2Port 18 }


feLAN2PortBlockAllUnknown OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"This will make sure that all frames received on the port are blocked, unless they are tagged with the correct VID."
    ::= { feLAN2Port 19 }


feLAN2PortIGMPSnooping OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables IGMP snooping. Set to 1 for enable and 0 for disable."
    ::= { feLAN2Port 20 }


feLAN2PortAddUnicast OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the unicast mac address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aa:bb:cc:dd:ee:ff"
    ::= { feLAN2Port 21 }


feLAN2PortAddMulticast OBJECT-TYPE
    SYNTAX	IpAddress
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the IP multicast address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aaa.bbb.ccc.ddd"
    ::= { feLAN2Port 22 }


feLAN2PortArpMirroring OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Mirror ARP packets seen on the port to the CPU port."
    ::= { feLAN2Port 23 }


feLAN3Port OBJECT IDENTIFIER ::= { fePorts 5 }

feLAN3PortAutoNegotiation OBJECT-TYPE
    SYNTAX	INTEGER (0..10)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Enables/disables auto negotiation on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 1 }

feLAN3PortSpeedMode OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..10))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Sets/gets the speed and duplex mode on the port. Valid values are (100FD|100HD|10FD|10HD|AUTO|FD|HD)"
    ::= { feLAN3Port 2 }


feLAN3PortLinkStatus OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Gets the Link status for the port"
    ::= { feLAN3Port 3 }


feLAN3PortFlowControl OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables flow control on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 4 }


feLAN3PortIEEEQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on there IEEE priority tags. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 5 }


feLAN3PortIPQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on their IP4/IP6 priority fields. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 6 }

feLAN3PortFramePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(DA) Frame Priority Override on an ATU match. XX_FRAME_PRIO_OVERRIDE=0..1."
    ::= { feLAN3Port 7 }


feLAN3PortQueuePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(SA) Queue Priority Override on an ATU match. XX_QUEUE_PRIO_OVERRIDE=0..1."
    ::= { feLAN3Port 8 }


feLAN3PortQueuePriority OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Queue priority, input parameters: PRIO:ENABLE     PRIO: 0 - 7  ENABLE: 0 - 1  "
    ::= { feLAN3Port 9 }


feLAN3PortQoSPortMapRule OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces queue priority for a port. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 10 }


feLAN3PortVIDNRLEnable OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables per port the Non rate limit for VLANs with the NRL bit enabled. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 11 }


feLAN3PortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds/maps the port to a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN3Port 12 }


feLAN3PortDeletePortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Deletes the port from a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN3Port 13 }


feLAN3PortEgressRateLimitation OBJECT-TYPE
    SYNTAX	Integer32
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the egress limitation rate for the port. Input parameter is value in kbps"
    ::= { feLAN3Port 14 }


feLAN3PortIngressRateLimitation OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Sets a Port Input Rate Limit(PIRL) bucket. Input parameters are: bucket:rate:layer:(DROP|FC)"
    ::= { feLAN3Port 15 }


feLAN3PortDefaultVLAN OBJECT-TYPE
    SYNTAX	INTEGER
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the default VLAN ID(VID) for the port. Input parameter is 0 - 4095"
    ::= { feLAN3Port 16 }


feLAN3PortForceDefaultVID OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces the tagging of VID on all frames on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 17 }


feLAN3PortVLANPortMode OBJECT-TYPE
    SYNTAX	INTEGER (0..3)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the 802.1Q mode for the ingress port.
       Mode either 0=disable,
                   1=fallback,
                   2=check,
                   3=secure"
    ::= { feLAN3Port 18 }


feLAN3PortBlockAllUnknown OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"This will make sure that all frames received on the port are blocked, unless they are tagged with the correct VID."
    ::= { feLAN3Port 19 }


feLAN3PortIGMPSnooping OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables IGMP snooping. Set to 1 for enable and 0 for disable."
    ::= { feLAN3Port 20 }


feLAN3PortAddUnicast OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the unicast mac address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aa:bb:cc:dd:ee:ff"
    ::= { feLAN3Port 21 }


feLAN3PortAddMulticast OBJECT-TYPE
    SYNTAX	IpAddress
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the IP multicast address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aaa.bbb.ccc.ddd"
    ::= { feLAN3Port 22 }


feLAN3PortArpMirroring OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Mirror ARP packets seen on the port to the CPU port."
    ::= { feLAN3Port 23 }


feLAN4Port OBJECT IDENTIFIER ::= { fePorts 6 }

feLAN4PortAutoNegotiation OBJECT-TYPE
    SYNTAX	INTEGER (0..10)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Enables/disables auto negotiation on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 1 }

feLAN4PortSpeedMode OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..10))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION  
	"Sets/gets the speed and duplex mode on the port. Valid values are (100FD|100HD|10FD|10HD|AUTO|FD|HD)"
    ::= { feLAN4Port 2 }


feLAN4PortLinkStatus OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-only
    STATUS	current
    DESCRIPTION
	"Gets the Link status for the port"
    ::= { feLAN4Port 3 }


feLAN4PortFlowControl OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables flow control on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 4 }


feLAN4PortIEEEQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on there IEEE priority tags. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 5 }


feLAN4PortIPQoSPriority OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables prioritized frames based on their IP4/IP6 priority fields. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 6 }

feLAN4PortFramePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(DA) Frame Priority Override on an ATU match. XX_FRAME_PRIO_OVERRIDE=0..1."
    ::= { feLAN4Port 7 }


feLAN4PortQueuePriorityOverwrite OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Source Address(SA) or Destination Address(SA) Queue Priority Override on an ATU match. XX_QUEUE_PRIO_OVERRIDE=0..1."
    ::= { feLAN4Port 8 }


feLAN4PortQueuePriority OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Queue priority, input parameters: PRIO:ENABLE     PRIO: 0 - 7  ENABLE: 0 - 1  "
    ::= { feLAN4Port 9 }


feLAN4PortQoSPortMapRule OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces queue priority for a port. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 10 }


feLAN4PortVIDNRLEnable OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables per port the Non rate limit for VLANs with the NRL bit enabled. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 11 }


feLAN4PortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds/maps the port to a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN4Port 12 }


feLAN4PortDeletePortMap2PIRL OBJECT-TYPE
    SYNTAX	INTEGER (0..11)
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Deletes the port from a Port Ingress Rate Limitation (PIRL) bucket. Input parameter is PIRL bucket no 0 - 11."
    ::= { feLAN4Port 13 }


feLAN4PortEgressRateLimitation OBJECT-TYPE
    SYNTAX	Integer32
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the egress limitation rate for the port. Input parameter is value in kbps"
    ::= { feLAN4Port 14 }


feLAN4PortIngressRateLimitation OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Sets a Port Input Rate Limit(PIRL) bucket. Input parameters are: bucket:rate:layer:(DROP|FC)"
    ::= { feLAN4Port 15 }


feLAN4PortDefaultVLAN OBJECT-TYPE
    SYNTAX	INTEGER
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the default VLAN ID(VID) for the port. Input parameter is 0 - 4095"
    ::= { feLAN4Port 16 }


feLAN4PortForceDefaultVID OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Forces the tagging of VID on all frames on the port. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 17 }


feLAN4PortVLANPortMode OBJECT-TYPE
    SYNTAX	INTEGER (0..3)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Sets the 802.1Q mode for the ingress port.
       Mode either 0=disable,
                   1=fallback,
                   2=check,
                   3=secure"
    ::= { feLAN4Port 18 }


feLAN4PortBlockAllUnknown OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"This will make sure that all frames received on the port are blocked, unless they are tagged with the correct VID."
    ::= { feLAN4Port 19 }


feLAN4PortIGMPSnooping OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Enables/disables IGMP snooping. Set to 1 for enable and 0 for disable."
    ::= { feLAN4Port 20 }


feLAN4PortAddUnicast OBJECT-TYPE
    SYNTAX	OCTET STRING (SIZE(0..100))
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the unicast mac address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aa:bb:cc:dd:ee:ff"
    ::= { feLAN4Port 21 }


feLAN4PortAddMulticast OBJECT-TYPE
    SYNTAX	IpAddress
    MAX-ACCESS	write-only
    STATUS	current
    DESCRIPTION
	"Adds the IP multicast address statically to the Address Translation Unit (ATU) Switch table. Input parameter is: aaa.bbb.ccc.ddd"
    ::= { feLAN4Port 22}

feLAN4PortArpMirroring OBJECT-TYPE
    SYNTAX	INTEGER (0..1)
    MAX-ACCESS	read-write
    STATUS	current
    DESCRIPTION
	"Mirror ARP packets seen on the port to the CPU port."
    ::= { feLAN4Port 23 }




feModuleGroup OBJECT-GROUP
	OBJECTS {
		feSwitchEngine,
		feATU,
		feUnicastDelete,
		feMulticastDelete,
		feIGMPSnooping,
		feVTU,
		feVLANCreate,
		feVLANDelete,
		feClearVTU,
		feDumpPIRLBuckets,
		feDisablePIRLBucket,
		feVLANProviderMode,
		fePorts,
		feCPUPort,
		feCPUPortAutoNegotiation, feCPUPortSpeedMode, feCPUPortLinkStatus, feCPUPortFlowControl, feCPUPortIEEEQoSPriority, feCPUPortIPQoSPriority, feCPUPortFramePriorityOverwrite, feCPUPortQueuePriorityOverwrite, feCPUPortQueuePriority, feCPUPortQoSPortMapRule, feCPUPortVIDNRLEnable, feCPUPortMap2PIRL, feCPUPortDeletePortMap2PIRL, feCPUPortEgressRateLimitation, feCPUPortIngressRateLimitation, feCPUPortDefaultVLAN, feCPUPortForceDefaultVID, feCPUPortVLANPortMode, feCPUPortBlockAllUnknown, feCPUPortIGMPSnooping, feCPUPortAddUnicast, feCPUPortAddMulticast, 
		feWANPort,
		feWANPortAutoNegotiation, feWANPortSpeedMode, feWANPortLinkStatus, feWANPortFlowControl, feWANPortIEEEQoSPriority, feWANPortIPQoSPriority, feWANPortFramePriorityOverwrite, feWANPortQueuePriorityOverwrite, feWANPortQueuePriority, feWANPortQoSPortMapRule, feWANPortVIDNRLEnable, feWANPortMap2PIRL, feWANPortDeletePortMap2PIRL, feWANPortEgressRateLimitation, feWANPortIngressRateLimitation, feWANPortDefaultVLAN, feWANPortForceDefaultVID, feWANPortVLANPortMode, feWANPortBlockAllUnknown, feWANPortIGMPSnooping, feWANPortAddUnicast, feWANPortAddMulticast, feWANPortArpMirroring, 
		feLAN1Port,
		feLAN1PortAutoNegotiation, feLAN1PortSpeedMode, feLAN1PortLinkStatus, feLAN1PortFlowControl, feLAN1PortIEEEQoSPriority, feLAN1PortIPQoSPriority, feLAN1PortFramePriorityOverwrite, feLAN1PortQueuePriorityOverwrite, feLAN1PortQueuePriority, feLAN1PortQoSPortMapRule, feLAN1PortVIDNRLEnable, feLAN1PortMap2PIRL, feLAN1PortDeletePortMap2PIRL, feLAN1PortEgressRateLimitation, feLAN1PortIngressRateLimitation, feLAN1PortDefaultVLAN, feLAN1PortForceDefaultVID, feLAN1PortVLANPortMode, feLAN1PortBlockAllUnknown, feLAN1PortIGMPSnooping, feLAN1PortAddUnicast, feLAN1PortAddMulticast, feLAN1PortArpMirroring, 
		feLAN2Port,
		feLAN2PortAutoNegotiation, feLAN2PortSpeedMode, feLAN2PortLinkStatus, feLAN2PortFlowControl, feLAN2PortIEEEQoSPriority, feLAN2PortIPQoSPriority, feLAN2PortFramePriorityOverwrite, feLAN2PortQueuePriorityOverwrite, feLAN2PortQueuePriority, feLAN2PortQoSPortMapRule, feLAN2PortVIDNRLEnable, feLAN2PortMap2PIRL, feLAN2PortDeletePortMap2PIRL, feLAN2PortEgressRateLimitation, feLAN2PortIngressRateLimitation, feLAN2PortDefaultVLAN, feLAN2PortForceDefaultVID, feLAN2PortVLANPortMode, feLAN2PortBlockAllUnknown, feLAN2PortIGMPSnooping, feLAN2PortAddUnicast, feLAN2PortAddMulticast, feLAN2PortArpMirroring, 
		feLAN3Port,
		feLAN3PortAutoNegotiation, feLAN3PortSpeedMode, feLAN3PortLinkStatus, feLAN3PortFlowControl, feLAN3PortIEEEQoSPriority, feLAN3PortIPQoSPriority, feLAN3PortFramePriorityOverwrite, feLAN3PortQueuePriorityOverwrite, feLAN3PortQueuePriority, feLAN3PortQoSPortMapRule, feLAN3PortVIDNRLEnable, feLAN3PortMap2PIRL, feLAN3PortDeletePortMap2PIRL, feLAN3PortEgressRateLimitation, feLAN3PortIngressRateLimitation, feLAN3PortDefaultVLAN, feLAN3PortForceDefaultVID, feLAN3PortVLANPortMode, feLAN3PortBlockAllUnknown, feLAN3PortIGMPSnooping, feLAN3PortAddUnicast, feLAN3PortAddMulticast, feLAN3PortArpMirroring, 
		feLAN4Port,
		feLAN4PortAutoNegotiation, feLAN4PortSpeedMode, feLAN4PortLinkStatus, feLAN4PortFlowControl, feLAN4PortIEEEQoSPriority, feLAN4PortIPQoSPriority, feLAN4PortFramePriorityOverwrite, feLAN4PortQueuePriorityOverwrite, feLAN4PortQueuePriority, feLAN4PortQoSPortMapRule, feLAN4PortVIDNRLEnable, feLAN4PortMap2PIRL, feLAN4PortDeletePortMap2PIRL, feLAN4PortEgressRateLimitation, feLAN4PortIngressRateLimitation, feLAN4PortDefaultVLAN, feLAN4PortForceDefaultVID, feLAN4PortVLANPortMode, feLAN4PortBlockAllUnknown, feLAN4PortIGMPSnooping, feLAN4PortAddUnicast, feLAN4PortAddMulticast, feLAN4PortArpMirroring 
	}
    STATUS current
    DESCRIPTION
        "The objects are related to the DKTCOMEGA Fast Ethernet module, MIB rev 02_00."
    ::= { feMIB 4 }


END



