
AC-CONTROL-MIB DEFINITIONS ::= BEGIN


    IMPORTS
       

        OBJECT-TYPE, 
        MODULE-IDENTITY                             FROM SNMPv2-SMI
        TAddress, 
        DisplayString, 
        DateAndTime, TEXTUAL-CONVENTION, 
		RowPointer									FROM SNMPv2-TC
        IpAddress                                   FROM RFC1155-SMI
        Unsigned32,
		Integer32,
        enterprises                                 FROM SNMPv2-SMI
	RowStatus      				    FROM SNMPv2-TC

		SnmpAdminString								FROM SNMP-FRAMEWORK-MIB
		audioCodes,       
        acRegistrations,
        acGeneric, 
        acProducts,acBoardMibs						FROM AUDIOCODES-TYPES-MIB;

       
acControl  MODULE-IDENTITY       
    LAST-UPDATED "201301141127Z"          --Monday, January 14 2013
    ORGANIZATION "AudioCodes Ltd"
    CONTACT-INFO
    "Postal: Support
	     AudioCodes LTD
             1 Hayarden Street
             Airport City 
	     Lod, ISRAEL 70151
     Tel:    972-3-9764000
     Fax:    972-3-9764040
     Email:  support@audiocodes.com
     Web:    www.audiocodes.com"		

    DESCRIPTION       
    ""



    ::= {acBoardMibs 5}  








     acControlConfiguration OBJECT IDENTIFIER ::= {acControl 1}


     acControlCommonConfig OBJECT IDENTIFIER ::= {acControlConfiguration 1}


     acCPLink OBJECT IDENTIFIER ::= {acControlCommonConfig 1}


     acCPKeepAlive OBJECT IDENTIFIER ::= {acCPLink 1}


     acCPKeepAliveEnabled OBJECT-TYPE
       SYNTAX Integer32 (-2147483647..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Enables a proprietary keep-alive mechanism, in which a serviceChange
is send with UNDEFINED as the termination ID and restart
method.
 0 = disable
>0 = enable.
Access: Instant.
AC INI-Param: KEEPALIVEENABLED"
       ::= {acCPKeepAlive 1}



     acCPKeepAliveInterval OBJECT-TYPE
       SYNTAX Unsigned32 (1..300)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "This parameter is used to define the interval in seconds of
a KeepAlive message.
Access: Instant.
AC INI-Param: KEEPALIVEINTERVAL"
       ::= {acCPKeepAlive 2}



     acCPTransport OBJECT IDENTIFIER ::= {acCPLink 2}


     acCPTransportType OBJECT-TYPE
       SYNTAX INTEGER {
                  acCPTransport-UDP-IP(0)
,
                  acCPTransport-TCP-IP(1)
,
                  acCPTransport-SCTP-IP(2)

                  }
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Defines the transport type for the control protocol: 

0 = UDP
1 = TCP
2 = SCTP.
Access: Offline.
AC INI-Param: CPTRANSPORTTYPE "
       ::= {acCPTransport 1}



     acCPTransportRetransmitionTimeOut OBJECT-TYPE
       SYNTAX Integer32 (-2147483647..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Controls protocols retransmission timeout. Sets the initial
time (in msec) for the first retransmission. The retransmission
intervals thereafter increase exponentially.
Access: Instant.
AC INI-Param: MGCPRETRANSMISSIONTIMEOUT"
       ::= {acCPTransport 2}



     acCPTransportControlDiffServ OBJECT-TYPE
       SYNTAX Unsigned32 (0..63)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the value of the field 'DiffServ' in the IP header for
control traffic.

Range: 0 to 63.
Access: Offline.
AC INI-Param: CONTROLDIFFSERV"
       ::= {acCPTransport 3}



     acCPTransaction OBJECT IDENTIFIER ::= {acCPLink 3}


     acCPTransactionIDRange OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the range for the transaction ID. 

Default = 999997999.
Access: Instant.
AC INI-Param: TRANSACTIONIDRANGE"
       ::= {acCPTransaction 1}



     acCPTransactionIDBase OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the minimum number for the transaction ID. 

Default = 2000.
Access: Instant.
AC INI-Param: TRANSACTIONIDBASE"
       ::= {acCPTransaction 2}



     acCPTransactionRandomizeID OBJECT-TYPE
       SYNTAX INTEGER {
                  disable(0)
,
                  enable(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines if the transactions produced by the board start with
a fixed or random number. 

1 = Randomize On
Refer also to the parameters defining Transaction Id Range
and Transaction Id Base.
Access: Offline.
AC INI-Param: RANDOMIZETRANSACTIONID"
       ::= {acCPTransaction 3}



     acCPTransactionCommunicationLayerTimeout OBJECT-TYPE
       SYNTAX Unsigned32 (0..999)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Assumed delay of the communication layer. It is used in retransmission.
This parameter defines the maximal time to wait
for a response before declaring a disconnection (in seconds).
Access: Instant.
AC INI-Param: MGCPCOMMUNICATIONLAYERTIMEOUT"
       ::= {acCPTransaction 4}



     acCPDigitCollect OBJECT IDENTIFIER ::= {acControlCommonConfig 2}


     acCPDigitCollectUseEndOfDTMF OBJECT-TYPE
       SYNTAX Integer32 (-2147483647..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines if the detection of DTMF events is notified at the end
of DTMF or at the start of DTMF.

0 = at start of DTMF
1 = at the end of DTMF.
Access: Instant.
AC INI-Param: MGCPDTMFDETECTIONPOINT"
       ::= {acCPDigitCollect 1}



     acCPDigitCollectDTMFLength OBJECT-TYPE
       SYNTAX Integer32 (-2147483647..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the time to play DTMF (in msec).

Range: 0 to 65535.
Access: Instant.
AC INI-Param: DTMFDIGITLENGTH"
       ::= {acCPDigitCollect 2}



     acCPDigitCollectDTMFInterInterval OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the time between DTMFs played (in msec).

Range: 0 to 65535.
Access: Instant.
AC INI-Param: DTMFINTERDIGITINTERVAL"
       ::= {acCPDigitCollect 3}



     acCPDigitCollectMapTimeOutTimer OBJECT-TYPE
       SYNTAX Integer32 (-1..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the timeout value (T symbol) in a digit map, in increments
of 10. For MEGACO, it's the start timer. For the others,
it's the end timer.

When the value is -1, it means the hardcoded value (16000).
Access: Instant.
AC INI-Param: DIGITMAPTIMEOUTTIMER"
       ::= {acCPDigitCollect 4}



     acCPDigitCollectMapShortTimer OBJECT-TYPE
       SYNTAX Integer32 (-1..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the short timer (S Symbol) value in millisecond, in
a digit map.This timer is typically activated when the repetition
symbol '.' exists.

When the value is -1, it means the hardcoded value (3000).
Access: Instant.
AC INI-Param: cpDIGITMAPSHORTTIMER"
       ::= {acCPDigitCollect 5}



     acCPDigitCollectMapLongTimer OBJECT-TYPE
       SYNTAX Integer32 (-1..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the inter-digit long timer (L Symbol) value in millisecond,
in a digit map.This timer is typically activated between
collected digit when the end of the pattern is not reached
yet.

When the value is -1, it means the hardcoded value (16000).
Access: Instant.
AC INI-Param: cpDIGITMAPLONGTIMER"
       ::= {acCPDigitCollect 6}



     acCPDigitMap OBJECT IDENTIFIER ::= {acControlCommonConfig 3}


     acCPDigitMapDefaultName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..30))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Name of the provisioned digit map.

Range: String[30].
Access: Offline.
AC INI-Param: DIGITMAPNAME"
       ::= {acCPDigitMap 1}



     acCPDigitMapPatterns OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..500))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The digit map patterns separated by a vertical bar (|), as defined
in the MEGACO RFC. 

Range = String[500].
Access: Offline.
AC INI-Param: DIGITMAPPING"
       ::= {acCPDigitMap 2}



     acCPDigitMapDialedStringPrefix OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..8))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines a prefix to add to the dialed string.

Range = String[8].
Access: Instant.
AC INI-Param: DialedStringPrefix"
       ::= {acCPDigitMap 3}



     acCPNaming OBJECT IDENTIFIER ::= {acControlCommonConfig 4}


     acCPNamingGateWay OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..63))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the media gateway's identification name.

MGCP: Gateway's identification name towards the MGCP Call Agent.
If undefined, the gateway name holds the IP address of
the device.
Range: String[63].
Access: Offline.
AC INI-Param: GATEWAYNAME"
       ::= {acCPNaming 1}



     acCPNamingEndPoint OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..19))
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "MGCP: Gateway's endpoint name. This is a prefix used to identify
the endpoint, i.e., 'ACgw' in the following example: 
'ACgw5@acl.com'. 

MEGACO: Prefix of the endpoint part of the termination name

Range: String[19] 

Default: 
MGCP: 'Acgw'
MEGACO: 'line' for analog board and '/c' for trunking boards.
Access: Offline.
AC INI-Param: ENDPOINTNAME"
       ::= {acCPNaming 2}



     acCPNamingTrunk OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..19))
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "(MGCP) This parameter generates (together with the parameter
defining the Endpoint Prefix) a local endpoint name on trunk-enabled
media gateways.

(MEGACO) Prefix of the trunk part of the termination name.

Range: String[19]

Default:
MGCP = ' ' (empty string)
MEGACO = ' ' for analog boards and 's' for trunking boards.
Access: Offline.
AC INI-Param: TRUNKNAME"
       ::= {acCPNaming 3}



     acCPNamingEndpointPrefix OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..19))
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "(MGCP) This parameter generates (together with parameter Trunk
Name) a local endpoint name on trunk-enabled media gateways.

Range: String[19].
Access: Offline.
AC INI-Param: ENDPOINTPREFIX"
       ::= {acCPNaming 4}



     acCPNamingCallAgentDomain OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..63))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines a domain name to be used to connect with the Call Agent.
The parameter takes precedence over the Call Agent IP and
the provisioned Call Agent parameters.

Range = String[63]
Deprecated in MEGACO.
Access: Offline.
AC INI-Param: CALLAGENTDOMAINNAME"
       ::= {acCPNaming 5}



     acCPNamingCoderTblFileName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..47))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "This parameter defines the name of an external coders table.
In this table, the user can decide which coders will be used
in the system. The original file is a text file, and it is
converted by DCONVERT to a bynary file.
Access: Offline.
AC INI-Param: CODERTBLFILENAME"
       ::= {acCPNaming 6}



     acCPNamingSessionOwner OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..31))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the owner/creator of the session
Range = String[31].
Access: Instant.
AC INI-Param: CPSDPSESSIONOWNER"
       ::= {acCPNaming 7}



     acCPConference OBJECT IDENTIFIER ::= {acControlCommonConfig 5}


     acCPConferenceMaxUsers OBJECT-TYPE
       SYNTAX Unsigned32 (3..64)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the maximal number of users to reserve for a new conference.
The actual conference size can be more than this, but
never less.

Range: 3 to 64.
Access: Instant.
AC INI-Param: CONFERENCEMAXUSERS"
       ::= {acCPConference 1}



     acCPConferenceMaxSimultaneousSpeakers OBJECT-TYPE
       SYNTAX Unsigned32 (1..3)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the maximum number of users that can speak simultaneously
in a conference.

Range: 1 to 3.
Access: Instant.
AC INI-Param: CONFERENCEMAXSIMULTANEOUSSPEAKERS"
       ::= {acCPConference 2}



     acCPConferenceSignalGenerationEnable OBJECT-TYPE
       SYNTAX INTEGER {
                  no(0)
,
                  yes(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Generates a beep when a participant enters or exits the conference.

0 = Do not generate
1 = Generate.
Access: Instant.
AC INI-Param: CONFERENCESIGNALGENERATIONENABLE"
       ::= {acCPConference 3}



     acCPMedia OBJECT IDENTIFIER ::= {acControlCommonConfig 6}


     acCPMediaRTCPInterval OBJECT-TYPE
       SYNTAX Integer32 (-2147483647..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the time interval between the adjacent RTCP reports
(in msec).

Range: 0 to 65535.
Access: Instant.
AC INI-Param: RTCPINTERVAL"
       ::= {acCPMedia 1}



     acCPMediaDefaultCoder OBJECT-TYPE
       SYNTAX INTEGER {
                  non-Initialized(0)
,
                  g711Mulaw(1)
,
                  g711Alaw-64(2)
,
                  g726-16(3)
,
                  g726-24(4)
,
                  g726-32(5)
,
                  g726-40(6)
,
                  g727-16(7)
,
                  g727-24-16(8)
,
                  g727-24(9)
,
                  g727-32-16(10)
,
                  g727-32-24(11)
,
                  g727-32(12)
,
                  g727-40-16(13)
,
                  g727-40-24(14)
,
                  g727-40-32(15)
,
                  g723High-(16)
,
                  g723Low(17)
,
                  g729(18)
,
                  g728(19)
,
                  gSM(20)
,
                  transparent(21)
,
                  netCoder-4-8(22)
,
                  netCoder-5-6(23)
,
                  netCoder-6-4(24)
,
                  netCoder-7-2(25)
,
                  netCoder-8(26)
,
                  netCoder-8-8(27)
,
                  netCoder-9-6(28)
,
                  eVRC0(29)
,
                  eVRC-TFO(30)
,
                  eVRC-TTY(31)
,
                  qCELP-8(32)
,
                  qCELP-8-TFO(33)
,
                  qCELP-13(34)
,
                  qCELP-13-TFO(35)
,
                  g729E(36)
,
                  aMR-4-75(37)
,
                  aMR-5-15(38)
,
                  aMR-5-9(39)
,
                  aMR-6-7(40)
,
                  aMR-7-4(41)
,
                  aMR-7-95(42)
,
                  aMR-10-2(43)
,
                  aMR-12-2(44)
,
                  gSM-EFR(45)
,
                  iLBC13(46)
,
                  iLBC15(47)
,
                  bV16(48)
,
                  eVRC(49)
,
                  telepone-Event-RFC2833(50)
,
                  redundency-RTP-RFC2198(51)
,
                  mODEM-Relay(52)
,
                  comfortNoise-Coder(53)
,
                  iMAGET38(54)
,
                  nOOP(55)
,
                  g722(56)
,
                  eVRCB(57)
,
                  eVRC1(58)
,
                  eVRCB1(59)
,
                  aMR-WB(60)
,
                  eVRCB0(61)
,
                  g7291(62)
,
                  eg711A(63)
,
                  eg711U(64)
,
                  g729B(65)
,
                  h263(67)
,
                  h263-1998(68)
,
                  mP4V-ES(69)
,
                  h264(70)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "This parameter can be used to set a default coder for channel
opening. For the legal coder names, refer to the product's
User Manual.

Default = cpDPT_G711Mulaw_Coder.
Access: Instant.
AC INI-Param: MGCPDEFAULTCODER"
       ::= {acCPMedia 2}



     acCPMediaPacketizationPeriod OBJECT-TYPE
       SYNTAX Unsigned32 (5..120)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the default packetization period (Frame Size).

Default = 20 msec (for G.723 30)

Range: 5 to 80.
Access: Instant.
AC INI-Param: DEFAULTPACKETIZATIONPERIOD"
       ::= {acCPMedia 3}



     acCPMediaRecordCoder OBJECT-TYPE
       SYNTAX INTEGER {
                  g711Mulaw(1)
,
                  g711Alaw-64(2)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Determines the coder used for recording to a file.
Access: Instant.
AC INI-Param: cpRecordCoder"
       ::= {acCPMedia 4}



     acCPMediaPlayCoder OBJECT-TYPE
       SYNTAX INTEGER {
                  g711Mulaw(1)
,
                  g711Alaw-64(2)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Determines the coder type to be used when playing a file of
type .raw.
Access: Instant.
AC INI-Param: cpPlayCoder"
       ::= {acCPMedia 5}



     acCPMediaDefaultRealmName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..39))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "By default, the default CP media realm is the first realm appearing
in the CP media realm table.
The parameter enables the user to set any of the realms appearing
in the table as the default realm.
Access: Offline.
AC INI-Param: cpDefaultMediaRealmName"
       ::= {acCPMedia 6}



     acCPMediaDspAllocationMethod OBJECT-TYPE
       SYNTAX INTEGER {
                  disableSingleDSPAllocation(0)
,
                  enableSingleDSPAllocation(1)
,
                  enforceFullDSPAllocation(2) 

                  }
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "determines dsp allocation method in IP to IP call.
If this parameter is set to DISABLE_SINGLE_DSP_ALLOCATION (0)
, then two IP terminations with the same configuration will
not  allocate DSPs at all and two terminations with different
configuration will cause an allocation of 2 DSPs.

If this parameteris set to ENABLE_SINGLE_DSP_ALLOCATION (1),
 then two IP terminations with the same configuration will
not allocate   DSPs at all, transcoding with allocation of
one DSP will be used if possible, and two terminations with
different configuration will cause allocation of 2 DSPs.

If this parameter is set to  ENFORCE_FULL_DSP_ALLOCATION (2)
then two IP terminations with any configuration will cause
allocation of two DSPs.
Access: Instant.
AC INI-Param: CPMEDIARESOURCEOPTIMIZATION"
       ::= {acCPMedia 7}



     -- ****************************************
     -- acCPMediaRealm table declaration
     -- ****************************************
     acCPMediaRealmTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcCPMediaRealmEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Control Protocol media realm configuration table."
       ::= {acCPMedia 21}



     -- ****************************************
     -- acCPMediaRealm table entry
     -- ****************************************
     acCPMediaRealmEntry OBJECT-TYPE
       SYNTAX AcCPMediaRealmEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acCPMediaRealmIndex}
       ::= {acCPMediaRealmTable 1}



     -- ****************************************
     -- acCPMediaRealm TABLE
     -- ****************************************
     AcCPMediaRealmEntry ::= SEQUENCE {
       acCPMediaRealmIndex                             Unsigned32,
       acCPMediaRealmRowStatus                         RowStatus,
       acCPMediaRealmAction                            INTEGER,
       acCPMediaRealmActionRes                         INTEGER,
       acCPMediaRealmName                              SnmpAdminString,
       acCPMediaRealmIPv4If                            RowPointer,
       acCPMediaRealmIPv6If                            RowPointer,
       acCPMediaRealmPortRangeStart                    Integer32,
       acCPMediaRealmMediaSessionLeg                   Integer32,
       acCPMediaRealmPortRangeEnd                      Integer32,
       acCPMediaRealmTransRateRatio                    Unsigned32,
       acCPMediaRealmIsDefault                         INTEGER
     }



     acCPMediaRealmIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..15)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Index Field for line. Internal parameter.
AC INI-Param: CpMediaRealm_Index"
       ::= {acCPMediaRealmEntry 1}



     acCPMediaRealmRowStatus OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "ROWSTATUS field for line. Internal parameter.
AC INI-Param: N/A"
       ::= {acCPMediaRealmEntry 2}



     acCPMediaRealmAction OBJECT-TYPE
       SYNTAX INTEGER {
                  none(0)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS. Internal parameter.
AC INI-Param: N/A"
       ::= {acCPMediaRealmEntry 3}



     acCPMediaRealmActionRes OBJECT-TYPE
       SYNTAX INTEGER {
                  succeeded(0)

                  }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS RESULT. Internal parameter.
AC INI-Param: N/A"
       ::= {acCPMediaRealmEntry 4}



     acCPMediaRealmName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..38))
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "A string representing the name of the media realm.
Access: Offline.
AC INI-Param: CpMediaRealm_MediaRealmName"
       ::= {acCPMediaRealmEntry 5}



     acCPMediaRealmIPv4If OBJECT-TYPE
       SYNTAX RowPointer
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Select the OID of the IPv4 interface name corresponding to the
one appearing in the interface table.
The OID should be 1.3.6.1.4.1.5003.9.10.10.1.3.1.30.22.1.11.
acSysInterfaceIndex
Note: when ignore a default value will be SET: 0.0.
Access: Offline.
AC INI-Param: CpMediaRealm_IPv4IF"
       ::= {acCPMediaRealmEntry 6}



     acCPMediaRealmIPv6If OBJECT-TYPE
       SYNTAX RowPointer
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Select the OID of the IPv6interface name corresponding to the
one appearing in the interface table.
The OID should be 1.3.6.1.4.1.5003.9.10.10.1.3.1.30.22.1.11.
acSysInterfaceIndex
Note: when ignore a default value will be SET: 0.0.
Access: Offline.
AC INI-Param: CpMediaRealm_IPv6IF"
       ::= {acCPMediaRealmEntry 7}



     acCPMediaRealmPortRangeStart OBJECT-TYPE
       SYNTAX Integer32 (-1..60000)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The starting port for the range of media ports.
Access: Offline.
AC INI-Param: CpMediaRealm_PortRangeStart"
       ::= {acCPMediaRealmEntry 8}



     acCPMediaRealmMediaSessionLeg OBJECT-TYPE
       SYNTAX Integer32 (-1..6000)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           " The number of media sessions associated with the range of ports.
Access: Offline.
AC INI-Param: CpMediaRealm_MediaSessionLeg"
       ::= {acCPMediaRealmEntry 9}



     acCPMediaRealmPortRangeEnd OBJECT-TYPE
       SYNTAX Integer32 (-1..60000)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The ending port for the range of media ports.
AC INI-Param: CpMediaRealm_PortRangeEnd"
       ::= {acCPMediaRealmEntry 10}



     acCPMediaRealmTransRateRatio OBJECT-TYPE
       SYNTAX Unsigned32 (1..4294967295)
       MAX-ACCESS read-create
       STATUS obsolete
       DESCRIPTION
           "In case of trans-rating the ptime will be multiplied.
Access: Offline.
AC INI-Param: CpMediaRealm_TransRateRatio"
       ::= {acCPMediaRealmEntry 11}



     acCPMediaRealmIsDefault OBJECT-TYPE
       SYNTAX INTEGER {
                  false(0)
,
                  true(1)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Determines whether this is the default media realm or not.
Access: Offline.
AC INI-Param: CpMediaRealm_IsDefault"
       ::= {acCPMediaRealmEntry 12}



     acCPMisc OBJECT IDENTIFIER ::= {acControlCommonConfig 7}


     acCPMiscDialToneDuration OBJECT-TYPE
       SYNTAX Integer32 (-2147483647..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the timeout (in seconds) for the dial tone signal.

Range: 1 to 65535.
Access: Instant.
AC INI-Param: DIALTONEDURATION"
       ::= {acCPMisc 1}



     acCPMiscTrunkIDOffset OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Sets the offset to the trunk numbering. 
e.g., Offset = 2 causes the first trunk number to be 2. 

Note: This parameter was replaced by the parameter 'EP_NUM'.

Range: 0 to 4294967295.
Access: Offline.
AC INI-Param: MEGACOTRUNKIDOFFSET"
       ::= {acCPMisc 2}



     acCPMiscCompatibilityProfile OBJECT-TYPE
       SYNTAX Unsigned32 (0..131071)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "ControlS MGCP/MEGACO functioning for vendor-specific compatibility.
Refer to the product's User's Manual.

Range: Integer > 0

Refer to the product's User's Manual or the enumerator mgTMGCPProfile
for possible values.
Access: Offline.
AC INI-Param: MGCPCOMPATIBILITYPROFILE"
       ::= {acCPMisc 3}



     acCPMiscSDPProfile OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Controls MGCP/MEGACO functioning for SDP negotiation. The parameter
is bitwise.
Every new RFC support should be turned on or off with this
parameter. 
Each bit function is described in the control protocol chapter.
Access: Instant.
AC INI-Param: CPSDPPROFILE"
       ::= {acCPMisc 4}



     acCPVxml OBJECT IDENTIFIER ::= {acControlCommonConfig 8}


     acCPVxmlEnableVXML OBJECT-TYPE
       SYNTAX INTEGER {
                  disable(0)
,
                  enable(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Enables/disables the VXML stack. 

0=Disable
1=Enable.
Access: Offline.
AC INI-Param: EnableVXML"
       ::= {acCPVxml 1}



     acCPQualityOfExperience OBJECT IDENTIFIER ::= {acControlCommonConfig 9}


     acCPQualityOfExperienceConnectionMode OBJECT-TYPE
       SYNTAX INTEGER {
                  vQMServer(0)
,
                  vQMClient(1)
,
                  vQMNone(2)

                  }
       MAX-ACCESS read-write
       STATUS obsolete
       DESCRIPTION
           "Defines whether the module will connect to the VQMS (client)
or receive connection from the server (server).
Access: Instant.
AC INI-Param: QOEConnectionMode"
       ::= {acCPQualityOfExperience 1}



     acCPQualityOfExperienceInformationLevel OBJECT-TYPE
       SYNTAX INTEGER {
                  standard(0)
,
                  enahance(1)
,
                  debug(2)

                  }
       MAX-ACCESS read-write
       STATUS obsolete
       DESCRIPTION
           "Defines the quantity of VQ information sent the the serverl.
Access: Instant.
AC INI-Param: QOEInformationLevel"
       ::= {acCPQualityOfExperience 2}



     acCPQualityOfExperienceUseMosLQ OBJECT-TYPE
       SYNTAX INTEGER {
                  disable(0)
,
                  enable(1)

                  }
       MAX-ACCESS read-write
       STATUS obsolete
       DESCRIPTION
           "If it is enabled the moss_lq will be used by the board to calculate
the moss status instead of the moss_cq'.
Access: Instant.
AC INI-Param: QOEUseMosLQ"
       ::= {acCPQualityOfExperience 3}



     acCPQualityOfExperienceSendBufferSize OBJECT-TYPE
       SYNTAX Unsigned32 (0..4294967295)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the sending buffer size of the socket.
Access: Instant.
AC INI-Param: QOESendBufferSize"
       ::= {acCPQualityOfExperience 4}



     acCPQualityOfExperienceEnableTLS OBJECT-TYPE
       SYNTAX INTEGER {
                  disable(0)
,
                  enable(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines a domain name to be used to connect with the Call Agent.
Access: Offline.
AC INI-Param: QOEEnableTLS"
       ::= {acCPQualityOfExperience 5}



     acCPQualityOfExperienceServerIp OBJECT-TYPE
       SYNTAX IpAddress
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "in case VQM is at client configuration, this parameter defines
the server ip.
Access: Offline.
AC INI-Param: QOEServerIp"
       ::= {acCPQualityOfExperience 6}



     acCPQualityOfExperiencePort OBJECT-TYPE
       SYNTAX Unsigned32 (0..65534)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Quality Of Experience Port.
Access: Instant.
AC INI-Param: QOEPort"
       ::= {acCPQualityOfExperience 7}



     acCPQualityOfExperienceInterfaceName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..64))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "the interface to wait on in case of server (default is the default
control interface).
Access: Offline.
AC INI-Param: QOEInterfaceName"
       ::= {acCPQualityOfExperience 8}



     acCPQualityOfExperienceMOSCalculationAlgorithm OBJECT-TYPE
       SYNTAX INTEGER {
                  conversationalQuality-CQ(0)
,
                  listeningQuality-LQ(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Reporting of MOS-LQ (listening quality) or MOS-CQ (conversational
quality).
Access: Offline.
AC INI-Param: QOEUseMosLQ"
       ::= {acCPQualityOfExperience 9}



     -- ****************************************
     -- acCPQOERules table declaration
     -- ****************************************
     acCPQOERulesTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcCPQOERulesEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       ::= {acCPQualityOfExperience 21}



     -- ****************************************
     -- acCPQOERules table entry
     -- ****************************************
     acCPQOERulesEntry OBJECT-TYPE
       SYNTAX AcCPQOERulesEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acCPQOERulesMediaRealmIndex,acCPQOERulesRuleIndex}
       ::= {acCPQOERulesTable 1}



     -- ****************************************
     -- acCPQOERules TABLE
     -- ****************************************
     AcCPQOERulesEntry ::= SEQUENCE {
       acCPQOERulesMediaRealmIndex                     Unsigned32,
       acCPQOERulesRuleIndex                           Unsigned32,
       acCPQOERulesRowStatus                           RowStatus,
       acCPQOERulesAction                              INTEGER,
       acCPQOERulesActionRes                           INTEGER,
       acCPQOERulesMonitoredParam                      INTEGER,
       acCPQOERulesGreenYellowThreshold                Unsigned32,
       acCPQOERulesGreenYellowHystersis                Unsigned32,
       acCPQOERulesYellowRedThreshold                  Unsigned32,
       acCPQOERulesYellowRedHystersis                  Unsigned32,
       acCPQOERulesProfile                             INTEGER,
       acCPQOERulesGreenYellowOperation                INTEGER,
       acCPQOERulesGreenYellowOperationDetails         Unsigned32,
       acCPQOERulesYellowRedOperation                  INTEGER,
       acCPQOERulesYellowRedOperationDetails           Unsigned32,
       acCPQOERulesDirection                           INTEGER
     }



     acCPQOERulesMediaRealmIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..63)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The Media Realm Name index at acCPMediaRealmTable.
AC INI-Param: QOERules_MediaRealmIndex"
       ::= {acCPQOERulesEntry 1}



     acCPQOERulesRuleIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..9)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Rule Index.
AC INI-Param: QOERules_RuleIndex"
       ::= {acCPQOERulesEntry 2}



     acCPQOERulesRowStatus OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "ROWSTATUS Field for line.
AC INI-Param: QOERules_RowStatus"
       ::= {acCPQOERulesEntry 3}



     acCPQOERulesAction OBJECT-TYPE
       SYNTAX INTEGER {
                  none(0)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS.
AC INI-Param: QOERules_Action"
       ::= {acCPQOERulesEntry 4}



     acCPQOERulesActionRes OBJECT-TYPE
       SYNTAX INTEGER {
                  succeeded(0)

                  }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS RESULT.
AC INI-Param: QOERules_ActionRes"
       ::= {acCPQOERulesEntry 5}



     acCPQOERulesMonitoredParam OBJECT-TYPE
       SYNTAX INTEGER {
                  mos(0)
,
                  delay(1)
,
                  packetLoss(2)
,
                  jitter(3)
,
                  rerl(4)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "MonitoredParam.
Access: Online.
AC INI-Param: QOERules_MonitoredParam"
       ::= {acCPQOERulesEntry 6}



     acCPQOERulesGreenYellowThreshold OBJECT-TYPE
       SYNTAX Unsigned32 (0..4294967295)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "GreenYellowThreshold.
Access: Online.
AC INI-Param: QOERules_GreenYellowThreshold"
       ::= {acCPQOERulesEntry 7}



     acCPQOERulesGreenYellowHystersis OBJECT-TYPE
       SYNTAX Unsigned32 (0..4294967295)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "GreenYellowHystersis.
Access: Online.
AC INI-Param: QOERules_GreenYellowHysteresis"
       ::= {acCPQOERulesEntry 8}



     acCPQOERulesYellowRedThreshold OBJECT-TYPE
       SYNTAX Unsigned32 (0..4294967295)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "YellowRedThreshold.
Access: Online.
AC INI-Param: QOERules_YellowRedThreshold"
       ::= {acCPQOERulesEntry 9}



     acCPQOERulesYellowRedHystersis OBJECT-TYPE
       SYNTAX Unsigned32 (0..4294967295)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "YellowRedHystersis.
Access: Online.
AC INI-Param: QOERules_YellowRedHysteresis"
       ::= {acCPQOERulesEntry 10}



     acCPQOERulesProfile OBJECT-TYPE
       SYNTAX INTEGER {
                  noProfile(0)
,
                  lowSensitivity(1)
,
                  defaultSensitivity(2)
,
                  highSensitivity(3)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Profile.
Access: Online.
AC INI-Param: QOERules_Profile"
       ::= {acCPQOERulesEntry 11}



     acCPQOERulesGreenYellowOperation OBJECT-TYPE
       SYNTAX INTEGER {
                  notify(1)
,
                  activate2198(2)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The operation upon crossing green to yellow threshold.
Access: Online.
AC INI-Param: QOERules_GreenYellowOperation"
       ::= {acCPQOERulesEntry 12}



     acCPQOERulesGreenYellowOperationDetails OBJECT-TYPE
       SYNTAX Unsigned32 (0..255)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The specific details for the operation (relevant to Activate2198
only).
Access: Online.
AC INI-Param: QOERules_GreenYellowOperationDetails"
       ::= {acCPQOERulesEntry 13}



     acCPQOERulesYellowRedOperation OBJECT-TYPE
       SYNTAX INTEGER {
                  notify(1)
,
                  activate2198(2)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The operation upon crossing yellow to red threshold.
Access: Online.
AC INI-Param: QOERules_YellowRedOperation"
       ::= {acCPQOERulesEntry 14}



     acCPQOERulesYellowRedOperationDetails OBJECT-TYPE
       SYNTAX Unsigned32 (0..255)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The specific details for the operation (relevant to Activate2198
only).
Access: Online.
AC INI-Param: QOERules_YellowRedOperationDetails"
       ::= {acCPQOERulesEntry 15}



     acCPQOERulesDirection OBJECT-TYPE
       SYNTAX INTEGER {
                  deviceSide(0)
,
                  remoteSide(1)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Whether the paramter is monitored on the remote or local side.
Access: Online.
AC INI-Param: QOERules_Direction"
       ::= {acCPQOERulesEntry 16}



     acBandwidth OBJECT IDENTIFIER ::= {acControlCommonConfig 10}


     -- ****************************************
     -- acBandwidthManagement table declaration
     -- ****************************************
     acBandwidthManagementTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcBandwidthManagementEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       ::= {acBandwidth 21}



     -- ****************************************
     -- acBandwidthManagement table entry
     -- ****************************************
     acBandwidthManagementEntry OBJECT-TYPE
       SYNTAX AcBandwidthManagementEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acBandwidthManagementMediaRealmIndex,acBandwidthManagementThresholdIndex}
       ::= {acBandwidthManagementTable 1}



     -- ****************************************
     -- acBandwidthManagement TABLE
     -- ****************************************
     AcBandwidthManagementEntry ::= SEQUENCE {
       acBandwidthManagementMediaRealmIndex            Unsigned32,
       acBandwidthManagementThresholdIndex             Unsigned32,
       acBandwidthManagementRowStatus                  RowStatus,
       acBandwidthManagementAction                     INTEGER,
       acBandwidthManagementActionRes                  INTEGER,
       acBandwidthManagementRuleAction                 INTEGER,
       acBandwidthManagementThreshold                  Unsigned32,
       acBandwidthManagementHysteresis                 Unsigned32
     }



     acBandwidthManagementMediaRealmIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..63)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The Media Realm Name index at acCPMediaRealmTable.
AC INI-Param: BWManagement_MediaRealmIndex"
       ::= {acBandwidthManagementEntry 1}



     acBandwidthManagementThresholdIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..1)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Rule Index.
AC INI-Param: BWManagement_ThresholdIndex"
       ::= {acBandwidthManagementEntry 2}



     acBandwidthManagementRowStatus OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "ROWSTATUS Field for line.
Access: Offline.
AC INI-Param: BWManagement_RowStatus"
       ::= {acBandwidthManagementEntry 3}



     acBandwidthManagementAction OBJECT-TYPE
       SYNTAX INTEGER {
                  none(0)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS.
Access: Offline.
AC INI-Param: BWManagement_Action"
       ::= {acBandwidthManagementEntry 4}



     acBandwidthManagementActionRes OBJECT-TYPE
       SYNTAX INTEGER {
                  succeeded(0)

                  }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS RESULT.
AC INI-Param: BWManagement_ActionRes"
       ::= {acBandwidthManagementEntry 5}



     acBandwidthManagementRuleAction OBJECT-TYPE
       SYNTAX INTEGER {
                  reportOnly(0)
,
                  noMoreCalls(1)
,
                  lbrCalls(2)
,
                  ptimeMul2(3)
,
                  ptimeMul4(4)
,
                  noAction(5)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Rule Action.
Access: Offline.
AC INI-Param: BWManagement_RuleAction"
       ::= {acBandwidthManagementEntry 6}



     acBandwidthManagementThreshold OBJECT-TYPE
       SYNTAX Unsigned32 (0..4294967295)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Threshold.
Access: Offline.
AC INI-Param: BWManagement_Threshold"
       ::= {acBandwidthManagementEntry 7}



     acBandwidthManagementHysteresis OBJECT-TYPE
       SYNTAX Unsigned32 (0..4294967295)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Hysteresis.
Access: Offline.
AC INI-Param: BWManagement_Hysteresis"
       ::= {acBandwidthManagementEntry 8}



     acProvisionedCallAgent OBJECT IDENTIFIER ::= {acControlConfiguration 2}


     -- ****************************************
     -- acProvisionedCallAgent table declaration
     -- ****************************************
     acProvisionedCallAgentTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcProvisionedCallAgentEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Magaco Call agents Table.;The table defines the IP and port of each call agent.;The Row Status in this table is currently degenerated. It is permanently set to 'active(1)'. Also, changing other values in the table can be done freely (no need to set the Row Status to other values)."
       ::= {acProvisionedCallAgent 1}



     -- ****************************************
     -- acProvisionedCallAgent table entry
     -- ****************************************
     acProvisionedCallAgentEntry OBJECT-TYPE
       SYNTAX AcProvisionedCallAgentEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acProvisionedCallAgentIndex}
       ::= {acProvisionedCallAgentTable 1}



     -- ****************************************
     -- acProvisionedCallAgent TABLE
     -- ****************************************
     AcProvisionedCallAgentEntry ::= SEQUENCE {
       acProvisionedCallAgentRowStatus                 Unsigned32,
       acProvisionedCallAgentAction                    Unsigned32,
       acProvisionedCallAgentActionResult              Unsigned32,
       acProvisionedCallAgentIndex                     Unsigned32,
       acProvisionedCallAgentIp                        SnmpAdminString,
       acProvisionedCallAgentPort                      Unsigned32
     }



     acProvisionedCallAgentRowStatus OBJECT-TYPE
       SYNTAX Unsigned32 (1..1)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Provisioned call agent table row-status.
AC INI-Param: N/A"
       ::= {acProvisionedCallAgentEntry 1}



     acProvisionedCallAgentAction OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Provisioned call agent table action.
AC INI-Param: N/A"
       ::= {acProvisionedCallAgentEntry 2}



     acProvisionedCallAgentActionResult OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Provisioned call agent table result.
AC INI-Param: N/A"
       ::= {acProvisionedCallAgentEntry 3}



     acProvisionedCallAgentIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..9)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Megaco Call Agent Id.
AC INI-Param: N/A"
       ::= {acProvisionedCallAgentEntry 4}



     acProvisionedCallAgentIp OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..20))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Use this parameter to define a list of up to 10 legal IP addresses
separated by ',' or ';'  for the ServiceChange command.
The gateway starts connecting with the first and in case
of failure, attempts the others.
Deprecated in MEGACO.
Access: Offline.
AC INI-Param: PROVISIONEDCALLAGENTS"
       ::= {acProvisionedCallAgentEntry 5}



     acProvisionedCallAgentPort OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Use this parameter to define a list of up to 10 Call Agent UDP
ports separated by , or ; for each Call Agent defined
by the parameter used to specify the Allowed Call Agent Address.
Deprecated in MEGACO.
Access: Offline.
AC INI-Param: PROVISIONEDCALLAGENTSPORTS"
       ::= {acProvisionedCallAgentEntry 6}



     -- ****************************************
     -- acCallManagerGroups table declaration
     -- ****************************************
     acCallManagerGroupsTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcCallManagerGroupsEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "List the trunks in the group. Comma and range can be used"
       ::= {acProvisionedCallAgent 2}



     -- ****************************************
     -- acCallManagerGroups table entry
     -- ****************************************
     acCallManagerGroupsEntry OBJECT-TYPE
       SYNTAX AcCallManagerGroupsEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acCallManagerGroupsIndex}
       ::= {acCallManagerGroupsTable 1}



     -- ****************************************
     -- acCallManagerGroups TABLE
     -- ****************************************
     AcCallManagerGroupsEntry ::= SEQUENCE {
       acCallManagerGroupsIndex                        Unsigned32,
       acCallManagerGroupsRowStatus                    RowStatus,
       acCallManagerGroupsAction                       Unsigned32,
       acCallManagerGroupsActionResult                 Unsigned32,
       acCallManagerGroupsList                         SnmpAdminString,
       acCallManagerGroupsMGCType                      INTEGER,
       acCallManagerGroupsPrimaryMGCIndx               Unsigned32,
       acCallManagerGroupsSecondaryMGCIndx             Unsigned32
     }



     acCallManagerGroupsIndex OBJECT-TYPE
       SYNTAX Unsigned32 (1..10)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Call Manager Groups index.
AC INI-Param: CPCallManagerGroups_Index"
       ::= {acCallManagerGroupsEntry 1}



     acCallManagerGroupsRowStatus OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Call Manager Groups table row-status.
AC INI-Param: CPCallManagerGroups_RowStatus"
       ::= {acCallManagerGroupsEntry 2}



     acCallManagerGroupsAction OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Call Manager Groups table action.
AC INI-Param: CPCallManagerGroups_Action"
       ::= {acCallManagerGroupsEntry 3}



     acCallManagerGroupsActionResult OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Call Manager Groups table result.
AC INI-Param: CPCallManagerGroups_ActionRes"
       ::= {acCallManagerGroupsEntry 4}



     acCallManagerGroupsList OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..63))
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "List the trunks in the group. Comma and range can be used.
Access: Offline.
AC INI-Param: CPCallManagerGroups_GroupMembersList"
       ::= {acCallManagerGroupsEntry 5}



     acCallManagerGroupsMGCType OBJECT-TYPE
       SYNTAX INTEGER {
                  ip4(0)
,
                  dns(1)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "0- IP4 CA, 1- DNS (MGCPCallAgentDomainName).
Access: Offline.
AC INI-Param: CPCallManagerGroups_MGCType"
       ::= {acCallManagerGroupsEntry 6}



     acCallManagerGroupsPrimaryMGCIndx OBJECT-TYPE
       SYNTAX Unsigned32 (0..10)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Index of primary MGC in the call agents list. The value 0 means
there is no IP.
Access: Offline.
AC INI-Param: CPCallManagerGroups_PrimaryMGCIndx"
       ::= {acCallManagerGroupsEntry 7}



     acCallManagerGroupsSecondaryMGCIndx OBJECT-TYPE
       SYNTAX Unsigned32 (0..10)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Index of secondary MGC in the call agents list. If none - set
to 10.
Access: Offline.
AC INI-Param: CPCallManagerGroups_SecondaryMGCIndx"
       ::= {acCallManagerGroupsEntry 8}



     acMGCPConfig OBJECT IDENTIFIER ::= {acControlConfiguration 3}


     acMGCallAgent OBJECT IDENTIFIER ::= {acMGCPConfig 1}


     acMGCallAgentIP OBJECT-TYPE
       SYNTAX IpAddress
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The Call Agent IP address, in dotted notation, to be used for
the initial Restart in Progress (RSIP) message. Set to 0.0.0.0
to avoid sending RSIP. This parameter overrides the BootP
server's Call Agent IP address, if provided.
Range:  Legal IP address.
Access: Offline.
AC INI-Param: CALLAGENTIP"
       ::= {acMGCallAgent 1}



     acMGCallAgentPort OBJECT-TYPE
       SYNTAX Unsigned32 (0..65534)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the Call Agent port number. Defaults to the MGCP default
port number of 2427.

Range: 0 to 65534.
Access: Offline.
AC INI-Param: CALLAGENTPORT"
       ::= {acMGCallAgent 2}



     acMGCallAgentRedundantIP OBJECT-TYPE
       SYNTAX IpAddress
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the redundant Call Agent IP address to be used for the
initial Restart in Progress message (RSIP). Set to 0.0.0.0
to avoid sending RSIP.
Range = IP address in dotted format notation.
Access: Offline.
AC INI-Param: REDUNDANTAGENTIP"
       ::= {acMGCallAgent 3}



     acMGCallAgentRedundantPort OBJECT-TYPE
       SYNTAX Unsigned32 (0..65534)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the redundant Call Agent port number. Defaults to the
MGCP default port number of 2427.
Access: Offline.
AC INI-Param: REDUNDANTAGENTPORT"
       ::= {acMGCallAgent 4}



     acMGCallAgentRedundantDomainName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..64))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the redundant MGCP Call Agent domain name. 

Range = String[63]
Default = ' ' (empty string).
Access: Instant.
AC INI-Param: REDUNDANTCALLAGENTDOMAINNAME"
       ::= {acMGCallAgent 5}



     -- ****************************************
     -- acMGCallAgentRedundantIP table declaration
     -- ****************************************
     acMGCallAgentRedundantIPTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcMGCallAgentRedundantIPEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Defines the redundant Call Agent IP address to be used for the initial Restart in Progress message (RSIP).{@} Set to 0.0.0.0 to avoid sending RSIP.{@}Range = IP address in dotted format notation"
       ::= {acMGCallAgent 21}



     -- ****************************************
     -- acMGCallAgentRedundantIP table entry
     -- ****************************************
     acMGCallAgentRedundantIPEntry OBJECT-TYPE
       SYNTAX AcMGCallAgentRedundantIPEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acMGCallAgentRedundantIPIndex}
       ::= {acMGCallAgentRedundantIPTable 1}



     -- ****************************************
     -- acMGCallAgentRedundantIP TABLE
     -- ****************************************
     AcMGCallAgentRedundantIPEntry ::= SEQUENCE {
       acMGCallAgentRedundantIPIndex                   Unsigned32,
       acMGCallAgentRedundantIPAddress                 IpAddress
     }



     acMGCallAgentRedundantIPIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..2)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Call Agent number starting at 0.
AC INI-Param: N/A"
       ::= {acMGCallAgentRedundantIPEntry 1}



     acMGCallAgentRedundantIPAddress OBJECT-TYPE
       SYNTAX IpAddress
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "
Access: Offline.
AC INI-Param: RedundantAgentIP"
       ::= {acMGCallAgentRedundantIPEntry 2}



     -- ****************************************
     -- acMGCallAgentRedundantPort table declaration
     -- ****************************************
     acMGCallAgentRedundantPortTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcMGCallAgentRedundantPortEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Defines the redundant Call Agent port number.{@}Defaults to the MGCP default port number of 2427."
       ::= {acMGCallAgent 22}



     -- ****************************************
     -- acMGCallAgentRedundantPort table entry
     -- ****************************************
     acMGCallAgentRedundantPortEntry OBJECT-TYPE
       SYNTAX AcMGCallAgentRedundantPortEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acMGCallAgentRedundantPortIndex}
       ::= {acMGCallAgentRedundantPortTable 1}



     -- ****************************************
     -- acMGCallAgentRedundantPort TABLE
     -- ****************************************
     AcMGCallAgentRedundantPortEntry ::= SEQUENCE {
       acMGCallAgentRedundantPortIndex                 Unsigned32,
       acMGCallAgentRedundantPortNumber                Unsigned32
     }



     acMGCallAgentRedundantPortIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..2)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Call Agent number starting at 0.
AC INI-Param: N/A"
       ::= {acMGCallAgentRedundantPortEntry 1}



     acMGCallAgentRedundantPortNumber OBJECT-TYPE
       SYNTAX Unsigned32 (0..65534)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "
Access: Offline.
AC INI-Param: RedundantAgentPort"
       ::= {acMGCallAgentRedundantPortEntry 2}



     acMGCommunication OBJECT IDENTIFIER ::= {acMGCPConfig 2}


     acMGCommunicationConnectionIDBase OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the lowest number for the Connection ID values assigned
by the media gateway.
Access: Offline.
AC INI-Param: CONNECTIONIDBASE"
       ::= {acMGCommunication 1}



     acMGCommunicationConnectionIDRange OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the range for the Connection ID values assigned by the
gateway.
Default = 999999999.
Access: Offline.
AC INI-Param: CONNECTIONIDRANGE"
       ::= {acMGCommunication 2}



     acMGCommunicationGateWayPort OBJECT-TYPE
       SYNTAX Integer32 (-2147483647..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Users can use this parameter to force the media gateway to listen
to another UDP port instead of to the original 2427, as
defined in RFC 2705.

Range = 0 to 65535.
Access: Offline.
AC INI-Param: GATEWAYMGCPPORT"
       ::= {acMGCommunication 3}



     acMGMisc OBJECT IDENTIFIER ::= {acMGCPConfig 3}


     acMGMiscDigitmapMismatchNotification OBJECT-TYPE
       SYNTAX INTEGER {
                  doNotSend(0)
,
                  send(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The MGCP standard defines that if a number does not match the
digitmap definition, a notification is not sent.

One of the following values: 

1 = Send mismatch notification
 a digital mismatch notification is sent 

or 

0 = Do NOT send mismatch notification
 a digital mismatch notification is not sent. In the same way,
you can enable MGCP to send notifications upon matching
digitmap.
Access: Instant.
AC INI-Param: MGCPSendDigitmapMismatchNotification"
       ::= {acMGMisc 1}



     acMGMiscPiggyBackingEnable OBJECT-TYPE
       SYNTAX INTEGER {
                  disable(0)
,
                  enable(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "This parameter configures the option to send piggy backed commands
while RSIPS are sent. For example, if the event is triggered
by the board and RSIP was not sent yet, RSIP will be
sent and piggy back the event along with it, the call manager
will face endpoint restart and than the event.

Default = 1 (piggy back on)

0 = commands sent by gateway will not be piggy backed. 
1 =  commands sent by gateway will be piggy backed.
.
Access: Offline.
AC INI-Param: EnablePiggyBacking"
       ::= {acMGMisc 2}



     acMGMiscUseWildCardWithRSIP OBJECT-TYPE
       SYNTAX INTEGER {
                  disable(0)
,
                  enable(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "When wildcard is used RSIPs turn in a single message on EndPoint
Naming configuration and Single message for each trunk
in Trunk Naming configuration. If Off and number of channels
is less than 64 RSIP message sent for each Endpoint. 0 = Do
not use
1 = Use.
Access: Offline.
AC INI-Param: UseWildCardWithRSIP"
       ::= {acMGMisc 3}



     acMGMiscSDPProfile OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Controls MGCP functioning for SDP negotiation. The parameter
is bitwise.
Every new RFC support should be turned on or off with this
parameter. 
Each bit function is described in the control protocol chapter.
Access: Instant.
AC INI-Param: CPSDPPROFILE"
       ::= {acMGMisc 4}



     acMGMiscClearRequestBuffer OBJECT-TYPE
       SYNTAX INTEGER {
                  notClear(0)
,
                  clearOnXOnly(1)
,
                  clearOnXorDLCX(2)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Determines when signals and events are cleared.
0 = only an empty R: clears the event list and only an empty
S: clears and stops the current signals list.
Signals and events will be cleared only when new signals/events
are requested or an empty signals/events request is mentioned
in the command.
1 = if an encapsulated Request identifier (X:) is present in
the command, all TO signals and all events are cleared.
2 = same as value 1 , in addition If receive DLCX then all
signals are cleared (even if no (X:) is present in the command).
Access: Instant.
AC INI-Param: ClearRequestBuffer"
       ::= {acMGMisc 5}



     acMGNamePattern OBJECT IDENTIFIER ::= {acMGCPConfig 4}


     acMGNamePatternEndpoint OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..63))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the endpoint naming pattern for a gateway. The ‘*’ signs
will be replaced with an actual endpoint number or with
a wild-card sign. The string will contain up to 63 characters.

Default value will be “ACgw*”.
.
Access: Offline.
AC INI-Param: MGCPEndpointNamingPattern"
       ::= {acMGNamePattern 1}



     acMGNamePatternTrunk OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..63))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the trunk and B-channel naming pattern used by the gateway.
The ‘*’ signs will be replaced with a trunk or B-channel
number or with a wild-card sign. The string will contain
up to 63 characters. 

Default value will be “ds*/tr*”.
.
Access: Offline.
AC INI-Param: MGCPTrunkNamingPattern"
       ::= {acMGNamePattern 2}



     acMegacoConfig OBJECT IDENTIFIER ::= {acControlConfiguration 4}


     acLocalSwitching OBJECT IDENTIFIER ::= {acControlConfiguration 5}


     -- ****************************************
     -- acLocalSwitching table declaration
     -- ****************************************
     acLocalSwitchingTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcLocalSwitchingEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Local Switching definitions for analog ports"
       ::= {acLocalSwitching 1}



     -- ****************************************
     -- acLocalSwitching table entry
     -- ****************************************
     acLocalSwitchingEntry OBJECT-TYPE
       SYNTAX AcLocalSwitchingEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acLocalSwitchingIndex}
       ::= {acLocalSwitchingTable 1}



     -- ****************************************
     -- acLocalSwitching TABLE
     -- ****************************************
     AcLocalSwitchingEntry ::= SEQUENCE {
       acLocalSwitchingIndex                           Unsigned32,
       acLocalSwitchingRowStatus                       RowStatus,
       acLocalSwitchingPhoneNumber                     Unsigned32
     }



     acLocalSwitchingIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..23)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "
AC INI-Param: LocalSwitchingPorts_Index"
       ::= {acLocalSwitchingEntry 1}



     acLocalSwitchingRowStatus OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "
AC INI-Param: LocalSwitchingPorts_RowStatus"
       ::= {acLocalSwitchingEntry 2}



     acLocalSwitchingPhoneNumber OBJECT-TYPE
       SYNTAX Unsigned32
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Local Switching definitions for analog ports.
Access: Offline.
AC INI-Param: LocalSwitchingPorts_PhoneNumber"
       ::= {acLocalSwitchingEntry 3}



     acMCLink OBJECT IDENTIFIER ::= {acMegacoConfig 1}


     acMCCommunication OBJECT IDENTIFIER ::= {acMCLink 1}


     acMCCommunicationCheckLegalityOfMGC OBJECT-TYPE
       SYNTAX INTEGER {
                  disable(0)
,
                  enable(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "This parameter specifies if MEGACO rejects commands from an
MGC not in the provisioned list.

0 = Don't reject unknown MGCs
1 = Reject unknown MGC.
Access: Instant.
AC INI-Param: MEGACOCHECKLEGALITYOFMGC "
       ::= {acMCCommunication 1}



     acMCCommunicationGateWayMID OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..64))
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Defines the media gateway's MID towards the MEGACO Call Agent.
If empty or illegal, the MID holds the IP address of the
board.
Range: String[64].
Access: Offline.
AC INI-Param: MEGACO_MID"
       ::= {acMCCommunication 2}



     acMCCommunicationServiceChangeProfile OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..63))
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Specifies the Profile that will be displayed in the MEGACO serviceChange
command.

At this stage, the profile will not determine the features
supported.
Range = String[63].
Access: Offline.
AC INI-Param: CPSERVICECHANGEPROFILE"
       ::= {acMCCommunication 3}



     acMCCommunicationTimer OBJECT IDENTIFIER ::= {acMCLink 2}


     acMCCommunicationTimerMGProvisionalResponse OBJECT-TYPE
       SYNTAX Unsigned32 (0..20000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the provisional response timer for the media gateway
(in msec).

Range: 0 to 20000.
Access: Instant.
AC INI-Param: MGPROVISIONALRESPONSETIME"
       ::= {acMCCommunicationTimer 1}



     acMCCommunicationTimerMGCProvisionalResponse OBJECT-TYPE
       SYNTAX Unsigned32 (0..20000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the provisional response timer for the MGC (in msec).

Range: 0 to 20000.
Access: Instant.
AC INI-Param: MGCPROVISIONALRESPONSETIME"
       ::= {acMCCommunicationTimer 2}



     acMCCommunicationTimerMGExecutionTime OBJECT-TYPE
       SYNTAX Unsigned32 (0..2000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the estimated execution time of the media gateway (in
msec).

Range: 0 to 2000.
Access: Instant.
AC INI-Param: MGEXECUTIONTIME"
       ::= {acMCCommunicationTimer 3}



     acMCCommunicationTimerMGCExecutionTime OBJECT-TYPE
       SYNTAX Unsigned32 (0..2000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the estimated execution time of the MGC (in msec).

Range: 0 to 2000.
Access: Instant.
AC INI-Param: MGCEXECUTIONTIME"
       ::= {acMCCommunicationTimer 4}



     acMCCommunicationTimerHangTermTimeout OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Default timeout (in seconds) for sending Hanging Termination
event, when a request for Hanging Termination is sent without
parameters.

Range - 0 -65535.
Access: Instant.
AC INI-Param: MEGACOHangTermTimeout"
       ::= {acMCCommunicationTimer 5}



     acMCCommunicationTimerRestartMaxWaitingDelay OBJECT-TYPE
       SYNTAX Unsigned32 (0..600000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the Maximum Waiting Delay (in milliseconds) before restart
service change when the Media Gateway is powered on.
Access: Instant.
AC INI-Param: RestartMaximumWaitingDelay"
       ::= {acMCCommunicationTimer 6}



     acMCCommunicationTimerTargetMgResponseTime OBJECT-TYPE
       SYNTAX Unsigned32 (100..1000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The response time is defined as the time from the arrival of
a call set-up request until the response (in msec).

Range = 100-1000 in resolutions of 50 (i.e. 100, 150, 200,
250...).
Access: Instant.
AC INI-Param: TargetMG_ResponseTime"
       ::= {acMCCommunicationTimer 7}



     acMCNaming OBJECT IDENTIFIER ::= {acMegacoConfig 2}


     acMCNamePattern OBJECT IDENTIFIER ::= {acMCNaming 1}


     acMCNamePatternPhys OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..30))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the name pattern of a physical termination. 
For Example: 'tgw/t*/c*'. The '*' sign stands for the actual
numbers of the trunk and bchannel.

Range: String [30].
Access: Offline.
AC INI-Param: PHYSTERMNAMEPATTERN"
       ::= {acMCNamePattern 1}



     acMCNamePatternLogicalRTP OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..30))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the name pattern of an RTP termination.

For example: 'gw/rtp/*'. The '*' sign stands for the actual
number of the RTP termination.

Range: String [30].
Access: Offline.
AC INI-Param: LOGICALRTPTERMPATTERN"
       ::= {acMCNamePattern 2}



     acMCNamePatternLogicalATM OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..30))
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Defines the name pattern of an ATM termination.

Range: String [30].
Access: Offline.
AC INI-Param: LOGICALATMTERMPATTERN"
       ::= {acMCNamePattern 3}



     acMCNamePatternConf OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..32))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the name pattern of a conference termination.

Applicable to IPM-1610 and TP-6310 only.

Range: String[32].
Access: Offline.
AC INI-Param: CONFERENCETERMPATTERN"
       ::= {acMCNamePattern 4}



     acMCNamePatternBCTN OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..32))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the name pattern of a BCT termination.

Applicable to IPM-1610 and TP-6310 only.

Range: String[32].
Access: Offline.
AC INI-Param: BCTTERMPATTERN"
       ::= {acMCNamePattern 5}



     acMCNamePatternAudio OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..32))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the name pattern of an audio termination.

Applicable to IPM-1610 and TP-6310 only.

Range: String[32].
Access: Offline.
AC INI-Param: AUDIOTERMPATTERN"
       ::= {acMCNamePattern 6}



     acMCNamePatternTrunkTest OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..32))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the name pattern of a trunk test termination.

Applicable to IPM-1610 and TP-6310 only.

Range: String[32].
Access: Offline.
AC INI-Param: TRUNKTESTTERMPATTERN"
       ::= {acMCNamePattern 7}



     acMCNameNumber OBJECT IDENTIFIER ::= {acMCNaming 2}


     acMCNameNumberEphemeralIDOffset OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Offset for the ephemeral termination IDs in the gateway.
 e.g., offset = 100 causes the first ephemeral termination
ID to be 101. 
Note: This parameter was replaced by the parameter 'RTP_Num'.

Range = 0 to 4294967295.
Access: Instant.
AC INI-Param: MEGACOTERMINATIONIDOFFSET"
       ::= {acMCNameNumber 1}



     -- ****************************************
     -- acMCNameNumberPhysicalEndpoint table declaration
     -- ****************************************
     acMCNameNumberPhysicalEndpointTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcMCNameNumberPhysicalEndpointEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Magaco physical endpoint's numbering Table.;The table defines per level (e.g. trunk and channel) the numbering starting point and range.;The Row Status in this table is currently degenerated. It is permanently set to 'active(1)'. Also, changing other values in the table can be done freely (no need to set the Row Status to other values)."
       ::= {acMCNameNumber 21}



     -- ****************************************
     -- acMCNameNumberPhysicalEndpoint table entry
     -- ****************************************
     acMCNameNumberPhysicalEndpointEntry OBJECT-TYPE
       SYNTAX AcMCNameNumberPhysicalEndpointEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acMCNameNumberPhysicalEndpointIndex}
       ::= {acMCNameNumberPhysicalEndpointTable 1}



     -- ****************************************
     -- acMCNameNumberPhysicalEndpoint TABLE
     -- ****************************************
     AcMCNameNumberPhysicalEndpointEntry ::= SEQUENCE {
       acMCNameNumberPhysicalEndpointRowStatus         Unsigned32,
       acMCNameNumberPhysicalEndpointAction            Unsigned32,
       acMCNameNumberPhysicalEndpointActionResult      Unsigned32,
       acMCNameNumberPhysicalEndpointIndex             Unsigned32,
       acMCNameNumberPhysicalEndpointStart             Integer32,
       acMCNameNumberPhysicalEndpointMin               Unsigned32,
       acMCNameNumberPhysicalEndpointMax               Unsigned32
     }



     acMCNameNumberPhysicalEndpointRowStatus OBJECT-TYPE
       SYNTAX Unsigned32 (1..1)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Physical endpoint table row-status.
AC INI-Param: N/A"
       ::= {acMCNameNumberPhysicalEndpointEntry 1}



     acMCNameNumberPhysicalEndpointAction OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Physical endpoint table action.
AC INI-Param: N/A"
       ::= {acMCNameNumberPhysicalEndpointEntry 2}



     acMCNameNumberPhysicalEndpointActionResult OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Physical endpoint table result.
AC INI-Param: N/A"
       ::= {acMCNameNumberPhysicalEndpointEntry 3}



     acMCNameNumberPhysicalEndpointIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..4)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Index for table use.
AC INI-Param: N/A"
       ::= {acMCNameNumberPhysicalEndpointEntry 4}



     acMCNameNumberPhysicalEndpointStart OBJECT-TYPE
       SYNTAX Integer32 (-1..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the starting number for each name level (level 0 is
the left one when looking at the parameter defining Phys Term
Name Pattern). Thus, to start trunk numbering from 1, set
EP_NUM_0 to 1.

Range: Any positive number.
Access: Offline.
AC INI-Param: EP_NUM"
       ::= {acMCNameNumberPhysicalEndpointEntry 5}



     acMCNameNumberPhysicalEndpointMin OBJECT-TYPE
       SYNTAX Unsigned32 (0..255)
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Defines the minimum number for each name level (level 0 is the
left one, i.e., the trunk number).
Access: Offline.
AC INI-Param: EP_MIN"
       ::= {acMCNameNumberPhysicalEndpointEntry 6}



     acMCNameNumberPhysicalEndpointMax OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the maximum number for each name level (level 0 is the
left one, i.e., the trunk number).
Access: Offline.
AC INI-Param: EP_MAX"
       ::= {acMCNameNumberPhysicalEndpointEntry 7}



     -- ****************************************
     -- acMCNameNumberStreamEndpoint table declaration
     -- ****************************************
     acMCNameNumberStreamEndpointTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcMCNameNumberStreamEndpointEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Magaco stream endpoint's numbering Table.;The table defines per level the numbering starting point and range.;The Row Status in this table is currently degenerated. It is permanently set to 'active(1)'. Also, changing other values in the table can be done freely (no need to set the Row Status to other values)."
       ::= {acMCNameNumber 22}



     -- ****************************************
     -- acMCNameNumberStreamEndpoint table entry
     -- ****************************************
     acMCNameNumberStreamEndpointEntry OBJECT-TYPE
       SYNTAX AcMCNameNumberStreamEndpointEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acMCNameNumberStreamEndpointIndex}
       ::= {acMCNameNumberStreamEndpointTable 1}



     -- ****************************************
     -- acMCNameNumberStreamEndpoint TABLE
     -- ****************************************
     AcMCNameNumberStreamEndpointEntry ::= SEQUENCE {
       acMCNameNumberStreamEndpointRowStatus           Unsigned32,
       acMCNameNumberStreamEndpointAction              Unsigned32,
       acMCNameNumberStreamEndpointActionResult        Unsigned32,
       acMCNameNumberStreamEndpointIndex               Unsigned32,
       acMCNameNumberStreamEndpointRTPStart            Integer32,
       acMCNameNumberStreamEndpointATMStart            Integer32
     }



     acMCNameNumberStreamEndpointRowStatus OBJECT-TYPE
       SYNTAX Unsigned32 (1..1)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Stream endpoint table row-status.
AC INI-Param: N/A"
       ::= {acMCNameNumberStreamEndpointEntry 1}



     acMCNameNumberStreamEndpointAction OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Stream endpoint table action.
AC INI-Param: N/A"
       ::= {acMCNameNumberStreamEndpointEntry 2}



     acMCNameNumberStreamEndpointActionResult OBJECT-TYPE
       SYNTAX Unsigned32 (0..0)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Stream endpoint table result.
AC INI-Param: N/A"
       ::= {acMCNameNumberStreamEndpointEntry 3}



     acMCNameNumberStreamEndpointIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..1)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Index for table use.
AC INI-Param: N/A"
       ::= {acMCNameNumberStreamEndpointEntry 4}



     acMCNameNumberStreamEndpointRTPStart OBJECT-TYPE
       SYNTAX Integer32 (-1..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the starting number for each name's RTP termination
level.
Access: Instant.
AC INI-Param: RTP_NUM"
       ::= {acMCNameNumberStreamEndpointEntry 5}



     acMCNameNumberStreamEndpointATMStart OBJECT-TYPE
       SYNTAX Integer32 (-1..65535)
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Defines the starting number for each ATM termination level name.

Range: Any positive number.
Access: Instant.
AC INI-Param: ATM_NUM"
       ::= {acMCNameNumberStreamEndpointEntry 6}



     acMCPoolSize OBJECT IDENTIFIER ::= {acMegacoConfig 3}


     acMCPoolSizeProvisionedConf OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Provisioned conference size indicated by parameter X-PtEngr.

Applicable to IPM-1610 and TP-6310 only.

The value is dynamically limited according to the number of
DSP channels and the used feature key.

Range: 1 to 65535.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDCONFSIZE"
       ::= {acMCPoolSize 1}



     acMCPoolSizeProvisionedBCT OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Provisioned BCT size indicated by parameter X-PtEngr. 

Applicable to IPM-1610 and TP-6310 only.

Range: 1 to 65535.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDBCTSIZE"
       ::= {acMCPoolSize 2}



     acMCPoolSizeProvisionedAudio OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the provisioned audio size indicated by parameter X-PtEngr.

Applicable to IPM-1610 and TP-6310 only.

Range: 1 to 65535.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDAUDIOSIZE"
       ::= {acMCPoolSize 3}



     acMCPoolSizeNumOfTestTrunkPorts OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the provisioned TT (trunk testing) size indicated by
the parameter X-PtEngr.

Applicable to IPM-1610 and TP-6310 only.

Range: 1 to 65535.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDTRUNKTESTINGSIZE"
       ::= {acMCPoolSize 4}



     acMCProfile OBJECT IDENTIFIER ::= {acMegacoConfig 4}


     acMCProfileBinary OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Used to profile the binary ASN.1 encoding. 

Range: Integer >0
Refer to the product's User's Manual for possible values.
Access: Instant.
AC INI-Param: MEGACOASN1PROFILE"
       ::= {acMCProfile 1}



     acMCProfileAASPackages OBJECT-TYPE
       SYNTAX INTEGER {
                  tD-51standard(0)
,
                  h-248-9standard(1)
,
                  mGCP-Packet-Cable(2)
,
                  sIP-MSCML(3)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Selects the profile for the Advanced Audio Syntax specification.


0 = TD-51 standard
1 = H.248.9 standard
2 = MGCP Packet Cable
3 = SIP MSCML.
Access: Offline.
AC INI-Param: AASPACKAGESPROFILE"
       ::= {acMCProfile 2}



     acMCProfileTdmHairPinningMode OBJECT-TYPE
       SYNTAX INTEGER {
                  loopback(0)
,
                  pstn(1)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "determinewhich Hair-pinning mode is to be used:

mode 0 - will create TDM to TDM connection through IP software
Loopback 

mode 1 - will create “pure” hair-pinning i.e. TDM to TDM connection
through PSTN .
Access: Offline.
AC INI-Param: MegacoTdmHairPinningMode"
       ::= {acMCProfile 3}



     acMCMisc OBJECT IDENTIFIER ::= {acMegacoConfig 5}


     acMCMiscEncodingMethod OBJECT-TYPE
       SYNTAX INTEGER {
                   textEncoding(0)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Sets the MEGACO coding method. 

0 = Text mode.
Access: Offline.
AC INI-Param: MEGACOENCODING"
       ::= {acMCMisc 1}



     acMCMiscContextIDOffset OBJECT-TYPE
       SYNTAX Unsigned32 (0..20000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Offset for the context ID generated by the gateway.
e.g., offset = 100 causes the first context to be 101.

Range = 0 to 20000.
Access: Instant.
AC INI-Param: MEGACOCONTEXTIDOFFSET"
       ::= {acMCMisc 2}



     acMCMiscDisconnectBehavior OBJECT-TYPE
       SYNTAX INTEGER {
                  noActionOnDisconnect(1)
,
                  disableTrunksOnDisconnect(2)
,
                  resetBoardOnDisconnect(3)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Determines PBX behavior upon losing connectivity with H.248
Call agent or TPNCP.
1 = No Action -  keep routing traffic
2 = Disable Trunks - stop routing trafic BUT RTP remains active
3 = Reset Board - Stop all.
Access: Offline.
AC INI-Param: DisconnectBehavior"
       ::= {acMCMisc 3}



     acMCMiscMegacoVersion OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..10))
       MAX-ACCESS read-write
       STATUS deprecated
       DESCRIPTION
           "Determines the maximum Megaco Version number that is supported
by the device.
Access: Offline.
AC INI-Param: MegacoVersion"
       ::= {acMCMisc 4}



     acMCMiscSDPProfile OBJECT-TYPE
       SYNTAX Unsigned32 (0..2147483647)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Controls MEGACO functioning for SDP negotiation. The parameter
is bitwise.
Every new RFC support should be turned on or off with this
parameter. 
Each bit function is described in the control protocol chapter.
Access: Instant.
AC INI-Param: CPSDPPROFILE"
       ::= {acMCMisc 5}



     acMCAMS OBJECT IDENTIFIER ::= {acMegacoConfig 6}


     acMCAMSNumOfConferencePorts OBJECT-TYPE
       SYNTAX Unsigned32 (0..5000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Number Of Conference ports.  How many ports on the TPM are allocated
to the conferencing service.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDCONFSIZE"
       ::= {acMCAMS 1}



     acMCAMSNumOfTestTrunkPorts OBJECT-TYPE
       SYNTAX Unsigned32 (0..5000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Number Of Test Trunk ports.  How many ports on the TPM are allocated
to the Test Trunk service.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDTRUNKTESTINGSIZE"
       ::= {acMCAMS 2}



     acMCAMSNumOfLawfulInterceptPorts OBJECT-TYPE
       SYNTAX Unsigned32 (0..5000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Number Of Test Trunk ports.  How many ports on the TPM are allocated
to the Lawful Intercept service.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDBCTSIZE"
       ::= {acMCAMS 3}



     acMCAMSNumOfAnnouncementPorts OBJECT-TYPE
       SYNTAX Unsigned32 (0..5000)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Number Of Test Trunk ports.  How many ports on the TPM are allocated
to the Announcement service.
Access: Instant.
AC INI-Param: MEGACOPROVISIONEDAUDIOSIZE"
       ::= {acMCAMS 4}



     acMCVGW OBJECT IDENTIFIER ::= {acMegacoConfig 7}


     -- ****************************************
     -- acVGWConfiguration table declaration
     -- ****************************************
     acVGWConfigurationTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcVGWConfigurationEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Table provides the list of the gateway in the device and their configuration.{@}Virtual GW is represented as separate row in this table. "
       ::= {acMCVGW 21}



     -- ****************************************
     -- acVGWConfiguration table entry
     -- ****************************************
     acVGWConfigurationEntry OBJECT-TYPE
       SYNTAX AcVGWConfigurationEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acVGWConfigurationIndex}
       ::= {acVGWConfigurationTable 1}



     -- ****************************************
     -- acVGWConfiguration TABLE
     -- ****************************************
     AcVGWConfigurationEntry ::= SEQUENCE {
       acVGWConfigurationIndex                         Unsigned32,
       acVGWConfigurationRowStatus                     RowStatus,
       acVGWConfigurationAction                        INTEGER,
       acVGWConfigurationActionRes                     INTEGER,
       acVGWConfigurationVirtualGWName                 SnmpAdminString,
       acVGWConfigurationIPv4InterfaceName             SnmpAdminString,
       acVGWConfigurationIPv6InterfaceName             SnmpAdminString,
       acVGWConfigurationLocalPort                     Unsigned32,
       acVGWConfigurationAssociatedMembersList         SnmpAdminString,
       acVGWConfigurationServiceChangeProfile          SnmpAdminString,
       acVGWConfigurationMegacoVersion                 INTEGER,
       acVGWConfigurationMID                           SnmpAdminString,
       acVGWConfigurationMediaRealmName                SnmpAdminString,
       acVGWConfigurationLoadWeight                    Unsigned32
     }



     acVGWConfigurationIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..2)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Index Field for line.
AC INI-Param: MegacoGtwConfigurationTable_Index"
       ::= {acVGWConfigurationEntry 1}



     acVGWConfigurationRowStatus OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "ROWSTATUS Field for line.
AC INI-Param: MegacoGtwConfigutationTable_RowStatus"
       ::= {acVGWConfigurationEntry 2}



     acVGWConfigurationAction OBJECT-TYPE
       SYNTAX INTEGER {
                  none(0)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS.
AC INI-Param: MegacoGtwConfigutationTable_Action"
       ::= {acVGWConfigurationEntry 3}



     acVGWConfigurationActionRes OBJECT-TYPE
       SYNTAX INTEGER {
                  succeeded(0)

                  }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS RESULT.
AC INI-Param: MegacoGtwConfigutationTable_ActionRes"
       ::= {acVGWConfigurationEntry 4}



     acVGWConfigurationVirtualGWName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..17))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The descriptive name of the Virtual GW.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_VirtualGWName"
       ::= {acVGWConfigurationEntry 5}



     acVGWConfigurationIPv4InterfaceName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..15))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the pointer (Interface Name) to network Interface Table
for IP version 4 address interface name.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_IPv4InterfaceName"
       ::= {acVGWConfigurationEntry 6}



     acVGWConfigurationIPv6InterfaceName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..15))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the pointer (Interface name) to network Interface Table
for IP version 6 address interface name.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_IPv6InterfaceName"
       ::= {acVGWConfigurationEntry 7}



     acVGWConfigurationLocalPort OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the port to be used by the Media Gateway Controller to
communicate with this Virtual GW. The value 0 mean select
default port according to encoding method.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_LocalPort"
       ::= {acVGWConfigurationEntry 8}



     acVGWConfigurationAssociatedMembersList OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..64))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Defines the list of the Trunks/Interfaces. coma and range can
be used.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_AssociatedMembersList"
       ::= {acVGWConfigurationEntry 9}



     acVGWConfigurationServiceChangeProfile OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..64))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the service change profile.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_ServiceChangeProfile"
       ::= {acVGWConfigurationEntry 10}



     acVGWConfigurationMegacoVersion OBJECT-TYPE
       SYNTAX INTEGER {
                  megacoVersion1(1)
,
                  megacoVersion2(2)
,
                  megacoVersion3(3)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Megaco Version.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_MegacoVersion"
       ::= {acVGWConfigurationEntry 11}



     acVGWConfigurationMID OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..68))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the Virtual GW Message Identifier.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_MID"
       ::= {acVGWConfigurationEntry 12}



     acVGWConfigurationMediaRealmName OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..38))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the default media realm name (pointer to media realm
table).
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_MediaRealmName"
       ::= {acVGWConfigurationEntry 13}



     acVGWConfigurationLoadWeight OBJECT-TYPE
       SYNTAX Unsigned32 (1..5)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the weight of the VGW out of the total load.
VGW with higher values process more messages.
Access: Offline.
AC INI-Param: MegacoGtwConfigurationTable_LoadWeight"
       ::= {acVGWConfigurationEntry 14}



     -- ****************************************
     -- acVGWControllerLink table declaration
     -- ****************************************
     acVGWControllerLinkTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcVGWControllerLinkEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Table provides the list of the gateway controllers in the network and their configuration.{@}Each row represents link between Virtual Media GW and Media GW Controller."
       ::= {acMCVGW 22}



     -- ****************************************
     -- acVGWControllerLink table entry
     -- ****************************************
     acVGWControllerLinkEntry OBJECT-TYPE
       SYNTAX AcVGWControllerLinkEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acVGWControllerLinkVGWIndex,acVGWControllerLinkActivityOrder}
       ::= {acVGWControllerLinkTable 1}



     -- ****************************************
     -- acVGWControllerLink TABLE
     -- ****************************************
     AcVGWControllerLinkEntry ::= SEQUENCE {
       acVGWControllerLinkVGWIndex                     Unsigned32,
       acVGWControllerLinkActivityOrder                Unsigned32,
       acVGWControllerLinkRowStatus                    RowStatus,
       acVGWControllerLinkAction                       INTEGER,
       acVGWControllerLinkActionRes                    INTEGER,
       acVGWControllerLinkMGCAddressFormat             INTEGER,
       acVGWControllerLinkMGControllerAddress          SnmpAdminString,
       acVGWControllerLinkMGControllerPort             Unsigned32,
       acVGWControllerLinkTransportType                INTEGER
     }



     acVGWControllerLinkVGWIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..2)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The virtual GW index at MegacoGtwConfigutationTable.
AC INI-Param: MegacoGtwControllerLinkTable_VirtualGWIndex"
       ::= {acVGWControllerLinkEntry 1}



     acVGWControllerLinkActivityOrder OBJECT-TYPE
       SYNTAX Unsigned32 (1..10)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This parameter define the order of redundancy call agents (1
is the active CA).
AC INI-Param: MegacoGtwControllerLinkTable_ActivityOrder"
       ::= {acVGWControllerLinkEntry 2}



     acVGWControllerLinkRowStatus OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "ROWSTATUS Field for line.
AC INI-Param: MegacoGtwControllerLinkTable_RowStatus"
       ::= {acVGWControllerLinkEntry 3}



     acVGWControllerLinkAction OBJECT-TYPE
       SYNTAX INTEGER {
                  none(0)

                  }
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS.
AC INI-Param: MegacoGtwControllerLinkTable_Action"
       ::= {acVGWControllerLinkEntry 4}



     acVGWControllerLinkActionRes OBJECT-TYPE
       SYNTAX INTEGER {
                  succeeded(0)

                  }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Mangement Field for ACTIONS RESULT.
AC INI-Param: MegacoGtwControllerLinkTable_ActionRes"
       ::= {acVGWControllerLinkEntry 5}



     acVGWControllerLinkMGCAddressFormat OBJECT-TYPE
       SYNTAX INTEGER {
                  iPv4(0)
,
                  iPv6(1)
,
                  dNS(2)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the Define the format of the MGC address (IPv4, IPv6,
DNS).
Access: Offline.
AC INI-Param: MegacoGtwControllerLinkTable_MGCAddressFormat"
       ::= {acVGWControllerLinkEntry 6}



     acVGWControllerLinkMGControllerAddress OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..64))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The domain name or IP address of the MG Controller.
If a domain name is provided, then a DNS server must be configured.
Access: Offline.
AC INI-Param: MegacoGtwControllerLinkTable_MGControllerAddress"
       ::= {acVGWControllerLinkEntry 7}



     acVGWControllerLinkMGControllerPort OBJECT-TYPE
       SYNTAX Unsigned32 (0..65535)
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The port number MG Controller is listening for.
0 mean select default port according to encoding method.
Access: Offline.
AC INI-Param: MegacoGtwControllerLinkTable_MGControllerPort"
       ::= {acVGWControllerLinkEntry 8}



     acVGWControllerLinkTransportType OBJECT-TYPE
       SYNTAX INTEGER {
                  udpIP(0)
,
                  tcpIP(1)
,
                  sctpIP(2)

                  }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "Define the signaling transport type to be used for communication
with this MGC.
Access: Offline.
AC INI-Param: MegacoGtwControllerLinkTable_TransportType"
       ::= {acVGWControllerLinkEntry 9}



     acControlStatus OBJECT IDENTIFIER ::= {acControl 2}


     acActiveCallAgent OBJECT IDENTIFIER ::= {acControlStatus 1}


     acActiveCallAgentIp OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..20))
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Megaco Active Call Agent.
AC INI-Param: N/A"
       ::= {acActiveCallAgent 1}



     acActiveCallAgentPort OBJECT-TYPE
       SYNTAX Unsigned32 (0..32767)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Megaco Active Port.
AC INI-Param: N/A"
       ::= {acActiveCallAgent 2}



     acCurrentCalls OBJECT IDENTIFIER ::= {acControlStatus 2}


     acCallInfo OBJECT IDENTIFIER ::= {acCurrentCalls 1}


     -- ****************************************
     -- acCallInfo table declaration
     -- ****************************************
     acCallInfoTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcCallInfoEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       ::= {acCallInfo 1}



     -- ****************************************
     -- acCallInfo table entry
     -- ****************************************
     acCallInfoEntry OBJECT-TYPE
       SYNTAX AcCallInfoEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acCallInfoCallIndex}
       ::= {acCallInfoTable 1}



     -- ****************************************
     -- acCallInfo TABLE
     -- ****************************************
     AcCallInfoEntry ::= SEQUENCE {
       acCallInfoCallIndex                             Unsigned32,
       acCallInfoCallId                                SnmpAdminString,
       acCallInfoMediaType                             INTEGER,
       acCallInfoControlProtocol                       INTEGER,
       acCallInfoDuration                              Integer32
     }



     acCallInfoCallIndex OBJECT-TYPE
       SYNTAX Unsigned32 (0..5000)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The Index of a call.
AC INI-Param: N/A"
       ::= {acCallInfoEntry 1}



     acCallInfoCallId OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..64))
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Describes the Call ID in the control protocol.For mgcp, string,
For megaco asci.
AC INI-Param: N/A"
       ::= {acCallInfoEntry 2}



     acCallInfoMediaType OBJECT-TYPE
       SYNTAX INTEGER {
                  voice(1)
,
                  fax(2)
,
                  modem(3)
,
                  video(4)
,
                  transparent(5)
,
                  conference(6)

                  }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The type of the media transforming.
AC INI-Param: N/A"
       ::= {acCallInfoEntry 3}



     acCallInfoControlProtocol OBJECT-TYPE
       SYNTAX INTEGER {
                  mgcp(1)
,
                  megaco(2)
,
                  sip(3)
,
                  h323(4)

                  }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The name of the control protocol active now.
AC INI-Param: N/A"
       ::= {acCallInfoEntry 4}



     acCallInfoDuration OBJECT-TYPE
       SYNTAX Integer32 (-1..31536000)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "the duration of a call from the momet it started.
AC INI-Param: N/A"
       ::= {acCallInfoEntry 5}



     acCallHierarchy OBJECT IDENTIFIER ::= {acCurrentCalls 2}


     -- ****************************************
     -- acCallHierarchy table declaration
     -- ****************************************
     acCallHierarchyTable OBJECT-TYPE
       SYNTAX SEQUENCE OF AcCallHierarchyEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       ::= {acCallHierarchy 1}



     -- ****************************************
     -- acCallHierarchy table entry
     -- ****************************************
     acCallHierarchyEntry OBJECT-TYPE
       SYNTAX AcCallHierarchyEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           ""
       INDEX {acCallHierarchyCallIndex,acCallHierarchyLegType,acCallHierarchyLegID}
       ::= {acCallHierarchyTable 1}



     -- ****************************************
     -- acCallHierarchy TABLE
     -- ****************************************
     AcCallHierarchyEntry ::= SEQUENCE {
       acCallHierarchyCallIndex                        Integer32,
       acCallHierarchyLegType                          INTEGER,
       acCallHierarchyLegID                            Integer32,
       acCallHierarchyRowPointer                       RowPointer
     }



     acCallHierarchyCallIndex OBJECT-TYPE
       SYNTAX Integer32
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The Index of a call.
AC INI-Param: N/A"
       ::= {acCallHierarchyEntry 1}



     acCallHierarchyLegType OBJECT-TYPE
       SYNTAX INTEGER {
                  analog(1)
,
                  digital(2)
,
                  ip(3)
,
                  atm(4)
,
                  h110(5)
,
                  pci(6)

                  }
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Describes the Type of an end poit.
AC INI-Param: N/A"
       ::= {acCallHierarchyEntry 2}



     acCallHierarchyLegID OBJECT-TYPE
       SYNTAX Integer32 (0..20)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Describes the end point of a call by index.
AC INI-Param: N/A"
       ::= {acCallHierarchyEntry 3}



     acCallHierarchyRowPointer OBJECT-TYPE
       SYNTAX RowPointer
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "A pointer to the right instance in the current Leg table.
AC INI-Param: N/A"
       ::= {acCallHierarchyEntry 4}



     acMegacoStatus OBJECT IDENTIFIER ::= {acControlStatus 3}


     acMegacoStatusCurrentVersion OBJECT-TYPE
       SYNTAX Unsigned32 (1..3)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The Megaco version currently being used.
AC INI-Param: N/A"
       ::= {acMegacoStatus 1}





END
