-- =================================================================
-- Copyright (C) 2016 by HUAWEI TECHNOLOGIES. All rights reserved.
-- Description: MIB interface of BFD protocol configuration.
--              The Bidirectional Forwarding Detection (BFD) protocol
--              is standardized by the IETF. BFD detects the
--              traffic forwarding capability of the link or system by
--              quickly sending BFD control packets (the UDP packets in
--              a specified format) at intervals between two nodes.
-- Reference:
-- Version:     V1.55
--
-- =================================================================

    HUAWEI-BFD-MIB DEFINITIONS ::= BEGIN

        IMPORTS
            hwDatacomm
                FROM HUAWEI-MIB
            EnabledStatus
                FROM P-BRIDGE-MIB
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP
                FROM SNMPv2-CONF
            IpAddress, Integer32, Unsigned32, Counter32, OBJECT-TYPE,
            MODULE-IDENTITY, NOTIFICATION-TYPE
                FROM SNMPv2-SMI
            RowStatus, TEXTUAL-CONVENTION, TruthValue, DisplayString
                FROM SNMPv2-TC
            Ipv6Address
                FROM IPV6-TC
            InetAddressType, InetAddress
                FROM INET-ADDRESS-MIB;


        hwBFDMIB MODULE-IDENTITY
            LAST-UPDATED "201601080000Z"
            ORGANIZATION "Huawei Technologies Co.,Ltd."
            CONTACT-INFO
                "Huawei Industrial Base
                  Bantian, Longgang
                   Shenzhen 518129
                   People's Republic of China
                   Website: http://www.huawei.com
                   Email: support@huawei.com
                "
            DESCRIPTION
                "MIB interface of BFD protocol configuration.
                 The Bidirectional Forwarding Detection (BFD) protocol
                 is standardized by the IETF. BFD detects the
                 traffic forwarding capability of the link or system by
                 quickly sending BFD control packets (the UDP packets in
                 a specified format) at intervals between two nodes.
                "

            -- Revision history
              REVISION    "201601080000Z"
            DESCRIPTION "V1.55, add hwBfdSessConfbImpactFlag and hwBfdSessConfbImpactFlag."

            REVISION    "201601080000Z"
            DESCRIPTION "V1.54, add hwBfdSessFsmDiscordant and hwBfdSessFsmAccordant."

            REVISION    "201511080000Z"
            DESCRIPTION "V1.53, add hwBfdPWSessDownTrap and hwBfdPWSessUpTrap for Pw Bfd session."

            REVISION    "201510230000Z"
            DESCRIPTION "V1.52, add hwBfdSessApOperFailed for virtual access."
			
            REVISION    "201508040000Z"
            DESCRIPTION "V1.51, add hwBfdSessFaultDown and hwBfdSessResume."

            REVISION    "201507290000Z"
            DESCRIPTION "V1.50, modify the DESCRIPTION of hwBfdSessGlobalDefaultIpAddr."

            REVISION    "201507140000Z"
            DESCRIPTION "V1.49, move hwBfdSessCfgRemoteFailType from hwBfdAlarmTraps  to hwBfdNotifications."

            REVISION    "201507030000Z"
            DESCRIPTION "V1.48, add hwBfdSessCfgRemoteFailType and hwBfdSessCfgRemoteFail for virtual access."

            REVISION    "201409040000Z"
            DESCRIPTION "V1.47, modified the revision history."
			
            REVISION    "201409010000Z"
            DESCRIPTION "V1.46, modified the date of copyright."

            REVISION     "201406300000Z"
            DESCRIPTION  "V1.45, add hwBfdDynamicSessionTos for dynamic session tos in hwBfdScalarsObjects, add hwBfdv6MultiHopSessUpTrap,hwBfdv6MultiHopSessDownTrap for IPv6 MultiHop.
			             Add hwBfdSessPeerAddr,hwBfdSessBindType,hwBfdSessVrfIndex for hwBfdSessUpTrap and hwBfdSessDownTrap, add hwBfdv6SingleHopSessUpTrap,hwBfdv6SingleHopSessDownTrap for IPv6 SingleHop.
						 Add hwBfdDynamicSessionTos for dynamic session tos."
						 
            REVISION     "201405230000Z"
            DESCRIPTION  "V1.44, modified the scope of hwBfdIfConfName ."
			
            REVISION     "201401220000Z"
            DESCRIPTION  "V1.43, modified the description of hwBfdSessBindAppTypeMask for VTE/VPW/FRP/BGPLSP."

            REVISION     "201309220000Z"
            DESCRIPTION  "V1.42, modified the value and the description of hwBfdSessConfBindType for new bfd type bgpTunnel, modified the value and the description of hwBfdSessBindType for new bfd type bgpTunnel."

            REVISION     "201308160000Z"
            DESCRIPTION  "V1.41, modified the value and the description of hwBfdSessConfBindType for new bfd type ldpTunnel, modified the value and the description of hwBfdSessBindType for new bfd type ldpTunnel."

            REVISION     "201211230000Z"
            DESCRIPTION  "V1.40, add hwBfdStaticSessionTos for static session tos. Add hwBfdDynamicSessionTosEx for extend hwBfdDynamicSessionTos. Add hwBfdSessConfTOSEx for extend hwBfdSessConfTOS. Add hwBfdSessDscp to display dscp value when it is enable in a bfd session."

            REVISION     "201108170000Z"
            DESCRIPTION  "V1.25, add hwBfdSessBindAppTypeMask."

            REVISION     "201107140000Z"
            DESCRIPTION  "V1.24, add hwBfdDynamicSessionTos for dynamic session tos."

            REVISION     "201105110000Z"
            DESCRIPTION  "V1.23, modified BfdInterval to Integer32."

            REVISION     "201104270000Z"
            DESCRIPTION  "V1.22, removed the range of hwBfdSessActualRxInterval, hwBfdSessActualTxInterval, added the default value of hwBfdAdminStatus, hwBfdSessConfWTRInterval, hwBfdSessDetectMult, hwBfdSessDiscrAuto, hwBfdSessDynamicNumber, hwBfdSessInterfaceLimitNumber, hwBfdSessLimitNumber, hwBfdSessStaticNumber, hwBfdVersionNumber."

            REVISION     "201104130000Z"
            DESCRIPTION  "V1.21, modified the description of hwBfdIfConfEnable, hwBfdSessConfWTRInterval, hwBfdSessConfPSTFlag."

            REVISION     "201101120000Z"
            DESCRIPTION  "V1.20, modified for bfd mib standardization."

            REVISION     "201010200000Z"
            DESCRIPTION  "V1.19, updated the description and format."
            
            REVISION     "201008250000Z"
            DESCRIPTION  "V1.18, modified the trap nodes of hwBfdSessGroupUpTrap and hwBfdSessGroupDownTrap.
                          Updated the description and format."

            REVISION     "201008020000Z"
            DESCRIPTION  "V1.17, modified BfdInterval to Unsigned32."

            REVISION     "201008020000Z"
            DESCRIPTION  "V1.16, modified hwBfdSessConfRemoteDiscr and hwBfdSessRemoteDiscr's range from 1...16384 to 0...4294967295."
                       
            REVISION     "201007220000Z"
            DESCRIPTION  "V1.15, modified the description and format."
           
            REVISION     "201005190000Z"                               
            DESCRIPTION  "V1.14, modified syntax of hwBfdSessPerfLastSessDownTime and hwBfdSessionPerStartTime."  
           
            REVISION     "201004250000Z"                               
            DESCRIPTION  "V1.13, modified description of all leaves."    
           
            REVISION     "201004120000Z" 
            DESCRIPTION  "V1.12, updated the description and format."        
           
            REVISION     "201002120000Z" 
            DESCRIPTION  "V1.11, modified syntax of hwBfdSessPerfLastSessDownTime and hwBfdSessionPerStartTime."    
           
            REVISION     "201001130000Z" 
            DESCRIPTION  "V1.10, added four trap nodes of hwBfdSessUpTrap, hwBfdSessDownTrap, hwBfdSessGroupUpTrap
                          and hwBfdSessGroupDownTrap."    
                          
            REVISION     "200912240000Z" 
            DESCRIPTION  "V1.09, changed the range of leaves hwBfdSessConfDesiredMinRxInterval and 
                          hwBfdSessConfDesiredMinRxInterval."      
                                      
            REVISION     "200911270000Z" 
            DESCRIPTION  "V1.08, changed the range of leaf hwBfdSessRemoteDiscr as 0-4294967295."  
                                       
            REVISION     "200903040000Z" 
            DESCRIPTION  "V1.07, added flagNoPW, entireDynamic, staticAuto enum." 
           
            REVISION     "200806060000Z" 
            DESCRIPTION  "V1.06, added leaf hwBfdSessConfVlanID in table hwBfdSessionTable and changed the attribute of leaf hwBfdSessConfBindIfIndex as read-create."     
                                    
            REVISION     "200604270000Z"        
            DESCRIPTION  "V1.00, initial version." 

            ::= { hwDatacomm 38 }



--
-- Textual conventions
--
        BfdInterval ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION
                "Bfd Time Interval Type."
            SYNTAX Integer32

        BfdDiag ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION
                "Diagnostic code specifying the local system's reason for
                 the last session state changed.
                "
            SYNTAX Integer32


--
-- Node definitions
--
        hwBfdScalarsObjects OBJECT IDENTIFIER ::= { hwBFDMIB 1 }


        hwBfdVersionNumber OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The current version number of the BFD protocol is 1.
                 Default: 1
                "
            ::= { hwBfdScalarsObjects 1 }


        hwBfdAdminStatus OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Describe the administrative status of a BFD protocol.
                 Options:
                 1. enabled(1)   -denotes that the BFD Process is active on all interface
                 2. disabled(2)  -denotes that the BFD process is disabled on all interfaces
                 Default: 2
                "
            ::= { hwBfdScalarsObjects 2 }


        hwBfdSessLimitNumber OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Define the maximum number of BFD sessions allowed in the logic router.
                 Default: 0
                "
            ::= { hwBfdScalarsObjects 3 }


        hwBfdSessInterfaceLimitNumber OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Define the maximum number of BFD sessions allowed per board.
                 Default: 0
                "
            ::= { hwBfdScalarsObjects 4 }


        hwBfdSessStaticNumber OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of BFD static sessions.
                 Default: 0
                "
            ::= { hwBfdScalarsObjects 5 }


        hwBfdSessDynamicNumber OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of BFD dynamic sessions.
                 Default: 0
                "
            ::= { hwBfdScalarsObjects 6 }


        hwBfdSessGlobalDefaultIpAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Define the default multicast IP address used in BFD multicast detection.
                 Default: 224.0.0.184
                "
            ::= { hwBfdScalarsObjects 7 }


        hwBfdEchoPassiveStatus OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The passive Echo function of BFD.
                 Options:
                 1. enabled(1)  -denotes that the BFD EchoPassive capability is enabled
                 2. disabled(2) -denotes that the BFD EchoPassive capability is disabled
                 Default: 2
                "
            ::= { hwBfdScalarsObjects 8 }


        hwBfdEchoAclNum OBJECT-TYPE
            SYNTAX Unsigned32 (0 | 2000..2999)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The Acl Number for passive Echo function of BFD.
                 Default: 0
                "
            ::= { hwBfdScalarsObjects 9 }


        hwBfdSessDynamicPingInterval OBJECT-TYPE
            SYNTAX Unsigned32 (30..600)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Define the sending interval of the MPLS echo packet.
                 Default: 60
                 Unit: second
                "
            ::= { hwBfdScalarsObjects 10 }


        hwBfdSessDynamicSupportPassive OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The capability of automatically creating BFD sessions on the LSP egress.
                 Options:
                 1. enabled(1)  -denotes that the egress can create BFD sessions
                 2. disabled(2) -denotes that the egress can not create BFD sessions
                 Default: 2
                "
            ::= { hwBfdScalarsObjects 11 }

        hwBfdSessDelayUpTime OBJECT-TYPE
            SYNTAX Unsigned32 (0..600)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Define delay interval before the session turns to up.
                 Unit: second
                 Default: 0
                "
            ::= { hwBfdScalarsObjects 12 }


        hwBfdSessMultiDstPort OBJECT-TYPE
            SYNTAX Integer32 (0|3784|4784)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The destination UDP port of multi-hop BFD session. When the
                 administrative status of BFD protocol is disabled, this value
                 will be 0.
                 Default: 3784
                "
            ::= { hwBfdScalarsObjects 13 }

        hwBfdTrapSendInterval OBJECT-TYPE
            SYNTAX Integer32 (0|1..600)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Define the sending interval of TRAP message.
                 Unit: second
                 Default: 120
                "
            ::= { hwBfdScalarsObjects 14 }

        hwBfdLimitDeviceName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The device name which session number reached up limit."
            ::= { hwBfdScalarsObjects 15 }

        hwBfdDynamicSessionTos OBJECT-TYPE
            SYNTAX Unsigned32 (0..7)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The Tos-Exp of dynamic session.
                 Default: 7
                "
            ::= { hwBfdScalarsObjects 16 }

        hwBfdStaticSessionTos OBJECT-TYPE
            SYNTAX Unsigned32 (0..7 | 255)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The Tos-Exp of static session.
                 Default: 7
                "
            ::= { hwBfdScalarsObjects 17 }

        hwBfdDynamicSessionTosEx OBJECT-TYPE
            SYNTAX Unsigned32 (0..7 | 255)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The extended Tos-Exp of dynamic session.
                 Default: 7
                "
            ::= { hwBfdScalarsObjects 18 }

        hwBfdSessCfgRemoteFailType OBJECT-TYPE
            SYNTAX INTEGER
                {
                localDiscriminatorNonsupport(101),
                localDiscriminatorConflict(102)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The virtual access AP notify process bfd session configuration failed.
                 Options:
                 1. localDiscriminatorNonsupport(101)
                 2. localDiscriminatorConflict(102)
                "
            ::= { hwBfdScalarsObjects 19 }	

        hwBfdObjects OBJECT IDENTIFIER ::= { hwBFDMIB 2 }


        hwBfdIfConfTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBfdIfConfEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The interface configuration table of BFD.
                 The index of this table is hwBfdIfConfIndex.
                "
            ::= { hwBfdObjects 1 }


        hwBfdIfConfEntry OBJECT-TYPE
            SYNTAX HwBfdIfConfEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The interface configuration table of BFD.
                 The index of this entry is hwBfdIfConfIndex.
                "
            INDEX { hwBfdIfConfIndex }
            ::= { hwBfdIfConfTable 1 }


        HwBfdIfConfEntry ::=
            SEQUENCE {
                hwBfdIfConfIndex
                    Integer32,
                hwBfdIfConfName
                    OCTET STRING,
                hwBfdIfConfEnable
                    Integer32,
                hwBfdIfConfDeleting
                    Integer32,
                hwBfdIfConfAvailable
                    Integer32,
                hwBfdIfConfSessCnt
                    Integer32,
                hwBfdIfConfRowStatus
                    RowStatus
             }

        hwBfdIfConfIndex OBJECT-TYPE
            SYNTAX Integer32 (1..2147483647)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "It is the configuration index of this interface.
                 This index is automatically allocated inside the system
                 and is not user-configurable.
                "
            ::= { hwBfdIfConfEntry 1 }


        hwBfdIfConfName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the name of this Interface."
            ::= { hwBfdIfConfEntry 2 }


        hwBfdIfConfEnable OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
               "The flag whether the interface has enabled BFD.
                Options:
                1. disable(0) -Indicates that the interface has disabled BFD
                2. enable(1)  -Indicates that the interface has enabled BFD
               "
            ::= { hwBfdIfConfEntry 3 }


        hwBfdIfConfDeleting OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The flag that whether the interface is in deleting.
                 Options:
                 1. notDeleted(0)  -the interface is not deleted
                 2. deleted(1)     -the interface is deleted
                "
            ::= { hwBfdIfConfEntry 4 }


        hwBfdIfConfAvailable OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The flag that whether the interface is available.
                 Options:
                 1. notAvailable(0) -the interface is not available
                 2. available(1)    -the interface is available
                "
            ::= { hwBfdIfConfEntry 5 }


        hwBfdIfConfSessCnt OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The number of sessions that has been bound to this interface."
            ::= { hwBfdIfConfEntry 6 }


        hwBfdIfConfRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Used to manage the creation and deletion of conceptual rows."
            ::= { hwBfdIfConfEntry 7 }


        hwBfdSessionConfTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBfdSessionConfEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "BFD Session Configuration Table. Use this table to get/configure BFD sessions.
                 The index of this table is hwBfdSessConfName.
                "
            ::= { hwBfdObjects 2 }


        hwBfdSessionConfEntry OBJECT-TYPE
            SYNTAX HwBfdSessionConfEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "BFD Session Configuration Table. Use this table to get/configure BFD sessions.
                 The index of this entry is hwBfdSessConfName.
                "
            INDEX { hwBfdSessConfName }
            ::= { hwBfdSessionConfTable 1 }


        HwBfdSessionConfEntry ::=
            SEQUENCE {
                hwBfdSessConfName
                    OCTET STRING,
                hwBfdSessConfMIndex
                    Unsigned32,
                hwBfdSessConfLocalDiscr
                    Unsigned32,
                hwBfdSessConfRemoteDiscr
                    Unsigned32,
                hwBfdSessConfPeerAddr
                    IpAddress,
                hwBfdSessConfBindIfIndex
                    Unsigned32,
                hwBfdSessConfBindIfName
                    OCTET STRING,
                hwBfdSessConfDemandEnable
                    Integer32,
                hwBfdSessConfDemandTimerInterval
                    Unsigned32,
                hwBfdSessConfDetectMult
                    Unsigned32,
                hwBfdSessConfDesiredMinRxInterval
                    BfdInterval,
                hwBfdSessConfDesiredMinTxInterval
                    BfdInterval,
                hwBfdSessConfWTRInterval
                    Integer32,
                hwBfdSessConfTOS
                    Integer32,
                hwBfdSessConfPSTFlag
                    Integer32,
                hwBfdSessConfCommitFlag
                    Integer32,
                hwBfdSessConfAdminStatus
                    Integer32,
                hwBfdSessConfRowStatus
                    RowStatus,
                hwBfdSessConfSourceAddr
                    IpAddress,
                hwBfdSessConfVrfIndex
                    Unsigned32,
                hwBfdSessConfVPNName
                    OCTET STRING,
                hwBfdSessConfDefaultIp
                    INTEGER,
                hwBfdSessConfPISFlag
                    INTEGER,
                hwBfdSessConfBindType
                    INTEGER,
                hwBfdSessConfNextHop
                    IpAddress,
                hwBfdSessConfStaticLspName
                    OCTET STRING,
                hwBfdSessConfPWSecondaryFlag
                    INTEGER,
                hwBfdSessConfTunnelDetectType
                    INTEGER,
                hwBfdSessConfVcId
                    Unsigned32,
                hwBfdSessConfVsiName
                    OCTET STRING,
                hwBfdSessConfVsiPeerAddr
                    IpAddress,
                hwBfdSessConfDiscrAuto
                    EnabledStatus,
                hwBfdSessConfPeerIpv6Addr
                    Ipv6Address,
                hwBfdSessConfSourceIpv6Addr
                    Ipv6Address,
                hwBfdSessConfIpv6NextHop
                    Ipv6Address,
                hwBfdSessConfIsIpv6Addr
                    TruthValue,
                hwBfdSessConfKeychainName
                    OCTET STRING,
                hwBfdSessConfMeticulous
                    EnabledStatus,
                hwBfdSessConfLooseAuthentication
                    TruthValue,
                hwBfdSessConfOneArmEcho
                    EnabledStatus,
                hwBfdSessConfMinEchoRxInterval
                    Unsigned32,
                hwBfdSessConfPWTtlMode
                    INTEGER,
                hwBfdSessConfPWTtl
                    Integer32,
                hwBfdSessConfRemotePeerIpType
                    InetAddressType,
                hwBfdSessConfRemotePeerIp
                    InetAddress,
                hwBfdSessConfSelectBoard
                    DisplayString,
                hwBfdSessConfPWSPE
                    INTEGER,
                hwBfdSessConfPWTrackIfName
                    DisplayString,
                hwBfdSessConfIsPWTrackIf
                    EnabledStatus,
                hwBfdSessConfEncapsulationType
                    DisplayString,
                hwBfdSessConfPEVid
                    Unsigned32,
                hwBfdSessConfCEVid
                    Unsigned32,
                hwBfdSessConfTOSEx
                    Integer32,
                hwBfdSessConfbImpactFlag
                    INTEGER
             }

        hwBfdSessConfName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..15))
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "It is the name of this configuration model."
            ::= { hwBfdSessionConfEntry 1 }


        hwBfdSessConfMIndex OBJECT-TYPE
            SYNTAX Unsigned32 (1..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the configuration index of this session."
            ::= { hwBfdSessionConfEntry 2 }


        hwBfdSessConfLocalDiscr OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Define the local discriminator of the BFD session."
            ::= { hwBfdSessionConfEntry 3 }


        hwBfdSessConfRemoteDiscr OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Define the remote discriminator of the BFD session."
            ::= { hwBfdSessionConfEntry 4 }


        hwBfdSessConfPeerAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Define the IP address of the peer in the BFD session."
            ::= { hwBfdSessionConfEntry 5 }


        hwBfdSessConfBindIfIndex OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the index of the binding interface in the BFD configuration."
            ::= { hwBfdSessionConfEntry 6 }


        hwBfdSessConfBindIfName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the name of the binding interface in the BFD configuration."
            ::= { hwBfdSessionConfEntry 7 }


        hwBfdSessConfDemandEnable OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the flag of the BFD demand mode.
                 Options:
                 1. disabled(0) -disable the BFD demand mode
                 2. enabled(1)  -enable the BFD demand mode
                "
            DEFVAL { 0 }
            ::= { hwBfdSessionConfEntry 8 }


        hwBfdSessConfDemandTimerInterval OBJECT-TYPE
            SYNTAX Unsigned32 (0 | 500..300000)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Define the detecting interval in the BFD session with the demand mode.
                 Unit: millisecond
                "
            ::= { hwBfdSessionConfEntry 9 }


        hwBfdSessConfDetectMult OBJECT-TYPE
            SYNTAX Unsigned32 (3..50)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is Detect time multiplier of the configuration. The
                 negotiated transmit interval, multiplied by this value,
                 provides the detection time for the transmitting
                 system in Asynchronous mode.
                "
           ::= { hwBfdSessionConfEntry 10 }


        hwBfdSessConfDesiredMinRxInterval OBJECT-TYPE
            SYNTAX BfdInterval (1..2147483647)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This is the minimum interval of the configuration,in
                 milliseconds, between received BFD Control packets
                 that this system is capable of supporting.
                 Unit: millisecond
                "
            ::= { hwBfdSessionConfEntry 11 }


        hwBfdSessConfDesiredMinTxInterval OBJECT-TYPE
            SYNTAX BfdInterval (1..2147483647)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This is the minimum interval of the configuration,
                 in milliseconds, that the local system would
                 like to use when transmitting BFD Control packets.
                 Unit: millisecond
                "
            ::= { hwBfdSessionConfEntry 12 }


        hwBfdSessConfWTRInterval OBJECT-TYPE
            SYNTAX Integer32 (0..60)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The wait-to-restore (WTR) time of the BFD session.
                 The event that indicates the session changing into the Up 
                 state is reported to the application program only after 
                 the WTR times out.
                 Unit: minute 
                "  
            DEFVAL { 0 }       
            ::= { hwBfdSessionConfEntry 13 }


        hwBfdSessConfTOS OBJECT-TYPE
            SYNTAX Integer32 (0..7)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This is the TOS value of bfd packet."
            DEFVAL { 7 }
            ::= { hwBfdSessionConfEntry 14 }


        hwBfdSessConfPSTFlag OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The PST flag of the BFD session configuration. 
                 It indicates the status association between the current BFD 
                 session and the interface bound to the session.
                 Options:
                 1. disabled(0)  -indicates that the PST capability of the BFD session is disabled
                 2. enabled(1)   -indicates that the PST capability of the BFD session is enabled
                "
            DEFVAL { 0 }
            ::= { hwBfdSessionConfEntry 15 }


        hwBfdSessConfCommitFlag OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the commit flag of the configuration entry.
                 Options:
                 1. notCommit(0) -not commit
                 2. commit(1)    -commit
                "
            ::= { hwBfdSessionConfEntry 16 }


        hwBfdSessConfAdminStatus OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "A BFD session can be administratively enabled or disabled.
                 The AdminStatus field indicates the BFD session status.
                 Options:
                 1. 0 -disable
                 2. 1 -enable
                "
            ::= { hwBfdSessionConfEntry 17 }


        hwBfdSessConfRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Used to manage the creation and deletion of conceptual rows."
            ::= { hwBfdSessionConfEntry 18 }


        hwBfdSessConfSourceAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Define the source IP address of the BFD session."
            ::= { hwBfdSessionConfEntry 19 }


        hwBfdSessConfVrfIndex OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The index of the VPN interface."
            ::= { hwBfdSessionConfEntry 20 }


        hwBfdSessConfVPNName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..31))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The name of VPN interface."
            ::= { hwBfdSessionConfEntry 21 }


        hwBfdSessConfDefaultIp OBJECT-TYPE
            SYNTAX INTEGER
                {
                no(1),
                yes(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "BFD session use default multicast IP as the detect peer-ip
                 Options:
                 1. no(1)  -do not use the default multicast IP
                 2. yes(2) -use the default multicast IP
                "
            DEFVAL { 1 }
            ::= { hwBfdSessionConfEntry 22 }


        hwBfdSessConfPISFlag OBJECT-TYPE
            SYNTAX INTEGER
                {
                false(1),
                true(2),
                subif(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The state of BFD session is associated with the state of the binding interface
                 Options:
                 1. false(1) -do not associate with interface state
                 2. true(2)  -associate with interface state
                 3. subif(3) -associate with interface and correlative sub interface
                "
            DEFVAL { 1 }
            ::= { hwBfdSessionConfEntry 23 }


        hwBfdSessConfBindType OBJECT-TYPE
            SYNTAX INTEGER
                {
                interfaceIp(1),
                peerIp(2),
                sourceIp(3),
                ifAndSourceIp(4),
                fec(5),
                tunnelIf(6),
                ospf(7),
                isis(8),
                ldpLsp(9),
                staticLsp(10),
                teLsp(11),
                teTunnel(12),
                pw(13),
                vsiPw(15),
                ldpTunnel(21),
                bgpTunnel(22)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The binding type of the BFD session.
                 Options:
                 1. interfaceIp(1)    -BFD for IP with peer-ip and interface
                 2. peerIp(2)         -BFD for IP only with peer-ip
                 3. sourceIp(3)       -BFD for IP with peer-ip and source-ip
                 4. ifAndSourceIp(4)  -BFD for IP with peer-ip, interface and source-ip
                 5. fec(5)            -BFD for FEC(NOT support now)
                 6. tunnelIf(6)       -BFD for Tunnel interface(NOT support now)
                 7. ospf(7)           -BFD for OSPF
                 8. isis(8)           -BFD for ISIS
                 9. ldpLsp(9)         -BFD for LDP-LSP
                 10. staticLsp(10)    -BFD for static LSP
                 11. teLsp(11)        -BFD for TE-LSP
                 12. teTunnel(12)     -BFD for TE-Tunnel
                 13. pw(13)           -BFD for PW
                 14. vsiPw(15)        -BFD for VSI PW
                 15. ldpTunnel(21)    -BFD for LDP-Tunnel
                 16. bgpTunnel(22)    -BFD for BGP-Tunnel
                "
            ::= { hwBfdSessionConfEntry 24 }


        hwBfdSessConfNextHop OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the next hop of the BFD session."
            ::= { hwBfdSessionConfEntry 25 }


        hwBfdSessConfStaticLspName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..20))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the static LSP name of the BFD session."
            ::= { hwBfdSessionConfEntry 26 }


        hwBfdSessConfPWSecondaryFlag OBJECT-TYPE
            SYNTAX INTEGER
                {
                flagMasterPW(1),
                flagSecondaryPW(2),
                flagNoPW(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The role of the PW bound with BFD session.
                 Options:
                 1. flagMasterPW(1)   -master PW
                 2. flagSecondaryPW(2)-secondary PW
                 3. flagNoPW(3)       -no PW
                "
            DEFVAL { 1 }
            ::= { hwBfdSessionConfEntry 27 }


        hwBfdSessConfTunnelDetectType OBJECT-TYPE
            SYNTAX INTEGER
                {
                flagBothDown(1),
                flagNeighborDown(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Set the failure notifies policy type.
                 Options:
                 1. flagBothDown(1)     -notify applications when detecting both Detect-Down and Neighbor-Down
                 2. flagNeighborDown(2) -notify applications only when detecting Neighbor-Down
                "
            DEFVAL { 1 }
            ::= { hwBfdSessionConfEntry 28 }


        hwBfdSessConfVcId OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the ID of VC."
            ::= { hwBfdSessionConfEntry 29 }


        hwBfdSessConfVsiName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..31))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the name of VSI."
            ::= { hwBfdSessionConfEntry 30 }


        hwBfdSessConfVsiPeerAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "It is the peer-ip of VSI."
            ::= { hwBfdSessionConfEntry 31 }

        hwBfdSessConfDiscrAuto OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Describe whether the discriminator can be auto allocated.
                 Options:
                 1.enabled(1)  -the discriminator can be allocated automatically
                 2.disabled(2) -the discriminator can not be allocated automatically
                "
            DEFVAL { disabled }
            ::= { hwBfdSessionConfEntry 32 }

        hwBfdSessConfPeerIpv6Addr OBJECT-TYPE
            SYNTAX Ipv6Address
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Define the peer IPv6 address of the BFD session."
            ::= { hwBfdSessionConfEntry 33 }

        hwBfdSessConfSourceIpv6Addr OBJECT-TYPE
            SYNTAX Ipv6Address
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Define the source IPv6 address of the BFD session."
            ::= { hwBfdSessionConfEntry 34 }

        hwBfdSessConfIpv6NextHop OBJECT-TYPE
            SYNTAX Ipv6Address
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the next hop of the BFD session."
            ::= { hwBfdSessionConfEntry 35 }

        hwBfdSessConfIsIpv6Addr OBJECT-TYPE
            SYNTAX TruthValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Whether the peer address of the BFD session is IPv6 address."
            DEFVAL { false }
            ::= { hwBfdSessionConfEntry 36 }


        hwBfdSessConfKeychainName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..47))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Specify the name of the keychain for authentication."
            ::= { hwBfdSessionConfEntry 37 }

        hwBfdSessConfMeticulous OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Whether enable meticulous authentication for MD5 or SHA-1 type.
                 Options:
                 1. enabled(1)  -enable meticulous authentication for MD5 or SHA-1 type
                 2. disabled(2) -disabled meticulous authentication for MD5 or SHA-1 type
                "
            DEFVAL { disabled }
            ::= { hwBfdSessionConfEntry 38 }

        hwBfdSessConfLooseAuthentication OBJECT-TYPE
            SYNTAX TruthValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Whether loose authentication check.
                 Options:
                 1.True(1)  -loose-check
                 2.False(2) -do not loose-check
                "
            ::= { hwBfdSessionConfEntry 39 }

        hwBfdSessConfOneArmEcho OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies whether a session works in one-arm-echo mode.
                 Options:
                 1. enabled(1)  -indicates that the session works in one-arm-echo mode
                 2. disabled(2) -indicates that the session does not work in one-arm-echo mode
                "
            DEFVAL { disabled }
            ::= { hwBfdSessionConfEntry 40 }

        hwBfdSessConfMinEchoRxInterval OBJECT-TYPE
            SYNTAX Unsigned32 (0|1..4294967295)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the minimum interval between received BFD
                 Control packets, in milliseconds.This value reflects the capability of receiving
                 BFD Control packets.
                 Unit: millisecond
                "
            ::= { hwBfdSessionConfEntry 41 }

        hwBfdSessConfPWTtlMode OBJECT-TYPE
            SYNTAX INTEGER
            {
            config(1),
            auto(2),
            default(3),
            none(4)
            }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the configuration mode of a TTL used by
                 the BFD session for PW.
                 Options:
                 1. config(1) -indicates that the TTL is manually set
                 2. auto(2)   -indicates that the TTL is automatically calculated based on an IP address
                 3. default(3)-indicates that the TTL is 255 by default
                 4. none(4)   -indicates that the TTL is not in PW mode
                "
            ::= { hwBfdSessionConfEntry 42 }

        hwBfdSessConfPWTtl OBJECT-TYPE
            SYNTAX Integer32 (0..255)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the TTL used by the BFD session for PW.
                 The vlaue is configurable only when the configuration mode of a TTL is config.
                "
            ::= { hwBfdSessionConfEntry 43 }

        hwBfdSessConfRemotePeerIpType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the type of the destination address of the BFD
                 session for PW.
                "
            ::= { hwBfdSessionConfEntry 44 }

        hwBfdSessConfRemotePeerIp OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the destination IP address of the BFD session
                 for PW.
                "
            ::= { hwBfdSessionConfEntry 45 }

        hwBfdSessConfSelectBoard OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..47))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the main processing board of a BFD session."
            ::= { hwBfdSessionConfEntry 46 }

        hwBfdSessConfPWSPE OBJECT-TYPE
            SYNTAX INTEGER
            {
            upe(1),
            spe(2),
            none(3)
            }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the node on which a BFD session is set up.
                 The values are as follows.
                 Options:
                 1. upe(1)  -indicates that a BFD session is set up on a UPE to detect a PW
                 2. spe(2)  -indicates that a BFD session is set up on an SPE to detect a PW
                 3. none(3) -indicates that a BFD session does not detect a PW
                 Default: none
                "
            ::= { hwBfdSessionConfEntry 47 }

        hwBfdSessConfPWTrackIfName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the interface monitored by the BFD session for PW."
            ::= { hwBfdSessionConfEntry 48 }

        hwBfdSessConfIsPWTrackIf OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies whether the BFD session for
                 PW monitors an interface. The values are as follows.
                 Options:
                 1. enabled(1) -enables the BFD session for PW to monitor the interface
                 2. disabled(2)-disables the BFD session for PW from monitoring the interface
                "
            ::= { hwBfdSessionConfEntry 49 }

        hwBfdSessConfEncapsulationType OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..63))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the VC encapsulation type on an SPE.
                 The values are as follows:
                fr
                atm-aal5-sdu
                atm-trans-cell
                vlan
                ethernet
                hdlc
                ppp
                atm-nto1-vcc
                atm-nto1-vpc
                ip-layer2
                atm-1to1-vcc
                atm-1to1-vpc
                atm-aal5-pdu
                satop-e1
                satop-t1
                esopsn-basic
                ip-interworking
                "
            ::= { hwBfdSessionConfEntry 50 }

        hwBfdSessConfPEVid OBJECT-TYPE
            SYNTAX Unsigned32 (0..4094)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the outer tag of a sub-interface
                 for QinQ VLAN tag termination or the VLAN ID of a sub-interface for
                 dot1q VLAN tag termination.
                "
            ::= { hwBfdSessionConfEntry 51 }

        hwBfdSessConfCEVid OBJECT-TYPE
            SYNTAX Unsigned32 (0..4094)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies the inner tag in QinQ packets."
            ::= { hwBfdSessionConfEntry 52 }

        hwBfdSessConfTOSEx OBJECT-TYPE
            SYNTAX Integer32 (0..7 | 255)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This is the extended TOS value of bfd packet."
            DEFVAL { 7 }
            ::= { hwBfdSessionConfEntry 53 }

        hwBfdSessConfbImpactFlag OBJECT-TYPE
            SYNTAX INTEGER
                {
                no(1),
                yes(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "BFD session impact interface when the device reboot
                 Options:
                 1. no(1)  -do not impact interface when the device reboot
                 2. yes(2) -impact interface when the device reboot
                "
            DEFVAL { 1 }
            ::= { hwBfdSessionConfEntry 54 }

        hwBfdSessionTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBfdSessionEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The BFD Session Table describes the BFD sessions.
                 The index of this table is hwBfdSessIndex.
                "
            ::= { hwBfdObjects 3 }


        hwBfdSessionEntry OBJECT-TYPE
            SYNTAX HwBfdSessionEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The BFD Session Table describes the BFD sessions.
                 The index of this entry is hwBfdSessIndex.
                "
            INDEX { hwBfdSessIndex }
            ::= { hwBfdSessionTable 1 }


        HwBfdSessionEntry ::=
            SEQUENCE {
                hwBfdSessIndex
                    Unsigned32,
                hwBfdSessMIndex
                    Unsigned32,
                hwBfdSessBindVRRP
                    Integer32,
                hwBfdSessCfgName
                    OCTET STRING,
                hwBfdSessPeerAddr
                    IpAddress,
                hwBfdSessBindIfIndex
                    Integer32,
                hwBfdSessBindIfName
                    OCTET STRING,
                hwBfdSessLocalDiscr
                    Unsigned32,
                hwBfdSessRemoteDiscr
                    Unsigned32,
                hwBfdSessOperMode
                    Integer32,
                hwBfdSessDetectMult
                    Unsigned32,
                hwBfdSessDemandTimerInterval
                    BfdInterval,
                hwBfdSessActualRxInterval
                    BfdInterval,
                hwBfdSessActualTxInterval
                    BfdInterval,
                hwBfdSessWTRInterval
                    Integer32,
                hwBfdSessTOS
                    Integer32,
                hwBfdSessState
                    Integer32,
                hwBfdSessDiag
                    Integer32,
                hwBfdSessSourceAddr
                    IpAddress,
                hwBfdSessVrfIndex
                    Unsigned32,
                hwBfdSessVPNName
                    OCTET STRING,
                hwBfdSessType
                    INTEGER,
                hwBfdSessBindAppType
                    INTEGER,
                hwBfdSessDefaultIp
                    INTEGER,
                hwBfdSessPISFlag
                    INTEGER,
                hwBfdSessBindType
                    INTEGER,
                hwBfdSessNextHop
                    IpAddress,
                hwBfdSessStaticLspName
                    OCTET STRING,
                hwBfdSessLspIndex
                    Unsigned32,
                hwBfdSessPWSecondaryFlag
                    INTEGER,
                hwBfdSessTunnelDetectType
                    INTEGER,
                hwBfdSessVcId
                    Unsigned32,
                hwBfdSessVsiName
                    OCTET STRING,
                hwBfdSessVsiPeerAddr
                    IpAddress,
                hwBfdSessDiscrAuto
                    EnabledStatus,
                hwBfdSessPeerIpv6Addr
                    Ipv6Address,
                hwBfdSessSourceIpv6Addr
                    Ipv6Address,
                hwBfdSessIpv6NextHop
                    Ipv6Address,
                hwBfdSessIsIPv6Addr
                    TruthValue,
                hwBfdSessMeticulous
                    EnabledStatus,
                hwBfdSessLooseAuthentication
                    TruthValue,
                hwBfdSessAuthenticationStatus
                    Integer32,
                hwBfdSessOneArmEcho
                    EnabledStatus,
                hwBfdSessPWTtlMode
                    INTEGER,
                hwBfdSessPWTtl
                    Integer32,
                hwBfdSessRemotePeerIpType
                    InetAddressType,
                hwBfdSessRemotePeerIp
                    InetAddress,
                hwBfdSessSelectBoard
                    DisplayString,
                hwBfdSessPWSPE
                    INTEGER,
                hwBfdSessPWTrackIfName
                    DisplayString,
                hwBfdSessIsPWTrackIf
                    EnabledStatus,
                hwBfdSessEncapsulationType
                    DisplayString,
                hwBfdSessPEVid
                    Unsigned32,
                hwBfdSessCEVid
                    Unsigned32,
                hwBfdSessPeerInetAddrType
                    InetAddressType,
                hwBfdSessPeerInetAddr
                    InetAddress,
                hwBfdSessInetNextHopType
                    InetAddressType,
                hwBfdSessInetNextHop
                    InetAddress,
                hwBfdSessBindAppTypeMask
                    OCTET STRING,
                hwBfdSessDscp
                    Integer32,
                hwBfdSessPWId
                    Unsigned32
             }

        hwBfdSessIndex OBJECT-TYPE
            SYNTAX Unsigned32 (1..4294967295)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "It is unique and the Index of this session.
                 This index is automatically allocated inside the system
                 and is not user-configurable.
                "
            ::= { hwBfdSessionEntry 1 }


        hwBfdSessMIndex OBJECT-TYPE
            SYNTAX Unsigned32 (1..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This value indicate the configuration has Main Index."
            ::= { hwBfdSessionEntry 2 }


        hwBfdSessBindVRRP OBJECT-TYPE
            SYNTAX Integer32 (0..1)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Describe the capability of bound with VRRP for the BFD session.
                 Options:
                 1. notBind(0) -not bind
                 2. bind(1)    -bind
                "
            ::= { hwBfdSessionEntry 3 }


        hwBfdSessCfgName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..15))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This indicate the name of the session which
                 will be display course information or statistic
                 information of the session.
                "
            ::= { hwBfdSessionEntry 4 }


        hwBfdSessPeerAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Define the peer IP address of the BFD session."
            ::= { hwBfdSessionEntry 5 }


        hwBfdSessBindIfIndex OBJECT-TYPE
            SYNTAX Integer32 (0..2147483647)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the index of the binding interface in the BFD session"
            ::= { hwBfdSessionEntry 6 }


        hwBfdSessBindIfName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the name of the binding interface in the BFD session."
            ::= { hwBfdSessionEntry 7 }


        hwBfdSessLocalDiscr OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "A unique, nonzero discriminator value generated by the
                 transmitting system, used to demultiplex multiple BFD
                 sessions between the same pair of system.
                "
            ::= { hwBfdSessionEntry 8 }


        hwBfdSessRemoteDiscr OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The discriminator received from the corresponding remote
                 system. This field reflects back the received value of My
                 Discriminator, or is zero if that value is unknown.
                "
            ::= { hwBfdSessionEntry 9 }


        hwBfdSessOperMode OBJECT-TYPE
            SYNTAX Integer32 (0..4)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Describe the current operating mode configured with the BFD session.
                 Options:
                 1. 0 -asynchronous mode with echo function
                 2. 1 -asynchronous mode without echo function
                 3. 2 -demand mode with echo function
                 4. 3 -demand mode without echo function
                 5. 4 -asynchronous One-arm-echo mode
                "
            ::= { hwBfdSessionEntry 10 }


        hwBfdSessDetectMult OBJECT-TYPE
            SYNTAX Unsigned32 (3..50)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Detect time multiplier. The negotiated transmit interval,
                 multiplied by this value, provides the detection time for
                 the transmitting system in Asynchronous mode.
                 Default: 3
                "
            ::= { hwBfdSessionEntry 11 }


        hwBfdSessDemandTimerInterval OBJECT-TYPE
            SYNTAX BfdInterval
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the detecting interval in the BFD session with the demand mode.
                 Unit: millisecond
                "
            ::= { hwBfdSessionEntry 12 }


        hwBfdSessActualRxInterval OBJECT-TYPE
            SYNTAX BfdInterval
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This is the minimum interval, in milliseconds, between
                 received BFD Control packets that this system is capable
                 of supporting.
                 Unit: millisecond
                "
            ::= { hwBfdSessionEntry 13 }


        hwBfdSessActualTxInterval OBJECT-TYPE
            SYNTAX BfdInterval
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This is the minimum interval, in milliseconds, that the
                 local system would like to use when transmitting BFD
                 Control packets.
                 Unit: millisecond
                "
            ::= { hwBfdSessionEntry 14 }


        hwBfdSessWTRInterval OBJECT-TYPE
            SYNTAX Integer32 (0..60)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The WTR interval of the BFD session.
                 Unit: minute
                "
            ::= { hwBfdSessionEntry 15 }


        hwBfdSessTOS OBJECT-TYPE
            SYNTAX Integer32 (0..7)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This is the TOS value of bfd packet."
            ::= { hwBfdSessionEntry 16 }


        hwBfdSessState OBJECT-TYPE
            SYNTAX Integer32 (0..3)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Describe the current state of the BFD session.
                 Options:
                 1. 0 -admin down
                 2. 1 -down
                 3. 2 -init
                 4. 3 -up
                "
            ::= { hwBfdSessionEntry 17 }


        hwBfdSessDiag OBJECT-TYPE
            SYNTAX Integer32 (0..31)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "A diagnostic code specifying the local system's reason for
                 the last session state change.
                 Options:
                 1. 0      -no diagnostic
                 2. 1      -control detection time expired
                 3. 2      -echo function failed
                 4. 3      -neighbor signaled session down
                 5. 4      -forwarding plane reset
                 6. 5      -path down
                 7. 6      -concatenated path down
                 8. 7      -administratively down
                 9. 8      -reverse concatenated path down
                 10. 9     -neighbor signaled session down (receive admindown)
                 11. 10-31 -reserved for future use
                "
            ::= { hwBfdSessionEntry 18 }


        hwBfdSessSourceAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The source address of the session."
            ::= { hwBfdSessionEntry 19 }


        hwBfdSessVrfIndex OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The index of the VPN interface."
            ::= { hwBfdSessionEntry 20 }


        hwBfdSessVPNName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..31))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The name of VPN interface."
            ::= { hwBfdSessionEntry 21 }


        hwBfdSessType OBJECT-TYPE
            SYNTAX INTEGER
                {
                static(1),
                dynamic(2),
                entireDynamic(3),
                auto(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The type of the BFD session.
                 Options:
                 1. static(1)        -static
                 2. dynamic(2)       -dynamic
                 3. entireDynamic(3) -entire dynamic
                 4. auto(4)          -auto
                "
            ::= { hwBfdSessionEntry 22 }


--   other or unknown
        hwBfdSessBindAppType OBJECT-TYPE
            SYNTAX INTEGER
                {
                noApplication(1),
                vrrp(2),
                ifnet(3),
                vrrpAndIfnet(4),
                bgp(5),
                ospf(6),
                bgpAndOspf(7),
                oamLspmL2vpn(8),
                oamTnlL2vpn(9),
                lspmL2vpnTnlps(10),
                oamMplsfwL2vpn(11),
                isis(12),
                vsiPw(13),
                vrrpOamLspmL2vpn(14),
                vrrpOamTnlL2vpn(15),
                vrrpLspmL2vpnTnlps(16),
                vrrpOamMplsfwL2vpn(17),
                pim(18),
                bgpIsis(19),
                bgpPim(20),
                ospfIsis(21),
                ospfPim(22),
                isisPim(23),
                bgpOspfIsis(24),
                bgpOspfPim(25),
                bgpIsisPim(26),
                ospfIsisPim(27),
                bgpOspfIsisPim(28),
                bgp6(29),
                ospfv3(30),
                isis6(31),
                pim6(32),
                bgp6Ospfv3(33),
                bgp6Isis6(34),
                bgp6Pim6(35),
                ospfv3Isis6(36),
                ospfv3Pim6(37),
                isis6Pim6(38),
                bgp6Ospfv3Isis6(39),
                bgp6Ospfv3Pim6(40),
                bgp6Isis6Pim6(41),
                ospfv3Isis6Pim6(42),
                bgp6Ospfv3Isis6Pim6(43),
                auto(44),
                autoIsis(45),
                autoOspf(46),
                autoBgp(47),
                autoPim(48),
                autoIsisOspf(49),
                autoIsisBgp(50),
                autoIsisPim(51),
                autoOspfBgp(52),
                autoOspfPim(53),
                autoBgpPim(54),
                autoIsisOspfBgp(55),
                autoIsisOspfBgpPim(56),
                autoIsis6(57),
                autoOspfv3(58),
                autoBgp6(59),
                autoPim6(60),
                autoIsis6Ospfv3(61),
                autoIsis6Bgp6(62),
                autoIsis6Pim6(63),
                autoOspfv3Bgp6(64),
                autoOspfv3Pim6(65),
                autoBgp6Pim6(66),
                autoIsis6Ospfv3Bgp6(67),
                autoIsis6Ospfv3Bgp6Pim6(68),
                etrunk(69),
                etrunkIfnet(70),
                etrunkVrrp(71),
                etrunkVrrpIfnet(72),
                etrunkOamLspmL2vpn(73),
                etrunkOamTnlL2vpn(74),
                etrunkLspmL2vpnTnlps(75),
                etrunkOamMplsfwL2vpn(76),
                etrunkvsiPw(77),
                etrunkOamLspmL2vpnVrrp(78),
                etrunkOamTnlL2vpnVrrp(79),
                etrunkLspmL2vpnTnlpsVrrp(80),
                etrunkOamMplsfwL2vpnVrrp(81),
                rip(82),
                bgpRip(83),
                ospfRip(84),
                isisRip(85),
                pimRip(86),
                bgpOspfRip(87),
                bgpIsisRip(88),
                bgpPimRip(89),
                ospfIsisRip(90),
                ospfPimRip(91),
                isisPimRip(92),
                bgpOspfIsisRip(93),
                bgpOspfPimRip(94),
                ospfIsisPimRip(95),
                autoRip(96),
                autoBgpRip(97),
                autoOspfRip(98),
                autoIsisRip(99),
                autoPimRip(100),
                autoBgpOspfRip(101),
                autoBgpIsisRip(102),
                autoBgpPimRip(103),
                autoOspfIsisRip(104),
                autoOspfPimRip(105),
                autoIsisPimRip(106),
                autoBgpOspfIsisRip(107),
                autoBgpOspfPimRip(108),
                autoOspfIsisPimRip(109),
                autoIsisOspfBgpPimVrrp(110),
                autoIsisOspfPimVrrp(111),
                autoIsisOspfBgpVrrp(112),
                autoIsisBgpPimVrrp(113),
                autoOspfBgpPimVrrp(114),
                autoIsisOspfVrrp(115),
                autoIsisBgpVrrp(116),
                autoOspfBgpVrrp(117),
                autoIsisPimVrrp(118),
                autoOspfPimVrrp(119),
                autoBgpPimVrrp(120),
                autoIsisVrrp(121),
                autoOspfVrrp(122),
                autoBgpVrrp(123),
                autoPimVrrp(124),
                autoVrrp(125),
                autoVrrpBgp6(126),
                autoOspfv3Isis6Pim6(127),
                autoOspfBgpPim(128),
                autoIsisOspfPim(129),
                autoIsisPimBgp(130),
                bgpOspfIsisPimRip(131),
                autoBgpOspfIsisPimRip(132),
                bgpRsvp(133),
                ospfRsvp(134),
                isisRsvp(135),
                pimRsvp(136),
                ripRsvp(137),              
                bgpOspfRsvp(138),
                bgpIsisRsvp(139),
                bgpPimRsvp(140),
                bgpRipRsvp(141),
                ospfIsisRsvp(142),
                ospfPimRsvp(143),
                ospfRipRsvp(144),
                isisPimRsvp(145),
                isisRipRsvp(146),
                pimRipRsvp(147),
                bgpOspfIsisRsvp(148),
                bgpOspfPimRsvp(149),
                bgpOspfRipRsvp(150),
                bgpIsisPimRsvp(151),
                bgpIsisRipRsvp(152),
                bgpPimRipRsvp(153),     
                ospfIsisPimRsvp(154),
                ospfIsisRipRsvp(155),
                isisPimRipRsvp(156),       
                bgpOspfIsisPimRsvp(157),
                bgpOspfIsisRipRSvp(158),
                bgpOspfPimRipRsvp(159),
                bgpIsisPimRipRsvp(160),
                ospfIsisPimRipRsvp(161),
                bgpOspfIsisPimRipRsvp(162),                            
                autoRsvp(163),
                autoBgpRsvp(164),
                autoOspfRsvp(165),
                autoIsisRsvp(166),
                autoPimRsvp(167),
                autoRipRsvp(168),              
                autoBgpOspfRsvp(169),
                autoBgpIsisRsvp(170),
                autoBgpPimRsvp(171),
                autoBgpRipRsvp(172),
                autoOspfIsisRsvp(173),
                autoOspfPimRsvp(174),
                autoOspfRipRsvp(175),
                autoIsisPimRsvp(176),
                autoIsisRipRsvp(177),
                autoPimRipRsvp(178),              
                autoBgpOspfIsisRsvp(179),
                autoBgpOspfPimRsvp(180),
                autoBgpOspfRipRsvp(181),
                autoOspfIsisPimRsvp(182),
                autoOspfIsisRipRsvp(183),
                autoIsisPimRipRsvp(184),
                autoBgpOspfIsisPimRsvp(185),
                autoBgpOspfIsisRipRsvp(186),
                autoOspfIsisPimRipRsvp(187),
                rsvp(188)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Application type that this BFD session has been bound to
                 Options:
                 1. noApplication(1)              -No application
                 2. vrrp(2)                       -VRRP
                 3. ifnet(3)                      -IFNET
                 4. vrrpAndIfnet(4)               -VRRP&IFNET
                 5. bgp(5)                        -BGP
                 6. ospf(6)                       -OSPF
                 7. bgpAndOspf(7)                 -BGP&OSPF
                 8. oamLspmL2vpn(8)               -OAM&LSPM&L2VPN (for LDP LSP and static LSP)
                 9. oamTnlL2vpn(9)                -OAM&TUNNEL&L2VPN (for TE_Tunnnel)
                 10. lspmL2vpnTnlps(10)           -LSPM&TUNNEL_PS&L2VPN (for TE_LSP)
                 11. oamMplsfwL2vpn(11)           -OAM&MPLSFW&L2VPN (for PW)
                 12. isis(12)                     -ISIS
                 13. vsiPw(13)                    -VSIPW (for VSI PW)
                 14. vrrpOamLspmL2vpn(14)         -VRRP&OAM&LSPM&L2VPN
                 15. vrrpOamTnlL2vpn(15)          -VRRP&OAM&TUNNEL&L2VPN
                 16. vrrpLspmL2vpnTnlps(16)       -VRRP&LSPM&TUNNEL_PS&L2VPN
                 17. vrrpOamMplsfwL2vpn(17)       -VRRP&OAM&MPLSFW&L2VPN
                 18. pim(18)                      -PIM
                 19. bgpIsis(19)                  -BGP&ISIS
                 20. bgpPim(20)                   -BGP&PIM
                 21. ospfIsis(21)                 -OSPF&ISIS
                 22. ospfPim(22)                  -OSPF&PIM
                 23. isisPim(23)                  -ISIS&PIM
                 24. bgpOspfIsis(24)              -BGP&OSPF&ISIS
                 25. bgpOspfPim(25)               -BGP&OSPF&PIM
                 26. bgpIsisPim(26)               -BGP&ISIS&PIM
                 27. ospfIsisPim(27)              -OSPF&ISIS&PIM
                 28. bgpOspfIsisPim(28)           -BGPOSPF&ISIS&PIM
                 29. bgp6(29)                     -BGP6
                 30. ospfv3(30)                   -OSPFV3
                 31. isis6(31)                    -ISIS6
                 32. pim6(32)                     -PIM6
                 33. bgp6Ospfv3(33)               -BGP6&OSPFV3
                 34. bgp6Isis6(34)                -BGP6&ISIS6
                 35. bgp6Pim6(35)                 -BGP6&PIM6
                 36. ospfv3Isis6(36)              -OSPFV3&ISIS6
                 37. ospfv3Pim6(37)               -OSPFV3&PIM6
                 38. isis6Pim6(38)                -ISIS6&PIM6
                 39. bgp6Ospfv3Isis6(39)          -BGP6&OSPFV3&ISIS6
                 40. bgp6Ospfv3Pim6(40)           -BGP6&OSPFV3&PIM6
                 41. bgp6Isis6Pim6(41)            -BGP6&ISIS6&PIM6
                 42. ospfv3Isis6Pim6(42)          -OSPFV3&ISIS6&PIM6
                 43. bgp6Ospfv3Isis6Pim6(43)      -BGP6&OSPFV3&ISIS6&PIM6
                 44. auto(44)                     -AUTO
                 45. autoIsis(45)                 -AUTO&ISIS
                 46. autoOspf(46)                 -AUTO&OSPF
                 47. autoBgp(47)                  -AUTO&BGP
                 48. autoPim(48)                  -AUTO&PIM
                 49. autoIsisOspf(49)             -AUTO&ISIS&OSPF
                 50. autoIsisBgp(50)              -AUTO&ISIS&BGP
                 51. autoIsisPim(51)              -AUTO&ISIS&PIM
                 52. autoOspfBgp(52)              -AUTO&OSPF&BGP
                 53. autoOspfPim(53)              -AUTO&OSPF&PIM
                 54. autoBgpPim(54)               -AUTO&BGP&PIM
                 55. autoIsisOspfBgp(55)          -AUTO&ISIS&OSPF&BGP
                 56. autoIsisOspfBgpPim(56)       -AUTO&ISIS&OSPF&BGP&PIM
                 57. autoIsis6(57)                -AUTO&ISIS6
                 58. autoOspfv3(58)               -AUTO&OSPFV3
                 59. autoBgp6(59)                 -AUTO&BGP6
                 60. autoPim6(60)                 -AUTO&PIM6
                 61. autoIsis6Ospfv3(61)          -AUTO&ISIS6&OSPFV3
                 62. autoIsis6Bgp6(62)            -AUTO&ISIS6&BGP6
                 63. autoIsis6Pim6(63)            -AUTO&ISIS6&PIM6
                 64. autoOspfv3Bgp6(64)           -AUTO&OSPFV3&BGP6)
                 65. autoOspfv3Pim6(65)           -AUTO&OSPFV3&PIM6)
                 66. autoBgp6Pim6(66)             -AUTO&BGP6&PIM6
                 67. autoIsis6Ospfv3Bgp6(67)      -AUTO&ISIS6&OSPFV3&BGP6
                 68. autoIsis6Ospfv3Bgp6Pim6(68)  -AUTO&ISIS6&OSPFV3&BGP6&PIM6
                 69. etrunk(69)                   -ETRUNK
                 70. etrunkIfnet(70)              -ETRUNK&IFNET
                 71. etrunkVrrp(71)               -ETRUNK&VRRP
                 72. etrunkVrrpIfnet(72)          -ETRUNK&VRRP&IFNET
                 73. etrunkOamLspmL2vpn(73)       -ETRUNK&OAM&LSPM&L2VPN
                 74. etrunkOamTnlL2vpn(74)        -ETRUNK&OAM&TNL&L2VPN
                 75. etrunkLspmL2vpnTnlps(75)     -ETRUNK&LSPM&L2VPN&TNLPS
                 76. etrunkOamMplsfwL2vpn(76)     -ETRUNK&OAM&MPLSFW&L2VPN
                 77. etrunkvsiPw(77)              -ETRUNK&VSIPW
                 78. etrunkOamLspmL2vpnVrrp(78)   -ETRUNK&OAM&LSPM&L2VPN&VRRP
                 79. etrunkOamTnlL2vpnVrrp(79)    -ETRUNK&OAM&TNL&L2VPN&VRRP
                 80. etrunkLspmL2vpnTnlpsVrrp(80) -ETRUNK&LSMP&L2VPN&TNLPS&VRRP
                 81. etrunkOamMplsfwL2vpnVrrp(81) -ETRUNK&OAM&MPLSFW&L2VPN&VRRP
                 82. rip(82)                      -RIP
                 83. bgpRip(83)                   -BGP&RIP
                 84. ospfRip(84)                  -OSPF&RIP
                 85. isisRip(85)                  -ISIS&RIP
                 86. pimRip(86)                   -PIM&RIP
                 87. bgpOspfRip(87)               -BGP&OSPF&RIP
                 88. bgpIsisRip(88)               -BGP&ISIS&RIP
                 89. bgpPimRip(89)                -BGP&PIM&RIP
                 90. ospfIsisRip(90)              -OSPF&ISIS&RIP
                 91. ospfPimRip(91)               -OSPF&PIM&RIP
                 92. isisPimRip(92)               -ISIS&PIM&RIP
                 93. bgpOspfIsisRip(93)           -BGP&OSPF&ISIS&RIP
                 94. bgpOspfPimRip(94)            -BGP&OSPF&PIM&RIP
                 95. ospfIsisPimRip(95)           -OSPF&ISIS&PIM&RIP
                 96. autoRip(96)                  -AUTO&RIP
                 97. autoBgpRip(97)               -AUTO&BGP&RIP
                 98. autoOspfRip(98)              -AUTO&OSPF&RIP
                 99. autoIsisRip(99)              -AUTO&ISIS&RIP
                 100. autoPimRip(100)             -AUTO&PIM&RIP
                 101. autoBgpOspfRip(101)         -AUTO&BGP&OSPF&RIP
                 102. autoBgpIsisRip(102)         -AUTO&BGP&ISIS&RIP
                 103. autoBgpPimRip(103)          -AUTO&BGP&PIM&RIP
                 104. autoOspfIsisRip(104)        -AUTO&OSPF&ISIS&RIP
                 105. autoOspfPimRip(105)         -AUTO&OSPF&PIM&RIP
                 106. autoIsisPimRip(106)         -AUTO&ISIS&PIM&RIP
                 107. autoBgpOspfIsisRip(107)     -AUTO&BGP&OSPF&ISIS&RIP
                 108. autoBgpOspfPimRip(108)      -AUTO&BGP&OSPF&PIM&RIP
                 109. autoOspfIsisPimRip(109)     -AUTO&OSPF&ISIS&PIM&RIP
                 110. autoIsisOspfBgpPimVrrp(110) -AUTO&ISIS&OSPF&BGP&PIM&VRRP
                 111. autoIsisOspfPimVrrp(111)    -AUTO&ISIS&OSPF&PIM&VRRP
                 112. autoIsisOspfBgpVrrp(112)    -AUTO&ISIS&OSPF&BGP&VRRP
                 113. autoIsisBgpPimVrrp(113)     -AUTO&ISIS&BGP&PIM&VRRP
                 114. autoOspfBgpPimVrrp(114)     -AUTO&OSPF&BGP&PIM&VRRP
                 115. autoIsisOspfVrrp(115)       -AUTO&ISIS&OSPF&VRRP
                 116. autoIsisBgpVrrp(116)        -AUTO&ISIS&BGP&VRRP
                 117. autoOspfBgpVrrp(117)        -AUTO&OSPF&BGP&VRRP
                 118. autoIsisPimVrrp(118)        -AUTO&ISIS&PIM&VRRP
                 119. autoOspfPimVrrp(119)        -AUTO&OSPF&PIM&VRRP
                 120. autoBgpPimVrrp(120)         -AUTO&BGP&PIM&VRRP
                 121. autoIsisVrrp(121)           -AUTO&ISIS&VRRP
                 122. autoOspfVrrp(122)           -AUTO&OSPF&VRRP
                 123. autoBgpVrrp(123)            -AUTO&BGP&VRRP
                 124. autoPimVrrp(124)            -AUTO&PIM&VRRP
                 125. autoVrrp(125)               -AUTO&VRRP
                 126. autoVrrpBgp6(126)           -AUTO&VRRP&BGP6
                 127. autoOspfv3Isis6Pim6(127)    -AUTO&OSPFV3&ISIS6&PIM6
                 128. autoOspfBgpPim(128)         -AUTO&OSPF&BGP&PIM
                 129. autoIsisOspfPim(129)        -AUTO&ISIS&OSPF&PIM
                 130. autoIsisPimBgp(130)         -AUTO&ISIS&BGP&PIM
                 131. bgpOspfIsisPimRip(131)      -BGP&OSPF&ISIS&PIM&RIP
                 132. autoBgpOspfIsisPimRip(132)  -AUTO&BGP&OSPF&ISIS&PIM&RIP
                 133. bgpRsvp(133)                -BGP&RSVP
                 134. ospfRsvp(134)               -OSPF&RSVP
                 135. isisRsvp(135)               -ISIS&RSVP
                 136. pimRsvp(136)                -PIM&RSVP
                 137. ripRsvp(137)                -RIP&RSVP          
                 138. bgpOspfRsvp(138)            -BGP&OSPF&RSVP
                 139. bgpIsisRsvp(139)            -BGP&ISIS&RSVP
                 140. bgpPimRsvp(140)             -BGP&PIM&RSVP
                 141. bgpRipRsvp(141)             -BGP&RIP&RSVP
                 142. ospfIsisRsvp(142)           -OSPF&ISIS&RSVP
                 143. ospfPimRsvp(143)            -OSPF&PIM&RSVP
                 144. ospfRipRsvp(144)            -OSPF&RIP&RSVP
                 145. isisPimRsvp(145)            -ISIS&PIM&RSVP
                 146. isisRipRsvp(146)            -ISIS&RIP&RSVP
                 147. pimRipRsvp(147)             -PIM&RIP&RSVP
                 148. bgpOspfIsisRsvp(148)        -BGP&OSPF&ISIS&RSVP
                 149. bgpOspfPimRsvp(149)         -BGP&OSPF&PIM&RSVP
                 150. bgpOspfRipRsvp(150)         -BGP&OSPF&RIP&RSVP
                 151. bgpIsisPimRsvp(151)         -BGP&ISIS&PIM&RSVP
                 152. bgpIsisRipRsvp(152)         -BGP&ISIS&RIP&RSVP
                 153. bgpPimRipRsvp(153)          -BGP&PIM&RIP&RSVP
                 154. ospfIsisPimRsvp(154)        -OSPF&ISIS&PIM&RSVP
                 155. ospfIsisRipRsvp(155)        -OSPF&ISIS&RIP&RSVP
                 156. isisPimRipRsvp(156)         -ISIS&PIM&RIP&RSVP
                 157. bgpOspfIsisPimRsvp(157)     -BGP&OSPF&ISIS&PIM&RSVP
                 158. bgpOspfIsisRipRSvp(158)     -BGP&OSPF&ISIS&RIP&RSVP
                 159. bgpOspfPimRipRsvp(159)      -BGP&OSPF&PIM&RIP&RSVP
                 160. bgpIsisPimRipRsvp(160)      -BGP&ISIS&PIM&RIP&RSVP
                 161. ospfIsisPimRipRsvp(161)     -OSPF&ISIS&PIM&RIP&RSVP
                 162. bgpOspfIsisPimRipRsvp(162)  -BGP&OSPF&ISIS&PIM&RIP&RSVP       
                 163. autoRsvp(163)               -AUTO&RSVP
                 164. autoBgpRsvp(164)            -AUTO&BGP&RSVP
                 165. autoOspfRsvp(165)           -AUTO&OSPF&RSVP
                 166. autoIsisRsvp(166)           -AUTO&ISIS&RSVP
                 167. autoPimRsvp(167)            -AUTO&PIM&RSVP
                 168. autoRipRsvp(168)            -AUTO&RIP&RSVP
                 169. autoBgpOspfRsvp(169)        -AUTO&BGP&OSPF&RSVP
                 170. autoBgpIsisRsvp(170)        -AUTO&BGP&ISIS&RSVP
                 171. autoBgpPimRsvp(171)         -AUTO&BGP&PIM&RSVP
                 172. autoBgpRipRsvp(172)         -AUTO&BGP&RIP&RSVP
                 173. autoOspfIsisRsvp(173)       -AUTO&OSPF&ISIS&RSVP
                 174. autoOspfPimRsvp(174)        -AUTO&OSPF&PIM&RSVP
                 175. autoOspfRipRsvp(175)        -AUTO&OSPF&RIP&RSVP
                 176. autoIsisPimRsvp(176)        -AUTO&ISIS&PIM&RSVP
                 177. autoIsisRipRsvp(177)        -AUTO&ISIS&RIP&RSVP
                 178. autoPimRipRsvp(178)         -AUTO&PIM&RIP&RAVP
                 179. autoBgpOspfIsisRsvp(179)    -AUTO&BGP&OSPF&ISIS&RSVP
                 180. autoBgpOspfPimRsvp(180)     -AUTO&BGP&OSPF&PIM&RSVP
                 181. autoBgpOspfRipRsvp(181)     -AUTO&BGP&OSPF&RIP&RSVP
                 182. autoOspfIsisPimRsvp(182)    -AUTO&OSPF&ISIS&PIM&RSVP
                 183. autoOspfIsisRipRsvp(183)    -AUTO&OSPF&ISIS&RIP&RSVP
                 184. autoIsisPimRipRsvp(184)     -AUTO&ISIS&PIM&RIP&RSVP
                 185. autoBgpOspfIsisPimRsvp(185) -AUTO&BGP&OSPF&ISIS&PIM&RSVP
                 186. autoBgpOspfIsisRipRsvp(186) -AUTO&BGP&OSPF&ISIS&RIP&RSVP
                 187. autoOspfIsisPimRipRsvp(187) -AUTO&OSPF&ISIS&PIM&RIP&RSVP
                 188. rsvp(188)                   -RSVP
                "
            ::= { hwBfdSessionEntry 23 }


        hwBfdSessDefaultIp OBJECT-TYPE
            SYNTAX INTEGER
                {
                no(1),
                yes(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "BFD session use default multicast IP as the detect peer-ip
                 Options:
                 1. no(1)  -do not use the default multicast IP
                 2. yes(2) -use the default multicast IP
                "
            ::= { hwBfdSessionEntry 24 }


        hwBfdSessPISFlag OBJECT-TYPE
            SYNTAX INTEGER
                {
                false(1),
                true(2),
                subif(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The state of BFD session is associated with the state of the binding interface
                 Options:
                 1. false(1) -do not associate with interface state
                 2. true(2)  -ssociate with interface state
                 3. subif(3) -associate with interface and correlative sub interface
                "
            ::= { hwBfdSessionEntry 25 }


        hwBfdSessBindType OBJECT-TYPE
            SYNTAX INTEGER
                {
                interfaceIp(1),
                peerIp(2),
                sourceIp(3),
                ifAndSourceIp(4),
                fec(5),
                tunnelIf(6),
                ospf(7),
                isis(8),
                ldpLsp(9),
                staticLsp(10),
                teLsp(11),
                teTunnel(12),
                pw(13),
                vsiPw(15),
                ldpTunnel(21),
                bgpTunnel(22)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The binding type of the BFD session.
                 Options:
                 1. interfaceIp(1)   -BFD for IP with peer-ip and interface
                 2. peerIp(2)        -BFD for IP only with peer-ip
                 3. sourceIp(3)      -BFD for IP with peer-ip and source-ip
                 4. ifAndSourceIp(4) -BFD for IP with peer-ip, interface and source-ip
                 5. fec(5)           -BFD for FEC(NOT support now)
                 6. tunnelIf(6)      -BFD for Tunnel interface(NOT support now)
                 7. ospf(7)          -BFD for OSPF
                 8. isis(8)          -BFD for ISIS
                 9. ldpLsp(9)        -BFD for LDP-LSP
                 10. staticLsp(10)   -BFD for static LSP
                 11. teLsp(11)       -BFD for TE-LSP
                 12. teTunnel(12)    -BFD for TE-Tunnel
                 13. pw(13)          -BFD for PW;
                 14. vsiPw(15)       -BFD for VSI PW
                 15. ldpTunnel(21)   -BFD for LDP-Tunnel
                 16. bgpTunnel(22)   -BFD for BGP-Tunnel
                "
            ::= { hwBfdSessionEntry 26 }


        hwBfdSessNextHop OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the next hop of the BFD session."
            ::= { hwBfdSessionEntry 27 }


        hwBfdSessStaticLspName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..20))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the static LSP name of the BFD session."
            ::= { hwBfdSessionEntry 28 }


        hwBfdSessLspIndex OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the index of the static LSP or LDP LSP in BFD session, mapping the channel index in MPLS network."
            ::= { hwBfdSessionEntry 29 }


        hwBfdSessPWSecondaryFlag OBJECT-TYPE
            SYNTAX INTEGER
                {
                flagMasterPW(1),
                flagSecondaryPW(2),
                flagNoPW(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The role of the PW bound with BFD session.
                 Options:
                 1. flagMasterPW(1)    -master PW
                 2. flagSecondaryPW(2) -secondary PW
                 3. flagNoPW(3)        -no PW
                 Default: 1
                "
            ::= { hwBfdSessionEntry 30 }


        hwBfdSessTunnelDetectType OBJECT-TYPE
            SYNTAX INTEGER
                {
                flagBothDown(1),
                flagNeighborDown(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Set the failure notifies policy type.
                 Options:
                 1. flagBothDown(1)     -notify applications when detecting both Detect-Down and Neighbor-Down
                 2. flagNeighborDown(2) -notify applications only when detecting Neighbor-Down
                 Default: 1
                "
            ::= { hwBfdSessionEntry 31 }


        hwBfdSessVcId OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the ID of VC."
            ::= { hwBfdSessionEntry 32 }


        hwBfdSessVsiName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..31))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the name of VSI."
            ::= { hwBfdSessionEntry 33 }


        hwBfdSessVsiPeerAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the peer-ip of VSI."
            ::= { hwBfdSessionEntry 34 }

        hwBfdSessDiscrAuto OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Describe whether the discriminator can be auto allocated.
                 Options:
                 1. enabled(1)   -the discriminator can be allocated automatically
                 2. disabled(2)  -the discriminator can not be allocated automatically
                 Default: disabled
                "
            ::= { hwBfdSessionEntry 35 }

        hwBfdSessPeerIpv6Addr OBJECT-TYPE
            SYNTAX Ipv6Address
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Define the peer IPv6 address of the BFD session."
            ::= { hwBfdSessionEntry 36 }

        hwBfdSessSourceIpv6Addr OBJECT-TYPE
            SYNTAX Ipv6Address
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Define the source IPv6 address of the BFD session."
            ::= { hwBfdSessionEntry 37 }

        hwBfdSessIpv6NextHop OBJECT-TYPE
            SYNTAX Ipv6Address
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the next hop of the BFD session."
            ::= { hwBfdSessionEntry 38 }

        hwBfdSessIsIPv6Addr OBJECT-TYPE
            SYNTAX TruthValue
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Whether the peer address of the BFD session is IPv6 address.
                 Default: false
                "
            ::= { hwBfdSessionEntry 39 }

        hwBfdSessMeticulous OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Whether enable meticulous authentication for MD5 or SHA-1 type.
                 Options:
                 1. enabled(1)  -enable meticulous authentication for MD5 or SHA-1 type
                 2. disabled(2) -disabled meticulous authentication for MD5 or SHA-1 type
                 Default: 2
                "
            ::= { hwBfdSessionEntry 40 }

        hwBfdSessLooseAuthentication OBJECT-TYPE
            SYNTAX TruthValue
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Whether loose authentication check.
                 Options:
                 1. True(1)  -loose-check
                 2. False(2) -do not loose-check
                 Default: false
                "
            ::= { hwBfdSessionEntry 41 }

        hwBfdSessAuthenticationStatus OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Authentication status of the bfd session
                 Options:
                 1. 0       -authentication disable
                 2. 1       -interface board do not support bfd authentication
                 3. 2       -keychain does not exist
                 4. 3       -auth BFD session number exceed
                 5. 4       -authentication in operation normally
                 100. 100   -exception
                 Default: 0
                "
            ::= { hwBfdSessionEntry 42 }

        hwBfdSessOneArmEcho OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies whether a session works in one-arm-echo mode.
                 Options:
                 1. enabled(1)  -indicates that the session works in one-arm-echo mode
                 2. disabled(2) -indicates that the session does not work in one-arm-echo mode
                 Default: disabled
                "
            ::= { hwBfdSessionEntry 43 }

        hwBfdSessPWTtlMode OBJECT-TYPE
            SYNTAX INTEGER
                {
                config(1),
                auto(2),
                default(3),
                nottl(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the configuration mode of a TTL used by
                 the BFD session for PW.
                 Options:
                 1. config(1)   -indicates that the TTL is manually set
                 2. auto(2)     -indicates that the TTL is automatically calculated based on an IP address
                 3. default(3)  -indicates that the TTL is 255 by default
                 4. nottl(4)    -indicates that the TTL is not in PW mode
                "
            ::= { hwBfdSessionEntry 44 }

        hwBfdSessPWTtl OBJECT-TYPE
            SYNTAX Integer32 (0..255)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the TTL used by the BFD session for PW."
            ::= { hwBfdSessionEntry 45 }

        hwBfdSessRemotePeerIpType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the type of the destination address of the BFD
                 session for PW.
                "
            ::= { hwBfdSessionEntry 46 }

        hwBfdSessRemotePeerIp OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the destination IP address of the BFD session
                 for PW.
                "
            ::= { hwBfdSessionEntry 47 }

        hwBfdSessSelectBoard OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..47))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the main processing board of a BFD session."
            ::= { hwBfdSessionEntry 48 }

        hwBfdSessPWSPE OBJECT-TYPE
            SYNTAX INTEGER
            {
            upe(1),
            spe(2),
            none(3)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the node on which a BFD session is set up.
                 The values are as follows.
                 Options:
                 1. upe(1)  -indicates that a BFD session is set up on a UPE to detect a PW
                 2. spe(2)  -indicates that a BFD session is set up on an SPE to detect a PW
                 3. none(3) -indicates that a BFD session does not detect a PW
                 Default: none
                "
            ::= { hwBfdSessionEntry 49 }

        hwBfdSessPWTrackIfName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..64))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the interface monitored by the BFD session for PW."
            ::= { hwBfdSessionEntry 50 }

        hwBfdSessIsPWTrackIf OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies whether the BFD session for
                 PW monitors an interface. The values are as follows.
                 Options:
                 1. enabled(1)  -enables the BFD session for PW to monitor the interface
                 2. disabled(2) -disables the BFD session for PW from monitoring the interface
                "
            ::= { hwBfdSessionEntry 51 }

        hwBfdSessEncapsulationType OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..63))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the VC encapsulation type on an SPE.
                 The values are as follows:
                fr
                atm-aal5-sdu
                atm-trans-cell
                vlan
                ethernet
                hdlc
                ppp
                atm-nto1-vcc
                atm-nto1-vpc
                ip-layer2
                atm-1to1-vcc
                atm-1to1-vpc
                atm-aal5-pdu
                satop-e1
                satop-t1
                esopsn-basic
                ip-interworking
                "
            ::= { hwBfdSessionEntry 52 }

        hwBfdSessPEVid OBJECT-TYPE
            SYNTAX Unsigned32 (0..4094)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the outer tag of a sub-interface
                 for QinQ VLAN tag termination or the VLAN ID of a sub-interface for
                 dot1q VLAN tag termination.
                "
            ::= { hwBfdSessionEntry 53 }

        hwBfdSessCEVid OBJECT-TYPE
            SYNTAX Unsigned32 (0..4094)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the inner tag in QinQ packets."
            ::= { hwBfdSessionEntry 54 }

        hwBfdSessPeerInetAddrType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the type of the destination address of the BFD
                 session.
                "
            ::= { hwBfdSessionEntry 55 }

        hwBfdSessPeerInetAddr OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the destination IP address of the BFD session."
            ::= { hwBfdSessionEntry 56 }

        hwBfdSessInetNextHopType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the type of the next hop of the BFD
                 session.
                "
            ::= { hwBfdSessionEntry 57 }

        hwBfdSessInetNextHop OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the next hop of the BFD session."
            ::= { hwBfdSessionEntry 58 }

        hwBfdSessBindAppTypeMask OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "A value which indicates the set of applications that
                 this BFD session binds. Every bit indicates a application.
                 The corresponding bit and applications are as follows: 
                 bit  application
                   0  IFNET
                   1  Route-Management
                   2  OSPF
                   3  ISISL1
                   4  ISISL2
                   5  PIM
                   6  ISISL1L2
                   7  BGP
                   8  VRRP
                   9  LSPM
                  10  RSVP
                  11  LDP
                  12  TE
                  13  Product Private APP
                  14  L2VPN
                  15  OAM_MANAGER
                  16  VTE
                  17  VPW
                  18  MPLSFW
                  19  VGMP
                  20  LSPV
                  21  VSI_PW
                  22  ETHOAM
                  23  AUTO
                  24  E-TRUNK
                  25  OSPFv3
                  26  ISISL1_6
                  27  ISISL2_6
                  28  PIM6
                  29  ISISL1L2_6
                  30  BGP6
                  31  RM6
                  32  RBS
                  33  RIP
                  34  FRP
                  35  BGPLSP
                "
            ::= { hwBfdSessionEntry 59 }

        hwBfdSessDscp OBJECT-TYPE
            SYNTAX Integer32 (0..63 | 255)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This is the dscp value of bfd packet. 
                 255 is invalid value.
                "
            ::= { hwBfdSessionEntry 60 }

        hwBfdSessPWId OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It is the ID of PW."
            ::= { hwBfdSessionEntry 61 }

        hwBfdSessionPerTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBfdSessionPerEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table specifies BFD Session performance counters.
                 The index of this table is hwBfdSessPerIndex.
                "
            ::= { hwBfdObjects 4 }


        hwBfdSessionPerEntry OBJECT-TYPE
            SYNTAX HwBfdSessionPerEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table specifies BFD Session performance counters.
                 The index of this entry is hwBfdSessPerIndex.
                "
            INDEX { hwBfdSessPerIndex }
            ::= { hwBfdSessionPerTable 1 }


        HwBfdSessionPerEntry ::=
            SEQUENCE {
                hwBfdSessPerIndex
                    Unsigned32,
                hwBfdSessPerfPktIn
                    Counter32,
                hwBfdSessPerfPktInHC
                    Counter32,
                hwBfdSessPerfPktOut
                    Counter32,
                hwBfdSessPerfPktOutHC
                    Counter32,
                hwBfdSessPerfBadIn
                    Counter32,
                hwBfdSessPerfBadInHC
                    Counter32,
                hwBfdSessPerfBadOut
                    Counter32,
                hwBfdSessPerfBadOutHC
                    Counter32,
                hwBfdSessPerfLastSessDownTime
                    OCTET STRING,
                hwBfdSessPerfSessDownCount
                    Unsigned32,
                hwBfdSessPerfSessShortBreakCount
                    Unsigned32,
                hwBfdSessionPerStartTime
                    OCTET STRING
             }

        hwBfdSessPerIndex OBJECT-TYPE
            SYNTAX Unsigned32 (1..2147483647)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The index of BFD session statistics.
                 This index is automatically allocated inside the system
                 and is not user-configurable.
                "
            ::= { hwBfdSessionPerEntry 1 }


        hwBfdSessPerfPktIn OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the received Octets in local
                 system in this session.The total received packet number.
                "
            ::= { hwBfdSessionPerEntry 2 }


        hwBfdSessPerfPktInHC OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the received Octets in local
                 system in this session.The high 4 bytes of total received
                 packet number.
                "
            ::= { hwBfdSessionPerEntry 3 }


        hwBfdSessPerfPktOut OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the send Packets in local
                 system in this session.
                "
            ::= { hwBfdSessionPerEntry 4 }


        hwBfdSessPerfPktOutHC OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the send Packets in local
                 system in this session.The high 4 bytes of total send
                 packet number.
                "
            ::= { hwBfdSessionPerEntry 5 }


        hwBfdSessPerfBadIn OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the received Errors in local
                 system in this session.
                "
            ::= { hwBfdSessionPerEntry 6 }


        hwBfdSessPerfBadInHC OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the received Errors in local
                 system in this session.The high 4 bytes of total received wrong
                 packet number.
                "
            ::= { hwBfdSessionPerEntry 7 }


        hwBfdSessPerfBadOut OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the send Errors in local
                 system in this session.
                "
            ::= { hwBfdSessionPerEntry 8 }


        hwBfdSessPerfBadOutHC OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistical information of the send Errors in local
                 system in this session.The high 4 bytes of total send
                 wrong packet number.
                "
            ::= { hwBfdSessionPerEntry 9 }


        hwBfdSessPerfLastSessDownTime OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The time of session last time down."
            ::= { hwBfdSessionPerEntry 10 }


        hwBfdSessPerfSessDownCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total count of session down."
            ::= { hwBfdSessionPerEntry 11 }


        hwBfdSessPerfSessShortBreakCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total count of session shortbreak."
            ::= { hwBfdSessionPerEntry 12 }


        hwBfdSessionPerStartTime OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The time that session start detection."
            ::= { hwBfdSessionPerEntry 13 }


        hwBfdSlotTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBfdSlotEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The Slot table of BFD.
                 BFD statistics on specify board of containing the following objects.
                 The index of this table is hwBfdSlotID.
                "
            ::= { hwBfdObjects 5 }


        hwBfdSlotEntry OBJECT-TYPE
            SYNTAX HwBfdSlotEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The Slot table of BFD.
                 BFD statistics on specify board of containing the following objects.
                 The index of this entry is hwBfdSlotID.
                "
            INDEX { hwBfdSlotID }
            ::= { hwBfdSlotTable 1 }


        HwBfdSlotEntry ::=
            SEQUENCE {
                hwBfdSlotID
                    Unsigned32,
                hwBfdSlotReserveOneHopSessNum
                    Unsigned32,
                hwBfdSlotOneHopSessNum
                    Unsigned32,
                hwBfdSlotCurrentSessNum
                    Unsigned32,
                hwBfdSlotRowStatus
                    RowStatus
             }

        hwBfdSlotID OBJECT-TYPE
            SYNTAX Unsigned32 (0..31)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The ID of slot."
            ::= { hwBfdSlotEntry 1 }


        hwBfdSlotReserveOneHopSessNum OBJECT-TYPE
            SYNTAX Unsigned32 (0..512)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The number of session reserving for one-hop session on the board."
            ::= { hwBfdSlotEntry 2 }


        hwBfdSlotOneHopSessNum OBJECT-TYPE
            SYNTAX Unsigned32 (0..512)
            MAX-ACCESS read-only
            STATUS obsolete
            DESCRIPTION
                "The number of session for one-hop session on the board."
            ::= { hwBfdSlotEntry 3 }


        hwBfdSlotCurrentSessNum OBJECT-TYPE
            SYNTAX Unsigned32 (0..512)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The number of session on the board on current."
            ::= { hwBfdSlotEntry 4 }


        hwBfdSlotRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Used to manage the creation and deletion of conceptual rows."
            ::= { hwBfdSlotEntry 5 }


        hwBfdTtlConfTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBfdTtlConfEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The TTL configuration table.
                 The index of this table is hwBfdTtlConfAddr, hwBfdTtlConfMaskLen and hwBfdTtlConfType."
            ::= { hwBfdObjects 6 }


        hwBfdTtlConfEntry OBJECT-TYPE
            SYNTAX HwBfdTtlConfEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The TTL configuration table.
                 The index of this entry is hwBfdTtlConfAddr, hwBfdTtlConfMaskLen and hwBfdTtlConfType."
            INDEX { hwBfdTtlConfAddr, hwBfdTtlConfMaskLen,hwBfdTtlConfType}
            ::= { hwBfdTtlConfTable 1 }


        HwBfdTtlConfEntry ::=
            SEQUENCE {
                hwBfdTtlConfAddr
                    IpAddress,
                hwBfdTtlConfMaskLen
                    Integer32,
                hwBfdTtlConfType
                    INTEGER,
                hwBfdTtlConfValue
                    Integer32,
                hwBfdTtlConfRowStatus
                    RowStatus
             }

        hwBfdTtlConfAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "IP address."
            ::= { hwBfdTtlConfEntry 1 }


        hwBfdTtlConfMaskLen OBJECT-TYPE
            SYNTAX Integer32 (8..32)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Length of IP address mask."
            ::= { hwBfdTtlConfEntry 2 }


        hwBfdTtlConfType OBJECT-TYPE
            SYNTAX INTEGER
                {
                singleHop(1),
                multiHop(2)
                }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Type of BFD session.
                 Options:
                 1. singleHop(1) -single hop bfd session
                 2. multiHop(2)  -multi hop bfd session
                "
            ::= { hwBfdTtlConfEntry 3 }


        hwBfdTtlConfValue OBJECT-TYPE
            SYNTAX Integer32(1..255)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "TTL value."
            ::= { hwBfdTtlConfEntry 4 }


        hwBfdTtlConfRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The status of this table entry."
            ::= { hwBfdTtlConfEntry 50 }



        hwBfdPassiveAuthTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBfdPassiveAuthEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The authentication configuration table for entire dynamic bfd session on egress.
                 The index of this table is hwBfdPassiveAuthPeerAddr and hwBfdPassiveAuthProtocol.
                "
            ::= { hwBfdObjects 7 }


        hwBfdPassiveAuthEntry OBJECT-TYPE
            SYNTAX HwBfdPassiveAuthEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The authentication configuration table for entire dynamic bfd session on egress.
                 The index of this entry is hwBfdPassiveAuthPeerAddr and hwBfdPassiveAuthProtocol.
                "
            INDEX { hwBfdPassiveAuthPeerAddr, hwBfdPassiveAuthProtocol}
            ::= { hwBfdPassiveAuthTable 1 }


        HwBfdPassiveAuthEntry ::=
            SEQUENCE {
                hwBfdPassiveAuthPeerAddr
                    IpAddress,
                hwBfdPassiveAuthProtocol
                    Integer32,
                hwBfdPassiveAuthKeychainName
                    OCTET STRING,
                hwBfdPassiveAuthMeticulous
                    EnabledStatus,
                hwBfdPassiveAuthLoose
                    TruthValue,
                hwBfdPassiveAuthRowStatus
                    RowStatus
             }

        hwBfdPassiveAuthPeerAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Specify the Lsr-id IP address of the ingress."
            ::= { hwBfdPassiveAuthEntry 1 }

        hwBfdPassiveAuthProtocol OBJECT-TYPE
            SYNTAX Integer32 (1..2)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Specify the protocol on ingress.
                 Options:
                 1. te(1)  -MPLS TE protocol
                 2. ldp(2) -MPLS LDP protocol
                "
            ::= { hwBfdPassiveAuthEntry 2 }

        hwBfdPassiveAuthKeychainName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..47))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Specify the name of the keychain for authentication of entire dynamic bfd session."
            ::= { hwBfdPassiveAuthEntry 3 }

        hwBfdPassiveAuthMeticulous OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Whether enable meticulous authentication for MD5 or SHA-1 type.
                 Options:
                 1. enabled(1)  -enable meticulous authentication for MD5 or SHA-1 type
                 2. disabled(2) -disabled meticulous authentication for MD5 or SHA-1 type
                 Default: 2
                "
            ::= { hwBfdPassiveAuthEntry 4 }

        hwBfdPassiveAuthLoose OBJECT-TYPE
            SYNTAX TruthValue
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Whether loose authentication check.
                 Options:
                 1. True(1)  -loose-check
                 2. False(2) -do not loose-check
                 Default: false
                "
            ::= { hwBfdPassiveAuthEntry 5 }

        hwBfdPassiveAuthRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The status of this table entry."
            ::= { hwBfdPassiveAuthEntry 50 }


        hwBfdNotifications OBJECT IDENTIFIER ::= { hwBFDMIB 3 }


        hwBfdSessDown NOTIFICATION-TYPE
            OBJECTS { hwBfdSessCfgName, hwBfdSessPeerAddr, hwBfdSessBindIfIndex, hwBfdSessBindIfName, hwBfdSessDiag,
                hwBfdSessVrfIndex, hwBfdSessVPNName, hwBfdSessType, hwBfdSessDefaultIp, hwBfdSessBindType,
                hwBfdSessStaticLspName, hwBfdSessPWSecondaryFlag, hwBfdSessNextHop, hwBfdSessVcId, hwBfdSessVsiName,
                hwBfdSessVsiPeerAddr, hwBfdSessDiscrAuto, hwBfdSessPeerIpv6Addr, hwBfdSessIpv6NextHop }
            STATUS current
            DESCRIPTION
                "This trap occurred when the state of the BFD session
                 became down. The BFD session is characterized
                 by the objects in this node.
                "
            ::= { hwBfdNotifications 1 }


        hwBfdSessUp NOTIFICATION-TYPE
            OBJECTS { hwBfdSessCfgName, hwBfdSessPeerAddr, hwBfdSessBindIfIndex, hwBfdSessBindIfName, hwBfdSessDiag,
                hwBfdSessVrfIndex, hwBfdSessVPNName, hwBfdSessType, hwBfdSessDefaultIp, hwBfdSessBindType,
                hwBfdSessStaticLspName, hwBfdSessPWSecondaryFlag, hwBfdSessNextHop, hwBfdSessVcId, hwBfdSessVsiName,
                hwBfdSessVsiPeerAddr, hwBfdSessDiscrAuto, hwBfdSessPeerIpv6Addr, hwBfdSessIpv6NextHop }
            STATUS current
            DESCRIPTION
                "This trap occurred when the state of the BFD session
                 became up. The BFD session is characterized
                 by the objects in this node.
                "
            ::= { hwBfdNotifications 2 }


        hwBfdSessReachLimit NOTIFICATION-TYPE
            OBJECTS { hwBfdSessLimitNumber }
            STATUS current
            DESCRIPTION
                "There is the notify when the session number reach the global limit."
            ::= { hwBfdNotifications 3 }


        hwBfdSessReachLimitBindIf NOTIFICATION-TYPE
            OBJECTS { hwBfdSessConfBindIfName, hwBfdSessInterfaceLimitNumber }
            STATUS current
            DESCRIPTION
                "There is the notify when the session number reach the interface limit."
            ::= { hwBfdNotifications 4 }


        hwBfdSessReachLimitResume NOTIFICATION-TYPE
            OBJECTS { hwBfdSessLimitNumber }
            STATUS current
            DESCRIPTION
                "There is the notify when the session number reach the global limit was cleared. "
            ::= { hwBfdNotifications 5 }


        hwBfdSessReachLimitBindIfResume NOTIFICATION-TYPE
            OBJECTS { hwBfdSessConfBindIfName, hwBfdSessInterfaceLimitNumber, hwBfdLimitDeviceName  }
            STATUS current
            DESCRIPTION
                "There is the notify when the session number reach the interface limit was cleared. "
            ::= { hwBfdNotifications 6 }

        hwBfdSessCfgRemoteFail NOTIFICATION-TYPE
            OBJECTS { hwBfdSessCfgName, hwBfdSessLocalDiscr, hwBfdSessCfgRemoteFailType }
            STATUS current
            DESCRIPTION
                "This notification is generated when the virtual access AP process BFD configuration failed."
            ::= { hwBfdNotifications 7 }

        hwBfdSessFaultDown NOTIFICATION-TYPE
            OBJECTS { hwBfdSessCfgName, hwBfdSessLocalDiscr, hwBfdSessDiag, hwBfdSessBindIfName }
            STATUS current
            DESCRIPTION
                "This trap occurred when the state of the BFD session
                 became down. The BFD session is characterized
                 by the objects in this node.
                "
            ::= { hwBfdNotifications 8 }  
            

        hwBfdSessResume NOTIFICATION-TYPE
            OBJECTS { hwBfdSessCfgName, hwBfdSessLocalDiscr, hwBfdSessDiag, hwBfdSessBindIfName }
            STATUS current
            DESCRIPTION
                "This trap occurred when the state of the BFD session
                 resume from down state. The BFD session is characterized
                 by the objects in this node.
                "
            ::= { hwBfdNotifications 9 }

        hwBfdSessApOperFailed NOTIFICATION-TYPE
            OBJECTS {
                hwBfdCfgApUserName,
                hwBfdCfgApIPAddress,
                hwBfdCfgApID,
                hwBfdCfgApOperation,
                hwBfdCfgApReason }
            STATUS current
            DESCRIPTION
                "The operation failed to config access point."
            ::= { hwBfdNotifications 10 }

        hwBfdSessFsmDiscordant NOTIFICATION-TYPE
            OBJECTS { hwBfdSessCfgName, hwBfdSessLocalDiscr, hwBfdSessDiag, hwBfdSessBindIfName }
            STATUS current
            DESCRIPTION
                "This trap occurred when the state of the BFD session
                 FSM's board is different from the monitored link's board.
                 The BFD session is characterized by the objects in this node.
                "
            ::= { hwBfdNotifications 11 }  
            

        hwBfdSessFsmAccordant NOTIFICATION-TYPE
            OBJECTS { hwBfdSessCfgName, hwBfdSessLocalDiscr, hwBfdSessDiag, hwBfdSessBindIfName }
            STATUS current
            DESCRIPTION
                "This trap occurred when the state of the BFD session
                 FSM's board is the same as the monitored link's board.
                 The BFD session is characterized by the objects in this node.
                "
            ::= { hwBfdNotifications 12 }


        hwBfdConformance OBJECT IDENTIFIER ::= { hwBFDMIB 4 }


        hwBfdCompliances OBJECT IDENTIFIER ::= { hwBfdConformance 1 }


--  this module
        hwBfdFullCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION
                "The compliance statement for entities which
                 implement the Huawei BFD MIB.
                "
            MODULE -- this module
                MANDATORY-GROUPS { hwBfdGroup, hwBfdSessGroup, hwBfdObsoleteGroup, hwBfdNotificationGroup }
            ::= { hwBfdCompliances 1 }


        hwBfdGroups OBJECT IDENTIFIER ::= { hwBfdConformance 2 }


        hwBfdGroup OBJECT-GROUP
            OBJECTS { hwBfdVersionNumber, hwBfdAdminStatus, hwBfdSessLimitNumber, hwBfdSessInterfaceLimitNumber, hwBfdSessStaticNumber,
                hwBfdSessDynamicNumber, hwBfdSessGlobalDefaultIpAddr, hwBfdEchoPassiveStatus, hwBfdEchoAclNum, hwBfdSessDynamicPingInterval,
                hwBfdSessDynamicSupportPassive, hwBfdSessDelayUpTime, hwBfdSessMultiDstPort, hwBfdTrapSendInterval, hwBfdIfConfName, hwBfdIfConfDeleting, hwBfdIfConfAvailable, hwBfdIfConfSessCnt,
                hwBfdIfConfRowStatus, hwBfdSlotReserveOneHopSessNum,hwBfdSlotCurrentSessNum, hwBfdSlotRowStatus, hwBfdLimitDeviceName, hwBfdDynamicSessionTos, hwBfdStaticSessionTos, hwBfdDynamicSessionTosEx
                 }
            STATUS current
            DESCRIPTION
                "A collection of objects providing BFD global information."
            ::= { hwBfdGroups 1 }


        hwBfdSessGroup OBJECT-GROUP
            OBJECTS { hwBfdSessConfMIndex, hwBfdSessConfLocalDiscr, hwBfdSessConfRemoteDiscr, hwBfdSessConfPeerAddr, hwBfdSessConfBindIfIndex,
                hwBfdSessConfBindIfName, hwBfdSessConfDemandEnable, hwBfdSessConfDemandTimerInterval, hwBfdSessConfDetectMult, hwBfdSessConfDesiredMinRxInterval,
                hwBfdSessConfDesiredMinTxInterval, hwBfdSessConfWTRInterval, hwBfdSessConfTOS, hwBfdSessConfPSTFlag, hwBfdSessConfCommitFlag,
                hwBfdSessConfAdminStatus, hwBfdSessConfRowStatus, hwBfdSessConfSourceAddr, hwBfdSessConfVrfIndex, hwBfdSessConfVPNName,
                hwBfdSessConfDefaultIp, hwBfdSessConfPISFlag, hwBfdSessConfBindType, hwBfdSessConfNextHop, hwBfdSessConfStaticLspName,
                hwBfdSessConfPWSecondaryFlag, hwBfdSessConfTunnelDetectType, hwBfdSessConfVcId, hwBfdSessConfVsiName, hwBfdSessConfVsiPeerAddr, hwBfdSessConfDiscrAuto, hwBfdSessConfPeerIpv6Addr, hwBfdSessConfSourceIpv6Addr, hwBfdSessConfIpv6NextHop, hwBfdSessConfIsIpv6Addr,
                hwBfdSessConfKeychainName, hwBfdSessConfMeticulous, hwBfdSessConfLooseAuthentication, hwBfdSessConfPWTtlMode,
                hwBfdSessConfPWTtl, hwBfdSessConfRemotePeerIp, hwBfdSessConfRemotePeerIpType, hwBfdSessConfPWSPE, hwBfdSessConfPWTrackIfName, hwBfdSessConfIsPWTrackIf, hwBfdSessConfEncapsulationType,
                hwBfdSessConfPEVid, hwBfdSessConfCEVid, hwBfdSessConfTOSEx, hwBfdSessConfbImpactFlag, hwBfdSessMIndex, hwBfdSessBindVRRP,
                hwBfdSessCfgName, hwBfdSessPeerAddr, hwBfdSessBindIfIndex, hwBfdSessBindIfName, hwBfdSessLocalDiscr,
                hwBfdSessRemoteDiscr, hwBfdSessOperMode, hwBfdSessDetectMult, hwBfdSessDemandTimerInterval, hwBfdSessActualRxInterval,
                hwBfdSessActualTxInterval, hwBfdSessWTRInterval, hwBfdSessTOS, hwBfdSessState, hwBfdSessDiag,
                hwBfdSessSourceAddr, hwBfdSessVrfIndex, hwBfdSessVPNName, hwBfdSessType, hwBfdSessBindAppType,
                hwBfdSessDefaultIp, hwBfdSessPISFlag, hwBfdSessBindType, hwBfdSessNextHop, hwBfdSessStaticLspName,
                hwBfdSessLspIndex, hwBfdSessPWSecondaryFlag, hwBfdSessTunnelDetectType, hwBfdSessVcId, hwBfdSessVsiName, hwBfdSessVsiPeerAddr, hwBfdSessDiscrAuto, hwBfdSessPeerIpv6Addr, hwBfdSessSourceIpv6Addr, hwBfdSessIpv6NextHop, hwBfdSessIsIPv6Addr, hwBfdSessMeticulous,hwBfdSessLooseAuthentication, hwBfdSessAuthenticationStatus,
                hwBfdSessPWTtlMode, hwBfdSessPWTtl, hwBfdSessRemotePeerIp, hwBfdSessRemotePeerIpType, hwBfdSessSelectBoard, hwBfdSessPWSPE, hwBfdSessPWTrackIfName,
                hwBfdSessIsPWTrackIf, hwBfdSessEncapsulationType, hwBfdSessPEVid, hwBfdSessCEVid, hwBfdSessPeerInetAddrType, hwBfdSessPeerInetAddr, hwBfdSessInetNextHopType, hwBfdSessInetNextHop, hwBfdSessBindAppTypeMask, hwBfdSessDscp, hwBfdSessPerfPktIn,
                hwBfdSessPerfPktInHC, hwBfdSessPerfPktOut, hwBfdSessPerfPktOutHC, hwBfdSessPerfBadIn, hwBfdSessPerfBadInHC,
                hwBfdSessPerfBadOut, hwBfdSessPerfBadOutHC, hwBfdSessPerfLastSessDownTime, hwBfdSessPerfSessDownCount, hwBfdSessPerfSessShortBreakCount,
                hwBfdSessionPerStartTime, hwBfdTtlConfValue, hwBfdTtlConfRowStatus,
                hwBfdPassiveAuthPeerAddr, hwBfdPassiveAuthProtocol, hwBfdPassiveAuthKeychainName, hwBfdPassiveAuthMeticulous, hwBfdPassiveAuthLoose, hwBfdPassiveAuthRowStatus, hwBfdSessPWId}
            STATUS current
            DESCRIPTION
                "A collection of objects providing BFD session information."
            ::= { hwBfdGroups 2 }


        hwBfdObsoleteGroup OBJECT-GROUP
            OBJECTS { hwBfdIfConfEnable ,hwBfdSlotOneHopSessNum}
            STATUS obsolete
            DESCRIPTION
                "A collection of objects which are obsolete."
            ::= { hwBfdGroups 3 }


        hwBfdNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwBfdSessDown, hwBfdSessUp, hwBfdSessReachLimit, hwBfdSessReachLimitResume, hwBfdSessReachLimitBindIf, hwBfdSessReachLimitBindIfResume, hwBfdSessCfgRemoteFail }
            STATUS current
            DESCRIPTION
                "A collection of traps."
            ::= { hwBfdGroups 4 }

        hwBfdTrapsVbOids OBJECT IDENTIFIER ::= { hwBFDMIB 5 }
    
        hwBfdSessVlanID  OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The VLANID binding to BFD session.
                "  
            ::= { hwBfdTrapsVbOids 1 }  

        hwBfdCfgApUserName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..128))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The name of user failed to configure access point."
            ::= { hwBfdTrapsVbOids 2 }

        hwBfdCfgApIPAddress OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..128))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The IP-address of user failed to configure access point."
            ::= { hwBfdTrapsVbOids 3 }

        hwBfdCfgApID OBJECT-TYPE
            SYNTAX Unsigned32 (1..8191)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The ID of access point failed to be configured."
            ::= { hwBfdTrapsVbOids 4 }

        hwBfdCfgApOperation OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..128))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The operation of confiuration to access point."
            ::= { hwBfdTrapsVbOids 5 }

        hwBfdCfgApReason OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..128))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The reason of failed to configure access point."
            ::= { hwBfdTrapsVbOids 6 }			
            
        hwBfdTraps OBJECT IDENTIFIER ::= { hwBFDMIB 6 }
    
        hwBfdCommonTraps OBJECT IDENTIFIER ::= { hwBfdTraps 1 }
    
        hwBfdAlarmTraps OBJECT IDENTIFIER ::= { hwBfdTraps 2 }
    
        hwBfdAlarmTrapsPrefix OBJECT IDENTIFIER ::= { hwBfdAlarmTraps 0 }
        
        hwBfdSessUpTrap NOTIFICATION-TYPE
            OBJECTS 
            { 
                hwBfdSessLocalDiscr,
                hwBfdSessVlanID,
                hwBfdSessSourceAddr,
                hwBfdSessNextHop,
                hwBfdSessIndex,
                hwBfdSessPeerAddr, 
                hwBfdSessBindType,
                hwBfdSessVrfIndex
            }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the up(3) state from some other state.
                "
            ::= { hwBfdAlarmTraps 0 1 }
    
        hwBfdSessDownTrap NOTIFICATION-TYPE
            OBJECTS 
            { 
                hwBfdSessLocalDiscr,
                hwBfdSessVlanID,
                hwBfdSessSourceAddr,
                hwBfdSessNextHop,
                hwBfdSessIndex,
                hwBfdSessPeerAddr, 
                hwBfdSessBindType,
                hwBfdSessVrfIndex
            }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the down(1) or adminDown(0) states from some 
                 other state.
                "
            ::= { hwBfdAlarmTraps 0 2 }
            
        hwBfdv6SingleHopSessUpTrap NOTIFICATION-TYPE
            OBJECTS                     
            {
                hwBfdSessIndex,
                hwBfdSessVlanID,
                hwBfdSessSourceIpv6Addr,
                hwBfdSessPeerIpv6Addr
            }                           
            STATUS current              
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the up(3) state from some other state.
                "       
            ::= { hwBfdAlarmTraps 0 3 } 

         hwBfdv6SingleHopSessDownTrap NOTIFICATION-TYPE
            OBJECTS 
            {
                hwBfdSessIndex,
                hwBfdSessVlanID,
                hwBfdSessSourceIpv6Addr,
                hwBfdSessPeerIpv6Addr
            }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the down(1) or adminDown(0) states from some 
                 other state.
                "
            ::= { hwBfdAlarmTraps 0 4 }

        hwBfdv6MultiHopSessUpTrap NOTIFICATION-TYPE
            OBJECTS                     
            {
                hwBfdSessIndex,
                hwBfdSessVrfIndex,
                hwBfdSessSourceIpv6Addr,
                hwBfdSessPeerIpv6Addr
            }                           
            STATUS current              
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the up(3) state from some other state.
                "       
            ::= { hwBfdAlarmTraps 0 5 } 

         hwBfdv6MultiHopSessDownTrap NOTIFICATION-TYPE
            OBJECTS 
            {
                hwBfdSessIndex,
                hwBfdSessVrfIndex,
                hwBfdSessSourceIpv6Addr,
                hwBfdSessPeerIpv6Addr
            }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the down(1) or adminDown(0) states from some 
                 other state.
                "
            ::= { hwBfdAlarmTraps 0 6 }
        hwBfdPWSessUp NOTIFICATION-TYPE
            OBJECTS 
            {
                hwBfdSessIndex,
                hwBfdSessCfgName,
                hwBfdSessLocalDiscr,
                hwBfdSessDiag,
                hwBfdSessBindType,
                hwBfdSessPWSecondaryFlag,
                hwBfdSessPWId,
                hwBfdSessVsiName,
                hwBfdSessVsiPeerAddr
            }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the up(3) state from some other state.
                "
            ::= { hwBfdAlarmTraps 0 7 }
        hwBfdPWSessDown NOTIFICATION-TYPE
            OBJECTS 
            {
                hwBfdSessIndex,
                hwBfdSessCfgName,
                hwBfdSessLocalDiscr,
                hwBfdSessDiag,
                hwBfdSessBindType,
                hwBfdSessPWSecondaryFlag,
                hwBfdSessPWId,
                hwBfdSessVsiName,
                hwBfdSessVsiPeerAddr
            }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the bfdSessState
                 object for one entry in bfdSessionTable is about to 
                 enter the down(1) or adminDown(0) states from some 
                 other state.
                "
            ::= { hwBfdAlarmTraps 0 8 }
            
    END  
         
--       
-- HUAWEI-BFD-MIB.mib
--