-- This module defines enterprise MIBs for Configuration monitoring
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-SET-GEN-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenSetting, netscreenSettingMibModule
        FROM NETSCREEN-SMI
    IpAddress, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    ;

netscreenSetGenMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
         "obsolete nsSetGenSysIp"
    REVISION      "200508120000Z" -- Aug 12, 2005
    DESCRIPTION
        "This module defines the object that are used to monitor all
         the configuration info"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311100000Z" -- November 10, 2003
    DESCRIPTION
        "Correct spelling mistake"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "No Comment"
    REVISION      "200105270000Z" -- May 27, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenSettingMibModule 1 }

nsSetGeneral OBJECT IDENTIFIER ::= { netscreenSetting 1 }

nsSetGenSysIp OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        obsolete
    DESCRIPTION
        "System Ip address"
    ::= { nsSetGeneral 1 }

nsSetGenHostName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Host name of NetScreen device."
    ::= { nsSetGeneral 2 }

nsSetGenDomain OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Domain name of NetScreen device."
    ::= { nsSetGeneral 3 }

nsSetGenOpMode OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "NetScreen device can work in one of the tree mode:
         transparent, NAT  and route. This attribute indicates which
         operation mode it use."
    ::= { nsSetGeneral 4 }

nsSetGenSwVer OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..128))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "NetSceen OS version."
    ::= { nsSetGeneral 5 }

nsSetGenLicInfo OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "NetScreen OS license information."
    ::= { nsSetGeneral 6 }

nsSetGenSCSAdminEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "enable Command Security Shell"
    ::= { nsSetGeneral 7 }

nsSetGenDropSelfLogPac OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Log Packets to Self that are dropped"
    ::= { nsSetGeneral 8 }

END


