
-- *****************************************************************************
-- Juniper-ROUTER-MIB
--
-- Juniper Networks Enterprise MIB
--   The Router MIB.
--
-- Copyright (c) 2000, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2003 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-ROUTER-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32, Counter32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, DisplayString, RowStatus, TruthValue
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    SnmpEngineID
        FROM SNMP-FRAMEWORK-MIB
    JuniName
        FROM Juniper-TC
    JuniIpPolicyName, JuniIpPolicyExtendedCommunity
        FROM Juniper-IP-POLICY-MIB
    juniMibs
        FROM Juniper-MIBs;

juniRouterMIB  MODULE-IDENTITY
    LAST-UPDATED "200405062030Z"  -- 06-May-04 04:30 PM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The Router MIB is used to manage the creation and deletion as well as
        the administrative states of the protocols and functions that run within
        a designated router."
    -- Revision History
    REVISION    "200405062030Z"  -- 06-May-04 04:30 PM EDT  - JUNOSe 6.1
    DESCRIPTION
         "Added RLI-870 Virtual Router and Vrf count support."
    REVISION    "200309241731Z"  -- 24-Sep-03 01:31 PM EDT  - JUNOSe 6.0
    DESCRIPTION
         "Added RADIUS Proxy protocol support."
    REVISION    "200305221552Z"  -- 22-May-03 11:52 AM EDT  - JUNOSe 5.2
    DESCRIPTION
        "Added support for global export map and export map filter."
    REVISION    "200305102054Z"  -- 10-May-03 04:54 PM EDT  - JUNOSe 5.1
    DESCRIPTION
        "Added DHCPv6 protocol support."
    REVISION    "200304241325Z"  -- 24-Apr-03 09:25 AM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         Added TACACS+ and RADIUS Disconnect protocol support.
         Added SNMPv3 context engine ID to the virtual router table."
    REVISION    "200205101816Z"  -- 10-May-02 02:16 PM EDT  - JUNOSe 4.0
    DESCRIPTION
        "Added support for router context name string."
    REVISION    "200101241825Z"  -- 24-Jan-01 01:25 PM EST  - JUNOSe 3.0
    DESCRIPTION
        "Added support for VRF - virtual router forwarder.  Support is defined
         by these objects/table:
             juniRouterVrf
             juniRouterVrfTable
             juniRouterVrfRouteTargetTable"
    REVISION    "200001210000Z"  -- 21-Jan-00               - JUNOSe 1.3
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 32 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
JuniNextRouterIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Coordinates routerIndex value allocation for entries in an associated
        router table.  Clients must first read the routerIndex value from this
        object, then create an entry having the routerIndex value in the
        associated router table.

        The DESCRIPTION clause for an object of this type must identify the
        associated router table.

        A GET of this object returns the next available routerIndex value to be
        used to create an entry in the associated router table; or zero, if no
        valid routerIndex value is available.  This object also returns a value
        of zero when it is the lexicographic successor of a varbind presented in
        an SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that routerIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously.

        Unless specified otherwise by its MAX-ACCESS and DESCRIPTION clauses, an
        object of this type is read-only, and a SET of such an object returns a
        notWritable error."
    SYNTAX      Unsigned32

JuniRouterProtocolIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Identifies the router protocol."
    SYNTAX      INTEGER {
                    ip(1),
                    osi(2),
                    icmp(3),
                    igmp(4),
                    tcp(5),
                    udp(6),
                    bgp(7),
                    ospf(8),
                    isis(9),
                    rip(10),
                    snmp(11),
                    ntp(12),
                    generator(13),
                    localAddressServer(14),
                    dhcpProxy(15),
                    dhcpRelay(16),
                    nameResolver(17),
                    policyManager(18),
                    sscClient(19),
                    cops(20),
                    mgtm(21),
                    dvmrp(22),
                    pim(23),
                    msdp(24),
                    mpls(25),
                    radius(26),
                    mplsMgr(27),
                    dhcpLocalServer(28),
                    tacacsPlus(29),
                    radiusDisconnect(30),
                    dhcpv6LocalServer(31),
                    radiusProxy(32)}


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniRouterObjects   OBJECT IDENTIFIER ::= { juniRouterMIB 1 }
juniRouterSummaryCounts   OBJECT IDENTIFIER ::= { juniRouterObjects 6 }

--- 
--- Summary Count Objects
---
juniRouterSummaryScalars OBJECT IDENTIFIER
    ::= {juniRouterSummaryCounts 1}

juniRouterSummaryNonParentVRsConfigured  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of VRs without VRFs configured."
    ::= { juniRouterSummaryScalars 1 }

juniRouterSummaryParentVRsConfigured  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of VRs with VRFs configured."
    ::= { juniRouterSummaryScalars 2 }

juniRouterSummaryVRFsConfigured  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of VRFs configured."
    ::= { juniRouterSummaryScalars 3 }

juniRouterSummaryTotalConfigured  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Virtual Routers and VRFs configured."
    ::= { juniRouterSummaryScalars 4}


-- /////////////////////////////////////////////////////////////////////////////
--
-- Routers
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- Router ID selection for creating "virtual" routers.
--
juniRouterNextRouterIndex  OBJECT-TYPE
    SYNTAX      JuniNextRouterIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinates routerIndex and juniRouterVrfIndex value allocation for
        entries in the juniRouterTable and juniRouterVrfTable, respectively.

        A GET of this object returns the next available routerIndex value to be
        used to create an entry in the associated router table; or zero, if no
        valid routerIndex value is available.  This object also returns a value
        of zero when it is the lexicographic successor of a varbind presented in
        an SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that routerIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniRouterObjects 1 }

--
-- The Router Table
--
juniRouterTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniRouterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for routers present in the system."
    ::= { juniRouterObjects 2 }

juniRouterEntry  OBJECT-TYPE
    SYNTAX      JuniRouterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry in this table represents a single router.  Creating and/or
        deleting entries in this table causes corresponding entries to be
        created or deleted in the juniRouterProtocolTable.  Note that VRFs also
        appear as entries in this table and can be differentiated by the
        juniRouterVrf object.  The juniRouterVrfTable shows the parent / child
        relationship between routers and VRFs present in the system."
    INDEX     { juniRouterIndex }
    ::= { juniRouterTable 1 }

JuniRouterEntry ::= SEQUENCE {
    juniRouterIndex             Unsigned32,
    juniRouterName              JuniName,
    juniRouterRowStatus         RowStatus,
    juniRouterVrf               TruthValue,
    juniRouterContextName       OCTET STRING,
    juniRouterContextEngineID   SnmpEngineID,
    juniRouterSummaryVRFCount   Counter32}

juniRouterIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The routerIndex of this router.  When creating entries in this table,
        suitable values for this object are determined by reading
        juniRouterNextRouterIndex."
    ::= { juniRouterEntry 1 }

juniRouterName  OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administratively assigned name given to this router.  The name must
        be unique within the context of this table and cannot be changed after
        the router instance is created."
    ::= { juniRouterEntry 2 }

juniRouterRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniRouterRowStatus
            juniRouterName

        In addition, when creating an entry the following conditions must hold:

            A value for juniRouterIndex must have been determined previously by
            reading juniRouterNextRouterIndex.

        A corresponding entries in juniRouterProtocolTable are created/destroyed
        as a result of creating/destroying an entry in this table."
    ::= { juniRouterEntry 3 }

juniRouterVrf  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Identifies whether this router is a VRF or not.  A value of true(1)
        indicates that this is a VRF; a value of false(2) indicates that it is
        not."
    ::= { juniRouterEntry 4 }

juniRouterContextName  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(7..14))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An internally derived/assigned name given to this router with a
        specific format:
                routerN

        where N is a decimal number (with no leading zeroes) in the range
        1..16777215 corresponding to the value of the least significant 24 bits
        of the juniRouterIndex (the router UID).  The name is unique within the
        context of this table."
    ::= { juniRouterEntry 5 }

juniRouterContextEngineID  OBJECT-TYPE
    SYNTAX      SnmpEngineID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The virtual router SNMP engine's administratively-unique identifier.
        This is used as the contextEngineId to reach the virtual router's
        SNMP context via the system-wide SNMP engine using SNMPv3."
    REFERENCE
        "An Architecture for Describing Simple Network Management Protocol
        (SNMP) Management Frameworks (RFC3411) clause 3.3.2."
    ::= { juniRouterEntry 6 }

juniRouterSummaryVRFCount  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of VRFs contained in the VR." 
    ::= { juniRouterEntry 7 }


--
-- The Router Protocol Table
--
juniRouterProtocolTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniRouterProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for each protocol supported by the router
        entry created in the juniRouterTable."
    ::= { juniRouterObjects 3 }

juniRouterProtocolEntry  OBJECT-TYPE
    SYNTAX      JuniRouterProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry provides administrative control on a router protocol for the
        router designated by the first indice to this table.  The second indice
        identifies the router protocol.

        Entries in this table are created as a side-effect of row creation in
        the juniRouterTable or juniRouterVrfTable."
    INDEX     { juniRouterProtocolRouterIndex,
                juniRouterProtocolProtocolIndex }
    ::= { juniRouterProtocolTable 1 }

JuniRouterProtocolEntry ::= SEQUENCE {
    juniRouterProtocolRouterIndex    Unsigned32,
    juniRouterProtocolProtocolIndex  JuniRouterProtocolIndex,
    juniRouterProtocolRowStatus      RowStatus }

juniRouterProtocolRouterIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The routerIndex of this router.  This object is the same as the
        juniRouterIndex object defined in the juniRouterTable."
    ::= { juniRouterProtocolEntry 1 }

juniRouterProtocolProtocolIndex  OBJECT-TYPE
    SYNTAX      JuniRouterProtocolIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Identities the router protocol."
    ::= { juniRouterProtocolEntry 2 }

juniRouterProtocolRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Administrative control and status of a protocol on a router.

        The following values can be read from this object:
          active(1)   - Indicates that the protocol on the designated router
                        is created, configured, and running.
          notReady(3) - Indicates that the protocol requires additional
                        configuration in a protocol specific MIB module.
                        Examples include the BGP and OSPF protocols, which
                        require additional configuration of protocol specific
                        parameters such as: Autonomous System (AS) for BGP,
                        and Process Id for OSPF.
          destroy(6)  - The destroy(3) operation can fail if there are
                        executing applications dependent on the protocol.
                        If an attempt is made to destroy(6) an active(1)
                        protocol that other applications are dependent on,
                        the rowStatus will read destroy(6).  Normally, when
                        a row is destroyed, the agent will cleaup and remove
                        the entry.

        The following values can be written to this object:
          active(1)      - Activate protocol on the designated router.
          createAndGo(4) - Create protocol on designated router.  The router
                           indicated by juniRouterProtocolRouterIndex must
                           already exist in the juniRouterTable.  The value of
                           the juniRouterProtocolProtocolIndex must be from the
                           set of protocol values defined by the
                           JuniRouterProtocolIndex type.
          destroy(6)     - Destroy protocol on designated router.  If the
                           operation is successful, the agent will remove the
                           entry.  If the operation failed, the row will remain
                           in the table with a rowStatus value of destroy(6).

            Conditions on destroy(6):
             1) The default router can not be deleted.
             2) The local router can not be deleted.  A local router is defined
                as the router that sourced the SNMP request.

        Upon creation of a router in the juniRouterTable, some protocol entries
        will appear in this table by default, which indicates that these
        protocols are created by the action of creating a router.  It is
        important to note, that this behavior may change over time by protocol
        type."
    ::= { juniRouterProtocolEntry 3 }

--
-- The Router VRF Table
--
juniRouterVrfTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniRouterVrfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for each VRF on each router entry created
        in the juniRouterTable."
    ::= { juniRouterObjects 4 }

juniRouterVrfEntry  OBJECT-TYPE
    SYNTAX      JuniRouterVrfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry provides administrative control on a router VRF for the
        router designated by the first indice of this table.  The second indice
        identifies the router VRF.

        The parent router must exist in the juniRouterTable before performing
        VRF row creation in this table"
    INDEX     { juniRouterVrfRouterIndex,
                juniRouterVrfRouterVrfIndex }
    ::= { juniRouterVrfTable 1 }

JuniRouterVrfEntry ::= SEQUENCE {
    juniRouterVrfRouterIndex                      Unsigned32,
    juniRouterVrfRouterVrfIndex                   Unsigned32,
    juniRouterVrfIpv4UnicastImportRouteMap        JuniIpPolicyName,
    juniRouterVrfIpv4UnicastExportRouteMap        JuniIpPolicyName,
    juniRouterVrfRouteDistinguisher               JuniIpPolicyExtendedCommunity,
    juniRouterVrfRowStatus                        RowStatus,
    juniRouterVrfRouterName                       JuniName,
    juniRouterVrfRouterDescription                DisplayString,
    juniRouterVrfIpv4UnicastGlobalExportRouteMap  JuniIpPolicyName,
    juniRouterVrfIpv4UnicastExportRouteMapFilter  TruthValue,
    juniRouterVrfIpv6UnicastImportRouteMap        JuniIpPolicyName,
    juniRouterVrfIpv6UnicastExportRouteMap        JuniIpPolicyName,
    juniRouterVrfIpv6UnicastGlobalExportRouteMap  JuniIpPolicyName,
    juniRouterVrfIpv6UnicastExportRouteMapFilter  TruthValue,
    juniRouterVrfIpv4UnicastGlobalImportRouteMap  JuniIpPolicyName,
    juniRouterVrfIpv4UnicastGlobalImportMaxRoutes Unsigned32,
    juniRouterVrfIpv6UnicastGlobalImportRouteMap  JuniIpPolicyName,
    juniRouterVrfIpv6UnicastGlobalImportMaxRoutes Unsigned32}

juniRouterVrfRouterIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The router index of this router, also referred to as the parent of the
        VRF.  This object is the same as the juniRouterIndex object defined in
        the juniRouterTable."
    ::= { juniRouterVrfEntry 1 }

juniRouterVrfRouterVrfIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VRF router index for this entry, also referred as the child of the
        parent router, which is identified by the first indice to this table."
    ::= { juniRouterVrfEntry 2 }

juniRouterVrfIpv4UnicastImportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router import route map for IPv4 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 3 }

juniRouterVrfIpv4UnicastExportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router export route map for IPv4 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 4 }

juniRouterVrfRouteDistinguisher  OBJECT-TYPE
    SYNTAX      JuniIpPolicyExtendedCommunity
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router route distinguisher."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 5 }

juniRouterVrfRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        *** LIMITED CONFIGURATION LEVEL ***
        RowStatus createAndGo/destroy operations have the following
        special-purpose semantics:
            createAndGo     Create an entry having the specified configuration
                            and append it to the target list, i.e. create an
                            juniRouterVrfEntry table entry with the associated
                            characteristics.
            destroy         Destroy the specified element.

        Entries in this table can be modified once the row has been created.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            A value for juniRouterVrfRouterIndex must have been determined
            previously by reading juniRouterNextRouterIndex.

            A parent router must exist in the juniRouterTable."
    ::= { juniRouterVrfEntry 7 }

juniRouterVrfRouterName  OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administratively assigned name given to this VRF router.  The name
        must be unique within the context of this table and cannot be changed
        after the router instance is created."
    ::= { juniRouterVrfEntry 8 }

juniRouterVrfRouterDescription  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..80))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administratively assigned description given to this VRF router."
    ::= { juniRouterVrfEntry 9 }

juniRouterVrfIpv4UnicastGlobalExportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router global export route map for IPv4 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 10 }

juniRouterVrfIpv4UnicastExportRouteMapFilter  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Is the VRF export map for IPv4 unicast routes allowed to 
        filter routes?"
    DEFVAL    { false }
    ::= { juniRouterVrfEntry 11 }

juniRouterVrfIpv6UnicastImportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router import route map for IPv6 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 12 }

juniRouterVrfIpv6UnicastExportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router export route map for IPv6 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 13 }

juniRouterVrfIpv6UnicastGlobalExportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router global export route map for IPv6 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 14 }

juniRouterVrfIpv6UnicastExportRouteMapFilter  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Is the VRF export map for IPv6 unicast routes allowed to 
        filter routes?"
    DEFVAL    { false }
    ::= { juniRouterVrfEntry 15 }

juniRouterVrfIpv4UnicastGlobalImportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router global import route map for IPv4 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 16 }

juniRouterVrfIpv4UnicastGlobalImportMaxRoutes  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The maximum number of IPv4 unicast routes which can be
        globaly imported."
    DEFVAL    { 100 }
    ::= { juniRouterVrfEntry 17 }

juniRouterVrfIpv6UnicastGlobalImportRouteMap  OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router global import route map for IPv6 unicast routes."
    DEFVAL    { "" }
    ::= { juniRouterVrfEntry 18 }

juniRouterVrfIpv6UnicastGlobalImportMaxRoutes  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The maximum number of IPv6 unicast routes which can be
        globaly imported."
    DEFVAL    { 100 }
    ::= { juniRouterVrfEntry 19 }

--
-- The Router VRF Route Target Table
--
juniRouterVrfRouteTargetTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniRouterVrfRouteTargetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for each route target for the router/VRF
        entry created in the juniRouterTable and juniRouterVrfTable."
    ::= { juniRouterObjects 5 }

juniRouterVrfRouteTargetEntry  OBJECT-TYPE
    SYNTAX      JuniRouterVrfRouteTargetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry provides administrative control on VRF route targets for the
        router/VRF pair designated by the first and second indice of this table.
        The third indice identifies the route target.

        The parent router must exist in the juniRouterTable and the VRF router
        must exist in the juniRouterVrfTable before performing creation of the
        route target in this table."
    INDEX     { juniRouterVrfRouteTargetRouterIndex,
                juniRouterVrfRouteTargetRouterVrfIndex,
                juniRouterVrfRouteTargetAddrFormat,
                juniRouterVrfRouteTargetRouteTarget }
    ::= { juniRouterVrfRouteTargetTable 1 }

JuniRouterVrfRouteTargetEntry ::= SEQUENCE {
    juniRouterVrfRouteTargetRouterIndex      Unsigned32,
    juniRouterVrfRouteTargetRouterVrfIndex   Unsigned32,
    juniRouterVrfRouteTargetAddrFormat       INTEGER,
    juniRouterVrfRouteTargetRouteTarget      JuniIpPolicyExtendedCommunity,
    juniRouterVrfRouteTargetType             INTEGER,
    juniRouterVrfRouteTargetRowStatus        RowStatus }

juniRouterVrfRouteTargetRouterIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The routerIndex of this router, also referred to as the parent of the
        VRF.  This object is the same as the juniRouterIndex object defined in
        the juniRouterTable."
    ::= { juniRouterVrfRouteTargetEntry 1 }

juniRouterVrfRouteTargetRouterVrfIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VRF router index for this entry, also referred as the child of the
        parent router, which is identified by the first indice to this table."
    ::= { juniRouterVrfRouteTargetEntry 2 }

juniRouterVrfRouteTargetAddrFormat  OBJECT-TYPE
    SYNTAX      INTEGER {
                    routeTargetFormatAsn(0),
                    routeTargetFormateIp(1) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The address format of the route target."
    ::= { juniRouterVrfRouteTargetEntry 3 }

juniRouterVrfRouteTargetRouteTarget  OBJECT-TYPE
    SYNTAX      JuniIpPolicyExtendedCommunity
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VRF router route target."
    ::= { juniRouterVrfRouteTargetEntry 4 }

juniRouterVrfRouteTargetType  OBJECT-TYPE
    SYNTAX      INTEGER {
                     routeTargetInvalid(0),
                     routeTargetImport(1),
                     routeTargetExport(2),
                     routeTargetBoth(3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VRF router route target type."
    ::= { juniRouterVrfRouteTargetEntry 5 }

juniRouterVrfRouteTargetRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        *** LIMITED CONFIGURATION LEVEL ***
        RowStatus createAndGo/destroy operations have the following
        special-purpose semantics:
            createAndGo     Create an entry having the specified configuration
                            and append it to the target list, i.e., create an
                            juniRouterVrfRouteTargetEntry table entry with the
                            associated characteristics.
            destroy         Destroy the specified element.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            A parent router must exist in the juniRouterTable.

            A VRF router must exist in the juniRouterVrfTable."
    ::= { juniRouterVrfRouteTargetEntry 6 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- juniRouterTrapControl      OBJECT IDENTIFIER ::= { juniRouterMIB 2 }
-- juniRouterTraps            OBJECT IDENTIFIER ::= { juniRouterMIB 3 }
-- juniRouterTrapPrefix       OBJECT IDENTIFIER ::= { juniRouterTraps 0 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniRouterConformance OBJECT IDENTIFIER ::= { juniRouterMIB 4 }
juniRouterCompliances OBJECT IDENTIFIER ::= { juniRouterConformance 1 }
juniRouterGroups      OBJECT IDENTIFIER ::= { juniRouterConformance 2 }

--
-- compliance statements
--
juniRouterCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "An obsolete compliance statement for entities which implement the
        Juniper Router MIB.  This statement became obsolete when support was
        added for VRFs within routers."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniRouterGroup }
    ::= { juniRouterCompliances 1 }                                -- JUNOSe 1.3

juniRouterCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "An obsolete compliance statement for entities which implement the
        Juniper Router MIB.  This statement became obsolete when support was
        added for the router context name."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniRouterGroup2 }
        GROUP       juniRouterVrfGroup
            DESCRIPTION
                "The VRF group is only required for entities which implement VRF
                routers."
    ::= { juniRouterCompliances 2 }                                -- JUNOSe 3.0

juniRouterCompliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        Router MIB.  This statement became obsolete when support was added for
        the router context engine ID."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniRouterGroup3 }
        GROUP       juniRouterVrfGroup2
            DESCRIPTION
                "The VRF group is only required for entities which implement VRF
                routers."
    ::= { juniRouterCompliances 3 }                                -- JUNOSe 4.0

juniRouterCompliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        Router MIB.  This statement became obsolete when the global export map
        and the export map filter option were added to the VRF group."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniRouterGroup4 }
        GROUP       juniRouterVrfGroup2
            DESCRIPTION
                "The VRF group is only required for entities which implement VRF
                routers."
    ::= { juniRouterCompliances 4 }                                -- JUNOSe 5.0

juniRouterCompliance5  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        Router MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniRouterGroup4 }
        GROUP       juniRouterVrfGroup3
            DESCRIPTION
                "The VRF group is only required for entities which implement VRF
                routers."
    ::= { juniRouterCompliances 5 }                                -- JUNOSe 5.2

juniRouterCompliance6  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        Router MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniRouterGroup5,
            juniRouterSummaryScalarsGroup}
        GROUP       juniRouterVrfGroup3
            DESCRIPTION
                "The VRF group is only required for entities which implement VRF
                routers."
    ::= { juniRouterCompliances 7 }                                -- JUNOSe 6.1

juniRouterCompliance7  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper
        Router MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniRouterGroup5,
            juniRouterSummaryScalarsGroup}
        GROUP       juniRouterVrfGroup4
            DESCRIPTION
                "The VRF group is only required for entities which implement VRF
                routers."
    ::= { juniRouterCompliances 8 }                                -- JUNOSe 7.1

--
-- units of conformance
--
juniRouterGroup  OBJECT-GROUP
    OBJECTS {
        juniRouterNextRouterIndex,
        juniRouterName,
        juniRouterRowStatus,
        juniRouterProtocolRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of routers and
        routing protocols in a Juniper product.  This group became obsolete when
        support was added for VRFs within routers."
    ::= { juniRouterGroups 1 }                                     -- JUNOSe 1.3

juniRouterGroup2  OBJECT-GROUP
    OBJECTS {
        juniRouterNextRouterIndex,
        juniRouterName,
        juniRouterRowStatus,
        juniRouterVrf,
        juniRouterProtocolRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of routers and
        routing protocols in a Juniper product.  This group became obsolete when
        support was added for the router context name."
    ::= { juniRouterGroups 2 }                                     -- JUNOSe 3.0

juniRouterVrfGroup  OBJECT-GROUP
    OBJECTS {
        juniRouterVrfIpv4UnicastImportRouteMap,
        juniRouterVrfIpv4UnicastExportRouteMap,
        juniRouterVrfRouteDistinguisher,
        juniRouterVrfRowStatus,
        juniRouterVrfRouterName,
        juniRouterVrfRouteTargetType,
        juniRouterVrfRouteTargetRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of VRFs within
        routers in a Juniper product.  This group became obsolete when the VRF
        router description object was added."
    ::= { juniRouterGroups 3 }                                     -- JUNOSe 3.0

juniRouterGroup3  OBJECT-GROUP
    OBJECTS {
        juniRouterNextRouterIndex,
        juniRouterName,
        juniRouterRowStatus,
        juniRouterVrf,
        juniRouterProtocolRowStatus,
        juniRouterContextName }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of routers and
        routing protocols in a Juniper product.  This group became obsolete when
        the contect engine ID object was added."
    ::= { juniRouterGroups 4 }                                     -- JUNOSe 4.0

juniRouterVrfGroup2  OBJECT-GROUP
    OBJECTS {
        juniRouterVrfIpv4UnicastImportRouteMap,
        juniRouterVrfIpv4UnicastExportRouteMap,
        juniRouterVrfRouteDistinguisher,
        juniRouterVrfRowStatus,
        juniRouterVrfRouterName,
        juniRouterVrfRouterDescription,
        juniRouterVrfRouteTargetType,
        juniRouterVrfRouteTargetRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of VRFs within
        routers in a Juniper product.  This group became obsolete when the
        global export map and the export map filter option were added."
    ::= { juniRouterGroups 5 }                                     -- JUNOSe 4.0

juniRouterGroup4  OBJECT-GROUP
    OBJECTS {
        juniRouterNextRouterIndex,
        juniRouterName,
        juniRouterRowStatus,
        juniRouterVrf,
        juniRouterProtocolRowStatus,
        juniRouterContextName,
        juniRouterContextEngineID }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of routers and
        routing protocols in a Juniper product.  This group became obsolete when
        the summaryVRfCount object was added."
    ::= { juniRouterGroups 6 }                                     -- JUNOSe 5.0


juniRouterVrfGroup3  OBJECT-GROUP
    OBJECTS {
        juniRouterVrfIpv4UnicastImportRouteMap,
        juniRouterVrfIpv4UnicastExportRouteMap,
        juniRouterVrfRouteDistinguisher,
        juniRouterVrfRowStatus,
        juniRouterVrfRouterName,
        juniRouterVrfRouterDescription,
        juniRouterVrfIpv4UnicastGlobalExportRouteMap,
        juniRouterVrfIpv4UnicastExportRouteMapFilter,
        juniRouterVrfRouteTargetType,
        juniRouterVrfRouteTargetRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of VRFs within
        routers in a Juniper product.  This group became obsolete when the
        global import map was added and when support for separate ipv4 and
        ipv6 route maps was added."
    ::= { juniRouterGroups 7 }                                     -- JUNOSe 5.2

juniRouterGroup5  OBJECT-GROUP
    OBJECTS {
        juniRouterNextRouterIndex,
        juniRouterName,
        juniRouterRowStatus,
        juniRouterVrf,
        juniRouterProtocolRowStatus,
        juniRouterContextName,
        juniRouterContextEngineID,
        juniRouterSummaryVRFCount}
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of routers and routing
        protocols in a Juniper product."
    ::= { juniRouterGroups 8 }                                     -- JUNOSe 6.1

juniRouterSummaryScalarsGroup  OBJECT-GROUP
    OBJECTS {
        juniRouterSummaryNonParentVRsConfigured,
        juniRouterSummaryParentVRsConfigured,
        juniRouterSummaryVRFsConfigured,
        juniRouterSummaryTotalConfigured}
    STATUS      current
    DESCRIPTION
        "A collection of objects providing summary counts for number of virtual routers
        and virtual router forwarding instances (VRFs) in a Juniper product."
    ::= { juniRouterGroups 9 }                                     -- JUNOSe 6.1

juniRouterVrfGroup4  OBJECT-GROUP
    OBJECTS {
        juniRouterVrfIpv4UnicastImportRouteMap,
        juniRouterVrfIpv4UnicastExportRouteMap,
        juniRouterVrfRouteDistinguisher,
        juniRouterVrfRowStatus,
        juniRouterVrfRouterName,
        juniRouterVrfRouterDescription,
        juniRouterVrfIpv4UnicastGlobalExportRouteMap,
        juniRouterVrfIpv4UnicastExportRouteMapFilter,
        juniRouterVrfIpv6UnicastImportRouteMap,
        juniRouterVrfIpv6UnicastExportRouteMap,
        juniRouterVrfIpv6UnicastGlobalExportRouteMap,
        juniRouterVrfIpv6UnicastExportRouteMapFilter,
        juniRouterVrfIpv4UnicastGlobalImportRouteMap,
        juniRouterVrfIpv4UnicastGlobalImportMaxRoutes,
        juniRouterVrfIpv6UnicastGlobalImportRouteMap,
        juniRouterVrfIpv6UnicastGlobalImportMaxRoutes,
        juniRouterVrfRouteTargetType,
        juniRouterVrfRouteTargetRowStatus }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of VRFs within routers in
        a Juniper product."
    ::= { juniRouterGroups 10 }                                    -- JUNOSe 7.1

END
