ALCATEL-IND1-VIRTUAL-CHASSIS-MIB DEFINITIONS ::= BEGIN

IMPORTS
         OBJECT-TYPE,
         OBJECT-IDENTITY,
         MODULE-IDENTITY,
         NOTIFICATION-TYPE,
         Integer32, Unsigned32,
         Counter32, TimeTicks   FROM SNMPv2-SMI
         softentIND1VirtualChassisManager FROM ALCATEL-IND1-BASE
         TruthValue,
         MacAddress,
         TEXTUAL-CONVENTION,
         RowStatus              FROM SNMPv2-TC
         SnmpAdminString        FROM SNMP-FRAMEWORK-MIB
         MODULE-COMPLIANCE,
         OBJECT-GROUP,
         NOTIFICATION-GROUP     FROM SNMPv2-CONF
         InterfaceIndex, InterfaceIndexOrZero         FROM IF-MIB;


alcatelIND1VirtualChassisMIB MODULE-IDENTITY
    LAST-UPDATED "201105250000Z"
    ORGANIZATION "Alcatel-Lucent, Enterprise Solutions Division"
    CONTACT-INFO
     "Please consult with Customer Service to ensure the most appropriate
      version of this document is used with the products in question:

                 Alcatel-Lucent, Enterprise Solutions Division
                (Formerly Alcatel Internetworking, Incorporated)
                        26801 West Agoura Road
                     Agoura Hills, CA  91301-5122
                       United States Of America

     Telephone:               North America  +1 800 995 2696
                              Latin America  +1 877 919 9526
                              Europe         +31 23 556 0100
                              Asia           +65 394 7933
                              All Other      +1 818 878 4507

     Electronic Mail:         support@ind.alcatel.com
     World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
     File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"
    DESCRIPTION
        "This module describes an authoritative enterprise-specific Simple
        etwork Management Protocol (SNMP) Management Information Base (MIB):

        For the Birds Of Prey Product Line, this is the Chassis Supervision
        Chassis MIB
        for managing physical chassis objects not covered in the IETF
        Entity MIB (rfc 2737).

        The right to make changes in specification and other information
        contained in this document without prior notice is reserved.

        No liability shall be assumed for any incidental, indirect, special, or
        consequential damages whatsoever arising from or related to this
        document or the information contained herein.

        Vendors, end-users, and other interested parties are granted
        non-exclusive license to use this specification in connection with
        management of the products for which it is intended to be used.

                   Copyright (C) 1995-2007 Alcatel-Lucent
                       ALL RIGHTS RESERVED WORLDWIDE"

    REVISION      "201105250000Z"

  DESCRIPTION
     "Addressing discrepancies with Alcatel Standard."
     ::= { softentIND1VirtualChassisManager 1 }

    alcatelIND1VirtualChassisMIBNotifications OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Virtual-Chassis manager MIB
            Subsystem Managed Objects."
        ::= { alcatelIND1VirtualChassisMIB 0 }

    alcatelIND1VirtualChassisMIBObjects OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Virtual-Chassis manager MIB
            Subsystem Managed Objects."
        ::= { alcatelIND1VirtualChassisMIB 1 }


    alcatelIND1VirtualChassisMIBConformance OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Chassis Supervision Virtual Chassis MIB
            Subsystem Conformance Information."
        ::= { alcatelIND1VirtualChassisMIB 2}


    alcatelIND1VirtualChassisMIBVCSP OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch for VC Split Protection."
        ::= { alcatelIND1VirtualChassisMIB 3 }

    alcatelIND1VirtualChassisMIBGroups OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Chassis Supervision Virtual Chassis MIB
            Subsystem Units Of Conformance."
        ::= { alcatelIND1VirtualChassisMIBConformance 1 }


    alcatelIND1VirtualChassisMIBCompliances OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Chassis Supervision Virtual Chassis MIB
            Subsystem Compliance Statements."
        ::= { alcatelIND1VirtualChassisMIBConformance 2 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- Virtual-Chassis TEXTUAL-CONVENTION
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

VirtualOperChassisId ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                "Chassis identifier globally unique within a virtual-chassis domain,
                 which is a set of chassis configured to operate together
                 providing virtual-chassis services. When the value of this object
                 is equal to 0, the chassis operates in stand-alone mode; otherwise,
                 the chassis is capable of operating in a virtual-chassis system.
                 This chassis ID is defined as following to do configuration.
                 Standalone mode or boot up:
                          (0) local chassis configuraiton
                 VC mode: (0) all chassis configuration Note: this is not valid for get case
                          (1..6) this indicates chassis id of virtual-chassis mode
                          (101..) this indicates a chassis with duplicated chassis id status"
                SYNTAX Integer32 (0..255)

VirtualConfigChassisId ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                "This is a configuraion for chassis id.
                 (0) if no chassis id been applied
                 (1..6) configure VC valid chassis id"
                SYNTAX Integer32 (0..6)

VirtualChassisHelloInterval ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                "Time interval, in seconds, at which hello messages will be sent to the peer."
                SYNTAX Integer32 (0..65535)

VirtualChassisControlVlan ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual Chassis control vlan."
                SYNTAX Integer32 (2..4094)

VirtualChassisCmmSlot ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "CMM slot indicator."
                SYNTAX INTEGER {
                        notPresent(0),
                        cmmSlot1(65),
                        cmmSlot2(66)
                    }

VirtualChassisNiSlot ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "NI slot indicator."
                SYNTAX Integer32 (0..8)

VirtualChassisVflId ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual Fabric Link Id."
                SYNTAX Integer32 (0..7)

VirtualChassisConsistency ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual-chassis parameter consistency status with master chassis. 
                         inconsis(0): able to compare with master chassis but not consistent 
                         consis(1): able to compare with master chassis and consistent
                         na(2): not able to compare with master chassis since virtual-chassis is not connected yet  
                         disabeled(3):  not able to compare with master because of standalone mode"
                SYNTAX INTEGER {
                        inconsistent(0),
                        consistent(1),
                        na(2),
                        disabled(3)
                    }

VirtualChassisRole ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual-chassis chassis role: 
                         unassigned(0): init chassis role and election not complete yet
                         master(1): indicate chasis is in master role after election
                         slave(2): indicate chasis is in slave role after election
                         inconsistent(3): indicate chassis is not consistent after election
                         startuperror(4): chassis unable to start in virtual-chassis mode"
                SYNTAX INTEGER {
                        unassigned(0),
                        master(1),
                        slave(2),
                        inconsistent(3),
                        startuperror(4)
                    }


VirtualChassisStatus ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual-chassis chassis status: 
                        init(0): init state
                        running(1): running state
                        invalidChassisId(2): invalid chassis id in vcsetup.cfg file
                        helloDown(3): hello down
                        duplicateChassisId(4): duplicate chassis id
                        mismatchImage(5): images cross chassis are mismatching
                        mismatchChassisType(6): slave's chassis type is different compared to the master's value
                        mismatchHelloInterval(7): slave's hello interval is different compared to the master's value
                        mismatchControlVlan(8): slave's control VLAN is different compared to the master's value
                        mismatchGroup(9): slave's chassis group is different compared to the master's value
                        mismatchLicenseConfig(10): slave's license settings are different compared to the master's value
                        invalidLicense(11): invalid license settings
                        splitTopology(12): the topology was split and the slave chassis became isolated from the master
                        commandShutdown(13): chassis shutdown initiated by explicit management command
                        failureShutdown(14): chassis shutdown triggered by a serious initialization failure"
                SYNTAX INTEGER {
                        init(0),
                        running(1),
                        invalidChassisId(2),
                        helloDown(3),
                        duplicateChassisId(4),
                        mismatchImage(5),
                        mismatchChassisType(6),
                        mismatchHelloInterval(7),
                        mismatchControlVlan(8),
                        mismatchGroup(9), 
                        mismatchLicenseConfig(10),
                        invalidLicense(11),
                        splitTopology(12),
                        commandShutdown(13),
                        failureShutdown(14)
                    }

VirtualChassisGroup ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual Chassis group."
                SYNTAX Integer32 (0..255)

VirtualChassisPriority ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual Chassis priority."
                SYNTAX Integer32 (0..255)

VirtualChassisSlotResetStatus ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual-chassis slot reset status: 
                         supported(0): This slot can be reset without spliting virtual chassis setup
                         split(1): Reset this slot will split virtual chassis setup
                         "
                SYNTAX INTEGER {
                        supported(0),
                        split(1)
                    }

VirtualChassisType ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual-chassis chassis type: 
                        invalid(0): Only support Rushmore, Tor, Shasta, Medora, Everest 
                        rushmore(1): OS10k
                        tor(2): OS6900
                        shasta(3): OS6860
                        medora(4): OS9900
                        everest(5): OS6865
                         "
                SYNTAX INTEGER {
                        invalid(0),
                        rushmore(1),
                        tor(2),
                        shasta(3),
                        medora(4),
                        everest(5)
                    }

VirtualChassisVflSpeedType ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual-chassis VFL speed type: 
                        unassigned(0): VFL speed type is unassigned   
                        unkown(1): VFL speed is unknown
                        mismatch(2): This VFL has member ports operating at different speeds 
                        tenGB(3): All member ports of this VFL are operating at 10 Gbps
                        fourtyGB(4): All member ports of this VFL are operating at 40 Gbps
                        twentyOneGB(5): All member ports of this VFL are operating at 21 Gbps
                         "
                SYNTAX INTEGER {
                        unassigned(0),
                        unknown(1),
                        mismatch(2),
                        tenGB(3),
                        fortyGB(4),
                        twentyOneGB(5)
                    }

VirtualChassisVflMode ::= TEXTUAL-CONVENTION
                STATUS current
                DESCRIPTION
                        "Virtual-chassis VFL mode: 
                        static(1): user needs to manually configure vfl and associated vfl member port   
                        auto(2): vfl id will be automatically assigned to proper vfl member port
                         "
                SYNTAX INTEGER {
                        static(1),
                        auto(2)
                    }


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- Virtual-Chassis MIB
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

-- ----------------------------------------------------------
-- Virtual-Chassis Local Info
-- ----------------------------------------------------------

virtualChassisLocalInfo   OBJECT IDENTIFIER ::= { alcatelIND1VirtualChassisMIBObjects 1 }

virtualChassisLocalInfoChasId OBJECT-TYPE
        SYNTAX VirtualOperChassisId
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Virtual Chassis Local chassis ID"
::= { virtualChassisLocalInfo 1 }

-- ----------------------------------------------------------
-- Virtual-Chassis Global Table
-- ----------------------------------------------------------

virtualChassisGlobalTable OBJECT-TYPE
        SYNTAX SEQUENCE OF VirtualChassisGlobalEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Global Table"
::= { alcatelIND1VirtualChassisMIBObjects 2 }

virtualChassisGlobalEntry OBJECT-TYPE
        SYNTAX VirtualChassisGlobalEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Global Table Entry"
        INDEX { virtualChassisOperChasId }
::= { virtualChassisGlobalTable 1 }


VirtualChassisGlobalEntry ::= SEQUENCE
        {
                virtualChassisOperChasId                VirtualOperChassisId,
                virtualChassisConfigChassisId           VirtualConfigChassisId,
                virtualChassisRole                      VirtualChassisRole,
                virtualChassisPreviousRole              VirtualChassisRole,
                virtualChassisStatus                    VirtualChassisStatus,
                virtualChassisOperPriority              VirtualChassisPriority,
                virtualChassisConfigPriority            VirtualChassisPriority,
                virtualChassisGroup                     VirtualChassisGroup,
                virtualChassisMac                       MacAddress,
                virtualChassisUpTime                    TimeTicks,
                virtualChassisDesigNI                   VirtualChassisNiSlot,
                virtualChassisPriCmm                    VirtualChassisCmmSlot,
                virtualChassisSecCmm                    VirtualChassisCmmSlot,
                virtualChassisOperHelloInterval         VirtualChassisHelloInterval,
                virtualChassisOperControlVlan           VirtualChassisControlVlan, 
                virtualChassisConfigHelloInterval       VirtualChassisHelloInterval,
                virtualChassisConfigControlVlan         VirtualChassisControlVlan,
                virtualChassisType                      VirtualChassisType ,
                virtualChassisLicense                   SnmpAdminString ,
                virtualChassisOperChasIdConsis          VirtualChassisConsistency,
                virtualChassisConfigChasIdConsis        VirtualChassisConsistency,
                virtualChassisOperControlVlanConsis     VirtualChassisConsistency,
                virtualChassisConfigControlVlanConsis   VirtualChassisConsistency,
                virtualChassisOperHelloIntervalConsis   VirtualChassisConsistency,
                virtualChassisConfigHelloIntervalConsis VirtualChassisConsistency,
                virtualChassisChassisTypeConsis         VirtualChassisConsistency,
                virtualChassisGroupConsis               VirtualChassisConsistency,
                virtualChassisLicenseConsis             VirtualChassisConsistency,
                virtualChassisGlobalConsis              VirtualChassisConsistency,
                virtualChassisNumOfNeighbor             Integer32 ,
                virtualChassisNumOfDirectNeighbor       Integer32,
                virtualChassisVflMode                   VirtualChassisVflMode

        }
virtualChassisOperChasId OBJECT-TYPE
        SYNTAX VirtualOperChassisId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Operational Virtual-Chassis chassis ID."
::= { virtualChassisGlobalEntry 1 }

virtualChassisConfigChassisId OBJECT-TYPE
        SYNTAX VirtualConfigChassisId
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Configured Virtual-Chassis chassis ID.
        : This object can be configured for the local chassis or for a specific chassis."
    DEFVAL { 0}
::= { virtualChassisGlobalEntry 2 }

virtualChassisRole OBJECT-TYPE
        SYNTAX VirtualChassisRole
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis chassis role"
::= { virtualChassisGlobalEntry 3 }

virtualChassisPreviousRole OBJECT-TYPE
        SYNTAX VirtualChassisRole
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis previous chassis role"
::= { virtualChassisGlobalEntry 4 }

virtualChassisStatus OBJECT-TYPE
        SYNTAX      VirtualChassisStatus
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "Virtual-Chassis chassis status"
::= { virtualChassisGlobalEntry 5 }

virtualChassisOperPriority OBJECT-TYPE
        SYNTAX VirtualChassisPriority
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis operational chassis priority"
::= { virtualChassisGlobalEntry 6 }

virtualChassisConfigPriority OBJECT-TYPE
        SYNTAX VirtualChassisPriority
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Virtual-Chassis configured chassis priority
        This object can be configured for the local chassis and for a specific chassis."
DEFVAL { 100 }
::= { virtualChassisGlobalEntry 7 }

virtualChassisGroup OBJECT-TYPE
        SYNTAX VirtualChassisGroup
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Virtual-Chassis chassis group.
        When a master chassis is present in the topology, the chassis group can only be configured according to the following rules:
        1. With exactly the same chassis group value as the current master chassis when the configuration applies to a single and specific chassis.   
        2. With any value within the valid range as long as the configuration applies to all chassis at the same time." 
DEFVAL { 0}
::= { virtualChassisGlobalEntry 8 }

virtualChassisMac OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis chassis mac address."
::= { virtualChassisGlobalEntry 9 }

virtualChassisUpTime OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis chassis up time"
::= { virtualChassisGlobalEntry 10 }

virtualChassisDesigNI OBJECT-TYPE
        SYNTAX VirtualChassisNiSlot
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis designated NI slot num"
::= { virtualChassisGlobalEntry 11 }

virtualChassisPriCmm OBJECT-TYPE
        SYNTAX VirtualChassisCmmSlot
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis primary CMM slot num"
::= { virtualChassisGlobalEntry 12 }

virtualChassisSecCmm OBJECT-TYPE
        SYNTAX VirtualChassisCmmSlot 
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis secondary CMM slot num"
::= { virtualChassisGlobalEntry 13 }

virtualChassisOperHelloInterval OBJECT-TYPE
        SYNTAX VirtualChassisHelloInterval
        UNITS           "seconds"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Operational Virtual-Chassis hello interval."
DEFVAL {10}
::= { virtualChassisGlobalEntry 14 }

virtualChassisOperControlVlan OBJECT-TYPE
        SYNTAX VirtualChassisControlVlan
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Operational Virtual-Chassis control VLAN."
::= { virtualChassisGlobalEntry 15 }

virtualChassisConfigHelloInterval OBJECT-TYPE
        SYNTAX VirtualChassisHelloInterval
        UNITS           "seconds"
        MAX-ACCESS read-write
        STATUS deprecated
        DESCRIPTION
        "This is deprecated from release 7.3.3.R01."
DEFVAL {2}
::= { virtualChassisGlobalEntry 16 }

virtualChassisConfigControlVlan OBJECT-TYPE
        SYNTAX VirtualChassisControlVlan
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Configured Virtual-Chassis control VLAN.
        This object can be configured for the local chassis, for a specific chassis and for all chassis."
DEFVAL { 4094}
::= { virtualChassisGlobalEntry 17 }

virtualChassisType OBJECT-TYPE
        SYNTAX VirtualChassisType
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis chassis type"
::= { virtualChassisGlobalEntry 18 }

virtualChassisLicense OBJECT-TYPE
        SYNTAX SnmpAdminString (SIZE (0..255))
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis chassis License string. A: Advanced; B: Data Center"
::= { virtualChassisGlobalEntry 19 }

virtualChassisOperChasIdConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 20 }

virtualChassisConfigChasIdConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 21 }

virtualChassisOperControlVlanConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 22 }

virtualChassisConfigControlVlanConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 23 }

virtualChassisOperHelloIntervalConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared hello interval with master chassis"
::= { virtualChassisGlobalEntry 24 }

virtualChassisConfigHelloIntervalConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS deprecated
        DESCRIPTION
        "This is deprecated from release 7.3.3.R01."
::= { virtualChassisGlobalEntry 25 }

virtualChassisChassisTypeConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 26 }

virtualChassisGroupConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 27 }

virtualChassisLicenseConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 28 }

virtualChassisGlobalConsis OBJECT-TYPE
        SYNTAX VirtualChassisConsistency
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis consis status compared with master chassis"
::= { virtualChassisGlobalEntry 29 }

virtualChassisNumOfNeighbor OBJECT-TYPE
        SYNTAX Integer32 (0..65535)
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis neighbor count"
::= { virtualChassisGlobalEntry 30 }


virtualChassisNumOfDirectNeighbor OBJECT-TYPE
        SYNTAX Integer32 (0..65535)
        MAX-ACCESS  read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis direct neighbor count"
::= { virtualChassisGlobalEntry 31 }

virtualChassisVflMode OBJECT-TYPE
        SYNTAX VirtualChassisVflMode
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Virtual-Chassis vfl mode:        
        static(0): user needs to manually configure vfl and associated vfl member port   
        auto(1): vfl id will be automatically assigned to proper vfl member port" 
DEFVAL {static}
::= { virtualChassisGlobalEntry 32 }

-- ----------------------------------------------------------
-- Virtual-Chassis Neighbor Table
-- ----------------------------------------------------------

virtualChassisNeighborTable OBJECT-TYPE
        SYNTAX SEQUENCE OF VirtualChassisNeighborEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Neighbor Table"
::= { alcatelIND1VirtualChassisMIBObjects 3 }

virtualChassisNeighborEntry OBJECT-TYPE
        SYNTAX VirtualChassisNeighborEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Neighbor Table Entry"
        INDEX { virtualChassisOperChasId, virtualChassisNeighborChasId }
::= { virtualChassisNeighborTable 1 }


VirtualChassisNeighborEntry ::= SEQUENCE
        {
                virtualChassisNeighborChasId            VirtualOperChassisId,
                virtualChassisNeighborShortestPath      SnmpAdminString,
                virtualChassisNeighborIsDirect          TruthValue
        }
virtualChassisNeighborChasId OBJECT-TYPE
        SYNTAX VirtualOperChassisId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual-Chassis Neighbor chassis ID."
::= { virtualChassisNeighborEntry 1 }

virtualChassisNeighborShortestPath OBJECT-TYPE
        SYNTAX SnmpAdminString (SIZE (0..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Configured Virtual-Chassis neighbor shortest path. The format will be <chass_id>/<vfl_id>-><chass_id>/<vfl_id>-><chass_id>/<vfl_id>. EX: 2/0->1/0->3/1 "
::= { virtualChassisNeighborEntry 2 }

virtualChassisNeighborIsDirect OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
        "To determine if this is a direct neighbor"
::= { virtualChassisNeighborEntry 3 }

-- ----------------------------------------------------------
-- Virtual-Chassis Chassis Reset List Table
-- ----------------------------------------------------------

virtualChassisChassisResetListTable OBJECT-TYPE
        SYNTAX SEQUENCE OF VirtualChassisChassisResetListEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Chassis reset list Table"
::= { alcatelIND1VirtualChassisMIBObjects 4}

virtualChassisChassisResetListEntry OBJECT-TYPE
        SYNTAX VirtualChassisChassisResetListEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Chassis Reset List Table Entry"
        INDEX { virtualChassisOperChasId}
::= { virtualChassisChassisResetListTable 1 }


VirtualChassisChassisResetListEntry ::= SEQUENCE
        {
                virtualChassisChassisResetList          SnmpAdminString
        }

virtualChassisChassisResetList OBJECT-TYPE
        SYNTAX SnmpAdminString (SIZE (0..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Indicate the chassis reset list."
::= { virtualChassisChassisResetListEntry 1 }


-- ----------------------------------------------------------
-- Virtual-Chassis Slot Reset List Table
-- ----------------------------------------------------------

virtualChassisSlotResetStatusTable OBJECT-TYPE
        SYNTAX SEQUENCE OF VirtualChassisSlotResetStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Slot reset Status Table"
::= { alcatelIND1VirtualChassisMIBObjects 5 }

virtualChassisSlotResetStatusEntry OBJECT-TYPE
        SYNTAX VirtualChassisSlotResetStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Slot Reset Status Table Entry"
        INDEX { virtualChassisOperChasId,virtualChassisSlotNum}
::= { virtualChassisSlotResetStatusTable 1 }

VirtualChassisSlotResetStatusEntry ::= SEQUENCE
        {
                virtualChassisSlotNum                   VirtualChassisNiSlot,
                virtualChassisSlotResetStatus           VirtualChassisSlotResetStatus
        }

virtualChassisSlotNum OBJECT-TYPE
        SYNTAX VirtualChassisNiSlot
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual-Chassis slot num."
::= { virtualChassisSlotResetStatusEntry 1 }

virtualChassisSlotResetStatus OBJECT-TYPE
        SYNTAX VirtualChassisSlotResetStatus
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Virtual-Chassis slot reset status."
::= { virtualChassisSlotResetStatusEntry 2}

-- ----------------------------------------------------------
-- Virtual-Chassis Vfl Table
-- ----------------------------------------------------------

virtualChassisVflTable OBJECT-TYPE
        SYNTAX SEQUENCE OF VirtualChassisVflEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Virtual Fabric Link Table
        This object can be configured for the local chassis or for a specific chassis."
::= { alcatelIND1VirtualChassisMIBObjects 6 }

virtualChassisVflEntry OBJECT-TYPE
        SYNTAX VirtualChassisVflEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Chassis Virtual Fabric Link Table Entry"
        INDEX { virtualChassisOperChasId, virtualChassisVflId }
::= { virtualChassisVflTable 1 }


VirtualChassisVflEntry ::= SEQUENCE
        {
                virtualChassisVflId              VirtualChassisVflId,
                virtualChassisVflDefaultVlan     Integer32,
                virtualChassisVflOperStatus      INTEGER,
                virtualChassisVflPrimaryPort     InterfaceIndexOrZero,
                virtualChassisVflActivePortNum   Integer32,
                virtualChassisVflConfigPortNum   Integer32,
                virtualChassisVflRowStatus       RowStatus,
                virtualChassisVflDirectNeighborChasId       VirtualOperChassisId,
                virtualChassisVflSpeedType       VirtualChassisVflSpeedType
        }

virtualChassisVflId OBJECT-TYPE
        SYNTAX VirtualChassisVflId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Virtual Fabric Link Interface IfIndex"
::= { virtualChassisVflEntry 1 }

virtualChassisVflDefaultVlan OBJECT-TYPE
        SYNTAX Integer32 (1..4094)
        MAX-ACCESS read-create
        STATUS deprecated
        DESCRIPTION
        "Virtual Fabric Link default vlan"
    DEFVAL { 1}
::= { virtualChassisVflEntry 2 }

virtualChassisVflOperStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        disabled(0),
                        up(1),
                        down(2)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "Virtual Fabric Link Operational Status"
::= { virtualChassisVflEntry 3 }

virtualChassisVflPrimaryPort OBJECT-TYPE
        SYNTAX InterfaceIndexOrZero
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "Virtual Fabric Link primary Port ifindex. 0 is for default value when virtual fabric link is not up"
::= { virtualChassisVflEntry 4 }

virtualChassisVflActivePortNum OBJECT-TYPE
        SYNTAX Integer32 (0..8)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "Number of active member ports of participating on the Virtual Fabric Link."
::= { virtualChassisVflEntry 5 }

virtualChassisVflConfigPortNum OBJECT-TYPE
        SYNTAX Integer32 (0..8)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "Number of ports configured as members of the Virtual Fabric Link."
::= { virtualChassisVflEntry 6 }

virtualChassisVflRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
        "Virtual Fabric Link RowStatus for creationh and deletion"
::= { virtualChassisVflEntry 7 }

virtualChassisVflDirectNeighborChasId OBJECT-TYPE
        SYNTAX VirtualOperChassisId
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The Chassis ID of the direct neighbor that is reachable via this VFL link,
         or 0 if no neighbor."
::= { virtualChassisVflEntry 8 }

virtualChassisVflSpeedType OBJECT-TYPE
        SYNTAX VirtualChassisVflSpeedType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "Virtual Fabric Link speed type"
::= { virtualChassisVflEntry 9 }


-- ----------------------------------------------------------
-- Virtual-Chassis Vfl Member Port Table
-- ----------------------------------------------------------

virtualChassisVflMemberPortTable OBJECT-TYPE
        SYNTAX SEQUENCE OF VirtualChassisVflMemberPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Fabric Link Member Port Table.
        This object can be configured for the local chassis or for a specific chassis."
::= { alcatelIND1VirtualChassisMIBObjects 7 }


virtualChassisVflMemberPortEntry OBJECT-TYPE
        SYNTAX VirtualChassisVflMemberPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Fabric Link Member Port Table Entry."
        INDEX { virtualChassisOperChasId, 
                virtualChassisVflId, 
                virtualChassisVflMemberPortIfindex }
::= { virtualChassisVflMemberPortTable 1 }

VirtualChassisVflMemberPortEntry ::= SEQUENCE
        {
                virtualChassisVflMemberPortIfindex       InterfaceIndex,
                virtualChassisVflMemberPortIsPrimay      TruthValue,
                virtualChassisVflMemberPortOperStatus        INTEGER,
                virtualChassisVflMemberPortRowStatus     RowStatus
        }

virtualChassisVflMemberPortIfindex OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
        "Virtual Fabric Link Member Port ifIndex."
::= { virtualChassisVflMemberPortEntry 1 }


virtualChassisVflMemberPortIsPrimay OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
        "To determine if this Virtual Fabric Link Member Port is primary or not"
::= { virtualChassisVflMemberPortEntry 2 }

virtualChassisVflMemberPortOperStatus OBJECT-TYPE
                SYNTAX INTEGER
                    {
                        disabled(0),
                        up(1),
                        down(2)
                    }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
        "Virtual Fabric Link Member Port operational status"
::= { virtualChassisVflMemberPortEntry 3 }

virtualChassisVflMemberPortRowStatus OBJECT-TYPE
                SYNTAX RowStatus
                MAX-ACCESS read-create
                STATUS current
                DESCRIPTION
        "Virtual Fabric Link Member Port RowStatus for creation and deletion"
::= { virtualChassisVflMemberPortEntry 4 }

-- ----------------------------------------------------------
-- Virtual-Chassis Trap info
-- ----------------------------------------------------------

virtualChassisTrapInfo   OBJECT IDENTIFIER ::= { alcatelIND1VirtualChassisMIBObjects 8 }

virtualChassisDiagnostic OBJECT-TYPE
        SYNTAX INTEGER {
                duplexMode (1),
                speed (2)
               }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Indicates why a port configured as virtual-fabric member is unable to join the virtual-fabric link"
::= { virtualChassisTrapInfo 1 }

virtualChassisUpgradeCompleteStatus OBJECT-TYPE
        SYNTAX INTEGER {
                success (1),
                failure (2)
               }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Indicates whether the software upgrade process has failed after a timeout or completed successfully.
        Note that if the process fails, it may be still possible for the system to recover if the process
        successfully completes later after the expired timeout." 

::= { virtualChassisTrapInfo 2 }

-- ----------------------------------------------------------
-- Virtual-Chassis auto-Vfl Port Table
-- ----------------------------------------------------------

virtualChassisAutoVflPortTable OBJECT-TYPE
        SYNTAX SEQUENCE OF VirtualChassisAutoVflPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Auto Virtual Fabric Link Port Table."
::= { alcatelIND1VirtualChassisMIBObjects 9 }


virtualChassisAutoVflPortEntry OBJECT-TYPE
        SYNTAX VirtualChassisAutoVflPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Virtual Fabric Link Member Port Table Entry."
        INDEX { virtualChassisAutoVflPortIfindex }
::= { virtualChassisAutoVflPortTable 1 }

VirtualChassisAutoVflPortEntry ::= SEQUENCE
        {
                virtualChassisAutoVflPortIfindex                InterfaceIndex,
                virtualChassisAutoVflIfindex                    InterfaceIndexOrZero,
                virtualChassisAutoVflPortMemberStatus           INTEGER,
                virtualChassisAutoVflPortRowStatus     RowStatus
        }

virtualChassisAutoVflPortIfindex OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
        "Auto virtual Fabric Link Member Port ifIndex."
::= { virtualChassisAutoVflPortEntry 1 }


virtualChassisAutoVflIfindex OBJECT-TYPE
                SYNTAX InterfaceIndexOrZero
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
        "Virtual Fabric Link ifIndex which is automatically assigned to this member port"
::= { virtualChassisAutoVflPortEntry 2 }

virtualChassisAutoVflPortMemberStatus OBJECT-TYPE
                SYNTAX INTEGER
                    {
                        up(1),
                        down(2),
                        unassigned(3)
                    }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
        "Auto Virtual Fabric Link Port Member Port operational status"
::= { virtualChassisAutoVflPortEntry 3 }

virtualChassisAutoVflPortRowStatus OBJECT-TYPE
                SYNTAX RowStatus
                MAX-ACCESS read-create
                STATUS current
                DESCRIPTION
        "Auto Virtual Fabric Link Port RowStatus for creation and deletion"
::= { virtualChassisAutoVflPortEntry 4 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
--  NOTIFICATIONS
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

        virtualChassisStatusChange NOTIFICATION-TYPE
           OBJECTS {
                virtualChassisOperChasId,
                virtualChassisStatus
           }
           STATUS   current
           DESCRIPTION
               "Critical trap indicates chassis status change."
           ::= { alcatelIND1VirtualChassisMIBNotifications 1 }

        virtualChassisRoleChange NOTIFICATION-TYPE
           OBJECTS {
                virtualChassisOperChasId,
                virtualChassisRole
           }
           STATUS   current
           DESCRIPTION
               "Critical trap indicates chassis role change."
           ::= { alcatelIND1VirtualChassisMIBNotifications 2 }

        
        virtualChassisVflStatusChange NOTIFICATION-TYPE
           OBJECTS {
                virtualChassisOperChasId, 
                virtualChassisVflId, 
                virtualChassisVflOperStatus
           }
           STATUS   current
           DESCRIPTION
               "Critical trap indicates vflink status change."
           ::= { alcatelIND1VirtualChassisMIBNotifications 3 }
        
        virtualChassisVflMemberPortStatusChange NOTIFICATION-TYPE
           OBJECTS {
                virtualChassisOperChasId, 
                virtualChassisVflId, 
                virtualChassisVflMemberPortIfindex,
                virtualChassisVflMemberPortOperStatus
           }
           STATUS   deprecated
           DESCRIPTION
               "This trap is been deprecated since 7.3.3.R01."
           ::= { alcatelIND1VirtualChassisMIBNotifications 4 }

        virtualChassisVflMemberPortJoinFailure NOTIFICATION-TYPE
           OBJECTS {
                virtualChassisOperChasId, 
                virtualChassisVflId, 
                virtualChassisVflMemberPortIfindex,  
                virtualChassisDiagnostic
           }
           STATUS   current
           DESCRIPTION
               "Major trap indicates a port configured as virtual-fabric member is unable to join the virtual-fabric link."
           ::= { alcatelIND1VirtualChassisMIBNotifications 5 }

        virtualChassisUpgradeComplete NOTIFICATION-TYPE
           OBJECTS {
                virtualChassisUpgradeCompleteStatus
           }
           STATUS   current
           DESCRIPTION
               "Critical trap that indicates whether the software upgrade process has failed after a timeout or completed successfully.
                Note that if the process fails, it may be still possible for the system to recover if the process
                successfully completes later after the expired timeout." 
           ::= { alcatelIND1VirtualChassisMIBNotifications 6 }

        virtualChassisVflSpeedTypeChange NOTIFICATION-TYPE
           OBJECTS {
                virtualChassisOperChasId, 
                virtualChassisVflId, 
                virtualChassisVflSpeedType
           }
           STATUS   current
           DESCRIPTION
               "Critical trap indicates whenever vfl speed type is changed."
           ::= { alcatelIND1VirtualChassisMIBNotifications 7 }
   
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- COMPLIANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

    alcatelIND1VirtualChassisMIBCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
            "Compliance statement for Virtual-Chassis Supervision."
        MODULE
            MANDATORY-GROUPS
            {

                virtualChassisLocalInfoGroup,
                virtualChassisGlobalGroup,
                virtualChassisNeighborGroup,
                virtualChassisChassisResetListGroup,
                virtualChassisSlotRestStatusGroup,
                virtualChassisVflGroup,
                virtualChassisVflMemberPortGroup

            }
        ::= { alcatelIND1VirtualChassisMIBCompliances 1 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- UNITS OF CONFORMANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
        virtualChassisLocalInfoGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisLocalInfoChasId
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis Config Group."

        ::= { alcatelIND1VirtualChassisMIBGroups 1 }    

    virtualChassisGlobalGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisConfigChassisId,
                virtualChassisRole,
                virtualChassisPreviousRole,
                virtualChassisStatus,
                virtualChassisOperPriority,
                virtualChassisConfigPriority,
                virtualChassisGroup,
                virtualChassisMac,
                virtualChassisUpTime,
                virtualChassisDesigNI,
                virtualChassisPriCmm,
                virtualChassisSecCmm,
                virtualChassisOperHelloInterval,
                virtualChassisOperControlVlan, 
                virtualChassisConfigHelloInterval,
                virtualChassisConfigControlVlan,
                virtualChassisType,
                virtualChassisLicense,
                virtualChassisOperChasIdConsis,
                virtualChassisConfigChasIdConsis,
                virtualChassisOperControlVlanConsis,
                virtualChassisConfigControlVlanConsis,
                virtualChassisOperHelloIntervalConsis,
                virtualChassisConfigHelloIntervalConsis,
                virtualChassisChassisTypeConsis,
                virtualChassisGroupConsis,
                virtualChassisLicenseConsis,
                virtualChassisGlobalConsis,
                virtualChassisNumOfNeighbor,
                virtualChassisNumOfDirectNeighbor,
                virtualChassisVflMode
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis Config Group."

        ::= { alcatelIND1VirtualChassisMIBGroups 2 }

        virtualChassisNeighborGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisNeighborShortestPath,
                virtualChassisNeighborIsDirect
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis neighbor Group."

        ::= { alcatelIND1VirtualChassisMIBGroups 3 }    
 
  
        virtualChassisChassisResetListGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisChassisResetList
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis chassis reset list Group."

        ::= { alcatelIND1VirtualChassisMIBGroups 4 }    

        virtualChassisSlotRestStatusGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisSlotResetStatus
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis slot reset statusGroup."

        ::= { alcatelIND1VirtualChassisMIBGroups 5 }  

    virtualChassisVflGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisVflDefaultVlan,
                virtualChassisVflOperStatus,
                virtualChassisVflPrimaryPort,
                virtualChassisVflActivePortNum,
                virtualChassisVflConfigPortNum,
                virtualChassisVflRowStatus,
                virtualChassisVflDirectNeighborChasId,
                virtualChassisVflSpeedType
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis Vfl Group."
        ::= { alcatelIND1VirtualChassisMIBGroups 6 }
    virtualChassisVflMemberPortGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisVflMemberPortIsPrimay,
                virtualChassisVflMemberPortOperStatus,
                virtualChassisVflMemberPortRowStatus
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis Vfl Member Port Group."
        ::= { alcatelIND1VirtualChassisMIBGroups 7 }

  virtualChassisTrapInfoGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisDiagnostic,
                virtualChassisUpgradeCompleteStatus
        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis trap info Group."
        ::= { alcatelIND1VirtualChassisMIBGroups 8 }

  virtualChassisTrapOBJGroup NOTIFICATION-GROUP
        NOTIFICATIONS
        {
                virtualChassisStatusChange,
                virtualChassisRoleChange,
                virtualChassisVflStatusChange,
                virtualChassisVflMemberPortStatusChange,
                virtualChassisVflMemberPortJoinFailure,
                virtualChassisUpgradeComplete,
                virtualChassisVflSpeedTypeChange

        }
        STATUS  current
        DESCRIPTION
            "Chassis Supervision Virtual-Chassis trap object Group."
        ::= { alcatelIND1VirtualChassisMIBGroups 9 }

    virtualChassisAutoVflPortGroup OBJECT-GROUP
        OBJECTS
        {
                virtualChassisAutoVflIfindex,
                virtualChassisAutoVflPortMemberStatus,
                virtualChassisAutoVflPortRowStatus
        }
        STATUS  current
        DESCRIPTION
            "Auto Virtual-Chassis Vfl Port Group."
        ::= { alcatelIND1VirtualChassisMIBGroups 10 }

END

