-- *****************************************************************
-- Meru Networks Enterprise Specific MIB
--
-- Copyright (c) 2005 by Meru Networks
-- All rights reserved
--
-- *****************************************************************

MERU-TOPOLOGY-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    NOTIFICATION-TYPE, 
    OBJECT-TYPE, 
    MODULE-IDENTITY, 
    OBJECT-IDENTITY,
    enterprises, 
    Counter32, 
    Counter64, 
    Gauge32, 
    TimeTicks, 
    IpAddress, 
    Integer32
        FROM SNMPv2-SMI
    Ipv6Address
        FROM IPV6-TC
    TEXTUAL-CONVENTION, 
    TimeInterval, 
    TimeStamp,
    DateAndTime, 
    TruthValue, 
    DisplayString, 
    MacAddress, 
    RowStatus
        FROM SNMPv2-TC
    mwConfiguration
        FROM MERU-SMI
    MwlEncryptionAlgorithm,
    MwlCapabilityModeBits,
    MwlApType,
    MwlApIfModeType,
    MwlAssociationState,
    MwlOnOffSwitch
        FROM MERU-TC;

  mwTopology  MODULE-IDENTITY
    LAST-UPDATED "200506050000Z"
    ORGANIZATION "Meru Networks"
    CONTACT-INFO "support@merunetworks.com"
    DESCRIPTION
        "This MIB defines all the managed objects used to manage the Meru WLAN 
         Topology Configuration infrastructure"
    ::= { mwConfiguration 13 } 
  
    
  
  mwApAssignedTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApAssignedEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Assigned Stations "
    ::= { mwTopology 1 }

  mwApAssignedEntry  OBJECT-TYPE
    SYNTAX MwApAssignedEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Assigned Stations "
    INDEX {  mwApAssignedTableIndex  }
    ::= { mwApAssignedTable 1 }

  MwApAssignedEntry  ::=  SEQUENCE { 
       mwApAssignedTableIndex                                      Integer32, 
       mwApAssignedApMac                                           MacAddress,
       mwApAssignedEssid                                           DisplayString,
       mwApAssigneddbState                                         MwlAssociationState,
       mwApAssignedPrevRssi                                        Integer32,
       mwApAssignedRxPackets                                       Unsigned32,
       mwApAssignedTxPackets                                       Unsigned32,
       mwApAssignedRadioType                                       MwlApIfModeType,
       mwApAssignedAuthKeyType                                     MwlEncryptionAlgorithm,
       mwApAssignedCurrentRssi                                     Integer32,
       mwApAssignedVirtualPort                                     MacAddress,
       mwApAssignedNmsApNodeId                                     Integer32,
       mwApAssignedApDeviceType                                    MwlApType,
       mwApAssignedLastActivity                                    TimeTicks,
       mwApAssignedCapabilities                                    MwlCapabilityModeBits,
       mwApAssignedNmsApNodeName                                   DisplayString 
  }
   
   
  mwApAssignedTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApAssignedEntry 1 }

  mwApAssignedApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Client MAC"
    ::= { mwApAssignedEntry    2 }

  mwApAssignedEssid  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes SSID"
    ::= { mwApAssignedEntry    3 }

  mwApAssigneddbState  OBJECT-TYPE
    SYNTAX MwlAssociationState
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Association State"
    ::= { mwApAssignedEntry    4 }

  mwApAssignedPrevRssi  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Previous RSSI"
    ::= { mwApAssignedEntry    5 }

  mwApAssignedRxPackets  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Packets Received"
    ::= { mwApAssignedEntry    6 }

  mwApAssignedTxPackets  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Packets Sent"
    ::= { mwApAssignedEntry    7 }

  mwApAssignedRadioType  OBJECT-TYPE
    SYNTAX MwlApIfModeType
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes RF Band"
    ::= { mwApAssignedEntry    8 }

  mwApAssignedAuthKeyType  OBJECT-TYPE
    SYNTAX MwlEncryptionAlgorithm
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Key Type"
    ::= { mwApAssignedEntry    9 }

  mwApAssignedCurrentRssi  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Current RSSI"
    ::= { mwApAssignedEntry   10 }

  mwApAssignedNmsApNodeId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwApAssignedEntry   11 }

  mwApAssignedApDeviceType  OBJECT-TYPE
    SYNTAX MwlApType
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Type"
    ::= { mwApAssignedEntry   12 }

  mwApAssignedLastActivity  OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Last Activity"
    ::= { mwApAssignedEntry   13 }

  mwApAssignedNmsApNodeName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwApAssignedEntry   14 }

  mwApAssignedVirtualPort  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Virtual Port"
    ::= { mwApAssignedEntry   15 }

  mwApAssignedCapabilities  OBJECT-TYPE
    SYNTAX MwlCapabilityModeBits
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Capabilities"
    ::= { mwApAssignedEntry   16 }

  mwApDiscoveredTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApDiscoveredEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Discovered APs and Stations "
    ::= { mwTopology 2 }

  mwApDiscoveredEntry  OBJECT-TYPE
    SYNTAX MwApDiscoveredEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Discovered APs and Stations "
    INDEX {  mwApDiscoveredTableIndex  }
    ::= { mwApDiscoveredTable 1 }

  MwApDiscoveredEntry  ::=  SEQUENCE { 
       mwApDiscoveredTableIndex                                    Integer32, 
       mwApDiscoveredApMac                                         MacAddress,
       mwApDiscoveredEssid                                         DisplayString,
       mwApDiscoveredBssid                                         MacAddress,
       mwApDiscoveredChannel                                       Unsigned32,
       mwApDiscoveredPrevRssi                                      Integer32,
       mwApDiscoveredRxPackets                                     Unsigned32,
       mwApDiscoveredRadioType                                     MwlApIfModeType,
       mwApDiscoveredWiredRogue                                    MwlOnOffSwitch,
       mwApDiscoveredCurrentRssi                                   Integer32,
       mwApDiscoveredNmsApNodeId                                   Integer32,
       mwApDiscoveredApDeviceType                                  MwlApType,
       mwApDiscoveredLastActivity                                  TimeTicks,
       mwApDiscoveredNmsApNodeName                                 DisplayString,
       mwApDiscoveredConfirmedChannel                              Unsigned32 
  }
   
   
  mwApDiscoveredTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApDiscoveredEntry 1 }

  mwApDiscoveredApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes MAC Address"
    ::= { mwApDiscoveredEntry    2 }

  mwApDiscoveredEssid  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes SSID"
    ::= { mwApDiscoveredEntry    3 }

  mwApDiscoveredBssid  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes BSSID"
    ::= { mwApDiscoveredEntry    4 }

  mwApDiscoveredChannel  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Operated Channel"
    ::= { mwApDiscoveredEntry    5 }

  mwApDiscoveredPrevRssi  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Previous RSSI"
    ::= { mwApDiscoveredEntry    6 }

  mwApDiscoveredRxPackets  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Packets Received"
    ::= { mwApDiscoveredEntry    7 }

  mwApDiscoveredRadioType  OBJECT-TYPE
    SYNTAX MwlApIfModeType
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes RF Band"
    ::= { mwApDiscoveredEntry    8 }

  mwApDiscoveredWiredRogue  OBJECT-TYPE
    SYNTAX MwlOnOffSwitch
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Rogue Detected on the wire"
    ::= { mwApDiscoveredEntry    9 }

  mwApDiscoveredCurrentRssi  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Current RSSI"
    ::= { mwApDiscoveredEntry   10 }

  mwApDiscoveredNmsApNodeId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwApDiscoveredEntry   11 }

  mwApDiscoveredApDeviceType  OBJECT-TYPE
    SYNTAX MwlApType
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Device Type"
    ::= { mwApDiscoveredEntry   12 }

  mwApDiscoveredLastActivity  OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Last activity"
    ::= { mwApDiscoveredEntry   13 }

  mwApDiscoveredNmsApNodeName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwApDiscoveredEntry   14 }

  mwApDiscoveredConfirmedChannel  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Confirmed-Channel"
    ::= { mwApDiscoveredEntry   15 }

  mwTopoApTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwTopoApEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Wireless Resources "
    ::= { mwTopology 4 }

  mwTopoApEntry  OBJECT-TYPE
    SYNTAX MwTopoApEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Wireless Resources "
    INDEX {  mwTopoApTableIndex  }
    ::= { mwTopoApTable 1 }

  MwTopoApEntry  ::=  SEQUENCE { 
       mwTopoApTableIndex                                          Integer32, 
       mwTopoApNodeId                                              Unsigned32,
       mwTopoApNodeName                                            DisplayString,
       mwTopoApAttachedCount                                       Unsigned32,
       mwTopoApAssignedCount                                       Unsigned32,
       mwTopoApNeighborsCount                                      Unsigned32,
       mwTopoApResourceRequest                                     Unsigned32,
       mwTopoApResourceAllocated                                   Unsigned32 
  }
   
   
  mwTopoApTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwTopoApEntry 1 }

  mwTopoApNodeId  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwTopoApEntry    2 }

  mwTopoApNodeName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwTopoApEntry    3 }

  mwTopoApAttachedCount  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Attached Count"
    ::= { mwTopoApEntry    4 }

  mwTopoApAssignedCount  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Assigned Count"
    ::= { mwTopoApEntry    5 }

  mwTopoApNeighborsCount  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Neighbor Count"
    ::= { mwTopoApEntry    6 }

  mwTopoApResourceRequest  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Resource Requested"
    ::= { mwTopoApEntry    7 }

  mwTopoApResourceAllocated  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Resource Allocated"
    ::= { mwTopoApEntry    8 }

  mwTopoApapTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwTopoApapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Number of AP edges "
    ::= { mwTopology 5 }

  mwTopoApapEntry  OBJECT-TYPE
    SYNTAX MwTopoApapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Number of AP edges "
    INDEX {  mwTopoApapTableIndex  }
    ::= { mwTopoApapTable 1 }

  MwTopoApapEntry  ::=  SEQUENCE { 
       mwTopoApapTableIndex                                        Integer32, 
       mwTopoApapHeadId                                            Unsigned32,
       mwTopoApapTailId                                            Unsigned32,
       mwTopoApapHeadName                                          DisplayString,
       mwTopoApapTailName                                          DisplayString 
  }
   
   
  mwTopoApapTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwTopoApapEntry 1 }

  mwTopoApapHeadId  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Detecting AP ID"
    ::= { mwTopoApapEntry    2 }

  mwTopoApapTailId  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Sibling AP ID"
    ::= { mwTopoApapEntry    3 }

  mwTopoApapHeadName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Detecting AP Name"
    ::= { mwTopoApapEntry    4 }

  mwTopoApapTailName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Sibling AP Name"
    ::= { mwTopoApapEntry    5 }

  mwTopoStaTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwTopoStaEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Stations Topology "
    ::= { mwTopology 6 }

  mwTopoStaEntry  OBJECT-TYPE
    SYNTAX MwTopoStaEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Stations Topology "
    INDEX {  mwTopoStaTableIndex  }
    ::= { mwTopoStaTable 1 }

  MwTopoStaEntry  ::=  SEQUENCE { 
       mwTopoStaTableIndex                                         Integer32, 
       mwTopoStaBssId                                              MacAddress,
       mwTopoStaMssId                                              MacAddress,
       mwTopoStaMacAddress                                         MacAddress,
       mwTopoStaAssocState                                         MwlAssociationState,
       mwTopoStaAssignedAp                                         Unsigned32,
       mwTopoStaHandoffTime                                        DateAndTime,
       mwTopoStaLastActiveTime                                     DateAndTime,
       mwTopoStaAssignedApName                                     DisplayString 
  }
   
   
  mwTopoStaTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwTopoStaEntry 1 }

  mwTopoStaBssId  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes BSSID"
    ::= { mwTopoStaEntry    2 }

  mwTopoStaMssId  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes MSSID"
    ::= { mwTopoStaEntry    3 }

  mwTopoStaMacAddress  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes MAC Address"
    ::= { mwTopoStaEntry    4 }

  mwTopoStaAssocState  OBJECT-TYPE
    SYNTAX MwlAssociationState
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Association State"
    ::= { mwTopoStaEntry    5 }

  mwTopoStaAssignedAp  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Assigned AP"
    ::= { mwTopoStaEntry    6 }

  mwTopoStaHandoffTime  OBJECT-TYPE
    SYNTAX DateAndTime
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Last Handoff Time"
    ::= { mwTopoStaEntry    7 }

  mwTopoStaLastActiveTime  OBJECT-TYPE
    SYNTAX DateAndTime
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Last Active Time"
    ::= { mwTopoStaEntry    8 }

  mwTopoStaAssignedApName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Assigned AP Name"
    ::= { mwTopoStaEntry    9 }

  mwTopoStaapTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwTopoStaapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Station/AP Edge Records "
    ::= { mwTopology 7 }

  mwTopoStaapEntry  OBJECT-TYPE
    SYNTAX MwTopoStaapEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes Station/AP Edge Records "
    INDEX {  mwTopoStaapTableIndex  }
    ::= { mwTopoStaapTable 1 }

  MwTopoStaapEntry  ::=  SEQUENCE { 
       mwTopoStaapTableIndex                                       Integer32, 
       mwTopoStaapRssi                                             Integer32,
       mwTopoStaapStaId                                            MacAddress,
       mwTopoStaapApId                                             Unsigned32,
       mwTopoStaapApName                                           DisplayString,
       mwTopoStaapAssigned                                         MwlOnOffSwitch 
  }
   
   
  mwTopoStaapTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwTopoStaapEntry 1 }

  mwTopoStaapRssi  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes RSSI"
    ::= { mwTopoStaapEntry    2 }

  mwTopoStaapStaId  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Station MAC Address"
    ::= { mwTopoStaapEntry    3 }

  mwTopoStaapApId  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP ID"
    ::= { mwTopoStaapEntry    4 }

  mwTopoStaapApName  OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP Name"
    ::= { mwTopoStaapEntry    5 }

  mwTopoStaapAssigned  OBJECT-TYPE
    SYNTAX MwlOnOffSwitch
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Assigned"
    ::= { mwTopoStaapEntry    6 }

  mwApNeighborTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApNeighborEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Neighbors List "
    ::= { mwTopology 8 }

  mwApNeighborEntry  OBJECT-TYPE
    SYNTAX MwApNeighborEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Neighbors List "
    INDEX {  mwApNeighborTableIndex  }
    ::= { mwApNeighborTable 1 }

  MwApNeighborEntry  ::=  SEQUENCE { 
       mwApNeighborTableIndex                                      Integer32, 
       mwApNeighborApMac                                           MacAddress,
       mwApNeighborChannel                                         Unsigned32,
       mwApNeighborNmsApNodeId                                     Integer32,
       mwApNeighborNeighborApId                                    Integer32,
       mwApNeighborNeighborApMac                                   MacAddress,
       mwApNeighborNmsApInterfaceId                                Integer32,
       mwApNeighborNeighborApCurrentRssi                           Integer32,
       mwApNeighborNeighborApControllerIndex                       Integer32 
  }
   
   
  mwApNeighborTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApNeighborEntry 1 }

  mwApNeighborNmsApNodeId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP-ID"
    ::= { mwApNeighborEntry    2 }

  mwApNeighborNmsApInterfaceId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Interface Id"
    ::= { mwApNeighborEntry    3 }

  mwApNeighborApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes MAC Address"
    ::= { mwApNeighborEntry    4 }

  mwApNeighborChannel  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Channel"
    ::= { mwApNeighborEntry    5 }

  mwApNeighborNeighborApId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Neighbor AP-ID"
    ::= { mwApNeighborEntry    6 }

  mwApNeighborNeighborApMac  OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes MAC Address"
    ::= { mwApNeighborEntry    7 }

  mwApNeighborNeighborApControllerIndex  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes ControllerIndex"
    ::= { mwApNeighborEntry    8 }

  mwApNeighborNeighborApCurrentRssi  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes RSSI"
    ::= { mwApNeighborEntry    9 }

  mwApNeighborDetailsTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwApNeighborDetailsEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Neighbors Consolidated List "
    ::= { mwTopology 9 }

  mwApNeighborDetailsEntry  OBJECT-TYPE
    SYNTAX MwApNeighborDetailsEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes AP Neighbors Consolidated List "
    INDEX {  mwApNeighborDetailsTableIndex  }
    ::= { mwApNeighborDetailsTable 1 }

  MwApNeighborDetailsEntry  ::=  SEQUENCE { 
       mwApNeighborDetailsTableIndex                               Integer32, 
       mwApNeighborDetailsChannel                                  Unsigned32,
       mwApNeighborDetailsLocalAp                                  Integer32,
       mwApNeighborDetailsRemoteAp                                 Integer32,
       mwApNeighborDetailsRssiLevel1                               Integer32,
       mwApNeighborDetailsRssiLevel2                               Integer32,
       mwApNeighborDetailsRssiLevel3                               Integer32,
       mwApNeighborDetailsRssiLevel4                               Integer32,
       mwApNeighborDetailsNmsApNodeId                              Integer32,
       mwApNeighborDetailsNmsApInterfaceId                         Integer32 
  }
   
   
  mwApNeighborDetailsTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwApNeighborDetailsEntry 1 }

  mwApNeighborDetailsNmsApNodeId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes AP-ID"
    ::= { mwApNeighborDetailsEntry    2 }

  mwApNeighborDetailsNmsApInterfaceId  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Interface Id"
    ::= { mwApNeighborDetailsEntry    3 }

  mwApNeighborDetailsChannel  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Channel"
    ::= { mwApNeighborDetailsEntry    4 }

  mwApNeighborDetailsLocalAp  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Number of Local APs"
    ::= { mwApNeighborDetailsEntry    5 }

  mwApNeighborDetailsRemoteAp  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Number of Remote APs"
    ::= { mwApNeighborDetailsEntry    6 }

  mwApNeighborDetailsRssiLevel1  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Number of APs with RSSI greater than -45"
    ::= { mwApNeighborDetailsEntry    7 }

  mwApNeighborDetailsRssiLevel2  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Number of APs with RSSI greater than -65"
    ::= { mwApNeighborDetailsEntry    8 }

  mwApNeighborDetailsRssiLevel3  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Number of APs with RSSI greater than -85"
    ::= { mwApNeighborDetailsEntry    9 }

  mwApNeighborDetailsRssiLevel4  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only 
    STATUS     current
    DESCRIPTION
         "This object describes Number of APs with RSSI less than -85"
    ::= { mwApNeighborDetailsEntry   10 }

  
END
   