OMNITRON-TC-MIB DEFINITIONS ::= BEGIN

-- *****************************************************************************
-- TEXTUAL-CONVENTIONs MIB for Omnitron Systems Technology Enterprise MIBs
-- *****************************************************************************

IMPORTS
    MODULE-IDENTITY, Integer32, Unsigned32, Counter64, enterprises
        FROM SNMPv2-SMI         -- RFC-2578
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC;         -- RFC 2579


ostOmnitronTcMib MODULE-IDENTITY
    LAST-UPDATED "201505131200Z"     -- May 13, 2015
    ORGANIZATION "Omnitron Systems Technology, Inc."
    CONTACT-INFO "Omnitron Systems Technology, Inc.
                  38 Tesla
                  Irvine, CA 92618-4670
                  USA

             Tel: (949) 250 6510
             Fax: (949) 250 6514
          E-mail: info@omnitron-systems.com
   International:  949 250 6510

                  Technical Support and Customer Service
             Tel: (800) 675 8410
          E-mail: support@omnitron-systems.com
   International:  949 250 6510"

    DESCRIPTION
            "Omnitron TC MIB for use with v5.2 iConverter Management Modules
             and NetOutlook

             Copyright 2015 Omnitron Systems Technology, Inc.
             All rights reserved
            "

    REVISION    "201505131200Z"     -- May 13, 2015
    DESCRIPTION "Added OstIpv6Addr, OstIpAddr
                "

    REVISION    "201501211200Z"     -- January 21, 2015
    DESCRIPTION "Initial version of v5.2 MIB.
                   Added OstAccessibiltyType from the OMNITRON-ACL-MIB
                "
    ::= { enterprises 7342 11 }

omnitron                OBJECT IDENTIFIER ::= { enterprises 7342 }
icAgent                 OBJECT IDENTIFIER ::= { omnitron 1 }


-- *****************************************************************************
-- Textual Conventions (TC)
-- *****************************************************************************
-- TC definitions are placed in alphabetical order

OstAccessibiltyType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Accessibilty type enumeration.

         deny(1)       Access to the module is not allowed
         permit(2)     Access to the module is allowed
        "
    SYNTAX      INTEGER {
                  deny        (1),
                  permit      (2)
                }


OstClassOfService ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "Class of service setting.  0=discard, 1=lowest class, 4=highest class"
    SYNTAX      Unsigned32 (0..4)


OstClockFreq ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-2"
    STATUS      current
    DESCRIPTION
        "Clock frequency in hundreths of MHz."
    SYNTAX      Unsigned32


OstCosL2cpDstAddr ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
        "L2CP destination address enumeration.

         Index | Destination Address | Name
         ------+--------------------+---------
             1 | 01-80-C2-00-00-00   | RSTP
             2 | 01-80-C2-00-00-01   | Pause
             3 | 01-80-C2-00-00-02   | LACP
             4 | 01-80-C2-00-00-02   | Marker
             5 | 01-80-C2-00-00-02   | Link OAM
             6 | 01-80-C2-00-00-02   |
             7 | 01-80-C2-00-00-03   | 802.1x
             8 | 01-80-C2-00-00-04   | IEEE MAC
             9 | 01-80-C2-00-00-05   |
            10 | 01-80-C2-00-00-06   |
            11 | 01-80-C2-00-00-07   | E-LMI
            12 | 01-80-C2-00-00-08   | Pr Bridge
            13 | 01-80-C2-00-00-09   |
            14 | 01-80-C2-00-00-0A   |
            15 | 01-80-C2-00-00-0B   |
            16 | 01-80-C2-00-00-0C   |
            17 | 01-80-C2-00-00-0D   | GVRP
            18 | 01-80-C2-00-00-0E   | LLDP
            19 | 01-80-C2-00-00-0F   |
            20 | 01-80-C2-00-00-20   | GARP
        "
    SYNTAX      Unsigned32 (1..20)


OstCosNameString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "A class of service name."
    SYNTAX      OCTET STRING (SIZE(1..45))


OstCosNameStringOrNone ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "A class of service name or an empty string."
    SYNTAX      OCTET STRING (SIZE(0..45))


OstCosTrustType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "CoS trust type enumeration.

         Green traffic is marked with low drop precedence and yellow
         traffic is marked with high drop precedence.

         cosTrust(1)        Trust frame. The frames priority
                            determines the egress class.

         cosUsePri(2)       Use the priority ostCosPriority for the
                            frame. The frame will egress with ostCosPriority
                            priority and ostCosPrirority determines the
                            egress class.

         cosUseClass(3)     Use the class ostCosClass for the frame.
                            The frame will egress with the frames
                            priority and the ostCosClass egress class.

         cosUsePriClass(4)  Use the priority ostCosPriority and class
                            ostCosClass for the frame. The frames will
                            egress with ostCosPri and ostCosClass egress
                            class.

         cosGreenYellow(5)  Use ostCosGreenPriority and ostCosGreenClass for
                            green traffic. Use ostCosYellowPriority and
                            ostCosYellowClass for yellow traffic.
        "
    SYNTAX      INTEGER {
                  cosTrust          (1),
                  cosUsePri         (2),
                  cosUseClass       (3),
                  cosUsePriClass    (4),
                  cosGreenYellow    (5)
                }


OstEgressSchedulingProfileIndexType ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "A value that uniquely identifies an Egress Scheduling Profile.

        The valid values are 1 to X, where X is the maximum supported profile.
        The maximum value for X for the GM4 is 4.
       "
    SYNTAX      Unsigned32 (1..8)


OstEgressQueueIndexType ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "A value that uniquely identifies an Egress Queue.

        The valid values are 1 to X, where X is the maximum supported profile.
        The maximum value for X for the GM4 is 4.
       "
    SYNTAX      Unsigned32 (1..8)


OstElpsProtectType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the ELPS protection type.  The value can be one
        of the following:

        e1plus1UniNoAps(1)   1 unidirectional without APS communication
        e1plus1UniAps(2)     1 unidirectional switching with APS communication
        e1plus1BiAps(3)      1 bidirectional w/APS communication
        e1to1(4)             1:1 bidirectional w/APS communication
        notAvailable(5)      Protect Type is unknown or not available, value returned
                                 for status read, not allowed to write
       "
    SYNTAX      INTEGER {
                  e1plus1UniNoAps (1),
                  e1plus1UniAps   (2),
                  e1plus1BiAps    (3),
                  e1to1           (4),
                  notAvailable    (5)
                }


OstElpsRequestStates ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the current request/state of either the local or
        remote (partner) ELPS instance.  The value can be one of the following:

        noRequest(0)             No Request (NR), lowest priority
        doNotRevert(1)           Do Not Revert (DNR)
        revertRequest(2)         Revert request (RR)
        exercise(4)              Exercise APS protocol (EXER)
        waitToRestore(5)         Wait to restore (WTR)
        manualSwitchWorking(6)   Manual swtich to working (MS-W)
        manualSwitch(7)          Manual switch (MS)
        signalDegrade(9)         Signal degrade (SD)
        signalFailWorking(11)    Signal fail for working (SF)
        forcedSwitch(13)         Forced switch (FS)
        signalFailProtection(14) Signal fail for protection (SF-P)
        lockoutProtection(15)    Lock of protection (LO), highest priority
        notAvailable(16)         Status is unknown or not available, value returned
                                 for status read, not allowed to write
       "
    SYNTAX      INTEGER {
                  noRequest            (0),
                  doNotRevert          (1),
                  revertRequest        (2),
                  exercise             (4),
                  waitToRestore        (5),
                  manualSwitchWorking  (6),
                  manualSwitch         (7),
                  signalDegrade        (9),
                  signalFailWorking    (11),
                  forcedSwitch         (13),
                  signalFailProtection (14),
                  lockoutProtection    (15),
                  notAvailable         (16)
                }


OstElpsSignalStates ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the requested or bridged signal for either
        the local or remote (partner) ELPS instance.  The value can be one of
        the following:

        nullSignal(0)            Null signal. This indicates the signal that
                                 the near-end requests be carried over the
                                 protection path
        normalSignal(1)          Normal traffic signal. This indicates the
                                 signal that is bridged onto the protection
                                 path.
        notAvailable(2)          Protect Type is unknown or not available, value
                                 returned for status read, not allowed to write
       "
    SYNTAX      INTEGER {
                  nullSignal           (0),
                  normalSignal         (1),
                  notAvailable         (2)
                }


OstErpsLinkState ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the current port link state. This is a
        function that indicates whether the current port is linked.
        The value can be one of the following:

        na(0)                    Not Applicable, port state is unknown
        up(1)                    Port is linked and capable of passing traffic
        down(2)                  Port is not linked and is not capable of
                                 passing traffic
       "
    SYNTAX      INTEGER {
                  na(0),
                  up(1),
                  down(2)
                }


OstErpsPortState ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the current forwarding state of the port.
        The value can be one of the following:

        na(0)                    Not Applicable, port state is unknown
        forward(1)               Port is in the forwarding state
        blocked(2)               Port is in the blocked state
       "
    SYNTAX      INTEGER {
                  na(0),
                  forward(1),
                  blocked(2)
                }


OstErpsPortType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the Ring Port type. The value can be one of the
        following:

        rp0(1)                   Ring Port 0
        rp1(2)                   Ring Port 1
       "
    SYNTAX      INTEGER {
                  rp0(1),
                  rp1(2)
                }


OstErpsRingStates ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the current request/state of either the local or
        remote (partner) ERPS instance.  The value can be one of the following:

        noRequest(0)             No Request (NR), local, lowest priority
        rapsNr(1)                Ring APS (R-APS) No Request (NR), remote
        rapsNrRb(2)              Ring APS (R-APS) No Request (NR), RPL Blocked (RB), remote
        wtbRunning(3)            Wait to Block (WTB) running, local
        wtbExpires(4)            Wait to Block (WTB) expires, local
        wtrRunning(5)            Wait to Restore (WTR) running, local
        wtrExpires(6)            Wait to Restore (WTR) expires, local
        manualSwitch(7)          Manual Switch (MS), local
        rapsManualSwitch(8)      Ring APS (R-APS) Manual Switch (MS), remote
        rapsSignalFail(9)        Ring APS (R-APS) Signal Fail (SF), remote
        localClearSignalFail(10) Local clear Signal Fail (SF), local
        localSignalFail(11)      Local Signal Fail (SF), local
        rapsForcedSwitch(12)     Ring APS (R-APS) Forced Switch (FS), remote
        forcedSwtich(13)         Forced Switch (FS), local
        clear(14)                Clear, local
       "
    REFERENCE
       "[ITU-T G.8032] Table 10-1"
    SYNTAX      INTEGER {
                  noRequest            (0),
                  rapsNr               (1),
                  rapsNrRb             (2),
                  wtbRunning           (3),
                  wtbExpires           (4),
                  wtrRunning           (5),
                  wtrExpires           (6),
                  manualSwitch         (7),
                  rapsManualSwitch     (8),
                  rapsSignalFail       (9),
                  localClearSignalFail (10),
                  localSignalFail      (11),
                  rapsForcedSwitch     (12),
                  forcedSwtich         (13),
                  clear                (14)
                }


OstErpsRingStatus ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that represents the current ring status. This is state machine node
        state value for the ERPS instance.  The value can be one of the
        following:

        initializing(1)          State machine initialization
        idle(2)                  Idle State (A)
        protection(3)            Protection (B)
        manualSwitch(4)          Manual Switch (C)
        forcedSwitch(5)          Forced Switch (D)
        pending(6)               Pending (E)
       "
    REFERENCE
       "[ITU-T G.8032] Table 10-2"
    SYNTAX      INTEGER {
                  initializing         (1),
                  idle                 (2),
                  protection           (3),
                  manualSwitch         (4),
                  forcedSwitch         (5),
                  pending              (6)
                }


OstErrorString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "The SNMP error string for further definition of a SNMP error."
    SYNTAX      OCTET STRING (SIZE(0..255))


OstEvcNameString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "An EVC name."
    SYNTAX      OCTET STRING (SIZE(1..45))


OstEvcNameStringOrNone ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "An EVC name or an empty string."
    SYNTAX      OCTET STRING (SIZE(0..45))


OstFileNameString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "A internal file name."
    SYNTAX      OCTET STRING (SIZE(1..45))


OstFingerprintString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "The fingerprint value for SSH protocol."
    SYNTAX      OCTET STRING (SIZE(1..64))


OstFloatValue ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "Floating point data type as represented in an octet string.
        Legal values and precision are indicated by the appropriate object.
        Only numbers and the decimal place are legal digit values.

        Example values:
           1000
           1500.05
           1545.25
       "
    SYNTAX      OCTET STRING (SIZE(0..20))


OstFrameCount64 ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
        "Frame counter value."
    SYNTAX      Counter64


OstFrameSizeList ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "
        Denotes a list of one or more frame sizes.

        1. Frame sizes have a value from 64 to 10240 bytes for the GM3, GM4,
           and GM4-PoE. Frame sizes have a value from 64 to 10240 bytes for
           the XM5.

        2. Individual frame sizes are included when separated by a comma ','.

        3. A range of frame sizes is included when separated by '..'.

        4. A range of sizes ending in a colon and a value, i.e. start..end:value,
           is the frame increment size for the next iteration (min value is 4)

        5. Ranges must be organized min size to max size, i.e. min..max

        6. Individual sizes can be mixed in any order

        Example values:
          64
          64..1024:64
          64,128,256,512,1024,1280,1518,10000
       "
    SYNTAX      OCTET STRING (SIZE(1..255))


OstIndexIntegerNextFree ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "An integer which may be used as a new index in a table.

        The special value of 0 indicates that no more new entries can
        be created in the relevant table.

        When a MIB is used for configuration, an object with this
        SYNTAX always contains a legal value (if non-zero) for an
        index that is not currently used in the relevant table. The
        Command Generator (Network Management Application) reads this
        variable and uses the (non-zero) value read when creating a
        new row with an SNMP SET.  When the SET is performed, the
        Command Responder (agent) MUST determine whether the value is
        indeed still unused; Two Network Management Applications may
        attempt to create a row (configuration entry) simultaneously
        and use the same value. If it is currently unused, the SET
        succeeds and the Command Responder (agent) changes the value
        of this object, according to an implementation-specific
        algorithm.  If the value is in use, however, the SET fails.
        The Network Management Application MUST then re-read this
        variable to obtain a new usable value.

        An OBJECT-TYPE definition using this SYNTAX MUST specify the
        relevant table for which the object is providing this
        functionality.
       "
    SYNTAX      Unsigned32 (0..16)


OstIpPriorityList ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "Selects IP priority values.  Valid values are from 0 to 63.
        Format:
            X       selects a single PCP priority value
            X..Y    selects a range of PCP priority values, X to Y
            X,Y     selects PCP priority values seperated by a comma
        Example values:
         0
         2..5
         0,2..5
       "
    SYNTAX      OCTET STRING (SIZE(0..14))


OstIpv6Addr ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "2x:2x:2x:2x:2x:2x:2x:2x"
    STATUS      current
    DESCRIPTION
       "This data type is used to model the IPv6 address. This is a
        binary string of up to 8 octets in network byte-order.
       "
    SYNTAX      OCTET STRING (SIZE(16..16))


OstIpAddr ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "This data type is used to model both IPv4 and IPv6 addresses. It
        is a hexadecimcal octet string with separators between number groups:
        either '.' for IPv4 or ':' for IPv6. The IP type is derived based upon
        the format of the string. Valid IP addreses:
            '192.168.1.220'
            'fe80:0000:0:0:1234:5678:abcd:efff'

       "
    SYNTAX      OCTET STRING (SIZE(0..39))


OstMhfCreation ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "Indicates if the Management Entity can create MHFs.

        The valid values are:
                ostMHFdefault(2) MHFs can be created on this VID on any
                        Bridge port through which this VID can pass.
                ostMHFexplicit(3) MHFs can be created for this VID only on
                        Bridge ports through which this VID can
                        pass, and only if a MEP is created at some
                        lower MD Level.
       "
    SYNTAX      INTEGER {
                  ostMHFdefault (1),
                  ostMHFexplicit (2)
                }


OstMipdMethodOfCreation ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Indicates the method of how this Mip table entry was created
        The valid values are:
                ostExplicit(1) indicates the Mip was created explicitly
                        through a command.
                ostImplicitMa(2) indicates the Mip was created implicitly
                        through the MA command.
                ostImplicitMde(3) indicates the Mip was created implicitly
                        through the CFM default Md table.
                ostExplicitImplicitMa(4) indicates the Mip was created both
                        implicitly and explicitly through the MA command.
        "
    SYNTAX      INTEGER {
                ostExplicit(1),
                ostImplicitMa(2),
                ostImplicitMde(3),
                ostExplicitImplicitMa(4)
                }


OstModeType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The module Mode Type as AP, SP or neither.

         normal(1)   Not specifically AP or SP
         ap(2)       Access Provider
         sp(3)       Service Provider
        "
    SYNTAX INTEGER {
        normal (1),
        ap    (2),
        sp     (3)
    }


OstModuleSingleIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "A value that uniquely identifies the chassis and slot in which the module is located.
       Base 10 Format: CCSS where
            CC is the chassis index, 1 to 99
            SS is the slot index, 1 to 99"
    SYNTAX      Unsigned32 (101..9999)


OstPcpPriorityList ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "Selects PCP priority values.  Valid values are from 0 to 7.
        Format:
            X       selects a single PCP priority value
            X..Y    selects a range of PCP priority values, X to Y
            X,Y     selects PCP priority values seperated by a comma
        Example values:
         0
         2..5
         0,2..5
       "
    SYNTAX      OCTET STRING (SIZE(0..14))


OstPortClockType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that indicates the TDM port recovery state/mode.
       "
    SYNTAX      INTEGER {
        adaptiveIdle(1),
        adaptiveAcqu(2),
        adaptiveTrk1(3),
        adaptiveTrk2(4),
        holdOver(5),
        coax(6),
        internal(7),
        line(8)
    }


OstPortList ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "Denotes a list of one or more ports, separated by comma characters, in the
        form of an ASCII string, which is case insensitive.

        Port  Description
        ----  ------------------
         1    Port 1
         2    Port 2
         3    Port 3
         4    Port 4
         5    Port 5
         6    Port 6
         7    Port 7
         8    Port 8
         9    Port 9
         10   Port 10
         11   Port 11
         12   Port 12
         13   Port 13
         14   Port 14
         15   Port 15
         16   Port 16
         17   Port 17
         a    backplane port A
         b    backplane port B
         mgt1 management port 1
         mgt2 management port 2
         all  includes all ports

        Example: '1,2,a,mgt1'
        "
    SYNTAX      OCTET STRING


OstPortNumber ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "This object selects the port number for the specific test
        instance that is configured.

        This value is dependent upon actual product accessed. The port number
        for a specific port can be determined by selecting the module type
        and then the port that is accessed. A value of '0' indicates that
        no port is defined.

        Module Type        P1   P2   P3   P4   P5   BP A  BP B  Mgt1  Mgt2
        -----------------  ---  ---  ---  ---  ---  ----  ----  ----  ----
        3-port plug-in     1    2    3    n/a  n/a  4     5     6     7
        3-port standalone  1    2    3    n/a  n/a  n/a   n/a   6     7
        2-port plug-in     1    2    n/a  n/a  n/a  3     4     5     6
        2-port standalone  1    2    n/a  n/a  n/a  n/a   n/a   5     6
        4-port             1    2    3    4    n/a  5     6     n/a   n/a
        5-port             1    2    3    4    5    n/a   n/a   6     7

        For the 7 port module: Port 1 - Port 7 are ports 1 - 7 are the front
        facing ports, port 8 is the dedicated management port, port 9 is Mgt1
        and port 10 is Mgt2.

        For the 16 port module: Port 1 - Port 16 are the customer facing
        ports, port 17 is the dedicated management port, port 18 is Mgt1 and
        port 19 is Mgt2.

        Other values are undefined.
      "
    SYNTAX      Unsigned32 (0..99)


OstPortSingleIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "A value that uniquely identifies a module port, and the chassis and slot in
       which the module is located.
       Base 10 Format: CCSSPP where
            CC is the chassis index, 1 to 99
            SS is the slot index, 1 to 99
            PP is the port index, 1 to 99"
    SYNTAX      Unsigned32 (10101..999999)


OstPriority ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "Priority setting."
    SYNTAX      Unsigned32 (0..7)


OstProbeNameString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "An EVC name."
    SYNTAX      OCTET STRING (SIZE(1..45))


OstProfileNameString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "A test profile name."
    SYNTAX      OCTET STRING (SIZE(1..45))


OstTestResultType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that indicates the result of a test.  The value can be one of
        the following:

        pass(1)              Indicates the test has passed successfully
        fail(2)              Indicates the test has failed
        oversubscribe(3)     Indicates the test failed due to oversubscription
                             of a resource
       "
    SYNTAX      INTEGER {
                  pass            (1),
                  fail            (2),
                  oversubscribe   (3)
                }


OstTestStatusType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "A value that indicates the status of the current test instance.  The
        value can be one of the following:

        testNotStarted(1)    Current test instance has not started yet,
                             not fully configured, or waiting for loop-up
        testInProcess(2)     Current test instance is currently running
        testStopped(3)       Current test instance has been stopped after running
                             for a period of time
        testCompleted(4)     Current test instance has completed
        testInitializing(5)  Current test is the process of starting, used to
                             restart a test in process, completed, or stopped
       "
    SYNTAX      INTEGER {
                  testNotStarted  (1),
                  testInProcess   (2),
                  testStopped     (3),
                  testCompleted   (4),
                  testInitializing(5)
                }


OstUnsigned64 ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
       "A non-negative 64-bit bit integer, without counter semantics, between 0
        and 2^64-1 inclusive (0 to 18446744073709551615 decimal).

        It can have a MAX-ACCESS of read-only or read-write.

        SYNTAX is Counter64 for the encoding rules only.
       "
    SYNTAX      Counter64


OstUserNameString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "A string that is used to identify a specific user."
    SYNTAX      OCTET STRING (SIZE(1..32))


OstVlanId ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
        "The VLAN-ID that uniquely identifies a VLAN.  This
        is the 12-bit VLAN-ID used in the VLAN Tag header."
    SYNTAX      Integer32 (0..4095)


OstVlanIdList ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS      current
    DESCRIPTION
       "Denotes a list of one or more VLAN IDs.
       VLAN IDs have a value of 0 to 4095.
       Individual VLAN IDs are included when separated by a comma ','.
       A range of VLAN IDs is included when separated by '..'.
       An asterisk indicates untagged data.
       'rest' selects remaining VLAN IDs.
       'all' selects all VLAN IDs.
       Example values:
         100,110
         100..110
         100,110,200..210
         100,110,200..210,500..510
       "
    SYNTAX      OCTET STRING (SIZE(0..110))


END