ExaltComProducts DEFINITIONS ::= BEGIN
    IMPORTS
    MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE,
    IpAddress, Integer32, Gauge32
        FROM SNMPv2-SMI
    exaltcommunications, EthMainStatusT, EthAuxStatusT, AuxNmsMode,
    EthPortMode, Te1StatusT, Te1LboT, EnableStatusT,
    Te1LineCodeT, Te1LoopBackModeT, AlarmLevelT,
    Led4ColorT, VlanStatusT, VlanGroupT, ExaltEnableT, AcmModulationT,
    FileTransferTypeT, FileTransferStartT, NtpClientEnableT, TimeZoneT
        FROM ExaltComm
    OBJECT-GROUP
        FROM SNMPv2-CONF
    DisplayString, TEXTUAL-CONVENTION
        FROM SNMPv2-TC;

    productsMIB MODULE-IDENTITY
        LAST-UPDATED        "201304291021Z"
        ORGANIZATION        "Exalt"
        CONTACT-INFO        "Exalt Wireless Inc.
                            250 E Hacienda Ave.,
                            Campbell, CA, 95008
                            USA"

        DESCRIPTION         "Exalt devices"

        REVISION            "201304291021Z"
        DESCRIPTION         "This is the Exalt Products mib. rev:1.01"
        ::= { exaltcommunications 1 }

    PwType ::= TEXTUAL-CONVENTION
        DISPLAY-HINT	    "255a"
        STATUS		    current
        DESCRIPTION         "This is a PW field."
        SYNTAX		    OCTET STRING (SIZE(8..16))



    productsMIBNotifications OBJECT IDENTIFIER ::= { productsMIB 1 }

    productsMIBObjects OBJECT IDENTIFIER ::= { productsMIB 2 }

    radioInfo OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "Common Radio Information to all Exalt devices."
        ::= { productsMIBObjects 1 }

    modelName OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..20))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "A descriptive name for the Radio.  See Web, Radio Information, Model Name."
        ::= { radioInfo 1 }

    partNumber OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..20))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Part Number of the Radio.  See Web, Radio Information, Part Number."
        ::= { radioInfo 2 }

    serialNumber OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..20))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Radio Serial Number.  See Web, Radio Inforamtion, Serial Number."
        ::= { radioInfo 3 }

    interfaceType OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..30))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Interfaces available on this radio.  Ethernet, T1/E1, etc.
                            See Web, Radio Information, Interface Type."
        ::= { radioInfo 4 }

    firmwareVersion OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Radio Firmware Version.  See Web, Radio Information, Firmware Version."
        ::= { radioInfo 5 }

    bootVersion OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Radio Boot Code Version.  See Web, Radio Information, Boot Version."
        ::= { radioInfo 6 }

    rdkDbVer OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Device RDK Database Version. See Web, Radio Information, RDK Database Version."
        ::= { radioInfo 11 }

    txFreqRange OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Radio Tx Frequency Range.
                            FDD radios have a Tx and Rx frequency range.
                            See Web, Radio Information, RF Transmit range.
                            TDD radios have one frequency range.
                            See Web, Radio Information, RF Frequency Band."
        ::= { radioInfo 12 }

    rxFreqRange OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Radio Rx Frequency Range.
                            FDD radios have a Tx and Rx frequency range.
                            See Web, Radio Information, RF Receive range.
                            TDD radios have one frequency range.
                            See Web, Radio Information, RF Frequency Band."
        ::= { radioInfo 13 }

    rfFreqBand OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Device Frequency Band (Range).
                            TDD radios have N/A value in this field.
                            FDD radios have TX High or TX Low depending on used diplexer and Transmit frequency.
                            See Web, Radio Information, Tx Band."
        ::= { radioInfo 14 }

    hwId OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Device Hardware ID number. See Web, Radio Information, Hardware ID number"
        ::= { radioInfo 15 }

    modelNumber OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Model Number of the Radio. See Web, Radio Information, Model Number"
        ::= { radioInfo 16 }

    licenseFeatures OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..128))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The list of the features enabled by License Key"
        ::= { radioInfo 17 }

    radioAdmin OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "Radio Administration parameters."
        ::= { productsMIBObjects 2 }

    sysDate OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(10))
        UNITS               "MM/DD/YYYY"
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Radio System Date, MM/DD/YYYY.  See Web, Administration, Settings, Date.
                            To make permanent, write save to commitAdminSettings after change.
                            After commit, SNMP restarts and will be down for 30 seconds."
        ::= { radioAdmin 1 }

    sysTime OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(8))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Radio System Time, HH:MM:SS, as 24 hours.  See Web, Administration, Settings, Time.
                            To make permanent, write save to commitAdminSettings after change.
                            After commit, SNMP restarts and will be down for 30 seconds."
        ::= { radioAdmin 2 }

    radioName OBJECT IDENTIFIER ::= { radioAdmin 3 }

    rnLocal OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(1..32))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The user specifiable Radio Name for this radio.
                            See Web, Administration, Settings, Radio Name.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioName 1 }

    rnRemote OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Radio Name of the Radio at the far end of this RF Link.
                            Can only be set at that radio.  See Web, Administration, Settings, Radio Name."
        ::= { radioName 2 }

    linkName OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..32))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The user specifiable Link Name for this radio.
                            See Web, Administration, Settings, Link Name.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 4 }

    linkSecKey OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(12))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Link Security Key must match on both ends of an RF Link for traffic to pass.
                            See Web, Administration, Settings, Link Security Key.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 5 }

    adminPassword OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(1..16))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The password for admin login to Web/CLI.
                            See Web, Administration, Settings, Admin Password.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 6 }

    userPassword OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(1..16))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The password for user login to Web/CLI.
                            See Web, Administration, Settings, User Password.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 7 }

    ipAddress OBJECT IDENTIFIER ::= { radioAdmin 8 }

    ipLocal OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The IP address of local radio.
                            This IP address is used to manage radio.
                            See Web, Administration, Settings, IP Address.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { ipAddress 1 }

    ipRemote OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The IP address of the remote Radio.
                            This IP address is used to manage Remote radio.
                            Can only be set at that radio. See Web, Administration, Settings, IP Address."
        ::= { ipAddress 2 }

    subnetMask OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Subnet Mask for IP address of local radio.
                            See Web, Administration, Settings, IP Mask.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 9 }

    ipAddressNetmask OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(9..18))
        UNITS               "IP/NN Where NN=00 To 32"
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The IP address and Subnet Mask of local radio. ie 10.0.0.1/24.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 10 }

    defaultGateway OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Default Gateway for local radio port.
                            See Web, Administration, Settings, Default Gateway.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 11 }

    aesEnable OBJECT-TYPE
        SYNTAX		    INTEGER {
                                aesDisable( 0 ),
                                aesEnable( 1 )
                            }
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The AES enable(0)/disable(1).
                            AES (Advance Encryption Standard) can be implemented to provide additional 
                            data security for the wireless link. 
                            This function requires an upgrade license key (purchased separately).
                            See Web, Administration, Settings, AES Settings, Enable AES.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 12 }

    aesKey OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(1..64))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The symmetric AES key for encrypt/decrypt payload data.
                            Different bitlength encryption license keys (for example, 128-bit and 256-bit)
                            are available, depending on model type and license type.
                            AES Key should match both on local radio and far end radio.
                            See Web, Administration, Settings, AES Settings, AES Key.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 13 }


    licKey OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(1..32))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The license key which defines radio features and capabilities.
                            See Web, Administration, Settings, License Key.
                            To make permanent, write save to commitAdminSettings after change."
        ::= { radioAdmin 14 }

    -- rdkKey OBJECT-TYPE ::= { radioAdmin 15 }
    -- domainName OBJECT-TYPE ::= { radioAdmin 16 }

    snmpConfig OBJECT IDENTIFIER ::= { radioAdmin 17 }

    trapIpaddr1 OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The IP address to which the SNMP traps are directed.
                            See Web, Administration, SNMP, Traps, Trap Destination IP Address."
        ::= { snmpConfig 1 }

    trapIpaddrEnable1 OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Enable/Disable trap ip address."
        ::= { snmpConfig 2 }

    trapIpaddr2 OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The IP address to which the SNMP traps are directed.
                            See Web, Administration, SNMP, Traps, Trap Destination IP Address."
        ::= { snmpConfig 3 }

    trapIpaddrEnable2 OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Enable/Disable trap ip address."
        ::= { snmpConfig 4 }

    trapIpaddr3 OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The IP address to which the SNMP traps are directed.
                            See Web, Administration, SNMP, Traps, Trap Destination IP Address."
        ::= { snmpConfig 5 }

    trapIpaddrEnable3 OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Enable/Disable trap ip address."
        ::= { snmpConfig 6 }

    trapIpaddr4 OBJECT-TYPE
        SYNTAX              IpAddress
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The IP address to which the SNMP traps are directed.
                            See Web, Administration, SNMP, Traps, Trap Destination IP Address."
        ::= { snmpConfig 7 }

    trapIpaddrEnable4 OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Enable/Disable trap ip address."
        ::= { snmpConfig 8 }

    trapAuth OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Authentication trap enable(1)/disable(0).
                            This is an SNMP standard trap when password information for SNMP is incorrect.
                            See Web, Administration, SNMP, Traps, Authentication Trap."
        ::= { snmpConfig 9 }

    trapReboot OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Reboot trap enable(0)/disable(1).
                            This trap is sent after any radio reboot to inform the manager of the reboot status.
                            See Web, Administration, SNMP, Traps, Radio Reboot Trap."
        ::= { snmpConfig 10 }

    trapLocLinkStat OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Local Link Status trap enable(0)/disable(1).
                            This trap is sent when Link is in errored state (equivalent to the Link LED).
                            See Web, Administration, SNMP, Traps, Local Link Status Trap."
        ::= { snmpConfig 11 }

    trapLocAlarmStat OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Local Alarm Status trap enable(0)/disable(1).
                            This trap is sent when local radio Status is in errored state 
                            (equivalent to the Status LED).
                            See Web, Administration, SNMP, Traps, Local Radio Status Trap."
        ::= { snmpConfig 12 }

    trapRemAlarmStat OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Remote Alarm Status trap enable(0)/disable(1).
                            This trap is sent when remote radio Status is in errored state 
                            (equivalent to the Status LED).
                            See Web, Administration, SNMP, Traps, Remote Radio Status Trap."
        ::= { snmpConfig 13 }

    trapLocTempStat OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Local Temperature Status trap enable(0)/disable(1).
                            This trap is sent when the internal temperature reaches the warning point.
                            See Web, Administration, SNMP, Traps, Temperature Status Trap."
        ::= { snmpConfig 14 }

    trapv1Enable OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "SNMPv1 Traps enable(0)/disable(1).
                            Enables traps for SNMP protocol version 1.
                            See Web, Administration, SNMP, Traps, Enable SNMPv1 Traps."
        ::= { snmpConfig 15 }

    trapv2cEnable OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "SNMPv2c Traps enable(0)/disable(1).
                            Enables traps for SNMP protocol version 2c.
                            See Web, Administration, SNMP, Traps, Enable SNMPv2c Traps."
        ::= { snmpConfig 16 }

    trapv3Enable OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "SNMPv3 Traps enable(0)/disable(1).
                            Enables traps for SNMP protocol version 3.
                            See Web, Administration, SNMP, Traps, Enable SNMPv3 Traps."
        ::= { snmpConfig 17 }

    trapLocRslStat OBJECT-TYPE
        SYNTAX              EnableStatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Local RSL Status trap enable(0)/disable(1).
                            This trap is sent when the local RSL drops below the value set in the
                            RSL Threshold Value (dBm) field.
                            See Web, Administration, SNMP, Traps, Local RSL Status Trap."
        ::= { snmpConfig 18 }

    trapLocRslThreshold OBJECT-TYPE
        SYNTAX              INTEGER
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Local RSL Threshold.
                            Exalt recommends that this trap be set to a value 5dBm or 10dBm above 
                            the threshold as a warning that the system has faded and may be approaching an outage.
                            See Web, Administration, SNMP, Traps, Threshold Value."
        ::= { snmpConfig 19 }

    commitSnmpSettings OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(4..200))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Option strings to be written are: save, clear, correspondingly saving changes to
                            configuration to the persistent storage or clearing unsaved changes."
        ::= { snmpConfig 1000 }


    ntp OBJECT-IDENTITY
        STATUS              current
        DESCRIPTION         "NTP and Time zone configuration."
        ::= { radioAdmin 18 }

    ntpClientEnable OBJECT-TYPE
        SYNTAX              NtpClientEnableT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "this mib to enable/disable the NTP client in the radio.
                             0 - disable NTP client. 
                             1 - enable with 1 NTP server. 
                             2 - enable with 2 NTP servers.
                             3 - enable with 3 NTP servers.
                             4 - enable with 4 NTP servers."

        ::= { ntp 1 }

    ntpServer1IpAddr OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(7..15))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "IP address for the first NTP server in xxx.xxx.xxx.xxx format"

        ::= { ntp 2 }

    ntpServer2IpAddr OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(7..15))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "IP address for the second NTP server in xxx.xxx.xxx.xxx format"
        ::= { ntp 3 }

    ntpServer3IpAddr OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(7..15))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "IP address for the third NTP server in xxx.xxx.xxx.xxx format"
        ::= { ntp 4 }

    ntpServer4IpAddr OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(7..15))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "IP address for the forth NTP server in xxx.xxx.xxx.xxx format"
        ::= { ntp 5 }

    ntpTimeZoneSelect OBJECT-TYPE
        SYNTAX              TimeZoneT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION        "Time Zone selection.

                            0 - (GMT-11:00) Samoa
                            1 - (GMT-10.00) Hawaii
                            2 - (GMT-09:00) Alaska
                            3 - (GMT-08:00) Pacific Time
                            4 - (GMT-07:00) Arizona
                            5 - (GMT-07:00) Montain Time
                            6 - (GMT-06:00) Central Time
                            7 - (GMT-05:00) Eastern Time
                            8 - (GMT-05:00) Indiana (East)
                            9 - (GMT-04:00) Atlantic Time (Canada)
                            10- (GMT) Coordinated Universal Time
                            11- (GMT) London
                            12- (GMT+01:00) Berlin
                            13- (GMT+01:00) Belgrade
                            14- (GMT+01:00) Paris
                            15- (GMT+02:00) Cairo
                            16- (GMT+02:00) Helsinki
                            17- (GMT+03:00) Baghdad
                            18- (GMT+03:00) Moscow
                            19- (GMT+03:30) Tehran
                            20- (GMT+04:30) Kabul
                            21- (GMT+05:00) Karachi
                            22- (GMT+07:00) Bangkok
                            23- (GMT+08:00) Shanghai
                            24- (GMT+08:00) Taipei
                            25- (GMT+09:00) Tokyo
                            26- (GMT+09:00) Seoul
                            27- (GMT+10:00) Sydney
                            28- (GMT+10:00) Vladivostok"

        ::= { ntp 6 }

    commitNtpSettings OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(4..200))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "This command allows saving or clear the NTP and Tome Zone configuration.
                            If the save includes the change of time zone, the radio will automatically reboot
                            to take effect the newly selected time zone. 
                            Option strings to be written are: save, clear, correspondingly saving changes to
                            configuration to the persistent storage or clearing unsaved changes."
        ::= { ntp 1000 }

    commitAdminSettings OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(4..200))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Commit Administration settings command. Valid values: 'save', 'clear'.
                            Configuration changes via SNMP do not take effect until 
                            'save' (Commit) command is sent to this parameter.
                            'clear' (Cancel) command is used to cancel configuration changes before commit operation.
                            In case of invalid configuration this parameter contains text description of the problem."
        ::= { radioAdmin 1000 }

    radioConfig OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "The Radio Configuration Section."
        ::= { productsMIBObjects 3 }

    systemConfig OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "This is the device specific configuration section."
        ::= { radioConfig 1 }

    commitSystemSettings OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Commit System Configuration settings command. Valid values: 'save', 'clear'.
                            Configuration changes via SNMP do not take effect until 
                            'save' (Commit) command is sent to this parameter.
                            'clear' (Cancel) command is used to cancel configuration changes before commit operation.
                            In case of invalid configuration this parameter contains text description of the problem."
        ::= { systemConfig 1000 }

    interface OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "Radio Interfaces Configuration section."
        ::= { radioConfig 2 }

    te1 OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "T1,E1 interfaces Configuration section.
                            Section allows to configure T1/E1 ports on the radio if any."
        ::= { interface 2 }

    te1NumChannels OBJECT-TYPE
        SYNTAX              Gauge32
        UNITS               "channels"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Number of T1 or E1 channels supported by the Radio."
        ::= { te1 1 }

    te1NumActiveChannels OBJECT-TYPE
        SYNTAX              Gauge32
        UNITS               "channels"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Current number of channels available, based
                             on bandwitdh of the RF link and the license key."
        ::= { te1 2 }

    selectT1orE1 OBJECT-TYPE
        SYNTAX              INTEGER {
                                t1( 0 ),
                                e1( 1 )
                            }
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Select operation mode of T1/E1 interfaces. Either T1(0) or E1(1).
                            See Web, Configuration, Interface, T1/E1, Set To E1/T1 Mode button."
        ::= { te1 3 }

    te1Interfaces OBJECT-TYPE
        SYNTAX              SEQUENCE OF Te1InterfacesEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "Attributes for T1 or E1 ports."
        ::= { te1 4 }

    te1Interface OBJECT-TYPE
        SYNTAX              Te1InterfacesEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "An entry in the T1/E1 Attribute table."
        INDEX               {
                                te1Status, t1LBO, te1AIS, t1LineCode, te1LoopBackMode
                            }
        ::= { te1Interfaces 1 }

    Te1InterfacesEntry ::= SEQUENCE {
        te1Status
            Te1StatusT,
        t1LBO
            Te1LboT,
        te1AIS
            Te1StatusT,
        t1LineCode
            Te1LineCodeT,
        te1LoopBackMode
            Te1LoopBackModeT
    }

    te1Status OBJECT-TYPE
        SYNTAX              Te1StatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The T1/E1 status: enable(1)/disable(0).
                            Parameter allows to enable/disable each individual T1 channel.
                            See Web, Configuration, Interface, T1/E1, Status.
                            To make permanent, write save to commitTe1Settings after change."
        ::= { te1Interface 1 }

    t1LBO OBJECT-TYPE
        SYNTAX              Te1LboT
        UNITS               "feet"
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Line Build Out length range.
                            Valid values (ft): lbo0to133(0), lbo133to266(1), lbo266to399(2), lbo399to533(3), lbo533to655(4).
                            See Web, Configuration, Interface, T1/E1, LBO.
                            To make permanent, write save to commitTe1Settings after change."
        ::= { te1Interface 2 }

    te1AIS OBJECT-TYPE
        SYNTAX              Te1StatusT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The T1/E1 AIS enabled flag: enable(1)/disable(0).
                            If enabled, the radio places an AIS code on the output of the associated interface 
                            if and when the link fails or when there is no E1 signal available from the far
                            end to provide the user at the local end.
                            See Web, Configuration, Interface, T1/E1, AIS.
                            To make permanent, write save to commitTe1Settings after change."
        ::= { te1Interface 3 }

    t1LineCode OBJECT-TYPE
        SYNTAX              Te1LineCodeT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The T1/E1 Line Code type: b8zs(0), ami(1). 
                            See Web, Configuration, Interface, T1/E1, AIS, Line Code.
                            To make permanent, write save to commitTe1Settings after change."
        ::= { te1Interface 4 }

    te1LoopBackMode OBJECT-TYPE
        SYNTAX              Te1LoopBackModeT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Loop Back Mode for a T1/E1 interface.
                            Valid values: disabled(0), ExternalLocal(1), ExternalRemote(2), Internal(3).
                            All loopback configurations control the loop at the Line Interface integrated circuit,
                            which is the device wired directly to the front panel ports.
                            See Web, Configuration, Interface, T1/E1, AIS, Loopback.
                            To make permanent, write save to commitTe1Settings after change."
        ::= { te1Interface 5 }

    commitTe1Settings OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(4..200))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The Commit TE1 Configuration settings command. Valid values: 'save', 'clear'.
                            Configuration changes to TE1 ports via SNMP do not take effect until 
                            'save' (Commit) command is sent to this parameter.
                            'clear' (Cancel) command is used to cancel configuration changes before commit operation.
                            In case of invalid configuration this parameter contains text description of the problem."
        ::= { te1 1000 }

    fileManagement OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "The File Management Section. 
                            This section allows to initiate Upload/Download firmware/configuration/logs, 
                            perform Firmware activation procedure."
        ::= { radioConfig 3 }

    currentFwFilename OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..100))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The file name of the currently running firmware.
                            See Web, Administration, File Management, File Activation, Current File."
        ::= { fileManagement 1 }

    alternateFwFilename OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..100))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The file name of the alternate firmware image.
                            See Web, Administration, File Management, File Activation, Alternative File."
        ::= { fileManagement 2 }

    swapFWimage OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..200))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Swap the firmware images and restart radio.
                            To perform swap operation 'swap' command needs to be sent to this parameter.
                            For ExtendAirG2 to perform revert to factory operation 'factory' command needs to be sent.
                            Radio will become unavailable for several minutes."
        ::= { fileManagement 3 }

    fileTransfer OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "The File Transfer Section.
                            This section allows to initiate Upload/Download firmware/configuration/logs 
                            over TFTP protocol."
        ::= { fileManagement 4 }

    factoryFwFilename OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..100))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The file name of the factory firmware image.
                            See Web, Administration, File Management, File Activation, Factory File."
        ::= { fileManagement 5 }

    tftpServerIp            OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(7..15))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The TFTP Server IP address.
                            "
        ::= { fileTransfer 1 }

    uploadFilename          OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..127))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The name of the file for upload operation.
                            For configuration file uploadFilename should be always 'config.xml'.
                            uploadFilename value should match the file name in TFTP server folder."
        ::= { fileTransfer 2 }

    transferType            OBJECT-TYPE
        SYNTAX              FileTransferTypeT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "The file transfer type.
                            Valid values:
                              - uploadFirmware(0)
                              - uploadConfig(1)
                              - uploadRDD(2) (Valid only for TDD radios)
                              - downloadFirmware(3)
                              - downloadConfig(4)
                              - downloadMIBs(5)
                              - downloadEventLogs(6).
                            The actual operation starts via updating transferStart parameter value."
        ::= { fileTransfer 3 }

    transferStart           OBJECT-TYPE
        SYNTAX              FileTransferStartT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "TransferStart parameter is used to initiate file transfer operation.
                            Send startTransfer(1) to this parameter."
        ::= { fileTransfer 4 }

    transferStatus          OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..127))
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The current file transfer status."
        ::= { fileTransfer 5 }

    radioMonitor OBJECT-IDENTITY
        STATUS		current
        DESCRIPTION         "Monitor Various components."
        ::= { productsMIBObjects 4 }

    -- gps OBJECT IDENTIFIER ::= { radioMonitor 1 }
    -- satelliteInView OBJECT-TYPE ::= { gps 1 }
    alarms OBJECT IDENTIFIER ::= { radioMonitor 2 }


    almLocal OBJECT IDENTIFIER     ::=  { alarms 3 }
    locSysAlarms OBJECT IDENTIFIER  ::= { almLocal 1 }
    locEthAlarms OBJECT IDENTIFIER  ::= { almLocal 2 }
    locTe1Alarms OBJECT IDENTIFIER  ::= { almLocal 3 }
 --   gigEAlarms OBJECT IDENTIFIER ::= { locAlarms 4 }
 --   locDS3Alarms OBJECT IDENTIFIER  ::= { locAlarms 5 }
 --   locV35Alarms OBJECT IDENTIFIER  ::= { locAlarms 6 }
 --   locOduAlarms OBJECT IDENTIFIER  ::= { locAlarms 7 }

    locLinkState OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Link Status Alarm.
                            Possible values:
                             - almNORMAL(0) - Error-free connection (BER<10e-6)
                             - almMINOR(1)  - Errorred connection (BER<10e-3)
                             - almMAJOR(2) - No link (BER>10e-3)
                            See Web, Monitor, Alarms, Link"
        ::= { locSysAlarms 1 }

    locTempAlarm OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Temperature Alarm state.
                            Possible values:
                             - almNORMAL(0) - Normal temprature range
                             - almMINOR(1)  - Exceeding normal temprature range
                            See Web, Monitor, Alarms, Temperature"
        ::= { locSysAlarms 2 }

    locCurrentTemp OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "C"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Internal Temperature in Celsius."
        ::= { locSysAlarms 3 }

    locCurrentTempS OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Internal Temperature as a string. "
        ::= { locSysAlarms 4 }

    -- locCollocAlarm OBJECT-TYPE ::= { locSysAlarms 8 }
    -- remCollocAlarm OBJECT-TYPE ::= { remSysAlarms 8 }

    locLinkSecMismatch OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "This is link security mismatch alarm.
                            This alarm tells if the Link Security Key is matching or not.
                            Possible values:
                             - almNORMAL(0) - Link Secutiry keys match
                             - almMAJOR(2) - Link Secutiry keys do not match
                            "
        ::= { locSysAlarms 9 }

    locLinkStateV OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Vertical Link Status Alarm. -<g89><>"
        ::= { locSysAlarms 15 }

    locLinkStateH OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Horizontal Link Status Alarm. -<g89><>"
        ::= { locSysAlarms 16 }

-- T1/E1
     locTe1LinkSummary   OBJECT-TYPE
        SYNTAX              Led4ColorT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The T1/E1 Link Summary LED color. "
        ::= { locTe1Alarms 1 }

    locTE1Alarms OBJECT-TYPE
        SYNTAX              SEQUENCE OF Te1Alarms1Entry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "The Local T1/E1 Interface Alarms."
        ::= { locTe1Alarms 2 }

    locTe1AlarmsEntry OBJECT-TYPE
        SYNTAX              Te1Alarms1Entry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "T1/E1 Alarms table Entry."
        INDEX               {
                                locTe1Alarm
                            }
        ::= { locTE1Alarms 1 }

    Te1Alarms1Entry ::= SEQUENCE {
        locTe1Alarm
            AlarmLevelT
    }

    locTe1Alarm OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Alarms state for the Local T1/E1 Channel.
                            Possible values:
                             - almNORMAL(0) - Enabled and connection present
                             - almMAJOR(2) - Enabled and no connection present
                             - almDisable(3) - Disabled and no connection present
                             - almNotAvailable(4) - T1/E1 channel is not available
                            See Web, Monitor, Alarms, T1/E1 Input"
        ::= { locTe1AlarmsEntry 1 }

-- end of te1 local alarms

    almRemote OBJECT IDENTIFIER     ::= { alarms 4 }
    remSysAlarms OBJECT IDENTIFIER  ::= { almRemote 1 }
    remEthAlarms OBJECT IDENTIFIER  ::= { almRemote 2 }
    remTe1Alarms OBJECT IDENTIFIER  ::= { almRemote 3 }

    remLinkState OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Link Status Alarm for far end radio.
                            Possible values:
                             - almNORMAL(0) - Error-free connection (BER<10e-6)
                             - almMINOR(1)  - Errorred connection (BER<10e-3)
                             - almMAJOR(2) - No link (BER>10e-3)
                             - almNotAvailable(4) - Telemetry is down
                            See Web, Monitor, Alarms, Link"
        ::= { remSysAlarms 1 }

    remTempAlarm OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Temperature Alarm state for far end radio.
                            Possible values:
                             - almNORMAL(0) - Normal temprature range
                             - almMINOR(1)  - Exceeding normal temprature range
                             - almNotAvailable(4) - Telemetry is down
                            See Web, Monitor, Alarms, Temperature"
        ::= { remSysAlarms 2 }

    remCurrentTemp OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "C"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Internal Temperature in Celsius for far end radio. "
        ::= { remSysAlarms 3 }

    remCurrentTempS OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The internal Temperature as a string for far end radio. "
        ::= { remSysAlarms 4 }

--    remCollocAlarm OBJECT-TYPE         ::= { remSysAlarms 8 }

    remLinkSecMismatch OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "This is link security mismatch alarm.
                            This alarm tells if the Link Security Key is matching or not.
                            Possible values:
                             - almNORMAL(0) - Link Secutiry keys match
                             - almMAJOR(2) - Link Secutiry keys do not match
                             - almNotAvailable(4) - Telemetry is down
                            "
        ::= { remSysAlarms 9 }

    remLinkStateV OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Vertical Link Status Alarm. -<g89><>"
        ::= { remSysAlarms 15 }

    remLinkStateH OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Horizontal Link Status Alarm. -<g89><>"
        ::= { remSysAlarms 16 }

-- remote Te1 alarms
    remTe1LinkSummary OBJECT-TYPE
        SYNTAX              Led4ColorT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The T1/E1 Link Summary LED color. "
        ::= { remTe1Alarms 1 }

    remTE1Alarms OBJECT-TYPE
        SYNTAX              SEQUENCE OF Te1AlarmsEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "The Remotel T1/E1 Interface Alarms."
        ::= { remTe1Alarms  2 }

    remTe1AlarmsEntry OBJECT-TYPE
        SYNTAX              Te1AlarmsEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "T1/E1 Alarms table Entry."
        INDEX               {
                                remTe1Alarm
                            }
        ::= { remTE1Alarms 1 }

    Te1AlarmsEntry ::= SEQUENCE {
        remTe1Alarm
            AlarmLevelT
    }

    remTe1Alarm OBJECT-TYPE
        SYNTAX              AlarmLevelT
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Alarms state for the Local T1/E1 Channel of far end radio.
                            Possible values:
                             - almNORMAL(0) - Enabled and connection present
                             - almMAJOR(2) - Enabled and no connection present
                             - almDisable(3) - Disabled and no connection present
                             - almNotAvailable(4) - Telemetry is down or T1/E1 channel is not available
                            See Web, Monitor, Alarms, T1/E1 Input"
        ::= { remTe1AlarmsEntry 1 }

-- end remote Te1 alarms


    performance OBJECT IDENTIFIER ::= { radioMonitor 3 }

    perfLocal OBJECT IDENTIFIER ::= { performance 1 }

    perfRemote OBJECT IDENTIFIER ::= { performance 2 }


    locCurrentBER OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "BER * 1000000.0"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Curent Bit-Error Rate as scaled integer for local radio.
                            The BER multiplied by 1,000,000.
                            If the link is operating perfectly, this should indicate zero.
                            See Web, Monitor, Performance, Current BER"
        ::= { perfLocal 1 }

    locCurrentBERstr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Current Bit-Error Rate as a string. "
        ::= { perfLocal 2 }

    locCurrentRSL OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Current RSL is the measurement of the received signal level.
                            When the RSL falls below the threshold specification, 
                            the link disconnects and will not reconnect until 
                            the RSL is above the threshold specification.
                            See Web, Monitor, Performance, Current RSL"
        ::= { perfLocal 3 }

    locCurrentRSLstr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Current RSL as a string."
        ::= { perfLocal 4 }

    locErrorDuration OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "Seconds"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Error Duration indicates the total number of seconds that occurred where 
                            there was at least one bit error since the last time that 
                            the radio statistics counter was reset.
                            See Web, Monitor, Performance, Errored Seconds"
        ::= { perfLocal 5 }

    locErrorDurationStr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Error Duration as a formatted string."
        ::= { perfLocal 6 }

    locUnavailDuration OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "Seconds"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Unavailable Duration keeps track of every second where the BER equals or exceeds 1x10-3, 
                            as well as any seconds where there is a complete loss of radio communication.
                            See Web, Monitor, Performance, Unavailable Seconds"
        ::= { perfLocal 7 }

    locUnavailDurationStr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Unavailable Duration as a formatted string."
        ::= { perfLocal 8 }

    locMinRSL OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Minimum RSL indicates the worst (lowest) received signal level 
                            that occurred since the last counter reset.
                            See Web, Monitor, Performance, Minimum RSL"
        ::= { perfLocal 9 }

    locMinRSLstr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Minimum RSL value as a string."
        ::= { perfLocal 10 }

    locMinRSLtimestamp OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Minimum RSL Timestamp indicates the date and time when the Minimum RSL occurred.
                            See Web, Monitor, Performance, Minimum RSL Timestamp"
        ::= { perfLocal 11 }

    locMaxRSL OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Maximum RSL indicates the best (highest) RSL 
                            that occurred since the last counter reset.
                            See Web, Monitor, Performance, Maximum RSL"
        ::= { perfLocal 12 }

    locMaxRSLstr OBJECT-TYPE
        SYNTAX              DisplayString
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Maximum RSL level As string."
        ::= { perfLocal 13 }

    locSampleDuration OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "Seconds"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Sample Duration indicates the amount of time passed since the last counter reset.
                            See Web, Monitor, Performance, Time Since Reset"
        ::= { perfLocal 14 }

    locSampleDurationStr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Sample Duration value as a formatted string."
        ::= { perfLocal 15 }
 
    locEthPerfInterfaces    OBJECT-TYPE
        SYNTAX              SEQUENCE OF LocEthPerfInterfacesEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "Performance characteristics of local Ethernet interfaces"
        ::= { perfLocal 16 }

    locEthPerfInterfacesEntry     OBJECT-TYPE
        SYNTAX              LocEthPerfInterfacesEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION         "An entry in the Performance characteristics of local Ethernet interfaces table"
        INDEX               {
                                locEthUtilizationIn,
                                locEthUtilizationOut,
                                locEthSpeed
                            }
        ::= { locEthPerfInterfaces 1 }

    LocEthPerfInterfacesEntry ::= SEQUENCE {
        locEthUtilizationIn   Integer32,
        locEthUtilizationOut  Integer32,
        locEthSpeed           DisplayString
    }

    locEthUtilizationIn     OBJECT-TYPE
        SYNTAX              Integer32 (0..100)
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Inbound ethernet utilization (%).
                            See Web, Analysis, Ethernet Utilization."
        ::= { locEthPerfInterfacesEntry 1 }

    locEthUtilizationOut    OBJECT-TYPE
        SYNTAX              Integer32 (0..100)
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Outbound ethernet utilization (%).
                            See Web, Analysis, Ethernet Utilization."
        ::= { locEthPerfInterfacesEntry 2 }

    locEthSpeed    OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Current Ethernet Speed.
                            See Web, Monitor, Ethernet Performance."
        ::= { locEthPerfInterfacesEntry 3 }
 
    locEthUtilizationWatermarkEnabled OBJECT-TYPE
        SYNTAX              ExaltEnableT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Ethernet utilization watermark enable(1)/disable(0).
                            See Web, Analysis, Ethernet Utilization, Ethernet Utilization Watermark."
        ::= { perfLocal 17 }

    locEthUtilizationWatermark OBJECT-TYPE
        SYNTAX              Integer32 (0..100)
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Ethernet utilization watermark level (%).
                            See Web, Analysis, Ethernet Utilization, Watermark level."
        ::= { perfLocal 18 }

    locEthUtilizationWatermarkTrapEnabled OBJECT-TYPE
        SYNTAX              ExaltEnableT
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Ethernet utilization watermark trap enable(1)/disable(0).
                            The watermark trap function allows administrators to receive an SNMP trap
                            when watermark conditions are exceeded.
                            See Web, Analysis, Ethernet Utilization, Enable Ethernet Utilization Trap."
        ::= { perfLocal 19 }

    locEthUtilizationWatermarkTrapDuration OBJECT-TYPE
        SYNTAX              Integer32 (0..1440)
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Ethernet utilization trap limit in minutes/day (0-1440 minutes).
                            See Web, Analysis, Ethernet Utilization, Send trap if watermark hit duration exceeds."
        ::= { perfLocal 20 }
 
    locMaximumTxModulation OBJECT-TYPE
       SYNTAX               AcmModulationT
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The highest/maximum Tx modulation when ACM is enabled since the last counter reset.
                            See Web, Monitor, Performance, Tx modulation."
       ::= { perfLocal 100 }
    
    locActiveTxModulation OBJECT-TYPE
       SYNTAX               AcmModulationT
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The active Tx modulation when ACM is enabled.
                            See Web, Monitor, Performance, Tx modulation."
       ::= { perfLocal 101 }
    
    locMinimumTxModulation OBJECT-TYPE
       SYNTAX               AcmModulationT
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The lowest/minimum Tx modulation when ACM is enabled since the last counter reset.
                            See Web, Monitor, Performance, Tx modulation."
       ::= { perfLocal 102 }
    
    
    locMaximumRxModulation OBJECT-TYPE
       SYNTAX               AcmModulationT
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The highest/maximum Rx modulation when ACM is enabled since the last counter reset.
                            See Web, Monitor, Performance, Rx modulation."
       ::= { perfLocal 103 }
    
    
    locActiveRxModulation OBJECT-TYPE
       SYNTAX               AcmModulationT
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The active Rx modulation when ACM is enabled.
                            See Web, Monitor, Performance, Rx modulation."
       ::= { perfLocal 104 }
    
    
    locMinimumRxModulation OBJECT-TYPE
       SYNTAX               AcmModulationT
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The lowest/minimum Rx modulation when ACM is enabled since the last counter reset.
                            See Web, Monitor, Performance, Rx modulation."
       ::= { perfLocal 105 }
    
    
    --
    -- ACM Tx/Rx Ethernet throughtput
    --
    
    locMaximumTxEthernetThroughput OBJECT-TYPE
       SYNTAX               INTEGER
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The highest/maximum Tx Ethernet throughput in Mbps when ACM is enabled 
                            since the last counter reset.
                            See Web, Monitor, Performance, Tx Ethernet Throughput."
       ::= { perfLocal 106 }
    
    
    locActiveTxEthernetThroughput OBJECT-TYPE
       SYNTAX               INTEGER
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The active Tx Ethernet throughput in Mbps when ACM is enabled.
                            See Web, Monitor, Performance, Tx Ethernet Throughput."
       ::= { perfLocal 107 }
    
    
    locMinimumTxEthernetThroughput OBJECT-TYPE
       SYNTAX               INTEGER
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The lowest/minimum Tx Ethernet throughput in Mbps when ACM is enabled
                            since the last counter reset.
                            See Web, Monitor, Performance, Tx Ethernet Throughput."
       ::= { perfLocal 108 }
    
    
    locMaximumRxEthernetThroughput OBJECT-TYPE
       SYNTAX               INTEGER
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The highest/maximum Rx Ethernet throughput in Mbps when ACM is enabled
                            since the last counter reset.
                            See Web, Monitor, Performance, Rx Ethernet Throughput."
       ::= { perfLocal 109 }
    
    
    locActiveRxEthernetThroughput OBJECT-TYPE
       SYNTAX               INTEGER
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The active Rx Ethernet throughput in Mbps when ACM is enabled.
                            See Web, Monitor, Performance, Rx Ethernet Throughput."
       ::= { perfLocal 110 }
    
    
    locMinimumRxEthernetThroughput OBJECT-TYPE
       SYNTAX               INTEGER
       MAX-ACCESS           read-only
       STATUS               current
       DESCRIPTION          "The lowest/minimum Rx Ethernet throughput in Mbps when ACM is enabled
                            since the last counter reset.
                            See Web, Monitor, Performance, Rx Ethernet Throughput."
       ::= { perfLocal 111 }
    
    locResetStats OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Write 'reset' to locResetStats to clear the Performance statistics."
        ::= { perfLocal 1000 }


    remCurrentBER OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "BER * 1000000.0"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Curent Bit-Error Rate as scaled integer for far end radio.
                            The BER multiplied by 1,000,000.
                            If the link is operating perfectly, this should indicate zero.
                            See Web, Monitor, Performance, Current BER"
        ::= { perfRemote 1 }

    remCurrentBERstr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Current Bit-Error Rate as a string. Far end radio"
        ::= { perfRemote 2 }

    remCurrentRSL OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Current RSL is the measurement of the received signal level.
                            When the RSL falls below the threshold specification, 
                            the link disconnects and will not reconnect until 
                            the RSL is above the threshold specification.
                            See Web, Monitor, Performance, Current RSL"
        ::= { perfRemote 3 }

    remCurrentRSLstr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Current RSL as a string."
        ::= { perfRemote 4 }

    remErrorDuration OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "Seconds"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Error Duration indicates the total number of seconds that occurred where 
                            there was at least one bit error since the last time that 
                            the radio statistics counter was reset.
                            See Web, Monitor, Performance, Errored Seconds, Remote column."
        ::= { perfRemote 5 }

    remErrorDurationStr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Error Duration as a formatted string. Far end radio."
        ::= { perfRemote 6 }

    remUnavailDuration OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "Seconds"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Unavailable Duration keeps track of every second where the BER equals or exceeds 1x10-3, 
                            as well as any seconds where there is a complete loss of radio communication.
                            See Web, Monitor, Performance, Unavailable Seconds"
        ::= { perfRemote 7 }

    remUnavailDurationStr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Unavailable Duration as a formatted string. Far end radio."
        ::= { perfRemote 8 }

    remMinRSL OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Minimum RSL indicates the worst (lowest) received signal level 
                            that occurred since the last counter reset.
                            See Web, Monitor, Performance, Minimum RSL, Remote column."
        ::= { perfRemote 9 }

    remMinRSLstr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Minimum RSL value as a string. Far end radio."
        ::= { perfRemote 10 }

    remMinRSLtimestamp OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Minimum RSL Timestamp indicates the date and time when the Minimum RSL occurred.
                            See Web, Monitor, Performance, Minimum RSL Timestamp, Remote column."
        ::= { perfRemote 11 }

    remMaxRSL OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Maximum RSL indicates the best (highest) RSL 
                            that occurred since the last counter reset.
                            See Web, Monitor, Performance, Maximum RSL, Remote column."
        ::= { perfRemote 12 }

    remMaxRSLstr OBJECT-TYPE
        SYNTAX              DisplayString
        UNITS               "dBm"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Maximum RSL level As string. Far end radio."
        ::= { perfRemote 13 }

    remSampleDuration OBJECT-TYPE
        SYNTAX              Integer32
        UNITS               "Seconds"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Sample Duration indicates the amount of time passed since the last counter reset.
                            See Web, Monitor, Performance, Time Since Reset, Remote column."
        ::= { perfRemote 14 }

    remSampleDurationStr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Sample Duration value as a formatted string. Far end radio."
        ::= { perfRemote 15 }

    remResetStats OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Write 'reset' to remResetStats to clear the Performance statistics."
        ::= { perfRemote 1000 }

    userThroughput OBJECT IDENTIFIER ::= { radioMonitor 5 }

    aggregateUserThroughput OBJECT-TYPE
        SYNTAX              DisplayString
        UNITS               "MBit/s"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Aggregated User Throughput. 
                            For FDD radios this parameter is always equal to fullDuplexEthernetThroughput."
        ::= { userThroughput 1 }

    inboundEthernetThroughput OBJECT-TYPE
        SYNTAX              DisplayString
        UNITS               "MBit/s"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Inbound Ethernet Throughput.
                            For FDD radios this parameter is always N/A."
        ::= { userThroughput 2 }

    outboundEthernetThroughput OBJECT-TYPE
        SYNTAX              DisplayString
        UNITS               "MBit/s"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "Outbound Ethernet Throughput.
                            For FDD radios this parameter is always N/A."
        ::= { userThroughput 3 }

    fullDuplexEthernetThroughput OBJECT-TYPE
        SYNTAX              DisplayString
        UNITS               "MBit/s"
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION         "The Full Duplex Ethernet Throughput is determined by 
                            the combination of settings for Mode and Bandwidth.
                            See Web, Monitor, User Throughput, Full Duplex Ethernet Throughput."
        ::= { userThroughput 4 }

    radioReboot OBJECT-TYPE
        SYNTAX              DisplayString (SIZE(0..100))
        MAX-ACCESS          read-write
        STATUS              current
        DESCRIPTION         "Reboot the radio device.
                            Send 'reboot' to radioReboot parameter to reboot the radio device."
        ::= { productsMIBObjects 1000 }

    productsMIBConformance OBJECT IDENTIFIER ::= { productsMIB 3 }

    productsMIBCompliances OBJECT IDENTIFIER ::= { productsMIBConformance 1 }

    productsMIBGroups OBJECT IDENTIFIER ::= { productsMIBConformance 2 }

    productsAllObjects OBJECT-GROUP
        OBJECTS	{
        		modelName,
        		partNumber,
        		serialNumber,
        		interfaceType,
        		firmwareVersion,
			bootVersion,
        		rfFreqBand,
        		sysDate,
        		sysTime,
        		rnLocal,
        		rnRemote,
        		linkName,
        		linkSecKey,
        		adminPassword,
        		userPassword,
        		ipLocal,
        		ipRemote,
        		subnetMask,
        		ipAddressNetmask,
        		defaultGateway,
        		commitAdminSettings,
        		te1NumChannels,
        		te1NumActiveChannels,
        		selectT1orE1,
        		commitTe1Settings,
        		currentFwFilename,
        		alternateFwFilename,
        		swapFWimage,
        		locLinkState,
                        locLinkStateV,
                        locLinkStateH,
        		locTe1LinkSummary,
        		locTempAlarm,
        		locCurrentTemp,
        		locCurrentTempS,
		        locLinkSecMismatch,
        		remLinkState,
                        remLinkStateV,
                        remLinkStateH,
        		remTe1LinkSummary,
        		remTempAlarm,
        		remCurrentTemp,
        		remCurrentTempS,
		        remLinkSecMismatch,
        		locCurrentBER,
        		locCurrentBERstr,
        		locCurrentRSL,
        		locCurrentRSLstr,
        		locErrorDuration,
        		locErrorDurationStr,
        		locUnavailDuration,
        		locUnavailDurationStr,
        		locMinRSL,
        		locMinRSLstr,
        		locMinRSLtimestamp,
        		locMaxRSL,
        		locMaxRSLstr,
        		locSampleDuration,
        		locSampleDurationStr,
        		locResetStats,
        		remCurrentBER,
        		remCurrentBERstr,
        		remCurrentRSL,
        		remCurrentRSLstr,
        		remErrorDuration,
        		remErrorDurationStr,
        		remUnavailDuration,
        		remUnavailDurationStr,
        		remMinRSL,
        		remMinRSLstr,
        		remMinRSLtimestamp,
        		remMaxRSL,
        		remMaxRSLstr,
        		remSampleDuration,
        		remSampleDurationStr,
        		remResetStats,
        		radioReboot,
        		te1Status,
        		t1LBO,
        		te1AIS,
        		t1LineCode,
        		te1LoopBackMode,
        		locTe1Alarm,
        		remTe1Alarm,
			aesEnable,
			licKey,
                aggregateUserThroughput,
                inboundEthernetThroughput,
                outboundEthernetThroughput,
                fullDuplexEthernetThroughput,
                locEthUtilizationIn,
                locEthUtilizationOut,
                locEthUtilizationWatermarkEnabled,
                locEthUtilizationWatermark,
                locEthUtilizationWatermarkTrapEnabled,
                locEthUtilizationWatermarkTrapDuration
        	}
        STATUS		    current
        DESCRIPTION         "This automatically created object group contains
                            all those objects that do not belong to any other
                            OBJECT-GROUP"
        ::= { productsMIBGroups 1 }

END

