-- This file was included in WWP MIB release 04-10-01-0027
 --
 -- WWP-LEOS-PORT-MIB.my
 --
 --

 WWP-LEOS-PORT-MIB DEFINITIONS ::= BEGIN

 IMPORTS                
   Integer32, Unsigned32, Counter32, Gauge32, TimeTicks, OBJECT-TYPE, NOTIFICATION-TYPE, MODULE-IDENTITY                  
        FROM SNMPv2-SMI                 
   DisplayString, MacAddress, TEXTUAL-CONVENTION, TruthValue, RowStatus
        FROM SNMPv2-TC
   sysName, sysLocation
        FROM RFC1213-MIB                                                        
   wwpModules, wwpModulesLeos           
        FROM WWP-SMI
   dot3adAggPortActorAdminKey, dot3adAggPortListPorts
	FROM IEEE8023-LAG-MIB;

        
 wwpLeosPortMIB MODULE-IDENTITY
         LAST-UPDATED "201205250000Z"
         ORGANIZATION "Ciena, Inc"
         CONTACT-INFO
                  "Mib Meister
                   115 North Sullivan Road
                   Spokane Valley, WA 99037
                   USA           
                   Phone:  +1 509 242 9000
                   Email:  support@ciena.com"
	  DESCRIPTION
                  "This MIB defines the managed objects for Ethernet ports."

          REVISION    "201205250000Z"
          DESCRIPTION
	          "Added wwpLeosEtherPortAdvertSpeed and wwpLeosEtherPortAdvertDuplex to WwpLeosEtherPortEntry  MIB object"	   
          REVISION    "201102020000Z"
          DESCRIPTION
	          "Added admitOnlyUntagged to wwpLeosEtherPortAcceptableFrameTypes MIB object"	   
          REVISION    "201011010000Z" 
          DESCRIPTION
          	  "Added wwpLeosEtherPortEgressCosPolicy"
          REVISION    "201007280000Z" 
          DESCRIPTION
          	  "Added wwpLeosEtherFixedRColor and wwpLeosEtherPortFrameCosMapId mib objects"
          REVISION    "201005051700Z"      
          DESCRIPTION
                  "Added changed length of wwpLeosPortDescr from 32 to 128."
          REVISION    "200811140000Z"
          DESCRIPTION
          	  "Added wwpLeosEtherPortEgressPortQueueMapId to wwpLeosEtherPortEntryTable.
          	   Added 10 gig option to wwpLeosEtherInterfaceType, wwpLeosEtherAdminSpeed and wwpLeosEtherOperSpeed"
          REVISION    "200807210000Z" 
          DESCRIPTION
          	  "Added wwpLeosEtherPortResolvedCosPolicy,wwpLeosEtherPortMode and wwpLeosEtherFixedRcos mib objects"
          REVISION    "200708110000Z"
          DESCRIPTION
                  "Added new mib object wwpLeosEtherPortStateMirrorGroupType."
          REVISION    "200706200000Z"
          DESCRIPTION
                  "Added new mib object wwpLeosEtherPortUntagDataVid."
          REVISION    "200605260000Z"
          DESCRIPTION
                  "Added new mib object wwpLeosEtherPortOperAutoNeg."                   
          REVISION    "200605180000Z"
          DESCRIPTION
                  "Added new mib object wwpLeosEtherPortStateMirrorGroupOperStatus.
                   Added new mib object wwpLeosEtherPortStateMirrorGroupNumSrcPorts.
                   Added new mib object wwpLeosEtherPortStateMirrorGroupNumDstPorts.
                   Added new mib object wwpLeosEtherPortStateMirrorGroupMemOperState."
          REVISION    "200603150000Z"
          DESCRIPTION
                  "This MIB module is for the Extension of the dot1dBasePortTable for WWP Products"
          REVISION    "200507280000Z"
          DESCRIPTION
                  "Added eumeration to wwpLeosEtherPortAdminSpeed."
          REVISION    "200404181700Z"
          DESCRIPTION
                  "Added new tables to support port state mirroring feature."            
          ::= { wwpModulesLeos 2 }


 --
 -- Textual conventions
 --

 PortList ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Each octet within this value specifies a set of eight
        ports, with the first octet specifying ports 1 through
        8, the second octet specifying ports 9 through 16, etc.
        Within each octet, the most significant bit represents
        the lowest numbered port, and the least significant bit
        represents the highest numbered port.  Thus, each port
        of the bridge is represented by a single bit within the
        value of this object.  If that bit has a value of '1'
        then that port is included in the set of ports; the port
        is not included if its bit has a value of '0'."
    SYNTAX      OCTET STRING (SIZE (0..255))

  PortEgressFrameCosPolicy ::= TEXTUAL-CONVENTION
  	STATUS			current
  	DESCRIPTION		"Egress cos policy to use on this port
			         ignore means leave egress map disabled"
  	SYNTAX			INTEGER {
  					ingore (1),
  					rcosToL2OuterPcpMap (2)
				}

  PortIngressFixedColor ::= TEXTUAL-CONVENTION
  	STATUS			current
  	DESCRIPTION		"Egress cos policy to use on this port
			         ignore means leave egress map disabled"
  	SYNTAX			INTEGER {
  					green (1),
  					yellow (2)
				}

    
 --
 -- Node definitions
 --
        
 wwpLeosPortMIBObjects OBJECT IDENTIFIER ::= { wwpLeosPortMIB 1 }
 
 wwpLeosEtherPort OBJECT IDENTIFIER ::= { wwpLeosPortMIBObjects 1 }

 wwpLeosEtherPortNotif OBJECT IDENTIFIER ::= { wwpLeosPortMIBObjects 2 }

 -- Notifications 
  
 wwpLeosPortMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosPortMIB 2 } 
 wwpLeosPortMIBNotifications       OBJECT IDENTIFIER ::=  
                       { wwpLeosPortMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosPortMIBConformance OBJECT IDENTIFIER ::= { wwpLeosPortMIB 3 } 
 wwpLeosPortMIBCompliances OBJECT IDENTIFIER ::= { wwpLeosPortMIBConformance 1 }                
 wwpLeosPortMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosPortMIBConformance 2 }

 
 wwpLeosEtherPortTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosEtherPortEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of Ethernet Ports."
     ::= { wwpLeosEtherPort 1 }
                
 wwpLeosEtherPortEntry OBJECT-TYPE
     SYNTAX       WwpLeosEtherPortEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Port Entry in the Ethernet Port Table."
     INDEX { wwpLeosEtherPortId }
     ::= { wwpLeosEtherPortTable 1 } 

 WwpLeosEtherPortEntry ::= SEQUENCE { 
     wwpLeosEtherPortId                         INTEGER,
     wwpLeosEtherPortName                       DisplayString,
     wwpLeosEtherPortDesc                       DisplayString,
     wwpLeosEtherPortType                       INTEGER,
     wwpLeosEtherPortPhysAddr                   MacAddress,
     wwpLeosEtherPortAutoNeg                    TruthValue,
     wwpLeosEtherPortAdminStatus                INTEGER,
     wwpLeosEtherPortOperStatus                 INTEGER,
     wwpLeosEtherPortAdminSpeed                 INTEGER,
     wwpLeosEtherPortOperSpeed                  INTEGER,
     wwpLeosEtherPortAdminDuplex                INTEGER,
     wwpLeosEtherPortOperDuplex                 INTEGER,
     wwpLeosEtherPortAdminFlowCtrl              INTEGER,
     wwpLeosEtherPortOperFlowCtrl               INTEGER, 
     wwpLeosEtherIngressPvid                    INTEGER,
     wwpLeosEtherUntagEgressVlanId              INTEGER,
     wwpLeosEtherPortAcceptableFrameTypes       INTEGER,
     wwpLeosEtherPortUntaggedPriority           INTEGER,
     wwpLeosEtherPortMaxFrameSize               INTEGER,
     wwpLeosEtherPortVlanIngressFiltering       TruthValue,
     wwpLeosEtherPortAdminAdvertisedFlowCtrl    INTEGER,
     wwpLeosEtherPortVplsPortType               INTEGER,
     wwpLeosEtherPortIngressCosPolicy           INTEGER,
     wwpLeosEtherPortIngressFixedDot1dPri       INTEGER,
     wwpLeosEtherPortUntagDataVsi               INTEGER,
     wwpLeosEtherPortOperationalSpeed           Gauge32,
     wwpLeosEtherPortUntagCtrlVsi               INTEGER,
     wwpLeosEtherPortMirrorPort                 TruthValue,
     wwpLeosEtherPortMirrorEncap                INTEGER,
     wwpLeosEtherPortMirrorEncapVid             INTEGER,
     wwpLeosEtherPortMirrorEncapTpid            INTEGER,
     wwpLeosEtherPortMirrorIngress              INTEGER,
     wwpLeosEtherPortMirrorEgress               INTEGER,
     wwpLeosEtherPortUntagDataVsiType           INTEGER,
     wwpLeosEtherPortUntagCtrlVsiType           INTEGER,
     wwpLeosEtherPortVsIngressFiltering         TruthValue,
     wwpLeosEtherPortOperAutoNeg                INTEGER,
     wwpLeosEtherPortUpTime                     TimeTicks,
     wwpLeosEtherPortUntagDataVid               INTEGER,
     wwpLeosEtherPortPhyLoopback                TruthValue,
     wwpLeosEtherPortVlanIngressFilterStrict    TruthValue,
     wwpLeosEtherPortMacSaDaSwap                TruthValue,
     wwpLeosEtherPortMacSaDaSwapVlan            INTEGER,
     wwpLeosEtherPortResolvedCosPolicy          INTEGER,
     wwpLeosEtherPortMode                       INTEGER,
     wwpLeosEtherFixedRcos                      INTEGER,
     wwpLeosEtherPortEgressPortQueueMapId       INTEGER,
     wwpLeosEtherPortResolvedCosMapId           INTEGER,
     wwpLeosEtherPortResolvedCosRemarkL2        TruthValue,
     wwpLeosEtherPortL2TransformMode            INTEGER,
     wwpLeosEtherPortLinkFlapDetection          TruthValue,
     wwpLeosEtherPortLinkFlapCount              INTEGER,
     wwpLeosEtherPortLinkFlapDetectTime         INTEGER,
     wwpLeosEtherPortLinkFlapHoldTime           INTEGER,
     wwpLeosEtherFixedRColor                    PortIngressFixedColor,
     wwpLeosEtherPortFrameCosMapId              INTEGER,
     wwpLeosEtherPortEgressCosPolicy		      PortEgressFrameCosPolicy,
     wwpLeosEtherPortEgressSpeed                Gauge32,
     wwpLeosEtherPortAdaptiveRateSpeed          Gauge32,
     wwpLeosEtherPortIfgDecrease                Integer32,
     wwpLeosEtherPortAdvertSpeed                INTEGER,
     wwpLeosEtherPortAdvertDuplex               INTEGER 
  } 
 

 wwpLeosEtherPortId   OBJECT-TYPE
     SYNTAX         INTEGER (1..65535) 
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "Port ID for the instance.  Port ID's start at 1, 
             and may not be consecutive for each additional port. 
             This port Id should refer to the dot1dBasePort in the 
             Dot1dBasePortEntry."
     ::= { wwpLeosEtherPortEntry 1 }            
 
 wwpLeosEtherPortName OBJECT-TYPE
     SYNTAX      DisplayString (SIZE (0..8))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
             "A textual string containing information about the
             port. This string should indicate about the physical
             location of the port as well."
     ::= { wwpLeosEtherPortEntry 2 }
 
 wwpLeosEtherPortDesc OBJECT-TYPE
     SYNTAX      DisplayString (SIZE (0..128))
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
             "A textual string containing port description."
     ::= { wwpLeosEtherPortEntry 3 }

 wwpLeosEtherPortType OBJECT-TYPE
     SYNTAX        INTEGER {
                        ethernet(1),
                        fastEthernet(2),
                        hundredFx(3),
                        gigEthernet(4),                 
                        lagPort(5),
                        unknown(6),
                        gigHundredFx(7),
                        tripleSpeed(8),
                        tenGigEthernet(9),
                        gigTenGigEthernet(10)
                   }
     MAX-ACCESS    read-only
     STATUS        current
     DESCRIPTION
             "The port type for the port."
     ::= { wwpLeosEtherPortEntry 4 }  

 wwpLeosEtherPortPhysAddr OBJECT-TYPE
     SYNTAX       MacAddress
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "The ethernet MAC address for the port. This information can also
             be achieved via dot1dTpFdbTable"
     ::= { wwpLeosEtherPortEntry 5 }
                
 wwpLeosEtherPortAutoNeg  OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "The object sets the port to AUTO NEG MOde and vice versa.
             Specific platforms may have requirements of configuring
             speed before moving the port to out of AUTO-NEG mode."
     ::= { wwpLeosEtherPortEntry 6 }

 wwpLeosEtherPortAdminStatus OBJECT-TYPE
     SYNTAX       INTEGER {
                       up(1),
                       down(2)
                  }
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "The desired state of the port."
     ::= { wwpLeosEtherPortEntry 7 }
                
 wwpLeosEtherPortOperStatus OBJECT-TYPE
     SYNTAX        INTEGER {
                        up(1),
                        down(2),
                        notauth(3),
                        lbtx(4),
                        lbrx(5),
                        linkflap(6)
                   }
     MAX-ACCESS    read-only
     STATUS        current
     DESCRIPTION
             "The current operational state of Port."
     ::= { wwpLeosEtherPortEntry 8 }
                
 wwpLeosEtherPortAdminSpeed OBJECT-TYPE
     SYNTAX        INTEGER {
                        tenMb(1),
                        hundredMb(2),
                        gig(3),
                        auto(4),
                        tenGig(5)
                   }
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION
             "Desired speed of the port. 
             Set the port speed to be either 10MB, 100MB, or gig.  Set the
             port speed to auto to enable automatic port speed detection.
             The default value for this object depends upon the platform."
     ::= { wwpLeosEtherPortEntry 9 }
                
 wwpLeosEtherPortOperSpeed OBJECT-TYPE
     SYNTAX      INTEGER {
                        unknown(0),
                        tenMb(1),
                        hundredMb(2),
                        gig(3),
                        tenGig(4)
                   }
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
             "The current operational speed of the port."
     ::= { wwpLeosEtherPortEntry 10 }
                
 wwpLeosEtherPortAdminDuplex OBJECT-TYPE
     SYNTAX         INTEGER {
                         half(1),
                         full(2)
                     }
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
             "The desired mode for the port. It can be set to either half or 
             full duplex operation. The default value for this object 
             depends upon the platform."
     ::= { wwpLeosEtherPortEntry 11 }
                
 wwpLeosEtherPortOperDuplex OBJECT-TYPE
     SYNTAX        INTEGER {
                        half(1),
                        full(2)   
                   }
     MAX-ACCESS    read-only
     STATUS        current
     DESCRIPTION
             "The current duplex mode of the port."
     ::= { wwpLeosEtherPortEntry 12 }
                
 wwpLeosEtherPortAdminFlowCtrl OBJECT-TYPE
     SYNTAX           INTEGER {
                           unknown(1),
                           off(2),
                           asymTx(3),
                           asymRx(4),
                           sym(5)                           
                      }
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "Configures the ports flow control operation."
     ::= { wwpLeosEtherPortEntry 13 }
                
 wwpLeosEtherPortOperFlowCtrl OBJECT-TYPE
      SYNTAX          INTEGER {
                           unknown(1),
                           off(2),
                           asymTx(3),
                           asymRx(4),
                           sym(5)                           
                      }
     MAX-ACCESS       read-only
     STATUS           current
     DESCRIPTION
             "Shows ports flow control configuration."
     ::= { wwpLeosEtherPortEntry 14 }
                
 wwpLeosEtherIngressPvid OBJECT-TYPE
     SYNTAX           INTEGER (1..24576)  
     MAX-ACCESS       read-write
     STATUS           current    
     DESCRIPTION
             "The Ingress PVID, the VLAN ID associated with untagged frames ingressing 
              the port or if tunnel is enabled on this port. The max value for this 
              object is platform dependent. Refer to architecture document for details 
              of platform dependency."
     REFERENCE
         "IEEE 802.1Q/D11 Section 12.10.1.1"
     DEFVAL      { 1 } 
     ::= { wwpLeosEtherPortEntry 15 }
          
 wwpLeosEtherUntagEgressVlanId OBJECT-TYPE
     SYNTAX           INTEGER (0..24576)
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "All the egress frames whose VLAN id matches the wwpLeosEtherUntagEgressVlanId, will 
              egress the port as untagged. To egress the frames tagged set 
              wwpLeosEtherUntagEgressVlanId to 0. The max value for this object is 
              platform dependent. Refer to architecture document for 
              details of platform dependency."
     ::= { wwpLeosEtherPortEntry 16 }
 
 wwpLeosEtherPortAcceptableFrameTypes OBJECT-TYPE
     SYNTAX           INTEGER {
                          admitAll(1),
                          admitOnlyVlanTagged(2),
                          admitOnlyUntagged(3)
                      }
    MAX-ACCESS        read-write
    STATUS            current
    DESCRIPTION
            "When this is admitOnlyVlanTagged(2) the device will
            discard untagged frames or Priority-Tagged frames
            received on this port.  When admitOnlyUntagged(3) is set,
            the device will discard VLAN tagged frames received on
            this port.  With admitOnlyUntagged(3) and admitAll(1),
            untagged frames or Priority-Tagged frames received on this
            port will be accepted and assigned to the PVID for this port.

            This control does not affect VLAN independent BPDU
            frames, such as GVRP and STP.  It does affect VLAN
            dependent BPDU frames, such as GMRP."
    REFERENCE
        "IEEE 802.1Q/D11 Section 12.10.1.3"
    DEFVAL      { admitAll }
     ::= { wwpLeosEtherPortEntry 17 }
          
 wwpLeosEtherPortUntaggedPriority OBJECT-TYPE
     SYNTAX       INTEGER {     
                       p0(0),
                       p1(1),
                       p2(2),
                       p3(3),
                       p4(4),
                       p5(5),
                       p6(6),
                       p7(7)
                   }
     MAX-ACCESS    read-write
     STATUS        deprecated
     DESCRIPTION
             "The 802.1p packet priority to be assigned to packets ingressing 
              this port that do not have an 802.1Q VLAN header. This priority 
              is also assigned to ingress frame if tunnel is enabled on this port."
     ::= { wwpLeosEtherPortEntry 18 }

 wwpLeosEtherPortMaxFrameSize OBJECT-TYPE
    SYNTAX           INTEGER (1522..9216)
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
            "Setting this object will set the max frame size allowed on a 
             port. The max frame size can vary from 1522 bytes to 9216 bytes. 
             Default value is 1526 bytes."
    ::= { wwpLeosEtherPortEntry 19 }

 
 wwpLeosEtherPortVlanIngressFiltering   OBJECT-TYPE
     SYNTAX         TruthValue
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
             "When this is true(1) the device will discard incoming
              frames for VLANs which do not include this Port in its
              Member set.  When false(2), the port will accept all
              incoming frames."
     DEFVAL { true }
     ::= { wwpLeosEtherPortEntry 20 }
 
 wwpLeosEtherPortAdminAdvertisedFlowCtrl OBJECT-TYPE
     SYNTAX           INTEGER {
                           unknown(1),
                           off(2),
                           asymTx(3),
                           sym(4),
                           symAsymRx(5)
                      }
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "This object specifies the advertised flow control
              for given port."
     ::= { wwpLeosEtherPortEntry 21 }
     
 wwpLeosEtherPortVplsPortType OBJECT-TYPE
     SYNTAX           INTEGER {
                                                notDefined(1),
                                                subscriber(2),
                                                networkFacing(3)                                                
                                        }
     MAX-ACCESS       read-only
     STATUS           current
     DESCRIPTION
             "This object specifies whether port is in subscriber type,
              network facing side or both. "
     ::= { wwpLeosEtherPortEntry 22 }
     
 wwpLeosEtherPortIngressCosPolicy OBJECT-TYPE
     SYNTAX           INTEGER {                                                 
                                                leave(1),
                                                fixed(2),
                                                ippInherit(3),
                                                phbgInherit(4)
                                        }
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "This object specifies the ingress cos policy to be applied to all 
              frames coming in on the given port."
     ::= { wwpLeosEtherPortEntry 23 }     
      
 wwpLeosEtherPortIngressFixedDot1dPri OBJECT-TYPE
     SYNTAX           INTEGER (0..7)
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "The 802.1p packet priority to be assigned to packets ingressing 
              this port that do not have an 802.1Q VLAN header. This priority 
              is also assigned to ingress untagged frame if the virtual switch 
              cos policy is set to 'fix' for a given port."
     ::= { wwpLeosEtherPortEntry 24 }
     
  wwpLeosEtherPortUntagDataVsi OBJECT-TYPE
     SYNTAX           INTEGER (0..65535)
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "This object specifies the virtual switch to be used for this 
              port if data frame is untagged. If this object is set to 0 then 
              device will unset this object. 
              When setting this object to Mpls Vsi Index then wwpLeosEtherPortUntagDataVsiType must also
              be set to mpls (Use multiple set operation)"
     ::= { wwpLeosEtherPortEntry 25 } 
     
  wwpLeosEtherPortOperationalSpeed OBJECT-TYPE
     SYNTAX      Gauge32
     UNITS      "kbps"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
             "An estimate of the port's current bandwidth in k-bits per second
              for given port."
     ::= { wwpLeosEtherPortEntry 26 }
     
  wwpLeosEtherPortUntagCtrlVsi OBJECT-TYPE
     SYNTAX           INTEGER (0..65535)
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "This object specifies the virtual switch to be used for this 
              port if control frame is untagged. If this object is set to 0 then 
              device will unset this object. 
              When setting this object to Mpls Vsi Index then wwpLeosEtherPortUntagCtrlVsiType must also
              be set to mpls (Use multiple set operation)"
     ::= { wwpLeosEtherPortEntry 27 } 
 
  wwpLeosEtherPortMirrorPort  OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines whether the port will allow traffic from other ports to 
             be mirrored to this port.
             To allow traffic from other ports to be sent to this port, set this object to
             True(1). This port is known as a mirror port.
             If set to true, then other ports may set the values of their 
             wwpLeosEtherPortMirrorIngress or wwpLeosEtherPortMirrorEgress
             objects to the port index of this port.
             Setting this object to false(2) disables this port as a mirror port."           
     DEFVAL { false }
     ::= { wwpLeosEtherPortEntry 28 }
  
  wwpLeosEtherPortMirrorIngress  OBJECT-TYPE
     SYNTAX       INTEGER (0..65535)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "The value of this object is the port index of a mirror port. The ingress traffic
             of this port can be mirrored by setting the destination port's wwpLeosEtherPortMirrorPort
             object to true.
             If the value of this object is set to zero this port's ingress traffic will not be mirrored."
     DEFVAL {0}
     ::= { wwpLeosEtherPortEntry 29 }

  wwpLeosEtherPortMirrorEgress  OBJECT-TYPE
     SYNTAX       INTEGER (0..65535)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "The value of this object is the port index of a mirror port. The egress traffic
             of this port can be mirrored by setting the destination port's wwpLeosEtherPortMirrorPort
             object to true.
             If the value of this object is set to zero this port's egress traffic will not be mirrored."            
     DEFVAL {0}
     ::= { wwpLeosEtherPortEntry 30 }

  wwpLeosEtherPortUntagDataVsiType  OBJECT-TYPE
     SYNTAX       INTEGER { 
                  ethernet(1),
                  mpls(2)                    
               }
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object specifies the virtual switch instance type associated with this
              port. This object defaults to ethernet and specifies if  
              wwpLeosEtherPortUntagDataVsi belongs to ethernet virtual switch table 
              (wwpLeosVplsVirtualSwitchEthTable in WWP-LEOS-VPLS-MIB) 
              or mpls virtual switch table (wwpLeosVplsVirtualSwitchMplsTable in
              WWP-LEOS-VPLS-MIB).
              When setting wwpLeosEtherPortUntagDataVsi to MPLS Vsi Index then this object must also be set to
              mpls (Use mutliple set operation)."            
     DEFVAL {ethernet}
     ::= { wwpLeosEtherPortEntry 31 }
 
 wwpLeosEtherPortUntagCtrlVsiType  OBJECT-TYPE
     SYNTAX       INTEGER { 
                  ethernet(1),
                  mpls(2)                    
               }
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object specifies the virtual switch instance type associated with this
              port. This object defaults to ethernet and specifies if  
              wwpLeosEtherPortUntagCtrlVsi belongs to ethernet virtual switch table 
              (wwpLeosVplsVirtualSwitchEthTable) or mpls virtual switch table
              (wwpLeosVplsVirtualSwitchMplsTable).
              When setting wwpLeosEtherPortUntagCtrlVsi to MPLS Vsi Index then this object must also be set to
              mpls (Use mutliple set operation)"            
     DEFVAL {ethernet}
     ::= { wwpLeosEtherPortEntry 32 }

 wwpLeosEtherPortVsIngressFiltering   OBJECT-TYPE
     SYNTAX         TruthValue
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
             "This item is applicable to this port when the port is
              added as a per-port member to a virtual switch. If true(1) the device
              will discard incoming tagged frames. If false(2) the device will
              forwared incoming tagged frames so long as those customer tagged
              frames do not match another virtual switch with this port included as
              a per-port-per-vlan member."
     DEFVAL { false }
     ::= { wwpLeosEtherPortEntry 33 } 
     
 wwpLeosEtherPortOperAutoNeg  OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "The object specifies the operational auto neg state."
     ::= { wwpLeosEtherPortEntry 34 }
 
 wwpLeosEtherPortUpTime  OBJECT-TYPE
     SYNTAX       TimeTicks
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "The object specifies the port up time in hundredths of a second."
     ::= { wwpLeosEtherPortEntry 35 }

 wwpLeosEtherPortUntagDataVid OBJECT-TYPE
     SYNTAX           INTEGER (0..24576)  
     MAX-ACCESS       read-write
     STATUS           current    
     DESCRIPTION
             "The Ingress Untagged Data Vid, the VLAN ID stamped on untagged frames
              ingressing the port or if tunnel is enabled on this port. To disable
              tagging of untagged data on ingress write a value of 0. The max value
              for this object is platform dependent. Refer to architecture document
              for details of platform dependency."
     REFERENCE
         "IEEE 802.1Q/D11 Section 12.10.1.1"
     DEFVAL      { 1 } 
     ::= { wwpLeosEtherPortEntry 36 }

 wwpLeosEtherPortPhyLoopback  OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines whether the phy has been placed in loopback mode,
             which causes frames egressing the port to be looped back to the port."
     DEFVAL { false }
     ::= { wwpLeosEtherPortEntry 37 }

 wwpLeosEtherPortVlanIngressFilterStrict  OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This item is applicable to this port when the port is
              added as a to a virtual switch. If true(1) the legacy ingress filter behavior
              will be enforced at member addition (drop bit will be set to drop untagged
              traffic).  If false, the splat bit will not be changed.  Note that external 
              VLAN associations are also maintained when strict is false."
     DEFVAL { false }
     ::= { wwpLeosEtherPortEntry 38 }
     
 wwpLeosEtherPortMacSaDaSwap  OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines whether the MAC SA and DA will be swapped on
             frames egressing the port.  This only works on a 311V."
     DEFVAL { false }
     ::= { wwpLeosEtherPortEntry 39 }
     
  wwpLeosEtherPortMacSaDaSwapVlan  OBJECT-TYPE
     SYNTAX       INTEGER (0..24576)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines whether the MAC SA and DA will be swapped on
             specific VLAN frames egressing the port.  This only works on a 311V."
     DEFVAL { 0 }
     ::= { wwpLeosEtherPortEntry 40 }
    
   wwpLeosEtherPortResolvedCosPolicy  OBJECT-TYPE
  SYNTAX INTEGER {
                          dot1d(1),
                          l3DscpCos(2),
                          fixedCos(3),
                          unknown(99)
                      }
    MAX-ACCESS        read-write
    STATUS            current
    DESCRIPTION  
      " The Resolved Cost Policy.
      Setting this attribute is not supported in leos version 4"
     ::= { wwpLeosEtherPortEntry 41 }
     
  wwpLeosEtherPortMode  OBJECT-TYPE   
    SYNTAX  INTEGER {
             rj45(1),
                sfp(2),
                default(3),
                unknown(99)
            }
      MAX-ACCESS        read-write
    STATUS            current
    DESCRIPTION 
      "The mode of the port
      Setting this attribute is not supported in leos version 4"
    ::= { wwpLeosEtherPortEntry 42 }
    
  wwpLeosEtherFixedRcos  OBJECT-TYPE
    SYNTAX   INTEGER (0..7)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION   
      "The fixed Resolve Cost value.
      Setting this attribute is not supported in leos version 4"
    ::= { wwpLeosEtherPortEntry 43 }
    
 wwpLeosEtherPortEgressPortQueueMapId  OBJECT-TYPE
    SYNTAX   INTEGER (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION   
      "The Egress-port-Queue associated with this port.
      Setting this attribute is not supported in leos version 4"
    ::= { wwpLeosEtherPortEntry 44 }  
    
 wwpLeosEtherPortResolvedCosMapId   OBJECT-TYPE
   SYNTAX      INTEGER (1..65535)
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "RCOS map id for the port.
      Setting this attribute is not supported in leos version 4"
   ::= { wwpLeosEtherPortEntry 45 }  
   
 wwpLeosEtherPortResolvedCosRemarkL2   OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "The object specifies whether to remark L2 based on L3. This applies when the 
      resolved cos policy is either l3-dscp-cos or dot1d-tag1-cos but not when it is 
      fixed-cos policy. Setting this attribute is not supported in leos version 4"
   ::= { wwpLeosEtherPortEntry 46 }

  wwpLeosEtherPortL2TransformMode   OBJECT-TYPE
   SYNTAX      INTEGER  {
                   none(0),
                   iPush-e-Pop(1),
                   iStamp-Push-e-QualifiedPopStamp(2),
                   iPush-e-PopStamp(3)
                  }                   
   MAX-ACCESS     read-write
   STATUS         current
   DESCRIPTION
      "L2 transform action for port.
      Setting this attribute is not supported in leos version 4"
   DEFVAL { 1 }
   ::= { wwpLeosEtherPortEntry  47 }

  wwpLeosEtherPortLinkFlapDetection  OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines whether link flap detection will be
             enabled on the port."
     DEFVAL { false }
     ::= { wwpLeosEtherPortEntry 48 }
       
  wwpLeosEtherPortLinkFlapCount  OBJECT-TYPE
     SYNTAX       INTEGER (1..64)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines how many link down events are required
             to trigger a link flap event."
     DEFVAL { 5 }
     ::= { wwpLeosEtherPortEntry 49 }

  wwpLeosEtherPortLinkFlapDetectTime  OBJECT-TYPE
     SYNTAX       INTEGER (1..600)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines the time in seconds during which link
             down events are accumlated to trigger a link flap event."
     DEFVAL { 10 }
     ::= { wwpLeosEtherPortEntry 50 }

  wwpLeosEtherPortLinkFlapHoldTime  OBJECT-TYPE
     SYNTAX       INTEGER (0..600)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines the time in seconds that a port will
             be operationally disabled after a link flap event, before
             it is re-enabled.  A value of zero causes the port to
             remain disabled until manually enabled."
     DEFVAL { 300 }
     ::= { wwpLeosEtherPortEntry 51 }

  wwpLeosEtherFixedRColor  OBJECT-TYPE
     SYNTAX       PortIngressFixedColor
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This sets the fixed color to green (default) or yellow.
              Setting this attribute is not supported in saos version 4"
     DEFVAL { 1 }
     ::= { wwpLeosEtherPortEntry 52 }

 wwpLeosEtherPortFrameCosMapId   OBJECT-TYPE
   SYNTAX      INTEGER (1..65535)
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "Frame COS map id for the port.
      Setting this attribute is not supported in leos version 4"
   DEFVAL { 1 }
   ::= { wwpLeosEtherPortEntry 53 }  


 wwpLeosEtherPortEgressCosPolicy   OBJECT-TYPE
   SYNTAX      PortEgressFrameCosPolicy 
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "Sets the egress frame cos policy
      Setting this attribute is not supported in leos version 4"
   DEFVAL { 1 }
   ::= { wwpLeosEtherPortEntry 54 }
   
  wwpLeosEtherPortEgressSpeed OBJECT-TYPE
     SYNTAX       Gauge32
     UNITS        "kbps"
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION  "An estimate of the port's current egress bandwidth restriction
                   in k-bits per second for given port.  A value of 0 means there
		             is no active restriction. This attribute not supported in leos
                   version 6"
     ::= { wwpLeosEtherPortEntry 55 }
     
  wwpLeosEtherPortAdaptiveRateSpeed OBJECT-TYPE
     SYNTAX       Gauge32
     UNITS        "kbps"
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION  "An estimate of the port's current adaptive-rate bandwidth restriction
                   in k-bits per second for given port.  A value of 0 means there is no
		             active restriction. This attribute not supported in leos version 6"
     ::= { wwpLeosEtherPortEntry 56 }
  
  wwpLeosEtherPortMirrorEncap OBJECT-TYPE
     SYNTAX           INTEGER {
                           none(0),
                           vlanTag(1)
                      }
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines whether the port will encapsulate mirrored
             frames by adding a vlan-tag. (Or, in the case where a mirrored
             frame is already tagged, by adding a further vlan-tag to the frame)
             To allow mirrored traffic to be encapsulated, set this object to
             vlan-tag(1). 
             If set to vlan-tag, then the values of 
             wwpLeosEtherPortMirrorEncapVid and wwpLeosEtherPortMirrorEncapTpid
             will be used to populate tag added to each mirrored frame.
             Setting this object to none(0) indicates no tag is to be added
             to the mirrored frames."           
     DEFVAL { none }
     ::= { wwpLeosEtherPortEntry 57 }
  
  wwpLeosEtherPortMirrorEncapVid OBJECT-TYPE
     SYNTAX           INTEGER (0..24576)
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "This object defines the VID that will be added to mirrored frames
              when the mirroring encapsulation mode is vlan-tag"
     DEFVAL { 1 }
     ::= { wwpLeosEtherPortEntry 58 }
  
  wwpLeosEtherPortMirrorEncapTpid OBJECT-TYPE
     SYNTAX           INTEGER {
                           tpid8100(1),
                           tpid9100(2),
                           tpid88A8(3)
                      }
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "This object defines the tpid used in the tag that is added to
              mirrored frames, when the mirroring encapsulation mode is vlan-tag"
     DEFVAL { tpid8100 }
     ::= { wwpLeosEtherPortEntry 59 }

  wwpLeosEtherPortIfgDecrease  OBJECT-TYPE
     SYNTAX       Integer32(0..5)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "This object defines the number of bytes that will be subtracted   
              from the minimum standard IFG of 12 bytes as defined in IEEE 802.3.
              SAOS 6.x only supports a value of 0 or 4."
     DEFVAL { 0 }
     ::= { wwpLeosEtherPortEntry 60 }

  wwpLeosEtherPortAdvertSpeed OBJECT-TYPE
     SYNTAX        INTEGER {
                        not-applicable(1),
                        ten(2),
                        hundred(3),
                        gigabit(4),
                        ten-hundred-gigabit(5)                 
                   }
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION
             "This object defines the speed capabilities that will be advertised during the auto-negotiation process."
     DEFVAL { ten-hundred-gigabit }
     ::= { wwpLeosEtherPortEntry 61 }  

   wwpLeosEtherPortAdvertDuplex OBJECT-TYPE
     SYNTAX        INTEGER {
                        not-applicable(1),
                        half(2),
                        full(3),
                        half-full(4)
                   }
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION
             "This object defines the duplex capabilities that will be advertised during the auto-negotiation process."
     DEFVAL { half-full }
     ::= { wwpLeosEtherPortEntry 62 }  
 

 -- 
 -- Port Flush Table
 --
 wwpLeosEtherPortFlushTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosEtherPortFlushEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of port flush entries."
     ::= { wwpLeosEtherPort 2 }
                
 wwpLeosEtherPortFlushEntry OBJECT-TYPE
     SYNTAX       WwpLeosEtherPortFlushEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Broadcast containment port entry in the Ethernet Port Table."
     INDEX { wwpLeosEtherPortId }
     ::= { wwpLeosEtherPortFlushTable 1 } 

 WwpLeosEtherPortFlushEntry ::= SEQUENCE { 
     wwpLeosEtherPortFlushActivate       TruthValue
 }
 
 wwpLeosEtherPortFlushActivate OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
             "Setting this object to 'true' will cause 
             the Macs to be flushed for the port 
             specified by wwpLeosEtherPortId."
     DEFVAL { false }
     ::= { wwpLeosEtherPortFlushEntry 1 }           
 
 --
 -- Port Traps enable/disable
 --
 wwpLeosEtherPortTrapsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosEtherPortTrapsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of Ethernet Ports Traps."
     ::= { wwpLeosEtherPort 3 }
                
 wwpLeosEtherPortTrapsEntry OBJECT-TYPE
     SYNTAX       WwpLeosEtherPortTrapsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Port Traps Entry in the Ethernet Port Trap Table."
     INDEX { wwpLeosEtherPortId }
     ::= { wwpLeosEtherPortTrapsTable 1 } 

 WwpLeosEtherPortTrapsEntry ::= SEQUENCE { 
     wwpLeosEtherPortTrapsState     INTEGER     
  } 

 wwpLeosEtherPortTrapsState   OBJECT-TYPE
     SYNTAX         INTEGER {
                        disable(1),
                        enable(2)
                    }
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
             "Setting this object will enable or disable all traps on given port."
     ::= { wwpLeosEtherPortTrapsEntry 1 }
 
 --
 -- Port State Mirror Group Table
 --                        
 wwpLeosEtherPortStateMirrorGroupTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosEtherPortStateMirrorGroupEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "This table can be used to keep track of all the port state mirror
              groups.
              
              To create entry in this table along with indexes following mib 
              objects must be set using multiple set operation
              wwpLeosEtherPortStateMirrorGroupName must be valid string.
              wwpLeosEtherPortStateMirrorGroupStatus must be set."
     ::= { wwpLeosEtherPort 4 }
                
 wwpLeosEtherPortStateMirrorGroupEntry OBJECT-TYPE
     SYNTAX       WwpLeosEtherPortStateMirrorGroupEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Each entry in this table will define the port state mirror group."
     INDEX { wwpLeosEtherPortStateMirrorGroupId }
     ::= { wwpLeosEtherPortStateMirrorGroupTable 1 } 

 WwpLeosEtherPortStateMirrorGroupEntry ::= SEQUENCE {
     wwpLeosEtherPortStateMirrorGroupId            INTEGER, 
     wwpLeosEtherPortStateMirrorGroupName          DisplayString, 
     wwpLeosEtherPortStateMirrorGroupOperStatus    INTEGER, 
     wwpLeosEtherPortStateMirrorGroupNumSrcPorts   Counter32, 
     wwpLeosEtherPortStateMirrorGroupNumDstPorts   Counter32, 
     wwpLeosEtherPortStateMirrorGroupOperStatus    INTEGER, 
     wwpLeosEtherPortStateMirrorGroupStatus        RowStatus,
     wwpLeosEtherPortStateMirrorGroupType    INTEGER
  } 
 
 wwpLeosEtherPortStateMirrorGroupId   OBJECT-TYPE
     SYNTAX         INTEGER (1..65535)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used as index in the table and is used
              to identify the unique group id."
     ::= { wwpLeosEtherPortStateMirrorGroupEntry 1 }                                                     
                                                     
 wwpLeosEtherPortStateMirrorGroupName   OBJECT-TYPE
     SYNTAX         DisplayString (SIZE(1..15))
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "This mib object is used to specify the name of the group."
     ::= { wwpLeosEtherPortStateMirrorGroupEntry 2 }
  
  wwpLeosEtherPortStateMirrorGroupOperStatus   OBJECT-TYPE
     SYNTAX         INTEGER {
                               disabled(1),
                               enabled(2)
                            }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used to specify the operational status of the group."
     ::= { wwpLeosEtherPortStateMirrorGroupEntry 3 }
  
  wwpLeosEtherPortStateMirrorGroupNumSrcPorts   OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used to specify the total number of source ports 
              that exists in the group."
     ::= { wwpLeosEtherPortStateMirrorGroupEntry 4 }
 
 wwpLeosEtherPortStateMirrorGroupNumDstPorts   OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used to specify the total number of destination ports 
              that exists in the group."
     ::= { wwpLeosEtherPortStateMirrorGroupEntry 5 }
                                                            
 wwpLeosEtherPortStateMirrorGroupStatus   OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "Used to manage the creation and deletion of the 
             conceptual rows in this table."
     ::= { wwpLeosEtherPortStateMirrorGroupEntry 6 }

 wwpLeosEtherPortStateMirrorGroupType      OBJECT-TYPE
     SYNTAX         INTEGER {
                               unidirectional(1),
                               bidirectional(2)
                            }
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
             "This mib object is used to specify the directional mode type for the 
              port state mirror group. A uni-directional(1) mirror group type will only
              mirror the port state of the source port(s) to the destination port(s).
              The bi-directional(2) mirror group type will mirror state of either the
              source port(s) to the destination port(s) or the state of the destination
              port(s) will be mirrored to the source port(s). Where there are more than
              one source or destination ports the combined state of the source or destination
              group will be the combined 'OR'ed status of all the ports in either the source
              or destination groups. In other words, if one or more source ports is 'UP'
              then the source group is 'UP' and the mirrored destination state may be 'UP'.
              The default for this object type is uni-directional."
     ::= { wwpLeosEtherPortStateMirrorGroupEntry 7 }


 --
 -- Port State Mirror Group Membership Table
 --                        
 wwpLeosEtherPortStateMirrorGroupMemTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosEtherPortStateMirrorGroupMemEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "This table is used to keep track of port group membership."
     ::= { wwpLeosEtherPort 5 }
                
 wwpLeosEtherPortStateMirrorGroupMemEntry OBJECT-TYPE
     SYNTAX       WwpLeosEtherPortStateMirrorGroupMemEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Each entry in this table is used to represent the membership of port 
              to a given group and group type."
     INDEX { wwpLeosEtherPortStateMirrorGroupId, wwpLeosEtherPortId }
     ::= { wwpLeosEtherPortStateMirrorGroupMemTable 1 } 

 WwpLeosEtherPortStateMirrorGroupMemEntry ::= SEQUENCE {
     wwpLeosEtherPortStateMirrorGroupMemType    INTEGER, 
     wwpLeosEtherPortStateMirrorGroupMemOperState  INTEGER, 
     wwpLeosEtherPortStateMirrorGroupMemStatus     RowStatus     
  }                           
  
 wwpLeosEtherPortStateMirrorGroupMemType OBJECT-TYPE
     SYNTAX       INTEGER {
               srcPort(1),
               dstPort(2)
               }
     MAX-ACCESS   read-create
     STATUS       current
     DESCRIPTION
             "Setting this object will specify the type of group this port is member of for a given port state mirror 
              group. This object can only be set while creating the entry. This object cannot be modified once entry 
              is created." 
     DEFVAL { srcPort }
     ::= { wwpLeosEtherPortStateMirrorGroupMemEntry 1 }
 
 wwpLeosEtherPortStateMirrorGroupMemOperState   OBJECT-TYPE
     SYNTAX         INTEGER {
                  disabled(1),
                  enabled(2)
               }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used to specify the operational status of the port."
     ::= { wwpLeosEtherPortStateMirrorGroupMemEntry 2 }
     
 wwpLeosEtherPortStateMirrorGroupMemStatus   OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "Used to manage the creation and deletion of the 
             conceptual rows in this table."
     ::= { wwpLeosEtherPortStateMirrorGroupMemEntry 3 }
     
 --
 -- Traps Defination
 -- 
 wwpLeosEtherStndLinkUpDownTrapsEnable OBJECT-TYPE
     SYNTAX       TruthValue       
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "Setting this object to 'false(2)' will cause
              standard Link Up Down Traps to be suppressed." 
     DEFVAL { true }
     ::= { wwpLeosEtherPortNotif 1 }
     
 wwpLeosEtherPortLinkUpDownTrapsEnable OBJECT-TYPE
     SYNTAX       TruthValue       
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "Setting this object to 'true(1)' will cause
              wwp specific port up down trap to be generated." 
     DEFVAL { false }
     ::= { wwpLeosEtherPortNotif 2 }

 wwpLeosEtherAggPortLinkUpDownTrapsEnable OBJECT-TYPE
     SYNTAX		TruthValue
     MAX-ACCESS		read-write
     STATUS		current
     DESCRIPTION	"Setting this object to 'true(1)' will cause wwp
			specific agg port up down trap to be generated
     			for a link state change on a physical port that
     			is a member of a agg."
     DEFVAL { false }
     ::= { wwpLeosEtherPortNotif 3 }
     
 wwpLeosEthLinkUp  NOTIFICATION-TYPE
        OBJECTS    {  sysName,
                      sysLocation, 
                      wwpLeosEtherPortId,
                      wwpLeosEtherPortName,  
                      wwpLeosEtherPortType,
                      wwpLeosEtherPortAdminStatus,
                      wwpLeosEtherPortOperStatus,
                      wwpLeosEtherPortDesc   
                   }
        STATUS     current
        DESCRIPTION  
                "A wwpLeosEthLinkUp trap signifies that the SNMP entity, acting in
                 an agent role, has detected that the ifOperStatus object for
                 one of its communication links has entered the up state."
        ::= { wwpLeosPortMIBNotifications 3 } 
        
 wwpLeosEthLinkDown  NOTIFICATION-TYPE
        OBJECTS    { sysName,
                     sysLocation,
                     wwpLeosEtherPortId,
                     wwpLeosEtherPortType,
                     wwpLeosEtherPortName,
                     wwpLeosEtherPortAdminStatus,
                     wwpLeosEtherPortOperStatus,
                     wwpLeosEtherPortDesc   
                   }
        STATUS     current
        DESCRIPTION  
                "A wwpLeosEthLinkDown trap signifies that the SNMP entity, acting in
                 an agent role, has detected that the ifOperStatus object for
                 one of its communication links has entered the down state."
        ::= { wwpLeosPortMIBNotifications 4 } 

 wwpLeosEthAdminSpeedIncompatible  NOTIFICATION-TYPE
        OBJECTS    { wwpLeosEtherPortId
                   }
        STATUS     current
        DESCRIPTION  
                "A wwpLeosEthAdminSpeedIncompatible trap is generated when the port
                 administrative speed doesn't match the speed of the SFP transceiver
                 installed."
        ::= { wwpLeosPortMIBNotifications 5 } 

 wwpLeosEthLinkFlap  NOTIFICATION-TYPE
        OBJECTS    { sysName,
                     sysLocation,
                     wwpLeosEtherPortId,
                     wwpLeosEtherPortType,
                     wwpLeosEtherPortName,
                     wwpLeosEtherPortOperStatus,
                     wwpLeosEtherPortDesc,
                     wwpLeosEtherPortLinkFlapHoldTime   
                   }
        STATUS     current
        DESCRIPTION  
                "A wwpLeosEthLinkFlap trap signifies that the SNMP entity,
                 acting in an agent role, has detected that the ifOperStatus
                 object for one of its communication links has been changed
                 due to link flap detection."
        ::= { wwpLeosPortMIBNotifications 6 } 

 wwpLeosAggLinkUpDown  NOTIFICATION-TYPE
        OBJECTS    {  sysName,
                      sysLocation, 
                      wwpLeosEtherPortId,
                      wwpLeosEtherPortName,  
                      wwpLeosEtherPortDesc,  
                      wwpLeosEtherPortType,
                      wwpLeosEtherPortAdminStatus,
                      wwpLeosEtherPortOperStatus,
                      dot3adAggPortActorAdminKey,
		      dot3adAggPortListPorts,
                      wwpLeosEtherPortName,
                      wwpLeosEtherPortDesc
                   }
        STATUS     current
        DESCRIPTION  
                "A wwpLeosAggLinkUpDown trap signifies that the SNMP entity,
                 acting in an agent role, has detected that the ifOperStatus
                 object for one of its communication links has changed state."
        ::= { wwpLeosPortMIBNotifications 7 } 
          
 END
 