-- JUNIPER-MOBILITY-CHARGING-MIB 
-- Copyright (c) 2011-2013, Juniper Networks, Inc.
-- All rights reserved.
--
-- This file contains the SGW (MIURA) charging mib information. 
--The contents of this document are subject to change without notice.
--

JUNIPER-MOBILITY-SGW-CHARGING-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
     Counter32,  Counter64, Gauge32, Integer32,Unsigned32, IpAddress
        FROM SNMPv2-SMI
    TruthValue
        FROM SNMPv2-TC
    TEXTUAL-CONVENTION, DisplayString, RowStatus, TruthValue
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    jnxMbgGwIndex, jnxMbgGwName
        FROM JUNIPER-MOBILE-GATEWAYS
    jnxMobileGatewaySgw
        FROM JUNIPER-MBG-SMI;


jnxMbgSgwChargingMib MODULE-IDENTITY
    LAST-UPDATED        "201106271430Z" -- Tue Jun 27 14:30:00 2011 UTC
    ORGANIZATION        "Juniper Networks, Inc."
    CONTACT-INFO
                        "Juniper Technical Assistance Center
                        Juniper Networks, Inc.
                        1133 Innovation Way
                        Sunnyvale, CA 94089
                        E-mail: support@juniper.net"

    DESCRIPTION
         "This is Juniper Networks implementation of Mobility Charging MIB for 
    SGW (Serving Gateway ) in 3GPP LTE network."

    REVISION "201110101430Z"    -- 10 Oct, 2011
    DESCRIPTION
                "CGF group and CGF tables index keys has changed to 
                gateway id and profile id. Gateway id and gateway name has 
                added to all the traps."
    
    REVISION "201203161430Z"    -- 16 March, 2012
    DESCRIPTION
                "SGW Charging global statistics table has added."
    ::= { jnxMobileGatewaySgw 3 }

jnxMbgSgwCgNotifications      OBJECT IDENTIFIER ::= { jnxMbgSgwChargingMib 0 }
jnxMbgSgwChargingObjects      OBJECT IDENTIFIER ::= { jnxMbgSgwChargingMib 1 }

jnxMbgSgwCgLpsStatsTable OBJECT-TYPE
   SYNTAX        SEQUENCE OF  JnxMbgSgwCgLpsStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
       "A table listing the stats for all Local persistent storage stats 
        configured on the SGW."
   ::= { jnxMbgSgwChargingObjects 1 }

jnxMbgSgwCgCgfGroupsStatsTable OBJECT-TYPE
   SYNTAX        SEQUENCE OF JnxMbgSgwCgCgfGrpStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
       "A table listing the stats for all (Charging Gateway Function) CGF 
        Groups configured on the SGW."
   ::= { jnxMbgSgwChargingObjects 2 }

jnxMbgSgwCgNotificationVars   OBJECT IDENTIFIER ::= { 
                                             jnxMbgSgwChargingObjects 3 }

jnxMbgSgwCgCgfStatsTable OBJECT-TYPE
   SYNTAX        SEQUENCE OF JnxMbgSgwCgCgfStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
         "A table listing the statistics for all CGF configured on the SGW."
   ::= { jnxMbgSgwChargingObjects 4 }

jnxMbgSgwCgGlobalStatsTable OBJECT-TYPE
   SYNTAX        SEQUENCE OF JnxMbgSgwCgGlobalStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
         "A table listing the charging global statistics of the SGW."
   ::= { jnxMbgSgwChargingObjects 5 }
--
-- CG LPS Stats
--
jnxMbgSgwCgLpsStatsEntry OBJECT-TYPE
   SYNTAX        JnxMbgSgwCgLpsStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
         "A conceptual row listing the statistics for each
          LPS configured on the SGW."
   INDEX         {jnxMbgGwIndex }
   ::= { jnxMbgSgwCgLpsStatsTable 1 }

JnxMbgSgwCgLpsStatsEntry ::= SEQUENCE {
   jnxMbgSgwCgFilesOnLcStorage        Gauge32,
   jnxMbgSgwCgLcStorageAvailSpace     Gauge32
}

jnxMbgSgwCgFilesOnLcStorage OBJECT-TYPE
   SYNTAX        Gauge32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
         "The number of Files containing Charging Data Records (CDRs) present 
          on the Local Storage Device.Incremented when a file containing CDRs 
          is closed on the Local storage device Decremented when sftp is done 
          and a file is removed from the Local storage device"
   ::= { jnxMbgSgwCgLpsStatsEntry 1 }

jnxMbgSgwCgLcStorageAvailSpace OBJECT-TYPE
   SYNTAX        Gauge32 
   UNITS         "MBytes"
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
         "The space available on the Local Storage Device in MB."
   ::= { jnxMbgSgwCgLpsStatsEntry 2 }

--
-- CGF Group Stats
--
jnxMbgSgwCgCgfGroupStatsEntry OBJECT-TYPE
   SYNTAX        JnxMbgSgwCgCgfGrpStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
         "A conceptual row listing the statistics for each
          CGF Server configured on the SGW."
   INDEX         { jnxMbgGwIndex, jnxMbgSgwCgCgfGrpProfId }
   ::= { jnxMbgSgwCgCgfGroupsStatsTable 1 }

JnxMbgSgwCgCgfGrpStatsEntry ::= SEQUENCE {
   jnxMbgSgwCgCgfGrpProfId            Unsigned32,
   jnxMbgSgwCgCgfGrpDRTReqTx          Counter32,
   jnxMbgSgwCgCgfGrpDRTReqRx          Counter32,
   jnxMbgSgwCgCgfGrpDRTReqTmout       Counter32,
   jnxMbgSgwCgCgfGrpDRTSucRspRx       Counter32,
   jnxMbgSgwCgCgfGrpDRTErrRspRx       Counter32,
   jnxMbgSgwCgCgfGrpRediReqRx         Counter32,
   jnxMbgSgwCgCgfGrpRediRspTx         Counter32,
   jnxMbgSgwCgCgfGrpSwitchovers       Counter32,
   jnxMbgSgwCgCgfGrpBatchReqTx        Counter32,
   jnxMbgSgwCgCgfGrpBatchRspErrors    Counter32,
   jnxMbgSgwCgCgfGrpBatchCDRsTx       Counter32,
   jnxMbgSgwCgCgfGroupTotalWFA        Counter32,
   jnxMbgSgwCgCgfGroupProfName        DisplayString
}

jnxMbgSgwCgCgfGrpProfId OBJECT-TYPE
   SYNTAX        Unsigned32
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
        "This will identify the CGF Group profile id uniquely and used as 
         secondary key for CGF group table"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 1 }

jnxMbgSgwCgCgfGrpDRTReqTx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
        "Total number of the DRT (Detailed Record Time) request transmitted 
         for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 2 }

jnxMbgSgwCgCgfGrpDRTReqRx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION
        "Total number of the DRT request received for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 3 }

jnxMbgSgwCgCgfGrpDRTReqTmout OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
        "Total number of the DRT request timeouts happend for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 4 }

jnxMbgSgwCgCgfGrpDRTSucRspRx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   
        " Total number of the DRT success responses received"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 5 }

jnxMbgSgwCgCgfGrpDRTErrRspRx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
        "Total number of the DRT error responses received for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 6 }

jnxMbgSgwCgCgfGrpRediReqRx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   
        "Total number of the redirection responses received for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 7 }

jnxMbgSgwCgCgfGrpRediRspTx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
        "Total number of the redirection reqests transmitted for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 8 }

jnxMbgSgwCgCgfGrpSwitchovers OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
        " Total number of the switch overs on the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 9 }

jnxMbgSgwCgCgfGrpBatchReqTx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
        " Total number of the batch req transmitted for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 10 }

jnxMbgSgwCgCgfGrpBatchRspErrors OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
        " Tatal number of the batch response errors for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 11 }

jnxMbgSgwCgCgfGrpBatchCDRsTx OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   
        " Total number of the batch CDRs transmitted for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 12 }

jnxMbgSgwCgCgfGroupTotalWFA OBJECT-TYPE
   SYNTAX        Counter32
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   
        " Total WFA available for the CGF group"
   ::= { jnxMbgSgwCgCgfGroupStatsEntry 13 }

jnxMbgSgwCgCgfGroupProfName OBJECT-TYPE
    SYNTAX      DisplayString   
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string that uniquely identifies the TSP Profile."
    ::= { jnxMbgSgwCgCgfGroupStatsEntry 14 }
--
-- CGF Stats
--

jnxMbgSgwCgCgfStatsEntry OBJECT-TYPE
   SYNTAX        JnxMbgSgwCgCgfStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
         "A conceptual row listing the statistics for each
          CGF Server configured on the SGW."
   INDEX         {jnxMbgGwIndex, jnxMbgSgwCgCgfIndex }
   ::= { jnxMbgSgwCgCgfStatsTable 1 }

JnxMbgSgwCgCgfStatsEntry ::= SEQUENCE {
   jnxMbgSgwCgCgfIndex             Unsigned32,
   jnxMbgSgwCgCgfIpAddress         IpAddress,
   jnxMbgSgwCgCgfStatus            INTEGER,
   jnxMbgSgwCgCgfUpDuration        Counter64,
   jnxMbgSgwCgCgfDownDuration      Counter64,
   jnxMbgSgwCgCgfEchoReqTx         Counter64, 
   jnxMbgSgwCgCgfEchoReqRx         Counter64,
   jnxMbgSgwCgCgfEchoReqTmout      Counter64, 
   jnxMbgSgwCgCgfEchoRespTx        Counter64,
   jnxMbgSgwCgCgfEchoRespRx        Counter64,
   jnxMbgSgwCgCgfVerUnsuppTx       Counter64,
   jnxMbgSgwCgCgfVerUnsuppRx       Counter64,
   jnxMbgSgwCgCgfNodeAliveReqTx    Counter64,
   jnxMbgSgwCgCgfNodeAliveReqRx    Counter64,
   jnxMbgSgwCgCgfNodeAliveReqTmout Counter64,
   jnxMbgSgwCgCgfNodeAliveRespTx   Counter64,
   jnxMbgSgwCgCgfNodeAliveRespRx   Counter64,
   jnxMbgSgwCgCgfRedirectReqRx     Counter64,
   jnxMbgSgwCgCgfRedirectRespTx    Counter64, 
   jnxMbgSgwCgCgfDRTReqTx          Counter64,
   jnxMbgSgwCgCgfDRTReqTmout       Counter64,
   jnxMbgSgwCgCgfDRTSuccRespRx     Counter64,
   jnxMbgSgwCgCgfDRTErrRespRx      Counter64,
   jnxMbgSgwCgCgfCdrTx             Counter64,
   jnxMbgSgwCgCgfDRTRTTMean        Counter64,
   jnxMbgSgwCgCgfDRTRTTMin         Counter64,
   jnxMbgSgwCgCgfDRTRTTMax         Counter64,
   jnxMbgSgwCgCgfTransToDownState  Counter64,
   jnxMbgSgwCgCgfContainers        Counter64,
   jnxMbgSgwCgCgfProfileName       DisplayString
}

jnxMbgSgwCgCgfIndex OBJECT-TYPE
   SYNTAX        Unsigned32
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
         "A number representing each CGF Server whose statistics
          is being generated."
    ::= { jnxMbgSgwCgCgfStatsEntry 1 }

jnxMbgSgwCgCgfIpAddress OBJECT-TYPE
   SYNTAX        IpAddress
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "CGF Server IP-address."
   ::= { jnxMbgSgwCgCgfStatsEntry 2 }

jnxMbgSgwCgCgfStatus OBJECT-TYPE
   SYNTAX        INTEGER {
        up(1),     -- server is up
        down(2)     -- server is not reachable or unconfigured
   }
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION 
         "This indicates the state of the CGF Server i.e UP or DOWN."
   ::= { jnxMbgSgwCgCgfStatsEntry 3 }

jnxMbgSgwCgCgfUpDuration OBJECT-TYPE
   SYNTAX        Counter64
   UNITS         "minutes"
   MAX-ACCESS    not-accessible
   STATUS         obsolete
   DESCRIPTION   "Total duration in minutes for which the CGF Server
                  was in UP State."
   ::= { jnxMbgSgwCgCgfStatsEntry 4 }

jnxMbgSgwCgCgfDownDuration OBJECT-TYPE
   SYNTAX        Counter64
   UNITS         "minutes"
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total duration in minutes for which the CGF Server 
                  was in DOWN State."
   ::= { jnxMbgSgwCgCgfStatsEntry 5 }

jnxMbgSgwCgCgfEchoReqTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Echo Requests transmitted to the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 6 }

jnxMbgSgwCgCgfEchoReqRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Echo Requests received from the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 7 }

jnxMbgSgwCgCgfEchoReqTmout OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Echo Requests to the CGF Server that 
                  timed out."
   ::= { jnxMbgSgwCgCgfStatsEntry 8 }

jnxMbgSgwCgCgfEchoRespTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Echo Responses transmitted to the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 9 }

jnxMbgSgwCgCgfEchoRespRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Echo Responses received from the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 10 }

jnxMbgSgwCgCgfVerUnsuppTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Version Unsupported messages transmitted to 
                 the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 11 }

jnxMbgSgwCgCgfVerUnsuppRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Version Unsupported messages received 
                 from the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 12 }

jnxMbgSgwCgCgfNodeAliveReqTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total number of Node Alive Requests transmitted to the
                  CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 13 }

jnxMbgSgwCgCgfNodeAliveReqRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Node Alive Requests received from 
                  the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 14 }

jnxMbgSgwCgCgfNodeAliveReqTmout OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total number of Node Alive Requests to the CGF Server 
                  that timed out."
   ::= { jnxMbgSgwCgCgfStatsEntry 15 }

jnxMbgSgwCgCgfNodeAliveRespTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Node Alive Responses transmitted 
                  to the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 16 }

jnxMbgSgwCgCgfNodeAliveRespRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total number of Node Alive Responses received from 
                  the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 17 }

jnxMbgSgwCgCgfRedirectReqRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Redirect Requests received from 
                  the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 18 }

jnxMbgSgwCgCgfRedirectRespTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Redirect Responses transmitted 
                  to the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 19 }

jnxMbgSgwCgCgfDRTReqTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Data Record Transfer Requests transmitted to 
                  the CGF Server.This includes the retransmission counts also."
   ::= { jnxMbgSgwCgCgfStatsEntry 20 }

jnxMbgSgwCgCgfDRTReqTmout OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total number of Data Record Transfer Requests to the CGF  
                 Server that timed out after the configured number of retries."
   ::= { jnxMbgSgwCgCgfStatsEntry 21 }

jnxMbgSgwCgCgfDRTSuccRespRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Data Record Transfer Responses indicating 
                  success received from the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 22 }

jnxMbgSgwCgCgfDRTErrRespRx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of Data Record Transfer Responses indicating 
                  error received from the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 23 }


jnxMbgSgwCgCgfCdrTx OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total number of Call Data Records (CDRs) transmitted 
                  to the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 24 }

jnxMbgSgwCgCgfDRTRTTMean OBJECT-TYPE
   SYNTAX        Counter64
   UNITS         "seconds"
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION
        "Mean Round Trip Time of the Data Record Transfer Request and Response 
         to and from the CGF Server in seconds. This is calculated from the 
         average of the minimum and maximum round trip times of the Data Record 
         Transfer Request. This is applicable for CGF Servers which are 
         connected via UDP protocol."
   ::= { jnxMbgSgwCgCgfStatsEntry 25 }

jnxMbgSgwCgCgfDRTRTTMin OBJECT-TYPE
   SYNTAX        Counter64
   UNITS         "seconds"
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION
        "Minimum Round Trip Time of the Data Record Transfer Request and 
        Response to and from the CGF Server in seconds. This is 
        applicable for CGF Servers which are connected via UDP protocol."
   ::= { jnxMbgSgwCgCgfStatsEntry 26 }

jnxMbgSgwCgCgfDRTRTTMax OBJECT-TYPE
   SYNTAX        Counter64
   UNITS         "seconds"
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION
        "Maximum Round Trip Time of the Data Record Transfer Request and 
         Response to and from the CGF Server in seconds.This is 
         applicable for CGF Servers which are connected via UDP protocol."
   ::= { jnxMbgSgwCgCgfStatsEntry 27 }

jnxMbgSgwCgCgfTransToDownState OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total number of transitions of the CGF Server to 
                  the DOWN state."
   ::= { jnxMbgSgwCgCgfStatsEntry 28 }

jnxMbgSgwCgCgfContainers OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    not-accessible
   STATUS        obsolete
   DESCRIPTION   "Total number of closed containers to the CGF Server."
   ::= { jnxMbgSgwCgCgfStatsEntry 29 }
jnxMbgSgwCgCgfProfileName OBJECT-TYPE
    SYNTAX      DisplayString  
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string that uniquely identifies the CGF Peer Profile."
    ::= { jnxMbgSgwCgCgfStatsEntry 30 }

 jnxMbgSgwCgGlobalStatsEntry OBJECT-TYPE
   SYNTAX       JnxMbgSgwCgGlobalStatsEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION 
         "A conceptual row listing the statistics for each SGW charging
          global statistics."
   INDEX         { jnxMbgGwIndex }
   ::= { jnxMbgSgwCgGlobalStatsTable 1 }

JnxMbgSgwCgGlobalStatsEntry ::= SEQUENCE {
   jnxMbgSgwCgCdrSendErrors           Counter64,
   jnxMbgSgwCgCdrEncodeErrors         Counter64,
   jnxMbgSgwCgCdrAllocFailures        Counter64,
   jnxMbgSgwCgContFailures            Counter64,
   jnxMbgSgwCgCmBearersCreated        Counter64,
   jnxMbgSgwCgCmBearersDeleted        Counter64
}

-- Charging Global Stats
jnxMbgSgwCgCdrSendErrors OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of CDR send errors to charging module."
   ::= { jnxMbgSgwCgGlobalStatsEntry 1 }

jnxMbgSgwCgCdrEncodeErrors OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of CDR (charging data record) encoding errors."
   ::= { jnxMbgSgwCgGlobalStatsEntry 2 }

jnxMbgSgwCgCdrAllocFailures OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of CDR memory allocation failures."
   ::= { jnxMbgSgwCgGlobalStatsEntry 3 }

jnxMbgSgwCgContFailures OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of container failures."
   ::= { jnxMbgSgwCgGlobalStatsEntry 4 }

jnxMbgSgwCgCmBearersCreated OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number bearers created."
   ::= { jnxMbgSgwCgGlobalStatsEntry 5 }

jnxMbgSgwCgCmBearersDeleted OBJECT-TYPE
   SYNTAX        Counter64
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION   "Total number of bearers destroyed."
   ::= { jnxMbgSgwCgGlobalStatsEntry 6 }

jnxMbgSgwCgServerName OBJECT-TYPE
    SYNTAX      DisplayString  (SIZE (0..31))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
    "A string that uniquely identifies the CGF server name." 
   ::= { jnxMbgSgwCgNotificationVars 1 }

jnxMbgSgwCgServicePicName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..31))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
    "This identifies the session-pic, in the form ms-a/b/0, 
     where <a> is the slot and <b> could be either 0 or 1."
   ::= { jnxMbgSgwCgNotificationVars 2 }
jnxMbgSgwCgCDRDest OBJECT-TYPE
    SYNTAX        INTEGER {
                      cdrcgf       (1),    
                      cdrbackup    (2),    
                      cdrnobackup  (3) }
    MAX-ACCESS    accessible-for-notify
    STATUS        current
    DESCRIPTION 
"This indicates any transisitions in the state of the CGF.
Value 1 indicates one of the CGF for the Group came up. Redirecting CDRs to the Active CGF.
Value 2 indicates last active CGF for the Group went down. CDRs being written to backup Local storage device.
Value 3 indicates last active CGF for the Group went down. Backup Local storage device not configured."
   ::= { jnxMbgSgwCgNotificationVars 3 }

jnxMbgSgwCgTSPName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..31)) 
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that uniquely identifies the Transport Profile."
    ::= { jnxMbgSgwCgNotificationVars 4 }

jnxMbgSgwCgMemLimit OBJECT-TYPE
    SYNTAX        INTEGER {
                      memfulldisconnectnew          (1),
                      memfulldisconnectnewrslvd     (2),
                      memfulldisconnectexistnew     (3),
                      memfulldisconnectexistnewrslvd(4)
    }
    MAX-ACCESS    accessible-for-notify
    STATUS        current
    DESCRIPTION 
"This indicates any transisitions in the state of the CGF.
Value 1 indicates System has reached Level 1 critical memory threshold. 
Action - Check the CGF server connections. If local storage is enabled,
         please ftp the charging records immediately.
         If local storage is not enabled, please enable it so the
         charging records can be stored in local persistent storage. 
Risk -  No new sessions will be allowed.
Value 2 indicates System reaching Level 1 critical memory threshold
        condition has been resolved.
Value 3 indicates System has reached Level 2 critical memory threshold.
Action - Check the CGF server connections. If local storage is enabled,
         please ftp the charging records immediately.
         If local storage is not enabled, please enable it so the
         charging records can be stored in local persistent storage.
Risk -  New and existing sessions will be not be allowed.
Value 4 indicates System reaching Level 2 critical memory threshold
        condition has been resolved."
    ::= { jnxMbgSgwCgNotificationVars 5 }

jnxMbgSgwCgLcsSpace OBJECT-TYPE
    SYNTAX        INTEGER {
                      localstoragememlevel1     (1),
                      localstoragememlevel2     (2),
                      localstoragememlevel3     (3)
    }
    MAX-ACCESS    accessible-for-notify
    STATUS        current 
    DESCRIPTION
    "Water marking for the local storage levels in charged of RE."
   ::= { jnxMbgSgwCgNotificationVars 6 }

jnxMbgSgwCgLcsUtil OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "percent"
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The percentage of the total of Local Storage
         Space by one the Charged on RE"
        ::= { jnxMbgSgwCgNotificationVars 7 }

jnxMbgSgwCgAlarmStatus OBJECT-TYPE
    SYNTAX        INTEGER {
                      raised	    (1),
                      cleared	    (2)
    }
    MAX-ACCESS    accessible-for-notify
    STATUS        current 
    DESCRIPTION
    "Value 1 indicates that the Alarm for a particular condition is present.
    Value 2 indicates that the Alarm for a particular condition is absent."
   ::= { jnxMbgSgwCgNotificationVars 8 }

jnxMbgSgwCgProfileName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that identifies a charging profile ."
    ::= { jnxMbgSgwCgNotificationVars 9 }

jnxMbgSgwCgPrevMMState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that indicates the maintenance-mode state ."
    ::= { jnxMbgSgwCgNotificationVars 10 }

jnxMbgSgwCgNewMMState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that indicates the maintenance-mode state ."
    ::= { jnxMbgSgwCgNotificationVars 11 }

jnxMbgSgwCgTProfileName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that identifies a charging profile ."
    ::= { jnxMbgSgwCgNotificationVars 12 }

jnxMbgSgwCgTPrevMMState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that indicates the maintenance-mode state ."
    ::= { jnxMbgSgwCgNotificationVars 13 }

jnxMbgSgwCgTNewMMState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that indicates the maintenance-mode state ."
    ::= { jnxMbgSgwCgNotificationVars 14 }

jnxMbgSgwCgSGwName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "A string that indicates the gateway name"
    ::= { jnxMbgSgwCgNotificationVars 15 }

jnxMbgSgwCgCgfProfName OBJECT-TYPE
  SYNTAX      DisplayString 
  MAX-ACCESS   accessible-for-notify
  STATUS      current
  DESCRIPTION
    "A string that uniquely identifies the CGF Profile."
  ::= { jnxMbgSgwCgNotificationVars 16 }

jnxMbgSgwCgGtpGWUpNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgServerName, 
                   jnxMbgSgwCgServicePicName }
     STATUS        current
     DESCRIPTION
        "This notification signifies that the specified server has been
        marked alive.  The ServerName identifies the server and the
        SPIdentfier identifies the session-pic which originated this
        notification."
    ::= { jnxMbgSgwCgNotifications 1 }

jnxMbgSgwCgGtpGWDownNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgServerName, 
                   jnxMbgSgwCgServicePicName }
    STATUS         current
    DESCRIPTION
        "This notification signifies that the specified server has been
        marked dead.  The ServerName identifies the server and the
        SPIdentfier identifies the session-pic which originated this
        notification."
    ::= { jnxMbgSgwCgNotifications 2 }

jnxMbgSgwCgCDRDestNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgCDRDest,
                   jnxMbgSgwCgTSPName,
                   jnxMbgSgwCgCgfIpAddress }
    STATUS         current
    DESCRIPTION
          "This signifies change in the destination of the CDRs 
           (Charging Data Record)"
::= { jnxMbgSgwCgNotifications 3 } 

jnxMbgSgwCgServiceUpNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgServicePicName } 
    STATUS         current
    DESCRIPTION
        "This signifies the Charging daemon is UP on the SP."
::= { jnxMbgSgwCgNotifications 4 } 

jnxMbgSgwCgMMStateChangeNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgProfileName,
                   jnxMbgSgwCgPrevMMState,
                   jnxMbgSgwCgNewMMState }
    STATUS         current
    DESCRIPTION
        "This indicates that the given charging profile underwent a change
         in the maintenance-mode."
    ::= { jnxMbgSgwCgNotifications 5 }

jnxMbgSgwCgTMMStateChangeNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgTProfileName,
                   jnxMbgSgwCgTPrevMMState,
                   jnxMbgSgwCgTNewMMState }
    STATUS         current
    DESCRIPTION
        "This indicates that the given transport profile underwent a change
         in the maintenance-mode."
    ::= { jnxMbgSgwCgNotifications 6 }

jnxMbgSgwCgMemHighThresNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgTSPName,
                   jnxMbgSgwCgServicePicName,
                   jnxMbgSgwCgMemLimit,
                   jnxMbgSgwCgAlarmStatus }
    STATUS         current 
    DESCRIPTION
          "This trap indicates the alarm status on the node associated with the utilization of inernal memory space for charging records. This alarm is sent outwhen the utilization exceeds or falls below configured high threshold value. Thealarm status (Active/Clear)is indicated by the jnxMbgSgwCgAlarmStatus variable."
      ::= { jnxMbgSgwCgNotifications 7 } 

jnxMbgSgwCgMemMediumThresNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgTSPName,
                   jnxMbgSgwCgServicePicName,
                   jnxMbgSgwCgMemLimit,
                   jnxMbgSgwCgAlarmStatus }
    STATUS         current
    DESCRIPTION
         "This trap indicates the alarm status on the node associated with the  utilization of inernal memory space for charging records. This alarm is sent outwhen the utilization exceeds or falls below configured medium threshold value. The alarm status (Active/Clear)is indicated by the jnxMbgSgwCgAlarmStatus variable."
      ::= { jnxMbgSgwCgNotifications 8 } 

jnxMbgSgwCgMemLowThresNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgTSPName,
                   jnxMbgSgwCgServicePicName,
                   jnxMbgSgwCgMemLimit,
                   jnxMbgSgwCgAlarmStatus }
    STATUS          current
    DESCRIPTION
          "This trap indicates the alarm status on the node associated with the utilization of inernal memory space for charging records. This alarm is sent outwhen the utilization exceeds or falls below configured low threshold value. The alarm status (Active/Clear)is indicated by the jnxMbgSgwCgAlarmStatus variable."
      ::= { jnxMbgSgwCgNotifications 9 }

jnxMbgSgwCgLcsThresHighNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgAlarmStatus,
                   jnxMbgSgwCgLcsUtil }
    STATUS         current
    DESCRIPTION
          "This trap indicates the alarm status on the node associated with the utilization of local storage space for charging records. This alarm is sent out when the utilization exceeds or falls below configured high threshold of available disk space. The alarm status (Active/Clear)is indicated by the jnxMbgSgwCgAlarmStatus variable."
    ::= { jnxMbgSgwCgNotifications 10 }

jnxMbgSgwCgLcsThresMediumNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgAlarmStatus,
                   jnxMbgSgwCgLcsUtil }
    STATUS         current
    DESCRIPTION
          "This trap indicates the alarm status on the node associated with the utilization of local storage space for charging records. This alarm is sent outwhen the utilization exceeds or falls below configured medium threshold of available disk space. The alarm status (Active/Clear)is indicated by the jnxMbgSgwCgAlarmStatus variable."
    ::= { jnxMbgSgwCgNotifications 11 }

jnxMbgSgwCgLcsThresLowNotify NOTIFICATION-TYPE
    OBJECTS      { jnxMbgGwName,
                   jnxMbgSgwCgAlarmStatus,  
                   jnxMbgSgwCgLcsUtil }
    STATUS         current
    DESCRIPTION
          "This trap indicates the alarm status on the node associated with the utilization of local storage space for charging records. This alarm is sent out when the utilization exceeds or falls below configured low threshold of available disk space. The alarm status (Active/Clear)is indicated by the jnxMbgSgwCgAlarmStatus variable."
    ::= { jnxMbgSgwCgNotifications 12 }

END

