    F10-Z-SERIES-CHASSIS-MIB DEFINITIONS ::= BEGIN
    --  This module provides authoritative definitions for Z-series
    --  Dell Networking OS Chassis MIB.
    --
    --  This module will be extended, as needed.
    --  

    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE, 
        Gauge32, Integer32, TimeTicks
            FROM SNMPv2-SMI
        DisplayString, MacAddress
            FROM SNMPv2-TC
        MODULE-COMPLIANCE, OBJECT-GROUP
            FROM SNMPv2-CONF
        f10Mgmt
            FROM FORCE10-SMI
        F10SwDate, F10ChassisType, F10ProcessorModuleType,
        F10MfgDate, F10HundredthdB, F10SSeriesPortType,
        F10CardOperStatus
            FROM FORCE10-TC;                
    
    f10ZSerChassisMib MODULE-IDENTITY
    LAST-UPDATED "201404161200Z"  -- Apr 16, 2014 12:00:00 GMT
    
    ORGANIZATION "Dell Inc."

    CONTACT-INFO "http://www.force10networks.com/support"

    DESCRIPTION
       "Dell Networking OS Z-Series Chassis MIB."

    REVISION     "201404161200Z"
    DESCRIPTION
          "Updated Contact info and Description."

    REVISION     "201310101200Z"
    DESCRIPTION
          "Initial version of this mib."
           ::= { f10Mgmt 25 }   


    -- ### Groups ###

    f10ZSerChassisObject OBJECT IDENTIFIER ::={ f10ZSerChassisMib 1 }
    chObjects            OBJECT IDENTIFIER ::={ f10ZSerChassisObject 1 }
    chSysObjects         OBJECT IDENTIFIER ::={ f10ZSerChassisObject 2 }

    -- ### Chassis Information

       chType    OBJECT-TYPE
         SYNTAX        F10ChassisType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The type of chassis."
         ::= { chObjects 1 }

       chSwVersion    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..16))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Current FTOS image version running in the system.
              The version string will be in following format
              major_ver.minor_ver(maintenance_ver.patch_ver)"
         ::= { chObjects 2 }

       chMacAddr    OBJECT-TYPE
         SYNTAX        MacAddress
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "A 6-octet MAC Address assigned to this Chassis."
         ::= { chObjects 3 }

       chSerialNumber    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..14))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis's serial number."
         ::= { chObjects 4 }

       chPartNum    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..11))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis manufacturer's part number."
         ::= { chObjects 5 }

       chProductRev    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..3))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis manufacturer's product revision."
         ::= { chObjects 6 }

       chVendorId    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..3))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis manufacturer vendor's id."
         ::= { chObjects 7 }

       chMfgDate    OBJECT-TYPE
         SYNTAX        F10MfgDate
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The date the chassis was manufactured."
         ::= { chObjects 8 }

       chCountryCode    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..2))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis manufacturer's country code."
         ::= { chObjects 9 }

       chPiecePartID    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..24))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis's piece part ID."
         ::= { chObjects 10 }

       chPPIDRevision    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..3))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis's piece part ID revision."
         ::= { chObjects 11 }

       chServiceTag    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..7))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis's service tag."
         ::= { chObjects 12 }

       chExpressServiceCode    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..14))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The chassis's express service code."
         ::= { chObjects 13 }

       chNum10GigEtherPorts    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The number of 10G Ethernet/802.3 interfaces
              in the chassis."
         ::= { chObjects 14 }

       chNum40GigEtherPorts    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The number of 40G Ethernet/802.3 interfaces
              in the chassis."
         ::= { chObjects 15 }

       chNumLineCards    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The number of line cards currently supported in the chassis."
         ::= { chObjects 16 }

       chNumFanTrays    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Number of Fan trays in the chassis."
         ::= { chObjects 17 }

       chNumPowerSupplies    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Number of Power supplies in the chassis."
         ::= { chObjects 18 }


    -- ### Chassis System  ###
    
    -- ## Processor Table
    
       chSysProcessorTable    OBJECT-TYPE
         SYNTAX        SEQUENCE OF ChSysProcessorEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A list of Processors resident in the chassis.
              The card table contains the Processor information
              of each Processor in the chassis."
         ::= { chSysObjects 1 }

       chSysProcessorEntry    OBJECT-TYPE
         SYNTAX        ChSysProcessorEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A list of Processor's entries containing information
              for Processors in the system."
         INDEX    { chSysProcessorIndex }
         ::= { chSysProcessorTable 1 }

       ChSysProcessorEntry    ::=
         SEQUENCE {
            chSysProcessorIndex     Integer32,
            chSysProcessorType      F10ProcessorModuleType,
            chSysProcessorUpTime    TimeTicks,
            chSysProcessorMemSize   Integer32
         }

       chSysProcessorIndex    OBJECT-TYPE
         SYNTAX        Integer32 (1..5)
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A unique index for each Processor within the
              chassis. The valid entries are 1 to the value
              of number of processors.
              In Z9500, Index 1 - Control Processor
                        Index 2 - Routing Processor
                        Index 3 - LineCard Processor 0
                        Index 4 - LineCard Processor 1
                        Index 5 - LineCard Processor 2"
         ::= { chSysProcessorEntry 1 }

       chSysProcessorType    OBJECT-TYPE
         SYNTAX        F10ProcessorModuleType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The type of module running on the Processor."
         ::= { chSysProcessorEntry 2 }

       chSysProcessorUpTime    OBJECT-TYPE
         SYNTAX        TimeTicks
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The SysUpTime for this Processor."
         ::= { chSysProcessorEntry 3 }

       chSysProcessorMemSize    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The size of the RAM in MB."
         ::= { chSysProcessorEntry 4 }

    -- ## Software Module Table 

       chSysSwModuleTable    OBJECT-TYPE
         SYNTAX        SEQUENCE OF ChSysSwModuleEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A list of software version information in 
             a processor."
         ::= { chSysObjects 2 }

       chSysSwModuleEntry    OBJECT-TYPE 
         SYNTAX        ChSysSwModuleEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A software module entry containing version 
             number information for a particular processor."
         INDEX    { chSysProcessorIndex }
         ::= { chSysSwModuleTable 1 }

       ChSysSwModuleEntry    ::=
         SEQUENCE {
            chSysSwModuleRuntimeImgVersion       DisplayString,
            chSysSwModuleRuntimeImgDate          F10SwDate,
            chSysSwModuleBootFlashImgVersion     DisplayString,
            chSysSwModuleBootSelectorImgVersion  DisplayString,
            chSysSwModuleNextRebootImage         INTEGER,
            chSysSwModuleCurrentBootImage        INTEGER,
            chSysSwModuleInPartitionAImgVers     DisplayString,
            chSysSwModuleInPartitionBImgVers     DisplayString
         }

       chSysSwModuleRuntimeImgVersion    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..16))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Current FTOS image version running in the system.
              The version string will be in following format
              major_ver.minor_ver(maintenance_ver.patch_ver)"
         ::= { chSysSwModuleEntry 1 }

       chSysSwModuleRuntimeImgDate    OBJECT-TYPE
         SYNTAX        F10SwDate (SIZE (0..10))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The release date of this software module."
         ::= { chSysSwModuleEntry 2 }

       chSysSwModuleBootFlashImgVersion    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..16))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "This provides the Grub image version that is currently
              running in the processor."
         ::= { chSysSwModuleEntry 3 }

       chSysSwModuleBootSelectorImgVersion    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..16))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "This provides the BIOS image version that is currently
              running in the processor."
         ::= { chSysSwModuleEntry 4 }

       chSysSwModuleNextRebootImage    OBJECT-TYPE
         SYNTAX        INTEGER {
                           partitionA(1),
                           partitionB(2),
                           networkBoot(3)
                       }
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The image selection, when the chassis is rebooted.
              partitionA - Image stored in bootflash partition A:
              partitionB - Image stored in bootflash partition B:
              networkBoot - will be booted via network."
         ::= { chSysSwModuleEntry 5 }

       chSysSwModuleCurrentBootImage    OBJECT-TYPE
         SYNTAX        INTEGER {
                           partitionA(1),
                           partitionB(2),
                           networkBoot(3)
                       }
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The current image is booted from.
              partitionA - Image stored in bootflash partition A:
              partitionB - Image stored in bootflash partition B:
              networkBoot - Booted via network."
         ::= { chSysSwModuleEntry 6 }

       chSysSwModuleInPartitionAImgVers    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..16))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "This provides the FTOS system image version
              that is stored in partition A: and The version 
              string has Major and Minor release numbers. It 
              also denotes if the release is Maintenance, 
              Technical, Patch, Beta, or Generally Available"
         ::= { chSysSwModuleEntry 7 }

       chSysSwModuleInPartitionBImgVers    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..16))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "This provides the FTOS system image version
              that is stored in partition B: and  The version
              string has Major and Minor release numbers. It
              also denotes if the release is Maintenance,
              Technical, Patch, Beta, or Generally Available"
         ::= { chSysSwModuleEntry 8 }

    -- ## Processor and Memory Utilization Table

       chSysCpuUtilTable    OBJECT-TYPE
         SYNTAX        SEQUENCE OF ChSysCpuUtilEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A table listing the processor and memory utilization of 
              of each CPU in the system."
         ::= { chSysObjects 3 }
         
       chSysCpuUtilEntry    OBJECT-TYPE
         SYNTAX         ChSysCpuUtilEntry
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
             "Processor and Memory Utilization entry for a 
              particular CPU."
         INDEX    { chSysProcessorIndex }
         ::= { chSysCpuUtilTable 1 }

       ChSysCpuUtilEntry   ::=
         SEQUENCE {
            chSysCpuUtil5Sec          Gauge32,
            chSysCpuUtil1Min          Gauge32,
            chSysCpuUtil5Min          Gauge32,
            chSysCpuUtilMemUsage      Gauge32,
            chSysCpuUtilFlashUsage    Gauge32
         }

       chSysCpuUtil5Sec    OBJECT-TYPE
         SYNTAX        Gauge32(0..100)
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "CPU utilization in percentage for last 5 seconds."
         ::= { chSysCpuUtilEntry 1 }

       chSysCpuUtil1Min    OBJECT-TYPE
         SYNTAX        Gauge32(0..100)
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "CPU utilization in percentage for last 1 minute."
         ::= { chSysCpuUtilEntry 2 }

       chSysCpuUtil5Min    OBJECT-TYPE
         SYNTAX        Gauge32(0..100)
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "CPU utilization in percentage for last 5 minutes."
         ::= { chSysCpuUtilEntry 3 }

       chSysCpuUtilMemUsage    OBJECT-TYPE
         SYNTAX        Gauge32(0..100)
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Total Memory usage in percentage."
         ::= { chSysCpuUtilEntry 4 }

       chSysCpuUtilFlashUsage  OBJECT-TYPE
         SYNTAX        Gauge32(0..100)
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Total Flash usage in percentage."
         ::= { chSysCpuUtilEntry 5 }

    -- ## Linecard Table
    
       chSysLineCardTable    OBJECT-TYPE
         SYNTAX        SEQUENCE OF ChSysLineCardEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A list of line cards resident in the chassis.
              This table contains the information on each linecard
              in the chassis."
         ::= { chSysObjects 4 }

       chSysLineCardEntry    OBJECT-TYPE
         SYNTAX        ChSysLineCardEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "Entry for each line card in the chassis."
         INDEX    { chSysLineCardIndex }
         ::= { chSysLineCardTable 1 }

       ChSysLineCardEntry    ::=
         SEQUENCE {
            chSysLineCardIndex                Integer32,
            chSysLineCardType                 INTEGER,
            chSysLineCardDescription          DisplayString,
            chSysLineCardStatus               F10CardOperStatus,
            chSysLineCardTemp                 Integer32,
            chSysLineCardNum10GigEtherPorts   Integer32,
            chSysLineCardNum40GigEtherPorts   Integer32
         }

       chSysLineCardIndex    OBJECT-TYPE
         SYNTAX        Integer32 (1..3)
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A unique index for each line card in the chassis."
         ::= { chSysLineCardEntry 1 }

       chSysLineCardType    OBJECT-TYPE
         SYNTAX        INTEGER {
                         z9500LC36(1),
                         z9500LC48(2)
                       }
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Line card's type. In Z9500, there is 36 40G port line card and
              48 40G port line card.
              z9500LC36 - 36 (40G) port LC
              z9500LC48 - 48 (40G) port LC."
         ::= { chSysLineCardEntry 2 }

       chSysLineCardDescription    OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..40))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "A short description of the line card."
         ::= { chSysLineCardEntry 3 }

       chSysLineCardStatus    OBJECT-TYPE
         SYNTAX        F10CardOperStatus
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The current operational state of the line card."
         ::= { chSysLineCardEntry 4 }

       chSysLineCardTemp    OBJECT-TYPE
         SYNTAX        Integer32
         UNITS         "degrees Centigrade"
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Temperature of the Line card."
         ::= { chSysLineCardEntry 5 }

       chSysLineCardNum10GigEtherPorts    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The number of 10G Ethernet/802.3 interfaces
              in the line card."
         ::= { chSysLineCardEntry 6 }

       chSysLineCardNum40GigEtherPorts    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The number of 40G Ethernet/802.3 interfaces
              in the line card."
         ::= { chSysLineCardEntry 7 }

    -- ## Port Table 

       chSysPortTable OBJECT-TYPE
         SYNTAX        SEQUENCE OF ChSysPortEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A list of ports in the Z-series chassis."
         ::= { chSysObjects 5 }

       chSysPortEntry  OBJECT-TYPE 
         SYNTAX        ChSysPortEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A port entry containing objects for a
              particular port."
         INDEX    { chSysLineCardIndex,
                    chSysPortIndex }
         ::= { chSysPortTable 1 }

       ChSysPortEntry    ::=
         SEQUENCE {
            chSysPortIndex        Integer32,
            chSysPortType         F10SSeriesPortType,
            chSysPortAdminStatus  INTEGER,
            chSysPortOperStatus   INTEGER,
            chSysPortIfIndex      Integer32,           
            chSysPortXfpRxPower   F10HundredthdB,
            chSysPortXfpRxTemp    Integer32,
            chSysPortXfpTxPower   F10HundredthdB
         }

       chSysPortIndex OBJECT-TYPE
         SYNTAX        Integer32 (1..192)
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A unique index for each port within the Line Card.
              Line card 0 will have index from 1 to 144
              Line card 1 will have index from 1 to 192
              Line card 2 will have index from 1 to 192."
         ::= { chSysPortEntry 1 }

       chSysPortType  OBJECT-TYPE
         SYNTAX        F10SSeriesPortType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The type of port in the unit."
         ::= { chSysPortEntry 2 }

       chSysPortAdminStatus    OBJECT-TYPE
         SYNTAX      INTEGER {
                         up(1),
                         down(2)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The admin status of the port.
              The port admin status is Up if 
              the user has configured it to be up 
              otherwise, the admin status is Down."
         ::= { chSysPortEntry 3 }

       chSysPortOperStatus    OBJECT-TYPE
         SYNTAX      INTEGER {
                       ready(1),
                       portDown(2),
                       portProblem(3),
                       cardProblem(4),
                       cardDown(5),
                       notPresent(6)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The operational status provides further
              condition of the port.
              If the chSysPortAdminStatus is 'up', the 
              valid state is
              'ready' - the card is present and 
                      ready and the chSysPortAdminStatus
                      status is 'up'.
              'portDown'    - the port is down or not enabled.
              'portProblem' - port hardware problems.
              'cardProblem' - not used.  Same as cardDown.
              'cardDown'    - the card is downed.
              'notPresent' - the card is not present."
         ::= { chSysPortEntry 4 }

       chSysPortIfIndex    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The index of ifIndex in the Interface Mib.
              This index can link to the ifEntry to get
              this interface/port information"
         ::= { chSysPortEntry 5 }

       chSysPortXfpRxPower    OBJECT-TYPE
         SYNTAX        F10HundredthdB
         UNITS         "dB"
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The power signal strength (dB) received for
              1G/10G/40G Ethernet/802.3 interface."
         ::= { chSysPortEntry 6 }

       chSysPortXfpRxTemp    OBJECT-TYPE
         SYNTAX        Integer32
         UNITS         "degrees Centigrade"
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The temperature value received for the optics."
         ::= { chSysPortEntry 7 }

       chSysPortXfpTxPower    OBJECT-TYPE
         SYNTAX        F10HundredthdB
         UNITS         "dB"
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The power signal strength (dB) Transmitted for
              1G/10G/40G Ethernet/802.3 interface."

         ::= { chSysPortEntry 8 }


    -- ## Power Supply Table

       chSysPowerSupplyTable    OBJECT-TYPE
         SYNTAX        SEQUENCE OF ChSysPowerSupplyEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A list of power supply resident
              in the Z-series chassis."
         ::= { chSysObjects 6 }

       chSysPowerSupplyEntry    OBJECT-TYPE
         SYNTAX        ChSysPowerSupplyEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A power supply entry containing objects for a
              particular power supply."
         INDEX    { chSysPowerSupplyIndex }
         ::= { chSysPowerSupplyTable 1 }

       ChSysPowerSupplyEntry    ::=
         SEQUENCE {
            chSysPowerSupplyIndex              Integer32,
            chSysPowerSupplyOperStatus         INTEGER,
            chSysPowerSupplyType               INTEGER,
            chSysPowerSupplyPiecePartID        DisplayString,
            chSysPowerSupplyPPIDRevision       DisplayString,
            chSysPowerSupplyServiceTag         DisplayString,
            chSysPowerSupplyExpressServiceCode DisplayString,
            chSysPowerSupplyUsage              Integer32
         }

       chSysPowerSupplyIndex    OBJECT-TYPE
         SYNTAX        Integer32 (1..4)
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "The unique index of the power supply."
         ::= { chSysPowerSupplyEntry 1 }

       chSysPowerSupplyOperStatus    OBJECT-TYPE
         SYNTAX      INTEGER {
                         up(1),
                         down(2),
                         absent(3)
                     }
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The status of the power supply."
         ::= { chSysPowerSupplyEntry 2 }

       chSysPowerSupplyType    OBJECT-TYPE
         SYNTAX      INTEGER {
                         ac(1),
                         dc(2)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The type of the power supply."
         ::= { chSysPowerSupplyEntry 3 }

       chSysPowerSupplyPiecePartID OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..24))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The power supply's piece part id."
         ::= { chSysPowerSupplyEntry 4 }

       chSysPowerSupplyPPIDRevision OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..3))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The power supply's PPID revision."
         ::= { chSysPowerSupplyEntry 5 }

       chSysPowerSupplyServiceTag OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..7))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The power supply's service tag."
         ::= { chSysPowerSupplyEntry 6 }

       chSysPowerSupplyExpressServiceCode OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..14))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The power supply's express service code."
         ::= { chSysPowerSupplyEntry 7 }

       chSysPowerSupplyUsage    OBJECT-TYPE
         SYNTAX        Integer32
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "Power usage of this Power Supply in Watts."
         ::= { chSysPowerSupplyEntry 8 }

    -- ## Fan Tray Table

       chSysFanTrayTable    OBJECT-TYPE
         SYNTAX        SEQUENCE OF ChSysFanTrayEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A list of fan tray resident in the Z-series chassis."
         ::= { chSysObjects 7 }

       chSysFanTrayEntry    OBJECT-TYPE
         SYNTAX        ChSysFanTrayEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "A fan entry containing objects for a
              particular fan tray."
         INDEX    { chSysFanTrayIndex }
         ::= { chSysFanTrayTable 1 }

       ChSysFanTrayEntry    ::=
         SEQUENCE {
            chSysFanTrayIndex              Integer32,
            chSysFanTrayOperStatus         INTEGER,
            chSysFanTrayPiecePartID        DisplayString,
            chSysFanTrayPPIDRevision       DisplayString,
            chSysFanTrayServiceTag         DisplayString,
            chSysFanTrayExpressServiceCode DisplayString
         }

       chSysFanTrayIndex    OBJECT-TYPE
         SYNTAX        Integer32 (1..5)
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "The unique index of the fan tray."
         ::= { chSysFanTrayEntry 1 }

       chSysFanTrayOperStatus    OBJECT-TYPE
         SYNTAX      INTEGER {
                         up(1),
                         down(2),
                         absent(3)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The status of the fan tray."
         ::= { chSysFanTrayEntry 2 }

       chSysFanTrayPiecePartID OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..24))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The fan tray's piece part id."
         ::= { chSysFanTrayEntry 3 }
                
       chSysFanTrayPPIDRevision OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..3))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The fan tray's PPID revision."
         ::= { chSysFanTrayEntry 4 }
                
       chSysFanTrayServiceTag OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..7))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The fan tray's service tag."
         ::= { chSysFanTrayEntry 5 }

       chSysFanTrayExpressServiceCode OBJECT-TYPE
         SYNTAX        DisplayString (SIZE (0..14))
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The fan tray's express service code."
         ::= { chSysFanTrayEntry 6 }


    -- ## Software Cores Table

       chSysSwCoresTable  OBJECT-TYPE
        SYNTAX        SEQUENCE OF ChSysCoresEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
            "A table containing information about the software
             cores that have been generated as a result of
             system failures."
        ::= { chSysObjects 8 }

      chSysCoresEntry  OBJECT-TYPE
        SYNTAX        ChSysCoresEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
            "A row in the software core table representing
             information about a core that has been generated."
        INDEX    { chSysProcessorIndex,
                   chSysCoresInstance  }
        ::= { chSysSwCoresTable 1 }

      ChSysCoresEntry    ::=
        SEQUENCE {
           chSysCoresInstance         INTEGER,
           chSysCoresFileName         DisplayString,
           chSysCoresTimeCreated      F10SwDate,
           chSysCoresProcessorName    DisplayString,
           chSysCoresProcess          DisplayString
        }

       chSysCoresInstance    OBJECT-TYPE
        SYNTAX        INTEGER
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION
            "The instance of the core for the process which
             which generated the core since the same process
             may have generated multiple cores."
        ::= { chSysCoresEntry 1 }

       chSysCoresFileName    OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION
            "The name of the core file including the core."
        ::= { chSysCoresEntry 2 }

       chSysCoresTimeCreated    OBJECT-TYPE
        SYNTAX        F10SwDate
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION
            "The time at which the core file was created."
        ::= { chSysCoresEntry 3 }

       chSysCoresProcessorName  OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION
            "The processor which generated the core."
        ::= { chSysCoresEntry 4 }

       chSysCoresProcess    OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION
            "The name of the process which generated the core."
        ::= { chSysCoresEntry 5 }


    -- ### conformance information ###
    f10ZSeriesChassisMibConformance    OBJECT IDENTIFIER ::= { f10ZSerChassisMib 2 }
    f10ZSeriesChassisMibCompliances    OBJECT IDENTIFIER ::= { f10ZSeriesChassisMibConformance 1 }
    f10ZSeriesChassisMibGroups         OBJECT IDENTIFIER ::= { f10ZSeriesChassisMibConformance 2 }

    -- ## compliance statements
    f10ZSeriesChassisMibCompliance MODULE-COMPLIANCE
        STATUS                  current
        DESCRIPTION
            "The compliance statement for Dell Networking
            product which implement the Z-Series
            Chassis MIB."
        MODULE    -- this module
        MANDATORY-GROUPS {
            f10ZSeriesComponentGroup,
            f10ZSeriesSystemGroup
        }
        ::= { f10ZSeriesChassisMibCompliances 1 }

    -- ## units of conformance

    f10ZSeriesComponentGroup    OBJECT-GROUP
        OBJECTS {
        chType,
        chSwVersion,
        chMacAddr,
        chSerialNumber,
        chPartNum,
        chProductRev,
        chVendorId,
        chMfgDate,
        chCountryCode,
        chPiecePartID,
        chPPIDRevision,
        chServiceTag,
        chExpressServiceCode,
        chNum10GigEtherPorts,
        chNum40GigEtherPorts,
        chNumLineCards,
        chNumFanTrays,
        chNumPowerSupplies
        }
        STATUS    current
        DESCRIPTION
            "A collection of objects providing the
            overall Z-series chassis information."
        ::= { f10ZSeriesChassisMibGroups 1 }

    f10ZSeriesSystemGroup    OBJECT-GROUP
        OBJECTS {
	chSysProcessorType,
	chSysProcessorUpTime,
	chSysProcessorMemSize,
	chSysSwModuleRuntimeImgVersion,
	chSysSwModuleRuntimeImgDate,
	chSysSwModuleBootFlashImgVersion,
	chSysSwModuleBootSelectorImgVersion,
	chSysSwModuleNextRebootImage,
	chSysSwModuleCurrentBootImage,
	chSysSwModuleInPartitionAImgVers,
	chSysSwModuleInPartitionBImgVers,
	chSysCpuUtil5Sec,
	chSysCpuUtil1Min,
	chSysCpuUtil5Min,
	chSysCpuUtilMemUsage,
        chSysCpuUtilFlashUsage,
	chSysLineCardType,
	chSysLineCardDescription,
	chSysLineCardStatus,
	chSysLineCardTemp,
	chSysLineCardNum10GigEtherPorts,
	chSysLineCardNum40GigEtherPorts,
	chSysPortType,
	chSysPortAdminStatus,
	chSysPortOperStatus,
	chSysPortIfIndex,
	chSysPortXfpRxPower,
	chSysPortXfpRxTemp,
	chSysPortXfpTxPower,
	chSysPowerSupplyOperStatus,
	chSysPowerSupplyType,
	chSysPowerSupplyPiecePartID,
	chSysPowerSupplyPPIDRevision,
	chSysPowerSupplyServiceTag,
	chSysPowerSupplyExpressServiceCode,
	chSysPowerSupplyUsage,
	chSysFanTrayOperStatus,
	chSysFanTrayPiecePartID,
	chSysFanTrayPPIDRevision,
	chSysFanTrayServiceTag,
	chSysFanTrayExpressServiceCode,
        chSysCoresInstance,
        chSysCoresFileName,
        chSysCoresTimeCreated,
        chSysCoresProcessorName,
        chSysCoresProcess
	}
	STATUS   current
	DESCRIPTION
            "A collection of objects providing the
	     chassis system hardware information."
	::= { f10ZSeriesChassisMibGroups 2 }

    END
