	XF-TOP-MIB DEFINITIONS ::= BEGIN
 
		IMPORTS
			enterprises, Integer32, Gauge32, MODULE-IDENTITY			
				FROM SNMPv2-SMI			
			TEXTUAL-CONVENTION			
				FROM SNMPv2-TC;
	
	
		-- 1.3.6.1.4.1.193.81
		miniLinkXF MODULE-IDENTITY 
			LAST-UPDATED "201210101600Z"		-- October 10, 2012 at 16:00 GMT
			ORGANIZATION 
				"Ericsson"
			CONTACT-INFO 
				" "
			DESCRIPTION 
				"This MIB specifies the highest level OIDs for 
				the MINI-LINK Traffic Node product.
				"

			REVISION "201210101600Z"		-- October 10, 2012 at 16:00 GMT
			DESCRIPTION 
				"T : Fixed minor syntax warnings"
			REVISION "201208311600Z"		-- August 31, 2012 at 16:00 GMT
			DESCRIPTION 
				"S : Changed to legal revision"
			REVISION "201206131600Z"		-- June 13, 2012 at 16:00 GMT
			DESCRIPTION 
				"P : Added xfRps subtree."
			REVISION "201109101200Z"		-- September 10, 2011 at 12:00 GMT
			DESCRIPTION 
				"O : Added xfCesService subtree."
			REVISION "201009221100Z"		-- September 22, 2010 at 11:00 GMT
			DESCRIPTION 
				"N : Added xfPT6010 subtree for PT6010"
			REVISION "201004201000Z"		-- April 20, 2010 at 10:00 GMT
			DESCRIPTION 
				"M : Added xfCN500 subtree for compact node 500."
			REVISION "201001261000Z"		-- January 26, 2010 at 10:00 GMT
			DESCRIPTION 
				"L : Added xfCN210 subtree for compact node 210."
			REVISION "200903161200Z"		-- March 16, 2009 at 12:00 GMT
			DESCRIPTION 
				"K : corrected Xf24HrsSeconds to 86400.
				"
			REVISION "200901221100Z"		-- January 22, 2009 at 11:00 GMT
			DESCRIPTION 
				"J : Length of xfProductRevison increased
				    from 10 to 40."
			REVISION "200802251444Z"		-- February 25, 2008 at 14:44 GMT
			DESCRIPTION 
				"H : Added xfSdhAdm"
			REVISION "200601261224Z"		-- January 26, 2006 at 12:24 GMT
			DESCRIPTION 
				"G added xfAtmAggregationUnit"
			REVISION "200502251600Z"		-- February 25, 2005 at 16:00 GMT
			DESCRIPTION 
				"F changed xfServiceApplications to
				  added xfIpSau"
			REVISION "200401231111Z"		-- January 23, 2004 at 11:11 GMT
			DESCRIPTION 
				"E Added xfRadioLink"
			REVISION "200306190924Z"		-- June 19, 2003 at 09:24 GMT
			DESCRIPTION 
				"D 
				Changed the Xf15MinSeconds and
				Xf24Seconds to start with 1"
			REVISION "200203071329Z"		-- March 07, 2002 at 13:29 GMT
			DESCRIPTION 
				"C 
				Added TC for Product
				number and revision
				Added TCs for seconds counter 15min
				and 24hrs
				Changed contact info
				"
			REVISION "200110081501Z"		-- October 08, 2001 at 15:01 GMT
			DESCRIPTION 
				"B etoall: xfMCR instead xfRadio"
			REVISION "200104020000Z"		-- April 02, 2001 at 00:00 GMT
			DESCRIPTION 
				"Rev. A   etoall
				Initial version"
			::= { ericsson 81 }

		
	
--
-- Textual conventions
--
	
		XfProductnumber ::= TEXTUAL-CONVENTION
			DISPLAY-HINT "30t"
			STATUS current			
			DESCRIPTION 
				"A string indicating the product number
				like 'RORJ605 001/1'. The string must be compliant to 
				standard Ericsson format for product numbers."
			SYNTAX OCTET STRING (SIZE (0..30))

		XfProductRevision ::= TEXTUAL-CONVENTION
			DISPLAY-HINT "40t"
			STATUS current
			DESCRIPTION 
				"String indicating a product revision like 'R1A00'. 
				The string must comply to standard Ericsson product 
				revision numbers.
				"
			SYNTAX OCTET STRING (SIZE (0..40))

		Xf24HrsSeconds ::= TEXTUAL-CONVENTION
		    DISPLAY-HINT "d"
			STATUS current
			DESCRIPTION 
				"General definition for perfomance threshold for 24 hours."
			SYNTAX Integer32 (1..86400)

		Xf15MinSeconds ::= TEXTUAL-CONVENTION
		    DISPLAY-HINT "d"
			STATUS current
			DESCRIPTION 
				"General definition for perfomance threshold for 15 minutes."
			SYNTAX Integer32 (1..900)

		Xf24HrsSecondsGauge ::= TEXTUAL-CONVENTION
			DISPLAY-HINT "d"
			STATUS current
			DESCRIPTION 
				"General definition for counting the number of seconds 
				in 24 hours."
			SYNTAX Gauge32 (0..86400)

		Xf15MinSecondsGauge ::= TEXTUAL-CONVENTION
			DISPLAY-HINT "d"
			STATUS current
			DESCRIPTION
				"General definition for counting the number of seconds 
				in 15 minutes."
			SYNTAX Gauge32 (0..900)

	
--
-- Node definitions
--
	
		-- 1.3.6.1.4.1.193
		ericsson OBJECT IDENTIFIER ::= { enterprises 193 }

		
		-- 1.3.6.1.4.1.193.81.1
		xfSysId OBJECT IDENTIFIER ::= { miniLinkXF 1 }

		
		-- 1.3.6.1.4.1.193.81.2
		xfPlatform OBJECT IDENTIFIER ::= { miniLinkXF 2 }

		
-- XfMediaSpecific branch is meant for the Link Applications.
		-- 1.3.6.1.4.1.193.81.3
		xfMediaSpecific OBJECT IDENTIFIER ::= { miniLinkXF 3 }

		
		-- 1.3.6.1.4.1.193.81.3.1
		xfPDH OBJECT IDENTIFIER ::= { xfMediaSpecific 1 }

		
		-- 1.3.6.1.4.1.193.81.3.2
		xfSDH OBJECT IDENTIFIER ::= { xfMediaSpecific 2 }

		
		-- 1.3.6.1.4.1.193.81.3.3
		xfMCR OBJECT IDENTIFIER ::= { xfMediaSpecific 3 }

		
-- XfRadioLink is used for the MMU3 generation, both
-- medium as well as high capacity.
		-- 1.3.6.1.4.1.193.81.3.4
		xfRadioLink OBJECT IDENTIFIER ::= { xfMediaSpecific 4 }

		
		-- 1.3.6.1.4.1.193.81.4
		xfServiceApplications OBJECT IDENTIFIER ::= { miniLinkXF 4 }

		
		-- 1.3.6.1.4.1.193.81.4.1
		xfEthernetBridge OBJECT IDENTIFIER ::= { xfServiceApplications 1 }

		
		-- 1.3.6.1.4.1.193.81.4.2
		xfAtmAggregationUnit OBJECT IDENTIFIER ::= { xfServiceApplications 2 }

		
		-- 1.3.6.1.4.1.193.81.4.3
		xfSdhAdm OBJECT IDENTIFIER ::= { xfServiceApplications 3 }

		
		-- 1.3.6.1.4.1.193.81.4.4
		xfCesService OBJECT IDENTIFIER ::= { xfServiceApplications 4 }

		
		-- 1.3.6.1.4.1.193.81.4.5
		xfRps OBJECT IDENTIFIER ::= { xfServiceApplications 5 }

		
		-- 1.3.6.1.4.1.193.81.5
		xfIpSau OBJECT IDENTIFIER ::= { miniLinkXF 5 }

		
-- Used by Compact Node 210.
		-- 1.3.6.1.4.1.193.81.6
		xfCN210 OBJECT IDENTIFIER ::= { miniLinkXF 6 }

		
-- Used by Compact Node 500.
		-- 1.3.6.1.4.1.193.81.7
		xfCN500 OBJECT IDENTIFIER ::= { miniLinkXF 7 }

		
-- Used by PT6010.
		-- 1.3.6.1.4.1.193.81.8
		xfPT6010 OBJECT IDENTIFIER ::= { miniLinkXF 8 }

		
	
	END

--
-- 3_19603-crxr10201_1_top.mi2
--
