

        -- Teldat, S.A.
        -- Parque Tecnologico de Madrid
        -- 28760, Tres Cantos (Madrid)
        -- Tlf: +34-918076565
        -- Fax: +34-918076521
        -- e-mail: id@teldat.com


        -- MIB privada de Teldat


        -- Historial:
        --      12-04-16    P. Alonso           USB3.0
        --      11-03-16    Benjamin G.         DR 416 Regesta Compact PLC
	--      02-03-16    jmarcos             DR 284. New device Teldat H2 Rail
	--      04-02-16    L. Saiz             New SMGT events subsystem
        --      22-12-15    S. Font             H2 Auto Plus correction
        --      10-12-15    S. Font             H2 Auto Plus
        --      24-03-15    Benjamin G.         DR 336 GPS on H2Auto.
        --      18-11-15    fmiguel.            New device H2Rail-Lite2 (M1 based with Rail board).
        --      10-11-15    fmiguel.            New product H2 Rail-Lite.
	--      02-11-15    P. Nogueira         Revision for mib2c
        --      20-10-15    Benjamin G.         DR 161 Regesta PLC PRIME.
        --      16-10-15    A.Campa             CFM fix compilation II	
        --      11-09-15    S. Font             MII cards for iM
        --      27-05-15    E. Amorena          Teldat iM: ethernet with switch and poe.
        --      25-03-15    I. Serrano          New USB-Ethernet interface adapter	
        --      12-09-14    A. Mata             Variable to save running configuration
        --      05-12-14    J. Lamamie          DHCPv6 Server Stateless
	--      03-11-14    P. Nogueira         WNMS
        --      24-07-14    Benjamin G.         New products H2 Automotive. 	
        --      12-09-14    A. Mata             Removed UDAFO and DEP
        --      31-07-14    Benjamin G.         New products line bintec RVC series. 
        --      30-07-14    A. Mata             Visoralarm no longer supported
        --      20-06-14    S. Font             New product Teldat V for DSL over ISDN (Annex BJ)
        --      19-02-14    fmiguel		New product RegestaLite
	--      14-02-14    I. Munoz            Rebranding bintec elmeg	
	--      31-01-14    I. Serrano          Standard format of SNMP traps	
        --  	03-12-13    F. Hernandez       	XI 3280. Alsa Custom Trap.
        --      24-09-13    fmiguel             New product Connect 4GE
        --      16-09-13    fmiguel             New product Connect 104KF
        --      06-09-13    fmiguel             New product Connect 104V
        --      19-06-13    P. Alonso           Wrong ID for Teldat 4Ge or ESR-WWAN-ENABLER..
        --      14-06-13    P. Alonso           Compilation errors.
        --      12-06-13    P. Alonso           Teldat 4Ge or ESR-WWAN-ENABLER.
        --      08-04-13    A. Mata             Device identifiers added for ALU devices.
        --      02-04-13    I. Munoz            XH-2788. Group of traps added to 
        --                                      telAdminStatusSRESubRecordTable.
        --      07-03-13    N. Moro             XI 2441. MSDP protocol
        --      05-03-13    fmiguel             USB Ethernet adapter
        --      19-02-13    fmiguel             New product Teldat M1
        --      11-02-13    P. Nogueira         Teldat-V: switch management
     	--      22-01-13    I. Munoz            Code clean-up.
        -- 17.0 02-01-13    E. Amorena          Compilation error
        -- 16.9 29-11-12    E. Amorena          Mibs checks
        -- 16.8 22-11-12    Benjamín G.         Events subsystem NIC and add H1 Rail device.
        -- 16.7 22-11-12    J. Lamamie          OSPFv3. Commented duplicate RIP6.
        -- 16.6 13-11-12    N. Moro             PIM protocol and MROUTE
        -- 16.5 12-11-12    E. Amorena          New ACL events subsystem
        -- 16.4 09-07-12    P. Nogueira         WLAN subinterfaces on Colibri platforms
        -- 16.3 27-07-12    M. Fadón            New product Connect 104
        -- 16.2 07-06-12    C. Godoy            Subsistema de eventos LLDP, RIP6 y MLD6.
        -- 16.1 30-01-12    J. Rodrigo          Nuevos interfaces
        -- 16.0 14-12-11    GrupoIPv6           Nuevo IPv6: Fase 1
        -- 15.9 18-01-12    V. Espejo           Subsistema de eventos IPSF
        -- 15.8 20-07-11    S. Font             Subsistema de eventos SDEV
        -- 15.7 18-07-11    M.A. Pastor         Atlas 60: añadidos equipos,
        --                                      licencias, tipos de placa, tipos
        --                                      de interfaz y tipos de conector
        -- 15.6 20-05-11    M.A. Pastor         Añadidos equipos, tipos de placa,
        --                                      tipos de interfaz, conectores,
        --                                      subsistemas de eventos y licencias
        -- 15.5 23-12-10    P. Nogueira         Subinterfaces WLAN
        -- 15.4 29-12-10    P. Ortiz            RegestaPro6xER. Feature ACAT
        -- 15.3 27-10-10    E. Amorena          Nuevo equipo RegestaPro6xER
        -- 15.2 15-10-10    M. Fadón            XI 988. iRouter Pro. Feature VLI.
        -- 15.1 05-10-10    P. Ortiz            Equipos Regesta-1, RP81 y RP82
        -- 15.0 30-06-10    M.A. Pastor         Compatibilidad con Spectrum
        -- 14.9 10-03-10    I. Muñoz            Se añade conector usb en teladminstatusiftable
        -- 14.8 30-12-09    FdMB                Plataforma H1+
        -- 14.7 03-11-09    FdMB                Plataforma T200W
        -- 14.6 23-10-09    FdMB                Plataforma H4
        -- 14.5 07-09-09    Benjamín G.         PMP-909 Agente SPI.
        -- 14.4 08-07-09    I. Muñoz            Revisión de todas las MIB para
        --                  M.A. Pastor         evitar warnings y errores de
        --                                      compilación
        -- 14.3 31-08-09    N. Moro             PMP 855. Contadores de bits en entrada
        -- 14.2 03-07-09    FdMB                Equipos C1+L y V1
        -- 14.1 20-05-09    Benjamín G.         Cambio nombre H1 Ind. a AUTOMOTIVE.
        -- 14.0 08-04-09    Benjamín G.         Equipo Teldat G1N
        -- 13.9 18-03-09    Benjamín G.         Equipo Teldat H1 Industrial
        -- 13.8 11-03-09    J.Sirodey           Equipo Teldat T200 pasa a ser Teldat T200G
        -- 13.7 31-10-08    M.Fad & P.Ort       Prot MGCP obsoletando el anterior
        -- 13.6 30-07-08    FdMB                Plataforma TELDAT_T200
        -- 13.5 24-06-08    R. Roldan           Se añade susbsistema NETFLOW y
        --                                      RIP obsoletando el anterior
        -- 13.4 05-03-08    J. Herrero          Reservado sistema de eventos para PIO
        -- 13.3 05-03-08    M. Fadón            VyDa 4M
        -- 13.2 21-02-08    M.A. Pastor         Actualización de los tipos de
        --                  J. Herrero          interfaz y de los tipos de
        --                                      conector para soportar todos los
        --                                      incluidos en el CIT.
        --                                      Se añaden los subsistemas de
        --                                      eventos ME, ARLY, DNS Updater,
        --                                      UDP6, ICMP6, RIP6, SSL y SCCP
        -- 13.1 24-01-08    P. Nogueira         Eventos para CDP
        -- 13.0 30-11-07    P. Ortiz            Protocolo SSH
        -- 12.9 27-01-08    F. Tresgallo        Subsistema de eventos EOAM
        -- 12.8 11-09-07    P. Nogueira         Eventos para 802.1X
        -- 12.7 02-08-07    M.A. Berrojo        Subsistema de eventos ISTD
        -- 12.6 30-10-07    M.A. Berrojo        Subsistema de eventos WWAN
        -- 12.5 14-09-07    FdMB                ATLAS260/ATASL160
        -- 12.4 20-06-07    P. Nogueira         Eventos para TFTP
        -- 12.3 20-06-07    P. Nogueira         Subinterfaces BVI
        -- 12.2 18-06-07    M.A. Berrojo        Subsistema de eventos cell
        -- 12.1 16-06-07    FdMB                Plataformas H1.
        -- 12.0 18-04-07    R. Roldan           PMP 554: facilidad confirm-cfg-needed por SNMP
        -- 11.9 19-03-07    M.A. Berrojo        voip-cellular y cellular
        -- 11.8 08-03-07    P. Alonso           Traps BFD.
        -- 11.7 20-12-06    M. Fadón            Traps NOE y AFS.
        -- 11.6 05-12-06    Benjamín G.         Traps X28.
        -- 11.5 20/10/06    J. Iglesias         Subsistema TIDP
        -- 11.4 26-07-06    P. Nogueira         Eventos de RSTP
        -- 11.3 10/10/06    A. Mata             Traps para IRVOZ
        -- 11.2 19/09/06    M.A. Pastor         Nuevo equipo CIRUS
        -- 11.1 06-07-06    C. García           CIRUS: Implementación bridge-spoofing
        -- 11.0 15-06-06    FdMB                (II) HAP 222: Atlas3g. Soporte 85xx. Plataforma PQIII
        -- 10.9 16-02-06    FdMB                Plataformas X2-a, X4-a.
        -- 10.2 30-05-06    M.A. Pastor         La TELDAT-MIB no compilaba
        -- 10.1 02-03-06    M.A. Berrojo        Interfaz voip dummy
        -- 10.0 28-02-06    J. Rodrigo          VisorALARM_EU, VisorALARM_US.
        -- 10.8 16-02-06    FdMB                Plataformas X1-a.
        -- 10.7 14/12/05    P. Nogueira         EAP
        -- 10.6 24-01-05    FdMB                GigabitEthernet eTSEC PQIII
        -- 10.5 22/11/05    J.Sirodey           C8+, C9+
        -- 10.4 04-01-06    S. Font             G4[i]-CDMA, G3[i]-CDMA, G1[i]-CDMA
        -- 10.3 30-11-05    FDMB                CISCO-HDLC
        -- 10.2 12/12/05    Benjamín G.         Traps SCADA FW.
        -- 10.1 22/11/05    FdMB                C1+
        -- 10.0 29/08/05    M. Fadon            VyDa-Compacto
        -- 9.9  24/10/05    P. Marzo            Cliente STUN
        -- 9.8  18/10/05    P. Nogueira         WLAN
        -- 9.7  28/09/05    FdMB                ATLAS152
        -- 9.6  03/10/05    M.A. Pastor         La TELDAT-MIB no compilaba
        -- 9.5  20/09/05    FdMB                ATLAS300 de verdad (ATLAS150+BUS@100+CPU@400)
        -- 9.4  15/09/05    J. Roman            Se obsoleta parte no utilizada
        -- 9.3  13/09/05    P. Alonso           Protocolo NHRP
        -- 9.2  05/09/05    O. Mateo            Subsistema de eventos SNAT
        -- 9.1  29/08/05    M. Fadon            Nuevas licencias VyDa
        -- 9.0  29/07/05    S. Font             G PLus (corregir 8.8 y 8.9)
        -- 8.9  26/07/05    S. Font             G PLus (completar 8.8)
        -- 8.8  21/07/05    S. Font             G PLus
        -- 8.7  21/07/05    FdMB                Atlas2G Sondas Web
        -- 8.6  14/07/05    M.A. Pastor         La TELDAT-MIB no compilaba
        -- 8.5  14/07/05    FdMB                Tarjeta PCI-GIGABIT-Ethernet
        -- 8.4  17/06/05    M. Fadon            Nuevo subsistema de eventos
        --                                      TLPHY y se elimina mib h323
        -- 8.3  17/06/05    M.A. Pastor         No se había añadido el ATLAS 250
        --                                      en telobjid ni en
        --                                      telAdminStatusSystemCode.
        --                                      Se corrige la etiqueta
        --                                      correspondiente al ATLAS 50 en
        --                                      el tipo enumerado de
        --                                      telAdminStatusSystemCode
        -- 8.2  30/05/05    R. Sánchez          Eventos de consola
        -- 8.1  03/06/05    M.A. Pastor         Nuevos tipos de hardware:
        --                                      * PCI soporte VoIP analógico
        --                                        3DXS, 1FXO con bypass
        --                                      * PCI soporte VoIP analógico
        --                                        2FXS, 2FXO con bypass
        --                                      * PCI E1/T1 sobre Acodes 490x
        --                                      * PCI soporte VoIP isdn BRI-TE
        --                                      * Soporte ISDN VoIP como dial
        -- 8.0  26/04/05    J. Sirodey          ATLAS 50
        -- 7.9  09/05/05    M.A. Pastor         DHCP cliente
        -- 7.8  27/04/05    FdMB                Tarjetas PCI-ATM-PQ2 y PCI-BRI-PQ2
        -- 7.7  21/03/05    D. Rodriguez        IPHC
        -- 7.6  16/03/05    M. Fadon            Protocolo SIP
        -- 7.5  16/03/05    S. Font             Teldat C1i/S1i [SNA] [IPSec] VOIP CR
        -- 7.4  18/01/05    FdMB                TeldatA (Modular hija analogica)
        -- 7.3  17/01/05    FdMB                Completadas licencias ATLAS 150
        -- 7.2  21/01/05    M.A. Pastor         Licencias VoIP corregidas
        -- 7.1  17/01/05    D. Rodriguez        Protocolo VRRP
        -- 7.0  10/01/05    P. Marzo            Agregada licencia VoIP
        -- 6.9  22/12/04    Benjamin G.         Protocolo SCADA.
        -- 6.8  14/12/04    M.A. Pastor         Corregidos identificadores de
        --                                      licencias (deben comenzar con
        --                                      minúscula)
        -- 6.7  13/12/04    FdMB                Completadas licencias ATLAS 250
        -- 6.6  09/12/04    M.A. Pastor         ATLAS 100-B
        -- 6.5  09/12/04    M.A. Pastor         Nuevas licencias para ATLAS 100
        -- 6.4  29/11/04    M.A. Pastor         Corregidos valores medio activo
        -- 6.3  25/11/04    M.A. Pastor         Se añaden nuevos tipos de placa
        -- 6.2  25/11/04    M.A. Pastor         Esta MIB no compilaba
        -- 6.1  24/11/04    M. Fuertes          Se agrega interfaz virtual de bridge (BVI)
        -- 6.0  26/10/04    S. Font             C4G
        -- 5.9  20/10/04    P. Nogueira         SR-DSCC4-HSSI
        -- 5.8  04/10/04    FdMB                SR_PCMCIA_SERIAL
        -- 5.7  28/09/04    O. Mateo            Subsistema de eventos IKE
        -- 5.6  22/09/04    M.A. Pastor         Se acortan los nombres de los
        --                                      identificadores en los tipos
        --                                      enumerados (no se compilaba en
        --                                      OpenView)
        -- 5.5  10/09/04    FdMB                ATLAS300
        -- 5.4  09/09/04    Benjamin G.         PMP(HT53) Se añade sub. TTTP.
        -- 5.3  01-09-04    M.A. Berrojo        Se soportan eventos voip
        -- 5.2  09/07/04    M.A. Pastor         Cambio en las variables que
        --                                      ejecutan el restart y el reload
        --                                      para que coincidan con la acción
        --                                      que realizan en equipos antiguos
        -- 5.1  05/05/04    M.A. Pastor         Nuevos equipos Atlas 300 y C1G.
        -- 5.0  23/06/04    M.A. Pastor         Nuevas licencias (CR: Calidad de
        --                                      Respaldo) y nuevo subsistema de
        --                                      eventos NSLA
        -- 4.9  01/06/04    M.A. Pastor         Nuevos tipos de interfaz (PCI
        --                                      soporte VoIP analógico y L2TP)
        --                                      y nuevos subsistemas de eventos
        --                                      (Telnet y L2TP)
        -- 4.8  11/05/04    M.A. Pastor         Se añaden las licencias de los
        --                                      equipos antiguos por si desde
        --                                      una misma estación se quiere
        --                                      gestionar todo un parque en el
        --                                      que todavía convivan este tipo
        --                                      de equipos junto con los nuevos
        -- 4.7  05/05/04    M.A. Pastor         Revisión tipos de interfaz.
        --                                      Se añaden nuevas licencias.
        --                                      Notificación de eventos mediante
        --                                      mensajes syslog. Se obsoletan
        --                                      las alarmas propietarias.
        -- 4.6  04/02/04    M.A. Pastor         Revisión tipos de interfaz y
        --                                      subsistemas de eventos.
        -- 4.5  09/12/03    F. Hernández        Cambio en las traps generadas en
        --                                      el proceso de sondeo de los
        --                                      estados de los TE-Circuits
        -- 4.4  20/11/03    M.A. Pastor         Nuevo tipo de placa (board type)
        -- 4.3  14/11/03    M.A. Pastor         Nuevas licencias y códigos de
        --                                      gestión de los equipos.
        -- 4.2  22/10/03    M.A. Pastor         Nuevas licencias, códigos de
        --                                      equipo, tipos de interfaz y
        --                                      subsistemas de eventos.
        --                                      Los equipos Teldat C5x pasan a
        --                                      denominarse Teldat C4x SNA.
        -- 4.1  19/09/03    M.A. Pastor         Nuevos equipos Teldat C1/S1/G1.
        --                                      Motorola FEC con Switch KS8995M
        -- 4.0  19/09/03    F. Hernández        Traps generadas en el proceso de
        --                                      sondeo de los estados de los
        --                                      TE-Circuits encargado por MCI
        -- 3.9  24/07/03    M.A. Pastor         Nuevas licencias y sublicencias.
        --                                      Revisión del subsistema de
        --                                      eventos, de los códigos de
        --                                      equipo y de los tipos de interfaz
        -- 3.8  05/12/02    M.A. Pastor         Nuevas variables para obtener el
        --                                      tipo de placa y la revisión de
        --                                      la misma y para saber si está o
        --                                      no montado el controlador de
        --                                      SmartCard.
        --                                      Se aprovecha para revisar el
        --                                      sistema de eventos, licencias y
        --                                      códigos de los equipos
        -- 3.7  16/10/02    P. Nogueira         Nuevas variables relacionadas
        --                                      con la elección del medio activo
        --                                      (Flash o SmartCard)
        -- 3.6  19/07/02    M.A. Pastor         Se actualizan los códigos o
        --                                      identificadores de los equipos
        --                                      de Teldat en telobjid. También
        --                                      se revisa el sistema de eventos
        -- 3.4  14/02/02    M.A. Pastor         Nuevas licencias para C2-UP
        --                                      y C6. Cambios en las licencias
        --                                      correspondientes al Visornet
        -- 3.3  14/02/02    M.A. Pastor         Se corrige la descripción de la
        --                                      variable sreEvnStatusAct (no se
        --                                      indicaban bien los valores de
        --                                      las máscaras a aplicar)
        -- 3.2  04/02/02    M.A. Pastor         Cambios en los tipos de los
        --                                      interfaces
        -- 3.1  04/02/02    M.A. Pastor         Nuevas licencias para Centrix-D
        --                                      y Centrix-Sec-A (versión Atlas).
        --                                      Nuevo código de equipo para el
        --                                      C2-UP.
        --                                      Se agregan los posibles tipos de
        --                                      conector que no se contemplaban
        -- 3.0  21/01/01    M.A. Pastor         Nuevos equipos Centrix-Sec y
        --                                      Atlas-D. Inclusión de la
        --                                      licencia de C-Master_Router
        -- 2.9  14/12/01    M.A. Pastor         Revisión del sistema de eventos
        -- 2.8  25/10/01    J. L. Fuentes       Se agregan los interfaces serie
        --                                      sincrono y asincrono
        -- 2.7  25/10/01    M.A. Pastor         Revision de las licencias y de
        --                                      los códigos de los equipos
        -- 2.6  01/10/01    N. Villaseñor       Traducción a inglés
        -- 2.5  10/04/01    M.A. Pastor         Se actualizan los posibles tipos
        --                                      de interfaces y se agrega el
        --                                      interfaz de Loopback
        -- 2.4  01/12/00    M.A. Pastor         Modificaciones para que pueda ser
        --                                      compilada utilizando compiladores
        --                                      distintos del de Teldat
        -- 2.3  13/12/99    V.Ruiz-Ruano        Añado OID de subsistema ICU PLUS
        --                                      para que haga de enterprise en
        --                                      TRAPS específicas de Teldat
        -- 2.2  01/03/99    V.Ruiz-Ruano        Elimino SRETrapEquipo, puesto que
        --                                      no todas las TRAPS devuelven el
        --                                      equipo como tercer parámetro.
        -- 2.1  01/03/99    V.Ruiz-Ruano        Añado los OIDs que harán la
        --                                      función de Enterprise en las TRAPS

        -- 2.0          08/07/98    Jose Picot  Agregacion de nuevos equipos

        -- 1.0 (beta)   27/06/97    Eduardo Tejedor y Jorge Sirodey
        --                          Implementacion inicial

    --------------------------------------------------------------------------

TELDAT-MIB DEFINITIONS ::= BEGIN


    IMPORTS
            enterprises, IpAddress, Counter, Opaque
        FROM RFC1155-SMI
            OBJECT-TYPE
        FROM RFC-1212
            DisplayString
        FROM RFC1213-MIB
            TRAP-TYPE
        FROM RFC-1215;

    teldat  OBJECT IDENTIFIER ::= { enterprises 2007 }

    -- Grupos en la MIB de TELDAT

    teladmin            OBJECT IDENTIFIER ::= { teldat 1 }
    -- telxface         OBJECT IDENTIFIER ::= { teldat 2 }
    telproto            OBJECT IDENTIFIER ::= { teldat 3 }
    telproducts         OBJECT IDENTIFIER ::= { teldat 4 }
    -- telDot3ChipSets  OBJECT IDENTIFIER ::= { teldat 5 }


    -- --------------
    -- Grupo teladmin
    -- --------------

    telobjid    OBJECT IDENTIFIER ::= { teladmin 1 }

    -- Identificadores de los equipos de Teldat.

    -- Notas:
    -- 1) Este valor no coincide con el de la rama de telproducts donde se
    --    encuentra la MIB privada de ese equipo.
    -- 2) Inicialmente este OID tenia como mision identificar el equipo que
    --    habia originado una trap a partir de este valor, que se incluia como
    --    un parametro de la trap. Actualmente no se incluye tal variable en las
    --    traps.
    -- 3) Se sigue incluyendo este OID en el campo enterprise de las traps
    --    standard.

    -- equipo-rexis-ft         OBJECT IDENTIFIER ::= { telobjid 3 }

    -- equipo-bir-64           OBJECT IDENTIFIER ::= { telobjid 11 }

    equipo-rexis-mru        OBJECT IDENTIFIER ::= { telobjid 15 }

    equipo-mbbu             OBJECT IDENTIFIER ::= { telobjid 16 }

    equipo-bir-u            OBJECT IDENTIFIER ::= { telobjid 20 }

    equipo-ebano            OBJECT IDENTIFIER ::= { telobjid 21 }

    equipo-nucleox-plus     OBJECT IDENTIFIER ::= { telobjid 32 }

    equipo-cbra             OBJECT IDENTIFIER ::= { telobjid 33 }

    equipo-centrix-b        OBJECT IDENTIFIER ::= { telobjid 34 }

    equipo-centrix-p        OBJECT IDENTIFIER ::= { telobjid 35 }

    equipo-temis            OBJECT IDENTIFIER ::= { telobjid 36 }

    equipo-novacom          OBJECT IDENTIFIER ::= { telobjid 37 }

    equipo-router-maestro   OBJECT IDENTIFIER ::= { telobjid 38 }

    equipo-cbra20           OBJECT IDENTIFIER ::= { telobjid 39 }

    equipo-np20h            OBJECT IDENTIFIER ::= { telobjid 40 }

    equipo-icu-plus         OBJECT IDENTIFIER ::= { telobjid 41 }

    equipo-centrix-f        OBJECT IDENTIFIER ::= { telobjid 42 }

    equipo-cbra-tar         OBJECT IDENTIFIER ::= { telobjid 43 }

    equipo-aura             OBJECT IDENTIFIER ::= { telobjid 44 }

    equipo-kronos           OBJECT IDENTIFIER ::= { telobjid 45 }

    -- equipo-cbra-adsl     OBJECT IDENTIFIER ::= { telobjid 46 }

    equipo-teldat-C2        OBJECT IDENTIFIER ::= { telobjid 46 }

    equipo-operador-remoto  OBJECT IDENTIFIER ::= { telobjid 47 }

    equipo-visor            OBJECT IDENTIFIER ::= { telobjid 48 }

    equipo-voxnet           OBJECT IDENTIFIER ::= { telobjid 49 }

    equipo-dusac32          OBJECT IDENTIFIER ::= { telobjid 50 }

    equipo-novacom-x25      OBJECT IDENTIFIER ::= { telobjid 51 }

    equipo-enaplan          OBJECT IDENTIFIER ::= { telobjid 52 }

    equipo-teldat-C3        OBJECT IDENTIFIER ::= { telobjid 53 }

    equipo-atlas-standard   OBJECT IDENTIFIER ::= { telobjid 56 }   --$M4.3

    equipo-teldat-C2B       OBJECT IDENTIFIER ::= { telobjid 57 }

    equipo-teldat-CSW       OBJECT IDENTIFIER ::= { telobjid 58 }

    equipo-teldat-C3-1      OBJECT IDENTIFIER ::= { telobjid 59 }

    equipo-teldat-C3B-1     OBJECT IDENTIFIER ::= { telobjid 60 }

    equipo-teldat-C2BM      OBJECT IDENTIFIER ::= { telobjid 61 }

    equipo-atlas-basico     OBJECT IDENTIFIER ::= { telobjid 62 }   --$M4.3

    equipo-teldat-C2i       OBJECT IDENTIFIER ::= { telobjid 63 }

    equipo-teldat-C3i       OBJECT IDENTIFIER ::= { telobjid 64 }

    equipo-teldat-C3B       OBJECT IDENTIFIER ::= { telobjid 65 }

    equipo-teldat-C3G       OBJECT IDENTIFIER ::= { telobjid 66 }

    -- equipo-teldat-C4-teldat-C5      OBJECT IDENTIFIER ::= { telobjid 67 }

    equipo-teldat-C4        OBJECT IDENTIFIER ::= { telobjid 67 }   --$M4.2

    -- equipo-teldat-C4i-teldat-C5i    OBJECT IDENTIFIER ::= { telobjid 68 }

    equipo-teldat-C4i       OBJECT IDENTIFIER ::= { telobjid 68 }   --$M4.2

    -- equipo-teldat-C4B-teldat-C5B    OBJECT IDENTIFIER ::= { telobjid 69 }

    equipo-teldat-C4B       OBJECT IDENTIFIER ::= { telobjid 69 }   --$M4.2

    equipo-centrix-sec      OBJECT IDENTIFIER ::= { telobjid 70 }

    equipo-centrix-d        OBJECT IDENTIFIER ::= { telobjid 71 }

    equipo-teldat-C2-UP     OBJECT IDENTIFIER ::= { telobjid 72 }

    equipo-teldat-C6        OBJECT IDENTIFIER ::= { telobjid 73 }

    equipo-centrix-ng       OBJECT IDENTIFIER ::= { telobjid 74 }   --$M3.9

    equipo-atlas-voxnet     OBJECT IDENTIFIER ::= { telobjid 75 }   --$M3.9

    equipo-s2               OBJECT IDENTIFIER ::= { telobjid 76 }   --$M4.3

    equipo-s4               OBJECT IDENTIFIER ::= { telobjid 77 }   --$M4.3

    equipo-s2i              OBJECT IDENTIFIER ::= { telobjid 78 }   --$M4.3

    equipo-s4i              OBJECT IDENTIFIER ::= { telobjid 79 }   --$M4.3

    equipo-g2               OBJECT IDENTIFIER ::= { telobjid 80 }   --$M4.3

    equipo-g3               OBJECT IDENTIFIER ::= { telobjid 81 }   --$M4.3

    equipo-g4               OBJECT IDENTIFIER ::= { telobjid 82 }   --$M4.3

    equipo-g2i              OBJECT IDENTIFIER ::= { telobjid 83 }   --$M4.3

    equipo-g3i              OBJECT IDENTIFIER ::= { telobjid 84 }   --$M4.3

    equipo-g4i              OBJECT IDENTIFIER ::= { telobjid 85 }   --$M4.3

    equipo-c1               OBJECT IDENTIFIER ::= { telobjid 86 }   --$M4.3

    equipo-c1B              OBJECT IDENTIFIER ::= { telobjid 87 }   --$M4.3

    equipo-c1i              OBJECT IDENTIFIER ::= { telobjid 88 }   --$M4.3

    equipo-s1               OBJECT IDENTIFIER ::= { telobjid 89 }   --$M4.3

    equipo-s1i              OBJECT IDENTIFIER ::= { telobjid 90 }   --$M4.3

    equipo-g1               OBJECT IDENTIFIER ::= { telobjid 91 }   --$M4.3

    equipo-g1i              OBJECT IDENTIFIER ::= { telobjid 92 }   --$M4.3

    equipo-g3-lite          OBJECT IDENTIFIER ::= { telobjid 93 }   --$M4.3

    equipo-C3G-lite         OBJECT IDENTIFIER ::= { telobjid 94 }   --$M4.3

    equipo-atlas-100        OBJECT IDENTIFIER ::= { telobjid 96 }   --$M4.3

    equipo-atlas-300V       OBJECT IDENTIFIER ::= { telobjid 97 }   --$M4.7

    equipo-c1G              OBJECT IDENTIFIER ::= { telobjid 98 }   --$M4.7

    equipo-atlas-250        OBJECT IDENTIFIER ::= { telobjid 101 }

    equipo-c4G              OBJECT IDENTIFIER ::= { telobjid 102 }  --$M6.0

    equipo-atlas-100B       OBJECT IDENTIFIER ::= { telobjid 103 }

    equipo-atlas-150        OBJECT IDENTIFIER ::= { telobjid 104 }

    equipo-a2               OBJECT IDENTIFIER ::= { telobjid 105 }

    equipo-a3               OBJECT IDENTIFIER ::= { telobjid 106 }

    equipo-a4               OBJECT IDENTIFIER ::= { telobjid 107 }

    equipo-a2i              OBJECT IDENTIFIER ::= { telobjid 108 }

    equipo-a3i              OBJECT IDENTIFIER ::= { telobjid 109 }

    equipo-a4i              OBJECT IDENTIFIER ::= { telobjid 110 }

    equipo-a1               OBJECT IDENTIFIER ::= { telobjid 111 }

    equipo-a1i              OBJECT IDENTIFIER ::= { telobjid 112 }

    equipo-g4-cdma          OBJECT IDENTIFIER ::= { telobjid 114 }

    equipo-g4i-cdma         OBJECT IDENTIFIER ::= { telobjid 115 }

    equipo-g3-cdma          OBJECT IDENTIFIER ::= { telobjid 116 }

    equipo-g3i-cdma         OBJECT IDENTIFIER ::= { telobjid 117 }

    equipo-g1-cdma          OBJECT IDENTIFIER ::= { telobjid 118 }

    equipo-g1i-cdma         OBJECT IDENTIFIER ::= { telobjid 119 }

    equipo-c1plus           OBJECT IDENTIFIER ::= { telobjid 122 }

    equipo-c1iplus          OBJECT IDENTIFIER ::= { telobjid 123 }

    equipo-atlas-50         OBJECT IDENTIFIER ::= { telobjid 126 }

    equipo-g4plus           OBJECT IDENTIFIER ::= { telobjid 127 }

    equipo-g3plus           OBJECT IDENTIFIER ::= { telobjid 128 }

    equipo-g1plus           OBJECT IDENTIFIER ::= { telobjid 129 }

    equipo-g4iplus          OBJECT IDENTIFIER ::= { telobjid 130 }

    equipo-g3iplus          OBJECT IDENTIFIER ::= { telobjid 131 }

    equipo-g1iplus          OBJECT IDENTIFIER ::= { telobjid 132 }

    equipo-atlas-250SW      OBJECT IDENTIFIER ::= { telobjid 133 }

    equipo-atlas-150SW      OBJECT IDENTIFIER ::= { telobjid 134 }

    equipo-atlas-50SW       OBJECT IDENTIFIER ::= { telobjid 135 }

    equipo-vyda-1M          OBJECT IDENTIFIER ::= { telobjid 136 }

    equipo-vyda-2M          OBJECT IDENTIFIER ::= { telobjid 137 }

    equipo-vyda-3M          OBJECT IDENTIFIER ::= { telobjid 138 }

    equipo-atlas-300        OBJECT IDENTIFIER ::= { telobjid 139 }

    equipo-atlas-152        OBJECT IDENTIFIER ::= { telobjid 140 }

    equipo-vyda-compact     OBJECT IDENTIFIER ::= { telobjid 141 }

    equipo-C8plus           OBJECT IDENTIFIER ::= { telobjid 142 }

    equipo-C8iplus           OBJECT IDENTIFIER ::= { telobjid 143 }

    equipo-C9plus           OBJECT IDENTIFIER ::= { telobjid 144 }

    equipo-C9iplus           OBJECT IDENTIFIER ::= { telobjid 145 }

    equipo-atlas-360        OBJECT IDENTIFIER ::= { telobjid 146 }

    equipo-c1plus-SW        OBJECT IDENTIFIER ::= { telobjid 147 }

    equipo-c1a              OBJECT IDENTIFIER ::= { telobjid 148 }

    equipo-s1a              OBJECT IDENTIFIER ::= { telobjid 149 }

    equipo-g1a              OBJECT IDENTIFIER ::= { telobjid 150 }

    equipo-g1a-cdma         OBJECT IDENTIFIER ::= { telobjid 151 }

    equipo-a1a              OBJECT IDENTIFIER ::= { telobjid 152 }

    equipo-c2a              OBJECT IDENTIFIER ::= { telobjid 155 }

    equipo-s2a              OBJECT IDENTIFIER ::= { telobjid 156 }

    equipo-g2a              OBJECT IDENTIFIER ::= { telobjid 157 }

    equipo-a2a              OBJECT IDENTIFIER ::= { telobjid 158 }

    equipo-c4a              OBJECT IDENTIFIER ::= { telobjid 159 }

    equipo-s4a              OBJECT IDENTIFIER ::= { telobjid 160 }

    equipo-g4a              OBJECT IDENTIFIER ::= { telobjid 161 }

    equipo-g4a-cdma         OBJECT IDENTIFIER ::= { telobjid 162 }

    equipo-a4a              OBJECT IDENTIFIER ::= { telobjid 163 }

    equipo-cirus            OBJECT IDENTIFIER ::= { telobjid 165 }

    equipo-h1               OBJECT IDENTIFIER ::= { telobjid 166 }

    equipo-atlas-260        OBJECT IDENTIFIER ::= { telobjid 167 }

    equipo-atlas-160        OBJECT IDENTIFIER ::= { telobjid 168 }

    equipo-vyda-4M          OBJECT IDENTIFIER ::= { telobjid 169 }

    equipo-t200g            OBJECT IDENTIFIER ::= { telobjid 170 }

    equipo-h1-auto          OBJECT IDENTIFIER ::= { telobjid 171 }

    equipo-g1n              OBJECT IDENTIFIER ::= { telobjid 172 }

    equipo-v1               OBJECT IDENTIFIER ::= { telobjid 173 }

    equipo-c1plusl          OBJECT IDENTIFIER ::= { telobjid 174 }

    equipo-h4               OBJECT IDENTIFIER ::= { telobjid 175 }

    equipo-t200             OBJECT IDENTIFIER ::= { telobjid 176 }

    equipo-h1plus           OBJECT IDENTIFIER ::= { telobjid 177 }

    equipo-regesta-rp81     OBJECT IDENTIFIER ::= { telobjid 178 }

    equipo-regesta-rp82     OBJECT IDENTIFIER ::= { telobjid 179 }

    equipo-regesta-1        OBJECT IDENTIFIER ::= { telobjid 180 }

    equipo-f1plus           OBJECT IDENTIFIER ::= { telobjid 181 }

    equipo-l1plus           OBJECT IDENTIFIER ::= { telobjid 183 }

    equipo-regesta-rp61er   OBJECT IDENTIFIER ::= { telobjid 184 }

    equipo-regesta-rp62er   OBJECT IDENTIFIER ::= { telobjid 185 }

    equipo-3geplus          OBJECT IDENTIFIER ::= { telobjid 186 }

    equipo-atlas-60         OBJECT IDENTIFIER ::= { telobjid 187 }

    equipo-3geplus-cdma      OBJECT IDENTIFIER ::= { telobjid 188 }

    equipo-h1auto-plus      OBJECT IDENTIFIER ::= { telobjid 189 }

    equipo-k                OBJECT IDENTIFIER ::= { telobjid 190 }

    equipo-v                OBJECT IDENTIFIER ::= { telobjid 191 }

    equipo-connect-104      OBJECT IDENTIFIER ::= { telobjid 192 }

    equipo-h1rail           OBJECT IDENTIFIER ::= { telobjid 193 }

    equipo-kf               OBJECT IDENTIFIER ::= { telobjid 194 }

    equipo-m1               OBJECT IDENTIFIER ::= { telobjid 199 }

    equipo-m1f               OBJECT IDENTIFIER ::= { telobjid 200 }

    equipo-4Ge              OBJECT IDENTIFIER ::= { telobjid 201 }

    router-oa5710v           OBJECT IDENTIFIER ::= { telobjid 202 }

    router-oa5720            OBJECT IDENTIFIER ::= { telobjid 203 }

    router-oa5840            OBJECT IDENTIFIER ::= { telobjid 204 }

    router-oa5850            OBJECT IDENTIFIER ::= { telobjid 205 }

    router-oa5725r61er       OBJECT IDENTIFIER ::= { telobjid 206 }

    router-oa5725r62er       OBJECT IDENTIFIER ::= { telobjid 207 }

    router-oa5725a3g         OBJECT IDENTIFIER ::= { telobjid 208 }

    router-oa5725alte        OBJECT IDENTIFIER ::= { telobjid 209 }

    router-esrwwanenabler    OBJECT IDENTIFIER ::= { telobjid 210 }

    equipo-connect-104-v     OBJECT IDENTIFIER ::= { telobjid 211 }

    equipo-connect-104-kf    OBJECT IDENTIFIER ::= { telobjid 212 }

    equipo-connect-4ge       OBJECT IDENTIFIER ::= { telobjid 213 }

    equipo-bintecrsc         OBJECT IDENTIFIER ::= { telobjid 214 }

    equipo-regesta-lite      OBJECT IDENTIFIER ::= { telobjid 215 }
    
    equipo-bintecrvc         OBJECT IDENTIFIER ::= { telobjid 216 }
        
    equipo-H2auto            OBJECT IDENTIFIER ::= { telobjid 217 }

    equipo-iM8               OBJECT IDENTIFIER ::= { telobjid 219 }

    equipo-iM8-Plus          OBJECT IDENTIFIER ::= { telobjid 220 }

    equipo-H2auto-Plus       OBJECT IDENTIFIER ::= { telobjid 221 }
 
    equipo-regesta-plc       OBJECT IDENTIFIER ::= { telobjid 222 }

    equipo-Atlas-i70         OBJECT IDENTIFIER ::= { telobjid 223 }

    equipo-Atlas-i70-Plus    OBJECT IDENTIFIER ::= { telobjid 224 }

    equipo-h2rail-lite       OBJECT IDENTIFIER ::= { telobjid 225 }
        
    equipo-h2rail-lite2      OBJECT IDENTIFIER ::= { telobjid 226 }

    equipo-h2rail            OBJECT IDENTIFIER ::= { telobjid 227 }

    equipo-regesta-comp-plc  OBJECT IDENTIFIER ::= { telobjid 229 }

    -- Identificadores de los parametros de las traps propietarias de Teldat

    -- sreTrapVar1 OBJECT IDENTIFIER ::= { telobjid 4 }     $M2.2

    -- sreTrapVar2 OBJECT IDENTIFIER ::= { telobjid 5 }     $M2.2

    -- sreTrapVar3 OBJECT IDENTIFIER ::= { telobjid 6 }     $M2.2

    -- sreTrapVar4 OBJECT IDENTIFIER ::= { telobjid 7 }     $M2.2

    -- sreTrapVar5 OBJECT IDENTIFIER ::= { telobjid 8 }     $M2.2

    -- sreTrapVar6 OBJECT IDENTIFIER ::= { telobjid 9 }     $M2.2

    -- sreTrapVar7 OBJECT IDENTIFIER ::= { telobjid 10 }    $M2.2

    -- sreTrapVar8 OBJECT IDENTIFIER ::= { telobjid 11 }    $M2.2

    -- sreTrapVar9 OBJECT IDENTIFIER ::= { telobjid 12 }    $M2.2

    teldatSreTrap   OBJECT IDENTIFIER ::= { telobjid 1 }

    -- sreTrapSubSist  OBJECT IDENTIFIER ::= { telobjid 2 }

    -- sreTrapEvento   OBJECT IDENTIFIER ::= { telobjid 3 }

    -- sreTrapEquipo    OBJECT IDENTIFIER ::= { telobjid 4 }    comentada por $M2.2

    sreTrapSubSist OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "First variable inside the variable-bindings field of the SNMP
            Trap-PDU: Events subsystem number."
        ::= { telobjid 2 }

    sreTrapEvento OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Second variable inside the variable-bindings field of the SNMP
            Trap-PDU: Event number (inside the subsystem)."
        ::= { telobjid 3 }

    sreTrapVar1 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Third variable inside the variable-bindings field of the SNMP
            Trap-PDU: first variable of the event mask."
        ::= { telobjid 4 }

     sreTrapVar2 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Fourth variable inside the variable-bindings field of the SNMP
            Trap-PDU: second variable of the event mask."
        ::= { telobjid 5 }

    sreTrapVar3 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Fifth variable inside the variable-bindings field of the SNMP
            Trap-PDU: third variable of the event mask."
        ::= { telobjid 6 }

    sreTrapVar4 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Sixth variable inside the variable-bindings field of the SNMP
            Trap-PDU: fourth variable of the event mask."
        ::= { telobjid 7 }

    sreTrapVar5 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Seventh variable inside the variable-bindings field of the SNMP
            Trap-PDU: fifth variable of the event mask."
        ::= { telobjid 8 }

    sreTrapVar6 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Eighth variable inside the variable-bindings field of the SNMP
            Trap-PDU: sixth variable of the event mask."
        ::= { telobjid 9 }

    sreTrapVar7 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Ninth variable inside the variable-bindings field of the SNMP
            Trap-PDU: seventh variable of the event mask."
        ::= { telobjid 10 }

    sreTrapVar8 OBJECT-TYPE
        SYNTAX Opaque
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Tenth variable inside the variable-bindings field of the SNMP
            Trap-PDU: eighth variable of the event mask."
        ::= { telobjid 11 }

    sreTrapVar9 OBJECT-TYPE
        SYNTAX  Opaque
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Eleventh variable inside the variable-bindings field of the SNMP
            Trap-PDU: ninth variable of the event mask."
        ::= { telobjid 12 }


  -- Identificadores de los subsistemas que tienen TRAP asociada    $M2.1
  -- En el apartado { teldatSreTrap xyz} xyz es el valor correspondiente al
  -- fichero trpparam.h

    teldatSreTrap-GW        OBJECT IDENTIFIER ::= { teldatSreTrap 1 }
    teldatSreTrap-FLT       OBJECT IDENTIFIER ::= { teldatSreTrap 2 }
    teldatSreTrap-BRS       OBJECT IDENTIFIER ::= { teldatSreTrap 3 }
    teldatSreTrap-ARP       OBJECT IDENTIFIER ::= { teldatSreTrap 5 }
    teldatSreTrap-IP        OBJECT IDENTIFIER ::= { teldatSreTrap 10 }
    teldatSreTrap-ICMP      OBJECT IDENTIFIER ::= { teldatSreTrap 11 }
    teldatSreTrap-TCP       OBJECT IDENTIFIER ::= { teldatSreTrap 12 }
    teldatSreTrap-UDP       OBJECT IDENTIFIER ::= { teldatSreTrap 13 }
    teldatSreTrap-ORIP      OBJECT IDENTIFIER ::= { teldatSreTrap 15 }
--  teldatSreTrap-EGP       OBJECT IDENTIFIER ::= { teldatSreTrap 16 }  $M3.9
    teldatSreTrap-SPF       OBJECT IDENTIFIER ::= { teldatSreTrap 17 }
--  teldatSreTrap-MSPF      OBJECT IDENTIFIER ::= { teldatSreTrap 18 }  $M2.9
    teldatSreTrap-TFTP      OBJECT IDENTIFIER ::= { teldatSreTrap 19 }
--  teldatSreTrap-TN        OBJECT IDENTIFIER ::= { teldatSreTrap 20 }  $M2.9
    teldatSreTrap-SNMP      OBJECT IDENTIFIER ::= { teldatSreTrap 21 }
--  teldatSreTrap-IPX       OBJECT IDENTIFIER ::= { teldatSreTrap 35 }  $M2.9
    teldatSreTrap-SRT       OBJECT IDENTIFIER ::= { teldatSreTrap 72 }
--  teldatSreTrap-STP       OBJECT IDENTIFIER ::= { teldatSreTrap 73 }  $M2.9
    teldatSreTrap-BR        OBJECT IDENTIFIER ::= { teldatSreTrap 74 }
--  teldatSreTrap-SRLY      OBJECT IDENTIFIER ::= { teldatSreTrap 75 }  $M2.9
    teldatSreTrap-FTP       OBJECT IDENTIFIER ::= { teldatSreTrap 80 }  --$M2.9
    teldatSreTrap-ETH       OBJECT IDENTIFIER ::= { teldatSreTrap 81 }
--  teldatSreTrap-PN        OBJECT IDENTIFIER ::= { teldatSreTrap 82 }  $M2.9
    teldatSreTrap-SL        OBJECT IDENTIFIER ::= { teldatSreTrap 83 }
    teldatSreTrap-TKR       OBJECT IDENTIFIER ::= { teldatSreTrap 84 }
--  teldatSreTrap-X25       OBJECT IDENTIFIER ::= { teldatSreTrap 85 }  $M2.9
--  teldatSreTrap-MAN       OBJECT IDENTIFIER ::= { teldatSreTrap 87 }  $M2.9
--  teldatSreTrap-FDDI      OBJECT IDENTIFIER ::= { teldatSreTrap 88 }  $M2.9
--  teldatSreTrap-ATR       OBJECT IDENTIFIER ::= { teldatSreTrap 89 }  $M2.9
    teldatSreTrap-SDLC      OBJECT IDENTIFIER ::= { teldatSreTrap 90 }
    teldatSreTrap-FR        OBJECT IDENTIFIER ::= { teldatSreTrap 92 }
    teldatSreTrap-PPP       OBJECT IDENTIFIER ::= { teldatSreTrap 95 }
--  teldatSreTrap-X251      OBJECT IDENTIFIER ::= { teldatSreTrap 96 }  $M2.9
    teldatSreTrap-X252      OBJECT IDENTIFIER ::= { teldatSreTrap 97 }
    teldatSreTrap-X253      OBJECT IDENTIFIER ::= { teldatSreTrap 98 }
    teldatSreTrap-RDSI      OBJECT IDENTIFIER ::= { teldatSreTrap 99 }
--  teldatSreTrap-IPPN      OBJECT IDENTIFIER ::= { teldatSreTrap 100 } $M2.9
--  teldatSreTrap-R2        OBJECT IDENTIFIER ::= { teldatSreTrap 100 } $M2.9
--  teldatSreTrap-WRS       OBJECT IDENTIFIER ::= { teldatSreTrap 101 } $M2.9
--  teldatSreTrap-LNM       OBJECT IDENTIFIER ::= { teldatSreTrap 102 } $M2.9
    teldatSreTrap-LLC       OBJECT IDENTIFIER ::= { teldatSreTrap 103 }
--  teldatSreTrap-BGP       OBJECT IDENTIFIER ::= { teldatSreTrap 104 } $M2.9
--  teldatSreTrap-MCF       OBJECT IDENTIFIER ::= { teldatSreTrap 105 } $M2.9
--  teldatSreTrap-DLSO      OBJECT IDENTIFIER ::= { teldatSreTrap 107 } $M2.9
--  teldatSreTrap-V25B      OBJECT IDENTIFIER ::= { teldatSreTrap 108 } $M2.9
    teldatSreTrap-BAN       OBJECT IDENTIFIER ::= { teldatSreTrap 109 }
    teldatSreTrap-NBS       OBJECT IDENTIFIER ::= { teldatSreTrap 110 }
    teldatSreTrap-CIF       OBJECT IDENTIFIER ::= { teldatSreTrap 111 }
    teldatSreTrap-GSTP      OBJECT IDENTIFIER ::= { teldatSreTrap 112 }
--  teldatSreTrap-NVA       OBJECT IDENTIFIER ::= { teldatSreTrap 113 } $M2.9
    teldatSreTrap-FRBK      OBJECT IDENTIFIER ::= { teldatSreTrap 114 }
    teldatSreTrap-PRI       OBJECT IDENTIFIER ::= { teldatSreTrap 115 }
    teldatSreTrap-DLS       OBJECT IDENTIFIER ::= { teldatSreTrap 116 }
--  teldatSreTrap-IPTN      OBJECT IDENTIFIER ::= { teldatSreTrap 117 } $M2.9
    teldatSreTrap-PCMC      OBJECT IDENTIFIER ::= { teldatSreTrap 118 }
    teldatSreTrap-LAPD      OBJECT IDENTIFIER ::= { teldatSreTrap 119 }
    teldatSreTrap-TNIP      OBJECT IDENTIFIER ::= { teldatSreTrap 120 }
--  teldatSreTrap-BIRU      OBJECT IDENTIFIER ::= { teldatSreTrap 121 }     Está definida en biru.mib  (pruebas)
--  teldatSreTrap-EBANO     OBJECT IDENTIFIER ::= { teldatSreTrap 122 }     Está definida en ebano.mib (pruebas)
    teldatSreTrap-MBBU      OBJECT IDENTIFIER ::= { teldatSreTrap 123 }
    teldatSreTrap-BIR64     OBJECT IDENTIFIER ::= { teldatSreTrap 124 }
    teldatSreTrap-REXISMRU  OBJECT IDENTIFIER ::= { teldatSreTrap 125 }
    teldatSreTrap-REXISFT   OBJECT IDENTIFIER ::= { teldatSreTrap 126 }
    teldatSreTrap-ICUPLUS   OBJECT IDENTIFIER ::= { teldatSreTrap 127 } --$M2.3
    teldatSreTrap-Q933      OBJECT IDENTIFIER ::= { teldatSreTrap 128 } --$M2.9
    teldatSreTrap-IPPN      OBJECT IDENTIFIER ::= { teldatSreTrap 129 } --$M2.9
    teldatSreTrap-RAD       OBJECT IDENTIFIER ::= { teldatSreTrap 130 } --$M2.9
    teldatSreTrap-H323      OBJECT IDENTIFIER ::= { teldatSreTrap 131 } --$M2.9
--  teldatSreTrap-MIT       OBJECT IDENTIFIER ::= { teldatSreTrap 132 } $M2.9
    teldatSreTrap-DHCP      OBJECT IDENTIFIER ::= { teldatSreTrap 133 } --$M2.9
    teldatSreTrap-IP6       OBJECT IDENTIFIER ::= { teldatSreTrap 134 } --$M2.9
    teldatSreTrap-TVRP      OBJECT IDENTIFIER ::= { teldatSreTrap 135 } --$M2.9
    teldatSreTrap-ATM       OBJECT IDENTIFIER ::= { teldatSreTrap 136 } --$M2.9
--  teldatSreTrap-OLD0      OBJECT IDENTIFIER ::= { teldatSreTrap 137 } $M2.9
    teldatSreTrap-IPSEC     OBJECT IDENTIFIER ::= { teldatSreTrap 138 } --$M2.9
    teldatSreTrap-NTP       OBJECT IDENTIFIER ::= { teldatSreTrap 139 } --$M2.9
    teldatSreTrap-ADSL      OBJECT IDENTIFIER ::= { teldatSreTrap 140 } --$M2.9
--  teldatSreTrap-CIF       OBJECT IDENTIFIER ::= { teldatSreTrap 141 } $M2.9
    teldatSreTrap-HTTP      OBJECT IDENTIFIER ::= { teldatSreTrap 142 } --$M2.9
    teldatSreTrap-DEP       OBJECT IDENTIFIER ::= { teldatSreTrap 144 } --$M2.9
    teldatSreTrap-ASDP      OBJECT IDENTIFIER ::= { teldatSreTrap 145 } --$M2.9
    teldatSreTrap-LDAP      OBJECT IDENTIFIER ::= { teldatSreTrap 146 } --$M2.9
    teldatSreTrap-SCEP      OBJECT IDENTIFIER ::= { teldatSreTrap 147 } --$M2.9
    teldatSreTrap-P3OE      OBJECT IDENTIFIER ::= { teldatSreTrap 148 } --$M2.9
    teldatSreTrap-AT        OBJECT IDENTIFIER ::= { teldatSreTrap 149 } --$M2.9
    teldatSreTrap-ASYNC     OBJECT IDENTIFIER ::= { teldatSreTrap 150 } --$M2.9
    teldatSreTrap-SYNC      OBJECT IDENTIFIER ::= { teldatSreTrap 151 } --$M2.9
    teldatSreTrap-DNS       OBJECT IDENTIFIER ::= { teldatSreTrap 152 } --$M3.6
    teldatSreTrap-VSN       OBJECT IDENTIFIER ::= { teldatSreTrap 153 } --$M3.6
    teldatSreTrap-NAPT      OBJECT IDENTIFIER ::= { teldatSreTrap 154 } --$M3.6
    teldatSreTrap-VID       OBJECT IDENTIFIER ::= { teldatSreTrap 155 } --$M3.6
    teldatSreTrap-PRL       OBJECT IDENTIFIER ::= { teldatSreTrap 156 } --$M3.6
    teldatSreTrap-HDSL      OBJECT IDENTIFIER ::= { teldatSreTrap 157 } --$M3.6
    teldatSreTrap-PGMO      OBJECT IDENTIFIER ::= { teldatSreTrap 158 } --$M3.6
    teldatSreTrap-RTSP      OBJECT IDENTIFIER ::= { teldatSreTrap 159 } --$M3.6
    teldatSreTrap-DNAT      OBJECT IDENTIFIER ::= { teldatSreTrap 160 } --$M3.8
    teldatSreTrap-G703      OBJECT IDENTIFIER ::= { teldatSreTrap 161 } --$M3.9
    teldatSreTrap-POLR      OBJECT IDENTIFIER ::= { teldatSreTrap 162 } --$M3.9
    teldatSreTrap-XN        OBJECT IDENTIFIER ::= { teldatSreTrap 163 } --$M3.9
    teldatSreTrap-XNS       OBJECT IDENTIFIER ::= { teldatSreTrap 164 } --$M3.9
    teldatSreTrap-IPX       OBJECT IDENTIFIER ::= { teldatSreTrap 165 } --$M3.9
    teldatSreTrap-IGMP      OBJECT IDENTIFIER ::= { teldatSreTrap 166 } --$M3.9
    teldatSreTrap-AINST     OBJECT IDENTIFIER ::= { teldatSreTrap 167 } --$M3.9
    teldatSreTrap-BGP       OBJECT IDENTIFIER ::= { teldatSreTrap 169 } --$M4.6
    teldatSreTrap-NSM       OBJECT IDENTIFIER ::= { teldatSreTrap 170 } --$M4.6
    teldatSreTrap-TLNT      OBJECT IDENTIFIER ::= { teldatSreTrap 171 } --$M4.9
    teldatSreTrap-L2TP      OBJECT IDENTIFIER ::= { teldatSreTrap 172 } --$M4.9
    teldatSreTrap-NSLA      OBJECT IDENTIFIER ::= { teldatSreTrap 173 } --$M5.0
    teldatSreTrap-VOIP      OBJECT IDENTIFIER ::= { teldatSreTrap 174 } --$M5.3
    teldatSreTrap-TTTP      OBJECT IDENTIFIER ::= { teldatSreTrap 175 } --$M5.4
    teldatSreTrap-IKE       OBJECT IDENTIFIER ::= { teldatSreTrap 176 }
    teldatSreTrap-HSSI      OBJECT IDENTIFIER ::= { teldatSreTrap 177 }
    teldatSreTrap-SCADA     OBJECT IDENTIFIER ::= { teldatSreTrap 178 }
    teldatSreTrap-VRRP      OBJECT IDENTIFIER ::= { teldatSreTrap 179 }
    teldatSreTrap-SIP       OBJECT IDENTIFIER ::= { teldatSreTrap 180 }
    teldatSreTrap-IPHC      OBJECT IDENTIFIER ::= { teldatSreTrap 181 }
    teldatSreTrap-DHCPC     OBJECT IDENTIFIER ::= { teldatSreTrap 182 }
    teldatSreTrap-CNSL      OBJECT IDENTIFIER ::= { teldatSreTrap 183 }
    teldatSreTrap-TLPHY     OBJECT IDENTIFIER ::= { teldatSreTrap 184 }
    teldatSreTrap-NHRP      OBJECT IDENTIFIER ::= { teldatSreTrap 185 }
    teldatSreTrap-SNAT      OBJECT IDENTIFIER ::= { teldatSreTrap 186 }
    teldatSreTrap-STUN      OBJECT IDENTIFIER ::= { teldatSreTrap 187 }
    teldatSreTrap-WLAN      OBJECT IDENTIFIER ::= { teldatSreTrap 188 }
    teldatSreTrap-SCDFW     OBJECT IDENTIFIER ::= { teldatSreTrap 189 }
    teldatSreTrap-HDLC      OBJECT IDENTIFIER ::= { teldatSreTrap 190 }
    teldatSreTrap-EAP       OBJECT IDENTIFIER ::= { teldatSreTrap 191 }
    teldatSreTrap-EIBZ      OBJECT IDENTIFIER ::= { teldatSreTrap 192 }
    teldatSreTrap-PHYS      OBJECT IDENTIFIER ::= { teldatSreTrap 193 }
    teldatSreTrap-SPOOF     OBJECT IDENTIFIER ::= { teldatSreTrap 194 }
    teldatSreTrap-IRVOZ     OBJECT IDENTIFIER ::= { teldatSreTrap 195 }
    teldatSreTrap-RSTP      OBJECT IDENTIFIER ::= { teldatSreTrap 196 }
    teldatSreTrap-TIDP      OBJECT IDENTIFIER ::= { teldatSreTrap 197 }
    teldatSreTrap-NOE       OBJECT IDENTIFIER ::= { teldatSreTrap 198 }
    teldatSreTrap-AFS       OBJECT IDENTIFIER ::= { teldatSreTrap 199 }
    teldatSreTrap-X28       OBJECT IDENTIFIER ::= { teldatSreTrap 200 }
    teldatSreTrap-BFD       OBJECT IDENTIFIER ::= { teldatSreTrap 203 }
    teldatSreTrap-DNSU      OBJECT IDENTIFIER ::= { teldatSreTrap 204 }
    teldatSreTrap-UDP6      OBJECT IDENTIFIER ::= { teldatSreTrap 205 }
    teldatSreTrap-ICM6O     OBJECT IDENTIFIER ::= { teldatSreTrap 206 }
--  teldatSreTrap-RIP6      OBJECT IDENTIFIER ::= { teldatSreTrap 207 }
    teldatSreTrap-CELL      OBJECT IDENTIFIER ::= { teldatSreTrap 208 }
    teldatSreTrap-SSL       OBJECT IDENTIFIER ::= { teldatSreTrap 209 }
    teldatSreTrap-SCCP      OBJECT IDENTIFIER ::= { teldatSreTrap 210 }
    teldatSreTrap-WWAN      OBJECT IDENTIFIER ::= { teldatSreTrap 211 }
    teldatSreTrap-ISTD      OBJECT IDENTIFIER ::= { teldatSreTrap 212 }
    teldatSreTrap-DOT1X     OBJECT IDENTIFIER ::= { teldatSreTrap 213 }
    teldatSreTrap-EOAM      OBJECT IDENTIFIER ::= { teldatSreTrap 214 }
    teldatSreTrap-SSH       OBJECT IDENTIFIER ::= { teldatSreTrap 215 }
    teldatSreTrap-CDP       OBJECT IDENTIFIER ::= { teldatSreTrap 216 }
    teldatSreTrap-PIO       OBJECT IDENTIFIER ::= { teldatSreTrap 217 }
    teldatSreTrap-FLOW      OBJECT IDENTIFIER ::= { teldatSreTrap 218 }
    teldatSreTrap-RIP       OBJECT IDENTIFIER ::= { teldatSreTrap 219 }
    teldatSreTrap-MGCP      OBJECT IDENTIFIER ::= { teldatSreTrap 220 }
    teldatSreTrap-TIPS      OBJECT IDENTIFIER ::= { teldatSreTrap 221 }
    teldatSreTrap-SRVP      OBJECT IDENTIFIER ::= { teldatSreTrap 222 }
    teldatSreTrap-SPI       OBJECT IDENTIFIER ::= { teldatSreTrap 223 }
    teldatSreTrap-VLI       OBJECT IDENTIFIER ::= { teldatSreTrap 224 }
    teldatSreTrap-ACAT      OBJECT IDENTIFIER ::= { teldatSreTrap 225 }
    teldatSreTrap-AAA       OBJECT IDENTIFIER ::= { teldatSreTrap 226 }
    teldatSreTrap-SDEV      OBJECT IDENTIFIER ::= { teldatSreTrap 227 }
    teldatSreTrap-G104      OBJECT IDENTIFIER ::= { teldatSreTrap 228 }
    teldatSreTrap-I101      OBJECT IDENTIFIER ::= { teldatSreTrap 229 }
    teldatSreTrap-IPSF      OBJECT IDENTIFIER ::= { teldatSreTrap 230 }
    teldatSreTrap-DH6C      OBJECT IDENTIFIER ::= { teldatSreTrap 231 }
    teldatSreTrap-NEIG      OBJECT IDENTIFIER ::= { teldatSreTrap 232 }
    teldatSreTrap-ND        OBJECT IDENTIFIER ::= { teldatSreTrap 233 }
    teldatSreTrap-ICM6      OBJECT IDENTIFIER ::= { teldatSreTrap 234 }
    teldatSreTrap-LLDP      OBJECT IDENTIFIER ::= { teldatSreTrap 235 }
    teldatSreTrap-RIP6      OBJECT IDENTIFIER ::= { teldatSreTrap 236 }
    teldatSreTrap-MLD6      OBJECT IDENTIFIER ::= { teldatSreTrap 237 }
    teldatSreTrap-PIM       OBJECT IDENTIFIER ::= { teldatSreTrap 238 }
    teldatSreTrap-MRTE      OBJECT IDENTIFIER ::= { teldatSreTrap 239 }
    teldatSreTrap-ACL       OBJECT IDENTIFIER ::= { teldatSreTrap 240 }
    teldatSreTrap-SPF6      OBJECT IDENTIFIER ::= { teldatSreTrap 241 }
    teldatSreTrap-NIC       OBJECT IDENTIFIER ::= { teldatSreTrap 242 }
    teldatSreTrap-MSDP      OBJECT IDENTIFIER ::= { teldatSreTrap 244 }
    teldatSreTrap-ACT       OBJECT IDENTIFIER ::= { teldatSreTrap 245 }
    teldatSreTrap-TDGS      OBJECT IDENTIFIER ::= { teldatSreTrap 255 }
    teldatSreTrap-GPSF      OBJECT IDENTIFIER ::= { teldatSreTrap 256 }
    teldatSreTrap-WNMS      OBJECT IDENTIFIER ::= { teldatSreTrap 257 }
    teldatSreTrap-DH6S      OBJECT IDENTIFIER ::= { teldatSreTrap 259 }
    teldatSreTrap-CFM       OBJECT IDENTIFIER ::= { teldatSreTrap 264 }
    teldatSreTrap-PRIME     OBJECT IDENTIFIER ::= { teldatSreTrap 265 }
    teldatSreTrap-SMGT      OBJECT IDENTIFIER ::= { teldatSreTrap 266 }

    telstatus   OBJECT IDENTIFIER ::= { teladmin 2 }

    -- --------------------------
    -- Grupo telAdminStatusSystem
    -- --------------------------
    telAdminStatusSystem    OBJECT IDENTIFIER ::= { telstatus 1 }

    -- $M2.7
    telAdminStatusSystemCode OBJECT-TYPE
        SYNTAX  INTEGER{
--                rexis-ft(3),
--                bir-64(11),
                rexis-mru(15),
                mbbu(16),
                bir-u(20),
                ebano(21),
                nucleox-plus(32),
                cbra(33),
                centrix-b(34),
                centrix-p(35),
                temis(36),
                novacom(37),
                master-router(38),
                cbra2x(39),
                np2xh(40),
                icu-plus(41),
                centrix-f(42),
                cbra-tar(43),
                aura(44),
                kronos(45),
                teldat-C(46),
                remote-operator(47),
                visor(48),
                voxnet(49),
                dusac32(50),
                novacom-x25(51),
                enaplan(52),
                teldat-C3(53),
                atlas(56),
                c2B(57),
                web-probe(58),
                c3-1(59),
                c3B-1(60),
                c2BM(61),
                basic-atlas(62),
                c2i(63),
                c3i(64),
                c3B(65),
                c3G(66),
                -- c4-c5(67),
                c4(67),             --$M4.2
                -- c4i-c5i(68),
                c4i(68),            --$M4.2
                -- c4B-c5B(69),
                c4B(69),            --$M4.2
                centrix-sec(70),
                centrix-d(71),
                c2-UP(72),
                c6(73),             --$M3.8
                centrix-ng(74),     --$M3.9
                atlas-voxnet(75),   --$M3.9
                s2(76),             --$M4.3
                s4(77),             --$M4.3
                s2i(78),            --$M4.3
                s4i(79),            --$M4.3
                g2(80),             --$M4.3
                g3(81),             --$M4.3
                g4(82),             --$M4.3
                g2i(83),            --$M4.3
                g3i(84),            --$M4.3
                g4i(85),            --$M4.3
                c1(86),             --$M4.3
                c1B(87),            --$M4.3
                c1i(88),            --$M4.3
                s1(89),             --$M4.3
                s1i(90),            --$M4.3
                g1(91),             --$M4.3
                g1i(92),            --$M4.3
                g3-lite(93),        --$M4.3
                c3G-lite(94),       --$M4.3
                atlas-100(96),      --$M4.3
                atlas-300V(97),      --$M4.7
                c1G(98),            --$M4.7
                atlas-250(101),
                c4G(102),           --$M6.0
                atlas-100B(103),
                atlas-150(104),
                a2(105),
                a3(106),
                a4(107),
                a2i(108),
                a3i(109),
                a4i(110),
                a1(111),
                a1i(112),
                g4-cdma(114),
                g4i-cdma(115),
                g3-cdma(116),
                g3i-cdma(117),
                g1-cdma(118),
                g1i-cdma(119),
                c1plus(122),
                c1iplus(123),
                atlas-50(126),
                g4plus(127),
                g3plus(128),
                g1plus(129),
                g4iplus(130),
                g3iplus(131),
                g1iplus(132),
                atlas-250-web-probe(133),
                atlas-150-web-probe(134),
                atlas-50-web-probe(135),
                vyda-1M(136),
                vyda-2M(137),
                vyda-3M(138),
                atlas-300(139),
                atlas-152(140),
                vyda-compact(141),
                c8plus(142),
                c8iplus(143),
                c9plus(144),
                c9iplus(145),
                atlas-360(146),
                c1plus-web-probe(147),
                c1a(148),
                s1a(149),
                g1a(150),
                g1a-cdma(151),
                a1a(152),
                c2a(155),
                s2a(156),
                g2a(157),
                a2a(158),
                c4a(159),
                s4a(160),
                g4a(161),
                g4a-cdma(162),
                a4a(163),
                cirus(165),
                h1(166),
                atlas-260(167),
                atlas-160(168),
                vyda-4M(169),
                teldat-t200g(170),
                teldat-h1-auto(171),
                teldat-g1n(172),
                teldat-v1(173),
                teldat-c1plusl(174),
                teldat-h4(175),
                teldat-t200(176),
                teldat-h1plus(177),
                regesta-rp81(178),
                regesta-rp82(179),
                regesta-1(180),
                teldat-f1plus(181),
                teldat-l1plus(183),
                regesta-rp61er(184),
                regesta-rp62er(185),
                teldat-3geplus(186),
                atlas-60(187),
                teldat-3geplus-cdma(188),
                teldat-h1auto-plus(189),
                teldat-k(190),
                teldat-v(191),
                connect-104(192),
                teldat-h1rail(193),
                teldat-kf(194),
                teldat-m1(199),
                teldat-m1f(200),
                teldat-4Ge(201),
                oa5710v(202),
                oa5720(203),
                oa5840(204),
                oa5850(205),
                oa5725r61er(206),
                oa5725r62er(207),
                oa5725a3g(208),
                oa5725alte(209),
                esrwwanenabler(210),
                connect-104v(211),
                connect-104kf(212),
                connect-4ge(213),
                bintecrsc(214),
                regesta-lite(215),
                bintecrvc(216),
                teldat-h2auto(217),
                teldat-im8(219),
                teldat-im8plus(220),
                teldat-h2auto-plus(221),
                regesta-plc(222),
                atlasi70(223),
                atlasi70plus(224),
                teldat-h2rail-lite(225),
                teldat-h2rail-lite2(226),
                teldat-h2rail(227),
                regesta-compact-plc(229)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Product identifier determined by Teldat identifiers table."
        ::={ telAdminStatusSystem 1 }

    -- $M2.7 $M3.9
    telAdminStatusSystemSwLicLev OBJECT-TYPE
        SYNTAX  INTEGER{
                default(0),
                teldatC(1),
                atlas(2),
                visornet(3),
                teldatS(4),
                teldatG(5),
                atlas2G(6),
                atlas150(7),
                teldatA(8),
                atlas50(9),
                atlas300(10),
                atlas152(11),
                teldatc1plus(12),
                teldatc8plus(13),
                teldatc9plus(14),
                atlas360(15),
                teldatH1(16),
                atlas260(17),
                atlas160(18),
                teldatt200g(19),
                teldath1auto(20),
                teldatg1n(21),
                teldatc1pluslite(22),
                teldatv1(23),
                teldatH4-teldatl1plus(24),
                teldatt200(25),
                teldath1plus-teldatf1plus-teldat3Geplus(26),
                regestaPro-ER(27),
                atlas60(28),
                teldath1autoplus(29),
                teldatv(30),
                teldatconnect104(31),
                teldatk(32),
                teldathrail(33),
                teldatm1(34),
                teldat4ge(35),
                teldatconnect104v(36),
                teldatconnect104kf(37),
                teldatconnect4ge(38),
                teldath2auto(39),
                teldatim8(40),
                teldatim8plus(41),
                atlasi70(42),
                atlasi70plus(43),
                teldath2autoplus(44),
                teldath2rail(45)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Main level of software licence. This variable indicates the
            specific family where the product is included. The value 0 is the
            default value taken when the real value is not associated to any
            licence recognized or supported. The possible values for this
            variable and their meaning are:
            (1)  Teldat C.
            (2)  Atlas.
            (3)  Visornet.
            (4)  Teldat S.
            (5)  Teldat G.
            (6)  Atlas 2G.
            (7)  Atlas 150.
            (8)  Teldat A.
            (9)  Atlas 50.
            (10) Atlas 300.
            (11) Atlas 152.
            (12) Teldat C1+.
            (13) Teldat C8+.
            (14) Teldat C9+.
            (15) Atlas 360.
            (16) Teldat H.
            (17) Atlas 260.
            (18) Atlas 160.
            (19) Teldat T200G.
            (20) Teldat H1 Auto.
            (21) Teldat G1N.
            (22) Teldat C1+L.
            (23) Teldat V1.
            (24) Teldat H4 or L1+.
            (25) Teldat T200.
            (26) Teldat H1+, Teldat F1+ or Teldat 3Ge+.
            (27) RegestaPro-ER.
            (28) Atlas 60.
            (29) Teldat H1 Auto.+
            (30) Teldat V
            (31) Teldat Connect 104
            (32) Teldat K
            (33) Teldat H Rail Family
            (34) Teldat M1
            (35) Teldat 4Ge
            (36) Teldat Connect 104V
            (37) Teldat Connect 104KF
            (38) Teldat Connect 4Ge
            (39) Teldat H2 Auto. 
            (40) Teldat H2 Auto Plus.
            (41) Teldat H2 Rail.

            If the value of this variable is teldatC (1), atlas (2),
            visornet (3), teldatS (4), teldatG (5), atlas2g (5), atlas150 (7),
            teldatA (8) or atlas50 (9) it will be necessary to consider also the
            value of the next variable to completely determine the type of the
            accessed product. In any other case, different products can take the
            same value for this level of software licence and second level of
            software licence will be always 0, so it will be not possible to
            distinguish them through their licence."
        ::={ telAdminStatusSystem 2 }

    -- $M2.7
    telAdminStatusSystemSwLicSub OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Second level of software licence. This variable is used to know the
            family funcionality group inside the family indicated with the
            previous value. The value 0 is the only value taken by this variable
            in 360-based routers, and also the default value taken when the
            real value is not associated to any licence recognized or supported.
            It is necessary to consider also the value of the previous variable
            to completely determine the type of the product accessed."
        ::={ telAdminStatusSystem 3 }

    telAdminStatusSystemNumSerie OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Series number of the node."
        ::={ telAdminStatusSystem 4 }

    telAdminStatusSystemPcbType OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Board type."
        ::={ telAdminStatusSystem 5 }

    telAdminStatusSystemAppVersion OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Version of the application running at the moment in the system."
        ::={ telAdminStatusSystem 6 }

    telAdminStatusSystemBootVersion OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Version of the system eprom software."
        ::={ telAdminStatusSystem 7 }

    telAdminStatusSystemClock OBJECT-TYPE
        SYNTAX  OCTET STRING(SIZE(8))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Node time and date. 8 Bytes EBCDIC show respectively
            seconds, minutes, padding, day, month, week day (monday, etc)
            and year."
        ::={ telAdminStatusSystem 8 }

    --$M3.8
    telAdminStatusSystemBoardType OBJECT-TYPE
        SYNTAX  INTEGER{
                adsl-860(8),
                visornet-860(16),
                h1-autoplus(24),
                adsl-855(32),
                h1-rail(40),
                cbra-univ(56),
                visornet-2C(48),
                atlas(64),
                cbra-dual(72),
                tldt-new-C3(80),
                univ-tjt(88),   --$M3.9
                tldt-m(96),     --$M4.4
                hermes(112),
                univ-bas(120),
                zeus(128),
                nike(136),
                minos(144),
                pnlp(152),
                hades(160),
                tldt-m-a(168),
                univ-tjt-a(184),
                at-h1(192),
                tldt-t200(176),
                h1-auto(200),
                at-h4(208),
                tldt-t200-w(216),
                h1-like-h2-rail(224),
                ares(272),
                at-160(288),
                iropro(296),
                tldt-k(304),
                tldt-m1(312),
                anteth4g(320),
                tldt-im1(328),
                tldt-im2(336),
                tldt-h2-auto-plus(368),
                tldt-h2-rail(376),
                c1plusl(520),
                v1(528),
                h1plus(536),
                c1plusl-b(544),
                c1plusl-ur2(552),
                c1plusl-annexm(560),
                rp61er(576),
                rp62er(584),
                rp61er-ac(592),
                rp62er-ac(600),
                vdsl2(608),
                rp62er-ur2(616),
                rp61er-ur2(624),
                rp62er-ac-ur2(632),
                rp61er-ac-ur2(640),
                rp62er-bj(648),
                rp61er-bj(656),
                rp62er-ac-bj(664),
                rp61er-ac-bj(672),
                rp62er-j(680),
                rp61er-j(688),
                rp62er-ac-j(696),
                rp61er-ac-j(704),
                rp62er-b(712),
                rp61er-b(720),
                rp62er-ac-b(728),
                rp61er-ac-b(736),
                rp21er(744),
                rp22er(752),
                v1-bj(760),
                rp-plc(872),
                rp-cmp-plc(880)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Board type."
        ::={ telAdminStatusSystem 9 }

    --$M3.8
    telAdminStatusSystemBoardRevision OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Board revision."
        ::={ telAdminStatusSystem 10 }

    --$M3.8
    telAdminStatusSystemSmartCard OBJECT-TYPE
        SYNTAX  INTEGER{
                no(0),
                yes(1)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This variable indicates whether Smart Card controler is installed.
            Possible values: no(0), yes(1)."
        ::={ telAdminStatusSystem 11 }

    -- Tabla telAdminStatusLedsTable

    telAdminStatusLedsTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelAdminStatusLedsEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The table telAdminStatusLedsTable contains information about
            leds."
        ::={ telstatus 2 }

    telAdminStatusLedsEntry OBJECT-TYPE
        SYNTAX  TelAdminStatusLedsEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry contains the number and state of each led."
        INDEX   { telAdminStatusLedNum }
        ::={ telAdminStatusLedsTable 1 }

    TelAdminStatusLedsEntry ::=
        SEQUENCE{
            telAdminStatusLedNum
                INTEGER,
            telAdminStatusLedStatus
                INTEGER
                }

    telAdminStatusLedNum OBJECT-TYPE
        SYNTAX  INTEGER{
                led-1(1),
                led-2(2),
                led-3(3),
                led-4(4),
                led-5(5),
                led-6(6),
                led-7(7),
                led-8(8),
                led-9(9),
                led-10(10),
                led-11(11),
                led-12(12),
                led-13(13),
                led-14(14),
                led-15(15),
                led-16(16),
                led-17(17),
                led-18(18),
                led-19(19),
                led-20(20),
                led-21(21),
                led-22(22),
                led-23(23),
                led-24(24)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Led identifier number."
        ::={ telAdminStatusLedsEntry 1 }

    telAdminStatusLedStatus OBJECT-TYPE
        SYNTAX  INTEGER{
                off(0),
                red(1),
                green(2),
                orange(3)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Led state."
        ::={ telAdminStatusLedsEntry 2 }

    -- Tabla telAdminStatusBugsTable

    telAdminStatusBugsTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelAdminStatusBugsEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "The table named telAdminStatusBugsTable gives information about
            the system bug messages."
        ::={ telstatus 3 }

    telAdminStatusBugsEntry OBJECT-TYPE
        SYNTAX  TelAdminStatusBugsEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "Each entry contains the message number (1 is the last) and the
            string of the corresponding message."
        INDEX   { telAdminStatusBugNum }
        ::={ telAdminStatusBugsTable 1 }

    TelAdminStatusBugsEntry ::=
        SEQUENCE{
            telAdminStatusBugNum
                INTEGER,
            telAdminStatusBugMsg
                DisplayString
        }

    telAdminStatusBugNum OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Bug number."
        ::={ telAdminStatusBugsEntry 1 }

    telAdminStatusBugMsg OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Bug text."
        ::={ telAdminStatusBugsEntry 2 }

    telAdminStatusBugsClear OBJECT-TYPE
        SYNTAX  INTEGER{
                not-delete-bugs(0),
                delete-bugs(1)
            }
        ACCESS  read-write
        STATUS  obsolete
        DESCRIPTION
            "In a writing operation, 1 resets the number of bugs stored
            by the system, in a reading operation it is always 0."
        ::={ telstatus 4 }

    telAdminStatusReload OBJECT-TYPE
        SYNTAX  INTEGER{
                undefined(0),
                reset(1),
                already-reset(2),
                not-reset(3)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "In a writing operation 1 resets the system (Reset Hard),
            In a reading operation, 0 shows unknown output from the last
            set operation, 2 shows the set operation succeded and 3 shows
            the last set operation failed."
        ::={ telstatus 5 }

    telAdminStatusRestart OBJECT-TYPE
        SYNTAX  INTEGER{
                undefined(0),
                restart(1),
                restarted(2),
                not-restarted(3)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "In a writing operation 1 resets the system (Reset Soft),
            In a reading operation, 0 shows the unknown output from the last
            set operation, 2 shows the set operation succeded and 3 shows
            the last set operation failed."
        ::={ telstatus 6 }

    telAdminStatusSaveConfig OBJECT-TYPE
        SYNTAX  INTEGER{
                undefined(0),
                save-configuration(1),
                saved-configuration(2),
                not-saved-configuration(3)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "In a writing operation 1 saves to RAM the current system
            configuration. In a reading operation, 0 shows unknown output from
            the last set operation, 2 shows the set operation succeded
            and 3 shows the last set operation failed."
        ::={ telstatus 7 }

    -- Grupo telAdminStatusSram

    telAdminStatusSram  OBJECT IDENTIFIER ::= { telstatus 8 }

    -- Tabla telAdminStatusSramRecordTable

    telAdminStatusSramRecordTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelAdminStatusSramRecordEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "The table telAdminStatusSramRecordTable contains information about
            non volatil or SRAM system memory. This memory consists of records
            that are instances of concrete types and subtypes."
        ::={ telAdminStatusSram 1 }

    telAdminStatusSramRecordEntry OBJECT-TYPE
        SYNTAX  TelAdminStatusSramRecordEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "Each entry gives information about type, subtype, instance and
            specific object in SRAM."
        INDEX   { sramRecordType,
                  sramRecordSubtype,
                  sramRecordInstance }
        ::={ telAdminStatusSramRecordTable 1 }

    TelAdminStatusSramRecordEntry ::=
        SEQUENCE{
            sramRecordType
                INTEGER,
            sramRecordSubtype
                INTEGER,
            sramRecordInstance
                INTEGER,
            sramRecordItem
                Opaque
        }

    sramRecordType OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "SRAM register type."
        ::= { telAdminStatusSramRecordEntry 1 }

    sramRecordSubtype OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "SRAM register subtype."
        ::= { telAdminStatusSramRecordEntry 2 }

    sramRecordInstance OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Instance of the SRAM register."
        ::= { telAdminStatusSramRecordEntry 3 }

    sramRecordItem OBJECT-TYPE
        SYNTAX  Opaque
        ACCESS  read-write
        STATUS  obsolete
        DESCRIPTION
            "Specific SRAM register. Since registers may have different sizes
            depending on the data type of the object (type and subtype), the
            writing operations only must be performed if the data type of each
            object (type and subtype) is known. In case data types were not
            similar, the final configuration could result erroneous."
        ::= { telAdminStatusSramRecordEntry 4}

    -- Grupo telAdminStatusSRE

    telAdminStatusSRE   OBJECT IDENTIFIER ::= { telstatus 9 }

    -- Tabla telAdminStatusSRESubRecordTable

    telAdminStatusSRESubRecordTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelAdminStatusSRESubRecordEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The table telAdminStatusSRESubRecordTable contains information
            about the event subsystem."
        ::={ telAdminStatusSRE 1 }

    telAdminStatusSRESubRecordEntry OBJECT-TYPE
        SYNTAX  TelAdminStatusSRESubRecordEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry contains information about identifier, short name,
            long name, level, event number and if the concrete subsystem
            is enabled or not for traces, syslog messages and/or SNMP traps."
        INDEX   { sreSubId }
        ::={ telAdminStatusSRESubRecordTable 1 }

    TelAdminStatusSRESubRecordEntry ::=
        SEQUENCE{
            sreSubId
                INTEGER,
            sreSubShortName
                DisplayString,
            sreSubLongName
                DisplayString,
            sreSubNumEvent
                INTEGER,
            sreSubTraceLvlConf
                INTEGER,
            sreSubSyslogLvlConf
                INTEGER,
            sreSubTrapLvlConf
                INTEGER,
            sreSubTrap1LvlConf
                INTEGER,
            sreSubTrap2LvlConf
                INTEGER,
            sreSubTrap3LvlConf
                INTEGER,
            sreSubTrap4LvlConf
                INTEGER
        }

    sreSubId OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Subsystem identifier."
        ::= { telAdminStatusSRESubRecordEntry 1 }

    sreSubShortName OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Subsystem short name."
        ::= { telAdminStatusSRESubRecordEntry 2 }

    sreSubLongName OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Subsystem long name."
        ::= { telAdminStatusSRESubRecordEntry 3 }

    sreSubNumEvent OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Number of subsystem defined events."
        ::= { telAdminStatusSRESubRecordEntry 4}

    sreSubTraceLvlConf OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This mask defines the way the subsystem is enabled for traces. The
            mask´s meaning is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSRESubRecordEntry 5}

    sreSubSyslogLvlConf OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This mask defines the way the subsystem is enabled for syslog
            messages.
            The mask´s meaning is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSRESubRecordEntry 6}

    sreSubTrapLvlConf OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This mask defines the way the subsystem is enabled for SNMP traps.
            The mask´s meaning is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSRESubRecordEntry 7}

    sreSubTrap1LvlConf OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This mask defines the way the subsystem is enabled for SNMP traps
            group 1.
            The mask´s meaning is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSRESubRecordEntry 8}

    sreSubTrap2LvlConf OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This mask defines the way the subsystem is enabled for SNMP traps
            group 2.
            The mask´s meaning is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSRESubRecordEntry 9}

    sreSubTrap3LvlConf OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This mask defines the way the subsystem is enabled for SNMP traps
            group 3.
            The mask´s meaning is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSRESubRecordEntry 10}

    sreSubTrap4LvlConf OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This mask defines the way the subsystem is enabled for SNMP traps
            group 4.
            The mask´s meaning is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSRESubRecordEntry 11}

    -- Tabla telAdminStatusSREEventRecordTable

    telAdminStatusSREEventRecordTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelAdminStatusSREEventRecordEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The table telAdminStatusSREEventRecordTable contains information
            about the subsystem events."
        ::={ telAdminStatusSRE 2 }

    telAdminStatusSREEventRecordEntry OBJECT-TYPE
        SYNTAX  TelAdminStatusSREEventRecordEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry contains information about the subsystem identifier,
            event identifier in the subsystem, mask of the event message,
            event level, times the event occured, current enable mask and
            configured enable mask."
        INDEX   { sreEvnSubId, sreEvnEvnId }
        ::={ telAdminStatusSREEventRecordTable 1 }

    TelAdminStatusSREEventRecordEntry ::=
        SEQUENCE{
            sreEvnSubId
                INTEGER,
            sreEvnEvnId
                INTEGER,
            sreEvnMsg
                DisplayString,
            sreEvnLvl
                INTEGER,
            sreEvnMeter
                Counter,
            sreEvnStatusAct
                INTEGER,
            sreEvnStatusCon
                INTEGER
        }

    sreEvnSubId OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, it is similar
            to the subsystem identifier that exists in the subsystem table."
        ::= { telAdminStatusSREEventRecordEntry 1 }

    sreEvnEvnId OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREEventRecordEntry 2 }

    sreEvnMsg OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event message mask."
        ::= { telAdminStatusSREEventRecordEntry 3 }

    sreEvnLvl OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Message level. It is a mask with the following meaning:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSREEventRecordEntry 4}

    sreEvnMeter OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Times the event has ocurred since the last restart/reload.
            The meaning of the mask is:
            (UI-ERROR,0x0001); (CI-ERROR,0x0002); (UE-ERROR,0x0004);
            (CE-ERROR,0x0008); (ERROR,0x000F); (U-INFO,0x0010); (C-INFO,0x0020);
            (INFO,0x0030); (P-TRACE,0x0100); (U-TRACE,0x0200); (C-TRACE,0x0400)
            (TRACE,0x0700); (STANDARD,0x001F); (ALWAYS,0x8000); (ALL,0xFFFF)"
        ::= { telAdminStatusSREEventRecordEntry 5}

    sreEvnStatusAct OBJECT-TYPE
        SYNTAX  INTEGER(0..255)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The mask defines the way the event is enabled at the moment.
            The meaning of the mask is:
            (for traces,0x01); (for syslog messages, 0x02);
            (for SNMP traps, 0x04); (all, 0x07); (for specific traps with
            correspondence with generic traps, 0x08); (disabled, 0x00)"
        ::= { telAdminStatusSREEventRecordEntry 6}

    sreEvnStatusCon OBJECT-TYPE
        SYNTAX  INTEGER(0..255)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The mask defines the way the event is enabled in configuration at
            the moment. The meaning of the mask is:
            (for traces,0x01); (for syslog messages, 0x02);
            (for SNMP traps, 0x04); (all, 0x07);
            (disabled, 0x00)"
        ::= { telAdminStatusSREEventRecordEntry 7}

    -- Tabla telAdminStatusSREGroupRecordTable

    telAdminStatusSREGroupRecordTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelAdminStatusSREGroupRecordEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The table telAdminStatusSREGroupRecordTable contains information
            about defined sets of events."
        ::={ telAdminStatusSRE 3 }

    telAdminStatusSREGroupRecordEntry OBJECT-TYPE
        SYNTAX  TelAdminStatusSREGroupRecordEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry contains information about the group identifier,
            group name, enable mask, and the event and subsystem identifier
            for each of the 20 possible events of the group."
        INDEX   { sreGrpId }
        ::={ telAdminStatusSREGroupRecordTable 1 }

    TelAdminStatusSREGroupRecordEntry ::=
        SEQUENCE{
            sreGrpId
                INTEGER,
            sreGrpName
                DisplayString,
            sreGrpStatusCon
                INTEGER,
            sreGrpGrpSub1Id
                INTEGER,
            sreGrpGrpEvn1Id
                INTEGER,
            sreGrpGrpSub2Id
                INTEGER,
            sreGrpGrpEvn2Id
                INTEGER,
            sreGrpGrpSub3Id
                INTEGER,
            sreGrpGrpEvn3Id
                INTEGER,
            sreGrpGrpSub4Id
                INTEGER,
            sreGrpGrpEvn4Id
                INTEGER,
            sreGrpGrpSub5Id
                INTEGER,
            sreGrpGrpEvn5Id
                INTEGER,
            sreGrpGrpSub6Id
                INTEGER,
            sreGrpGrpEvn6Id
                INTEGER,
            sreGrpGrpSub7Id
                INTEGER,
            sreGrpGrpEvn7Id
                INTEGER,
            sreGrpGrpSub8Id
                INTEGER,
            sreGrpGrpEvn8Id
                INTEGER,
            sreGrpGrpSub9Id
                INTEGER,
            sreGrpGrpEvn9Id
                INTEGER,
            sreGrpGrpSub10Id
                INTEGER,
            sreGrpGrpEvn10Id
                INTEGER,
            sreGrpGrpSub11Id
                INTEGER,
            sreGrpGrpEvn11Id
                INTEGER,
            sreGrpGrpSub12Id
                INTEGER,
            sreGrpGrpEvn12Id
                INTEGER,
            sreGrpGrpSub13Id
                INTEGER,
            sreGrpGrpEvn13Id
                INTEGER,
            sreGrpGrpSub14Id
                INTEGER,
            sreGrpGrpEvn14Id
                INTEGER,
            sreGrpGrpSub15Id
                INTEGER,
            sreGrpGrpEvn15Id
                INTEGER,
            sreGrpGrpSub16Id
                INTEGER,
            sreGrpGrpEvn16Id
                INTEGER,
            sreGrpGrpSub17Id
                INTEGER,
            sreGrpGrpEvn17Id
                INTEGER,
            sreGrpGrpSub18Id
                INTEGER,
            sreGrpGrpEvn18Id
                INTEGER,
            sreGrpGrpSub19Id
                INTEGER,
            sreGrpGrpEvn19Id
                INTEGER,
            sreGrpGrpSub20Id
                INTEGER,
            sreGrpGrpEvn20Id
                INTEGER
        }

    sreGrpId OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Group identifier."
        ::= { telAdminStatusSREGroupRecordEntry 1 }

    sreGrpName OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Group name."
        ::= { telAdminStatusSREGroupRecordEntry 2 }

    sreGrpStatusCon OBJECT-TYPE
        SYNTAX  INTEGER(0..255)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The mask defines the way the group is enabled at the moment.
            The meaning of the mask is:
            (for traces,0x01); (for syslog messages, 0x02);
            (for SNMP traps, 0x04); (all, 0x07);
            (disabled, 0x00)"
        ::= { telAdminStatusSREGroupRecordEntry 3 }

    sreGrpGrpSub1Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that apperars in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 4}

    sreGrpGrpEvn1Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 5}

    sreGrpGrpSub2Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 6}

    sreGrpGrpEvn2Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 7}

    sreGrpGrpSub3Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 8}

    sreGrpGrpEvn3Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 9}

    sreGrpGrpSub4Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 10}

    sreGrpGrpEvn4Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 11}

    sreGrpGrpSub5Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 12}

    sreGrpGrpEvn5Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 13}

    sreGrpGrpSub6Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 14}

    sreGrpGrpEvn6Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 15}

    sreGrpGrpSub7Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 16}

    sreGrpGrpEvn7Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 17}

    sreGrpGrpSub8Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 18}

    sreGrpGrpEvn8Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 19}

    sreGrpGrpSub9Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 20}

    sreGrpGrpEvn9Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 21}

    sreGrpGrpSub10Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 22}

    sreGrpGrpEvn10Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 23}

    sreGrpGrpSub11Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 24}

    sreGrpGrpEvn11Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 25}

    sreGrpGrpSub12Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 26}

    sreGrpGrpEvn12Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 27}

    sreGrpGrpSub13Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 28}

    sreGrpGrpEvn13Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 29}

    sreGrpGrpSub14Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 30}

    sreGrpGrpEvn14Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 31}

    sreGrpGrpSub15Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 32}

    sreGrpGrpEvn15Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 33}

    sreGrpGrpSub16Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 34}

    sreGrpGrpEvn16Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 35}

    sreGrpGrpSub17Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 36}

    sreGrpGrpEvn17Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 37}

    sreGrpGrpSub18Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 38}

    sreGrpGrpEvn18Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 39}

    sreGrpGrpSub19Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 40}

    sreGrpGrpEvn19Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 41}

    sreGrpGrpSub20Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Identifier of the subsystem the event belongs to, similar to the
            subsystem identifier that appears in the subsystems table."
        ::= { telAdminStatusSREGroupRecordEntry 42}

    sreGrpGrpEvn20Id OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Event identifier in the subsystem."
        ::= { telAdminStatusSREGroupRecordEntry 43}

   -- Variable de limpieza de configuracion de eventos

    telAdminStatusSREClearConf OBJECT-TYPE
        SYNTAX  INTEGER{
                with-configuration(0),
                without-configuration(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This variable deletes the events configuration of the router.
            If a set operation is performed we can select without-configuration
            (1) to delete the events configuration. The configuration
            takes effect after reseting the router."
        ::= { telAdminStatusSRE 4}

    -- Tabla telAdminStatusIfTable

    telAdminStatusIfTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelAdminStatusIfEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The table telAdminStatusifTable contains specific information about
            Teldat interfaces."
        ::={ telstatus 10 }

    telAdminStatusIfEntry OBJECT-TYPE
        SYNTAX  TelAdminStatusIfEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry gives information about the interface type, connector
            type, and a description of the hardware type for each interface."
        INDEX   { telAdminStatusIfIndex }
        ::={ telAdminStatusIfTable 1 }

    TelAdminStatusIfEntry ::=
        SEQUENCE{
            telAdminStatusIfIndex
                INTEGER,
            telAdminStatusIfType
                INTEGER,
            telAdminStatusIfCon
                INTEGER,
            telAdminStatusIfHdw
                DisplayString
                }

    telAdminStatusIfIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Interface index."
        ::={ telAdminStatusIfEntry 1 }

    -- $M2.5 $M3.2
    telAdminStatusIfType OBJECT-TYPE
        SYNTAX  INTEGER{
            --sr-PRO10(1),                  Pronet-10 interface
            --sr-PRO80(2),                  Pronet-80 interface
            --sr-ETHER(3),                  Interlan Ethernet interface
            --sr-1822(4),                   M/1822 ARPAnet interface
            --sr-COM2(5),                   SBE COM-2 serial interface
            sr-MICRO-NODE-X25-NET(1),       --Net ficticia de X25
            --sr-MICRO-NODE-RDSI-B-NET(2),  Net ficticia de RDSI
            sr-PCI-WAN-PQ2-SDLC(2),         --SDLC sobre WAN PCI
            sr-MICRO-NODE-ISAC-NET(3),      --Net ficticia canal D RDSI
            sr-MICRO-NODE-XOT-NET(4),
            sr-MICRO-NODE-270-NET(5),
            sr-COM4(6),                     --SBE COM-4 serial interface
            sr-PRO4(7),                     --Pronet-4 interface
            sr-IBD(8),                      --Self-boot hardware type
            --sr-PETH(9),                   Tldtnet Ethernet interface
            sr-PCI-AMDETH(9),               --AMD79C973 Ethernet Interface
            --sr-WDETH(10),                 Western Digital Ethernet interface (LER)
            sr-AMDETH(10),                  --AMD79C960 Ethernet Interface
            --sr-GWSL(11),                  GW Serial Line interface (LER)
            sr-QUIC-SL-X28(11),             --Serial Line interface - X.28
            sr-QUIC-SL-ASTM(12),            --SBE Com-4 X.25interface
            --sr-XCOM4(12),                 SBE Com-4 X.25interface
            --sr-FDDI(13),                  Fiber Distributed Data Interface
            sr-QUIC-SL-UDAFO(13),           --Interfaz UDAFO
            --sr-VLANE(14),                 SBE VLAN-E Ethernet interface
            sr-FASTETH(14),                 --860T Fast Ethernet
            sr-VCOM4(15),                   --SBE VCOM-4 serial interface
            --sr-ATR(16),                   Apollo Token Ring
            sr-dummy-voip(16),              --VOIP dummy
            sr-PCI-CELLULAR-VOIP(17),       --VOIP cellular
            sr-ATC2(18),                    --AT COM-2
            --sr-XATC2(19),                 AT COM-2 X.25
            --sr-I5ETH(20),                 Intel 82596 Ethernet interface
            --sr-GENSL(21),                 Dual Serial Line for CNX (Louie)
            sr-DIAL-G-HDLC(19),             --HDLC encapsulation dial circuit
            sr-DIAL-G-FR(20),               --FR encapsulation dial circuit
            sr-DIAL-G-PPP(21),              --PPP encapsulation dial circuit
            sr-DIAL-G-X25(22),              --X25 encapsulation dial circuit
            --sr-NP600(22),                 Racal InterLan NP600 smart Ethernet
            sr-SRLY-GWSL(23),               --SDLC relay interface for gateway SL
            sr-SRLY-ATC2(24),               --SDLC relay interface for ATComm2 SL
            sr-SRLY-G1SL(25),               --SDLC relay interface for Louie SL
            sr-FRGENSL(26),                 --Frame Relay on Genesis serial line
            sr-NSETH(27),                   --National Semiconductor Ethernet
            sr-TELDAT-BVI-SUBIFC(28),       --Subinterfaz BVI
            --sr-FRATC2(29),                Frame Relay on ATComm2 T1
            sr-TELDAT-FR-SUBIFC(29),        --Subinterfaz FR
            sr-PPPGENSL(30),                --PPP on Genesis serial line
            sr-PPPATC2(31),                 --PPP on ATComm2 T1
            sr-PPPCOM2(32),                 --PPP on P4200 COM2
            sr-QSL(33),                     --Quad Serial Line for CNX (Weasel)
            sr-PPPQSL(34),                  --PPP Quad Serial Line for CNX
            sr-FRQSL(35),                   --Frame Relay Quad Serial Line for CNX
            sr-SRLY-QSL(36),                --SDLC Relay Quad Serial Line for CNX
            sr-XQSL(37),                    --X.25 Quad Serial Line for CNX
            sr-NULL-DEV(38),                --NULL DEVICE
            sr-YDC-ISDN(39),                --ISDN port on CNX 500
            --sr-DIAL-SLC(40),              Tldtnet encapsulation dial circuit
            sr-DIAL-FR(40),                 --FR encapsulation dial circuit
            sr-DIAL-PPP(41),                --PPP encapsulation dial circuit
            sr-QUIC-PRI-SIG(42),            --Channel 16 signalling
            --sr-DNX-YDC-ISDN(42),          ISDN port on DNX 300
            sr-SDLC-QSL(43),                --SDLC protocol over QSL
            sr-QSLCH(44),                   --QSL for DNX
            sr-SDLC-QSLCH(45),              --SDLC protocol over QSL
            sr-PPP-QSLCH(46),               --PPP over QSL
            sr-FR-QSLCH(47),                --Frame Relay over QSL
            sr-XQSLCH(48),                  --X.25 Quad Serial Line for DNX
            sr-SRLY-QSLCH(49),              --SRLY Quad Serial Line for DNX
            sr-PCI-PRI-ACODES(50),          --PCI E1/T1 sobre Acodes 490x
            sr-PCI-BRI-ACODES(51),          --PCI soporte VoIP isdn BRI-TE
            sr-ISDN-VOIP(52),               --Soporte ISDN VoIP como dial
            sr-SL-HSSI(53),                 --SLC for High Speed Serial Interface
            sr-FR-HSSI(54),                 --Frame-Relay for HSSI
            sr-PPP-HSSI(55),                --PPP for HSSI
            sr-QUIC-ETH(56),                --Quicksilver Ethernet
            sr-QUIC-TKR(57),                --Quicksilver 802.5 Token-Ring
            sr-QUIC-SL-PSL(58),             --Quicksilver Serial - Tldtnet Serial
            sr-QUIC-SL-PPP(59),             --Quicksilver Serial - PPP
            sr-QUIC-SL-X25(60),             --Quicksilver Serial - X.25
            sr-QUIC-SL-FR(61),              --Quicksilver Serial - Frame Relay
            sr-QUIC-SL-SRLY(62),            --Quicksilver Serial - SDLC Relay
            sr-QUIC-SL-SDLC(63),            --Quicksilver Serial - Real SDLC
            sr-QUIC-SL-V25B(64),            --Quicksilver Serial - V.25bis
            sr-QUIC-ISDNH(65),              --Quicksilver ISDN - Host based
            sr-TEL-PRU(66),                 --Teldat test
            sr-TEL-PRU-FAST(67),            --Teldat test !!!! FAST  !!!!
            sr-TEL-MOTOROLA(68),            --Teldat Router->Node
            sr-TELDAT-TKR(69),              --Teldat Token Ring
            sr-TELDAT-ETH(70),              --Teldat Ethernet
            sr-TELDAT-ISAC(71),             --Controller ISAC de RDSI
            sr-TELDAT-XOT(72),              --Port XOT
            sr-TELDAT-270(73),              --Port 270
            sr-TELDAT-TNIP(74),             --IP Tunnel
            sr-TELDAT-MPPP(75),             --Multilink PPP
            sr-FR-ISDN(76),                 --FR over RDSI
            sr-TELDAT-ATM(77),              --ATM interface
            sr-TELDAT-ATM-SUBIFC(78),       --ATM subinterface
            sr-TELDAT-ASDP(79),             --Interfaz ASDP
            sr-QMC-BRI(80),                 --BRI
            sr-TELDAT-SYNC-SL(81),          --Interfaz serie sincrono   $M2.8
            sr-TELDAT-ASYNC-SL(82),         --Interfaz serie asincrono  $M2.8
            sr-QUIC-SL-APTB(83),            --Async Port Bridge $M3.9
            sr-TELDAT-ATM-FS(84),           --Generic ATM with FireStream $M3.9
            sr-TELDAT-LPBK(85),             --Interfaz de Loopback (real) $M3.9
            sr-TELDAT-PCI-PRI-M32X(86),     --PCI/PRI with Munich32X $M3.9
            sr-TELDAT-DIALROUT(87),         --Interfaz DIAL ROUTE $M3.9
            --sr-DSCC4-ASYNC(88),           ASYNC sobre PCI DSCC4 $M3.9
            sr-PCI-WAN-PQ2-ASYNC(88),       --ASYNC sobre PCI 8272
            sr-DSCC4-ATC2(89),              --AT sobre PCI DSCC4 $M3.9
            --sr-DSCC4-SYNC(90),            SYNC sobre PCI DSCC4 $M3.9
            sr-PCI-WAN-PQ2-SYN(90),         --SYNC sobre PCI 8272
            sr-PCI-AMD-MICREL-ETH(91),      --AMD79C973 Ethernet con Switch KS8995M $M3.9
            sr-MOT-MICREL-ETH(92),          --Motorola FEC con Switch KS8995M $M4.1
            sr-ALARM-RELY(93),              --Reenvia alarmas recibidas a Sw alarmas $M4.2
            sr-PCI-MEMORY-CARD(94),         --Tarjeta de memoria PCI $4.2
            sr-TELDAT-ETH-SUBIFC(95),       --Subinterfaz ethernet para vlan $M4.6
            sr-PCI-POTS-VOIP-CARD(96),      --PCI soporte VoIP analogico $M4.7
            sr-PCI-BRI-VOIP-CARD(97),       --PCI soporte VoIP isdn bri $M4.7
            sr-PCI-PRI-VOIP-CARD(98),       --PCI soporte VoIP isdn pri $M4.7
            sr-PCI-E-M-VOIP-CARD(99),       --PCI soporte VoIP analógico $M4.9
            sr-TELDAT-LOOPBACK(100),        --Loopback interface
            sr-TELDAT-L2TP(101),            --Interfaz virtual L2TP $M4.9
            sr-FCC-ETH(102),                --FCC Fast Ethernet Interface
            sr-PCMCIA-SERIAL(103),          --PCMCIA Serial (Modem o UMTS)
            sr-DSCC4-HSSI(104),             --HSSI sobre PCI DSCC4
            sr-TELDAT-BVI(105),             --Bridge Virtual Interface
            sr-QUIC-SL-SCADA(106),          --SCADA Serial Interface
            sr-TELDAT-ATM-PQ2SAR(107),      --Tarjeta PCI ATM con PQ2SAR
            sr-PCI-QMC-BRI(108),            --Tarjeta PCI PQ2BRI
            sr-PCI-POTS-3S10VOIP-CARD(109), --PCI soporte VoIP analógico 3DXS, 1FXO con bypass
            sr-PCI-POTS-2S2OVOIP-CARD(110), --PCI soporte VoIP analógico 2FXS, 2FXO con bypass
            sr-PCI-INTEL-GIGABIT-ETH(111),  --Tarjeta PCI GIGABIT Ethernet Intel 8254x
            sr-ATHEROS-WLAN-BASE(112),      --WLAN
            sr-FCC-MARVELL(113),            --Ethernet Switch 8 o 16 puertas
            sr-TELDAT-SEPI(114),            --Interfaz SEPI
            sr-FCC-MICREL(115),             --Ethernet Switch 4
            sr-ETSEC-ETH(116),              --Enhanced Three Speed Ethernet Controller Power Quicc III
            sr-EIB-ZENNIO(117),             --Interfaz EIB zennio
            sr-GPIO-12(118),
            sr-QUIC-AUTO-INST-SL(119),
            sr-PCI-PRI-PQ2(120),
            sr-ETSEC-MARVELL-ETH(121),      --ETSEC + SWITCH
            sr-QUIC-SL-MODEMEMU(122),       --Interfaz de emulación de modem AT
            sr-PCI-VALARM-SL-MDMEMU(123),   --AT Modem Emulatión sobre PCI VisorAlarm UL
            sr-PCI-VALARM-SL-SEPI(124),     --Interfaz SEPI sobre PCI VisorAlarm UL
            sr-PCI-CELLULAR(125),           --Interfaz PCI HSDPA
            sr-REMOTE-CELLULAR(126),        --Interfaz Remote Cellular
            sr-PCI-WAN-PQ2-SCADA(127),      --Interfaz SCADA sobre PMC de 3 WAN
            sr-TELDAT-ETH-SOFTETH(128),
            sr-TELDAT-ATM-SOFTSAR(129),     -- SOFTSAR
            sr-PCI-PQII-FCC-MARVELL-ETH(130), -- PQII + PCI + MARVELL
            sr-TELDAT-ETH-SOFTPTM(131),     -- SOFTPTM
            sr-TELDAT-SERIAL-SOFTUSB(132),  -- SOFTUSB
            sr-PCI-PQII-WDMPON(133),        -- PQII + PCI + INTEL + WDMPON(NORTEL)
            sr-TELDAT-SOFTWLAN-BASE(134),   -- SOFTWLAN
            sr-PCI-WAN-PQ2-ASTM(135),
            sr-PCI-WAN-PQ2-X28(136),
            sr-PCI-WAN-PQ2-ASDP(137),
            sr-TELDAT-SOFTNIC(138),
            sr-DIAL-G-DIP(139),             -- Direct IP Encapsulation dial circuit
            sr-TELDAT-USBNIC(140),
            sr-ATHEROS-WLAN-VAP(141),       --Subinterfaz WLAN
            sr-TELDAT-SOFTWAN(142),
            sr-TELDAT-SWETH(143),           --Interfaz Ethernet segregado de switch
            sr-QUIC-SL-IEC101GW(144),
            sr-PCI-WAN-PQ2-IEC101GW(145),
            sr-TELDAT-SOFTUART(146),
            sr-TELDAT-SOFTSCADA(147),
            sr-TELDAT-SOFTIEC101GW(148),
            sr-TELDAT-SOFTASDP(149),
            sr-STANDALONE-GPS(150),
            sr-SL-GPSDATA(151),
            sr-SOFTWLAN-VAP(152),
            sr-FSL-CELLULAR(153),           --Freescale EHCI-USB on-chip controller
            sr-SOFTETH-SWITCH(154),
            sr-TELDAT-USBETH(155),
            sr-TELDAT-SOFTUSBETH(156),
            sr-TELDAT-ETH-FMAN(157),
            sr-TELDAT-ETH-FMAN-SWITCH(158),
            sr-TELDAT-SOFTPRIME(159),
            sr-FSL-GPSUSB(160),
            sr-TELDAT-ETH-FMAN-MII(161),
            sr-XHCI-CELLULAR(162),          --Renesas XHCI-USB controller
            sr-MICRO-NODE-ROUTER(61441),    --Teldat Node->Router
            sr-MICRO-NODE-RDSI-B(61442),    --Teldat Channel B: X.25
            sr-MICRO-NODE-ISAC(61443),      --Teldat Channel D:X.25
            sr-MICRO-NODE-X25(61444),       --Teldat X.25
            sr-MICRO-NODE-XOT(61445),       --Teldat XOT
            sr-MICRO-NODE-270(61446)        --Teldat 270
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Teldat Specific Interface Type."
        ::={ telAdminStatusIfEntry 2 }

    telAdminStatusIfCon OBJECT-TYPE
        SYNTAX  INTEGER{
                no-conn(0),     -- Los valores se extraen del fichero comu.ha
                lan-conn(1),
                wan1-conn(2),
                wan2-conn(3),
                wan3-conn(4),
                wan4-conn(5),
                wan5-conn(6),
                wan6-conn(7),
                wan7-conn(8),
                wan8-conn(9),
                rdsi1-conn(10),
                rdsi2-conn(11),
                adsl1-conn(12),
                adsl2-conn(13),
                adsl3-conn(14),
                adsl4-conn(15),
                lan-conn-exp(16),
                uart1-conn(17),
                uart2-conn(18),
                uart3-conn(19),
                uart4-conn(20),
                rs232-conn(21),
                rs485-conn(22),
                slot1-conn(23),
                slot2-conn(24),
                slot3-conn(25),
                rf-conn(26),
                lan1-conn(27),
                lan2-conn(28),
                lan3-conn(29),
                lan4-conn(30),
                pots-conn(31),
                slot4-conn(32),
                slot5-conn(33),
                exp-switch1(34),
                usb-conn(35),
                ethwan-conn(36),
                config-conn(37),
                lan1-switch-conn(38),
                irp-slot3-conn(39),
                usb-uart-conn-1(40),
                usb-uart-conn-2(41),
                gps-conn(42),
                rf-conn-1(43),
                rf-conn-2(44),
                usb-conn-1(45),
                usb-conn-2(46),
                irp-slot2-conn(47),
                wifi1-conn(48),
                wifi2-conn(49),
                im-slot1-conn(50),
                im-slot2-conn(51),
                prime-pw-conn(52),
                slot1-switch-0-conn(53),
                slot1-switch-1-conn(54)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Connector related to the interface."
        ::={ telAdminStatusIfEntry 3 }

    telAdminStatusIfHdw OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Description of the hardware related to the interface."
        ::={ telAdminStatusIfEntry 4 }

    telAdminStatusEthTime OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Date and time Ethernet statistics were updated for last time."
        ::={ telstatus 11 }

    telAdminConfActDev OBJECT-TYPE
        SYNTAX  INTEGER
                    {
                        smartcard-flash(1),
                        smartcard(2),
                        flash(3)
                    }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Active Device. Device used to read and write configuration files."
        ::={ telstatus 12 }

    telAdminConfConfSavedDev OBJECT-TYPE
        SYNTAX  INTEGER
                    {
                        smartcard(1),
                        flash(2),
                        smartcard-flash(3)
                    }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Device where the last configuration has been saved."
        ::={ telstatus 13 }

    telAdminStatusConfirmConfig OBJECT-TYPE
        SYNTAX  INTEGER{
                confirmed(0),
                test-cnfg-inactive(1),
                test-cnfg-active(2),
                configuration-recovered(3),
                undefined(4)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "In a writing operation 1 confirms the current configuration.
            In a writing operation 0 rejects the current test configuration
            restarting the device with the previous configuration.
            In a reading operation, 0 shows that the current configuration has
            been confirmed, 1 shows that the current configuration has not been
            confirmed yet (therefore it is a testing configuration) and it is
            active the old ones, 2 shows that the current configuration
            has not been confirmed yet (therefore it is a testing configuration)
            and it is active the new ones, 3 shows that the old configuration
            has been recovered and it is confirmed and active, 4 shows unknown
            state"
        ::={ telstatus 14 }


    telAdminStatusConfirmEnabled OBJECT-TYPE
        SYNTAX  INTEGER{
                disable(0),
                enable(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "In a writing operation 1 enables the need to confirm the
            saved configuration. In a writing operation 0 disables the
            need to confirm the newly saved configurations.
            In a reading operation, 0 shows that the need to confirm the saved
            configurations is disabled. In a reading operation, 1 shows that
            the need to confirm the saved configurations is enabled."
        ::={ telstatus 15 }

     telAdminStatusTimeoutConfirm OBJECT-TYPE
        SYNTAX  INTEGER(60..3024000)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "In a writing operation values between 60 to 3024000 configures
            the new configuration test time which the device will wait before
            restarting the previous configuration if confirmation is not carried out.
            The minimum is one minute and the maximum is 5 weeks.
            In a reading operation, values between 60 to 3024000 shows the test
            time which the device will wait before restarting the previous
            configuration if confirmation is not carried out."
        ::={ telstatus 16 }

     telAdminStatusSaveRunningConfig OBJECT-TYPE
        SYNTAX  INTEGER{
                undefined(0),
                save-configuration(1),
                saved-configuration(2),
                not-saved-configuration(3)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "In a writing operation 1 saves to flash the current running
            configuration. In a reading operation, 0 shows unknown output from
            the last set operation, 2 shows the set operation succeeded
            and 3 shows the last set operation failed."
        ::={ telstatus 17 }


    -- $M4.0 $M4.5
    -- -----------------
    -- Grupo telMciTraps
    -- -----------------
    -- En este grupo se recogen las traps que se generan en para el proceso
    -- de sondeo de los estados de los TE-Circuits encargado por MCI

    telMciTraps                     OBJECT IDENTIFIER ::= { teladmin 3 }

    -- Datos del TE-Circuit
    -- telTrapVarIPAddr                OBJECT IDENTIFIER ::= { telMciTraps 1 }
    -- telTrapVarVelCir                OBJECT IDENTIFIER ::= { telMciTraps 2 }
    -- telTrapVarVelBckp               OBJECT IDENTIFIER ::= { telMciTraps 3 }
    -- telTrapVarPrioBackp             OBJECT IDENTIFIER ::= { telMciTraps 4 }
    -- telTrapVarTipoBackp             OBJECT IDENTIFIER ::= { telMciTraps 5 }
    -- telTrapVarTipoEquip             OBJECT IDENTIFIER ::= { telMciTraps 6 }

    -- Datos de la WildCard
    -- telTrapVarCustomerName          OBJECT IDENTIFIER ::= { telMciTraps 7 }
    -- telTrapVarRouterName            OBJECT IDENTIFIER ::= { telMciTraps 8 }
    -- telTrapVarRouterPort            OBJECT IDENTIFIER ::= { telMciTraps 9 }
    -- telTrapVarCircuitID             OBJECT IDENTIFIER ::= { telMciTraps 10 }

    -- Secuencia del trap
    -- telTrapVarSequenceNum           OBJECT IDENTIFIER ::= { telMciTraps 11 }

    -- Datos del TE-Circuit

    telTrapVarIPAddr OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "IP address of the circuit."
        ::= { telMciTraps 1 }

    telTrapVarVelCir OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Speed of the circuit."
        ::= { telMciTraps 2 }

    telTrapVarVelBckp OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Speed of the backup line."
        ::= { telMciTraps 3 }

    telTrapVarPrioBackp OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Backup priority."
        ::= { telMciTraps 4 }

    telTrapVarTipoBackp OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Backup type."
        ::= { telMciTraps 5 }

    telTrapVarTipoEquip OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Device model."
        ::= { telMciTraps 6 }

    -- Datos de la WildCard

    telTrapVarCustomerName OBJECT-TYPE
        SYNTAX DisplayString
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Customer Name."
        ::= { telMciTraps 7 }

    telTrapVarRouterName OBJECT-TYPE
        SYNTAX DisplayString
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Router name. Format: ShortCustomerName+LocationName+ESP+aXXX."
        ::= { telMciTraps 8 }

    telTrapVarRouterPort OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Port or the router."
        ::= { telMciTraps 9 }

    telTrapVarCircuitID OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Circuit identifier."
        ::= { telMciTraps 10 }

    -- Secuencia del trap

    telTrapVarSequenceNum OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Number of the sequence."
        ::= { telMciTraps 11 }

    -- Traps generadas

    -- Circuito pasa a estado UP
    telTECircuitTrapUp TRAP-TYPE
        ENTERPRISE telMciTraps
        VARIABLES { telTrapVarIPAddr, telTrapVarVelCir, telTrapVarVelBckp,
                    telTrapVarPrioBackp, telTrapVarTipoBackp,
                    telTrapVarTipoEquip, telTrapVarCustomerName,
                    telTrapVarRouterName, telTrapVarRouterPort,
                    telTrapVarCircuitID, telTrapVarSequenceNum }
        DESCRIPTION
            "The TE-Circuit is UP."
        ::= 1

    -- Circuito pasa a estado BACKUP
    telTECircuitTrapBackup TRAP-TYPE
        ENTERPRISE telMciTraps
        VARIABLES { telTrapVarIPAddr, telTrapVarVelCir, telTrapVarVelBckp,
                    telTrapVarPrioBackp, telTrapVarTipoBackp,
                    telTrapVarTipoEquip, telTrapVarCustomerName,
                    telTrapVarRouterName, telTrapVarRouterPort,
                    telTrapVarCircuitID, telTrapVarSequenceNum }
        DESCRIPTION
            "The TE-Circuit is BACKUP."
        ::= 2

    -- Circuito pasa a estado DOWN
    telTECircuitTrapDown TRAP-TYPE
        ENTERPRISE telMciTraps
        VARIABLES { telTrapVarIPAddr, telTrapVarVelCir, telTrapVarVelBckp,
                    telTrapVarPrioBackp, telTrapVarTipoBackp,
                    telTrapVarTipoEquip, telTrapVarCustomerName,
                    telTrapVarRouterName, telTrapVarRouterPort,
                    telTrapVarCircuitID, telTrapVarSequenceNum }
        DESCRIPTION
            "The TE-Circuit is DOWN."
        ::= 3

    -- --------------
    -- Grupo telproto
    -- --------------

    -- Grupo del Protocolo IP
    telproip            OBJECT IDENTIFIER ::= { telproto 2 }

    -- Router por defecto
    teldefgw            OBJECT IDENTIFIER ::= { telproip 1 }

    telProtoIpDefGwAddress OBJECT-TYPE
        SYNTAX  IpAddress
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "IP address of the default router of the system."
        ::= { teldefgw 1 }

    telProtoIpDefGwCost OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Cost of the default router of the system."
        ::= { teldefgw 2 }

    telProtoIpDefGwAge OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Age of the default router of the system."
        ::= { teldefgw 3 }

    -- Grupo de frame-relay
    telprofr    OBJECT IDENTIFIER ::= { telproto 3 }

    -- Tabla telfrLmiTable

    telfrLmiTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelfrLmiEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The table telfrLmiTable contains LMI information about each
            frame-relay interface of the system."
        ::={ telprofr 1 }

    telfrLmiEntry OBJECT-TYPE
        SYNTAX  TelfrLmiEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry contains LMI information of the interface."
        INDEX   { telfrLmiifIndex }
        ::={ telfrLmiTable 1 }

    TelfrLmiEntry ::=
        SEQUENCE{
            telfrLmiifIndex
                INTEGER,
            telfrLmiBroadcas
                INTEGER,
            telfrLmiMonitConges
                INTEGER,
            telfrLmiMonitCIR
                INTEGER,
            telfrLmiOrphans
                INTEGER,
            telfrLmiIRIncrement
                INTEGER,
            telfrLmiIRDecrement
                INTEGER,
            telfrLmiMIRCIR
                INTEGER
        }

    telfrLmiifIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Frame-relay interface (ifIndex)."
        ::={ telfrLmiEntry 1 }

    telfrLmiBroadcas OBJECT-TYPE
        SYNTAX  INTEGER{
                false(0),
                true(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "It points out if there is a broadcast service in the interface."
        ::={ telfrLmiEntry 2 }

    telfrLmiMonitConges OBJECT-TYPE
        SYNTAX  INTEGER{
                false(0),
                true(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "It points out if the interface performs congestion monitoring."
        ::={ telfrLmiEntry 3 }

    telfrLmiMonitCIR OBJECT-TYPE
        SYNTAX  INTEGER{
                false(0),
                true(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "It points out if the interface performs CIR monitoring."
        ::={ telfrLmiEntry 4 }

    telfrLmiOrphans OBJECT-TYPE
        SYNTAX  INTEGER{
                false(0),
                true(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "It points out if orphan circuits exit."
        ::={ telfrLmiEntry 5 }

    telfrLmiIRIncrement OBJECT-TYPE
        SYNTAX  INTEGER(1..100)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Percentage of IR increase."
        ::={ telfrLmiEntry 6 }

    telfrLmiIRDecrement OBJECT-TYPE
        SYNTAX  INTEGER(1..100)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Percentage of IR decrease."
        ::={ telfrLmiEntry 7 }

    telfrLmiMIRCIR OBJECT-TYPE
        SYNTAX  INTEGER(1..100)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "MIR as CIR percentage."
        ::={ telfrLmiEntry 8 }

    -- Tabla telfrCircuitTable

    telfrCircuitTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelfrCircuitEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The table telfrCircuitTable contains information about every
            configured PVC circuit in the different frame-relay interfaces
            of the system. This information does no appear in the frCircuitTable
            table."
        ::={ telprofr 2 }

    telfrCircuitEntry OBJECT-TYPE
        SYNTAX  TelfrCircuitEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry contains information about every PVC of the interface."
        INDEX   { telfrCircuitifIndex, telfrCircuitDlci }
        ::={ telfrCircuitTable 1 }

    TelfrCircuitEntry ::=
        SEQUENCE{
            telfrCircuitifIndex
                INTEGER,
            telfrCircuitDlci
                INTEGER,
            telfrCircuitCifrar
                INTEGER,
            telfrCircuitBack-Up-FR
                INTEGER,
            telfrCircuitBack-Up-RDSI
                INTEGER,
            telfrCircuitBack-Up-RDSI-siempre
                INTEGER,
            telfrCircuitName
                DisplayString
        }

    telfrCircuitifIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Frame-relay interface (ifIndex)."
        ::={ telfrCircuitEntry 1 }

    telfrCircuitDlci OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "DLCI number of the PVC."
        ::={ telfrCircuitEntry 2 }

    telfrCircuitCifrar OBJECT-TYPE
        SYNTAX  INTEGER{
                false(0),
                true(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
        "Coding or not data."
        ::={ telfrCircuitEntry 3 }

    telfrCircuitBack-Up-FR OBJECT-TYPE
        SYNTAX  INTEGER(16..1007)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Back Up circuit through frame-relay."
        ::={ telfrCircuitEntry 4 }

    telfrCircuitBack-Up-RDSI OBJECT-TYPE
        SYNTAX  INTEGER(16..1007)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Back Up circuit through RDSI."
        ::={ telfrCircuitEntry 5 }

    telfrCircuitBack-Up-RDSI-siempre OBJECT-TYPE
        SYNTAX  INTEGER{
                false(0),
                true(1)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Back Up to RDSI when this is possible through FR, regardless of the
            reasons."
        ::={ telfrCircuitEntry 6 }

    telfrCircuitName OBJECT-TYPE
        SYNTAX  DisplayString(SIZE(0..23))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Circuit name assigned."
        ::={ telfrCircuitEntry 7 }

    -- Grupo de isdn
    telproisdn  OBJECT IDENTIFIER ::= { telproto 4 }

    -- Tabla telproisdncallTable

    telproisdncallTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelproisdncallEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "The table telproisdncallTable contains information about the rdsi
            active calls of the system."
        ::={ telproisdn 1 }

    telproisdncallEntry OBJECT-TYPE
        SYNTAX  TelproisdncallEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "Each entry contains information about a rdsi line."
        INDEX   { telproisdncallid }
        ::={ telproisdncallTable 1 }

    TelproisdncallEntry ::=
        SEQUENCE{
            telproisdncallstatus
                INTEGER,
            telproisdncalltype
                INTEGER,
            telproisdncallref
                INTEGER,
            telproisdncallchannel
                INTEGER,
            telproisdncallid
                INTEGER,
            telproisdncallcallednum
                DisplayString,
            telproisdncallcallingnum
                DisplayString,
            telproisdncallchargedunits
                INTEGER,
            telproisdncallinittime
                OCTET STRING,
            telproisdncallinitdate
                OCTET STRING
            }

    telproisdncallstatus OBJECT-TYPE
        SYNTAX  INTEGER{
            inactive(0),
            active(1)
            }
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Call state. It shows if there is really an active call
            in this line."
        ::={ telproisdncallEntry 1 }

    telproisdncalltype OBJECT-TYPE
        SYNTAX  INTEGER{
            incoming(0),
            outgoing(1)
            }
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Call type."
        ::={ telproisdncallEntry 2 }

    telproisdncallref OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Call reference."
        ::={ telproisdncallEntry 3 }

    telproisdncallchannel OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Channel B used to perform the call."
        ::={ telproisdncallEntry 4 }

    telproisdncallid OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "RDSI line used to perform the call."
        ::={ telproisdncallEntry 5 }

    telproisdncallcallednum OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Called number."
        ::={ telproisdncallEntry 6 }

    telproisdncallcallingnum OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Calling number."
        ::={ telproisdncallEntry 7 }

    telproisdncallchargedunits OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Cost of the call."
        ::={ telproisdncallEntry 8 }

    telproisdncallinittime OBJECT-TYPE
        SYNTAX  OCTET STRING
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Byte string that shows hours, minutes and seconds since
            the call was initiated."
        ::={ telproisdncallEntry 9 }

    telproisdncallinitdate OBJECT-TYPE
        SYNTAX  OCTET STRING
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Byte string that shows the date the call was initiated."
        ::={ telproisdncallEntry 10 }

    -- Tabla telproisdncallhistoryTable

    telproisdncallhistoryTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF TelproisdncallhistoryEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "The table telproisdncallhistoryTable contains information about
            the rdsi calls released of the system."
        ::={ telproisdn 2 }

    telproisdncallhistoryEntry OBJECT-TYPE
        SYNTAX  TelproisdncallhistoryEntry
        ACCESS  not-accessible
        STATUS  obsolete
        DESCRIPTION
            "Each entry contains information about a released rdsi call."
        INDEX   { telproisdncallhistoryindex }
        ::={ telproisdncallhistoryTable 1 }

    TelproisdncallhistoryEntry ::=
        SEQUENCE{
            telproisdncallhistoryindex
                INTEGER,
            telproisdncallhistorytype
                INTEGER,
            telproisdncallhistoryref
                INTEGER,
            telproisdncallhistorychannel
                INTEGER,
            telproisdncallhistoryid
                INTEGER,
            telproisdncallhistorycallednum
                DisplayString,
            telproisdncallhistorycallingnum
                DisplayString,
            telproisdncallhistorychargedunits
                INTEGER,
            telproisdncallhistorycause
                INTEGER,
            telproisdncallhistorydiagnostic
                INTEGER,
            telproisdncallhistoryinittime
                OCTET STRING,
            telproisdncallhistoryendtime
                OCTET STRING,
            telproisdncallhistoryinitdate
                OCTET STRING,
            telproisdncallhistoryenddate
                OCTET STRING
            }

    telproisdncallhistoryindex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "The index identifies each table entry. The smallest indexes fit
            the calls released more time ago."
        ::={ telproisdncallhistoryEntry 1 }

    telproisdncallhistorytype OBJECT-TYPE
        SYNTAX  INTEGER{
                incoming(0),
                outgoing(1)
            }
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Call type."
        ::={ telproisdncallhistoryEntry 2 }

    telproisdncallhistoryref OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Call reference."
        ::={ telproisdncallhistoryEntry 3 }

    telproisdncallhistorychannel OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Channel B used to perform the call."
        ::={ telproisdncallhistoryEntry 4 }

    telproisdncallhistoryid OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "RDSI line used to perform the call."
        ::={ telproisdncallhistoryEntry 5 }

    telproisdncallhistorycallednum OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Called number."
        ::={ telproisdncallhistoryEntry 6 }

    telproisdncallhistorycallingnum OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Calling number."
        ::={ telproisdncallhistoryEntry 7 }

    telproisdncallhistorychargedunits OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Cost of the call."
        ::={ telproisdncallhistoryEntry 8 }

    telproisdncallhistorycause OBJECT-TYPE
        SYNTAX  INTEGER{
            non-attributed-number(1),
            no-route-to-destination(3),
            unacceptable-channel(6),
            normal-call-release(16),
            user-busy(17),
            user-do-not-answer(18),
            notified-user-no-answer-from-user(19),
            rejected-call(21),
            changed-number(22),
            destination-out-of-service(27),
            non-valid-number-format(28),
            normal(31),
            no-circuit-or-available-channel(34),
            network-out-of-service(38),
            temporal-failure(41),
            congestion-in-switching-node(42),
            demanded-circuit-or-non-available-channel(44),
            non-available-resources(47),
            non-available-quality-of-service(49),
            not-authorized-carrier-capacity(57),
            not-authorized-carrier-capacity-at-the-moment(58),
            service-class-or-non-available-option(63),
            not-performed-carrier-capacity(65),
            not-performed-channel-type(66),
            not-performed-option-or-service(79),
            non-valid-call-reference-value(81),
            non-existent-identified-channel(82),
            incompatible-destination(88),
            non-valid-message(95),
            mandatory-information-element-absent(96),
            message-type-non-existent-or-non-performed(97),
            message-non-existent-or-non-performed(98),
            information-element-non-existent-or-non-performed(99),
            information-element-content-non-valid(100),
            incompatible-message-with-call-status(101),
            recovering-at-timer-expiration(102),
            protocol-error(111),
            interworking(127)
            }
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Release reasons."
        ::={ telproisdncallhistoryEntry 9 }

    telproisdncallhistorydiagnostic OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Release diagnostic."
        ::={ telproisdncallhistoryEntry 10 }

    telproisdncallhistoryinittime OBJECT-TYPE
        SYNTAX  OCTET STRING
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "String of bytes that shows the hours, minutes and seconds since
            the call was initiated."
        ::={ telproisdncallhistoryEntry 11 }

    telproisdncallhistoryendtime OBJECT-TYPE
        SYNTAX  OCTET STRING
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "String of bytes that shows the hours, minutes and seconds since
            the call was finished."
        ::={ telproisdncallhistoryEntry 12 }

    telproisdncallhistoryinitdate OBJECT-TYPE
        SYNTAX  OCTET STRING
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Byte string that shows the date the call was initiated."
        ::={ telproisdncallhistoryEntry 13 }

    telproisdncallhistoryenddate OBJECT-TYPE
        SYNTAX  OCTET STRING
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
            "Byte string that shows the date the call was finished."
        ::={ telproisdncallhistoryEntry 14 }

    -- Traps relacionadas con la mib de teldat

    telSistemaEventos TRAP-TYPE
        ENTERPRISE teldat
        VARIABLES { sreTrapSubSist, sreTrapEvento, sreTrapVar1, sreTrapVar2,
                    sreTrapVar3, sreTrapVar4, sreTrapVar5, sreTrapVar6,
                    sreTrapVar7, sreTrapVar8, sreTrapVar9 }
        DESCRIPTION
            "This trap shows the event happened in the system. In order to
             identify the event, the trap has the mask of the event and
             its parameters, moreover, the subsystem and the event number
             in the subsystem. Furthermore it has the sequence number of
             the traps of the same type."
        ::= 1

    -- Identifier for new event traps

    telEventTraps                     OBJECT IDENTIFIER ::= { teladmin 4 }

END
