-- This module defines enterprise MIBs for VPN Phase two
-- negotiation.
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-VPN-PHASETWO-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenVpn, netscreenVpnMibModule
        FROM NETSCREEN-SMI
    Integer32, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    ;

netscreenVpnPhasetwoMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines NetScreen private MIBs for VPN Phase two
         negotiation."
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311130000Z" -- November 13, 2003
    DESCRIPTION
        "Correct spelling mistake"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "no comment"
    REVISION      "200105140000Z" -- May 14, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenVpnMibModule 6 }

NsVpnPhTwoEntry ::= SEQUENCE
{
    nsVpnPhTwoIndex           Integer32,
    nsVpnPhTwoName            DisplayString,
    nsVpnPhTwoPFS             Integer32,
    nsVpnPhTwoEncapMethod     INTEGER,
    nsVpnPhTwoESPEncryp       INTEGER,
    nsVpnPhTwoESPAuth         INTEGER,
    nsVpnPhTwoAhAuth          INTEGER,
    nsVpnPhTwoLifetime        Integer32,
    nsVpnPhTwoLifetimeMeasure INTEGER,
    nsVpnPhTwoLifetimeKb      Integer32,
    nsVpnPhTwoVsys            Integer32
}

nsVpnPhaseTwoCfg OBJECT IDENTIFIER ::= { netscreenVpn 6 }

nsVpnPhTwoTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsVpnPhTwoEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "To establish an IKE IPSec tunnel, two phases of negotiation
         are required. This table specifies the configuration attributes
         for Phase Two negotiation. In Phase 2, the participants
         negotiate the IPSec SAs for encrypting and  authenticating the
         ensuing exchanges of user data."
    ::= { nsVpnPhaseTwoCfg 1 }

nsVpnPhTwoEntry OBJECT-TYPE
    SYNTAX        NsVpnPhTwoEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each entry in the nsVpnPhTwoTable holds a set of configuration
         parameters associated with an instance of Phase 2 setting."
    INDEX
        { nsVpnPhTwoIndex }
    ::= { nsVpnPhTwoTable 1 }

nsVpnPhTwoIndex OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A unique value for phase Two table.  Its value ranges between
         1 and 65535 and may not be contiguous.  The index has no other
         meaning but a pure index"
    ::= { nsVpnPhTwoEntry 1 }

nsVpnPhTwoName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Phase two proposal name."
    ::= { nsVpnPhTwoEntry 2 }

nsVpnPhTwoPFS OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Perfect Forward Secrecy - Diffie-Hellman exchange group."
    ::= { nsVpnPhTwoEntry 3 }

nsVpnPhTwoEncapMethod OBJECT-TYPE
    SYNTAX        INTEGER {
        ah(0),
        esp(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Phase two proposal encapsulation method."
    ::= { nsVpnPhTwoEntry 4 }

nsVpnPhTwoESPEncryp OBJECT-TYPE
    SYNTAX        INTEGER {
        null(0),
        des(1),
        triple-des(2),
        aes(3),
        aes-192(4),
        aes-256(5)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Phase two proposal ESP encryption algorithm."
    ::= { nsVpnPhTwoEntry 5 }

nsVpnPhTwoESPAuth OBJECT-TYPE
    SYNTAX        INTEGER {
        null(0),
        md5(1),
        sha(2),
        sha-256(3)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Phase two proposal ESP authentication Algorithm."
    ::= { nsVpnPhTwoEntry 6 }

nsVpnPhTwoAhAuth OBJECT-TYPE
    SYNTAX        INTEGER {
        null(0),
        md5(1),
        sha(2)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Phase two proposal AH authentication Algorithm."
    ::= { nsVpnPhTwoEntry 7 }

nsVpnPhTwoLifetime OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Lifetime in time"
    ::= { nsVpnPhTwoEntry 8 }

nsVpnPhTwoLifetimeMeasure OBJECT-TYPE
    SYNTAX        INTEGER {
        second(0),
        minute(1),
        hours(2),
        days(3)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "life time measurement."
    ::= { nsVpnPhTwoEntry 9 }

nsVpnPhTwoLifetimeKb OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Lifetime in KBytes"
    ::= { nsVpnPhTwoEntry 10 }

nsVpnPhTwoVsys OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "vsys this proposal configuration belongs to."
    ::= { nsVpnPhTwoEntry 11 }

END


